{"text_format":"1","workbook":"xlsx","n_sheets":10,"sheets":["Main","Inertia","Drives","Motor","LinMotor","Hilfe","Help","Changes","Calc","Graphic"],"not_rendered":{"charts":5,"images":68,"macros":1,"external_links":0,"defined_names":203,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Main","index":0,"n_rows":197,"n_cols":22,"rows_kept":197,"cut":false,"hidden":false,"merged":[[4,20,7,20],[13,12,13,13],[9,7,9,10],[10,7,10,10],[22,16,23,17],[21,14,21,15],[21,8,21,9],[20,8,20,9],[58,7,59,7],[1,12,5,17],[8,1,8,10],[8,14,8,16],[19,11,19,17],[58,6,59,6],[58,8,59,8],[56,7,57,7],[56,8,57,8],[58,1,59,1],[58,2,59,2],[54,1,55,1],[56,1,57,1],[56,2,57,2],[54,2,55,2],[51,1,52,1],[60,6,61,6],[60,8,61,8],[22,13,23,13],[22,12,23,12],[24,10,25,10],[51,8,52,8],[26,8,27,8],[26,11,27,15],[26,9,27,9],[49,8,50,8],[26,10,27,10],[45,8,46,8],[54,7,55,7],[54,8,55,8],[47,8,48,8],[75,8,76,8],[75,6,76,7],[82,1,83,1],[82,2,83,2],[73,8,74,8],[75,3,76,3],[73,1,74,1],[73,2,74,2],[75,1,76,1],[90,0,92,0],[70,4,70,5],[68,4,69,5],[77,1,78,1],[77,2,78,2],[77,3,78,3],[80,1,81,1],[80,2,81,2],[80,3,81,3],[80,4,81,5],[71,4,72,5],[93,1,94,1],[91,10,92,10],[90,10,90,16],[77,4,78,5],[77,6,78,7],[77,8,78,8],[82,3,83,3],[82,4,83,5],[84,1,85,1],[84,2,85,2],[84,6,85,7],[84,8,85,8],[86,6,87,7],[86,8,87,8],[86,1,87,1],[86,2,87,2],[86,3,87,3],[86,4,87,5],[84,3,85,3],[84,4,85,5],[82,6,83,7],[82,8,83,8],[80,6,81,7],[80,8,81,8],[49,2,50,2],[51,2,52,2],[58,3,59,3],[58,4,59,4],[56,3,57,3],[56,4,57,4],[51,3,52,3],[54,4,55,4],[51,5,52,5],[49,3,50,3],[58,5,59,5],[56,5,57,5],[54,3,55,3],[54,5,55,5],[91,11,92,11],[91,5,92,5],[91,1,92,1],[91,2,92,2],[91,3,92,3],[91,4,92,4],[73,6,74,7],[73,3,74,3],[51,4,52,4],[75,2,76,2],[70,6,70,7],[68,8,69,8],[65,1,66,2],[75,4,76,5],[73,4,74,5],[71,1,72,1],[71,2,72,2],[65,3,66,3],[60,1,61,1],[60,2,61,2],[64,1,64,2],[60,3,61,3],[71,3,72,3],[71,8,72,8],[0,0,0,18],[9,2,9,3],[9,5,9,6],[29,1,29,2],[28,1,28,2],[22,3,23,3],[24,3,25,3],[20,16,20,17],[21,16,21,17],[22,14,23,15],[10,2,10,3],[20,4,20,5],[22,4,23,5],[26,6,27,6],[20,14,20,15],[20,6,20,7],[24,12,25,12],[24,11,25,11],[24,8,25,9],[22,6,23,7],[22,11,23,11],[22,8,23,9],[21,6,21,7],[1,1,5,11],[39,3,40,3],[24,4,25,5],[47,6,48,6],[45,6,46,6],[45,2,46,2],[26,4,27,5],[45,3,46,3],[49,7,50,7],[45,7,46,7],[47,7,48,7],[39,1,40,2],[45,1,46,1],[43,6,43,7],[47,1,48,1],[47,2,48,2],[47,3,48,3],[49,5,50,5],[47,4,48,4],[42,6,42,7],[42,4,42,5],[49,6,50,6],[47,5,48,5],[45,4,46,4],[49,1,50,1],[99,17,99,18],[100,17,100,18],[101,17,101,18],[102,17,102,18],[98,17,98,18],[10,5,10,6],[21,4,21,5],[31,4,31,7],[24,6,25,7],[19,4,19,9],[96,17,96,18],[97,17,97,18],[51,7,52,7],[51,6,52,6],[49,4,50,4],[43,4,43,5],[45,5,46,5],[60,7,61,7],[54,6,55,6],[56,6,57,6],[68,6,69,7],[60,5,61,5],[60,4,61,4],[71,6,72,7],[107,17,107,18],[108,17,108,18],[109,17,109,18],[110,17,110,18],[103,17,103,18],[104,17,104,18],[105,17,105,18],[106,17,106,18],[115,17,115,18],[116,17,116,18],[117,17,117,18],[118,17,118,18],[111,17,111,18],[112,17,112,18],[113,17,113,18],[114,17,114,18],[123,17,123,18],[124,17,124,18],[125,17,125,18],[126,17,126,18],[119,17,119,18],[120,17,120,18],[121,17,121,18],[122,17,122,18],[131,17,131,18],[132,17,132,18],[133,17,133,18],[134,17,134,18],[127,17,127,18],[128,17,128,18],[129,17,129,18],[130,17,130,18],[139,17,139,18],[140,17,140,18],[141,17,141,18],[142,17,142,18],[135,17,135,18],[136,17,136,18],[137,17,137,18],[138,17,138,18],[147,17,147,18],[148,17,148,18],[149,17,149,18],[150,17,150,18],[143,17,143,18],[144,17,144,18],[145,17,145,18],[146,17,146,18],[155,17,155,18],[174,17,174,18],[167,17,167,18],[168,17,168,18],[169,17,169,18],[170,17,170,18],[156,17,156,18],[157,17,157,18],[158,17,158,18],[151,17,151,18],[152,17,152,18],[153,17,153,18],[154,17,154,18],[163,17,163,18],[164,17,164,18],[165,17,165,18],[166,17,166,18],[159,17,159,18],[160,17,160,18],[161,17,161,18],[162,17,162,18],[171,17,171,18],[172,17,172,18],[173,17,173,18],[185,17,185,18],[186,17,186,18],[190,17,190,18],[183,17,183,18],[184,17,184,18],[175,17,175,18],[176,17,176,18],[196,17,196,18],[191,17,191,18],[192,17,192,18],[193,17,193,18],[194,17,194,18],[195,17,195,18],[187,17,187,18],[188,17,188,18],[189,17,189,18],[181,17,181,18],[182,17,182,18],[177,17,177,18],[178,17,178,18],[179,17,179,18],[180,17,180,18]]}
[]
[]
[{"$f":"MID(MID(CELL(\"Dateiname\"),FIND(\"[\",CELL(\"Dateiname\"))+1,FIND(\"]\",CELL(\"Dateiname\"))-FIND(\"[\",CELL(\"Dateiname\"))-1),1,(LEN(MID(CELL(\"Dateiname\"),FIND(\"[\",CELL(\"Dateiname\"))+1,FIND(\"]\",CELL(\"Dateiname\"))-FIND(\"[\",CELL(\"Dateiname\"))-1)))-(IF((MID(RIGHT(MID(CELL(\"Dateiname\"),FIND(\"[\",CELL(\"Dateiname\"))+1,FIND(\"]\",CELL(\"Dateiname\"))-FIND(\"[\",CELL(\"Dateiname\"))-1),5),1,1))=\".\",5,4)))","v":"AnyDim_V2.38"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Änderungshistorie"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ver 1.7 nach 1.8           26.06.2004 Hinzufügen von ca. 300 Linearmotoren ver. Baureihen H. Goergen"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ver 2.0 nach 2.1    14.11.07  H Krug","Berechnung erweitert dass 10 Fremdlinearmotoren   berechnet werden können in Reiter \"LinMotor\".  "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Reiter \"LinMotor\": Bei den L1S  25..75  Polpitch auf 48mm gesetzt  bei L1S 80..200  Polpitch auf 66mm. Gesetzt"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Im Reiter \"Main\"  bei Linmot auswahl  in Spalte \"R\"  Fehler im Induktivitätsscheck   L>Lmax und Umot> Umot  auf  Wert \"5\" in Berechnungsvorschrift  geändert "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Alle Platinum IC Linearmotoren auf UDC max = 330Vdc geändert "]
[null,{"$f":"IF(deutsch,\"Allgemeines\",\"General\")","v":"Allgemeines"},null,null,null,null,null,null,null,null,null,null,null,null,"Sprache/Language"]
[null,{"$f":"IF(deutsch,\"Bearbeiter:\",\"Author:\")","v":"Bearbeiter:"},null,null,"                                                                                                                                                                                                                                                                                                                              ",{"$f":"IF(deutsch,\"Kunde:\",\"Customer:\")","v":"Kunde:"}]
[null,{"$f":"IF(deutsch,\"Datum:\",\"Date:\")","v":"Datum:"},null,null,null,{"$f":"IF(deutsch,\"Anwendung:\",\"Application:\")","v":"Anwendung:"}]
[]
[]
[null,{"$f":"IF(deutsch,\"Motorart\",\"Motor type\")","v":"Motorart"},{"$f":"D91","v":""},"                ","Drive",null,"Uac max =",{"$f":"Drives!B2","v":480},{"$f":"IF(Drives!G2=\"\",\"\",\"P br int =\")","v":"P br int ="},{"$f":"IF(Drives!G2=\"\",\"\",Drives!G2)","v":100},null,{"$f":"IF(deutsch,\"AC-Spg. [V]\",\"AC-Voltage [V]\")","v":"AC-Spg. [V]"},{"$f":"MIN(ROUND((UAC_V*SQRT(2)-5)/10,0)*10,640)","v":320},null,{"$f":"IF(deutsch,\"Eingabeänderung\",\"Input changes\")","v":"Eingabeänderung"}]
[null,null,null,null,null,null,"I cont =",{"$f":"Drives!C2","v":12},{"$f":"IF(Drives!E2=\"\",\"\",\"L min =\")","v":"L min ="},{"$f":"IF(Drives!E2=\"\",\"\",Drives!E2/H14*UAC_V)","v":1.2937500000000002}]
[null,null,null,null,null,null,"I peak =",{"$f":"Drives!D2","v":24},{"$f":"IF(Drives!F2=\"\",\"\",\"L max =\")","v":"L max ="},{"$f":"IF(Drives!F2=\"\",\"\",Drives!F2/H14*UAC_V)","v":14.375}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF((Calc!B2-Drives!B2)>0,\"       AC Spannung inkonsistent\",\"\")","v":""}]
[null,{"$f":"IF(deutsch,\"Motorlinien\",\"Motor lines\")","v":"Motorlinien"}]
[]
[null,null,null,null,{"$f":"IF(deutsch,\"Mechanische Daten (Abtrieb)\",\"Mech. data (gear output side)\")","v":"Mechanische Daten (Abtrieb)"},null,null,null,null,null,null,{"$f":"IF(deutsch,\"Getriebe\",\"Gear\")","v":"Getriebe"}]
[null,null,null,null,{"$f":"IF(deutsch,\"Massenträgheit\",\"Inertia\")","v":"Massenträgheit"},null,{"$f":"IF(deutsch,\"Lastmoment\",\"Load\")","v":"Lastmoment"},null,{"$f":"IF(deutsch,\"Tr.-Reibung\",\"Dry friction\")","v":"Tr.-Reibung"},null,null,{"$f":"IF(deutsch,\"Faktor\",\"Ratio\")","v":"Faktor"},{"$f":"IF(deutsch,\"Trägheit\",\"Inertia\")","v":"Trägheit"},{"$f":"IF(deutsch,\"Wirkungsgr.\",\"Efficiency\")","v":"Wirkungsgr."},{"$f":"IF(deutsch,\"Eingangsdrehzahl\",\"Input speed\")","v":"Eingangsdrehzahl"},null,{"$f":"IF(deutsch,\"Mittl. Drehz.\",\"Avg.-Speed\")","v":"Mittl. Drehz."}]
[null,null,null,null,"[kgcm2]",null,"[Nm]",null,"[Nm]",null,null,"i","[kgcm2]","h","[1/min]",null,"[1/min]"]
[null,null,null,{"$f":"IF(Calc!A31,\"\",\"1.\")","v":""},25,null,0,null,0,null,null,1,0,1,{"$f":"IF(move1,gear*MAX(ABS(speed1),ABS(speed2)),gear*MAX(ABS(speed1),ABS(speed2),ABS(speed6)))","v":2400},null,{"$f":"IF(move1,(((ABS(speed2+speed1)/2*time1+ABS(speed2)*time2+ABS(speed2+speed1)/2*time3+speed1*time4)/time))*gear,(((ABS(speed2+speed1)/2*time1+ABS(speed2)*time2+ABS(speed2+speed1)/2*time3+speed1*time4+ABS(speed6+speed1)/2*time5+ABS(speed6)*time6+ABS(speed6+speed1)/2*time7+speed1*time8)/time))*gear)","v":451.55925155925155}]
[]
[null,null,null,{"$f":"IF(Calc!A31,\"\",\"2.\")","v":""},25,null,0,null,0]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L23>0,\"\",IF(deutsch,\"Fehler: Getriebefaktor <= 0\",\"Error: Gear ratio <= 0\"))","v":""}]
[]
[]
[]
[]
[null,null,null,null,{"$f":"IF(deutsch,\"Mechanische Daten\",\"Mechanical data\")","v":"Mechanische Daten"}]
[null,null,null,null,{"$f":"IF(deutsch,\"Gewicht\",\"Weight\")","v":"Gewicht"},{"$f":"IF(deutsch,\"Last\",\"Load\")","v":"Last"},{"$f":"IF(deutsch,\"Tr.Reibung\",\"Dry Fric.\")","v":"Tr.Reibung"},{"$f":"IF(deutsch,\"Wirkungsgr\",\"Efficiency\")","v":"Wirkungsgr"}]
[null,null,null,null,"[kg]","[N]","[N]","h"]
[null,null,null,{"$f":"IF(Calc!A31,\"\",\"1.\")","v":""},5,0,0,1]
[null,null,null,{"$f":"IF(Calc!A31,\"\",\"2.\")","v":""},5,0,0]
[]
[]
[null,{"$f":"IF(deutsch,\"Bewegungsprofil\",\"Motion profile\")","v":"Bewegungsprofil"}]
[null,{"$f":"IF(deutsch,\"Einheiten / Umdrehung\",\"Units / turn\")","v":"Einheiten / Umdrehung"},null,1]
[]
[]
[null,null,null,{"$f":"IF(deutsch,\"Bewegungszeit\",\"Cylce time\")","v":"Bewegungszeit"},{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Speed\")","v":"Geschwindigkeit"},null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},null,"Position",null,null,null,null,null,null,null,"M0 [Nm]",{"$f":"Calc!A108","v":4.51}]
[null,null,null,"t [ms]",{"$f":"IF(deutsch,\"Abtrieb\",\"Gear output side\")","v":"Abtrieb"},null,{"$f":"IF(deutsch,\"Abtrieb\",\"Gear output side\")","v":"Abtrieb"},null,{"$f":"IF(deutsch,\"Abtrieb\",\"Gear outp.\")","v":"Abtrieb"},null,null,null,null,null,null,null,"I0 [A]",{"$f":"Calc!A109","v":4.6900000000000004}]
[null,null,null,{"$f":"IF(Calc!A31,time1+time2+time3+time4,time1+time2+time3+time4+time5+time6+time7+time8)","v":481},{"$f":"IF(deutsch,\"[Einheiten/s]\",\"[Units/s]\")","v":"[Einheiten/s]"},"[1/min]",{"$f":"IF(deutsch,\"[Einheiten/s2]\",\"[Units/s2]\")","v":"[Einheiten/s2]"},"[rad/s2]",{"$f":"IF(deutsch,\"[Einheiten]\",\"[Units]\")","v":"[Einheiten]"},null,null,null,null,null,null,null,"Mn [Nm]",{"$f":"Calc!A110","v":4.0107045659157627}]
[null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},"t1 [ ms ]",81,0,{"$f":"E46/$D$40*60","v":0},{"$f":"(E48-E46)/D46*Calc!B30*1000","v":775.7037037037037},{"$f":"G46/ULU*2*PI()","v":4873.8901138358979},{"$f":"E46*D46/1000+((E48+E46)/2-E46)*D46/1000","v":1.62},null,null,null,null,null,null,null,"In [A]",{"$f":"Calc!A111","v":4.1347469751708896}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nn [min-1]",{"$f":"Calc!A112","v":2500}]
[null,{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Speed\")","v":"Geschwindigkeit"},"t2 [ ms ]",0,40,{"$f":"E48/$D$40*60","v":2400},0,0,{"$f":"I46+E48*D48/1000","v":1.62},null,null,null,null,null,null,null,"Mmax[Nm]",{"$f":"Calc!A113","v":12.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nmax[min-1]",{"$f":"Calc!A114","v":2500}]
[null,{"$f":"IF(deutsch,\"Verzögerung\",\"Deceleration\")","v":"Verzögerung"},"t3 [ ms ]",100,{"$f":"E46","v":0},{"$f":"E50/$D$40*60","v":0},{"$f":"(E50-E48)/D50*Calc!B30*1000","v":-628.31999999999994},{"$f":"G50/ULU*2*PI()","v":-3947.8509922070771},{"$f":"I48+((E50+E48)/2-E48)*D50/1000+E48*D50/1000","v":3.62},null,null,null,null,null,null,null,"RU-V [W]",{"$f":"Calc!A115","v":2.87}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LU-V [mH]",{"$f":"Calc!A116","v":11.4}]
[null,"Pause","t4 [ ms ]",300,{"$f":"E46","v":0},{"$f":"E52/$D$40*60","v":0},0,0,{"$f":"I50+E52*D52/1000","v":3.62},null,null,null,null,null,null,null,"KE [V/103]",{"$f":"Calc!A117","v":58.7}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Calc!A71,\"J [kgcm2]\",\"J[10-3kgm2\")","v":"J [kgcm2]"},{"$f":"IF(Calc!A71,10*Calc!A107,Calc!A107)","v":5.8600000000000012}]
[null,{"$f":"IF(deutsch,IF(move1,\"\",\"2. Fahrsatz\"),IF(move1,\"\",\"2. Motion task\"))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UDCmax [V]",{"$f":"Calc!A118","v":325}]
[null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},"t5 [ ms ]",1,{"$f":"E46","v":0},{"$f":"E55/$D$40*60","v":0},{"$f":"(E57-E55)/D55*AccType*1000","v":0},{"$f":"G55/ULU*2*PI()","v":0},{"$f":"I52+E55*D55/1000+((E57+E55)/2-E55)*D55/1000","v":3.62}]
[]
[null,{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Speed\")","v":"Geschwindigkeit"},"t6 [ ms ]",0,0,{"$f":"E57/$D$40*60","v":0},0,0,{"$f":"I55+E57*D57/1000","v":3.62}]
[]
[null,{"$f":"IF(deutsch,\"Verzögerung\",\"Deceleration\")","v":"Verzögerung"},"t7 [ ms ]",1,{"$f":"E55","v":0},{"$f":"E59/$D$40*60","v":0},{"$f":"(E59-E57)/D59*AccType*1000","v":0},{"$f":"G59/ULU*2*PI()","v":0},{"$f":"I57+((E59+E57)/2-E57)*D59/1000+E57*D59/1000","v":3.62}]
[]
[null,"Pause","t8 [ ms ]",0,{"$f":"E55","v":0},{"$f":"E61/$D$40*60","v":0},0,0,{"$f":"I59+E61*D61/1000","v":3.62}]
[]
[]
[]
[null,{"$f":"IF(deutsch,\"Bewegungsprofil\",\"Motion profile\")","v":"Bewegungsprofil"}]
[]
[]
[]
[null,null,null,{"$f":"IF(deutsch,\"Bewegungszeit\",\"Cycle time\")","v":"Bewegungszeit"},{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Speed\")","v":"Geschwindigkeit"},null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},null,"Position"]
[null,null,null,"t [ms]"]
[null,{"$f":"IF(deutsch,IF(move1,\"\",\"1. Fahrsatz\"),IF(move1,\"\",\"1. Motion task\"))","v":""},null,{"$f":"IF(Calc!A31,Ltime1+Ltime2+Ltime3+Ltime4,Ltime1+Ltime2+Ltime3+Ltime4+Ltime5+Ltime6+Ltime7+Ltime8)","v":130},"[m/s]",null,"[m/s2]",null,"[mm]",null,null,null,null,null,null,null,"Fn [N]",{"$f":"Calc!A108","v":4.51}]
[null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},"t1 [ ms ]",50,0,null,{"$f":"(E74-E72)/D72*AccType*1000","v":31.416},null,{"$f":"E72*D72+((E74+E72)/2-E72)*D72","v":25},null,null,null,null,null,null,null,"In [A]",{"$f":"Calc!A109","v":4.6900000000000004}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fmax [N]",{"$f":"Calc!A110","v":4.0107045659157627}]
[null,{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Const. speed\")","v":"Geschwindigkeit"},"t2 [ ms ]",0,1,null,0,null,{"$f":"I72+E74*D74","v":25},null,null,null,null,null,null,null,"Imax [A]",{"$f":"Calc!A111","v":4.1347469751708896}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"vmax [m/s]",{"$f":"Calc!A112","v":2500}]
[null,{"$f":"IF(deutsch,\"Verzögerung\",\"Deceleration\")","v":"Verzögerung"},"t3 [ ms ]",30,{"$f":"Lspeed1","v":0},null,{"$f":"(E76-E74)/D76*AccType*1000","v":-52.36},null,{"$f":"I74+((E76+E74)/2-E74)*D76+E74*D76","v":40},null,null,null,null,null,null,null,"RU-V [W]",{"$f":"Calc!A113","v":12.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LU-V [mH]",{"$f":"Calc!A114","v":2500}]
[null,"Pause","t4 [ ms ]",50,{"$f":"Lspeed1","v":0},null,0,null,{"$f":"I76+E78*D78","v":40},null,null,null,null,null,null,null,"KE [V/m/s]",{"$f":"Calc!A115","v":2.87}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G [kg]",{"$f":"Calc!A107","v":0.58600000000000008}]
[null,{"$f":"IF(deutsch,IF(move1,\"\",\"2. Fahrsatz\"),IF(move1,\"\",\"2. Motion task\"))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UDCmax [V]",{"$f":"Calc!A117","v":58.7}]
[null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},"t5 [ ms ]",1,{"$f":"Lspeed1","v":0},null,{"$f":"(E83-E81)/D81*AccType*1000","v":0},null,{"$f":"I78+E81*D81+((E83+E81)/2-E81)*D81","v":40}]
[]
[null,{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Speed\")","v":"Geschwindigkeit"},"t6 [ ms ]",0,0,null,0,null,{"$f":"I81+E83*D83","v":40}]
[]
[null,{"$f":"IF(deutsch,\"Verzögerung\",\"Deceleration\")","v":"Verzögerung"},"t7 [ ms ]",1,{"$f":"Lspeed1","v":0},null,{"$f":"(E85-E83)/D85*AccType*1000","v":0},null,{"$f":"I83+((E85+E83)/2-E83)*D85+E83*D85","v":40}]
[]
[null,"Pause","t8 [ ms ]",0,{"$f":"Lspeed1","v":0},null,0,null,{"$f":"I85+E87*D87","v":40}]
[]
[]
[]
[{"$f":"IF(deutsch,\"Motorkennlinie\",\"Motor curves\")","v":"Motorkennlinie"},null,null,{"$f":"IF(Calc!A140=0,\"\",Calc!A140)","v":""},{"$f":"IF(Calc!B140=0,\"\",Calc!B140)","v":""},{"$f":"IF(deutsch,\"Motordaten\",\"Motor data\")","v":"Motordaten"},null,null,null,null,{"$f":"IF(deutsch,\"Reglerdaten\",\"Drive data\")","v":"Reglerdaten"}]
[null,{"$f":"IF(deutsch,\"Typ\",\"Type\")","v":"Typ"},"Jext/Jmot","Trms","Tpk","n","T (t1)","T (t2)","T (t3)","T (t4)","Irms","Ipeak","Irms","Ipeak","P","PbrRMS","PbrPEAK"]
[null,null,null,null,null,null,"[Nm]","[Nm]","[Nm]","[Nm]",null,null,"[A]","[A]","[W]","[W]","[W]"]
["t","Filter\n (Maximum)",{"$f":"IF(jjbar<500,jjbar,IF(deutsch,\"alle\",\"all\"))","v":15},{"$f":"IF(mrmsbar<20,mrmsbar/10,IF(deutsch,\"alle\",\"all\"))","v":1.2},{"$f":"IF(mpkbar<20,mpkbar/10,IF(deutsch,\"alle\",\"all\"))","v":1.3},{"$f":"IF(nbar<20,nbar/10,IF(deutsch,\"alle\",\"all\"))","v":1.2},null,null,null,null,{"$f":"IF(irmsbar<20,irmsbar/10,IF(deutsch,\"alle\",\"all\"))","v":"alle"},{"$f":"IF(ipkbar<20,ipkbar/10,IF(deutsch,\"alle\",\"all\"))","v":"alle"}]
[]
[null,{"$f":"Calc!A70","v":"C041B (240 V)"}]
[305,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A97,1),INDEX(LinMotor!$B$1:$B$1291,A97,1))","v":"C041B (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A97,1),INDEX(LinMotor!$R$1:$R$1305,A97,1))","v":4.2662116040955622},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A97,1),INDEX(LinMotor!$S$1:$S$1305,A97,1))","v":1.1960708467031758},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A97,1),INDEX(LinMotor!$T$1:$T$1305,A97,1))","v":1.2328544992866872},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A97,1),INDEX(LinMotor!$U$1:$U$1305,A97,1))","v":0.96},{"$f":"IF(A97<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A97,1),INDEX(LinMotor!$V$1:$V$1305,A97,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A97,1),INDEX(LinMotor!$V$1:$V$1305,A97,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A97,1),INDEX(LinMotor!$V$1:$V$1305,A97,1))/1000,\"0.0k\")),\"\")","v":15.040824891297582},{"$f":"IF(A97<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A97,1),INDEX(LinMotor!$W$1:$W$1305,A97,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A97,1),INDEX(LinMotor!$X$1:$X$1305,A97,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A97,1),INDEX(LinMotor!$W$1:$W$1305,A97,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A97,1),INDEX(LinMotor!$X$1:$X$1305,A97,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A97,1),INDEX(LinMotor!$W$1:$W$1305,A97,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A97,1),INDEX(LinMotor!$X$1:$X$1305,A97,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A97<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A97,1),INDEX(LinMotor!$X$1:$X$1305,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A97,1),INDEX(LinMotor!$Z$1:$Z$1305,A97,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A97,1),INDEX(LinMotor!$X$1:$X$1305,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A97,1),INDEX(LinMotor!$Z$1:$Z$1305,A97,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A97,1),INDEX(LinMotor!$X$1:$X$1305,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A97,1),INDEX(LinMotor!$Z$1:$Z$1305,A97,1)))/1000,\"0.0k\")),\"\")","v":-12.183068161951041},{"$f":"IF(A97<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A97,1),INDEX(LinMotor!$Y$1:$Y$1305,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A97,1),INDEX(LinMotor!$AB$1:$AB$1305,A97,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A97,1),INDEX(LinMotor!$Y$1:$Y$1305,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A97,1),INDEX(LinMotor!$AB$1:$AB$1305,A97,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A97,1),INDEX(LinMotor!$Y$1:$Y$1305,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A97,1),INDEX(LinMotor!$AB$1:$AB$1305,A97,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A97,1),INDEX(LinMotor!$AD$1:$AD$1305,A97,1))","v":0.45811666616042362},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A97,1),INDEX(LinMotor!$AE$1:$AE$1305,A97,1))","v":0.65171349538235102},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A97,1),INDEX(LinMotor!$AF$1:$AF$1305,A97,1))","v":5.4973999939250833},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A97,1),INDEX(LinMotor!$AG$1:$AG$1305,A97,1))","v":15.641123889176423},{"$f":"IF(A97<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A97,1),INDEX(LinMotor!$AI$1:$AI$1305,A97,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A97,1),INDEX(LinMotor!$AI$1:$AI$1305,A97,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A97,1),INDEX(LinMotor!$AI$1:$AI$1305,A97,1))/1000,\"0.0k\")),\"\")","v":249.96108996018449},{"$f":"IF(A97<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A97,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A97,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A97,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A97,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A97,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A97,1))/1000,\"0.0k\")),\"\")","v":202.62899229856203},{"$f":"IF(A97<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A97,1),INDEX(LinMotor!$AK$1:$AK$1305,A97,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A97,1),INDEX(LinMotor!$AK$1:$AK$1305,A97,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A97,1),INDEX(LinMotor!$AK$1:$AK$1305,A97,1))/1000,\"0.0k\")),\"\")","v":"1.9k"},{"$f":"IF(T97=1,\"L<Lmin\",IF(T97=2,\"Udc>Umot\",IF(T97=3,\"L<Lmin & Udc>Umot\",IF(T97=4,\"L>Lmax\",IF(T97=5,\"L>Lmax & Udc>Umot\",\"\")))))","v":""}]
[307,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A98,1),INDEX(LinMotor!$B$1:$B$1291,A98,1))","v":"C042B (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A98,1),INDEX(LinMotor!$R$1:$R$1305,A98,1))","v":2.818489289740699},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A98,1),INDEX(LinMotor!$S$1:$S$1305,A98,1))","v":0.70383284393941781},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A98,1),INDEX(LinMotor!$T$1:$T$1305,A98,1))","v":0.72402920243693791},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A98,1),INDEX(LinMotor!$U$1:$U$1305,A98,1))","v":0.96},{"$f":"IF(A98<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A98,1),INDEX(LinMotor!$V$1:$V$1305,A98,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A98,1),INDEX(LinMotor!$V$1:$V$1305,A98,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A98,1),INDEX(LinMotor!$V$1:$V$1305,A98,1))/1000,\"0.0k\")),\"\")","v":16.507865815562184},{"$f":"IF(A98<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A98,1),INDEX(LinMotor!$W$1:$W$1305,A98,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A98,1),INDEX(LinMotor!$X$1:$X$1305,A98,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A98,1),INDEX(LinMotor!$W$1:$W$1305,A98,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A98,1),INDEX(LinMotor!$X$1:$X$1305,A98,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A98,1),INDEX(LinMotor!$W$1:$W$1305,A98,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A98,1),INDEX(LinMotor!$X$1:$X$1305,A98,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A98<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A98,1),INDEX(LinMotor!$X$1:$X$1305,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A98,1),INDEX(LinMotor!$Z$1:$Z$1305,A98,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A98,1),INDEX(LinMotor!$X$1:$X$1305,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A98,1),INDEX(LinMotor!$Z$1:$Z$1305,A98,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A98,1),INDEX(LinMotor!$X$1:$X$1305,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A98,1),INDEX(LinMotor!$Z$1:$Z$1305,A98,1)))/1000,\"0.0k\")),\"\")","v":-13.371371310605369},{"$f":"IF(A98<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A98,1),INDEX(LinMotor!$Y$1:$Y$1305,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A98,1),INDEX(LinMotor!$AB$1:$AB$1305,A98,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A98,1),INDEX(LinMotor!$Y$1:$Y$1305,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A98,1),INDEX(LinMotor!$AB$1:$AB$1305,A98,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A98,1),INDEX(LinMotor!$Y$1:$Y$1305,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A98,1),INDEX(LinMotor!$AB$1:$AB$1305,A98,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A98,1),INDEX(LinMotor!$AD$1:$AD$1305,A98,1))","v":0.52522357809959808},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A98,1),INDEX(LinMotor!$AE$1:$AE$1305,A98,1))","v":0.7471793087323505},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A98,1),INDEX(LinMotor!$AF$1:$AF$1305,A98,1))","v":6.3026829371951765},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A98,1),INDEX(LinMotor!$AG$1:$AG$1305,A98,1))","v":17.932303409576413},{"$f":"IF(A98<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A98,1),INDEX(LinMotor!$AI$1:$AI$1305,A98,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A98,1),INDEX(LinMotor!$AI$1:$AI$1305,A98,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A98,1),INDEX(LinMotor!$AI$1:$AI$1305,A98,1))/1000,\"0.0k\")),\"\")","v":274.34161104832947},{"$f":"IF(A98<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A98,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A98,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A98,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A98,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A98,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A98,1))/1000,\"0.0k\")),\"\")","v":222.39287003085852},{"$f":"IF(A98<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A98,1),INDEX(LinMotor!$AK$1:$AK$1305,A98,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A98,1),INDEX(LinMotor!$AK$1:$AK$1305,A98,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A98,1),INDEX(LinMotor!$AK$1:$AK$1305,A98,1))/1000,\"0.0k\")),\"\")","v":"2.1k"},{"$f":"IF(T98=1,\"L<Lmin\",IF(T98=2,\"Udc>Umot\",IF(T98=3,\"L<Lmin & Udc>Umot\",IF(T98=4,\"L>Lmax\",IF(T98=5,\"L>Lmax & Udc>Umot\",\"\")))))","v":""}]
[309,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A99,1),INDEX(LinMotor!$B$1:$B$1291,A99,1))","v":"C043B (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A99,1),INDEX(LinMotor!$R$1:$R$1305,A99,1))","v":2.1008403361344539},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A99,1),INDEX(LinMotor!$S$1:$S$1305,A99,1))","v":0.58291656188662189},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A99,1),INDEX(LinMotor!$T$1:$T$1305,A99,1))","v":0.59551836159120741},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A99,1),INDEX(LinMotor!$U$1:$U$1305,A99,1))","v":0.96},{"$f":"IF(A99<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A99,1),INDEX(LinMotor!$V$1:$V$1305,A99,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A99,1),INDEX(LinMotor!$V$1:$V$1305,A99,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A99,1),INDEX(LinMotor!$V$1:$V$1305,A99,1))/1000,\"0.0k\")),\"\")","v":17.984654520054463},{"$f":"IF(A99<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A99,1),INDEX(LinMotor!$W$1:$W$1305,A99,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A99,1),INDEX(LinMotor!$X$1:$X$1305,A99,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A99,1),INDEX(LinMotor!$W$1:$W$1305,A99,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A99,1),INDEX(LinMotor!$X$1:$X$1305,A99,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A99,1),INDEX(LinMotor!$W$1:$W$1305,A99,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A99,1),INDEX(LinMotor!$X$1:$X$1305,A99,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A99<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A99,1),INDEX(LinMotor!$X$1:$X$1305,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A99,1),INDEX(LinMotor!$Z$1:$Z$1305,A99,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A99,1),INDEX(LinMotor!$X$1:$X$1305,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A99,1),INDEX(LinMotor!$Z$1:$Z$1305,A99,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A99,1),INDEX(LinMotor!$X$1:$X$1305,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A99,1),INDEX(LinMotor!$Z$1:$Z$1305,A99,1)))/1000,\"0.0k\")),\"\")","v":-14.567570161244113},{"$f":"IF(A99<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A99,1),INDEX(LinMotor!$Y$1:$Y$1305,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A99,1),INDEX(LinMotor!$AB$1:$AB$1305,A99,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A99,1),INDEX(LinMotor!$Y$1:$Y$1305,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A99,1),INDEX(LinMotor!$AB$1:$AB$1305,A99,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A99,1),INDEX(LinMotor!$Y$1:$Y$1305,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A99,1),INDEX(LinMotor!$AB$1:$AB$1305,A99,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A99,1),INDEX(LinMotor!$AD$1:$AD$1305,A99,1))","v":0.43034157655905519},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A99,1),INDEX(LinMotor!$AE$1:$AE$1305,A99,1))","v":0.61220085140810399},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A99,1),INDEX(LinMotor!$AF$1:$AF$1305,A99,1))","v":5.1640989187086621},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A99,1),INDEX(LinMotor!$AG$1:$AG$1305,A99,1))","v":14.692820433794497},{"$f":"IF(A99<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A99,1),INDEX(LinMotor!$AI$1:$AI$1305,A99,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A99,1),INDEX(LinMotor!$AI$1:$AI$1305,A99,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A99,1),INDEX(LinMotor!$AI$1:$AI$1305,A99,1))/1000,\"0.0k\")),\"\")","v":298.88412895433595},{"$f":"IF(A99<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A99,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A99,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A99,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A99,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A99,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A99,1))/1000,\"0.0k\")),\"\")","v":242.28806920988129},{"$f":"IF(A99<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A99,1),INDEX(LinMotor!$AK$1:$AK$1305,A99,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A99,1),INDEX(LinMotor!$AK$1:$AK$1305,A99,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A99,1),INDEX(LinMotor!$AK$1:$AK$1305,A99,1))/1000,\"0.0k\")),\"\")","v":"2.3k"},""]
[311,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A100,1),INDEX(LinMotor!$B$1:$B$1291,A100,1))","v":"C044B (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A100,1),INDEX(LinMotor!$R$1:$R$1305,A100,1))","v":1.6778523489932886},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A100,1),INDEX(LinMotor!$S$1:$S$1305,A100,1))","v":0.49126870722333421},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A100,1),INDEX(LinMotor!$T$1:$T$1305,A100,1))","v":0.50120674108776386},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A100,1),INDEX(LinMotor!$U$1:$U$1305,A100,1))","v":1.1428571428571428},{"$f":"IF(A100<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A100,1),INDEX(LinMotor!$V$1:$V$1305,A100,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A100,1),INDEX(LinMotor!$V$1:$V$1305,A100,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A100,1),INDEX(LinMotor!$V$1:$V$1305,A100,1))/1000,\"0.0k\")),\"\")","v":19.446821554205236},{"$f":"IF(A100<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A100,1),INDEX(LinMotor!$W$1:$W$1305,A100,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A100,1),INDEX(LinMotor!$X$1:$X$1305,A100,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A100,1),INDEX(LinMotor!$W$1:$W$1305,A100,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A100,1),INDEX(LinMotor!$X$1:$X$1305,A100,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A100,1),INDEX(LinMotor!$W$1:$W$1305,A100,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A100,1),INDEX(LinMotor!$X$1:$X$1305,A100,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A100<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A100,1),INDEX(LinMotor!$X$1:$X$1305,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A100,1),INDEX(LinMotor!$Z$1:$Z$1305,A100,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A100,1),INDEX(LinMotor!$X$1:$X$1305,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A100,1),INDEX(LinMotor!$Z$1:$Z$1305,A100,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A100,1),INDEX(LinMotor!$X$1:$X$1305,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A100,1),INDEX(LinMotor!$Z$1:$Z$1305,A100,1)))/1000,\"0.0k\")),\"\")","v":-15.751925458906239},{"$f":"IF(A100<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A100,1),INDEX(LinMotor!$Y$1:$Y$1305,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A100,1),INDEX(LinMotor!$AB$1:$AB$1305,A100,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A100,1),INDEX(LinMotor!$Y$1:$Y$1305,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A100,1),INDEX(LinMotor!$AB$1:$AB$1305,A100,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A100,1),INDEX(LinMotor!$Y$1:$Y$1305,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A100,1),INDEX(LinMotor!$AB$1:$AB$1305,A100,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A100,1),INDEX(LinMotor!$AD$1:$AD$1305,A100,1))","v":0.37695297329066974},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A100,1),INDEX(LinMotor!$AE$1:$AE$1305,A100,1))","v":0.53625060593627283},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A100,1),INDEX(LinMotor!$AF$1:$AF$1305,A100,1))","v":4.5234356794880366},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A100,1),INDEX(LinMotor!$AG$1:$AG$1305,A100,1))","v":12.870014542470548},{"$f":"IF(A100<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A100,1),INDEX(LinMotor!$AI$1:$AI$1305,A100,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A100,1),INDEX(LinMotor!$AI$1:$AI$1305,A100,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A100,1),INDEX(LinMotor!$AI$1:$AI$1305,A100,1))/1000,\"0.0k\")),\"\")","v":323.18365163355026},{"$f":"IF(A100<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A100,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A100,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A100,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A100,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A100,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A100,1))/1000,\"0.0k\")),\"\")","v":261.98628621881483},{"$f":"IF(A100<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A100,1),INDEX(LinMotor!$AK$1:$AK$1305,A100,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A100,1),INDEX(LinMotor!$AK$1:$AK$1305,A100,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A100,1),INDEX(LinMotor!$AK$1:$AK$1305,A100,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[313,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A101,1),INDEX(LinMotor!$B$1:$B$1291,A101,1))","v":"C051B (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A101,1),INDEX(LinMotor!$R$1:$R$1305,A101,1))","v":0.91240875912408748},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A101,1),INDEX(LinMotor!$S$1:$S$1305,A101,1))","v":0.78068468335973451},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A101,1),INDEX(LinMotor!$T$1:$T$1305,A101,1))","v":0.83735030152459378},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A101,1),INDEX(LinMotor!$U$1:$U$1305,A101,1))","v":0.97959183673469385},{"$f":"IF(A101<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A101,1),INDEX(LinMotor!$V$1:$V$1305,A101,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A101,1),INDEX(LinMotor!$V$1:$V$1305,A101,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A101,1),INDEX(LinMotor!$V$1:$V$1305,A101,1))/1000,\"0.0k\")),\"\")","v":25.539184196500109},{"$f":"IF(A101<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A101,1),INDEX(LinMotor!$W$1:$W$1305,A101,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A101,1),INDEX(LinMotor!$X$1:$X$1305,A101,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A101,1),INDEX(LinMotor!$W$1:$W$1305,A101,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A101,1),INDEX(LinMotor!$X$1:$X$1305,A101,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A101,1),INDEX(LinMotor!$W$1:$W$1305,A101,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A101,1),INDEX(LinMotor!$X$1:$X$1305,A101,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A101<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A101,1),INDEX(LinMotor!$X$1:$X$1305,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A101,1),INDEX(LinMotor!$Z$1:$Z$1305,A101,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A101,1),INDEX(LinMotor!$X$1:$X$1305,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A101,1),INDEX(LinMotor!$Z$1:$Z$1305,A101,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A101,1),INDEX(LinMotor!$X$1:$X$1305,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A101,1),INDEX(LinMotor!$Z$1:$Z$1305,A101,1)))/1000,\"0.0k\")),\"\")","v":-20.686739199165086},{"$f":"IF(A101<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A101,1),INDEX(LinMotor!$Y$1:$Y$1305,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A101,1),INDEX(LinMotor!$AB$1:$AB$1305,A101,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A101,1),INDEX(LinMotor!$Y$1:$Y$1305,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A101,1),INDEX(LinMotor!$AB$1:$AB$1305,A101,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A101,1),INDEX(LinMotor!$Y$1:$Y$1305,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A101,1),INDEX(LinMotor!$AB$1:$AB$1305,A101,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A101,1),INDEX(LinMotor!$AD$1:$AD$1305,A101,1))","v":0.58890991017267624},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A101,1),INDEX(LinMotor!$AE$1:$AE$1305,A101,1))","v":0.83777902960976691},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A101,1),INDEX(LinMotor!$AF$1:$AF$1305,A101,1))","v":7.0669189220721149},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A101,1),INDEX(LinMotor!$AG$1:$AG$1305,A101,1))","v":20.106696710634406},{"$f":"IF(A101<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A101,1),INDEX(LinMotor!$AI$1:$AI$1305,A101,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A101,1),INDEX(LinMotor!$AI$1:$AI$1305,A101,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A101,1),INDEX(LinMotor!$AI$1:$AI$1305,A101,1))/1000,\"0.0k\")),\"\")","v":424.43166279694327},{"$f":"IF(A101<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A101,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A101,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A101,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A101,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A101,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A101,1))/1000,\"0.0k\")),\"\")","v":344.06219042270408},{"$f":"IF(A101<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A101,1),INDEX(LinMotor!$AK$1:$AK$1305,A101,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A101,1),INDEX(LinMotor!$AK$1:$AK$1305,A101,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A101,1),INDEX(LinMotor!$AK$1:$AK$1305,A101,1))/1000,\"0.0k\")),\"\")","v":"3.3k"},""]
[315,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A102,1),INDEX(LinMotor!$B$1:$B$1291,A102,1))","v":"C052B (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A102,1),INDEX(LinMotor!$R$1:$R$1305,A102,1))","v":0.69637883008356549},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A102,1),INDEX(LinMotor!$S$1:$S$1305,A102,1))","v":0.65137569629520042},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A102,1),INDEX(LinMotor!$T$1:$T$1305,A102,1))","v":0.70004695267124095},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A102,1),INDEX(LinMotor!$U$1:$U$1305,A102,1))","v":0.96},{"$f":"IF(A102<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A102,1),INDEX(LinMotor!$V$1:$V$1305,A102,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A102,1),INDEX(LinMotor!$V$1:$V$1305,A102,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A102,1),INDEX(LinMotor!$V$1:$V$1305,A102,1))/1000,\"0.0k\")),\"\")","v":29.681990793260617},{"$f":"IF(A102<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A102,1),INDEX(LinMotor!$W$1:$W$1305,A102,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A102,1),INDEX(LinMotor!$X$1:$X$1305,A102,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A102,1),INDEX(LinMotor!$W$1:$W$1305,A102,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A102,1),INDEX(LinMotor!$X$1:$X$1305,A102,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A102,1),INDEX(LinMotor!$W$1:$W$1305,A102,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A102,1),INDEX(LinMotor!$X$1:$X$1305,A102,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A102<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A102,1),INDEX(LinMotor!$X$1:$X$1305,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A102,1),INDEX(LinMotor!$Z$1:$Z$1305,A102,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A102,1),INDEX(LinMotor!$X$1:$X$1305,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A102,1),INDEX(LinMotor!$Z$1:$Z$1305,A102,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A102,1),INDEX(LinMotor!$X$1:$X$1305,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A102,1),INDEX(LinMotor!$Z$1:$Z$1305,A102,1)))/1000,\"0.0k\")),\"\")","v":-24.042412542541101},{"$f":"IF(A102<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A102,1),INDEX(LinMotor!$Y$1:$Y$1305,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A102,1),INDEX(LinMotor!$AB$1:$AB$1305,A102,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A102,1),INDEX(LinMotor!$Y$1:$Y$1305,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A102,1),INDEX(LinMotor!$AB$1:$AB$1305,A102,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A102,1),INDEX(LinMotor!$Y$1:$Y$1305,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A102,1),INDEX(LinMotor!$AB$1:$AB$1305,A102,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A102,1),INDEX(LinMotor!$AD$1:$AD$1305,A102,1))","v":0.7112970146230001},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A102,1),INDEX(LinMotor!$AE$1:$AE$1305,A102,1))","v":1.0118860497702482},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A102,1),INDEX(LinMotor!$AF$1:$AF$1305,A102,1))","v":8.5355641754760008},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A102,1),INDEX(LinMotor!$AG$1:$AG$1305,A102,1))","v":24.285265194485959},{"$f":"IF(A102<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A102,1),INDEX(LinMotor!$AI$1:$AI$1305,A102,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A102,1),INDEX(LinMotor!$AI$1:$AI$1305,A102,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A102,1),INDEX(LinMotor!$AI$1:$AI$1305,A102,1))/1000,\"0.0k\")),\"\")","v":493.28031038805045},{"$f":"IF(A102<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A102,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A102,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A102,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A102,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A102,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A102,1))/1000,\"0.0k\")),\"\")","v":399.87380528134889},{"$f":"IF(A102<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A102,1),INDEX(LinMotor!$AK$1:$AK$1305,A102,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A102,1),INDEX(LinMotor!$AK$1:$AK$1305,A102,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A102,1),INDEX(LinMotor!$AK$1:$AK$1305,A102,1))/1000,\"0.0k\")),\"\")","v":"3.8k"},""]
[317,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A103,1),INDEX(LinMotor!$B$1:$B$1291,A103,1))","v":"C052D (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A103,1),INDEX(LinMotor!$R$1:$R$1305,A103,1))","v":0.69637883008356549},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A103,1),INDEX(LinMotor!$S$1:$S$1305,A103,1))","v":0.65222517067269048},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A103,1),INDEX(LinMotor!$T$1:$T$1305,A103,1))","v":0.70170191000616122},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A103,1),INDEX(LinMotor!$U$1:$U$1305,A103,1))","v":1.1707317073170731},{"$f":"IF(A103<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A103,1),INDEX(LinMotor!$V$1:$V$1305,A103,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A103,1),INDEX(LinMotor!$V$1:$V$1305,A103,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A103,1),INDEX(LinMotor!$V$1:$V$1305,A103,1))/1000,\"0.0k\")),\"\")","v":29.681990793260617},{"$f":"IF(A103<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A103,1),INDEX(LinMotor!$W$1:$W$1305,A103,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A103,1),INDEX(LinMotor!$X$1:$X$1305,A103,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A103,1),INDEX(LinMotor!$W$1:$W$1305,A103,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A103,1),INDEX(LinMotor!$X$1:$X$1305,A103,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A103,1),INDEX(LinMotor!$W$1:$W$1305,A103,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A103,1),INDEX(LinMotor!$X$1:$X$1305,A103,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A103<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A103,1),INDEX(LinMotor!$X$1:$X$1305,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A103,1),INDEX(LinMotor!$Z$1:$Z$1305,A103,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A103,1),INDEX(LinMotor!$X$1:$X$1305,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A103,1),INDEX(LinMotor!$Z$1:$Z$1305,A103,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A103,1),INDEX(LinMotor!$X$1:$X$1305,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A103,1),INDEX(LinMotor!$Z$1:$Z$1305,A103,1)))/1000,\"0.0k\")),\"\")","v":-24.042412542541101},{"$f":"IF(A103<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A103,1),INDEX(LinMotor!$Y$1:$Y$1305,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A103,1),INDEX(LinMotor!$AB$1:$AB$1305,A103,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A103,1),INDEX(LinMotor!$Y$1:$Y$1305,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A103,1),INDEX(LinMotor!$AB$1:$AB$1305,A103,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A103,1),INDEX(LinMotor!$Y$1:$Y$1305,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A103,1),INDEX(LinMotor!$AB$1:$AB$1305,A103,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A103,1),INDEX(LinMotor!$AD$1:$AD$1305,A103,1))","v":0.57430647847338534},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A103,1),INDEX(LinMotor!$AE$1:$AE$1305,A103,1))","v":0.81700429203671898},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A103,1),INDEX(LinMotor!$AF$1:$AF$1305,A103,1))","v":6.8916777416806241},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A103,1),INDEX(LinMotor!$AG$1:$AG$1305,A103,1))","v":19.608103008881255},{"$f":"IF(A103<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A103,1),INDEX(LinMotor!$AI$1:$AI$1305,A103,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A103,1),INDEX(LinMotor!$AI$1:$AI$1305,A103,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A103,1),INDEX(LinMotor!$AI$1:$AI$1305,A103,1))/1000,\"0.0k\")),\"\")","v":493.28031038805045},{"$f":"IF(A103<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A103,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A103,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A103,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A103,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A103,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A103,1))/1000,\"0.0k\")),\"\")","v":399.87380528134889},{"$f":"IF(A103<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A103,1),INDEX(LinMotor!$AK$1:$AK$1305,A103,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A103,1),INDEX(LinMotor!$AK$1:$AK$1305,A103,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A103,1),INDEX(LinMotor!$AK$1:$AK$1305,A103,1))/1000,\"0.0k\")),\"\")","v":"3.8k"},""]
[319,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A104,1),INDEX(LinMotor!$B$1:$B$1291,A104,1))","v":"C053B (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A104,1),INDEX(LinMotor!$R$1:$R$1305,A104,1))","v":0.56433408577878108},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A104,1),INDEX(LinMotor!$S$1:$S$1305,A104,1))","v":0.6151020392019857},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A104,1),INDEX(LinMotor!$T$1:$T$1305,A104,1))","v":0.65712176048410065},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A104,1),INDEX(LinMotor!$U$1:$U$1305,A104,1))","v":0.96},{"$f":"IF(A104<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A104,1),INDEX(LinMotor!$V$1:$V$1305,A104,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A104,1),INDEX(LinMotor!$V$1:$V$1305,A104,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A104,1),INDEX(LinMotor!$V$1:$V$1305,A104,1))/1000,\"0.0k\")),\"\")","v":33.776058488882775},{"$f":"IF(A104<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A104,1),INDEX(LinMotor!$W$1:$W$1305,A104,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A104,1),INDEX(LinMotor!$X$1:$X$1305,A104,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A104,1),INDEX(LinMotor!$W$1:$W$1305,A104,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A104,1),INDEX(LinMotor!$X$1:$X$1305,A104,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A104,1),INDEX(LinMotor!$W$1:$W$1305,A104,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A104,1),INDEX(LinMotor!$X$1:$X$1305,A104,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A104<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A104,1),INDEX(LinMotor!$X$1:$X$1305,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A104,1),INDEX(LinMotor!$Z$1:$Z$1305,A104,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A104,1),INDEX(LinMotor!$X$1:$X$1305,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A104,1),INDEX(LinMotor!$Z$1:$Z$1305,A104,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A104,1),INDEX(LinMotor!$X$1:$X$1305,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A104,1),INDEX(LinMotor!$Z$1:$Z$1305,A104,1)))/1000,\"0.0k\")),\"\")","v":-27.358607375995042},{"$f":"IF(A104<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A104,1),INDEX(LinMotor!$Y$1:$Y$1305,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A104,1),INDEX(LinMotor!$AB$1:$AB$1305,A104,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A104,1),INDEX(LinMotor!$Y$1:$Y$1305,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A104,1),INDEX(LinMotor!$AB$1:$AB$1305,A104,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A104,1),INDEX(LinMotor!$Y$1:$Y$1305,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A104,1),INDEX(LinMotor!$AB$1:$AB$1305,A104,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A104,1),INDEX(LinMotor!$AD$1:$AD$1305,A104,1))","v":0.900240394024581},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A104,1),INDEX(LinMotor!$AE$1:$AE$1305,A104,1))","v":1.2806755510368051},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A104,1),INDEX(LinMotor!$AF$1:$AF$1305,A104,1))","v":10.802884728294972},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A104,1),INDEX(LinMotor!$AG$1:$AG$1305,A104,1))","v":30.736213224883322},{"$f":"IF(A104<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A104,1),INDEX(LinMotor!$AI$1:$AI$1305,A104,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A104,1),INDEX(LinMotor!$AI$1:$AI$1305,A104,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A104,1),INDEX(LinMotor!$AI$1:$AI$1305,A104,1))/1000,\"0.0k\")),\"\")","v":561.31897388985055},{"$f":"IF(A104<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A104,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A104,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A104,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A104,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A104,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A104,1))/1000,\"0.0k\")),\"\")","v":455.02881290636242},{"$f":"IF(A104<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A104,1),INDEX(LinMotor!$AK$1:$AK$1305,A104,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A104,1),INDEX(LinMotor!$AK$1:$AK$1305,A104,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A104,1),INDEX(LinMotor!$AK$1:$AK$1305,A104,1))/1000,\"0.0k\")),\"\")","v":"4.4k"},""]
[321,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A105,1),INDEX(LinMotor!$B$1:$B$1291,A105,1))","v":"C054B (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A105,1),INDEX(LinMotor!$R$1:$R$1305,A105,1))","v":0.47348484848484845},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A105,1),INDEX(LinMotor!$S$1:$S$1305,A105,1))","v":0.57995303105910745},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A105,1),INDEX(LinMotor!$T$1:$T$1305,A105,1))","v":0.62264146281844479},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A105,1),INDEX(LinMotor!$U$1:$U$1305,A105,1))","v":1.0434782608695652},{"$f":"IF(A105<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A105,1),INDEX(LinMotor!$V$1:$V$1305,A105,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A105,1),INDEX(LinMotor!$V$1:$V$1305,A105,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A105,1),INDEX(LinMotor!$V$1:$V$1305,A105,1))/1000,\"0.0k\")),\"\")","v":37.91886508564329},{"$f":"IF(A105<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A105,1),INDEX(LinMotor!$W$1:$W$1305,A105,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A105,1),INDEX(LinMotor!$X$1:$X$1305,A105,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A105,1),INDEX(LinMotor!$W$1:$W$1305,A105,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A105,1),INDEX(LinMotor!$X$1:$X$1305,A105,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A105,1),INDEX(LinMotor!$W$1:$W$1305,A105,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A105,1),INDEX(LinMotor!$X$1:$X$1305,A105,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A105<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A105,1),INDEX(LinMotor!$X$1:$X$1305,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A105,1),INDEX(LinMotor!$Z$1:$Z$1305,A105,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A105,1),INDEX(LinMotor!$X$1:$X$1305,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A105,1),INDEX(LinMotor!$Z$1:$Z$1305,A105,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A105,1),INDEX(LinMotor!$X$1:$X$1305,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A105,1),INDEX(LinMotor!$Z$1:$Z$1305,A105,1)))/1000,\"0.0k\")),\"\")","v":-30.714280719371061},{"$f":"IF(A105<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A105,1),INDEX(LinMotor!$Y$1:$Y$1305,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A105,1),INDEX(LinMotor!$AB$1:$AB$1305,A105,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A105,1),INDEX(LinMotor!$Y$1:$Y$1305,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A105,1),INDEX(LinMotor!$AB$1:$AB$1305,A105,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A105,1),INDEX(LinMotor!$Y$1:$Y$1305,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A105,1),INDEX(LinMotor!$AB$1:$AB$1305,A105,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A105,1),INDEX(LinMotor!$AD$1:$AD$1305,A105,1))","v":0.80519574750577172},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A105,1),INDEX(LinMotor!$AE$1:$AE$1305,A105,1))","v":1.1454657161288078},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A105,1),INDEX(LinMotor!$AF$1:$AF$1305,A105,1))","v":9.6623489700692602},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A105,1),INDEX(LinMotor!$AG$1:$AG$1305,A105,1))","v":27.491177187091385},{"$f":"IF(A105<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A105,1),INDEX(LinMotor!$AI$1:$AI$1305,A105,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A105,1),INDEX(LinMotor!$AI$1:$AI$1305,A105,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A105,1),INDEX(LinMotor!$AI$1:$AI$1305,A105,1))/1000,\"0.0k\")),\"\")","v":630.16762148095768},{"$f":"IF(A105<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A105,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A105,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A105,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A105,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A105,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A105,1))/1000,\"0.0k\")),\"\")","v":510.84042776500723},{"$f":"IF(A105<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A105,1),INDEX(LinMotor!$AK$1:$AK$1305,A105,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A105,1),INDEX(LinMotor!$AK$1:$AK$1305,A105,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A105,1),INDEX(LinMotor!$AK$1:$AK$1305,A105,1))/1000,\"0.0k\")),\"\")","v":"4.9k"},""]
[501,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A106,1),INDEX(LinMotor!$B$1:$B$1291,A106,1))","v":"AKM2G-43I 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A106,1),INDEX(LinMotor!$R$1:$R$1305,A106,1))","v":12.820512785611177},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A106,1),INDEX(LinMotor!$S$1:$S$1305,A106,1))","v":0.67261121462131612},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A106,1),INDEX(LinMotor!$T$1:$T$1305,A106,1))","v":0.62251818113285518},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A106,1),INDEX(LinMotor!$U$1:$U$1305,A106,1))","v":0.85127108470610457},{"$f":"IF(A106<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A106,1),INDEX(LinMotor!$V$1:$V$1305,A106,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A106,1),INDEX(LinMotor!$V$1:$V$1305,A106,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A106,1),INDEX(LinMotor!$V$1:$V$1305,A106,1))/1000,\"0.0k\")),\"\")","v":13.135133859375069},{"$f":"IF(A106<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A106,1),INDEX(LinMotor!$W$1:$W$1305,A106,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A106,1),INDEX(LinMotor!$X$1:$X$1305,A106,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A106,1),INDEX(LinMotor!$W$1:$W$1305,A106,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A106,1),INDEX(LinMotor!$X$1:$X$1305,A106,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A106,1),INDEX(LinMotor!$W$1:$W$1305,A106,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A106,1),INDEX(LinMotor!$X$1:$X$1305,A106,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A106<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A106,1),INDEX(LinMotor!$X$1:$X$1305,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A106,1),INDEX(LinMotor!$Z$1:$Z$1305,A106,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A106,1),INDEX(LinMotor!$X$1:$X$1305,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A106,1),INDEX(LinMotor!$Z$1:$Z$1305,A106,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A106,1),INDEX(LinMotor!$X$1:$X$1305,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A106,1),INDEX(LinMotor!$Z$1:$Z$1305,A106,1)))/1000,\"0.0k\")),\"\")","v":-10.639458426093805},{"$f":"IF(A106<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A106,1),INDEX(LinMotor!$Y$1:$Y$1305,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A106,1),INDEX(LinMotor!$AB$1:$AB$1305,A106,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A106,1),INDEX(LinMotor!$Y$1:$Y$1305,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A106,1),INDEX(LinMotor!$AB$1:$AB$1305,A106,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A106,1),INDEX(LinMotor!$Y$1:$Y$1305,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A106,1),INDEX(LinMotor!$AB$1:$AB$1305,A106,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A106,1),INDEX(LinMotor!$AD$1:$AD$1305,A106,1))","v":0.39353686214839967},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A106,1),INDEX(LinMotor!$AE$1:$AE$1305,A106,1))","v":0.55984272770972277},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A106,1),INDEX(LinMotor!$AF$1:$AF$1305,A106,1))","v":4.722442345780796},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A106,1),INDEX(LinMotor!$AG$1:$AG$1305,A106,1))","v":13.436225465033347},{"$f":"IF(A106<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A106,1),INDEX(LinMotor!$AI$1:$AI$1305,A106,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A106,1),INDEX(LinMotor!$AI$1:$AI$1305,A106,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A106,1),INDEX(LinMotor!$AI$1:$AI$1305,A106,1))/1000,\"0.0k\")),\"\")","v":218.29071211127351},{"$f":"IF(A106<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A106,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A106,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A106,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A106,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A106,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A106,1))/1000,\"0.0k\")),\"\")","v":176.95564949844169},{"$f":"IF(A106<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A106,1),INDEX(LinMotor!$AK$1:$AK$1305,A106,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A106,1),INDEX(LinMotor!$AK$1:$AK$1305,A106,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A106,1),INDEX(LinMotor!$AK$1:$AK$1305,A106,1))/1000,\"0.0k\")),\"\")","v":"1.7k"},""]
[502,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A107,1),INDEX(LinMotor!$B$1:$B$1291,A107,1))","v":"AKM2G-43I 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A107,1),INDEX(LinMotor!$R$1:$R$1305,A107,1))","v":12.820512785611177},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A107,1),INDEX(LinMotor!$S$1:$S$1305,A107,1))","v":0.67923996567656231},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A107,1),INDEX(LinMotor!$T$1:$T$1305,A107,1))","v":0.62251818113285518},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A107,1),INDEX(LinMotor!$U$1:$U$1305,A107,1))","v":0.85127108470610457},{"$f":"IF(A107<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A107,1),INDEX(LinMotor!$V$1:$V$1305,A107,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A107,1),INDEX(LinMotor!$V$1:$V$1305,A107,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A107,1),INDEX(LinMotor!$V$1:$V$1305,A107,1))/1000,\"0.0k\")),\"\")","v":13.135133859375069},{"$f":"IF(A107<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A107,1),INDEX(LinMotor!$W$1:$W$1305,A107,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A107,1),INDEX(LinMotor!$X$1:$X$1305,A107,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A107,1),INDEX(LinMotor!$W$1:$W$1305,A107,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A107,1),INDEX(LinMotor!$X$1:$X$1305,A107,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A107,1),INDEX(LinMotor!$W$1:$W$1305,A107,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A107,1),INDEX(LinMotor!$X$1:$X$1305,A107,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A107<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A107,1),INDEX(LinMotor!$X$1:$X$1305,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A107,1),INDEX(LinMotor!$Z$1:$Z$1305,A107,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A107,1),INDEX(LinMotor!$X$1:$X$1305,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A107,1),INDEX(LinMotor!$Z$1:$Z$1305,A107,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A107,1),INDEX(LinMotor!$X$1:$X$1305,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A107,1),INDEX(LinMotor!$Z$1:$Z$1305,A107,1)))/1000,\"0.0k\")),\"\")","v":-10.639458426093805},{"$f":"IF(A107<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A107,1),INDEX(LinMotor!$Y$1:$Y$1305,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A107,1),INDEX(LinMotor!$AB$1:$AB$1305,A107,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A107,1),INDEX(LinMotor!$Y$1:$Y$1305,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A107,1),INDEX(LinMotor!$AB$1:$AB$1305,A107,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A107,1),INDEX(LinMotor!$Y$1:$Y$1305,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A107,1),INDEX(LinMotor!$AB$1:$AB$1305,A107,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A107,1),INDEX(LinMotor!$AD$1:$AD$1305,A107,1))","v":0.39353686214839967},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A107,1),INDEX(LinMotor!$AE$1:$AE$1305,A107,1))","v":0.55984272770972277},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A107,1),INDEX(LinMotor!$AF$1:$AF$1305,A107,1))","v":4.722442345780796},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A107,1),INDEX(LinMotor!$AG$1:$AG$1305,A107,1))","v":13.436225465033347},{"$f":"IF(A107<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A107,1),INDEX(LinMotor!$AI$1:$AI$1305,A107,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A107,1),INDEX(LinMotor!$AI$1:$AI$1305,A107,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A107,1),INDEX(LinMotor!$AI$1:$AI$1305,A107,1))/1000,\"0.0k\")),\"\")","v":218.29071211127351},{"$f":"IF(A107<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A107,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A107,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A107,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A107,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A107,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A107,1))/1000,\"0.0k\")),\"\")","v":176.95564949844169},{"$f":"IF(A107<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A107,1),INDEX(LinMotor!$AK$1:$AK$1305,A107,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A107,1),INDEX(LinMotor!$AK$1:$AK$1305,A107,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A107,1),INDEX(LinMotor!$AK$1:$AK$1305,A107,1))/1000,\"0.0k\")),\"\")","v":"1.7k"},""]
[503,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A108,1),INDEX(LinMotor!$B$1:$B$1291,A108,1))","v":"AKM2G-43I 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A108,1),INDEX(LinMotor!$R$1:$R$1305,A108,1))","v":12.820512785611177},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A108,1),INDEX(LinMotor!$S$1:$S$1305,A108,1))","v":0.68315881685441837},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A108,1),INDEX(LinMotor!$T$1:$T$1305,A108,1))","v":0.62251818113285518},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A108,1),INDEX(LinMotor!$U$1:$U$1305,A108,1))","v":0.85127108470610457},{"$f":"IF(A108<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A108,1),INDEX(LinMotor!$V$1:$V$1305,A108,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A108,1),INDEX(LinMotor!$V$1:$V$1305,A108,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A108,1),INDEX(LinMotor!$V$1:$V$1305,A108,1))/1000,\"0.0k\")),\"\")","v":13.135133859375069},{"$f":"IF(A108<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A108,1),INDEX(LinMotor!$W$1:$W$1305,A108,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A108,1),INDEX(LinMotor!$X$1:$X$1305,A108,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A108,1),INDEX(LinMotor!$W$1:$W$1305,A108,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A108,1),INDEX(LinMotor!$X$1:$X$1305,A108,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A108,1),INDEX(LinMotor!$W$1:$W$1305,A108,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A108,1),INDEX(LinMotor!$X$1:$X$1305,A108,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A108<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A108,1),INDEX(LinMotor!$X$1:$X$1305,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A108,1),INDEX(LinMotor!$Z$1:$Z$1305,A108,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A108,1),INDEX(LinMotor!$X$1:$X$1305,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A108,1),INDEX(LinMotor!$Z$1:$Z$1305,A108,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A108,1),INDEX(LinMotor!$X$1:$X$1305,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A108,1),INDEX(LinMotor!$Z$1:$Z$1305,A108,1)))/1000,\"0.0k\")),\"\")","v":-10.639458426093805},{"$f":"IF(A108<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A108,1),INDEX(LinMotor!$Y$1:$Y$1305,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A108,1),INDEX(LinMotor!$AB$1:$AB$1305,A108,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A108,1),INDEX(LinMotor!$Y$1:$Y$1305,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A108,1),INDEX(LinMotor!$AB$1:$AB$1305,A108,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A108,1),INDEX(LinMotor!$Y$1:$Y$1305,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A108,1),INDEX(LinMotor!$AB$1:$AB$1305,A108,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A108,1),INDEX(LinMotor!$AD$1:$AD$1305,A108,1))","v":0.39353686214839967},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A108,1),INDEX(LinMotor!$AE$1:$AE$1305,A108,1))","v":0.55984272770972277},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A108,1),INDEX(LinMotor!$AF$1:$AF$1305,A108,1))","v":4.722442345780796},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A108,1),INDEX(LinMotor!$AG$1:$AG$1305,A108,1))","v":13.436225465033347},{"$f":"IF(A108<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A108,1),INDEX(LinMotor!$AI$1:$AI$1305,A108,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A108,1),INDEX(LinMotor!$AI$1:$AI$1305,A108,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A108,1),INDEX(LinMotor!$AI$1:$AI$1305,A108,1))/1000,\"0.0k\")),\"\")","v":218.29071211127351},{"$f":"IF(A108<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A108,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A108,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A108,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A108,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A108,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A108,1))/1000,\"0.0k\")),\"\")","v":176.95564949844169},{"$f":"IF(A108<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A108,1),INDEX(LinMotor!$AK$1:$AK$1305,A108,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A108,1),INDEX(LinMotor!$AK$1:$AK$1305,A108,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A108,1),INDEX(LinMotor!$AK$1:$AK$1305,A108,1))/1000,\"0.0k\")),\"\")","v":"1.7k"},""]
[512,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A109,1),INDEX(LinMotor!$B$1:$B$1291,A109,1))","v":"AKM2G-44J 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A109,1),INDEX(LinMotor!$R$1:$R$1305,A109,1))","v":9.8814227056346819},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A109,1),INDEX(LinMotor!$S$1:$S$1305,A109,1))","v":0.5672948511276763},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A109,1),INDEX(LinMotor!$T$1:$T$1305,A109,1))","v":0.49880370635802251},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A109,1),INDEX(LinMotor!$U$1:$U$1305,A109,1))","v":0.95556713066731125},{"$f":"IF(A109<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A109,1),INDEX(LinMotor!$V$1:$V$1305,A109,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A109,1),INDEX(LinMotor!$V$1:$V$1305,A109,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A109,1),INDEX(LinMotor!$V$1:$V$1305,A109,1))/1000,\"0.0k\")),\"\")","v":13.417819510752304},{"$f":"IF(A109<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A109,1),INDEX(LinMotor!$W$1:$W$1305,A109,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A109,1),INDEX(LinMotor!$X$1:$X$1305,A109,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A109,1),INDEX(LinMotor!$W$1:$W$1305,A109,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A109,1),INDEX(LinMotor!$X$1:$X$1305,A109,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A109,1),INDEX(LinMotor!$W$1:$W$1305,A109,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A109,1),INDEX(LinMotor!$X$1:$X$1305,A109,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A109<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A109,1),INDEX(LinMotor!$X$1:$X$1305,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A109,1),INDEX(LinMotor!$Z$1:$Z$1305,A109,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A109,1),INDEX(LinMotor!$X$1:$X$1305,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A109,1),INDEX(LinMotor!$Z$1:$Z$1305,A109,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A109,1),INDEX(LinMotor!$X$1:$X$1305,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A109,1),INDEX(LinMotor!$Z$1:$Z$1305,A109,1)))/1000,\"0.0k\")),\"\")","v":-10.868433803709365},{"$f":"IF(A109<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A109,1),INDEX(LinMotor!$Y$1:$Y$1305,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A109,1),INDEX(LinMotor!$AB$1:$AB$1305,A109,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A109,1),INDEX(LinMotor!$Y$1:$Y$1305,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A109,1),INDEX(LinMotor!$AB$1:$AB$1305,A109,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A109,1),INDEX(LinMotor!$Y$1:$Y$1305,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A109,1),INDEX(LinMotor!$AB$1:$AB$1305,A109,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A109,1),INDEX(LinMotor!$AD$1:$AD$1305,A109,1))","v":0.3387111775782386},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A109,1),INDEX(LinMotor!$AE$1:$AE$1305,A109,1))","v":0.48184810064798284},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A109,1),INDEX(LinMotor!$AF$1:$AF$1305,A109,1))","v":4.0645341309388634},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A109,1),INDEX(LinMotor!$AG$1:$AG$1305,A109,1))","v":11.564354415551588},{"$f":"IF(A109<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A109,1),INDEX(LinMotor!$AI$1:$AI$1305,A109,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A109,1),INDEX(LinMotor!$AI$1:$AI$1305,A109,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A109,1),INDEX(LinMotor!$AI$1:$AI$1305,A109,1))/1000,\"0.0k\")),\"\")","v":222.98862024098261},{"$f":"IF(A109<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A109,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A109,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A109,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A109,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A109,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A109,1))/1000,\"0.0k\")),\"\")","v":180.76397178726594},{"$f":"IF(A109<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A109,1),INDEX(LinMotor!$AK$1:$AK$1305,A109,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A109,1),INDEX(LinMotor!$AK$1:$AK$1305,A109,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A109,1),INDEX(LinMotor!$AK$1:$AK$1305,A109,1))/1000,\"0.0k\")),\"\")","v":"1.7k"},""]
[513,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A110,1),INDEX(LinMotor!$B$1:$B$1291,A110,1))","v":"AKM2G-44J 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A110,1),INDEX(LinMotor!$R$1:$R$1305,A110,1))","v":9.8814227056346819},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A110,1),INDEX(LinMotor!$S$1:$S$1305,A110,1))","v":0.57338001921028414},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A110,1),INDEX(LinMotor!$T$1:$T$1305,A110,1))","v":0.49880370635802251},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A110,1),INDEX(LinMotor!$U$1:$U$1305,A110,1))","v":0.95556713066731125},{"$f":"IF(A110<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A110,1),INDEX(LinMotor!$V$1:$V$1305,A110,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A110,1),INDEX(LinMotor!$V$1:$V$1305,A110,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A110,1),INDEX(LinMotor!$V$1:$V$1305,A110,1))/1000,\"0.0k\")),\"\")","v":13.417819510752304},{"$f":"IF(A110<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A110,1),INDEX(LinMotor!$W$1:$W$1305,A110,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A110,1),INDEX(LinMotor!$X$1:$X$1305,A110,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A110,1),INDEX(LinMotor!$W$1:$W$1305,A110,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A110,1),INDEX(LinMotor!$X$1:$X$1305,A110,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A110,1),INDEX(LinMotor!$W$1:$W$1305,A110,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A110,1),INDEX(LinMotor!$X$1:$X$1305,A110,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A110<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A110,1),INDEX(LinMotor!$X$1:$X$1305,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A110,1),INDEX(LinMotor!$Z$1:$Z$1305,A110,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A110,1),INDEX(LinMotor!$X$1:$X$1305,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A110,1),INDEX(LinMotor!$Z$1:$Z$1305,A110,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A110,1),INDEX(LinMotor!$X$1:$X$1305,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A110,1),INDEX(LinMotor!$Z$1:$Z$1305,A110,1)))/1000,\"0.0k\")),\"\")","v":-10.868433803709365},{"$f":"IF(A110<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A110,1),INDEX(LinMotor!$Y$1:$Y$1305,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A110,1),INDEX(LinMotor!$AB$1:$AB$1305,A110,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A110,1),INDEX(LinMotor!$Y$1:$Y$1305,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A110,1),INDEX(LinMotor!$AB$1:$AB$1305,A110,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A110,1),INDEX(LinMotor!$Y$1:$Y$1305,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A110,1),INDEX(LinMotor!$AB$1:$AB$1305,A110,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A110,1),INDEX(LinMotor!$AD$1:$AD$1305,A110,1))","v":0.3387111775782386},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A110,1),INDEX(LinMotor!$AE$1:$AE$1305,A110,1))","v":0.48184810064798284},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A110,1),INDEX(LinMotor!$AF$1:$AF$1305,A110,1))","v":4.0645341309388634},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A110,1),INDEX(LinMotor!$AG$1:$AG$1305,A110,1))","v":11.564354415551588},{"$f":"IF(A110<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A110,1),INDEX(LinMotor!$AI$1:$AI$1305,A110,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A110,1),INDEX(LinMotor!$AI$1:$AI$1305,A110,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A110,1),INDEX(LinMotor!$AI$1:$AI$1305,A110,1))/1000,\"0.0k\")),\"\")","v":222.98862024098267},{"$f":"IF(A110<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A110,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A110,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A110,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A110,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A110,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A110,1))/1000,\"0.0k\")),\"\")","v":180.76397178726594},{"$f":"IF(A110<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A110,1),INDEX(LinMotor!$AK$1:$AK$1305,A110,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A110,1),INDEX(LinMotor!$AK$1:$AK$1305,A110,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A110,1),INDEX(LinMotor!$AK$1:$AK$1305,A110,1))/1000,\"0.0k\")),\"\")","v":"1.7k"},""]
[514,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A111,1),INDEX(LinMotor!$B$1:$B$1291,A111,1))","v":"AKM2G-44J 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A111,1),INDEX(LinMotor!$R$1:$R$1305,A111,1))","v":9.8814227056346819},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A111,1),INDEX(LinMotor!$S$1:$S$1305,A111,1))","v":0.57702937904444207},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A111,1),INDEX(LinMotor!$T$1:$T$1305,A111,1))","v":0.49880370635802251},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A111,1),INDEX(LinMotor!$U$1:$U$1305,A111,1))","v":0.95556713066731125},{"$f":"IF(A111<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A111,1),INDEX(LinMotor!$V$1:$V$1305,A111,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A111,1),INDEX(LinMotor!$V$1:$V$1305,A111,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A111,1),INDEX(LinMotor!$V$1:$V$1305,A111,1))/1000,\"0.0k\")),\"\")","v":13.417819510752304},{"$f":"IF(A111<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A111,1),INDEX(LinMotor!$W$1:$W$1305,A111,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A111,1),INDEX(LinMotor!$X$1:$X$1305,A111,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A111,1),INDEX(LinMotor!$W$1:$W$1305,A111,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A111,1),INDEX(LinMotor!$X$1:$X$1305,A111,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A111,1),INDEX(LinMotor!$W$1:$W$1305,A111,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A111,1),INDEX(LinMotor!$X$1:$X$1305,A111,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A111<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A111,1),INDEX(LinMotor!$X$1:$X$1305,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A111,1),INDEX(LinMotor!$Z$1:$Z$1305,A111,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A111,1),INDEX(LinMotor!$X$1:$X$1305,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A111,1),INDEX(LinMotor!$Z$1:$Z$1305,A111,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A111,1),INDEX(LinMotor!$X$1:$X$1305,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A111,1),INDEX(LinMotor!$Z$1:$Z$1305,A111,1)))/1000,\"0.0k\")),\"\")","v":-10.868433803709365},{"$f":"IF(A111<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A111,1),INDEX(LinMotor!$Y$1:$Y$1305,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A111,1),INDEX(LinMotor!$AB$1:$AB$1305,A111,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A111,1),INDEX(LinMotor!$Y$1:$Y$1305,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A111,1),INDEX(LinMotor!$AB$1:$AB$1305,A111,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A111,1),INDEX(LinMotor!$Y$1:$Y$1305,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A111,1),INDEX(LinMotor!$AB$1:$AB$1305,A111,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A111,1),INDEX(LinMotor!$AD$1:$AD$1305,A111,1))","v":0.3387111775782386},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A111,1),INDEX(LinMotor!$AE$1:$AE$1305,A111,1))","v":0.48184810064798284},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A111,1),INDEX(LinMotor!$AF$1:$AF$1305,A111,1))","v":4.0645341309388634},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A111,1),INDEX(LinMotor!$AG$1:$AG$1305,A111,1))","v":11.564354415551588},{"$f":"IF(A111<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A111,1),INDEX(LinMotor!$AI$1:$AI$1305,A111,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A111,1),INDEX(LinMotor!$AI$1:$AI$1305,A111,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A111,1),INDEX(LinMotor!$AI$1:$AI$1305,A111,1))/1000,\"0.0k\")),\"\")","v":222.98862024098261},{"$f":"IF(A111<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A111,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A111,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A111,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A111,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A111,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A111,1))/1000,\"0.0k\")),\"\")","v":180.76397178726594},{"$f":"IF(A111<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A111,1),INDEX(LinMotor!$AK$1:$AK$1305,A111,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A111,1),INDEX(LinMotor!$AK$1:$AK$1305,A111,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A111,1),INDEX(LinMotor!$AK$1:$AK$1305,A111,1))/1000,\"0.0k\")),\"\")","v":"1.7k"},""]
[524,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A112,1),INDEX(LinMotor!$B$1:$B$1291,A112,1))","v":"AKM2G-51K 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A112,1),INDEX(LinMotor!$R$1:$R$1305,A112,1))","v":9.9206349993890548},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A112,1),INDEX(LinMotor!$S$1:$S$1305,A112,1))","v":0.70300344091176503},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A112,1),INDEX(LinMotor!$T$1:$T$1305,A112,1))","v":0.8543277545526361},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A112,1),INDEX(LinMotor!$U$1:$U$1305,A112,1))","v":0.65624883882366425},{"$f":"IF(A112<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A112,1),INDEX(LinMotor!$V$1:$V$1305,A112,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A112,1),INDEX(LinMotor!$V$1:$V$1305,A112,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A112,1),INDEX(LinMotor!$V$1:$V$1305,A112,1))/1000,\"0.0k\")),\"\")","v":13.412945583526268},{"$f":"IF(A112<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A112,1),INDEX(LinMotor!$W$1:$W$1305,A112,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A112,1),INDEX(LinMotor!$X$1:$X$1305,A112,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A112,1),INDEX(LinMotor!$W$1:$W$1305,A112,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A112,1),INDEX(LinMotor!$X$1:$X$1305,A112,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A112,1),INDEX(LinMotor!$W$1:$W$1305,A112,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A112,1),INDEX(LinMotor!$X$1:$X$1305,A112,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A112<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A112,1),INDEX(LinMotor!$X$1:$X$1305,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A112,1),INDEX(LinMotor!$Z$1:$Z$1305,A112,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A112,1),INDEX(LinMotor!$X$1:$X$1305,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A112,1),INDEX(LinMotor!$Z$1:$Z$1305,A112,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A112,1),INDEX(LinMotor!$X$1:$X$1305,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A112,1),INDEX(LinMotor!$Z$1:$Z$1305,A112,1)))/1000,\"0.0k\")),\"\")","v":-10.864485922656275},{"$f":"IF(A112<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A112,1),INDEX(LinMotor!$Y$1:$Y$1305,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A112,1),INDEX(LinMotor!$AB$1:$AB$1305,A112,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A112,1),INDEX(LinMotor!$Y$1:$Y$1305,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A112,1),INDEX(LinMotor!$AB$1:$AB$1305,A112,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A112,1),INDEX(LinMotor!$Y$1:$Y$1305,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A112,1),INDEX(LinMotor!$AB$1:$AB$1305,A112,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A112,1),INDEX(LinMotor!$AD$1:$AD$1305,A112,1))","v":0.58841719262137471},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A112,1),INDEX(LinMotor!$AE$1:$AE$1305,A112,1))","v":0.83707809314245551},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A112,1),INDEX(LinMotor!$AF$1:$AF$1305,A112,1))","v":7.0610063114564969},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A112,1),INDEX(LinMotor!$AG$1:$AG$1305,A112,1))","v":20.089874235418932},{"$f":"IF(A112<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A112,1),INDEX(LinMotor!$AI$1:$AI$1305,A112,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A112,1),INDEX(LinMotor!$AI$1:$AI$1305,A112,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A112,1),INDEX(LinMotor!$AI$1:$AI$1305,A112,1))/1000,\"0.0k\")),\"\")","v":222.90762121529011},{"$f":"IF(A112<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A112,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A112,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A112,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A112,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A112,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A112,1))/1000,\"0.0k\")),\"\")","v":180.69831056392974},{"$f":"IF(A112<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A112,1),INDEX(LinMotor!$AK$1:$AK$1305,A112,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A112,1),INDEX(LinMotor!$AK$1:$AK$1305,A112,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A112,1),INDEX(LinMotor!$AK$1:$AK$1305,A112,1))/1000,\"0.0k\")),\"\")","v":"1.7k"},""]
[525,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A113,1),INDEX(LinMotor!$B$1:$B$1291,A113,1))","v":"AKM2G-51K 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A113,1),INDEX(LinMotor!$R$1:$R$1305,A113,1))","v":9.9206349993890548},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A113,1),INDEX(LinMotor!$S$1:$S$1305,A113,1))","v":0.70907541130390095},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A113,1),INDEX(LinMotor!$T$1:$T$1305,A113,1))","v":0.8543277545526361},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A113,1),INDEX(LinMotor!$U$1:$U$1305,A113,1))","v":0.65624883882366425},{"$f":"IF(A113<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A113,1),INDEX(LinMotor!$V$1:$V$1305,A113,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A113,1),INDEX(LinMotor!$V$1:$V$1305,A113,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A113,1),INDEX(LinMotor!$V$1:$V$1305,A113,1))/1000,\"0.0k\")),\"\")","v":13.412945583526268},{"$f":"IF(A113<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A113,1),INDEX(LinMotor!$W$1:$W$1305,A113,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A113,1),INDEX(LinMotor!$X$1:$X$1305,A113,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A113,1),INDEX(LinMotor!$W$1:$W$1305,A113,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A113,1),INDEX(LinMotor!$X$1:$X$1305,A113,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A113,1),INDEX(LinMotor!$W$1:$W$1305,A113,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A113,1),INDEX(LinMotor!$X$1:$X$1305,A113,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A113<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A113,1),INDEX(LinMotor!$X$1:$X$1305,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A113,1),INDEX(LinMotor!$Z$1:$Z$1305,A113,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A113,1),INDEX(LinMotor!$X$1:$X$1305,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A113,1),INDEX(LinMotor!$Z$1:$Z$1305,A113,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A113,1),INDEX(LinMotor!$X$1:$X$1305,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A113,1),INDEX(LinMotor!$Z$1:$Z$1305,A113,1)))/1000,\"0.0k\")),\"\")","v":-10.864485922656275},{"$f":"IF(A113<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A113,1),INDEX(LinMotor!$Y$1:$Y$1305,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A113,1),INDEX(LinMotor!$AB$1:$AB$1305,A113,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A113,1),INDEX(LinMotor!$Y$1:$Y$1305,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A113,1),INDEX(LinMotor!$AB$1:$AB$1305,A113,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A113,1),INDEX(LinMotor!$Y$1:$Y$1305,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A113,1),INDEX(LinMotor!$AB$1:$AB$1305,A113,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A113,1),INDEX(LinMotor!$AD$1:$AD$1305,A113,1))","v":0.58841719262137471},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A113,1),INDEX(LinMotor!$AE$1:$AE$1305,A113,1))","v":0.83707809314245551},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A113,1),INDEX(LinMotor!$AF$1:$AF$1305,A113,1))","v":7.0610063114564969},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A113,1),INDEX(LinMotor!$AG$1:$AG$1305,A113,1))","v":20.089874235418932},{"$f":"IF(A113<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A113,1),INDEX(LinMotor!$AI$1:$AI$1305,A113,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A113,1),INDEX(LinMotor!$AI$1:$AI$1305,A113,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A113,1),INDEX(LinMotor!$AI$1:$AI$1305,A113,1))/1000,\"0.0k\")),\"\")","v":222.90762121529011},{"$f":"IF(A113<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A113,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A113,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A113,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A113,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A113,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A113,1))/1000,\"0.0k\")),\"\")","v":180.69831056392974},{"$f":"IF(A113<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A113,1),INDEX(LinMotor!$AK$1:$AK$1305,A113,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A113,1),INDEX(LinMotor!$AK$1:$AK$1305,A113,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A113,1),INDEX(LinMotor!$AK$1:$AK$1305,A113,1))/1000,\"0.0k\")),\"\")","v":"1.7k"},""]
[530,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A114,1),INDEX(LinMotor!$B$1:$B$1291,A114,1))","v":"AKM2G-52K 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A114,1),INDEX(LinMotor!$R$1:$R$1305,A114,1))","v":5.4585153436920901},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A114,1),INDEX(LinMotor!$S$1:$S$1305,A114,1))","v":0.43296980454629619},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A114,1),INDEX(LinMotor!$T$1:$T$1305,A114,1))","v":0.49713679076729023},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A114,1),INDEX(LinMotor!$U$1:$U$1305,A114,1))","v":0.96},{"$f":"IF(A114<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A114,1),INDEX(LinMotor!$V$1:$V$1305,A114,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A114,1),INDEX(LinMotor!$V$1:$V$1305,A114,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A114,1),INDEX(LinMotor!$V$1:$V$1305,A114,1))/1000,\"0.0k\")),\"\")","v":14.416966932251416},{"$f":"IF(A114<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A114,1),INDEX(LinMotor!$W$1:$W$1305,A114,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A114,1),INDEX(LinMotor!$X$1:$X$1305,A114,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A114,1),INDEX(LinMotor!$W$1:$W$1305,A114,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A114,1),INDEX(LinMotor!$X$1:$X$1305,A114,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A114,1),INDEX(LinMotor!$W$1:$W$1305,A114,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A114,1),INDEX(LinMotor!$X$1:$X$1305,A114,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A114<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A114,1),INDEX(LinMotor!$X$1:$X$1305,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A114,1),INDEX(LinMotor!$Z$1:$Z$1305,A114,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A114,1),INDEX(LinMotor!$X$1:$X$1305,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A114,1),INDEX(LinMotor!$Z$1:$Z$1305,A114,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A114,1),INDEX(LinMotor!$X$1:$X$1305,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A114,1),INDEX(LinMotor!$Z$1:$Z$1305,A114,1)))/1000,\"0.0k\")),\"\")","v":-11.677743215123646},{"$f":"IF(A114<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A114,1),INDEX(LinMotor!$Y$1:$Y$1305,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A114,1),INDEX(LinMotor!$AB$1:$AB$1305,A114,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A114,1),INDEX(LinMotor!$Y$1:$Y$1305,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A114,1),INDEX(LinMotor!$AB$1:$AB$1305,A114,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A114,1),INDEX(LinMotor!$Y$1:$Y$1305,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A114,1),INDEX(LinMotor!$AB$1:$AB$1305,A114,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A114,1),INDEX(LinMotor!$AD$1:$AD$1305,A114,1))","v":0.35484205888375997},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A114,1),INDEX(LinMotor!$AE$1:$AE$1305,A114,1))","v":0.50479577711504631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A114,1),INDEX(LinMotor!$AF$1:$AF$1305,A114,1))","v":4.2581047066051196},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A114,1),INDEX(LinMotor!$AG$1:$AG$1305,A114,1))","v":12.11509865076111},{"$f":"IF(A114<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A114,1),INDEX(LinMotor!$AI$1:$AI$1305,A114,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A114,1),INDEX(LinMotor!$AI$1:$AI$1305,A114,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A114,1),INDEX(LinMotor!$AI$1:$AI$1305,A114,1))/1000,\"0.0k\")),\"\")","v":239.59329321030404},{"$f":"IF(A114<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A114,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A114,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A114,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A114,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A114,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A114,1))/1000,\"0.0k\")),\"\")","v":194.22441937835589},{"$f":"IF(A114<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A114,1),INDEX(LinMotor!$AK$1:$AK$1305,A114,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A114,1),INDEX(LinMotor!$AK$1:$AK$1305,A114,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A114,1),INDEX(LinMotor!$AK$1:$AK$1305,A114,1))/1000,\"0.0k\")),\"\")","v":"1.9k"},""]
[531,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A115,1),INDEX(LinMotor!$B$1:$B$1291,A115,1))","v":"AKM2G-52K 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A115,1),INDEX(LinMotor!$R$1:$R$1305,A115,1))","v":5.4585153436920901},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A115,1),INDEX(LinMotor!$S$1:$S$1305,A115,1))","v":0.43678846986743158},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A115,1),INDEX(LinMotor!$T$1:$T$1305,A115,1))","v":0.49713679076729023},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A115,1),INDEX(LinMotor!$U$1:$U$1305,A115,1))","v":0.95629678804501661},{"$f":"IF(A115<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A115,1),INDEX(LinMotor!$V$1:$V$1305,A115,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A115,1),INDEX(LinMotor!$V$1:$V$1305,A115,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A115,1),INDEX(LinMotor!$V$1:$V$1305,A115,1))/1000,\"0.0k\")),\"\")","v":14.416966932251416},{"$f":"IF(A115<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A115,1),INDEX(LinMotor!$W$1:$W$1305,A115,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A115,1),INDEX(LinMotor!$X$1:$X$1305,A115,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A115,1),INDEX(LinMotor!$W$1:$W$1305,A115,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A115,1),INDEX(LinMotor!$X$1:$X$1305,A115,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A115,1),INDEX(LinMotor!$W$1:$W$1305,A115,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A115,1),INDEX(LinMotor!$X$1:$X$1305,A115,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A115<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A115,1),INDEX(LinMotor!$X$1:$X$1305,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A115,1),INDEX(LinMotor!$Z$1:$Z$1305,A115,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A115,1),INDEX(LinMotor!$X$1:$X$1305,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A115,1),INDEX(LinMotor!$Z$1:$Z$1305,A115,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A115,1),INDEX(LinMotor!$X$1:$X$1305,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A115,1),INDEX(LinMotor!$Z$1:$Z$1305,A115,1)))/1000,\"0.0k\")),\"\")","v":-11.677743215123646},{"$f":"IF(A115<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A115,1),INDEX(LinMotor!$Y$1:$Y$1305,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A115,1),INDEX(LinMotor!$AB$1:$AB$1305,A115,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A115,1),INDEX(LinMotor!$Y$1:$Y$1305,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A115,1),INDEX(LinMotor!$AB$1:$AB$1305,A115,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A115,1),INDEX(LinMotor!$Y$1:$Y$1305,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A115,1),INDEX(LinMotor!$AB$1:$AB$1305,A115,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A115,1),INDEX(LinMotor!$AD$1:$AD$1305,A115,1))","v":0.35484205888375997},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A115,1),INDEX(LinMotor!$AE$1:$AE$1305,A115,1))","v":0.50479577711504631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A115,1),INDEX(LinMotor!$AF$1:$AF$1305,A115,1))","v":4.2581047066051196},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A115,1),INDEX(LinMotor!$AG$1:$AG$1305,A115,1))","v":12.11509865076111},{"$f":"IF(A115<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A115,1),INDEX(LinMotor!$AI$1:$AI$1305,A115,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A115,1),INDEX(LinMotor!$AI$1:$AI$1305,A115,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A115,1),INDEX(LinMotor!$AI$1:$AI$1305,A115,1))/1000,\"0.0k\")),\"\")","v":239.59329321030404},{"$f":"IF(A115<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A115,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A115,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A115,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A115,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A115,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A115,1))/1000,\"0.0k\")),\"\")","v":194.22441937835589},{"$f":"IF(A115<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A115,1),INDEX(LinMotor!$AK$1:$AK$1305,A115,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A115,1),INDEX(LinMotor!$AK$1:$AK$1305,A115,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A115,1),INDEX(LinMotor!$AK$1:$AK$1305,A115,1))/1000,\"0.0k\")),\"\")","v":"1.9k"},""]
[532,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A116,1),INDEX(LinMotor!$B$1:$B$1291,A116,1))","v":"AKM2G-52K 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A116,1),INDEX(LinMotor!$R$1:$R$1305,A116,1))","v":5.4585153436920901},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A116,1),INDEX(LinMotor!$S$1:$S$1305,A116,1))","v":0.43862265033100262},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A116,1),INDEX(LinMotor!$T$1:$T$1305,A116,1))","v":0.49713679076729023},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A116,1),INDEX(LinMotor!$U$1:$U$1305,A116,1))","v":0.95629678804501661},{"$f":"IF(A116<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A116,1),INDEX(LinMotor!$V$1:$V$1305,A116,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A116,1),INDEX(LinMotor!$V$1:$V$1305,A116,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A116,1),INDEX(LinMotor!$V$1:$V$1305,A116,1))/1000,\"0.0k\")),\"\")","v":14.416966932251416},{"$f":"IF(A116<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A116,1),INDEX(LinMotor!$W$1:$W$1305,A116,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A116,1),INDEX(LinMotor!$X$1:$X$1305,A116,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A116,1),INDEX(LinMotor!$W$1:$W$1305,A116,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A116,1),INDEX(LinMotor!$X$1:$X$1305,A116,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A116,1),INDEX(LinMotor!$W$1:$W$1305,A116,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A116,1),INDEX(LinMotor!$X$1:$X$1305,A116,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A116<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A116,1),INDEX(LinMotor!$X$1:$X$1305,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A116,1),INDEX(LinMotor!$Z$1:$Z$1305,A116,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A116,1),INDEX(LinMotor!$X$1:$X$1305,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A116,1),INDEX(LinMotor!$Z$1:$Z$1305,A116,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A116,1),INDEX(LinMotor!$X$1:$X$1305,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A116,1),INDEX(LinMotor!$Z$1:$Z$1305,A116,1)))/1000,\"0.0k\")),\"\")","v":-11.677743215123646},{"$f":"IF(A116<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A116,1),INDEX(LinMotor!$Y$1:$Y$1305,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A116,1),INDEX(LinMotor!$AB$1:$AB$1305,A116,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A116,1),INDEX(LinMotor!$Y$1:$Y$1305,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A116,1),INDEX(LinMotor!$AB$1:$AB$1305,A116,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A116,1),INDEX(LinMotor!$Y$1:$Y$1305,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A116,1),INDEX(LinMotor!$AB$1:$AB$1305,A116,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A116,1),INDEX(LinMotor!$AD$1:$AD$1305,A116,1))","v":0.35484205888375997},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A116,1),INDEX(LinMotor!$AE$1:$AE$1305,A116,1))","v":0.50479577711504631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A116,1),INDEX(LinMotor!$AF$1:$AF$1305,A116,1))","v":4.2581047066051196},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A116,1),INDEX(LinMotor!$AG$1:$AG$1305,A116,1))","v":12.11509865076111},{"$f":"IF(A116<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A116,1),INDEX(LinMotor!$AI$1:$AI$1305,A116,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A116,1),INDEX(LinMotor!$AI$1:$AI$1305,A116,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A116,1),INDEX(LinMotor!$AI$1:$AI$1305,A116,1))/1000,\"0.0k\")),\"\")","v":239.59329321030404},{"$f":"IF(A116<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A116,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A116,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A116,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A116,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A116,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A116,1))/1000,\"0.0k\")),\"\")","v":194.22441937835589},{"$f":"IF(A116<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A116,1),INDEX(LinMotor!$AK$1:$AK$1305,A116,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A116,1),INDEX(LinMotor!$AK$1:$AK$1305,A116,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A116,1),INDEX(LinMotor!$AK$1:$AK$1305,A116,1))/1000,\"0.0k\")),\"\")","v":"1.9k"},""]
[534,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A117,1),INDEX(LinMotor!$B$1:$B$1291,A117,1))","v":"AKM2G-52L 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A117,1),INDEX(LinMotor!$R$1:$R$1305,A117,1))","v":5.4585153436920901},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A117,1),INDEX(LinMotor!$S$1:$S$1305,A117,1))","v":0.43453642796345021},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A117,1),INDEX(LinMotor!$T$1:$T$1305,A117,1))","v":0.49885699385987003},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A117,1),INDEX(LinMotor!$U$1:$U$1305,A117,1))","v":0.76020391625725048},{"$f":"IF(A117<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A117,1),INDEX(LinMotor!$V$1:$V$1305,A117,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A117,1),INDEX(LinMotor!$V$1:$V$1305,A117,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A117,1),INDEX(LinMotor!$V$1:$V$1305,A117,1))/1000,\"0.0k\")),\"\")","v":14.416966932251416},{"$f":"IF(A117<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A117,1),INDEX(LinMotor!$W$1:$W$1305,A117,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A117,1),INDEX(LinMotor!$X$1:$X$1305,A117,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A117,1),INDEX(LinMotor!$W$1:$W$1305,A117,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A117,1),INDEX(LinMotor!$X$1:$X$1305,A117,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A117,1),INDEX(LinMotor!$W$1:$W$1305,A117,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A117,1),INDEX(LinMotor!$X$1:$X$1305,A117,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A117<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A117,1),INDEX(LinMotor!$X$1:$X$1305,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A117,1),INDEX(LinMotor!$Z$1:$Z$1305,A117,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A117,1),INDEX(LinMotor!$X$1:$X$1305,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A117,1),INDEX(LinMotor!$Z$1:$Z$1305,A117,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A117,1),INDEX(LinMotor!$X$1:$X$1305,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A117,1),INDEX(LinMotor!$Z$1:$Z$1305,A117,1)))/1000,\"0.0k\")),\"\")","v":-11.677743215123646},{"$f":"IF(A117<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A117,1),INDEX(LinMotor!$Y$1:$Y$1305,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A117,1),INDEX(LinMotor!$AB$1:$AB$1305,A117,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A117,1),INDEX(LinMotor!$Y$1:$Y$1305,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A117,1),INDEX(LinMotor!$AB$1:$AB$1305,A117,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A117,1),INDEX(LinMotor!$Y$1:$Y$1305,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A117,1),INDEX(LinMotor!$AB$1:$AB$1305,A117,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A117,1),INDEX(LinMotor!$AD$1:$AD$1305,A117,1))","v":0.44355257360469991},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A117,1),INDEX(LinMotor!$AE$1:$AE$1305,A117,1))","v":0.63099472139380774},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A117,1),INDEX(LinMotor!$AF$1:$AF$1305,A117,1))","v":5.3226308832563989},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A117,1),INDEX(LinMotor!$AG$1:$AG$1305,A117,1))","v":15.143873313451387},{"$f":"IF(A117<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A117,1),INDEX(LinMotor!$AI$1:$AI$1305,A117,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A117,1),INDEX(LinMotor!$AI$1:$AI$1305,A117,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A117,1),INDEX(LinMotor!$AI$1:$AI$1305,A117,1))/1000,\"0.0k\")),\"\")","v":239.59329321030404},{"$f":"IF(A117<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A117,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A117,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A117,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A117,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A117,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A117,1))/1000,\"0.0k\")),\"\")","v":194.22441937835589},{"$f":"IF(A117<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A117,1),INDEX(LinMotor!$AK$1:$AK$1305,A117,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A117,1),INDEX(LinMotor!$AK$1:$AK$1305,A117,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A117,1),INDEX(LinMotor!$AK$1:$AK$1305,A117,1))/1000,\"0.0k\")),\"\")","v":"1.9k"},""]
[535,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A118,1),INDEX(LinMotor!$B$1:$B$1291,A118,1))","v":"AKM2G-52L 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A118,1),INDEX(LinMotor!$R$1:$R$1305,A118,1))","v":5.4585153436920901},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A118,1),INDEX(LinMotor!$S$1:$S$1305,A118,1))","v":0.43914666000879665},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A118,1),INDEX(LinMotor!$T$1:$T$1305,A118,1))","v":0.49885699385987003},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A118,1),INDEX(LinMotor!$U$1:$U$1305,A118,1))","v":0.76020391625725048},{"$f":"IF(A118<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A118,1),INDEX(LinMotor!$V$1:$V$1305,A118,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A118,1),INDEX(LinMotor!$V$1:$V$1305,A118,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A118,1),INDEX(LinMotor!$V$1:$V$1305,A118,1))/1000,\"0.0k\")),\"\")","v":14.416966932251416},{"$f":"IF(A118<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A118,1),INDEX(LinMotor!$W$1:$W$1305,A118,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A118,1),INDEX(LinMotor!$X$1:$X$1305,A118,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A118,1),INDEX(LinMotor!$W$1:$W$1305,A118,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A118,1),INDEX(LinMotor!$X$1:$X$1305,A118,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A118,1),INDEX(LinMotor!$W$1:$W$1305,A118,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A118,1),INDEX(LinMotor!$X$1:$X$1305,A118,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A118<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A118,1),INDEX(LinMotor!$X$1:$X$1305,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A118,1),INDEX(LinMotor!$Z$1:$Z$1305,A118,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A118,1),INDEX(LinMotor!$X$1:$X$1305,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A118,1),INDEX(LinMotor!$Z$1:$Z$1305,A118,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A118,1),INDEX(LinMotor!$X$1:$X$1305,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A118,1),INDEX(LinMotor!$Z$1:$Z$1305,A118,1)))/1000,\"0.0k\")),\"\")","v":-11.677743215123646},{"$f":"IF(A118<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A118,1),INDEX(LinMotor!$Y$1:$Y$1305,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A118,1),INDEX(LinMotor!$AB$1:$AB$1305,A118,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A118,1),INDEX(LinMotor!$Y$1:$Y$1305,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A118,1),INDEX(LinMotor!$AB$1:$AB$1305,A118,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A118,1),INDEX(LinMotor!$Y$1:$Y$1305,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A118,1),INDEX(LinMotor!$AB$1:$AB$1305,A118,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A118,1),INDEX(LinMotor!$AD$1:$AD$1305,A118,1))","v":0.44355257360469991},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A118,1),INDEX(LinMotor!$AE$1:$AE$1305,A118,1))","v":0.63099472139380774},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A118,1),INDEX(LinMotor!$AF$1:$AF$1305,A118,1))","v":5.3226308832563989},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A118,1),INDEX(LinMotor!$AG$1:$AG$1305,A118,1))","v":15.143873313451387},{"$f":"IF(A118<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A118,1),INDEX(LinMotor!$AI$1:$AI$1305,A118,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A118,1),INDEX(LinMotor!$AI$1:$AI$1305,A118,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A118,1),INDEX(LinMotor!$AI$1:$AI$1305,A118,1))/1000,\"0.0k\")),\"\")","v":239.59329321030404},{"$f":"IF(A118<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A118,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A118,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A118,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A118,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A118,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A118,1))/1000,\"0.0k\")),\"\")","v":194.22441937835589},{"$f":"IF(A118<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A118,1),INDEX(LinMotor!$AK$1:$AK$1305,A118,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A118,1),INDEX(LinMotor!$AK$1:$AK$1305,A118,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A118,1),INDEX(LinMotor!$AK$1:$AK$1305,A118,1))/1000,\"0.0k\")),\"\")","v":"1.9k"},""]
[540,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A119,1),INDEX(LinMotor!$B$1:$B$1291,A119,1))","v":"AKM2G-53L 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A119,1),INDEX(LinMotor!$R$1:$R$1305,A119,1))","v":3.7650602865692933},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A119,1),INDEX(LinMotor!$S$1:$S$1305,A119,1))","v":0.34671670751584893},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A119,1),INDEX(LinMotor!$T$1:$T$1305,A119,1))","v":0.37248762590834672},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A119,1),INDEX(LinMotor!$U$1:$U$1305,A119,1))","v":1},{"$f":"IF(A119<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A119,1),INDEX(LinMotor!$V$1:$V$1305,A119,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A119,1),INDEX(LinMotor!$V$1:$V$1305,A119,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A119,1),INDEX(LinMotor!$V$1:$V$1305,A119,1))/1000,\"0.0k\")),\"\")","v":15.420988280976562},{"$f":"IF(A119<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A119,1),INDEX(LinMotor!$W$1:$W$1305,A119,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A119,1),INDEX(LinMotor!$X$1:$X$1305,A119,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A119,1),INDEX(LinMotor!$W$1:$W$1305,A119,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A119,1),INDEX(LinMotor!$X$1:$X$1305,A119,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A119,1),INDEX(LinMotor!$W$1:$W$1305,A119,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A119,1),INDEX(LinMotor!$X$1:$X$1305,A119,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A119<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A119,1),INDEX(LinMotor!$X$1:$X$1305,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A119,1),INDEX(LinMotor!$Z$1:$Z$1305,A119,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A119,1),INDEX(LinMotor!$X$1:$X$1305,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A119,1),INDEX(LinMotor!$Z$1:$Z$1305,A119,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A119,1),INDEX(LinMotor!$X$1:$X$1305,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A119,1),INDEX(LinMotor!$Z$1:$Z$1305,A119,1)))/1000,\"0.0k\")),\"\")","v":-12.491000507591014},{"$f":"IF(A119<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A119,1),INDEX(LinMotor!$Y$1:$Y$1305,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A119,1),INDEX(LinMotor!$AB$1:$AB$1305,A119,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A119,1),INDEX(LinMotor!$Y$1:$Y$1305,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A119,1),INDEX(LinMotor!$AB$1:$AB$1305,A119,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A119,1),INDEX(LinMotor!$Y$1:$Y$1305,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A119,1),INDEX(LinMotor!$AB$1:$AB$1305,A119,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A119,1),INDEX(LinMotor!$AD$1:$AD$1305,A119,1))","v":0.35286645391478927},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A119,1),INDEX(LinMotor!$AE$1:$AE$1305,A119,1))","v":0.50198529560470584},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A119,1),INDEX(LinMotor!$AF$1:$AF$1305,A119,1))","v":4.2343974469774714},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A119,1),INDEX(LinMotor!$AG$1:$AG$1305,A119,1))","v":12.047647094512939},{"$f":"IF(A119<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A119,1),INDEX(LinMotor!$AI$1:$AI$1305,A119,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A119,1),INDEX(LinMotor!$AI$1:$AI$1305,A119,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A119,1),INDEX(LinMotor!$AI$1:$AI$1305,A119,1))/1000,\"0.0k\")),\"\")","v":256.278965205318},{"$f":"IF(A119<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A119,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A119,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A119,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A119,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A119,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A119,1))/1000,\"0.0k\")),\"\")","v":207.75052819278193},{"$f":"IF(A119<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A119,1),INDEX(LinMotor!$AK$1:$AK$1305,A119,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A119,1),INDEX(LinMotor!$AK$1:$AK$1305,A119,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A119,1),INDEX(LinMotor!$AK$1:$AK$1305,A119,1))/1000,\"0.0k\")),\"\")","v":"2.0k"},""]
[541,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A120,1),INDEX(LinMotor!$B$1:$B$1291,A120,1))","v":"AKM2G-53L 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A120,1),INDEX(LinMotor!$R$1:$R$1305,A120,1))","v":3.7650602865692933},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A120,1),INDEX(LinMotor!$S$1:$S$1305,A120,1))","v":0.35090449639973936},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A120,1),INDEX(LinMotor!$T$1:$T$1305,A120,1))","v":0.37248762590834672},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A120,1),INDEX(LinMotor!$U$1:$U$1305,A120,1))","v":0.98215903428621099},{"$f":"IF(A120<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A120,1),INDEX(LinMotor!$V$1:$V$1305,A120,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A120,1),INDEX(LinMotor!$V$1:$V$1305,A120,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A120,1),INDEX(LinMotor!$V$1:$V$1305,A120,1))/1000,\"0.0k\")),\"\")","v":15.420988280976562},{"$f":"IF(A120<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A120,1),INDEX(LinMotor!$W$1:$W$1305,A120,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A120,1),INDEX(LinMotor!$X$1:$X$1305,A120,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A120,1),INDEX(LinMotor!$W$1:$W$1305,A120,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A120,1),INDEX(LinMotor!$X$1:$X$1305,A120,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A120,1),INDEX(LinMotor!$W$1:$W$1305,A120,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A120,1),INDEX(LinMotor!$X$1:$X$1305,A120,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A120<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A120,1),INDEX(LinMotor!$X$1:$X$1305,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A120,1),INDEX(LinMotor!$Z$1:$Z$1305,A120,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A120,1),INDEX(LinMotor!$X$1:$X$1305,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A120,1),INDEX(LinMotor!$Z$1:$Z$1305,A120,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A120,1),INDEX(LinMotor!$X$1:$X$1305,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A120,1),INDEX(LinMotor!$Z$1:$Z$1305,A120,1)))/1000,\"0.0k\")),\"\")","v":-12.491000507591014},{"$f":"IF(A120<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A120,1),INDEX(LinMotor!$Y$1:$Y$1305,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A120,1),INDEX(LinMotor!$AB$1:$AB$1305,A120,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A120,1),INDEX(LinMotor!$Y$1:$Y$1305,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A120,1),INDEX(LinMotor!$AB$1:$AB$1305,A120,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A120,1),INDEX(LinMotor!$Y$1:$Y$1305,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A120,1),INDEX(LinMotor!$AB$1:$AB$1305,A120,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A120,1),INDEX(LinMotor!$AD$1:$AD$1305,A120,1))","v":0.35286645391478927},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A120,1),INDEX(LinMotor!$AE$1:$AE$1305,A120,1))","v":0.50198529560470584},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A120,1),INDEX(LinMotor!$AF$1:$AF$1305,A120,1))","v":4.2343974469774714},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A120,1),INDEX(LinMotor!$AG$1:$AG$1305,A120,1))","v":12.047647094512939},{"$f":"IF(A120<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A120,1),INDEX(LinMotor!$AI$1:$AI$1305,A120,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A120,1),INDEX(LinMotor!$AI$1:$AI$1305,A120,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A120,1),INDEX(LinMotor!$AI$1:$AI$1305,A120,1))/1000,\"0.0k\")),\"\")","v":256.278965205318},{"$f":"IF(A120<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A120,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A120,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A120,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A120,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A120,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A120,1))/1000,\"0.0k\")),\"\")","v":207.75052819278193},{"$f":"IF(A120<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A120,1),INDEX(LinMotor!$AK$1:$AK$1305,A120,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A120,1),INDEX(LinMotor!$AK$1:$AK$1305,A120,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A120,1),INDEX(LinMotor!$AK$1:$AK$1305,A120,1))/1000,\"0.0k\")),\"\")","v":"2.0k"},""]
[542,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A121,1),INDEX(LinMotor!$B$1:$B$1291,A121,1))","v":"AKM2G-53L 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A121,1),INDEX(LinMotor!$R$1:$R$1305,A121,1))","v":3.7650602865692933},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A121,1),INDEX(LinMotor!$S$1:$S$1305,A121,1))","v":0.35314994817840761},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A121,1),INDEX(LinMotor!$T$1:$T$1305,A121,1))","v":0.37248762590834672},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A121,1),INDEX(LinMotor!$U$1:$U$1305,A121,1))","v":0.98215903428621099},{"$f":"IF(A121<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A121,1),INDEX(LinMotor!$V$1:$V$1305,A121,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A121,1),INDEX(LinMotor!$V$1:$V$1305,A121,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A121,1),INDEX(LinMotor!$V$1:$V$1305,A121,1))/1000,\"0.0k\")),\"\")","v":15.420988280976562},{"$f":"IF(A121<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A121,1),INDEX(LinMotor!$W$1:$W$1305,A121,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A121,1),INDEX(LinMotor!$X$1:$X$1305,A121,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A121,1),INDEX(LinMotor!$W$1:$W$1305,A121,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A121,1),INDEX(LinMotor!$X$1:$X$1305,A121,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A121,1),INDEX(LinMotor!$W$1:$W$1305,A121,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A121,1),INDEX(LinMotor!$X$1:$X$1305,A121,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A121<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A121,1),INDEX(LinMotor!$X$1:$X$1305,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A121,1),INDEX(LinMotor!$Z$1:$Z$1305,A121,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A121,1),INDEX(LinMotor!$X$1:$X$1305,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A121,1),INDEX(LinMotor!$Z$1:$Z$1305,A121,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A121,1),INDEX(LinMotor!$X$1:$X$1305,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A121,1),INDEX(LinMotor!$Z$1:$Z$1305,A121,1)))/1000,\"0.0k\")),\"\")","v":-12.491000507591014},{"$f":"IF(A121<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A121,1),INDEX(LinMotor!$Y$1:$Y$1305,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A121,1),INDEX(LinMotor!$AB$1:$AB$1305,A121,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A121,1),INDEX(LinMotor!$Y$1:$Y$1305,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A121,1),INDEX(LinMotor!$AB$1:$AB$1305,A121,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A121,1),INDEX(LinMotor!$Y$1:$Y$1305,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A121,1),INDEX(LinMotor!$AB$1:$AB$1305,A121,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A121,1),INDEX(LinMotor!$AD$1:$AD$1305,A121,1))","v":0.35286645391478927},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A121,1),INDEX(LinMotor!$AE$1:$AE$1305,A121,1))","v":0.50198529560470584},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A121,1),INDEX(LinMotor!$AF$1:$AF$1305,A121,1))","v":4.2343974469774714},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A121,1),INDEX(LinMotor!$AG$1:$AG$1305,A121,1))","v":12.047647094512939},{"$f":"IF(A121<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A121,1),INDEX(LinMotor!$AI$1:$AI$1305,A121,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A121,1),INDEX(LinMotor!$AI$1:$AI$1305,A121,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A121,1),INDEX(LinMotor!$AI$1:$AI$1305,A121,1))/1000,\"0.0k\")),\"\")","v":256.278965205318},{"$f":"IF(A121<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A121,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A121,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A121,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A121,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A121,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A121,1))/1000,\"0.0k\")),\"\")","v":207.75052819278193},{"$f":"IF(A121<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A121,1),INDEX(LinMotor!$AK$1:$AK$1305,A121,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A121,1),INDEX(LinMotor!$AK$1:$AK$1305,A121,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A121,1),INDEX(LinMotor!$AK$1:$AK$1305,A121,1))/1000,\"0.0k\")),\"\")","v":"2.0k"},""]
[544,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A122,1),INDEX(LinMotor!$B$1:$B$1291,A122,1))","v":"AKM2G-53M 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A122,1),INDEX(LinMotor!$R$1:$R$1305,A122,1))","v":3.7650602865692933},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A122,1),INDEX(LinMotor!$S$1:$S$1305,A122,1))","v":0.34550573005757335},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A122,1),INDEX(LinMotor!$T$1:$T$1305,A122,1))","v":0.37248762590834672},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A122,1),INDEX(LinMotor!$U$1:$U$1305,A122,1))","v":0.8675572889721922},{"$f":"IF(A122<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A122,1),INDEX(LinMotor!$V$1:$V$1305,A122,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A122,1),INDEX(LinMotor!$V$1:$V$1305,A122,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A122,1),INDEX(LinMotor!$V$1:$V$1305,A122,1))/1000,\"0.0k\")),\"\")","v":15.420988280976562},{"$f":"IF(A122<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A122,1),INDEX(LinMotor!$W$1:$W$1305,A122,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A122,1),INDEX(LinMotor!$X$1:$X$1305,A122,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A122,1),INDEX(LinMotor!$W$1:$W$1305,A122,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A122,1),INDEX(LinMotor!$X$1:$X$1305,A122,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A122,1),INDEX(LinMotor!$W$1:$W$1305,A122,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A122,1),INDEX(LinMotor!$X$1:$X$1305,A122,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A122<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A122,1),INDEX(LinMotor!$X$1:$X$1305,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A122,1),INDEX(LinMotor!$Z$1:$Z$1305,A122,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A122,1),INDEX(LinMotor!$X$1:$X$1305,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A122,1),INDEX(LinMotor!$Z$1:$Z$1305,A122,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A122,1),INDEX(LinMotor!$X$1:$X$1305,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A122,1),INDEX(LinMotor!$Z$1:$Z$1305,A122,1)))/1000,\"0.0k\")),\"\")","v":-12.491000507591014},{"$f":"IF(A122<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A122,1),INDEX(LinMotor!$Y$1:$Y$1305,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A122,1),INDEX(LinMotor!$AB$1:$AB$1305,A122,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A122,1),INDEX(LinMotor!$Y$1:$Y$1305,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A122,1),INDEX(LinMotor!$AB$1:$AB$1305,A122,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A122,1),INDEX(LinMotor!$Y$1:$Y$1305,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A122,1),INDEX(LinMotor!$AB$1:$AB$1305,A122,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A122,1),INDEX(LinMotor!$AD$1:$AD$1305,A122,1))","v":0.3983664862261746},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A122,1),INDEX(LinMotor!$AE$1:$AE$1305,A122,1))","v":0.56671331640820777},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A122,1),INDEX(LinMotor!$AF$1:$AF$1305,A122,1))","v":4.780397834714095},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A122,1),INDEX(LinMotor!$AG$1:$AG$1305,A122,1))","v":13.601119593796986},{"$f":"IF(A122<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A122,1),INDEX(LinMotor!$AI$1:$AI$1305,A122,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A122,1),INDEX(LinMotor!$AI$1:$AI$1305,A122,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A122,1),INDEX(LinMotor!$AI$1:$AI$1305,A122,1))/1000,\"0.0k\")),\"\")","v":256.278965205318},{"$f":"IF(A122<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A122,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A122,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A122,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A122,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A122,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A122,1))/1000,\"0.0k\")),\"\")","v":207.75052819278193},{"$f":"IF(A122<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A122,1),INDEX(LinMotor!$AK$1:$AK$1305,A122,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A122,1),INDEX(LinMotor!$AK$1:$AK$1305,A122,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A122,1),INDEX(LinMotor!$AK$1:$AK$1305,A122,1))/1000,\"0.0k\")),\"\")","v":"2.0k"},""]
[545,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A123,1),INDEX(LinMotor!$B$1:$B$1291,A123,1))","v":"AKM2G-53M 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A123,1),INDEX(LinMotor!$R$1:$R$1305,A123,1))","v":3.7650602865692933},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A123,1),INDEX(LinMotor!$S$1:$S$1305,A123,1))","v":0.34962227127797246},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A123,1),INDEX(LinMotor!$T$1:$T$1305,A123,1))","v":0.37248762590834672},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A123,1),INDEX(LinMotor!$U$1:$U$1305,A123,1))","v":0.8675572889721922},{"$f":"IF(A123<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A123,1),INDEX(LinMotor!$V$1:$V$1305,A123,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A123,1),INDEX(LinMotor!$V$1:$V$1305,A123,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A123,1),INDEX(LinMotor!$V$1:$V$1305,A123,1))/1000,\"0.0k\")),\"\")","v":15.420988280976562},{"$f":"IF(A123<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A123,1),INDEX(LinMotor!$W$1:$W$1305,A123,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A123,1),INDEX(LinMotor!$X$1:$X$1305,A123,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A123,1),INDEX(LinMotor!$W$1:$W$1305,A123,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A123,1),INDEX(LinMotor!$X$1:$X$1305,A123,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A123,1),INDEX(LinMotor!$W$1:$W$1305,A123,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A123,1),INDEX(LinMotor!$X$1:$X$1305,A123,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A123<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A123,1),INDEX(LinMotor!$X$1:$X$1305,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A123,1),INDEX(LinMotor!$Z$1:$Z$1305,A123,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A123,1),INDEX(LinMotor!$X$1:$X$1305,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A123,1),INDEX(LinMotor!$Z$1:$Z$1305,A123,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A123,1),INDEX(LinMotor!$X$1:$X$1305,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A123,1),INDEX(LinMotor!$Z$1:$Z$1305,A123,1)))/1000,\"0.0k\")),\"\")","v":-12.491000507591014},{"$f":"IF(A123<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A123,1),INDEX(LinMotor!$Y$1:$Y$1305,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A123,1),INDEX(LinMotor!$AB$1:$AB$1305,A123,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A123,1),INDEX(LinMotor!$Y$1:$Y$1305,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A123,1),INDEX(LinMotor!$AB$1:$AB$1305,A123,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A123,1),INDEX(LinMotor!$Y$1:$Y$1305,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A123,1),INDEX(LinMotor!$AB$1:$AB$1305,A123,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A123,1),INDEX(LinMotor!$AD$1:$AD$1305,A123,1))","v":0.3983664862261746},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A123,1),INDEX(LinMotor!$AE$1:$AE$1305,A123,1))","v":0.56671331640820777},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A123,1),INDEX(LinMotor!$AF$1:$AF$1305,A123,1))","v":4.780397834714095},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A123,1),INDEX(LinMotor!$AG$1:$AG$1305,A123,1))","v":13.601119593796986},{"$f":"IF(A123<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A123,1),INDEX(LinMotor!$AI$1:$AI$1305,A123,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A123,1),INDEX(LinMotor!$AI$1:$AI$1305,A123,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A123,1),INDEX(LinMotor!$AI$1:$AI$1305,A123,1))/1000,\"0.0k\")),\"\")","v":256.278965205318},{"$f":"IF(A123<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A123,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A123,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A123,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A123,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A123,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A123,1))/1000,\"0.0k\")),\"\")","v":207.75052819278193},{"$f":"IF(A123<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A123,1),INDEX(LinMotor!$AK$1:$AK$1305,A123,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A123,1),INDEX(LinMotor!$AK$1:$AK$1305,A123,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A123,1),INDEX(LinMotor!$AK$1:$AK$1305,A123,1))/1000,\"0.0k\")),\"\")","v":"2.0k"},""]
[550,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A124,1),INDEX(LinMotor!$B$1:$B$1291,A124,1))","v":"AKM2G-54M 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A124,1),INDEX(LinMotor!$R$1:$R$1305,A124,1))","v":2.8735632549349721},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A124,1),INDEX(LinMotor!$S$1:$S$1305,A124,1))","v":0.29695809600365702},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A124,1),INDEX(LinMotor!$T$1:$T$1305,A124,1))","v":0.3002743948923311},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A124,1),INDEX(LinMotor!$U$1:$U$1305,A124,1))","v":1.0434782608695652},{"$f":"IF(A124<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A124,1),INDEX(LinMotor!$V$1:$V$1305,A124,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A124,1),INDEX(LinMotor!$V$1:$V$1305,A124,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A124,1),INDEX(LinMotor!$V$1:$V$1305,A124,1))/1000,\"0.0k\")),\"\")","v":16.425009629701709},{"$f":"IF(A124<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A124,1),INDEX(LinMotor!$W$1:$W$1305,A124,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A124,1),INDEX(LinMotor!$X$1:$X$1305,A124,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A124,1),INDEX(LinMotor!$W$1:$W$1305,A124,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A124,1),INDEX(LinMotor!$X$1:$X$1305,A124,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A124,1),INDEX(LinMotor!$W$1:$W$1305,A124,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A124,1),INDEX(LinMotor!$X$1:$X$1305,A124,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A124<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A124,1),INDEX(LinMotor!$X$1:$X$1305,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A124,1),INDEX(LinMotor!$Z$1:$Z$1305,A124,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A124,1),INDEX(LinMotor!$X$1:$X$1305,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A124,1),INDEX(LinMotor!$Z$1:$Z$1305,A124,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A124,1),INDEX(LinMotor!$X$1:$X$1305,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A124,1),INDEX(LinMotor!$Z$1:$Z$1305,A124,1)))/1000,\"0.0k\")),\"\")","v":-13.304257800058384},{"$f":"IF(A124<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A124,1),INDEX(LinMotor!$Y$1:$Y$1305,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A124,1),INDEX(LinMotor!$AB$1:$AB$1305,A124,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A124,1),INDEX(LinMotor!$Y$1:$Y$1305,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A124,1),INDEX(LinMotor!$AB$1:$AB$1305,A124,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A124,1),INDEX(LinMotor!$Y$1:$Y$1305,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A124,1),INDEX(LinMotor!$AB$1:$AB$1305,A124,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A124,1),INDEX(LinMotor!$AD$1:$AD$1305,A124,1))","v":0.35118555158082226},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A124,1),INDEX(LinMotor!$AE$1:$AE$1305,A124,1))","v":0.49959405595685086},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A124,1),INDEX(LinMotor!$AF$1:$AF$1305,A124,1))","v":4.2142266189698674},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A124,1),INDEX(LinMotor!$AG$1:$AG$1305,A124,1))","v":11.990257342964421},{"$f":"IF(A124<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A124,1),INDEX(LinMotor!$AI$1:$AI$1305,A124,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A124,1),INDEX(LinMotor!$AI$1:$AI$1305,A124,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A124,1),INDEX(LinMotor!$AI$1:$AI$1305,A124,1))/1000,\"0.0k\")),\"\")","v":272.96463720033182},{"$f":"IF(A124<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A124,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A124,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A124,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A124,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A124,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A124,1))/1000,\"0.0k\")),\"\")","v":221.27663700720805},{"$f":"IF(A124<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A124,1),INDEX(LinMotor!$AK$1:$AK$1305,A124,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A124,1),INDEX(LinMotor!$AK$1:$AK$1305,A124,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A124,1),INDEX(LinMotor!$AK$1:$AK$1305,A124,1))/1000,\"0.0k\")),\"\")","v":"2.1k"},""]
[551,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A125,1),INDEX(LinMotor!$B$1:$B$1291,A125,1))","v":"AKM2G-54M 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A125,1),INDEX(LinMotor!$R$1:$R$1305,A125,1))","v":2.8735632549349721},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A125,1),INDEX(LinMotor!$S$1:$S$1305,A125,1))","v":0.30096544514562967},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A125,1),INDEX(LinMotor!$T$1:$T$1305,A125,1))","v":0.3002743948923311},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A125,1),INDEX(LinMotor!$U$1:$U$1305,A125,1))","v":1.0329520939809811},{"$f":"IF(A125<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A125,1),INDEX(LinMotor!$V$1:$V$1305,A125,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A125,1),INDEX(LinMotor!$V$1:$V$1305,A125,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A125,1),INDEX(LinMotor!$V$1:$V$1305,A125,1))/1000,\"0.0k\")),\"\")","v":16.425009629701709},{"$f":"IF(A125<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A125,1),INDEX(LinMotor!$W$1:$W$1305,A125,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A125,1),INDEX(LinMotor!$X$1:$X$1305,A125,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A125,1),INDEX(LinMotor!$W$1:$W$1305,A125,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A125,1),INDEX(LinMotor!$X$1:$X$1305,A125,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A125,1),INDEX(LinMotor!$W$1:$W$1305,A125,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A125,1),INDEX(LinMotor!$X$1:$X$1305,A125,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A125<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A125,1),INDEX(LinMotor!$X$1:$X$1305,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A125,1),INDEX(LinMotor!$Z$1:$Z$1305,A125,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A125,1),INDEX(LinMotor!$X$1:$X$1305,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A125,1),INDEX(LinMotor!$Z$1:$Z$1305,A125,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A125,1),INDEX(LinMotor!$X$1:$X$1305,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A125,1),INDEX(LinMotor!$Z$1:$Z$1305,A125,1)))/1000,\"0.0k\")),\"\")","v":-13.304257800058384},{"$f":"IF(A125<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A125,1),INDEX(LinMotor!$Y$1:$Y$1305,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A125,1),INDEX(LinMotor!$AB$1:$AB$1305,A125,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A125,1),INDEX(LinMotor!$Y$1:$Y$1305,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A125,1),INDEX(LinMotor!$AB$1:$AB$1305,A125,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A125,1),INDEX(LinMotor!$Y$1:$Y$1305,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A125,1),INDEX(LinMotor!$AB$1:$AB$1305,A125,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A125,1),INDEX(LinMotor!$AD$1:$AD$1305,A125,1))","v":0.35118555158082226},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A125,1),INDEX(LinMotor!$AE$1:$AE$1305,A125,1))","v":0.49959405595685086},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A125,1),INDEX(LinMotor!$AF$1:$AF$1305,A125,1))","v":4.2142266189698674},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A125,1),INDEX(LinMotor!$AG$1:$AG$1305,A125,1))","v":11.990257342964421},{"$f":"IF(A125<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A125,1),INDEX(LinMotor!$AI$1:$AI$1305,A125,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A125,1),INDEX(LinMotor!$AI$1:$AI$1305,A125,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A125,1),INDEX(LinMotor!$AI$1:$AI$1305,A125,1))/1000,\"0.0k\")),\"\")","v":272.96463720033188},{"$f":"IF(A125<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A125,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A125,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A125,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A125,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A125,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A125,1))/1000,\"0.0k\")),\"\")","v":221.27663700720805},{"$f":"IF(A125<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A125,1),INDEX(LinMotor!$AK$1:$AK$1305,A125,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A125,1),INDEX(LinMotor!$AK$1:$AK$1305,A125,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A125,1),INDEX(LinMotor!$AK$1:$AK$1305,A125,1))/1000,\"0.0k\")),\"\")","v":"2.1k"},""]
[552,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A126,1),INDEX(LinMotor!$B$1:$B$1291,A126,1))","v":"AKM2G-54M 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A126,1),INDEX(LinMotor!$R$1:$R$1305,A126,1))","v":2.8735632549349721},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A126,1),INDEX(LinMotor!$S$1:$S$1305,A126,1))","v":0.30320911484117419},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A126,1),INDEX(LinMotor!$T$1:$T$1305,A126,1))","v":0.3002743948923311},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A126,1),INDEX(LinMotor!$U$1:$U$1305,A126,1))","v":1.0329520939809811},{"$f":"IF(A126<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A126,1),INDEX(LinMotor!$V$1:$V$1305,A126,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A126,1),INDEX(LinMotor!$V$1:$V$1305,A126,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A126,1),INDEX(LinMotor!$V$1:$V$1305,A126,1))/1000,\"0.0k\")),\"\")","v":16.425009629701709},{"$f":"IF(A126<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A126,1),INDEX(LinMotor!$W$1:$W$1305,A126,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A126,1),INDEX(LinMotor!$X$1:$X$1305,A126,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A126,1),INDEX(LinMotor!$W$1:$W$1305,A126,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A126,1),INDEX(LinMotor!$X$1:$X$1305,A126,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A126,1),INDEX(LinMotor!$W$1:$W$1305,A126,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A126,1),INDEX(LinMotor!$X$1:$X$1305,A126,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A126<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A126,1),INDEX(LinMotor!$X$1:$X$1305,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A126,1),INDEX(LinMotor!$Z$1:$Z$1305,A126,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A126,1),INDEX(LinMotor!$X$1:$X$1305,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A126,1),INDEX(LinMotor!$Z$1:$Z$1305,A126,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A126,1),INDEX(LinMotor!$X$1:$X$1305,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A126,1),INDEX(LinMotor!$Z$1:$Z$1305,A126,1)))/1000,\"0.0k\")),\"\")","v":-13.304257800058384},{"$f":"IF(A126<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A126,1),INDEX(LinMotor!$Y$1:$Y$1305,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A126,1),INDEX(LinMotor!$AB$1:$AB$1305,A126,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A126,1),INDEX(LinMotor!$Y$1:$Y$1305,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A126,1),INDEX(LinMotor!$AB$1:$AB$1305,A126,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A126,1),INDEX(LinMotor!$Y$1:$Y$1305,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A126,1),INDEX(LinMotor!$AB$1:$AB$1305,A126,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A126,1),INDEX(LinMotor!$AD$1:$AD$1305,A126,1))","v":0.35118555158082226},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A126,1),INDEX(LinMotor!$AE$1:$AE$1305,A126,1))","v":0.49959405595685086},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A126,1),INDEX(LinMotor!$AF$1:$AF$1305,A126,1))","v":4.2142266189698674},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A126,1),INDEX(LinMotor!$AG$1:$AG$1305,A126,1))","v":11.990257342964421},{"$f":"IF(A126<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A126,1),INDEX(LinMotor!$AI$1:$AI$1305,A126,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A126,1),INDEX(LinMotor!$AI$1:$AI$1305,A126,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A126,1),INDEX(LinMotor!$AI$1:$AI$1305,A126,1))/1000,\"0.0k\")),\"\")","v":272.96463720033188},{"$f":"IF(A126<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A126,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A126,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A126,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A126,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A126,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A126,1))/1000,\"0.0k\")),\"\")","v":221.27663700720805},{"$f":"IF(A126<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A126,1),INDEX(LinMotor!$AK$1:$AK$1305,A126,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A126,1),INDEX(LinMotor!$AK$1:$AK$1305,A126,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A126,1),INDEX(LinMotor!$AK$1:$AK$1305,A126,1))/1000,\"0.0k\")),\"\")","v":"2.1k"},""]
[554,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A127,1),INDEX(LinMotor!$B$1:$B$1291,A127,1))","v":"AKM2G-54N 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A127,1),INDEX(LinMotor!$R$1:$R$1305,A127,1))","v":2.8735632549349721},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A127,1),INDEX(LinMotor!$S$1:$S$1305,A127,1))","v":0.29771459758902286},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A127,1),INDEX(LinMotor!$T$1:$T$1305,A127,1))","v":0.3002743948923311},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A127,1),INDEX(LinMotor!$U$1:$U$1305,A127,1))","v":0.92709690169207093},{"$f":"IF(A127<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A127,1),INDEX(LinMotor!$V$1:$V$1305,A127,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A127,1),INDEX(LinMotor!$V$1:$V$1305,A127,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A127,1),INDEX(LinMotor!$V$1:$V$1305,A127,1))/1000,\"0.0k\")),\"\")","v":16.425009629701709},{"$f":"IF(A127<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A127,1),INDEX(LinMotor!$W$1:$W$1305,A127,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A127,1),INDEX(LinMotor!$X$1:$X$1305,A127,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A127,1),INDEX(LinMotor!$W$1:$W$1305,A127,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A127,1),INDEX(LinMotor!$X$1:$X$1305,A127,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A127,1),INDEX(LinMotor!$W$1:$W$1305,A127,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A127,1),INDEX(LinMotor!$X$1:$X$1305,A127,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A127<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A127,1),INDEX(LinMotor!$X$1:$X$1305,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A127,1),INDEX(LinMotor!$Z$1:$Z$1305,A127,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A127,1),INDEX(LinMotor!$X$1:$X$1305,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A127,1),INDEX(LinMotor!$Z$1:$Z$1305,A127,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A127,1),INDEX(LinMotor!$X$1:$X$1305,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A127,1),INDEX(LinMotor!$Z$1:$Z$1305,A127,1)))/1000,\"0.0k\")),\"\")","v":-13.304257800058384},{"$f":"IF(A127<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A127,1),INDEX(LinMotor!$Y$1:$Y$1305,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A127,1),INDEX(LinMotor!$AB$1:$AB$1305,A127,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A127,1),INDEX(LinMotor!$Y$1:$Y$1305,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A127,1),INDEX(LinMotor!$AB$1:$AB$1305,A127,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A127,1),INDEX(LinMotor!$Y$1:$Y$1305,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A127,1),INDEX(LinMotor!$AB$1:$AB$1305,A127,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A127,1),INDEX(LinMotor!$AD$1:$AD$1305,A127,1))","v":0.39207699131976598},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A127,1),INDEX(LinMotor!$AE$1:$AE$1305,A127,1))","v":0.55776592590176921},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A127,1),INDEX(LinMotor!$AF$1:$AF$1305,A127,1))","v":4.7049238958371919},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A127,1),INDEX(LinMotor!$AG$1:$AG$1305,A127,1))","v":13.386382221642462},{"$f":"IF(A127<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A127,1),INDEX(LinMotor!$AI$1:$AI$1305,A127,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A127,1),INDEX(LinMotor!$AI$1:$AI$1305,A127,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A127,1),INDEX(LinMotor!$AI$1:$AI$1305,A127,1))/1000,\"0.0k\")),\"\")","v":272.96463720033188},{"$f":"IF(A127<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A127,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A127,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A127,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A127,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A127,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A127,1))/1000,\"0.0k\")),\"\")","v":221.27663700720805},{"$f":"IF(A127<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A127,1),INDEX(LinMotor!$AK$1:$AK$1305,A127,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A127,1),INDEX(LinMotor!$AK$1:$AK$1305,A127,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A127,1),INDEX(LinMotor!$AK$1:$AK$1305,A127,1))/1000,\"0.0k\")),\"\")","v":"2.1k"},""]
[555,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A128,1),INDEX(LinMotor!$B$1:$B$1291,A128,1))","v":"AKM2G-54N 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A128,1),INDEX(LinMotor!$R$1:$R$1305,A128,1))","v":2.8735632549349721},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A128,1),INDEX(LinMotor!$S$1:$S$1305,A128,1))","v":0.30223964438045714},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A128,1),INDEX(LinMotor!$T$1:$T$1305,A128,1))","v":0.3002743948923311},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A128,1),INDEX(LinMotor!$U$1:$U$1305,A128,1))","v":0.92709690169207093},{"$f":"IF(A128<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A128,1),INDEX(LinMotor!$V$1:$V$1305,A128,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A128,1),INDEX(LinMotor!$V$1:$V$1305,A128,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A128,1),INDEX(LinMotor!$V$1:$V$1305,A128,1))/1000,\"0.0k\")),\"\")","v":16.425009629701709},{"$f":"IF(A128<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A128,1),INDEX(LinMotor!$W$1:$W$1305,A128,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A128,1),INDEX(LinMotor!$X$1:$X$1305,A128,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A128,1),INDEX(LinMotor!$W$1:$W$1305,A128,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A128,1),INDEX(LinMotor!$X$1:$X$1305,A128,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A128,1),INDEX(LinMotor!$W$1:$W$1305,A128,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A128,1),INDEX(LinMotor!$X$1:$X$1305,A128,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A128<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A128,1),INDEX(LinMotor!$X$1:$X$1305,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A128,1),INDEX(LinMotor!$Z$1:$Z$1305,A128,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A128,1),INDEX(LinMotor!$X$1:$X$1305,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A128,1),INDEX(LinMotor!$Z$1:$Z$1305,A128,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A128,1),INDEX(LinMotor!$X$1:$X$1305,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A128,1),INDEX(LinMotor!$Z$1:$Z$1305,A128,1)))/1000,\"0.0k\")),\"\")","v":-13.304257800058384},{"$f":"IF(A128<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A128,1),INDEX(LinMotor!$Y$1:$Y$1305,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A128,1),INDEX(LinMotor!$AB$1:$AB$1305,A128,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A128,1),INDEX(LinMotor!$Y$1:$Y$1305,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A128,1),INDEX(LinMotor!$AB$1:$AB$1305,A128,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A128,1),INDEX(LinMotor!$Y$1:$Y$1305,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A128,1),INDEX(LinMotor!$AB$1:$AB$1305,A128,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A128,1),INDEX(LinMotor!$AD$1:$AD$1305,A128,1))","v":0.39207699131976598},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A128,1),INDEX(LinMotor!$AE$1:$AE$1305,A128,1))","v":0.55776592590176921},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A128,1),INDEX(LinMotor!$AF$1:$AF$1305,A128,1))","v":4.7049238958371919},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A128,1),INDEX(LinMotor!$AG$1:$AG$1305,A128,1))","v":13.386382221642462},{"$f":"IF(A128<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A128,1),INDEX(LinMotor!$AI$1:$AI$1305,A128,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A128,1),INDEX(LinMotor!$AI$1:$AI$1305,A128,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A128,1),INDEX(LinMotor!$AI$1:$AI$1305,A128,1))/1000,\"0.0k\")),\"\")","v":272.96463720033188},{"$f":"IF(A128<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A128,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A128,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A128,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A128,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A128,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A128,1))/1000,\"0.0k\")),\"\")","v":221.27663700720805},{"$f":"IF(A128<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A128,1),INDEX(LinMotor!$AK$1:$AK$1305,A128,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A128,1),INDEX(LinMotor!$AK$1:$AK$1305,A128,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A128,1),INDEX(LinMotor!$AK$1:$AK$1305,A128,1))/1000,\"0.0k\")),\"\")","v":"2.1k"},""]
[560,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A129,1),INDEX(LinMotor!$B$1:$B$1291,A129,1))","v":"AKM2G-62L 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A129,1),INDEX(LinMotor!$R$1:$R$1305,A129,1))","v":2.7472527397738253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A129,1),INDEX(LinMotor!$S$1:$S$1305,A129,1))","v":0.39145424345627228},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A129,1),INDEX(LinMotor!$T$1:$T$1305,A129,1))","v":0.44438408080690633},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A129,1),INDEX(LinMotor!$U$1:$U$1305,A129,1))","v":1.0909090909090908},{"$f":"IF(A129<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A129,1),INDEX(LinMotor!$V$1:$V$1305,A129,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A129,1),INDEX(LinMotor!$V$1:$V$1305,A129,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A129,1),INDEX(LinMotor!$V$1:$V$1305,A129,1))/1000,\"0.0k\")),\"\")","v":16.619965300254588},{"$f":"IF(A129<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A129,1),INDEX(LinMotor!$W$1:$W$1305,A129,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A129,1),INDEX(LinMotor!$X$1:$X$1305,A129,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A129,1),INDEX(LinMotor!$W$1:$W$1305,A129,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A129,1),INDEX(LinMotor!$X$1:$X$1305,A129,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A129,1),INDEX(LinMotor!$W$1:$W$1305,A129,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A129,1),INDEX(LinMotor!$X$1:$X$1305,A129,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A129<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A129,1),INDEX(LinMotor!$X$1:$X$1305,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A129,1),INDEX(LinMotor!$Z$1:$Z$1305,A129,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A129,1),INDEX(LinMotor!$X$1:$X$1305,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A129,1),INDEX(LinMotor!$Z$1:$Z$1305,A129,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A129,1),INDEX(LinMotor!$X$1:$X$1305,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A129,1),INDEX(LinMotor!$Z$1:$Z$1305,A129,1)))/1000,\"0.0k\")),\"\")","v":-13.462171893206216},{"$f":"IF(A129<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A129,1),INDEX(LinMotor!$Y$1:$Y$1305,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A129,1),INDEX(LinMotor!$AB$1:$AB$1305,A129,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A129,1),INDEX(LinMotor!$Y$1:$Y$1305,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A129,1),INDEX(LinMotor!$AB$1:$AB$1305,A129,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A129,1),INDEX(LinMotor!$Y$1:$Y$1305,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A129,1),INDEX(LinMotor!$AB$1:$AB$1305,A129,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A129,1),INDEX(LinMotor!$AD$1:$AD$1305,A129,1))","v":0.37149474032437096},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A129,1),INDEX(LinMotor!$AE$1:$AE$1305,A129,1))","v":0.52848576272528158},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A129,1),INDEX(LinMotor!$AF$1:$AF$1305,A129,1))","v":4.4579368838924518},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A129,1),INDEX(LinMotor!$AG$1:$AG$1305,A129,1))","v":12.683658305406757},{"$f":"IF(A129<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A129,1),INDEX(LinMotor!$AI$1:$AI$1305,A129,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A129,1),INDEX(LinMotor!$AI$1:$AI$1305,A129,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A129,1),INDEX(LinMotor!$AI$1:$AI$1305,A129,1))/1000,\"0.0k\")),\"\")","v":276.20457465439478},{"$f":"IF(A129<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A129,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A129,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A129,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A129,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A129,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A129,1))/1000,\"0.0k\")),\"\")","v":223.9030668308726},{"$f":"IF(A129<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A129,1),INDEX(LinMotor!$AK$1:$AK$1305,A129,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A129,1),INDEX(LinMotor!$AK$1:$AK$1305,A129,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A129,1),INDEX(LinMotor!$AK$1:$AK$1305,A129,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[561,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A130,1),INDEX(LinMotor!$B$1:$B$1291,A130,1))","v":"AKM2G-62L 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A130,1),INDEX(LinMotor!$R$1:$R$1305,A130,1))","v":2.7472527397738253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A130,1),INDEX(LinMotor!$S$1:$S$1305,A130,1))","v":0.3954225943476134},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A130,1),INDEX(LinMotor!$T$1:$T$1305,A130,1))","v":0.44438408080690633},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A130,1),INDEX(LinMotor!$U$1:$U$1305,A130,1))","v":1.0552318289827101},{"$f":"IF(A130<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A130,1),INDEX(LinMotor!$V$1:$V$1305,A130,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A130,1),INDEX(LinMotor!$V$1:$V$1305,A130,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A130,1),INDEX(LinMotor!$V$1:$V$1305,A130,1))/1000,\"0.0k\")),\"\")","v":16.619965300254588},{"$f":"IF(A130<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A130,1),INDEX(LinMotor!$W$1:$W$1305,A130,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A130,1),INDEX(LinMotor!$X$1:$X$1305,A130,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A130,1),INDEX(LinMotor!$W$1:$W$1305,A130,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A130,1),INDEX(LinMotor!$X$1:$X$1305,A130,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A130,1),INDEX(LinMotor!$W$1:$W$1305,A130,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A130,1),INDEX(LinMotor!$X$1:$X$1305,A130,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A130<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A130,1),INDEX(LinMotor!$X$1:$X$1305,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A130,1),INDEX(LinMotor!$Z$1:$Z$1305,A130,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A130,1),INDEX(LinMotor!$X$1:$X$1305,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A130,1),INDEX(LinMotor!$Z$1:$Z$1305,A130,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A130,1),INDEX(LinMotor!$X$1:$X$1305,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A130,1),INDEX(LinMotor!$Z$1:$Z$1305,A130,1)))/1000,\"0.0k\")),\"\")","v":-13.462171893206216},{"$f":"IF(A130<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A130,1),INDEX(LinMotor!$Y$1:$Y$1305,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A130,1),INDEX(LinMotor!$AB$1:$AB$1305,A130,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A130,1),INDEX(LinMotor!$Y$1:$Y$1305,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A130,1),INDEX(LinMotor!$AB$1:$AB$1305,A130,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A130,1),INDEX(LinMotor!$Y$1:$Y$1305,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A130,1),INDEX(LinMotor!$AB$1:$AB$1305,A130,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A130,1),INDEX(LinMotor!$AD$1:$AD$1305,A130,1))","v":0.37149474032437096},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A130,1),INDEX(LinMotor!$AE$1:$AE$1305,A130,1))","v":0.52848576272528158},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A130,1),INDEX(LinMotor!$AF$1:$AF$1305,A130,1))","v":4.4579368838924518},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A130,1),INDEX(LinMotor!$AG$1:$AG$1305,A130,1))","v":12.683658305406757},{"$f":"IF(A130<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A130,1),INDEX(LinMotor!$AI$1:$AI$1305,A130,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A130,1),INDEX(LinMotor!$AI$1:$AI$1305,A130,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A130,1),INDEX(LinMotor!$AI$1:$AI$1305,A130,1))/1000,\"0.0k\")),\"\")","v":276.20457465439478},{"$f":"IF(A130<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A130,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A130,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A130,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A130,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A130,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A130,1))/1000,\"0.0k\")),\"\")","v":223.9030668308726},{"$f":"IF(A130<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A130,1),INDEX(LinMotor!$AK$1:$AK$1305,A130,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A130,1),INDEX(LinMotor!$AK$1:$AK$1305,A130,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A130,1),INDEX(LinMotor!$AK$1:$AK$1305,A130,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[562,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A131,1),INDEX(LinMotor!$B$1:$B$1291,A131,1))","v":"AKM2G-62L 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A131,1),INDEX(LinMotor!$R$1:$R$1305,A131,1))","v":2.7472527397738253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A131,1),INDEX(LinMotor!$S$1:$S$1305,A131,1))","v":0.39746969938201571},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A131,1),INDEX(LinMotor!$T$1:$T$1305,A131,1))","v":0.44438408080690633},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A131,1),INDEX(LinMotor!$U$1:$U$1305,A131,1))","v":1.0552318289827101},{"$f":"IF(A131<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A131,1),INDEX(LinMotor!$V$1:$V$1305,A131,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A131,1),INDEX(LinMotor!$V$1:$V$1305,A131,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A131,1),INDEX(LinMotor!$V$1:$V$1305,A131,1))/1000,\"0.0k\")),\"\")","v":16.619965300254588},{"$f":"IF(A131<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A131,1),INDEX(LinMotor!$W$1:$W$1305,A131,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A131,1),INDEX(LinMotor!$X$1:$X$1305,A131,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A131,1),INDEX(LinMotor!$W$1:$W$1305,A131,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A131,1),INDEX(LinMotor!$X$1:$X$1305,A131,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A131,1),INDEX(LinMotor!$W$1:$W$1305,A131,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A131,1),INDEX(LinMotor!$X$1:$X$1305,A131,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A131<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A131,1),INDEX(LinMotor!$X$1:$X$1305,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A131,1),INDEX(LinMotor!$Z$1:$Z$1305,A131,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A131,1),INDEX(LinMotor!$X$1:$X$1305,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A131,1),INDEX(LinMotor!$Z$1:$Z$1305,A131,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A131,1),INDEX(LinMotor!$X$1:$X$1305,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A131,1),INDEX(LinMotor!$Z$1:$Z$1305,A131,1)))/1000,\"0.0k\")),\"\")","v":-13.462171893206216},{"$f":"IF(A131<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A131,1),INDEX(LinMotor!$Y$1:$Y$1305,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A131,1),INDEX(LinMotor!$AB$1:$AB$1305,A131,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A131,1),INDEX(LinMotor!$Y$1:$Y$1305,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A131,1),INDEX(LinMotor!$AB$1:$AB$1305,A131,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A131,1),INDEX(LinMotor!$Y$1:$Y$1305,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A131,1),INDEX(LinMotor!$AB$1:$AB$1305,A131,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A131,1),INDEX(LinMotor!$AD$1:$AD$1305,A131,1))","v":0.37149474032437096},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A131,1),INDEX(LinMotor!$AE$1:$AE$1305,A131,1))","v":0.52848576272528158},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A131,1),INDEX(LinMotor!$AF$1:$AF$1305,A131,1))","v":4.4579368838924518},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A131,1),INDEX(LinMotor!$AG$1:$AG$1305,A131,1))","v":12.683658305406757},{"$f":"IF(A131<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A131,1),INDEX(LinMotor!$AI$1:$AI$1305,A131,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A131,1),INDEX(LinMotor!$AI$1:$AI$1305,A131,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A131,1),INDEX(LinMotor!$AI$1:$AI$1305,A131,1))/1000,\"0.0k\")),\"\")","v":276.20457465439478},{"$f":"IF(A131<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A131,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A131,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A131,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A131,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A131,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A131,1))/1000,\"0.0k\")),\"\")","v":223.9030668308726},{"$f":"IF(A131<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A131,1),INDEX(LinMotor!$AK$1:$AK$1305,A131,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A131,1),INDEX(LinMotor!$AK$1:$AK$1305,A131,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A131,1),INDEX(LinMotor!$AK$1:$AK$1305,A131,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[564,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A132,1),INDEX(LinMotor!$B$1:$B$1291,A132,1))","v":"AKM2G-62M 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A132,1),INDEX(LinMotor!$R$1:$R$1305,A132,1))","v":2.7472527397738253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A132,1),INDEX(LinMotor!$S$1:$S$1305,A132,1))","v":0.39515881431459743},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A132,1),INDEX(LinMotor!$T$1:$T$1305,A132,1))","v":0.44438408080690633},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A132,1),INDEX(LinMotor!$U$1:$U$1305,A132,1))","v":0.8571428571428571},{"$f":"IF(A132<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A132,1),INDEX(LinMotor!$V$1:$V$1305,A132,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A132,1),INDEX(LinMotor!$V$1:$V$1305,A132,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A132,1),INDEX(LinMotor!$V$1:$V$1305,A132,1))/1000,\"0.0k\")),\"\")","v":16.619965300254588},{"$f":"IF(A132<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A132,1),INDEX(LinMotor!$W$1:$W$1305,A132,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A132,1),INDEX(LinMotor!$X$1:$X$1305,A132,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A132,1),INDEX(LinMotor!$W$1:$W$1305,A132,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A132,1),INDEX(LinMotor!$X$1:$X$1305,A132,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A132,1),INDEX(LinMotor!$W$1:$W$1305,A132,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A132,1),INDEX(LinMotor!$X$1:$X$1305,A132,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A132<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A132,1),INDEX(LinMotor!$X$1:$X$1305,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A132,1),INDEX(LinMotor!$Z$1:$Z$1305,A132,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A132,1),INDEX(LinMotor!$X$1:$X$1305,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A132,1),INDEX(LinMotor!$Z$1:$Z$1305,A132,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A132,1),INDEX(LinMotor!$X$1:$X$1305,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A132,1),INDEX(LinMotor!$Z$1:$Z$1305,A132,1)))/1000,\"0.0k\")),\"\")","v":-13.462171893206216},{"$f":"IF(A132<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A132,1),INDEX(LinMotor!$Y$1:$Y$1305,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A132,1),INDEX(LinMotor!$AB$1:$AB$1305,A132,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A132,1),INDEX(LinMotor!$Y$1:$Y$1305,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A132,1),INDEX(LinMotor!$AB$1:$AB$1305,A132,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A132,1),INDEX(LinMotor!$Y$1:$Y$1305,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A132,1),INDEX(LinMotor!$AB$1:$AB$1305,A132,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A132,1),INDEX(LinMotor!$AD$1:$AD$1305,A132,1))","v":0.47066744175875325},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A132,1),INDEX(LinMotor!$AE$1:$AE$1305,A132,1))","v":0.66956813905532886},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A132,1),INDEX(LinMotor!$AF$1:$AF$1305,A132,1))","v":5.6480093011050387},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A132,1),INDEX(LinMotor!$AG$1:$AG$1305,A132,1))","v":16.069635337327892},{"$f":"IF(A132<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A132,1),INDEX(LinMotor!$AI$1:$AI$1305,A132,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A132,1),INDEX(LinMotor!$AI$1:$AI$1305,A132,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A132,1),INDEX(LinMotor!$AI$1:$AI$1305,A132,1))/1000,\"0.0k\")),\"\")","v":276.20457465439478},{"$f":"IF(A132<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A132,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A132,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A132,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A132,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A132,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A132,1))/1000,\"0.0k\")),\"\")","v":223.9030668308726},{"$f":"IF(A132<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A132,1),INDEX(LinMotor!$AK$1:$AK$1305,A132,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A132,1),INDEX(LinMotor!$AK$1:$AK$1305,A132,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A132,1),INDEX(LinMotor!$AK$1:$AK$1305,A132,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[565,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A133,1),INDEX(LinMotor!$B$1:$B$1291,A133,1))","v":"AKM2G-62M 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A133,1),INDEX(LinMotor!$R$1:$R$1305,A133,1))","v":2.7472527397738253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A133,1),INDEX(LinMotor!$S$1:$S$1305,A133,1))","v":0.39999017343510934},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A133,1),INDEX(LinMotor!$T$1:$T$1305,A133,1))","v":0.44438408080690633},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A133,1),INDEX(LinMotor!$U$1:$U$1305,A133,1))","v":0.83856135442558821},{"$f":"IF(A133<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A133,1),INDEX(LinMotor!$V$1:$V$1305,A133,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A133,1),INDEX(LinMotor!$V$1:$V$1305,A133,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A133,1),INDEX(LinMotor!$V$1:$V$1305,A133,1))/1000,\"0.0k\")),\"\")","v":16.619965300254588},{"$f":"IF(A133<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A133,1),INDEX(LinMotor!$W$1:$W$1305,A133,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A133,1),INDEX(LinMotor!$X$1:$X$1305,A133,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A133,1),INDEX(LinMotor!$W$1:$W$1305,A133,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A133,1),INDEX(LinMotor!$X$1:$X$1305,A133,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A133,1),INDEX(LinMotor!$W$1:$W$1305,A133,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A133,1),INDEX(LinMotor!$X$1:$X$1305,A133,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A133<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A133,1),INDEX(LinMotor!$X$1:$X$1305,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A133,1),INDEX(LinMotor!$Z$1:$Z$1305,A133,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A133,1),INDEX(LinMotor!$X$1:$X$1305,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A133,1),INDEX(LinMotor!$Z$1:$Z$1305,A133,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A133,1),INDEX(LinMotor!$X$1:$X$1305,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A133,1),INDEX(LinMotor!$Z$1:$Z$1305,A133,1)))/1000,\"0.0k\")),\"\")","v":-13.462171893206216},{"$f":"IF(A133<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A133,1),INDEX(LinMotor!$Y$1:$Y$1305,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A133,1),INDEX(LinMotor!$AB$1:$AB$1305,A133,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A133,1),INDEX(LinMotor!$Y$1:$Y$1305,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A133,1),INDEX(LinMotor!$AB$1:$AB$1305,A133,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A133,1),INDEX(LinMotor!$Y$1:$Y$1305,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A133,1),INDEX(LinMotor!$AB$1:$AB$1305,A133,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A133,1),INDEX(LinMotor!$AD$1:$AD$1305,A133,1))","v":0.47066744175875325},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A133,1),INDEX(LinMotor!$AE$1:$AE$1305,A133,1))","v":0.66956813905532886},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A133,1),INDEX(LinMotor!$AF$1:$AF$1305,A133,1))","v":5.6480093011050387},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A133,1),INDEX(LinMotor!$AG$1:$AG$1305,A133,1))","v":16.069635337327892},{"$f":"IF(A133<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A133,1),INDEX(LinMotor!$AI$1:$AI$1305,A133,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A133,1),INDEX(LinMotor!$AI$1:$AI$1305,A133,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A133,1),INDEX(LinMotor!$AI$1:$AI$1305,A133,1))/1000,\"0.0k\")),\"\")","v":276.20457465439478},{"$f":"IF(A133<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A133,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A133,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A133,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A133,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A133,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A133,1))/1000,\"0.0k\")),\"\")","v":223.9030668308726},{"$f":"IF(A133<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A133,1),INDEX(LinMotor!$AK$1:$AK$1305,A133,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A133,1),INDEX(LinMotor!$AK$1:$AK$1305,A133,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A133,1),INDEX(LinMotor!$AK$1:$AK$1305,A133,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[570,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A134,1),INDEX(LinMotor!$B$1:$B$1291,A134,1))","v":"AKM2G-63M 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A134,1),INDEX(LinMotor!$R$1:$R$1305,A134,1))","v":1.9230769178416716},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A134,1),INDEX(LinMotor!$S$1:$S$1305,A134,1))","v":0.31123355295030775},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A134,1),INDEX(LinMotor!$T$1:$T$1305,A134,1))","v":0.33983087063899553},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A134,1),INDEX(LinMotor!$U$1:$U$1305,A134,1))","v":1.1428571428571428},{"$f":"IF(A134<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A134,1),INDEX(LinMotor!$V$1:$V$1305,A134,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A134,1),INDEX(LinMotor!$V$1:$V$1305,A134,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A134,1),INDEX(LinMotor!$V$1:$V$1305,A134,1))/1000,\"0.0k\")),\"\")","v":18.520782449825255},{"$f":"IF(A134<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A134,1),INDEX(LinMotor!$W$1:$W$1305,A134,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A134,1),INDEX(LinMotor!$X$1:$X$1305,A134,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A134,1),INDEX(LinMotor!$W$1:$W$1305,A134,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A134,1),INDEX(LinMotor!$X$1:$X$1305,A134,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A134,1),INDEX(LinMotor!$W$1:$W$1305,A134,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A134,1),INDEX(LinMotor!$X$1:$X$1305,A134,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A134<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A134,1),INDEX(LinMotor!$X$1:$X$1305,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A134,1),INDEX(LinMotor!$Z$1:$Z$1305,A134,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A134,1),INDEX(LinMotor!$X$1:$X$1305,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A134,1),INDEX(LinMotor!$Z$1:$Z$1305,A134,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A134,1),INDEX(LinMotor!$X$1:$X$1305,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A134,1),INDEX(LinMotor!$Z$1:$Z$1305,A134,1)))/1000,\"0.0k\")),\"\")","v":-15.001833784358457},{"$f":"IF(A134<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A134,1),INDEX(LinMotor!$Y$1:$Y$1305,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A134,1),INDEX(LinMotor!$AB$1:$AB$1305,A134,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A134,1),INDEX(LinMotor!$Y$1:$Y$1305,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A134,1),INDEX(LinMotor!$AB$1:$AB$1305,A134,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A134,1),INDEX(LinMotor!$Y$1:$Y$1305,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A134,1),INDEX(LinMotor!$AB$1:$AB$1305,A134,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A134,1),INDEX(LinMotor!$AD$1:$AD$1305,A134,1))","v":0.3852984686408169},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A134,1),INDEX(LinMotor!$AE$1:$AE$1305,A134,1))","v":0.54812284798091604},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A134,1),INDEX(LinMotor!$AF$1:$AF$1305,A134,1))","v":4.6235816236898026},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A134,1),INDEX(LinMotor!$AG$1:$AG$1305,A134,1))","v":13.154948351541986},{"$f":"IF(A134<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A134,1),INDEX(LinMotor!$AI$1:$AI$1305,A134,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A134,1),INDEX(LinMotor!$AI$1:$AI$1305,A134,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A134,1),INDEX(LinMotor!$AI$1:$AI$1305,A134,1))/1000,\"0.0k\")),\"\")","v":307.79395422337035},{"$f":"IF(A134<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A134,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A134,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A134,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A134,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A134,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A134,1))/1000,\"0.0k\")),\"\")","v":249.51074901219886},{"$f":"IF(A134<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A134,1),INDEX(LinMotor!$AK$1:$AK$1305,A134,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A134,1),INDEX(LinMotor!$AK$1:$AK$1305,A134,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A134,1),INDEX(LinMotor!$AK$1:$AK$1305,A134,1))/1000,\"0.0k\")),\"\")","v":"2.4k"},""]
[571,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A135,1),INDEX(LinMotor!$B$1:$B$1291,A135,1))","v":"AKM2G-63M 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A135,1),INDEX(LinMotor!$R$1:$R$1305,A135,1))","v":1.9230769178416716},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A135,1),INDEX(LinMotor!$S$1:$S$1305,A135,1))","v":0.3148910848964116},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A135,1),INDEX(LinMotor!$T$1:$T$1305,A135,1))","v":0.33983087063899553},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A135,1),INDEX(LinMotor!$U$1:$U$1305,A135,1))","v":1.0858738243009276},{"$f":"IF(A135<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A135,1),INDEX(LinMotor!$V$1:$V$1305,A135,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A135,1),INDEX(LinMotor!$V$1:$V$1305,A135,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A135,1),INDEX(LinMotor!$V$1:$V$1305,A135,1))/1000,\"0.0k\")),\"\")","v":18.520782449825255},{"$f":"IF(A135<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A135,1),INDEX(LinMotor!$W$1:$W$1305,A135,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A135,1),INDEX(LinMotor!$X$1:$X$1305,A135,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A135,1),INDEX(LinMotor!$W$1:$W$1305,A135,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A135,1),INDEX(LinMotor!$X$1:$X$1305,A135,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A135,1),INDEX(LinMotor!$W$1:$W$1305,A135,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A135,1),INDEX(LinMotor!$X$1:$X$1305,A135,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A135<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A135,1),INDEX(LinMotor!$X$1:$X$1305,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A135,1),INDEX(LinMotor!$Z$1:$Z$1305,A135,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A135,1),INDEX(LinMotor!$X$1:$X$1305,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A135,1),INDEX(LinMotor!$Z$1:$Z$1305,A135,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A135,1),INDEX(LinMotor!$X$1:$X$1305,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A135,1),INDEX(LinMotor!$Z$1:$Z$1305,A135,1)))/1000,\"0.0k\")),\"\")","v":-15.001833784358457},{"$f":"IF(A135<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A135,1),INDEX(LinMotor!$Y$1:$Y$1305,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A135,1),INDEX(LinMotor!$AB$1:$AB$1305,A135,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A135,1),INDEX(LinMotor!$Y$1:$Y$1305,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A135,1),INDEX(LinMotor!$AB$1:$AB$1305,A135,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A135,1),INDEX(LinMotor!$Y$1:$Y$1305,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A135,1),INDEX(LinMotor!$AB$1:$AB$1305,A135,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A135,1),INDEX(LinMotor!$AD$1:$AD$1305,A135,1))","v":0.3852984686408169},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A135,1),INDEX(LinMotor!$AE$1:$AE$1305,A135,1))","v":0.54812284798091604},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A135,1),INDEX(LinMotor!$AF$1:$AF$1305,A135,1))","v":4.6235816236898026},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A135,1),INDEX(LinMotor!$AG$1:$AG$1305,A135,1))","v":13.154948351541986},{"$f":"IF(A135<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A135,1),INDEX(LinMotor!$AI$1:$AI$1305,A135,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A135,1),INDEX(LinMotor!$AI$1:$AI$1305,A135,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A135,1),INDEX(LinMotor!$AI$1:$AI$1305,A135,1))/1000,\"0.0k\")),\"\")","v":307.79395422337029},{"$f":"IF(A135<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A135,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A135,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A135,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A135,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A135,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A135,1))/1000,\"0.0k\")),\"\")","v":249.51074901219886},{"$f":"IF(A135<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A135,1),INDEX(LinMotor!$AK$1:$AK$1305,A135,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A135,1),INDEX(LinMotor!$AK$1:$AK$1305,A135,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A135,1),INDEX(LinMotor!$AK$1:$AK$1305,A135,1))/1000,\"0.0k\")),\"\")","v":"2.4k"},""]
[572,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A136,1),INDEX(LinMotor!$B$1:$B$1291,A136,1))","v":"AKM2G-63M 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A136,1),INDEX(LinMotor!$R$1:$R$1305,A136,1))","v":1.9230769178416716},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A136,1),INDEX(LinMotor!$S$1:$S$1305,A136,1))","v":0.31690390990790446},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A136,1),INDEX(LinMotor!$T$1:$T$1305,A136,1))","v":0.33983087063899553},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A136,1),INDEX(LinMotor!$U$1:$U$1305,A136,1))","v":1.0858738243009276},{"$f":"IF(A136<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A136,1),INDEX(LinMotor!$V$1:$V$1305,A136,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A136,1),INDEX(LinMotor!$V$1:$V$1305,A136,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A136,1),INDEX(LinMotor!$V$1:$V$1305,A136,1))/1000,\"0.0k\")),\"\")","v":18.520782449825255},{"$f":"IF(A136<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A136,1),INDEX(LinMotor!$W$1:$W$1305,A136,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A136,1),INDEX(LinMotor!$X$1:$X$1305,A136,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A136,1),INDEX(LinMotor!$W$1:$W$1305,A136,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A136,1),INDEX(LinMotor!$X$1:$X$1305,A136,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A136,1),INDEX(LinMotor!$W$1:$W$1305,A136,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A136,1),INDEX(LinMotor!$X$1:$X$1305,A136,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A136<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A136,1),INDEX(LinMotor!$X$1:$X$1305,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A136,1),INDEX(LinMotor!$Z$1:$Z$1305,A136,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A136,1),INDEX(LinMotor!$X$1:$X$1305,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A136,1),INDEX(LinMotor!$Z$1:$Z$1305,A136,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A136,1),INDEX(LinMotor!$X$1:$X$1305,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A136,1),INDEX(LinMotor!$Z$1:$Z$1305,A136,1)))/1000,\"0.0k\")),\"\")","v":-15.001833784358457},{"$f":"IF(A136<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A136,1),INDEX(LinMotor!$Y$1:$Y$1305,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A136,1),INDEX(LinMotor!$AB$1:$AB$1305,A136,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A136,1),INDEX(LinMotor!$Y$1:$Y$1305,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A136,1),INDEX(LinMotor!$AB$1:$AB$1305,A136,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A136,1),INDEX(LinMotor!$Y$1:$Y$1305,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A136,1),INDEX(LinMotor!$AB$1:$AB$1305,A136,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A136,1),INDEX(LinMotor!$AD$1:$AD$1305,A136,1))","v":0.3852984686408169},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A136,1),INDEX(LinMotor!$AE$1:$AE$1305,A136,1))","v":0.54812284798091604},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A136,1),INDEX(LinMotor!$AF$1:$AF$1305,A136,1))","v":4.6235816236898026},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A136,1),INDEX(LinMotor!$AG$1:$AG$1305,A136,1))","v":13.154948351541986},{"$f":"IF(A136<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A136,1),INDEX(LinMotor!$AI$1:$AI$1305,A136,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A136,1),INDEX(LinMotor!$AI$1:$AI$1305,A136,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A136,1),INDEX(LinMotor!$AI$1:$AI$1305,A136,1))/1000,\"0.0k\")),\"\")","v":307.79395422337035},{"$f":"IF(A136<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A136,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A136,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A136,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A136,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A136,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A136,1))/1000,\"0.0k\")),\"\")","v":249.51074901219886},{"$f":"IF(A136<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A136,1),INDEX(LinMotor!$AK$1:$AK$1305,A136,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A136,1),INDEX(LinMotor!$AK$1:$AK$1305,A136,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A136,1),INDEX(LinMotor!$AK$1:$AK$1305,A136,1))/1000,\"0.0k\")),\"\")","v":"2.4k"},""]
[574,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A137,1),INDEX(LinMotor!$B$1:$B$1291,A137,1))","v":"AKM2G-63N 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A137,1),INDEX(LinMotor!$R$1:$R$1305,A137,1))","v":1.9230769178416716},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A137,1),INDEX(LinMotor!$S$1:$S$1305,A137,1))","v":0.3118320248303551},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A137,1),INDEX(LinMotor!$T$1:$T$1305,A137,1))","v":0.33983087063899553},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A137,1),INDEX(LinMotor!$U$1:$U$1305,A137,1))","v":1.0434782608695652},{"$f":"IF(A137<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A137,1),INDEX(LinMotor!$V$1:$V$1305,A137,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A137,1),INDEX(LinMotor!$V$1:$V$1305,A137,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A137,1),INDEX(LinMotor!$V$1:$V$1305,A137,1))/1000,\"0.0k\")),\"\")","v":18.520782449825255},{"$f":"IF(A137<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A137,1),INDEX(LinMotor!$W$1:$W$1305,A137,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A137,1),INDEX(LinMotor!$X$1:$X$1305,A137,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A137,1),INDEX(LinMotor!$W$1:$W$1305,A137,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A137,1),INDEX(LinMotor!$X$1:$X$1305,A137,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A137,1),INDEX(LinMotor!$W$1:$W$1305,A137,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A137,1),INDEX(LinMotor!$X$1:$X$1305,A137,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A137<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A137,1),INDEX(LinMotor!$X$1:$X$1305,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A137,1),INDEX(LinMotor!$Z$1:$Z$1305,A137,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A137,1),INDEX(LinMotor!$X$1:$X$1305,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A137,1),INDEX(LinMotor!$Z$1:$Z$1305,A137,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A137,1),INDEX(LinMotor!$X$1:$X$1305,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A137,1),INDEX(LinMotor!$Z$1:$Z$1305,A137,1)))/1000,\"0.0k\")),\"\")","v":-15.001833784358457},{"$f":"IF(A137<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A137,1),INDEX(LinMotor!$Y$1:$Y$1305,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A137,1),INDEX(LinMotor!$AB$1:$AB$1305,A137,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A137,1),INDEX(LinMotor!$Y$1:$Y$1305,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A137,1),INDEX(LinMotor!$AB$1:$AB$1305,A137,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A137,1),INDEX(LinMotor!$Y$1:$Y$1305,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A137,1),INDEX(LinMotor!$AB$1:$AB$1305,A137,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A137,1),INDEX(LinMotor!$AD$1:$AD$1305,A137,1))","v":0.42585618818631188},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A137,1),INDEX(LinMotor!$AE$1:$AE$1305,A137,1))","v":0.60581996996354148},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A137,1),INDEX(LinMotor!$AF$1:$AF$1305,A137,1))","v":5.1102742582357426},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A137,1),INDEX(LinMotor!$AG$1:$AG$1305,A137,1))","v":14.539679279124995},{"$f":"IF(A137<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A137,1),INDEX(LinMotor!$AI$1:$AI$1305,A137,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A137,1),INDEX(LinMotor!$AI$1:$AI$1305,A137,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A137,1),INDEX(LinMotor!$AI$1:$AI$1305,A137,1))/1000,\"0.0k\")),\"\")","v":307.79395422337035},{"$f":"IF(A137<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A137,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A137,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A137,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A137,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A137,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A137,1))/1000,\"0.0k\")),\"\")","v":249.51074901219886},{"$f":"IF(A137<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A137,1),INDEX(LinMotor!$AK$1:$AK$1305,A137,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A137,1),INDEX(LinMotor!$AK$1:$AK$1305,A137,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A137,1),INDEX(LinMotor!$AK$1:$AK$1305,A137,1))/1000,\"0.0k\")),\"\")","v":"2.4k"},""]
[575,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A138,1),INDEX(LinMotor!$B$1:$B$1291,A138,1))","v":"AKM2G-63N 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A138,1),INDEX(LinMotor!$R$1:$R$1305,A138,1))","v":1.9230769178416716},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A138,1),INDEX(LinMotor!$S$1:$S$1305,A138,1))","v":0.3159919187069915},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A138,1),INDEX(LinMotor!$T$1:$T$1305,A138,1))","v":0.33983087063899553},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A138,1),INDEX(LinMotor!$U$1:$U$1305,A138,1))","v":0.97518652382892745},{"$f":"IF(A138<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A138,1),INDEX(LinMotor!$V$1:$V$1305,A138,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A138,1),INDEX(LinMotor!$V$1:$V$1305,A138,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A138,1),INDEX(LinMotor!$V$1:$V$1305,A138,1))/1000,\"0.0k\")),\"\")","v":18.520782449825255},{"$f":"IF(A138<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A138,1),INDEX(LinMotor!$W$1:$W$1305,A138,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A138,1),INDEX(LinMotor!$X$1:$X$1305,A138,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A138,1),INDEX(LinMotor!$W$1:$W$1305,A138,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A138,1),INDEX(LinMotor!$X$1:$X$1305,A138,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A138,1),INDEX(LinMotor!$W$1:$W$1305,A138,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A138,1),INDEX(LinMotor!$X$1:$X$1305,A138,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A138<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A138,1),INDEX(LinMotor!$X$1:$X$1305,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A138,1),INDEX(LinMotor!$Z$1:$Z$1305,A138,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A138,1),INDEX(LinMotor!$X$1:$X$1305,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A138,1),INDEX(LinMotor!$Z$1:$Z$1305,A138,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A138,1),INDEX(LinMotor!$X$1:$X$1305,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A138,1),INDEX(LinMotor!$Z$1:$Z$1305,A138,1)))/1000,\"0.0k\")),\"\")","v":-15.001833784358457},{"$f":"IF(A138<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A138,1),INDEX(LinMotor!$Y$1:$Y$1305,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A138,1),INDEX(LinMotor!$AB$1:$AB$1305,A138,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A138,1),INDEX(LinMotor!$Y$1:$Y$1305,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A138,1),INDEX(LinMotor!$AB$1:$AB$1305,A138,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A138,1),INDEX(LinMotor!$Y$1:$Y$1305,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A138,1),INDEX(LinMotor!$AB$1:$AB$1305,A138,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A138,1),INDEX(LinMotor!$AD$1:$AD$1305,A138,1))","v":0.42585618818631188},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A138,1),INDEX(LinMotor!$AE$1:$AE$1305,A138,1))","v":0.60581996996354148},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A138,1),INDEX(LinMotor!$AF$1:$AF$1305,A138,1))","v":5.1102742582357426},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A138,1),INDEX(LinMotor!$AG$1:$AG$1305,A138,1))","v":14.539679279124995},{"$f":"IF(A138<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A138,1),INDEX(LinMotor!$AI$1:$AI$1305,A138,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A138,1),INDEX(LinMotor!$AI$1:$AI$1305,A138,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A138,1),INDEX(LinMotor!$AI$1:$AI$1305,A138,1))/1000,\"0.0k\")),\"\")","v":307.79395422337035},{"$f":"IF(A138<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A138,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A138,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A138,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A138,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A138,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A138,1))/1000,\"0.0k\")),\"\")","v":249.51074901219886},{"$f":"IF(A138<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A138,1),INDEX(LinMotor!$AK$1:$AK$1305,A138,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A138,1),INDEX(LinMotor!$AK$1:$AK$1305,A138,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A138,1),INDEX(LinMotor!$AK$1:$AK$1305,A138,1))/1000,\"0.0k\")),\"\")","v":"2.4k"},""]
[583,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A139,1),INDEX(LinMotor!$B$1:$B$1291,A139,1))","v":"AKM2G-64N 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A139,1),INDEX(LinMotor!$R$1:$R$1305,A139,1))","v":1.4792899877515946},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A139,1),INDEX(LinMotor!$S$1:$S$1305,A139,1))","v":0.27481389151094343},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A139,1),INDEX(LinMotor!$T$1:$T$1305,A139,1))","v":0.29049215404248119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A139,1),INDEX(LinMotor!$U$1:$U$1305,A139,1))","v":1.2},{"$f":"IF(A139<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A139,1),INDEX(LinMotor!$V$1:$V$1305,A139,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A139,1),INDEX(LinMotor!$V$1:$V$1305,A139,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A139,1),INDEX(LinMotor!$V$1:$V$1305,A139,1))/1000,\"0.0k\")),\"\")","v":20.421599315698124},{"$f":"IF(A139<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A139,1),INDEX(LinMotor!$W$1:$W$1305,A139,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A139,1),INDEX(LinMotor!$X$1:$X$1305,A139,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A139,1),INDEX(LinMotor!$W$1:$W$1305,A139,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A139,1),INDEX(LinMotor!$X$1:$X$1305,A139,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A139,1),INDEX(LinMotor!$W$1:$W$1305,A139,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A139,1),INDEX(LinMotor!$X$1:$X$1305,A139,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A139<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A139,1),INDEX(LinMotor!$X$1:$X$1305,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A139,1),INDEX(LinMotor!$Z$1:$Z$1305,A139,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A139,1),INDEX(LinMotor!$X$1:$X$1305,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A139,1),INDEX(LinMotor!$Z$1:$Z$1305,A139,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A139,1),INDEX(LinMotor!$X$1:$X$1305,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A139,1),INDEX(LinMotor!$Z$1:$Z$1305,A139,1)))/1000,\"0.0k\")),\"\")","v":-16.541495445715483},{"$f":"IF(A139<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A139,1),INDEX(LinMotor!$Y$1:$Y$1305,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A139,1),INDEX(LinMotor!$AB$1:$AB$1305,A139,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A139,1),INDEX(LinMotor!$Y$1:$Y$1305,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A139,1),INDEX(LinMotor!$AB$1:$AB$1305,A139,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A139,1),INDEX(LinMotor!$Y$1:$Y$1305,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A139,1),INDEX(LinMotor!$AB$1:$AB$1305,A139,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A139,1),INDEX(LinMotor!$AD$1:$AD$1305,A139,1))","v":0.39726754672536085},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A139,1),INDEX(LinMotor!$AE$1:$AE$1305,A139,1))","v":0.56514997292784142},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A139,1),INDEX(LinMotor!$AF$1:$AF$1305,A139,1))","v":4.7672105607043305},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A139,1),INDEX(LinMotor!$AG$1:$AG$1305,A139,1))","v":13.563599350268193},{"$f":"IF(A139<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A139,1),INDEX(LinMotor!$AI$1:$AI$1305,A139,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A139,1),INDEX(LinMotor!$AI$1:$AI$1305,A139,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A139,1),INDEX(LinMotor!$AI$1:$AI$1305,A139,1))/1000,\"0.0k\")),\"\")","v":339.38332907761708},{"$f":"IF(A139<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A139,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A139,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A139,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A139,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A139,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A139,1))/1000,\"0.0k\")),\"\")","v":275.11842737156735},{"$f":"IF(A139<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A139,1),INDEX(LinMotor!$AK$1:$AK$1305,A139,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A139,1),INDEX(LinMotor!$AK$1:$AK$1305,A139,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A139,1),INDEX(LinMotor!$AK$1:$AK$1305,A139,1))/1000,\"0.0k\")),\"\")","v":"2.6k"},""]
[584,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A140,1),INDEX(LinMotor!$B$1:$B$1291,A140,1))","v":"AKM2G-64N 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A140,1),INDEX(LinMotor!$R$1:$R$1305,A140,1))","v":1.4792899877515946},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A140,1),INDEX(LinMotor!$S$1:$S$1305,A140,1))","v":0.27876866103213371},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A140,1),INDEX(LinMotor!$T$1:$T$1305,A140,1))","v":0.29049215404248119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A140,1),INDEX(LinMotor!$U$1:$U$1305,A140,1))","v":1.1366603728856379},{"$f":"IF(A140<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A140,1),INDEX(LinMotor!$V$1:$V$1305,A140,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A140,1),INDEX(LinMotor!$V$1:$V$1305,A140,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A140,1),INDEX(LinMotor!$V$1:$V$1305,A140,1))/1000,\"0.0k\")),\"\")","v":20.421599315698124},{"$f":"IF(A140<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A140,1),INDEX(LinMotor!$W$1:$W$1305,A140,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A140,1),INDEX(LinMotor!$X$1:$X$1305,A140,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A140,1),INDEX(LinMotor!$W$1:$W$1305,A140,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A140,1),INDEX(LinMotor!$X$1:$X$1305,A140,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A140,1),INDEX(LinMotor!$W$1:$W$1305,A140,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A140,1),INDEX(LinMotor!$X$1:$X$1305,A140,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A140<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A140,1),INDEX(LinMotor!$X$1:$X$1305,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A140,1),INDEX(LinMotor!$Z$1:$Z$1305,A140,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A140,1),INDEX(LinMotor!$X$1:$X$1305,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A140,1),INDEX(LinMotor!$Z$1:$Z$1305,A140,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A140,1),INDEX(LinMotor!$X$1:$X$1305,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A140,1),INDEX(LinMotor!$Z$1:$Z$1305,A140,1)))/1000,\"0.0k\")),\"\")","v":-16.541495445715483},{"$f":"IF(A140<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A140,1),INDEX(LinMotor!$Y$1:$Y$1305,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A140,1),INDEX(LinMotor!$AB$1:$AB$1305,A140,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A140,1),INDEX(LinMotor!$Y$1:$Y$1305,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A140,1),INDEX(LinMotor!$AB$1:$AB$1305,A140,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A140,1),INDEX(LinMotor!$Y$1:$Y$1305,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A140,1),INDEX(LinMotor!$AB$1:$AB$1305,A140,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A140,1),INDEX(LinMotor!$AD$1:$AD$1305,A140,1))","v":0.39726754672536085},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A140,1),INDEX(LinMotor!$AE$1:$AE$1305,A140,1))","v":0.56514997292784142},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A140,1),INDEX(LinMotor!$AF$1:$AF$1305,A140,1))","v":4.7672105607043305},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A140,1),INDEX(LinMotor!$AG$1:$AG$1305,A140,1))","v":13.563599350268193},{"$f":"IF(A140<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A140,1),INDEX(LinMotor!$AI$1:$AI$1305,A140,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A140,1),INDEX(LinMotor!$AI$1:$AI$1305,A140,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A140,1),INDEX(LinMotor!$AI$1:$AI$1305,A140,1))/1000,\"0.0k\")),\"\")","v":339.38332907761708},{"$f":"IF(A140<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A140,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A140,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A140,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A140,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A140,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A140,1))/1000,\"0.0k\")),\"\")","v":275.11842737156735},{"$f":"IF(A140<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A140,1),INDEX(LinMotor!$AK$1:$AK$1305,A140,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A140,1),INDEX(LinMotor!$AK$1:$AK$1305,A140,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A140,1),INDEX(LinMotor!$AK$1:$AK$1305,A140,1))/1000,\"0.0k\")),\"\")","v":"2.6k"},""]
[585,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A141,1),INDEX(LinMotor!$B$1:$B$1291,A141,1))","v":"AKM2G-64N 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A141,1),INDEX(LinMotor!$R$1:$R$1305,A141,1))","v":1.4792899877515946},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A141,1),INDEX(LinMotor!$S$1:$S$1305,A141,1))","v":0.28093225000741556},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A141,1),INDEX(LinMotor!$T$1:$T$1305,A141,1))","v":0.29049215404248119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A141,1),INDEX(LinMotor!$U$1:$U$1305,A141,1))","v":1.1366603728856379},{"$f":"IF(A141<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A141,1),INDEX(LinMotor!$V$1:$V$1305,A141,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A141,1),INDEX(LinMotor!$V$1:$V$1305,A141,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A141,1),INDEX(LinMotor!$V$1:$V$1305,A141,1))/1000,\"0.0k\")),\"\")","v":20.421599315698124},{"$f":"IF(A141<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A141,1),INDEX(LinMotor!$W$1:$W$1305,A141,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A141,1),INDEX(LinMotor!$X$1:$X$1305,A141,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A141,1),INDEX(LinMotor!$W$1:$W$1305,A141,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A141,1),INDEX(LinMotor!$X$1:$X$1305,A141,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A141,1),INDEX(LinMotor!$W$1:$W$1305,A141,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A141,1),INDEX(LinMotor!$X$1:$X$1305,A141,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A141<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A141,1),INDEX(LinMotor!$X$1:$X$1305,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A141,1),INDEX(LinMotor!$Z$1:$Z$1305,A141,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A141,1),INDEX(LinMotor!$X$1:$X$1305,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A141,1),INDEX(LinMotor!$Z$1:$Z$1305,A141,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A141,1),INDEX(LinMotor!$X$1:$X$1305,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A141,1),INDEX(LinMotor!$Z$1:$Z$1305,A141,1)))/1000,\"0.0k\")),\"\")","v":-16.541495445715483},{"$f":"IF(A141<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A141,1),INDEX(LinMotor!$Y$1:$Y$1305,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A141,1),INDEX(LinMotor!$AB$1:$AB$1305,A141,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A141,1),INDEX(LinMotor!$Y$1:$Y$1305,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A141,1),INDEX(LinMotor!$AB$1:$AB$1305,A141,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A141,1),INDEX(LinMotor!$Y$1:$Y$1305,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A141,1),INDEX(LinMotor!$AB$1:$AB$1305,A141,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A141,1),INDEX(LinMotor!$AD$1:$AD$1305,A141,1))","v":0.39726754672536085},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A141,1),INDEX(LinMotor!$AE$1:$AE$1305,A141,1))","v":0.56514997292784142},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A141,1),INDEX(LinMotor!$AF$1:$AF$1305,A141,1))","v":4.7672105607043305},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A141,1),INDEX(LinMotor!$AG$1:$AG$1305,A141,1))","v":13.563599350268193},{"$f":"IF(A141<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A141,1),INDEX(LinMotor!$AI$1:$AI$1305,A141,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A141,1),INDEX(LinMotor!$AI$1:$AI$1305,A141,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A141,1),INDEX(LinMotor!$AI$1:$AI$1305,A141,1))/1000,\"0.0k\")),\"\")","v":339.38332907761713},{"$f":"IF(A141<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A141,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A141,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A141,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A141,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A141,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A141,1))/1000,\"0.0k\")),\"\")","v":275.11842737156735},{"$f":"IF(A141<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A141,1),INDEX(LinMotor!$AK$1:$AK$1305,A141,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A141,1),INDEX(LinMotor!$AK$1:$AK$1305,A141,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A141,1),INDEX(LinMotor!$AK$1:$AK$1305,A141,1))/1000,\"0.0k\")),\"\")","v":"2.6k"},""]
[599,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A142,1),INDEX(LinMotor!$B$1:$B$1291,A142,1))","v":"AKM2G-71N 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A142,1),INDEX(LinMotor!$R$1:$R$1305,A142,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A142,1),INDEX(LinMotor!$S$1:$S$1305,A142,1))","v":0.3941568090209942},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A142,1),INDEX(LinMotor!$T$1:$T$1305,A142,1))","v":0.50320691129242934},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A142,1),INDEX(LinMotor!$U$1:$U$1305,A142,1))","v":1.0909090909090908},{"$f":"IF(A142<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A142,1),INDEX(LinMotor!$V$1:$V$1305,A142,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A142,1),INDEX(LinMotor!$V$1:$V$1305,A142,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A142,1),INDEX(LinMotor!$V$1:$V$1305,A142,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A142<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A142,1),INDEX(LinMotor!$W$1:$W$1305,A142,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A142,1),INDEX(LinMotor!$X$1:$X$1305,A142,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A142,1),INDEX(LinMotor!$W$1:$W$1305,A142,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A142,1),INDEX(LinMotor!$X$1:$X$1305,A142,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A142,1),INDEX(LinMotor!$W$1:$W$1305,A142,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A142,1),INDEX(LinMotor!$X$1:$X$1305,A142,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A142<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A142,1),INDEX(LinMotor!$X$1:$X$1305,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A142,1),INDEX(LinMotor!$Z$1:$Z$1305,A142,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A142,1),INDEX(LinMotor!$X$1:$X$1305,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A142,1),INDEX(LinMotor!$Z$1:$Z$1305,A142,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A142,1),INDEX(LinMotor!$X$1:$X$1305,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A142,1),INDEX(LinMotor!$Z$1:$Z$1305,A142,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A142<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A142,1),INDEX(LinMotor!$Y$1:$Y$1305,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A142,1),INDEX(LinMotor!$AB$1:$AB$1305,A142,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A142,1),INDEX(LinMotor!$Y$1:$Y$1305,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A142,1),INDEX(LinMotor!$AB$1:$AB$1305,A142,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A142,1),INDEX(LinMotor!$Y$1:$Y$1305,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A142,1),INDEX(LinMotor!$AB$1:$AB$1305,A142,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A142,1),INDEX(LinMotor!$AD$1:$AD$1305,A142,1))","v":0.5537603515335332},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A142,1),INDEX(LinMotor!$AE$1:$AE$1305,A142,1))","v":0.78777551868348883},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A142,1),INDEX(LinMotor!$AF$1:$AF$1305,A142,1))","v":6.6451242184023984},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A142,1),INDEX(LinMotor!$AG$1:$AG$1305,A142,1))","v":18.906612448403731},{"$f":"IF(A142<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A142,1),INDEX(LinMotor!$AI$1:$AI$1305,A142,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A142,1),INDEX(LinMotor!$AI$1:$AI$1305,A142,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A142,1),INDEX(LinMotor!$AI$1:$AI$1305,A142,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A142<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A142,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A142,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A142,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A142,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A142,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A142,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A142<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A142,1),INDEX(LinMotor!$AK$1:$AK$1305,A142,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A142,1),INDEX(LinMotor!$AK$1:$AK$1305,A142,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A142,1),INDEX(LinMotor!$AK$1:$AK$1305,A142,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[600,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A143,1),INDEX(LinMotor!$B$1:$B$1291,A143,1))","v":"AKM2G-71N 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A143,1),INDEX(LinMotor!$R$1:$R$1305,A143,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A143,1),INDEX(LinMotor!$S$1:$S$1305,A143,1))","v":0.39892658525130353},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A143,1),INDEX(LinMotor!$T$1:$T$1305,A143,1))","v":0.50320691129242934},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A143,1),INDEX(LinMotor!$U$1:$U$1305,A143,1))","v":1.0379046726148879},{"$f":"IF(A143<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A143,1),INDEX(LinMotor!$V$1:$V$1305,A143,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A143,1),INDEX(LinMotor!$V$1:$V$1305,A143,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A143,1),INDEX(LinMotor!$V$1:$V$1305,A143,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A143<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A143,1),INDEX(LinMotor!$W$1:$W$1305,A143,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A143,1),INDEX(LinMotor!$X$1:$X$1305,A143,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A143,1),INDEX(LinMotor!$W$1:$W$1305,A143,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A143,1),INDEX(LinMotor!$X$1:$X$1305,A143,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A143,1),INDEX(LinMotor!$W$1:$W$1305,A143,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A143,1),INDEX(LinMotor!$X$1:$X$1305,A143,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A143<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A143,1),INDEX(LinMotor!$X$1:$X$1305,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A143,1),INDEX(LinMotor!$Z$1:$Z$1305,A143,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A143,1),INDEX(LinMotor!$X$1:$X$1305,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A143,1),INDEX(LinMotor!$Z$1:$Z$1305,A143,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A143,1),INDEX(LinMotor!$X$1:$X$1305,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A143,1),INDEX(LinMotor!$Z$1:$Z$1305,A143,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A143<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A143,1),INDEX(LinMotor!$Y$1:$Y$1305,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A143,1),INDEX(LinMotor!$AB$1:$AB$1305,A143,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A143,1),INDEX(LinMotor!$Y$1:$Y$1305,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A143,1),INDEX(LinMotor!$AB$1:$AB$1305,A143,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A143,1),INDEX(LinMotor!$Y$1:$Y$1305,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A143,1),INDEX(LinMotor!$AB$1:$AB$1305,A143,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A143,1),INDEX(LinMotor!$AD$1:$AD$1305,A143,1))","v":0.5537603515335332},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A143,1),INDEX(LinMotor!$AE$1:$AE$1305,A143,1))","v":0.78777551868348883},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A143,1),INDEX(LinMotor!$AF$1:$AF$1305,A143,1))","v":6.6451242184023984},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A143,1),INDEX(LinMotor!$AG$1:$AG$1305,A143,1))","v":18.906612448403731},{"$f":"IF(A143<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A143,1),INDEX(LinMotor!$AI$1:$AI$1305,A143,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A143,1),INDEX(LinMotor!$AI$1:$AI$1305,A143,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A143,1),INDEX(LinMotor!$AI$1:$AI$1305,A143,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A143<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A143,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A143,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A143,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A143,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A143,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A143,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A143<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A143,1),INDEX(LinMotor!$AK$1:$AK$1305,A143,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A143,1),INDEX(LinMotor!$AK$1:$AK$1305,A143,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A143,1),INDEX(LinMotor!$AK$1:$AK$1305,A143,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[601,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A144,1),INDEX(LinMotor!$B$1:$B$1291,A144,1))","v":"AKM2G-71N 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A144,1),INDEX(LinMotor!$R$1:$R$1305,A144,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A144,1),INDEX(LinMotor!$S$1:$S$1305,A144,1))","v":0.40161092754438976},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A144,1),INDEX(LinMotor!$T$1:$T$1305,A144,1))","v":0.50320691129242934},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A144,1),INDEX(LinMotor!$U$1:$U$1305,A144,1))","v":1.0379046726148879},{"$f":"IF(A144<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A144,1),INDEX(LinMotor!$V$1:$V$1305,A144,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A144,1),INDEX(LinMotor!$V$1:$V$1305,A144,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A144,1),INDEX(LinMotor!$V$1:$V$1305,A144,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A144<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A144,1),INDEX(LinMotor!$W$1:$W$1305,A144,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A144,1),INDEX(LinMotor!$X$1:$X$1305,A144,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A144,1),INDEX(LinMotor!$W$1:$W$1305,A144,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A144,1),INDEX(LinMotor!$X$1:$X$1305,A144,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A144,1),INDEX(LinMotor!$W$1:$W$1305,A144,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A144,1),INDEX(LinMotor!$X$1:$X$1305,A144,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A144<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A144,1),INDEX(LinMotor!$X$1:$X$1305,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A144,1),INDEX(LinMotor!$Z$1:$Z$1305,A144,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A144,1),INDEX(LinMotor!$X$1:$X$1305,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A144,1),INDEX(LinMotor!$Z$1:$Z$1305,A144,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A144,1),INDEX(LinMotor!$X$1:$X$1305,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A144,1),INDEX(LinMotor!$Z$1:$Z$1305,A144,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A144<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A144,1),INDEX(LinMotor!$Y$1:$Y$1305,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A144,1),INDEX(LinMotor!$AB$1:$AB$1305,A144,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A144,1),INDEX(LinMotor!$Y$1:$Y$1305,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A144,1),INDEX(LinMotor!$AB$1:$AB$1305,A144,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A144,1),INDEX(LinMotor!$Y$1:$Y$1305,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A144,1),INDEX(LinMotor!$AB$1:$AB$1305,A144,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A144,1),INDEX(LinMotor!$AD$1:$AD$1305,A144,1))","v":0.5537603515335332},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A144,1),INDEX(LinMotor!$AE$1:$AE$1305,A144,1))","v":0.78777551868348883},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A144,1),INDEX(LinMotor!$AF$1:$AF$1305,A144,1))","v":6.6451242184023984},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A144,1),INDEX(LinMotor!$AG$1:$AG$1305,A144,1))","v":18.906612448403731},{"$f":"IF(A144<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A144,1),INDEX(LinMotor!$AI$1:$AI$1305,A144,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A144,1),INDEX(LinMotor!$AI$1:$AI$1305,A144,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A144,1),INDEX(LinMotor!$AI$1:$AI$1305,A144,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A144<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A144,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A144,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A144,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A144,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A144,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A144,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A144<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A144,1),INDEX(LinMotor!$AK$1:$AK$1305,A144,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A144,1),INDEX(LinMotor!$AK$1:$AK$1305,A144,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A144,1),INDEX(LinMotor!$AK$1:$AK$1305,A144,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[603,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A145,1),INDEX(LinMotor!$B$1:$B$1291,A145,1))","v":"AKM2G-71P 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A145,1),INDEX(LinMotor!$R$1:$R$1305,A145,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A145,1),INDEX(LinMotor!$S$1:$S$1305,A145,1))","v":0.39057928728011787},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A145,1),INDEX(LinMotor!$T$1:$T$1305,A145,1))","v":0.49815463298920043},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A145,1),INDEX(LinMotor!$U$1:$U$1305,A145,1))","v":0.88888888888888884},{"$f":"IF(A145<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A145,1),INDEX(LinMotor!$V$1:$V$1305,A145,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A145,1),INDEX(LinMotor!$V$1:$V$1305,A145,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A145,1),INDEX(LinMotor!$V$1:$V$1305,A145,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A145<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A145,1),INDEX(LinMotor!$W$1:$W$1305,A145,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A145,1),INDEX(LinMotor!$X$1:$X$1305,A145,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A145,1),INDEX(LinMotor!$W$1:$W$1305,A145,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A145,1),INDEX(LinMotor!$X$1:$X$1305,A145,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A145,1),INDEX(LinMotor!$W$1:$W$1305,A145,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A145,1),INDEX(LinMotor!$X$1:$X$1305,A145,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A145<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A145,1),INDEX(LinMotor!$X$1:$X$1305,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A145,1),INDEX(LinMotor!$Z$1:$Z$1305,A145,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A145,1),INDEX(LinMotor!$X$1:$X$1305,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A145,1),INDEX(LinMotor!$Z$1:$Z$1305,A145,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A145,1),INDEX(LinMotor!$X$1:$X$1305,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A145,1),INDEX(LinMotor!$Z$1:$Z$1305,A145,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A145<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A145,1),INDEX(LinMotor!$Y$1:$Y$1305,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A145,1),INDEX(LinMotor!$AB$1:$AB$1305,A145,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A145,1),INDEX(LinMotor!$Y$1:$Y$1305,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A145,1),INDEX(LinMotor!$AB$1:$AB$1305,A145,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A145,1),INDEX(LinMotor!$Y$1:$Y$1305,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A145,1),INDEX(LinMotor!$AB$1:$AB$1305,A145,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A145,1),INDEX(LinMotor!$AD$1:$AD$1305,A145,1))","v":0.66658612963223807},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A145,1),INDEX(LinMotor!$AE$1:$AE$1305,A145,1))","v":0.94828066430548119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A145,1),INDEX(LinMotor!$AF$1:$AF$1305,A145,1))","v":7.9990335555868572},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A145,1),INDEX(LinMotor!$AG$1:$AG$1305,A145,1))","v":22.758735943331548},{"$f":"IF(A145<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A145,1),INDEX(LinMotor!$AI$1:$AI$1305,A145,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A145,1),INDEX(LinMotor!$AI$1:$AI$1305,A145,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A145,1),INDEX(LinMotor!$AI$1:$AI$1305,A145,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A145<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A145,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A145,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A145,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A145,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A145,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A145,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A145<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A145,1),INDEX(LinMotor!$AK$1:$AK$1305,A145,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A145,1),INDEX(LinMotor!$AK$1:$AK$1305,A145,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A145,1),INDEX(LinMotor!$AK$1:$AK$1305,A145,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[604,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A146,1),INDEX(LinMotor!$B$1:$B$1291,A146,1))","v":"AKM2G-71P 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A146,1),INDEX(LinMotor!$R$1:$R$1305,A146,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A146,1),INDEX(LinMotor!$S$1:$S$1305,A146,1))","v":0.39650574074176015},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A146,1),INDEX(LinMotor!$T$1:$T$1305,A146,1))","v":0.49815463298920043},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A146,1),INDEX(LinMotor!$U$1:$U$1305,A146,1))","v":0.85737378467475867},{"$f":"IF(A146<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A146,1),INDEX(LinMotor!$V$1:$V$1305,A146,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A146,1),INDEX(LinMotor!$V$1:$V$1305,A146,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A146,1),INDEX(LinMotor!$V$1:$V$1305,A146,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A146<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A146,1),INDEX(LinMotor!$W$1:$W$1305,A146,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A146,1),INDEX(LinMotor!$X$1:$X$1305,A146,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A146,1),INDEX(LinMotor!$W$1:$W$1305,A146,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A146,1),INDEX(LinMotor!$X$1:$X$1305,A146,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A146,1),INDEX(LinMotor!$W$1:$W$1305,A146,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A146,1),INDEX(LinMotor!$X$1:$X$1305,A146,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A146<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A146,1),INDEX(LinMotor!$X$1:$X$1305,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A146,1),INDEX(LinMotor!$Z$1:$Z$1305,A146,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A146,1),INDEX(LinMotor!$X$1:$X$1305,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A146,1),INDEX(LinMotor!$Z$1:$Z$1305,A146,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A146,1),INDEX(LinMotor!$X$1:$X$1305,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A146,1),INDEX(LinMotor!$Z$1:$Z$1305,A146,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A146<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A146,1),INDEX(LinMotor!$Y$1:$Y$1305,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A146,1),INDEX(LinMotor!$AB$1:$AB$1305,A146,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A146,1),INDEX(LinMotor!$Y$1:$Y$1305,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A146,1),INDEX(LinMotor!$AB$1:$AB$1305,A146,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A146,1),INDEX(LinMotor!$Y$1:$Y$1305,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A146,1),INDEX(LinMotor!$AB$1:$AB$1305,A146,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A146,1),INDEX(LinMotor!$AD$1:$AD$1305,A146,1))","v":0.66658612963223807},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A146,1),INDEX(LinMotor!$AE$1:$AE$1305,A146,1))","v":0.94828066430548119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A146,1),INDEX(LinMotor!$AF$1:$AF$1305,A146,1))","v":7.9990335555868572},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A146,1),INDEX(LinMotor!$AG$1:$AG$1305,A146,1))","v":22.758735943331548},{"$f":"IF(A146<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A146,1),INDEX(LinMotor!$AI$1:$AI$1305,A146,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A146,1),INDEX(LinMotor!$AI$1:$AI$1305,A146,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A146,1),INDEX(LinMotor!$AI$1:$AI$1305,A146,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A146<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A146,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A146,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A146,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A146,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A146,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A146,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A146<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A146,1),INDEX(LinMotor!$AK$1:$AK$1305,A146,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A146,1),INDEX(LinMotor!$AK$1:$AK$1305,A146,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A146,1),INDEX(LinMotor!$AK$1:$AK$1305,A146,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[630,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A147,1),INDEX(LinMotor!$B$1:$B$1291,A147,1))","v":"AKM2G-74R 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A147,1),INDEX(LinMotor!$R$1:$R$1305,A147,1))","v":0.28216702985792697},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A147,1),INDEX(LinMotor!$S$1:$S$1305,A147,1))","v":0.29621825536122692},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A147,1),INDEX(LinMotor!$T$1:$T$1305,A147,1))","v":0.33988579350522558},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A147,1),INDEX(LinMotor!$U$1:$U$1305,A147,1))","v":1.618226291416049},{"$f":"IF(A147<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A147,1),INDEX(LinMotor!$V$1:$V$1305,A147,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A147,1),INDEX(LinMotor!$V$1:$V$1305,A147,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A147,1),INDEX(LinMotor!$V$1:$V$1305,A147,1))/1000,\"0.0k\")),\"\")","v":55.367393687502869},{"$f":"IF(A147<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A147,1),INDEX(LinMotor!$W$1:$W$1305,A147,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A147,1),INDEX(LinMotor!$X$1:$X$1305,A147,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A147,1),INDEX(LinMotor!$W$1:$W$1305,A147,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A147,1),INDEX(LinMotor!$X$1:$X$1305,A147,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A147,1),INDEX(LinMotor!$W$1:$W$1305,A147,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A147,1),INDEX(LinMotor!$X$1:$X$1305,A147,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A147<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A147,1),INDEX(LinMotor!$X$1:$X$1305,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A147,1),INDEX(LinMotor!$Z$1:$Z$1305,A147,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A147,1),INDEX(LinMotor!$X$1:$X$1305,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A147,1),INDEX(LinMotor!$Z$1:$Z$1305,A147,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A147,1),INDEX(LinMotor!$X$1:$X$1305,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A147,1),INDEX(LinMotor!$Z$1:$Z$1305,A147,1)))/1000,\"0.0k\")),\"\")","v":-44.847588886877318},{"$f":"IF(A147<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A147,1),INDEX(LinMotor!$Y$1:$Y$1305,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A147,1),INDEX(LinMotor!$AB$1:$AB$1305,A147,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A147,1),INDEX(LinMotor!$Y$1:$Y$1305,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A147,1),INDEX(LinMotor!$AB$1:$AB$1305,A147,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A147,1),INDEX(LinMotor!$Y$1:$Y$1305,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A147,1),INDEX(LinMotor!$AB$1:$AB$1305,A147,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A147,1),INDEX(LinMotor!$AD$1:$AD$1305,A147,1))","v":0.73918990740070445},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A147,1),INDEX(LinMotor!$AE$1:$AE$1305,A147,1))","v":1.0515662797012792},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A147,1),INDEX(LinMotor!$AF$1:$AF$1305,A147,1))","v":8.8702788888084534},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A147,1),INDEX(LinMotor!$AG$1:$AG$1305,A147,1))","v":25.237590712830702},{"$f":"IF(A147<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A147,1),INDEX(LinMotor!$AI$1:$AI$1305,A147,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A147,1),INDEX(LinMotor!$AI$1:$AI$1305,A147,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A147,1),INDEX(LinMotor!$AI$1:$AI$1305,A147,1))/1000,\"0.0k\")),\"\")","v":920.14195859632116},{"$f":"IF(A147<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A147,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A147,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A147,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A147,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A147,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A147,1))/1000,\"0.0k\")),\"\")","v":745.90584427238775},{"$f":"IF(A147<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A147,1),INDEX(LinMotor!$AK$1:$AK$1305,A147,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A147,1),INDEX(LinMotor!$AK$1:$AK$1305,A147,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A147,1),INDEX(LinMotor!$AK$1:$AK$1305,A147,1))/1000,\"0.0k\")),\"\")","v":"7.2k"},""]
[599,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A148,1),INDEX(LinMotor!$B$1:$B$1291,A148,1))","v":"AKM2G-71N 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A148,1),INDEX(LinMotor!$R$1:$R$1305,A148,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A148,1),INDEX(LinMotor!$S$1:$S$1305,A148,1))","v":0.3941568090209942},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A148,1),INDEX(LinMotor!$T$1:$T$1305,A148,1))","v":0.50320691129242934},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A148,1),INDEX(LinMotor!$U$1:$U$1305,A148,1))","v":1.0909090909090908},{"$f":"IF(A148<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A148,1),INDEX(LinMotor!$V$1:$V$1305,A148,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A148,1),INDEX(LinMotor!$V$1:$V$1305,A148,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A148,1),INDEX(LinMotor!$V$1:$V$1305,A148,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A148<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A148,1),INDEX(LinMotor!$W$1:$W$1305,A148,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A148,1),INDEX(LinMotor!$X$1:$X$1305,A148,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A148,1),INDEX(LinMotor!$W$1:$W$1305,A148,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A148,1),INDEX(LinMotor!$X$1:$X$1305,A148,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A148,1),INDEX(LinMotor!$W$1:$W$1305,A148,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A148,1),INDEX(LinMotor!$X$1:$X$1305,A148,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A148<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A148,1),INDEX(LinMotor!$X$1:$X$1305,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A148,1),INDEX(LinMotor!$Z$1:$Z$1305,A148,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A148,1),INDEX(LinMotor!$X$1:$X$1305,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A148,1),INDEX(LinMotor!$Z$1:$Z$1305,A148,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A148,1),INDEX(LinMotor!$X$1:$X$1305,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A148,1),INDEX(LinMotor!$Z$1:$Z$1305,A148,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A148<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A148,1),INDEX(LinMotor!$Y$1:$Y$1305,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A148,1),INDEX(LinMotor!$AB$1:$AB$1305,A148,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A148,1),INDEX(LinMotor!$Y$1:$Y$1305,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A148,1),INDEX(LinMotor!$AB$1:$AB$1305,A148,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A148,1),INDEX(LinMotor!$Y$1:$Y$1305,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A148,1),INDEX(LinMotor!$AB$1:$AB$1305,A148,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A148,1),INDEX(LinMotor!$AD$1:$AD$1305,A148,1))","v":0.5537603515335332},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A148,1),INDEX(LinMotor!$AE$1:$AE$1305,A148,1))","v":0.78777551868348883},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A148,1),INDEX(LinMotor!$AF$1:$AF$1305,A148,1))","v":6.6451242184023984},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A148,1),INDEX(LinMotor!$AG$1:$AG$1305,A148,1))","v":18.906612448403731},{"$f":"IF(A148<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A148,1),INDEX(LinMotor!$AI$1:$AI$1305,A148,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A148,1),INDEX(LinMotor!$AI$1:$AI$1305,A148,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A148,1),INDEX(LinMotor!$AI$1:$AI$1305,A148,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A148<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A148,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A148,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A148,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A148,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A148,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A148,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A148<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A148,1),INDEX(LinMotor!$AK$1:$AK$1305,A148,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A148,1),INDEX(LinMotor!$AK$1:$AK$1305,A148,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A148,1),INDEX(LinMotor!$AK$1:$AK$1305,A148,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[600,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A149,1),INDEX(LinMotor!$B$1:$B$1291,A149,1))","v":"AKM2G-71N 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A149,1),INDEX(LinMotor!$R$1:$R$1305,A149,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A149,1),INDEX(LinMotor!$S$1:$S$1305,A149,1))","v":0.39892658525130353},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A149,1),INDEX(LinMotor!$T$1:$T$1305,A149,1))","v":0.50320691129242934},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A149,1),INDEX(LinMotor!$U$1:$U$1305,A149,1))","v":1.0379046726148879},{"$f":"IF(A149<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A149,1),INDEX(LinMotor!$V$1:$V$1305,A149,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A149,1),INDEX(LinMotor!$V$1:$V$1305,A149,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A149,1),INDEX(LinMotor!$V$1:$V$1305,A149,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A149<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A149,1),INDEX(LinMotor!$W$1:$W$1305,A149,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A149,1),INDEX(LinMotor!$X$1:$X$1305,A149,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A149,1),INDEX(LinMotor!$W$1:$W$1305,A149,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A149,1),INDEX(LinMotor!$X$1:$X$1305,A149,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A149,1),INDEX(LinMotor!$W$1:$W$1305,A149,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A149,1),INDEX(LinMotor!$X$1:$X$1305,A149,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A149<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A149,1),INDEX(LinMotor!$X$1:$X$1305,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A149,1),INDEX(LinMotor!$Z$1:$Z$1305,A149,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A149,1),INDEX(LinMotor!$X$1:$X$1305,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A149,1),INDEX(LinMotor!$Z$1:$Z$1305,A149,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A149,1),INDEX(LinMotor!$X$1:$X$1305,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A149,1),INDEX(LinMotor!$Z$1:$Z$1305,A149,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A149<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A149,1),INDEX(LinMotor!$Y$1:$Y$1305,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A149,1),INDEX(LinMotor!$AB$1:$AB$1305,A149,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A149,1),INDEX(LinMotor!$Y$1:$Y$1305,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A149,1),INDEX(LinMotor!$AB$1:$AB$1305,A149,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A149,1),INDEX(LinMotor!$Y$1:$Y$1305,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A149,1),INDEX(LinMotor!$AB$1:$AB$1305,A149,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A149,1),INDEX(LinMotor!$AD$1:$AD$1305,A149,1))","v":0.5537603515335332},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A149,1),INDEX(LinMotor!$AE$1:$AE$1305,A149,1))","v":0.78777551868348883},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A149,1),INDEX(LinMotor!$AF$1:$AF$1305,A149,1))","v":6.6451242184023984},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A149,1),INDEX(LinMotor!$AG$1:$AG$1305,A149,1))","v":18.906612448403731},{"$f":"IF(A149<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A149,1),INDEX(LinMotor!$AI$1:$AI$1305,A149,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A149,1),INDEX(LinMotor!$AI$1:$AI$1305,A149,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A149,1),INDEX(LinMotor!$AI$1:$AI$1305,A149,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A149<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A149,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A149,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A149,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A149,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A149,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A149,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A149<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A149,1),INDEX(LinMotor!$AK$1:$AK$1305,A149,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A149,1),INDEX(LinMotor!$AK$1:$AK$1305,A149,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A149,1),INDEX(LinMotor!$AK$1:$AK$1305,A149,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[601,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A150,1),INDEX(LinMotor!$B$1:$B$1291,A150,1))","v":"AKM2G-71N 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A150,1),INDEX(LinMotor!$R$1:$R$1305,A150,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A150,1),INDEX(LinMotor!$S$1:$S$1305,A150,1))","v":0.40161092754438976},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A150,1),INDEX(LinMotor!$T$1:$T$1305,A150,1))","v":0.50320691129242934},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A150,1),INDEX(LinMotor!$U$1:$U$1305,A150,1))","v":1.0379046726148879},{"$f":"IF(A150<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A150,1),INDEX(LinMotor!$V$1:$V$1305,A150,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A150,1),INDEX(LinMotor!$V$1:$V$1305,A150,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A150,1),INDEX(LinMotor!$V$1:$V$1305,A150,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A150<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A150,1),INDEX(LinMotor!$W$1:$W$1305,A150,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A150,1),INDEX(LinMotor!$X$1:$X$1305,A150,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A150,1),INDEX(LinMotor!$W$1:$W$1305,A150,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A150,1),INDEX(LinMotor!$X$1:$X$1305,A150,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A150,1),INDEX(LinMotor!$W$1:$W$1305,A150,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A150,1),INDEX(LinMotor!$X$1:$X$1305,A150,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A150<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A150,1),INDEX(LinMotor!$X$1:$X$1305,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A150,1),INDEX(LinMotor!$Z$1:$Z$1305,A150,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A150,1),INDEX(LinMotor!$X$1:$X$1305,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A150,1),INDEX(LinMotor!$Z$1:$Z$1305,A150,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A150,1),INDEX(LinMotor!$X$1:$X$1305,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A150,1),INDEX(LinMotor!$Z$1:$Z$1305,A150,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A150<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A150,1),INDEX(LinMotor!$Y$1:$Y$1305,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A150,1),INDEX(LinMotor!$AB$1:$AB$1305,A150,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A150,1),INDEX(LinMotor!$Y$1:$Y$1305,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A150,1),INDEX(LinMotor!$AB$1:$AB$1305,A150,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A150,1),INDEX(LinMotor!$Y$1:$Y$1305,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A150,1),INDEX(LinMotor!$AB$1:$AB$1305,A150,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A150,1),INDEX(LinMotor!$AD$1:$AD$1305,A150,1))","v":0.5537603515335332},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A150,1),INDEX(LinMotor!$AE$1:$AE$1305,A150,1))","v":0.78777551868348883},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A150,1),INDEX(LinMotor!$AF$1:$AF$1305,A150,1))","v":6.6451242184023984},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A150,1),INDEX(LinMotor!$AG$1:$AG$1305,A150,1))","v":18.906612448403731},{"$f":"IF(A150<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A150,1),INDEX(LinMotor!$AI$1:$AI$1305,A150,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A150,1),INDEX(LinMotor!$AI$1:$AI$1305,A150,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A150,1),INDEX(LinMotor!$AI$1:$AI$1305,A150,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A150<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A150,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A150,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A150,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A150,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A150,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A150,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A150<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A150,1),INDEX(LinMotor!$AK$1:$AK$1305,A150,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A150,1),INDEX(LinMotor!$AK$1:$AK$1305,A150,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A150,1),INDEX(LinMotor!$AK$1:$AK$1305,A150,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[603,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A151,1),INDEX(LinMotor!$B$1:$B$1291,A151,1))","v":"AKM2G-71P 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A151,1),INDEX(LinMotor!$R$1:$R$1305,A151,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A151,1),INDEX(LinMotor!$S$1:$S$1305,A151,1))","v":0.39057928728011787},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A151,1),INDEX(LinMotor!$T$1:$T$1305,A151,1))","v":0.49815463298920043},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A151,1),INDEX(LinMotor!$U$1:$U$1305,A151,1))","v":0.88888888888888884},{"$f":"IF(A151<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A151,1),INDEX(LinMotor!$V$1:$V$1305,A151,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A151,1),INDEX(LinMotor!$V$1:$V$1305,A151,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A151,1),INDEX(LinMotor!$V$1:$V$1305,A151,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A151<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A151,1),INDEX(LinMotor!$W$1:$W$1305,A151,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A151,1),INDEX(LinMotor!$X$1:$X$1305,A151,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A151,1),INDEX(LinMotor!$W$1:$W$1305,A151,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A151,1),INDEX(LinMotor!$X$1:$X$1305,A151,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A151,1),INDEX(LinMotor!$W$1:$W$1305,A151,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A151,1),INDEX(LinMotor!$X$1:$X$1305,A151,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A151<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A151,1),INDEX(LinMotor!$X$1:$X$1305,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A151,1),INDEX(LinMotor!$Z$1:$Z$1305,A151,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A151,1),INDEX(LinMotor!$X$1:$X$1305,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A151,1),INDEX(LinMotor!$Z$1:$Z$1305,A151,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A151,1),INDEX(LinMotor!$X$1:$X$1305,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A151,1),INDEX(LinMotor!$Z$1:$Z$1305,A151,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A151<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A151,1),INDEX(LinMotor!$Y$1:$Y$1305,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A151,1),INDEX(LinMotor!$AB$1:$AB$1305,A151,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A151,1),INDEX(LinMotor!$Y$1:$Y$1305,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A151,1),INDEX(LinMotor!$AB$1:$AB$1305,A151,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A151,1),INDEX(LinMotor!$Y$1:$Y$1305,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A151,1),INDEX(LinMotor!$AB$1:$AB$1305,A151,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A151,1),INDEX(LinMotor!$AD$1:$AD$1305,A151,1))","v":0.66658612963223807},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A151,1),INDEX(LinMotor!$AE$1:$AE$1305,A151,1))","v":0.94828066430548119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A151,1),INDEX(LinMotor!$AF$1:$AF$1305,A151,1))","v":7.9990335555868572},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A151,1),INDEX(LinMotor!$AG$1:$AG$1305,A151,1))","v":22.758735943331548},{"$f":"IF(A151<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A151,1),INDEX(LinMotor!$AI$1:$AI$1305,A151,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A151,1),INDEX(LinMotor!$AI$1:$AI$1305,A151,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A151,1),INDEX(LinMotor!$AI$1:$AI$1305,A151,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A151<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A151,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A151,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A151,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A151,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A151,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A151,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A151<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A151,1),INDEX(LinMotor!$AK$1:$AK$1305,A151,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A151,1),INDEX(LinMotor!$AK$1:$AK$1305,A151,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A151,1),INDEX(LinMotor!$AK$1:$AK$1305,A151,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[604,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A152,1),INDEX(LinMotor!$B$1:$B$1291,A152,1))","v":"AKM2G-71P 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A152,1),INDEX(LinMotor!$R$1:$R$1305,A152,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A152,1),INDEX(LinMotor!$S$1:$S$1305,A152,1))","v":0.39650574074176015},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A152,1),INDEX(LinMotor!$T$1:$T$1305,A152,1))","v":0.49815463298920043},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A152,1),INDEX(LinMotor!$U$1:$U$1305,A152,1))","v":0.85737378467475867},{"$f":"IF(A152<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A152,1),INDEX(LinMotor!$V$1:$V$1305,A152,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A152,1),INDEX(LinMotor!$V$1:$V$1305,A152,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A152,1),INDEX(LinMotor!$V$1:$V$1305,A152,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A152<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A152,1),INDEX(LinMotor!$W$1:$W$1305,A152,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A152,1),INDEX(LinMotor!$X$1:$X$1305,A152,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A152,1),INDEX(LinMotor!$W$1:$W$1305,A152,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A152,1),INDEX(LinMotor!$X$1:$X$1305,A152,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A152,1),INDEX(LinMotor!$W$1:$W$1305,A152,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A152,1),INDEX(LinMotor!$X$1:$X$1305,A152,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A152<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A152,1),INDEX(LinMotor!$X$1:$X$1305,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A152,1),INDEX(LinMotor!$Z$1:$Z$1305,A152,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A152,1),INDEX(LinMotor!$X$1:$X$1305,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A152,1),INDEX(LinMotor!$Z$1:$Z$1305,A152,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A152,1),INDEX(LinMotor!$X$1:$X$1305,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A152,1),INDEX(LinMotor!$Z$1:$Z$1305,A152,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A152<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A152,1),INDEX(LinMotor!$Y$1:$Y$1305,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A152,1),INDEX(LinMotor!$AB$1:$AB$1305,A152,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A152,1),INDEX(LinMotor!$Y$1:$Y$1305,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A152,1),INDEX(LinMotor!$AB$1:$AB$1305,A152,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A152,1),INDEX(LinMotor!$Y$1:$Y$1305,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A152,1),INDEX(LinMotor!$AB$1:$AB$1305,A152,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A152,1),INDEX(LinMotor!$AD$1:$AD$1305,A152,1))","v":0.66658612963223807},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A152,1),INDEX(LinMotor!$AE$1:$AE$1305,A152,1))","v":0.94828066430548119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A152,1),INDEX(LinMotor!$AF$1:$AF$1305,A152,1))","v":7.9990335555868572},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A152,1),INDEX(LinMotor!$AG$1:$AG$1305,A152,1))","v":22.758735943331548},{"$f":"IF(A152<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A152,1),INDEX(LinMotor!$AI$1:$AI$1305,A152,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A152,1),INDEX(LinMotor!$AI$1:$AI$1305,A152,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A152,1),INDEX(LinMotor!$AI$1:$AI$1305,A152,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A152<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A152,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A152,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A152,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A152,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A152,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A152,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A152<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A152,1),INDEX(LinMotor!$AK$1:$AK$1305,A152,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A152,1),INDEX(LinMotor!$AK$1:$AK$1305,A152,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A152,1),INDEX(LinMotor!$AK$1:$AK$1305,A152,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[630,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A153,1),INDEX(LinMotor!$B$1:$B$1291,A153,1))","v":"AKM2G-74R 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A153,1),INDEX(LinMotor!$R$1:$R$1305,A153,1))","v":0.28216702985792697},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A153,1),INDEX(LinMotor!$S$1:$S$1305,A153,1))","v":0.29621825536122692},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A153,1),INDEX(LinMotor!$T$1:$T$1305,A153,1))","v":0.33988579350522558},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A153,1),INDEX(LinMotor!$U$1:$U$1305,A153,1))","v":1.618226291416049},{"$f":"IF(A153<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A153,1),INDEX(LinMotor!$V$1:$V$1305,A153,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A153,1),INDEX(LinMotor!$V$1:$V$1305,A153,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A153,1),INDEX(LinMotor!$V$1:$V$1305,A153,1))/1000,\"0.0k\")),\"\")","v":55.367393687502869},{"$f":"IF(A153<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A153,1),INDEX(LinMotor!$W$1:$W$1305,A153,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A153,1),INDEX(LinMotor!$X$1:$X$1305,A153,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A153,1),INDEX(LinMotor!$W$1:$W$1305,A153,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A153,1),INDEX(LinMotor!$X$1:$X$1305,A153,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A153,1),INDEX(LinMotor!$W$1:$W$1305,A153,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A153,1),INDEX(LinMotor!$X$1:$X$1305,A153,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A153<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A153,1),INDEX(LinMotor!$X$1:$X$1305,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A153,1),INDEX(LinMotor!$Z$1:$Z$1305,A153,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A153,1),INDEX(LinMotor!$X$1:$X$1305,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A153,1),INDEX(LinMotor!$Z$1:$Z$1305,A153,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A153,1),INDEX(LinMotor!$X$1:$X$1305,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A153,1),INDEX(LinMotor!$Z$1:$Z$1305,A153,1)))/1000,\"0.0k\")),\"\")","v":-44.847588886877318},{"$f":"IF(A153<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A153,1),INDEX(LinMotor!$Y$1:$Y$1305,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A153,1),INDEX(LinMotor!$AB$1:$AB$1305,A153,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A153,1),INDEX(LinMotor!$Y$1:$Y$1305,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A153,1),INDEX(LinMotor!$AB$1:$AB$1305,A153,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A153,1),INDEX(LinMotor!$Y$1:$Y$1305,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A153,1),INDEX(LinMotor!$AB$1:$AB$1305,A153,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A153,1),INDEX(LinMotor!$AD$1:$AD$1305,A153,1))","v":0.73918990740070445},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A153,1),INDEX(LinMotor!$AE$1:$AE$1305,A153,1))","v":1.0515662797012792},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A153,1),INDEX(LinMotor!$AF$1:$AF$1305,A153,1))","v":8.8702788888084534},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A153,1),INDEX(LinMotor!$AG$1:$AG$1305,A153,1))","v":25.237590712830702},{"$f":"IF(A153<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A153,1),INDEX(LinMotor!$AI$1:$AI$1305,A153,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A153,1),INDEX(LinMotor!$AI$1:$AI$1305,A153,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A153,1),INDEX(LinMotor!$AI$1:$AI$1305,A153,1))/1000,\"0.0k\")),\"\")","v":920.14195859632116},{"$f":"IF(A153<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A153,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A153,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A153,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A153,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A153,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A153,1))/1000,\"0.0k\")),\"\")","v":745.90584427238775},{"$f":"IF(A153<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A153,1),INDEX(LinMotor!$AK$1:$AK$1305,A153,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A153,1),INDEX(LinMotor!$AK$1:$AK$1305,A153,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A153,1),INDEX(LinMotor!$AK$1:$AK$1305,A153,1))/1000,\"0.0k\")),\"\")","v":"7.2k"},""]
[544,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A154,1),INDEX(LinMotor!$B$1:$B$1291,A154,1))","v":"AKM2G-53M 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A154,1),INDEX(LinMotor!$R$1:$R$1305,A154,1))","v":3.7650602865692933},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A154,1),INDEX(LinMotor!$S$1:$S$1305,A154,1))","v":0.34550573005757335},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A154,1),INDEX(LinMotor!$T$1:$T$1305,A154,1))","v":0.37248762590834672},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A154,1),INDEX(LinMotor!$U$1:$U$1305,A154,1))","v":0.8675572889721922},{"$f":"IF(A154<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A154,1),INDEX(LinMotor!$V$1:$V$1305,A154,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A154,1),INDEX(LinMotor!$V$1:$V$1305,A154,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A154,1),INDEX(LinMotor!$V$1:$V$1305,A154,1))/1000,\"0.0k\")),\"\")","v":15.420988280976562},{"$f":"IF(A154<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A154,1),INDEX(LinMotor!$W$1:$W$1305,A154,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A154,1),INDEX(LinMotor!$X$1:$X$1305,A154,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A154,1),INDEX(LinMotor!$W$1:$W$1305,A154,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A154,1),INDEX(LinMotor!$X$1:$X$1305,A154,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A154,1),INDEX(LinMotor!$W$1:$W$1305,A154,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A154,1),INDEX(LinMotor!$X$1:$X$1305,A154,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A154<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A154,1),INDEX(LinMotor!$X$1:$X$1305,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A154,1),INDEX(LinMotor!$Z$1:$Z$1305,A154,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A154,1),INDEX(LinMotor!$X$1:$X$1305,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A154,1),INDEX(LinMotor!$Z$1:$Z$1305,A154,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A154,1),INDEX(LinMotor!$X$1:$X$1305,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A154,1),INDEX(LinMotor!$Z$1:$Z$1305,A154,1)))/1000,\"0.0k\")),\"\")","v":-12.491000507591014},{"$f":"IF(A154<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A154,1),INDEX(LinMotor!$Y$1:$Y$1305,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A154,1),INDEX(LinMotor!$AB$1:$AB$1305,A154,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A154,1),INDEX(LinMotor!$Y$1:$Y$1305,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A154,1),INDEX(LinMotor!$AB$1:$AB$1305,A154,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A154,1),INDEX(LinMotor!$Y$1:$Y$1305,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A154,1),INDEX(LinMotor!$AB$1:$AB$1305,A154,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A154,1),INDEX(LinMotor!$AD$1:$AD$1305,A154,1))","v":0.3983664862261746},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A154,1),INDEX(LinMotor!$AE$1:$AE$1305,A154,1))","v":0.56671331640820777},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A154,1),INDEX(LinMotor!$AF$1:$AF$1305,A154,1))","v":4.780397834714095},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A154,1),INDEX(LinMotor!$AG$1:$AG$1305,A154,1))","v":13.601119593796986},{"$f":"IF(A154<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A154,1),INDEX(LinMotor!$AI$1:$AI$1305,A154,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A154,1),INDEX(LinMotor!$AI$1:$AI$1305,A154,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A154,1),INDEX(LinMotor!$AI$1:$AI$1305,A154,1))/1000,\"0.0k\")),\"\")","v":256.278965205318},{"$f":"IF(A154<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A154,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A154,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A154,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A154,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A154,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A154,1))/1000,\"0.0k\")),\"\")","v":207.75052819278193},{"$f":"IF(A154<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A154,1),INDEX(LinMotor!$AK$1:$AK$1305,A154,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A154,1),INDEX(LinMotor!$AK$1:$AK$1305,A154,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A154,1),INDEX(LinMotor!$AK$1:$AK$1305,A154,1))/1000,\"0.0k\")),\"\")","v":"2.0k"},""]
[545,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A155,1),INDEX(LinMotor!$B$1:$B$1291,A155,1))","v":"AKM2G-53M 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A155,1),INDEX(LinMotor!$R$1:$R$1305,A155,1))","v":3.7650602865692933},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A155,1),INDEX(LinMotor!$S$1:$S$1305,A155,1))","v":0.34962227127797246},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A155,1),INDEX(LinMotor!$T$1:$T$1305,A155,1))","v":0.37248762590834672},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A155,1),INDEX(LinMotor!$U$1:$U$1305,A155,1))","v":0.8675572889721922},{"$f":"IF(A155<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A155,1),INDEX(LinMotor!$V$1:$V$1305,A155,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A155,1),INDEX(LinMotor!$V$1:$V$1305,A155,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A155,1),INDEX(LinMotor!$V$1:$V$1305,A155,1))/1000,\"0.0k\")),\"\")","v":15.420988280976562},{"$f":"IF(A155<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A155,1),INDEX(LinMotor!$W$1:$W$1305,A155,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A155,1),INDEX(LinMotor!$X$1:$X$1305,A155,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A155,1),INDEX(LinMotor!$W$1:$W$1305,A155,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A155,1),INDEX(LinMotor!$X$1:$X$1305,A155,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A155,1),INDEX(LinMotor!$W$1:$W$1305,A155,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A155,1),INDEX(LinMotor!$X$1:$X$1305,A155,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A155<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A155,1),INDEX(LinMotor!$X$1:$X$1305,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A155,1),INDEX(LinMotor!$Z$1:$Z$1305,A155,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A155,1),INDEX(LinMotor!$X$1:$X$1305,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A155,1),INDEX(LinMotor!$Z$1:$Z$1305,A155,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A155,1),INDEX(LinMotor!$X$1:$X$1305,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A155,1),INDEX(LinMotor!$Z$1:$Z$1305,A155,1)))/1000,\"0.0k\")),\"\")","v":-12.491000507591014},{"$f":"IF(A155<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A155,1),INDEX(LinMotor!$Y$1:$Y$1305,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A155,1),INDEX(LinMotor!$AB$1:$AB$1305,A155,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A155,1),INDEX(LinMotor!$Y$1:$Y$1305,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A155,1),INDEX(LinMotor!$AB$1:$AB$1305,A155,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A155,1),INDEX(LinMotor!$Y$1:$Y$1305,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A155,1),INDEX(LinMotor!$AB$1:$AB$1305,A155,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A155,1),INDEX(LinMotor!$AD$1:$AD$1305,A155,1))","v":0.3983664862261746},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A155,1),INDEX(LinMotor!$AE$1:$AE$1305,A155,1))","v":0.56671331640820777},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A155,1),INDEX(LinMotor!$AF$1:$AF$1305,A155,1))","v":4.780397834714095},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A155,1),INDEX(LinMotor!$AG$1:$AG$1305,A155,1))","v":13.601119593796986},{"$f":"IF(A155<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A155,1),INDEX(LinMotor!$AI$1:$AI$1305,A155,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A155,1),INDEX(LinMotor!$AI$1:$AI$1305,A155,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A155,1),INDEX(LinMotor!$AI$1:$AI$1305,A155,1))/1000,\"0.0k\")),\"\")","v":256.278965205318},{"$f":"IF(A155<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A155,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A155,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A155,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A155,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A155,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A155,1))/1000,\"0.0k\")),\"\")","v":207.75052819278193},{"$f":"IF(A155<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A155,1),INDEX(LinMotor!$AK$1:$AK$1305,A155,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A155,1),INDEX(LinMotor!$AK$1:$AK$1305,A155,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A155,1),INDEX(LinMotor!$AK$1:$AK$1305,A155,1))/1000,\"0.0k\")),\"\")","v":"2.0k"},""]
[550,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A156,1),INDEX(LinMotor!$B$1:$B$1291,A156,1))","v":"AKM2G-54M 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A156,1),INDEX(LinMotor!$R$1:$R$1305,A156,1))","v":2.8735632549349721},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A156,1),INDEX(LinMotor!$S$1:$S$1305,A156,1))","v":0.29695809600365702},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A156,1),INDEX(LinMotor!$T$1:$T$1305,A156,1))","v":0.3002743948923311},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A156,1),INDEX(LinMotor!$U$1:$U$1305,A156,1))","v":1.0434782608695652},{"$f":"IF(A156<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A156,1),INDEX(LinMotor!$V$1:$V$1305,A156,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A156,1),INDEX(LinMotor!$V$1:$V$1305,A156,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A156,1),INDEX(LinMotor!$V$1:$V$1305,A156,1))/1000,\"0.0k\")),\"\")","v":16.425009629701709},{"$f":"IF(A156<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A156,1),INDEX(LinMotor!$W$1:$W$1305,A156,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A156,1),INDEX(LinMotor!$X$1:$X$1305,A156,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A156,1),INDEX(LinMotor!$W$1:$W$1305,A156,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A156,1),INDEX(LinMotor!$X$1:$X$1305,A156,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A156,1),INDEX(LinMotor!$W$1:$W$1305,A156,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A156,1),INDEX(LinMotor!$X$1:$X$1305,A156,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A156<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A156,1),INDEX(LinMotor!$X$1:$X$1305,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A156,1),INDEX(LinMotor!$Z$1:$Z$1305,A156,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A156,1),INDEX(LinMotor!$X$1:$X$1305,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A156,1),INDEX(LinMotor!$Z$1:$Z$1305,A156,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A156,1),INDEX(LinMotor!$X$1:$X$1305,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A156,1),INDEX(LinMotor!$Z$1:$Z$1305,A156,1)))/1000,\"0.0k\")),\"\")","v":-13.304257800058384},{"$f":"IF(A156<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A156,1),INDEX(LinMotor!$Y$1:$Y$1305,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A156,1),INDEX(LinMotor!$AB$1:$AB$1305,A156,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A156,1),INDEX(LinMotor!$Y$1:$Y$1305,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A156,1),INDEX(LinMotor!$AB$1:$AB$1305,A156,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A156,1),INDEX(LinMotor!$Y$1:$Y$1305,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A156,1),INDEX(LinMotor!$AB$1:$AB$1305,A156,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A156,1),INDEX(LinMotor!$AD$1:$AD$1305,A156,1))","v":0.35118555158082226},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A156,1),INDEX(LinMotor!$AE$1:$AE$1305,A156,1))","v":0.49959405595685086},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A156,1),INDEX(LinMotor!$AF$1:$AF$1305,A156,1))","v":4.2142266189698674},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A156,1),INDEX(LinMotor!$AG$1:$AG$1305,A156,1))","v":11.990257342964421},{"$f":"IF(A156<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A156,1),INDEX(LinMotor!$AI$1:$AI$1305,A156,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A156,1),INDEX(LinMotor!$AI$1:$AI$1305,A156,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A156,1),INDEX(LinMotor!$AI$1:$AI$1305,A156,1))/1000,\"0.0k\")),\"\")","v":272.96463720033182},{"$f":"IF(A156<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A156,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A156,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A156,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A156,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A156,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A156,1))/1000,\"0.0k\")),\"\")","v":221.27663700720805},{"$f":"IF(A156<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A156,1),INDEX(LinMotor!$AK$1:$AK$1305,A156,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A156,1),INDEX(LinMotor!$AK$1:$AK$1305,A156,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A156,1),INDEX(LinMotor!$AK$1:$AK$1305,A156,1))/1000,\"0.0k\")),\"\")","v":"2.1k"},""]
[551,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A157,1),INDEX(LinMotor!$B$1:$B$1291,A157,1))","v":"AKM2G-54M 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A157,1),INDEX(LinMotor!$R$1:$R$1305,A157,1))","v":2.8735632549349721},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A157,1),INDEX(LinMotor!$S$1:$S$1305,A157,1))","v":0.30096544514562967},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A157,1),INDEX(LinMotor!$T$1:$T$1305,A157,1))","v":0.3002743948923311},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A157,1),INDEX(LinMotor!$U$1:$U$1305,A157,1))","v":1.0329520939809811},{"$f":"IF(A157<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A157,1),INDEX(LinMotor!$V$1:$V$1305,A157,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A157,1),INDEX(LinMotor!$V$1:$V$1305,A157,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A157,1),INDEX(LinMotor!$V$1:$V$1305,A157,1))/1000,\"0.0k\")),\"\")","v":16.425009629701709},{"$f":"IF(A157<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A157,1),INDEX(LinMotor!$W$1:$W$1305,A157,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A157,1),INDEX(LinMotor!$X$1:$X$1305,A157,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A157,1),INDEX(LinMotor!$W$1:$W$1305,A157,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A157,1),INDEX(LinMotor!$X$1:$X$1305,A157,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A157,1),INDEX(LinMotor!$W$1:$W$1305,A157,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A157,1),INDEX(LinMotor!$X$1:$X$1305,A157,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A157<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A157,1),INDEX(LinMotor!$X$1:$X$1305,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A157,1),INDEX(LinMotor!$Z$1:$Z$1305,A157,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A157,1),INDEX(LinMotor!$X$1:$X$1305,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A157,1),INDEX(LinMotor!$Z$1:$Z$1305,A157,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A157,1),INDEX(LinMotor!$X$1:$X$1305,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A157,1),INDEX(LinMotor!$Z$1:$Z$1305,A157,1)))/1000,\"0.0k\")),\"\")","v":-13.304257800058384},{"$f":"IF(A157<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A157,1),INDEX(LinMotor!$Y$1:$Y$1305,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A157,1),INDEX(LinMotor!$AB$1:$AB$1305,A157,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A157,1),INDEX(LinMotor!$Y$1:$Y$1305,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A157,1),INDEX(LinMotor!$AB$1:$AB$1305,A157,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A157,1),INDEX(LinMotor!$Y$1:$Y$1305,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A157,1),INDEX(LinMotor!$AB$1:$AB$1305,A157,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A157,1),INDEX(LinMotor!$AD$1:$AD$1305,A157,1))","v":0.35118555158082226},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A157,1),INDEX(LinMotor!$AE$1:$AE$1305,A157,1))","v":0.49959405595685086},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A157,1),INDEX(LinMotor!$AF$1:$AF$1305,A157,1))","v":4.2142266189698674},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A157,1),INDEX(LinMotor!$AG$1:$AG$1305,A157,1))","v":11.990257342964421},{"$f":"IF(A157<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A157,1),INDEX(LinMotor!$AI$1:$AI$1305,A157,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A157,1),INDEX(LinMotor!$AI$1:$AI$1305,A157,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A157,1),INDEX(LinMotor!$AI$1:$AI$1305,A157,1))/1000,\"0.0k\")),\"\")","v":272.96463720033188},{"$f":"IF(A157<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A157,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A157,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A157,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A157,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A157,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A157,1))/1000,\"0.0k\")),\"\")","v":221.27663700720805},{"$f":"IF(A157<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A157,1),INDEX(LinMotor!$AK$1:$AK$1305,A157,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A157,1),INDEX(LinMotor!$AK$1:$AK$1305,A157,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A157,1),INDEX(LinMotor!$AK$1:$AK$1305,A157,1))/1000,\"0.0k\")),\"\")","v":"2.1k"},""]
[552,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A158,1),INDEX(LinMotor!$B$1:$B$1291,A158,1))","v":"AKM2G-54M 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A158,1),INDEX(LinMotor!$R$1:$R$1305,A158,1))","v":2.8735632549349721},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A158,1),INDEX(LinMotor!$S$1:$S$1305,A158,1))","v":0.30320911484117419},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A158,1),INDEX(LinMotor!$T$1:$T$1305,A158,1))","v":0.3002743948923311},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A158,1),INDEX(LinMotor!$U$1:$U$1305,A158,1))","v":1.0329520939809811},{"$f":"IF(A158<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A158,1),INDEX(LinMotor!$V$1:$V$1305,A158,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A158,1),INDEX(LinMotor!$V$1:$V$1305,A158,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A158,1),INDEX(LinMotor!$V$1:$V$1305,A158,1))/1000,\"0.0k\")),\"\")","v":16.425009629701709},{"$f":"IF(A158<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A158,1),INDEX(LinMotor!$W$1:$W$1305,A158,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A158,1),INDEX(LinMotor!$X$1:$X$1305,A158,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A158,1),INDEX(LinMotor!$W$1:$W$1305,A158,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A158,1),INDEX(LinMotor!$X$1:$X$1305,A158,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A158,1),INDEX(LinMotor!$W$1:$W$1305,A158,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A158,1),INDEX(LinMotor!$X$1:$X$1305,A158,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A158<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A158,1),INDEX(LinMotor!$X$1:$X$1305,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A158,1),INDEX(LinMotor!$Z$1:$Z$1305,A158,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A158,1),INDEX(LinMotor!$X$1:$X$1305,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A158,1),INDEX(LinMotor!$Z$1:$Z$1305,A158,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A158,1),INDEX(LinMotor!$X$1:$X$1305,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A158,1),INDEX(LinMotor!$Z$1:$Z$1305,A158,1)))/1000,\"0.0k\")),\"\")","v":-13.304257800058384},{"$f":"IF(A158<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A158,1),INDEX(LinMotor!$Y$1:$Y$1305,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A158,1),INDEX(LinMotor!$AB$1:$AB$1305,A158,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A158,1),INDEX(LinMotor!$Y$1:$Y$1305,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A158,1),INDEX(LinMotor!$AB$1:$AB$1305,A158,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A158,1),INDEX(LinMotor!$Y$1:$Y$1305,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A158,1),INDEX(LinMotor!$AB$1:$AB$1305,A158,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A158,1),INDEX(LinMotor!$AD$1:$AD$1305,A158,1))","v":0.35118555158082226},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A158,1),INDEX(LinMotor!$AE$1:$AE$1305,A158,1))","v":0.49959405595685086},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A158,1),INDEX(LinMotor!$AF$1:$AF$1305,A158,1))","v":4.2142266189698674},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A158,1),INDEX(LinMotor!$AG$1:$AG$1305,A158,1))","v":11.990257342964421},{"$f":"IF(A158<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A158,1),INDEX(LinMotor!$AI$1:$AI$1305,A158,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A158,1),INDEX(LinMotor!$AI$1:$AI$1305,A158,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A158,1),INDEX(LinMotor!$AI$1:$AI$1305,A158,1))/1000,\"0.0k\")),\"\")","v":272.96463720033188},{"$f":"IF(A158<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A158,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A158,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A158,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A158,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A158,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A158,1))/1000,\"0.0k\")),\"\")","v":221.27663700720805},{"$f":"IF(A158<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A158,1),INDEX(LinMotor!$AK$1:$AK$1305,A158,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A158,1),INDEX(LinMotor!$AK$1:$AK$1305,A158,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A158,1),INDEX(LinMotor!$AK$1:$AK$1305,A158,1))/1000,\"0.0k\")),\"\")","v":"2.1k"},""]
[554,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A159,1),INDEX(LinMotor!$B$1:$B$1291,A159,1))","v":"AKM2G-54N 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A159,1),INDEX(LinMotor!$R$1:$R$1305,A159,1))","v":2.8735632549349721},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A159,1),INDEX(LinMotor!$S$1:$S$1305,A159,1))","v":0.29771459758902286},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A159,1),INDEX(LinMotor!$T$1:$T$1305,A159,1))","v":0.3002743948923311},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A159,1),INDEX(LinMotor!$U$1:$U$1305,A159,1))","v":0.92709690169207093},{"$f":"IF(A159<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A159,1),INDEX(LinMotor!$V$1:$V$1305,A159,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A159,1),INDEX(LinMotor!$V$1:$V$1305,A159,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A159,1),INDEX(LinMotor!$V$1:$V$1305,A159,1))/1000,\"0.0k\")),\"\")","v":16.425009629701709},{"$f":"IF(A159<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A159,1),INDEX(LinMotor!$W$1:$W$1305,A159,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A159,1),INDEX(LinMotor!$X$1:$X$1305,A159,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A159,1),INDEX(LinMotor!$W$1:$W$1305,A159,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A159,1),INDEX(LinMotor!$X$1:$X$1305,A159,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A159,1),INDEX(LinMotor!$W$1:$W$1305,A159,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A159,1),INDEX(LinMotor!$X$1:$X$1305,A159,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A159<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A159,1),INDEX(LinMotor!$X$1:$X$1305,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A159,1),INDEX(LinMotor!$Z$1:$Z$1305,A159,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A159,1),INDEX(LinMotor!$X$1:$X$1305,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A159,1),INDEX(LinMotor!$Z$1:$Z$1305,A159,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A159,1),INDEX(LinMotor!$X$1:$X$1305,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A159,1),INDEX(LinMotor!$Z$1:$Z$1305,A159,1)))/1000,\"0.0k\")),\"\")","v":-13.304257800058384},{"$f":"IF(A159<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A159,1),INDEX(LinMotor!$Y$1:$Y$1305,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A159,1),INDEX(LinMotor!$AB$1:$AB$1305,A159,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A159,1),INDEX(LinMotor!$Y$1:$Y$1305,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A159,1),INDEX(LinMotor!$AB$1:$AB$1305,A159,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A159,1),INDEX(LinMotor!$Y$1:$Y$1305,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A159,1),INDEX(LinMotor!$AB$1:$AB$1305,A159,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A159,1),INDEX(LinMotor!$AD$1:$AD$1305,A159,1))","v":0.39207699131976598},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A159,1),INDEX(LinMotor!$AE$1:$AE$1305,A159,1))","v":0.55776592590176921},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A159,1),INDEX(LinMotor!$AF$1:$AF$1305,A159,1))","v":4.7049238958371919},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A159,1),INDEX(LinMotor!$AG$1:$AG$1305,A159,1))","v":13.386382221642462},{"$f":"IF(A159<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A159,1),INDEX(LinMotor!$AI$1:$AI$1305,A159,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A159,1),INDEX(LinMotor!$AI$1:$AI$1305,A159,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A159,1),INDEX(LinMotor!$AI$1:$AI$1305,A159,1))/1000,\"0.0k\")),\"\")","v":272.96463720033188},{"$f":"IF(A159<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A159,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A159,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A159,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A159,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A159,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A159,1))/1000,\"0.0k\")),\"\")","v":221.27663700720805},{"$f":"IF(A159<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A159,1),INDEX(LinMotor!$AK$1:$AK$1305,A159,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A159,1),INDEX(LinMotor!$AK$1:$AK$1305,A159,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A159,1),INDEX(LinMotor!$AK$1:$AK$1305,A159,1))/1000,\"0.0k\")),\"\")","v":"2.1k"},""]
[555,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A160,1),INDEX(LinMotor!$B$1:$B$1291,A160,1))","v":"AKM2G-54N 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A160,1),INDEX(LinMotor!$R$1:$R$1305,A160,1))","v":2.8735632549349721},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A160,1),INDEX(LinMotor!$S$1:$S$1305,A160,1))","v":0.30223964438045714},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A160,1),INDEX(LinMotor!$T$1:$T$1305,A160,1))","v":0.3002743948923311},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A160,1),INDEX(LinMotor!$U$1:$U$1305,A160,1))","v":0.92709690169207093},{"$f":"IF(A160<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A160,1),INDEX(LinMotor!$V$1:$V$1305,A160,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A160,1),INDEX(LinMotor!$V$1:$V$1305,A160,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A160,1),INDEX(LinMotor!$V$1:$V$1305,A160,1))/1000,\"0.0k\")),\"\")","v":16.425009629701709},{"$f":"IF(A160<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A160,1),INDEX(LinMotor!$W$1:$W$1305,A160,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A160,1),INDEX(LinMotor!$X$1:$X$1305,A160,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A160,1),INDEX(LinMotor!$W$1:$W$1305,A160,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A160,1),INDEX(LinMotor!$X$1:$X$1305,A160,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A160,1),INDEX(LinMotor!$W$1:$W$1305,A160,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A160,1),INDEX(LinMotor!$X$1:$X$1305,A160,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A160<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A160,1),INDEX(LinMotor!$X$1:$X$1305,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A160,1),INDEX(LinMotor!$Z$1:$Z$1305,A160,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A160,1),INDEX(LinMotor!$X$1:$X$1305,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A160,1),INDEX(LinMotor!$Z$1:$Z$1305,A160,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A160,1),INDEX(LinMotor!$X$1:$X$1305,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A160,1),INDEX(LinMotor!$Z$1:$Z$1305,A160,1)))/1000,\"0.0k\")),\"\")","v":-13.304257800058384},{"$f":"IF(A160<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A160,1),INDEX(LinMotor!$Y$1:$Y$1305,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A160,1),INDEX(LinMotor!$AB$1:$AB$1305,A160,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A160,1),INDEX(LinMotor!$Y$1:$Y$1305,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A160,1),INDEX(LinMotor!$AB$1:$AB$1305,A160,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A160,1),INDEX(LinMotor!$Y$1:$Y$1305,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A160,1),INDEX(LinMotor!$AB$1:$AB$1305,A160,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A160,1),INDEX(LinMotor!$AD$1:$AD$1305,A160,1))","v":0.39207699131976598},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A160,1),INDEX(LinMotor!$AE$1:$AE$1305,A160,1))","v":0.55776592590176921},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A160,1),INDEX(LinMotor!$AF$1:$AF$1305,A160,1))","v":4.7049238958371919},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A160,1),INDEX(LinMotor!$AG$1:$AG$1305,A160,1))","v":13.386382221642462},{"$f":"IF(A160<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A160,1),INDEX(LinMotor!$AI$1:$AI$1305,A160,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A160,1),INDEX(LinMotor!$AI$1:$AI$1305,A160,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A160,1),INDEX(LinMotor!$AI$1:$AI$1305,A160,1))/1000,\"0.0k\")),\"\")","v":272.96463720033188},{"$f":"IF(A160<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A160,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A160,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A160,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A160,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A160,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A160,1))/1000,\"0.0k\")),\"\")","v":221.27663700720805},{"$f":"IF(A160<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A160,1),INDEX(LinMotor!$AK$1:$AK$1305,A160,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A160,1),INDEX(LinMotor!$AK$1:$AK$1305,A160,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A160,1),INDEX(LinMotor!$AK$1:$AK$1305,A160,1))/1000,\"0.0k\")),\"\")","v":"2.1k"},""]
[560,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A161,1),INDEX(LinMotor!$B$1:$B$1291,A161,1))","v":"AKM2G-62L 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A161,1),INDEX(LinMotor!$R$1:$R$1305,A161,1))","v":2.7472527397738253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A161,1),INDEX(LinMotor!$S$1:$S$1305,A161,1))","v":0.39145424345627228},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A161,1),INDEX(LinMotor!$T$1:$T$1305,A161,1))","v":0.44438408080690633},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A161,1),INDEX(LinMotor!$U$1:$U$1305,A161,1))","v":1.0909090909090908},{"$f":"IF(A161<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A161,1),INDEX(LinMotor!$V$1:$V$1305,A161,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A161,1),INDEX(LinMotor!$V$1:$V$1305,A161,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A161,1),INDEX(LinMotor!$V$1:$V$1305,A161,1))/1000,\"0.0k\")),\"\")","v":16.619965300254588},{"$f":"IF(A161<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A161,1),INDEX(LinMotor!$W$1:$W$1305,A161,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A161,1),INDEX(LinMotor!$X$1:$X$1305,A161,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A161,1),INDEX(LinMotor!$W$1:$W$1305,A161,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A161,1),INDEX(LinMotor!$X$1:$X$1305,A161,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A161,1),INDEX(LinMotor!$W$1:$W$1305,A161,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A161,1),INDEX(LinMotor!$X$1:$X$1305,A161,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A161<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A161,1),INDEX(LinMotor!$X$1:$X$1305,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A161,1),INDEX(LinMotor!$Z$1:$Z$1305,A161,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A161,1),INDEX(LinMotor!$X$1:$X$1305,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A161,1),INDEX(LinMotor!$Z$1:$Z$1305,A161,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A161,1),INDEX(LinMotor!$X$1:$X$1305,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A161,1),INDEX(LinMotor!$Z$1:$Z$1305,A161,1)))/1000,\"0.0k\")),\"\")","v":-13.462171893206216},{"$f":"IF(A161<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A161,1),INDEX(LinMotor!$Y$1:$Y$1305,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A161,1),INDEX(LinMotor!$AB$1:$AB$1305,A161,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A161,1),INDEX(LinMotor!$Y$1:$Y$1305,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A161,1),INDEX(LinMotor!$AB$1:$AB$1305,A161,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A161,1),INDEX(LinMotor!$Y$1:$Y$1305,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A161,1),INDEX(LinMotor!$AB$1:$AB$1305,A161,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A161,1),INDEX(LinMotor!$AD$1:$AD$1305,A161,1))","v":0.37149474032437096},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A161,1),INDEX(LinMotor!$AE$1:$AE$1305,A161,1))","v":0.52848576272528158},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A161,1),INDEX(LinMotor!$AF$1:$AF$1305,A161,1))","v":4.4579368838924518},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A161,1),INDEX(LinMotor!$AG$1:$AG$1305,A161,1))","v":12.683658305406757},{"$f":"IF(A161<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A161,1),INDEX(LinMotor!$AI$1:$AI$1305,A161,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A161,1),INDEX(LinMotor!$AI$1:$AI$1305,A161,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A161,1),INDEX(LinMotor!$AI$1:$AI$1305,A161,1))/1000,\"0.0k\")),\"\")","v":276.20457465439478},{"$f":"IF(A161<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A161,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A161,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A161,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A161,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A161,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A161,1))/1000,\"0.0k\")),\"\")","v":223.9030668308726},{"$f":"IF(A161<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A161,1),INDEX(LinMotor!$AK$1:$AK$1305,A161,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A161,1),INDEX(LinMotor!$AK$1:$AK$1305,A161,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A161,1),INDEX(LinMotor!$AK$1:$AK$1305,A161,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[561,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A162,1),INDEX(LinMotor!$B$1:$B$1291,A162,1))","v":"AKM2G-62L 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A162,1),INDEX(LinMotor!$R$1:$R$1305,A162,1))","v":2.7472527397738253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A162,1),INDEX(LinMotor!$S$1:$S$1305,A162,1))","v":0.3954225943476134},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A162,1),INDEX(LinMotor!$T$1:$T$1305,A162,1))","v":0.44438408080690633},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A162,1),INDEX(LinMotor!$U$1:$U$1305,A162,1))","v":1.0552318289827101},{"$f":"IF(A162<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A162,1),INDEX(LinMotor!$V$1:$V$1305,A162,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A162,1),INDEX(LinMotor!$V$1:$V$1305,A162,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A162,1),INDEX(LinMotor!$V$1:$V$1305,A162,1))/1000,\"0.0k\")),\"\")","v":16.619965300254588},{"$f":"IF(A162<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A162,1),INDEX(LinMotor!$W$1:$W$1305,A162,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A162,1),INDEX(LinMotor!$X$1:$X$1305,A162,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A162,1),INDEX(LinMotor!$W$1:$W$1305,A162,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A162,1),INDEX(LinMotor!$X$1:$X$1305,A162,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A162,1),INDEX(LinMotor!$W$1:$W$1305,A162,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A162,1),INDEX(LinMotor!$X$1:$X$1305,A162,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A162<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A162,1),INDEX(LinMotor!$X$1:$X$1305,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A162,1),INDEX(LinMotor!$Z$1:$Z$1305,A162,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A162,1),INDEX(LinMotor!$X$1:$X$1305,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A162,1),INDEX(LinMotor!$Z$1:$Z$1305,A162,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A162,1),INDEX(LinMotor!$X$1:$X$1305,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A162,1),INDEX(LinMotor!$Z$1:$Z$1305,A162,1)))/1000,\"0.0k\")),\"\")","v":-13.462171893206216},{"$f":"IF(A162<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A162,1),INDEX(LinMotor!$Y$1:$Y$1305,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A162,1),INDEX(LinMotor!$AB$1:$AB$1305,A162,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A162,1),INDEX(LinMotor!$Y$1:$Y$1305,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A162,1),INDEX(LinMotor!$AB$1:$AB$1305,A162,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A162,1),INDEX(LinMotor!$Y$1:$Y$1305,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A162,1),INDEX(LinMotor!$AB$1:$AB$1305,A162,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A162,1),INDEX(LinMotor!$AD$1:$AD$1305,A162,1))","v":0.37149474032437096},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A162,1),INDEX(LinMotor!$AE$1:$AE$1305,A162,1))","v":0.52848576272528158},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A162,1),INDEX(LinMotor!$AF$1:$AF$1305,A162,1))","v":4.4579368838924518},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A162,1),INDEX(LinMotor!$AG$1:$AG$1305,A162,1))","v":12.683658305406757},{"$f":"IF(A162<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A162,1),INDEX(LinMotor!$AI$1:$AI$1305,A162,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A162,1),INDEX(LinMotor!$AI$1:$AI$1305,A162,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A162,1),INDEX(LinMotor!$AI$1:$AI$1305,A162,1))/1000,\"0.0k\")),\"\")","v":276.20457465439478},{"$f":"IF(A162<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A162,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A162,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A162,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A162,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A162,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A162,1))/1000,\"0.0k\")),\"\")","v":223.9030668308726},{"$f":"IF(A162<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A162,1),INDEX(LinMotor!$AK$1:$AK$1305,A162,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A162,1),INDEX(LinMotor!$AK$1:$AK$1305,A162,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A162,1),INDEX(LinMotor!$AK$1:$AK$1305,A162,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},{"$f":"IF(T162=1,\"L<Lmin\",IF(T162=2,\"Udc>Umot\",IF(T162=3,\"L<Lmin & Udc>Umot\",IF(T162=4,\"L>Lmax\",IF(T162=5,\"L>Lmax & Udc>Umot\",\"\")))))","v":""}]
[562,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A163,1),INDEX(LinMotor!$B$1:$B$1291,A163,1))","v":"AKM2G-62L 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A163,1),INDEX(LinMotor!$R$1:$R$1305,A163,1))","v":2.7472527397738253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A163,1),INDEX(LinMotor!$S$1:$S$1305,A163,1))","v":0.39746969938201571},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A163,1),INDEX(LinMotor!$T$1:$T$1305,A163,1))","v":0.44438408080690633},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A163,1),INDEX(LinMotor!$U$1:$U$1305,A163,1))","v":1.0552318289827101},{"$f":"IF(A163<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A163,1),INDEX(LinMotor!$V$1:$V$1305,A163,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A163,1),INDEX(LinMotor!$V$1:$V$1305,A163,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A163,1),INDEX(LinMotor!$V$1:$V$1305,A163,1))/1000,\"0.0k\")),\"\")","v":16.619965300254588},{"$f":"IF(A163<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A163,1),INDEX(LinMotor!$W$1:$W$1305,A163,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A163,1),INDEX(LinMotor!$X$1:$X$1305,A163,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A163,1),INDEX(LinMotor!$W$1:$W$1305,A163,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A163,1),INDEX(LinMotor!$X$1:$X$1305,A163,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A163,1),INDEX(LinMotor!$W$1:$W$1305,A163,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A163,1),INDEX(LinMotor!$X$1:$X$1305,A163,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A163<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A163,1),INDEX(LinMotor!$X$1:$X$1305,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A163,1),INDEX(LinMotor!$Z$1:$Z$1305,A163,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A163,1),INDEX(LinMotor!$X$1:$X$1305,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A163,1),INDEX(LinMotor!$Z$1:$Z$1305,A163,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A163,1),INDEX(LinMotor!$X$1:$X$1305,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A163,1),INDEX(LinMotor!$Z$1:$Z$1305,A163,1)))/1000,\"0.0k\")),\"\")","v":-13.462171893206216},{"$f":"IF(A163<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A163,1),INDEX(LinMotor!$Y$1:$Y$1305,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A163,1),INDEX(LinMotor!$AB$1:$AB$1305,A163,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A163,1),INDEX(LinMotor!$Y$1:$Y$1305,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A163,1),INDEX(LinMotor!$AB$1:$AB$1305,A163,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A163,1),INDEX(LinMotor!$Y$1:$Y$1305,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A163,1),INDEX(LinMotor!$AB$1:$AB$1305,A163,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A163,1),INDEX(LinMotor!$AD$1:$AD$1305,A163,1))","v":0.37149474032437096},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A163,1),INDEX(LinMotor!$AE$1:$AE$1305,A163,1))","v":0.52848576272528158},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A163,1),INDEX(LinMotor!$AF$1:$AF$1305,A163,1))","v":4.4579368838924518},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A163,1),INDEX(LinMotor!$AG$1:$AG$1305,A163,1))","v":12.683658305406757},{"$f":"IF(A163<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A163,1),INDEX(LinMotor!$AI$1:$AI$1305,A163,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A163,1),INDEX(LinMotor!$AI$1:$AI$1305,A163,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A163,1),INDEX(LinMotor!$AI$1:$AI$1305,A163,1))/1000,\"0.0k\")),\"\")","v":276.20457465439478},{"$f":"IF(A163<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A163,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A163,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A163,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A163,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A163,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A163,1))/1000,\"0.0k\")),\"\")","v":223.9030668308726},{"$f":"IF(A163<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A163,1),INDEX(LinMotor!$AK$1:$AK$1305,A163,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A163,1),INDEX(LinMotor!$AK$1:$AK$1305,A163,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A163,1),INDEX(LinMotor!$AK$1:$AK$1305,A163,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[564,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A164,1),INDEX(LinMotor!$B$1:$B$1291,A164,1))","v":"AKM2G-62M 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A164,1),INDEX(LinMotor!$R$1:$R$1305,A164,1))","v":2.7472527397738253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A164,1),INDEX(LinMotor!$S$1:$S$1305,A164,1))","v":0.39515881431459743},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A164,1),INDEX(LinMotor!$T$1:$T$1305,A164,1))","v":0.44438408080690633},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A164,1),INDEX(LinMotor!$U$1:$U$1305,A164,1))","v":0.8571428571428571},{"$f":"IF(A164<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A164,1),INDEX(LinMotor!$V$1:$V$1305,A164,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A164,1),INDEX(LinMotor!$V$1:$V$1305,A164,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A164,1),INDEX(LinMotor!$V$1:$V$1305,A164,1))/1000,\"0.0k\")),\"\")","v":16.619965300254588},{"$f":"IF(A164<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A164,1),INDEX(LinMotor!$W$1:$W$1305,A164,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A164,1),INDEX(LinMotor!$X$1:$X$1305,A164,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A164,1),INDEX(LinMotor!$W$1:$W$1305,A164,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A164,1),INDEX(LinMotor!$X$1:$X$1305,A164,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A164,1),INDEX(LinMotor!$W$1:$W$1305,A164,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A164,1),INDEX(LinMotor!$X$1:$X$1305,A164,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A164<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A164,1),INDEX(LinMotor!$X$1:$X$1305,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A164,1),INDEX(LinMotor!$Z$1:$Z$1305,A164,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A164,1),INDEX(LinMotor!$X$1:$X$1305,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A164,1),INDEX(LinMotor!$Z$1:$Z$1305,A164,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A164,1),INDEX(LinMotor!$X$1:$X$1305,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A164,1),INDEX(LinMotor!$Z$1:$Z$1305,A164,1)))/1000,\"0.0k\")),\"\")","v":-13.462171893206216},{"$f":"IF(A164<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A164,1),INDEX(LinMotor!$Y$1:$Y$1305,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A164,1),INDEX(LinMotor!$AB$1:$AB$1305,A164,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A164,1),INDEX(LinMotor!$Y$1:$Y$1305,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A164,1),INDEX(LinMotor!$AB$1:$AB$1305,A164,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A164,1),INDEX(LinMotor!$Y$1:$Y$1305,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A164,1),INDEX(LinMotor!$AB$1:$AB$1305,A164,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A164,1),INDEX(LinMotor!$AD$1:$AD$1305,A164,1))","v":0.47066744175875325},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A164,1),INDEX(LinMotor!$AE$1:$AE$1305,A164,1))","v":0.66956813905532886},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A164,1),INDEX(LinMotor!$AF$1:$AF$1305,A164,1))","v":5.6480093011050387},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A164,1),INDEX(LinMotor!$AG$1:$AG$1305,A164,1))","v":16.069635337327892},{"$f":"IF(A164<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A164,1),INDEX(LinMotor!$AI$1:$AI$1305,A164,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A164,1),INDEX(LinMotor!$AI$1:$AI$1305,A164,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A164,1),INDEX(LinMotor!$AI$1:$AI$1305,A164,1))/1000,\"0.0k\")),\"\")","v":276.20457465439478},{"$f":"IF(A164<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A164,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A164,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A164,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A164,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A164,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A164,1))/1000,\"0.0k\")),\"\")","v":223.9030668308726},{"$f":"IF(A164<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A164,1),INDEX(LinMotor!$AK$1:$AK$1305,A164,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A164,1),INDEX(LinMotor!$AK$1:$AK$1305,A164,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A164,1),INDEX(LinMotor!$AK$1:$AK$1305,A164,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[565,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A165,1),INDEX(LinMotor!$B$1:$B$1291,A165,1))","v":"AKM2G-62M 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A165,1),INDEX(LinMotor!$R$1:$R$1305,A165,1))","v":2.7472527397738253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A165,1),INDEX(LinMotor!$S$1:$S$1305,A165,1))","v":0.39999017343510934},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A165,1),INDEX(LinMotor!$T$1:$T$1305,A165,1))","v":0.44438408080690633},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A165,1),INDEX(LinMotor!$U$1:$U$1305,A165,1))","v":0.83856135442558821},{"$f":"IF(A165<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A165,1),INDEX(LinMotor!$V$1:$V$1305,A165,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A165,1),INDEX(LinMotor!$V$1:$V$1305,A165,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A165,1),INDEX(LinMotor!$V$1:$V$1305,A165,1))/1000,\"0.0k\")),\"\")","v":16.619965300254588},{"$f":"IF(A165<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A165,1),INDEX(LinMotor!$W$1:$W$1305,A165,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A165,1),INDEX(LinMotor!$X$1:$X$1305,A165,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A165,1),INDEX(LinMotor!$W$1:$W$1305,A165,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A165,1),INDEX(LinMotor!$X$1:$X$1305,A165,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A165,1),INDEX(LinMotor!$W$1:$W$1305,A165,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A165,1),INDEX(LinMotor!$X$1:$X$1305,A165,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A165<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A165,1),INDEX(LinMotor!$X$1:$X$1305,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A165,1),INDEX(LinMotor!$Z$1:$Z$1305,A165,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A165,1),INDEX(LinMotor!$X$1:$X$1305,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A165,1),INDEX(LinMotor!$Z$1:$Z$1305,A165,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A165,1),INDEX(LinMotor!$X$1:$X$1305,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A165,1),INDEX(LinMotor!$Z$1:$Z$1305,A165,1)))/1000,\"0.0k\")),\"\")","v":-13.462171893206216},{"$f":"IF(A165<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A165,1),INDEX(LinMotor!$Y$1:$Y$1305,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A165,1),INDEX(LinMotor!$AB$1:$AB$1305,A165,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A165,1),INDEX(LinMotor!$Y$1:$Y$1305,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A165,1),INDEX(LinMotor!$AB$1:$AB$1305,A165,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A165,1),INDEX(LinMotor!$Y$1:$Y$1305,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A165,1),INDEX(LinMotor!$AB$1:$AB$1305,A165,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A165,1),INDEX(LinMotor!$AD$1:$AD$1305,A165,1))","v":0.47066744175875325},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A165,1),INDEX(LinMotor!$AE$1:$AE$1305,A165,1))","v":0.66956813905532886},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A165,1),INDEX(LinMotor!$AF$1:$AF$1305,A165,1))","v":5.6480093011050387},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A165,1),INDEX(LinMotor!$AG$1:$AG$1305,A165,1))","v":16.069635337327892},{"$f":"IF(A165<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A165,1),INDEX(LinMotor!$AI$1:$AI$1305,A165,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A165,1),INDEX(LinMotor!$AI$1:$AI$1305,A165,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A165,1),INDEX(LinMotor!$AI$1:$AI$1305,A165,1))/1000,\"0.0k\")),\"\")","v":276.20457465439478},{"$f":"IF(A165<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A165,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A165,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A165,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A165,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A165,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A165,1))/1000,\"0.0k\")),\"\")","v":223.9030668308726},{"$f":"IF(A165<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A165,1),INDEX(LinMotor!$AK$1:$AK$1305,A165,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A165,1),INDEX(LinMotor!$AK$1:$AK$1305,A165,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A165,1),INDEX(LinMotor!$AK$1:$AK$1305,A165,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[570,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A166,1),INDEX(LinMotor!$B$1:$B$1291,A166,1))","v":"AKM2G-63M 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A166,1),INDEX(LinMotor!$R$1:$R$1305,A166,1))","v":1.9230769178416716},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A166,1),INDEX(LinMotor!$S$1:$S$1305,A166,1))","v":0.31123355295030775},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A166,1),INDEX(LinMotor!$T$1:$T$1305,A166,1))","v":0.33983087063899553},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A166,1),INDEX(LinMotor!$U$1:$U$1305,A166,1))","v":1.1428571428571428},{"$f":"IF(A166<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A166,1),INDEX(LinMotor!$V$1:$V$1305,A166,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A166,1),INDEX(LinMotor!$V$1:$V$1305,A166,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A166,1),INDEX(LinMotor!$V$1:$V$1305,A166,1))/1000,\"0.0k\")),\"\")","v":18.520782449825255},{"$f":"IF(A166<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A166,1),INDEX(LinMotor!$W$1:$W$1305,A166,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A166,1),INDEX(LinMotor!$X$1:$X$1305,A166,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A166,1),INDEX(LinMotor!$W$1:$W$1305,A166,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A166,1),INDEX(LinMotor!$X$1:$X$1305,A166,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A166,1),INDEX(LinMotor!$W$1:$W$1305,A166,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A166,1),INDEX(LinMotor!$X$1:$X$1305,A166,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A166<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A166,1),INDEX(LinMotor!$X$1:$X$1305,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A166,1),INDEX(LinMotor!$Z$1:$Z$1305,A166,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A166,1),INDEX(LinMotor!$X$1:$X$1305,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A166,1),INDEX(LinMotor!$Z$1:$Z$1305,A166,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A166,1),INDEX(LinMotor!$X$1:$X$1305,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A166,1),INDEX(LinMotor!$Z$1:$Z$1305,A166,1)))/1000,\"0.0k\")),\"\")","v":-15.001833784358457},{"$f":"IF(A166<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A166,1),INDEX(LinMotor!$Y$1:$Y$1305,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A166,1),INDEX(LinMotor!$AB$1:$AB$1305,A166,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A166,1),INDEX(LinMotor!$Y$1:$Y$1305,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A166,1),INDEX(LinMotor!$AB$1:$AB$1305,A166,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A166,1),INDEX(LinMotor!$Y$1:$Y$1305,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A166,1),INDEX(LinMotor!$AB$1:$AB$1305,A166,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A166,1),INDEX(LinMotor!$AD$1:$AD$1305,A166,1))","v":0.3852984686408169},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A166,1),INDEX(LinMotor!$AE$1:$AE$1305,A166,1))","v":0.54812284798091604},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A166,1),INDEX(LinMotor!$AF$1:$AF$1305,A166,1))","v":4.6235816236898026},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A166,1),INDEX(LinMotor!$AG$1:$AG$1305,A166,1))","v":13.154948351541986},{"$f":"IF(A166<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A166,1),INDEX(LinMotor!$AI$1:$AI$1305,A166,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A166,1),INDEX(LinMotor!$AI$1:$AI$1305,A166,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A166,1),INDEX(LinMotor!$AI$1:$AI$1305,A166,1))/1000,\"0.0k\")),\"\")","v":307.79395422337035},{"$f":"IF(A166<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A166,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A166,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A166,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A166,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A166,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A166,1))/1000,\"0.0k\")),\"\")","v":249.51074901219886},{"$f":"IF(A166<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A166,1),INDEX(LinMotor!$AK$1:$AK$1305,A166,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A166,1),INDEX(LinMotor!$AK$1:$AK$1305,A166,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A166,1),INDEX(LinMotor!$AK$1:$AK$1305,A166,1))/1000,\"0.0k\")),\"\")","v":"2.4k"},""]
[571,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A167,1),INDEX(LinMotor!$B$1:$B$1291,A167,1))","v":"AKM2G-63M 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A167,1),INDEX(LinMotor!$R$1:$R$1305,A167,1))","v":1.9230769178416716},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A167,1),INDEX(LinMotor!$S$1:$S$1305,A167,1))","v":0.3148910848964116},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A167,1),INDEX(LinMotor!$T$1:$T$1305,A167,1))","v":0.33983087063899553},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A167,1),INDEX(LinMotor!$U$1:$U$1305,A167,1))","v":1.0858738243009276},{"$f":"IF(A167<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A167,1),INDEX(LinMotor!$V$1:$V$1305,A167,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A167,1),INDEX(LinMotor!$V$1:$V$1305,A167,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A167,1),INDEX(LinMotor!$V$1:$V$1305,A167,1))/1000,\"0.0k\")),\"\")","v":18.520782449825255},{"$f":"IF(A167<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A167,1),INDEX(LinMotor!$W$1:$W$1305,A167,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A167,1),INDEX(LinMotor!$X$1:$X$1305,A167,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A167,1),INDEX(LinMotor!$W$1:$W$1305,A167,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A167,1),INDEX(LinMotor!$X$1:$X$1305,A167,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A167,1),INDEX(LinMotor!$W$1:$W$1305,A167,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A167,1),INDEX(LinMotor!$X$1:$X$1305,A167,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A167<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A167,1),INDEX(LinMotor!$X$1:$X$1305,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A167,1),INDEX(LinMotor!$Z$1:$Z$1305,A167,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A167,1),INDEX(LinMotor!$X$1:$X$1305,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A167,1),INDEX(LinMotor!$Z$1:$Z$1305,A167,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A167,1),INDEX(LinMotor!$X$1:$X$1305,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A167,1),INDEX(LinMotor!$Z$1:$Z$1305,A167,1)))/1000,\"0.0k\")),\"\")","v":-15.001833784358457},{"$f":"IF(A167<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A167,1),INDEX(LinMotor!$Y$1:$Y$1305,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A167,1),INDEX(LinMotor!$AB$1:$AB$1305,A167,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A167,1),INDEX(LinMotor!$Y$1:$Y$1305,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A167,1),INDEX(LinMotor!$AB$1:$AB$1305,A167,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A167,1),INDEX(LinMotor!$Y$1:$Y$1305,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A167,1),INDEX(LinMotor!$AB$1:$AB$1305,A167,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A167,1),INDEX(LinMotor!$AD$1:$AD$1305,A167,1))","v":0.3852984686408169},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A167,1),INDEX(LinMotor!$AE$1:$AE$1305,A167,1))","v":0.54812284798091604},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A167,1),INDEX(LinMotor!$AF$1:$AF$1305,A167,1))","v":4.6235816236898026},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A167,1),INDEX(LinMotor!$AG$1:$AG$1305,A167,1))","v":13.154948351541986},{"$f":"IF(A167<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A167,1),INDEX(LinMotor!$AI$1:$AI$1305,A167,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A167,1),INDEX(LinMotor!$AI$1:$AI$1305,A167,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A167,1),INDEX(LinMotor!$AI$1:$AI$1305,A167,1))/1000,\"0.0k\")),\"\")","v":307.79395422337029},{"$f":"IF(A167<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A167,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A167,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A167,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A167,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A167,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A167,1))/1000,\"0.0k\")),\"\")","v":249.51074901219886},{"$f":"IF(A167<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A167,1),INDEX(LinMotor!$AK$1:$AK$1305,A167,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A167,1),INDEX(LinMotor!$AK$1:$AK$1305,A167,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A167,1),INDEX(LinMotor!$AK$1:$AK$1305,A167,1))/1000,\"0.0k\")),\"\")","v":"2.4k"},""]
[572,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A168,1),INDEX(LinMotor!$B$1:$B$1291,A168,1))","v":"AKM2G-63M 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A168,1),INDEX(LinMotor!$R$1:$R$1305,A168,1))","v":1.9230769178416716},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A168,1),INDEX(LinMotor!$S$1:$S$1305,A168,1))","v":0.31690390990790446},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A168,1),INDEX(LinMotor!$T$1:$T$1305,A168,1))","v":0.33983087063899553},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A168,1),INDEX(LinMotor!$U$1:$U$1305,A168,1))","v":1.0858738243009276},{"$f":"IF(A168<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A168,1),INDEX(LinMotor!$V$1:$V$1305,A168,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A168,1),INDEX(LinMotor!$V$1:$V$1305,A168,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A168,1),INDEX(LinMotor!$V$1:$V$1305,A168,1))/1000,\"0.0k\")),\"\")","v":18.520782449825255},{"$f":"IF(A168<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A168,1),INDEX(LinMotor!$W$1:$W$1305,A168,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A168,1),INDEX(LinMotor!$X$1:$X$1305,A168,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A168,1),INDEX(LinMotor!$W$1:$W$1305,A168,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A168,1),INDEX(LinMotor!$X$1:$X$1305,A168,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A168,1),INDEX(LinMotor!$W$1:$W$1305,A168,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A168,1),INDEX(LinMotor!$X$1:$X$1305,A168,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A168<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A168,1),INDEX(LinMotor!$X$1:$X$1305,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A168,1),INDEX(LinMotor!$Z$1:$Z$1305,A168,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A168,1),INDEX(LinMotor!$X$1:$X$1305,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A168,1),INDEX(LinMotor!$Z$1:$Z$1305,A168,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A168,1),INDEX(LinMotor!$X$1:$X$1305,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A168,1),INDEX(LinMotor!$Z$1:$Z$1305,A168,1)))/1000,\"0.0k\")),\"\")","v":-15.001833784358457},{"$f":"IF(A168<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A168,1),INDEX(LinMotor!$Y$1:$Y$1305,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A168,1),INDEX(LinMotor!$AB$1:$AB$1305,A168,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A168,1),INDEX(LinMotor!$Y$1:$Y$1305,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A168,1),INDEX(LinMotor!$AB$1:$AB$1305,A168,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A168,1),INDEX(LinMotor!$Y$1:$Y$1305,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A168,1),INDEX(LinMotor!$AB$1:$AB$1305,A168,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A168,1),INDEX(LinMotor!$AD$1:$AD$1305,A168,1))","v":0.3852984686408169},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A168,1),INDEX(LinMotor!$AE$1:$AE$1305,A168,1))","v":0.54812284798091604},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A168,1),INDEX(LinMotor!$AF$1:$AF$1305,A168,1))","v":4.6235816236898026},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A168,1),INDEX(LinMotor!$AG$1:$AG$1305,A168,1))","v":13.154948351541986},{"$f":"IF(A168<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A168,1),INDEX(LinMotor!$AI$1:$AI$1305,A168,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A168,1),INDEX(LinMotor!$AI$1:$AI$1305,A168,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A168,1),INDEX(LinMotor!$AI$1:$AI$1305,A168,1))/1000,\"0.0k\")),\"\")","v":307.79395422337035},{"$f":"IF(A168<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A168,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A168,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A168,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A168,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A168,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A168,1))/1000,\"0.0k\")),\"\")","v":249.51074901219886},{"$f":"IF(A168<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A168,1),INDEX(LinMotor!$AK$1:$AK$1305,A168,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A168,1),INDEX(LinMotor!$AK$1:$AK$1305,A168,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A168,1),INDEX(LinMotor!$AK$1:$AK$1305,A168,1))/1000,\"0.0k\")),\"\")","v":"2.4k"},""]
[574,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A169,1),INDEX(LinMotor!$B$1:$B$1291,A169,1))","v":"AKM2G-63N 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A169,1),INDEX(LinMotor!$R$1:$R$1305,A169,1))","v":1.9230769178416716},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A169,1),INDEX(LinMotor!$S$1:$S$1305,A169,1))","v":0.3118320248303551},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A169,1),INDEX(LinMotor!$T$1:$T$1305,A169,1))","v":0.33983087063899553},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A169,1),INDEX(LinMotor!$U$1:$U$1305,A169,1))","v":1.0434782608695652},{"$f":"IF(A169<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A169,1),INDEX(LinMotor!$V$1:$V$1305,A169,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A169,1),INDEX(LinMotor!$V$1:$V$1305,A169,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A169,1),INDEX(LinMotor!$V$1:$V$1305,A169,1))/1000,\"0.0k\")),\"\")","v":18.520782449825255},{"$f":"IF(A169<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A169,1),INDEX(LinMotor!$W$1:$W$1305,A169,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A169,1),INDEX(LinMotor!$X$1:$X$1305,A169,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A169,1),INDEX(LinMotor!$W$1:$W$1305,A169,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A169,1),INDEX(LinMotor!$X$1:$X$1305,A169,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A169,1),INDEX(LinMotor!$W$1:$W$1305,A169,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A169,1),INDEX(LinMotor!$X$1:$X$1305,A169,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A169<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A169,1),INDEX(LinMotor!$X$1:$X$1305,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A169,1),INDEX(LinMotor!$Z$1:$Z$1305,A169,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A169,1),INDEX(LinMotor!$X$1:$X$1305,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A169,1),INDEX(LinMotor!$Z$1:$Z$1305,A169,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A169,1),INDEX(LinMotor!$X$1:$X$1305,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A169,1),INDEX(LinMotor!$Z$1:$Z$1305,A169,1)))/1000,\"0.0k\")),\"\")","v":-15.001833784358457},{"$f":"IF(A169<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A169,1),INDEX(LinMotor!$Y$1:$Y$1305,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A169,1),INDEX(LinMotor!$AB$1:$AB$1305,A169,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A169,1),INDEX(LinMotor!$Y$1:$Y$1305,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A169,1),INDEX(LinMotor!$AB$1:$AB$1305,A169,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A169,1),INDEX(LinMotor!$Y$1:$Y$1305,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A169,1),INDEX(LinMotor!$AB$1:$AB$1305,A169,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A169,1),INDEX(LinMotor!$AD$1:$AD$1305,A169,1))","v":0.42585618818631188},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A169,1),INDEX(LinMotor!$AE$1:$AE$1305,A169,1))","v":0.60581996996354148},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A169,1),INDEX(LinMotor!$AF$1:$AF$1305,A169,1))","v":5.1102742582357426},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A169,1),INDEX(LinMotor!$AG$1:$AG$1305,A169,1))","v":14.539679279124995},{"$f":"IF(A169<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A169,1),INDEX(LinMotor!$AI$1:$AI$1305,A169,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A169,1),INDEX(LinMotor!$AI$1:$AI$1305,A169,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A169,1),INDEX(LinMotor!$AI$1:$AI$1305,A169,1))/1000,\"0.0k\")),\"\")","v":307.79395422337035},{"$f":"IF(A169<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A169,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A169,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A169,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A169,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A169,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A169,1))/1000,\"0.0k\")),\"\")","v":249.51074901219886},{"$f":"IF(A169<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A169,1),INDEX(LinMotor!$AK$1:$AK$1305,A169,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A169,1),INDEX(LinMotor!$AK$1:$AK$1305,A169,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A169,1),INDEX(LinMotor!$AK$1:$AK$1305,A169,1))/1000,\"0.0k\")),\"\")","v":"2.4k"},""]
[575,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A170,1),INDEX(LinMotor!$B$1:$B$1291,A170,1))","v":"AKM2G-63N 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A170,1),INDEX(LinMotor!$R$1:$R$1305,A170,1))","v":1.9230769178416716},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A170,1),INDEX(LinMotor!$S$1:$S$1305,A170,1))","v":0.3159919187069915},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A170,1),INDEX(LinMotor!$T$1:$T$1305,A170,1))","v":0.33983087063899553},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A170,1),INDEX(LinMotor!$U$1:$U$1305,A170,1))","v":0.97518652382892745},{"$f":"IF(A170<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A170,1),INDEX(LinMotor!$V$1:$V$1305,A170,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A170,1),INDEX(LinMotor!$V$1:$V$1305,A170,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A170,1),INDEX(LinMotor!$V$1:$V$1305,A170,1))/1000,\"0.0k\")),\"\")","v":18.520782449825255},{"$f":"IF(A170<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A170,1),INDEX(LinMotor!$W$1:$W$1305,A170,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A170,1),INDEX(LinMotor!$X$1:$X$1305,A170,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A170,1),INDEX(LinMotor!$W$1:$W$1305,A170,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A170,1),INDEX(LinMotor!$X$1:$X$1305,A170,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A170,1),INDEX(LinMotor!$W$1:$W$1305,A170,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A170,1),INDEX(LinMotor!$X$1:$X$1305,A170,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A170<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A170,1),INDEX(LinMotor!$X$1:$X$1305,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A170,1),INDEX(LinMotor!$Z$1:$Z$1305,A170,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A170,1),INDEX(LinMotor!$X$1:$X$1305,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A170,1),INDEX(LinMotor!$Z$1:$Z$1305,A170,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A170,1),INDEX(LinMotor!$X$1:$X$1305,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A170,1),INDEX(LinMotor!$Z$1:$Z$1305,A170,1)))/1000,\"0.0k\")),\"\")","v":-15.001833784358457},{"$f":"IF(A170<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A170,1),INDEX(LinMotor!$Y$1:$Y$1305,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A170,1),INDEX(LinMotor!$AB$1:$AB$1305,A170,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A170,1),INDEX(LinMotor!$Y$1:$Y$1305,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A170,1),INDEX(LinMotor!$AB$1:$AB$1305,A170,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A170,1),INDEX(LinMotor!$Y$1:$Y$1305,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A170,1),INDEX(LinMotor!$AB$1:$AB$1305,A170,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A170,1),INDEX(LinMotor!$AD$1:$AD$1305,A170,1))","v":0.42585618818631188},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A170,1),INDEX(LinMotor!$AE$1:$AE$1305,A170,1))","v":0.60581996996354148},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A170,1),INDEX(LinMotor!$AF$1:$AF$1305,A170,1))","v":5.1102742582357426},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A170,1),INDEX(LinMotor!$AG$1:$AG$1305,A170,1))","v":14.539679279124995},{"$f":"IF(A170<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A170,1),INDEX(LinMotor!$AI$1:$AI$1305,A170,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A170,1),INDEX(LinMotor!$AI$1:$AI$1305,A170,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A170,1),INDEX(LinMotor!$AI$1:$AI$1305,A170,1))/1000,\"0.0k\")),\"\")","v":307.79395422337035},{"$f":"IF(A170<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A170,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A170,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A170,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A170,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A170,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A170,1))/1000,\"0.0k\")),\"\")","v":249.51074901219886},{"$f":"IF(A170<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A170,1),INDEX(LinMotor!$AK$1:$AK$1305,A170,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A170,1),INDEX(LinMotor!$AK$1:$AK$1305,A170,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A170,1),INDEX(LinMotor!$AK$1:$AK$1305,A170,1))/1000,\"0.0k\")),\"\")","v":"2.4k"},""]
[583,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A171,1),INDEX(LinMotor!$B$1:$B$1291,A171,1))","v":"AKM2G-64N 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A171,1),INDEX(LinMotor!$R$1:$R$1305,A171,1))","v":1.4792899877515946},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A171,1),INDEX(LinMotor!$S$1:$S$1305,A171,1))","v":0.27481389151094343},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A171,1),INDEX(LinMotor!$T$1:$T$1305,A171,1))","v":0.29049215404248119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A171,1),INDEX(LinMotor!$U$1:$U$1305,A171,1))","v":1.2},{"$f":"IF(A171<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A171,1),INDEX(LinMotor!$V$1:$V$1305,A171,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A171,1),INDEX(LinMotor!$V$1:$V$1305,A171,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A171,1),INDEX(LinMotor!$V$1:$V$1305,A171,1))/1000,\"0.0k\")),\"\")","v":20.421599315698124},{"$f":"IF(A171<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A171,1),INDEX(LinMotor!$W$1:$W$1305,A171,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A171,1),INDEX(LinMotor!$X$1:$X$1305,A171,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A171,1),INDEX(LinMotor!$W$1:$W$1305,A171,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A171,1),INDEX(LinMotor!$X$1:$X$1305,A171,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A171,1),INDEX(LinMotor!$W$1:$W$1305,A171,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A171,1),INDEX(LinMotor!$X$1:$X$1305,A171,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A171<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A171,1),INDEX(LinMotor!$X$1:$X$1305,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A171,1),INDEX(LinMotor!$Z$1:$Z$1305,A171,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A171,1),INDEX(LinMotor!$X$1:$X$1305,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A171,1),INDEX(LinMotor!$Z$1:$Z$1305,A171,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A171,1),INDEX(LinMotor!$X$1:$X$1305,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A171,1),INDEX(LinMotor!$Z$1:$Z$1305,A171,1)))/1000,\"0.0k\")),\"\")","v":-16.541495445715483},{"$f":"IF(A171<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A171,1),INDEX(LinMotor!$Y$1:$Y$1305,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A171,1),INDEX(LinMotor!$AB$1:$AB$1305,A171,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A171,1),INDEX(LinMotor!$Y$1:$Y$1305,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A171,1),INDEX(LinMotor!$AB$1:$AB$1305,A171,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A171,1),INDEX(LinMotor!$Y$1:$Y$1305,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A171,1),INDEX(LinMotor!$AB$1:$AB$1305,A171,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A171,1),INDEX(LinMotor!$AD$1:$AD$1305,A171,1))","v":0.39726754672536085},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A171,1),INDEX(LinMotor!$AE$1:$AE$1305,A171,1))","v":0.56514997292784142},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A171,1),INDEX(LinMotor!$AF$1:$AF$1305,A171,1))","v":4.7672105607043305},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A171,1),INDEX(LinMotor!$AG$1:$AG$1305,A171,1))","v":13.563599350268193},{"$f":"IF(A171<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A171,1),INDEX(LinMotor!$AI$1:$AI$1305,A171,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A171,1),INDEX(LinMotor!$AI$1:$AI$1305,A171,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A171,1),INDEX(LinMotor!$AI$1:$AI$1305,A171,1))/1000,\"0.0k\")),\"\")","v":339.38332907761708},{"$f":"IF(A171<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A171,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A171,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A171,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A171,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A171,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A171,1))/1000,\"0.0k\")),\"\")","v":275.11842737156735},{"$f":"IF(A171<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A171,1),INDEX(LinMotor!$AK$1:$AK$1305,A171,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A171,1),INDEX(LinMotor!$AK$1:$AK$1305,A171,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A171,1),INDEX(LinMotor!$AK$1:$AK$1305,A171,1))/1000,\"0.0k\")),\"\")","v":"2.6k"},""]
[584,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A172,1),INDEX(LinMotor!$B$1:$B$1291,A172,1))","v":"AKM2G-64N 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A172,1),INDEX(LinMotor!$R$1:$R$1305,A172,1))","v":1.4792899877515946},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A172,1),INDEX(LinMotor!$S$1:$S$1305,A172,1))","v":0.27876866103213371},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A172,1),INDEX(LinMotor!$T$1:$T$1305,A172,1))","v":0.29049215404248119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A172,1),INDEX(LinMotor!$U$1:$U$1305,A172,1))","v":1.1366603728856379},{"$f":"IF(A172<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A172,1),INDEX(LinMotor!$V$1:$V$1305,A172,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A172,1),INDEX(LinMotor!$V$1:$V$1305,A172,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A172,1),INDEX(LinMotor!$V$1:$V$1305,A172,1))/1000,\"0.0k\")),\"\")","v":20.421599315698124},{"$f":"IF(A172<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A172,1),INDEX(LinMotor!$W$1:$W$1305,A172,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A172,1),INDEX(LinMotor!$X$1:$X$1305,A172,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A172,1),INDEX(LinMotor!$W$1:$W$1305,A172,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A172,1),INDEX(LinMotor!$X$1:$X$1305,A172,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A172,1),INDEX(LinMotor!$W$1:$W$1305,A172,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A172,1),INDEX(LinMotor!$X$1:$X$1305,A172,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A172<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A172,1),INDEX(LinMotor!$X$1:$X$1305,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A172,1),INDEX(LinMotor!$Z$1:$Z$1305,A172,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A172,1),INDEX(LinMotor!$X$1:$X$1305,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A172,1),INDEX(LinMotor!$Z$1:$Z$1305,A172,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A172,1),INDEX(LinMotor!$X$1:$X$1305,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A172,1),INDEX(LinMotor!$Z$1:$Z$1305,A172,1)))/1000,\"0.0k\")),\"\")","v":-16.541495445715483},{"$f":"IF(A172<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A172,1),INDEX(LinMotor!$Y$1:$Y$1305,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A172,1),INDEX(LinMotor!$AB$1:$AB$1305,A172,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A172,1),INDEX(LinMotor!$Y$1:$Y$1305,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A172,1),INDEX(LinMotor!$AB$1:$AB$1305,A172,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A172,1),INDEX(LinMotor!$Y$1:$Y$1305,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A172,1),INDEX(LinMotor!$AB$1:$AB$1305,A172,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A172,1),INDEX(LinMotor!$AD$1:$AD$1305,A172,1))","v":0.39726754672536085},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A172,1),INDEX(LinMotor!$AE$1:$AE$1305,A172,1))","v":0.56514997292784142},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A172,1),INDEX(LinMotor!$AF$1:$AF$1305,A172,1))","v":4.7672105607043305},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A172,1),INDEX(LinMotor!$AG$1:$AG$1305,A172,1))","v":13.563599350268193},{"$f":"IF(A172<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A172,1),INDEX(LinMotor!$AI$1:$AI$1305,A172,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A172,1),INDEX(LinMotor!$AI$1:$AI$1305,A172,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A172,1),INDEX(LinMotor!$AI$1:$AI$1305,A172,1))/1000,\"0.0k\")),\"\")","v":339.38332907761708},{"$f":"IF(A172<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A172,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A172,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A172,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A172,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A172,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A172,1))/1000,\"0.0k\")),\"\")","v":275.11842737156735},{"$f":"IF(A172<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A172,1),INDEX(LinMotor!$AK$1:$AK$1305,A172,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A172,1),INDEX(LinMotor!$AK$1:$AK$1305,A172,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A172,1),INDEX(LinMotor!$AK$1:$AK$1305,A172,1))/1000,\"0.0k\")),\"\")","v":"2.6k"},""]
[585,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A173,1),INDEX(LinMotor!$B$1:$B$1291,A173,1))","v":"AKM2G-64N 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A173,1),INDEX(LinMotor!$R$1:$R$1305,A173,1))","v":1.4792899877515946},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A173,1),INDEX(LinMotor!$S$1:$S$1305,A173,1))","v":0.28093225000741556},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A173,1),INDEX(LinMotor!$T$1:$T$1305,A173,1))","v":0.29049215404248119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A173,1),INDEX(LinMotor!$U$1:$U$1305,A173,1))","v":1.1366603728856379},{"$f":"IF(A173<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A173,1),INDEX(LinMotor!$V$1:$V$1305,A173,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A173,1),INDEX(LinMotor!$V$1:$V$1305,A173,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A173,1),INDEX(LinMotor!$V$1:$V$1305,A173,1))/1000,\"0.0k\")),\"\")","v":20.421599315698124},{"$f":"IF(A173<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A173,1),INDEX(LinMotor!$W$1:$W$1305,A173,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A173,1),INDEX(LinMotor!$X$1:$X$1305,A173,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A173,1),INDEX(LinMotor!$W$1:$W$1305,A173,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A173,1),INDEX(LinMotor!$X$1:$X$1305,A173,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A173,1),INDEX(LinMotor!$W$1:$W$1305,A173,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A173,1),INDEX(LinMotor!$X$1:$X$1305,A173,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A173<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A173,1),INDEX(LinMotor!$X$1:$X$1305,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A173,1),INDEX(LinMotor!$Z$1:$Z$1305,A173,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A173,1),INDEX(LinMotor!$X$1:$X$1305,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A173,1),INDEX(LinMotor!$Z$1:$Z$1305,A173,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A173,1),INDEX(LinMotor!$X$1:$X$1305,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A173,1),INDEX(LinMotor!$Z$1:$Z$1305,A173,1)))/1000,\"0.0k\")),\"\")","v":-16.541495445715483},{"$f":"IF(A173<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A173,1),INDEX(LinMotor!$Y$1:$Y$1305,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A173,1),INDEX(LinMotor!$AB$1:$AB$1305,A173,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A173,1),INDEX(LinMotor!$Y$1:$Y$1305,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A173,1),INDEX(LinMotor!$AB$1:$AB$1305,A173,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A173,1),INDEX(LinMotor!$Y$1:$Y$1305,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A173,1),INDEX(LinMotor!$AB$1:$AB$1305,A173,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A173,1),INDEX(LinMotor!$AD$1:$AD$1305,A173,1))","v":0.39726754672536085},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A173,1),INDEX(LinMotor!$AE$1:$AE$1305,A173,1))","v":0.56514997292784142},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A173,1),INDEX(LinMotor!$AF$1:$AF$1305,A173,1))","v":4.7672105607043305},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A173,1),INDEX(LinMotor!$AG$1:$AG$1305,A173,1))","v":13.563599350268193},{"$f":"IF(A173<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A173,1),INDEX(LinMotor!$AI$1:$AI$1305,A173,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A173,1),INDEX(LinMotor!$AI$1:$AI$1305,A173,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A173,1),INDEX(LinMotor!$AI$1:$AI$1305,A173,1))/1000,\"0.0k\")),\"\")","v":339.38332907761713},{"$f":"IF(A173<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A173,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A173,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A173,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A173,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A173,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A173,1))/1000,\"0.0k\")),\"\")","v":275.11842737156735},{"$f":"IF(A173<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A173,1),INDEX(LinMotor!$AK$1:$AK$1305,A173,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A173,1),INDEX(LinMotor!$AK$1:$AK$1305,A173,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A173,1),INDEX(LinMotor!$AK$1:$AK$1305,A173,1))/1000,\"0.0k\")),\"\")","v":"2.6k"},""]
[599,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A174,1),INDEX(LinMotor!$B$1:$B$1291,A174,1))","v":"AKM2G-71N 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A174,1),INDEX(LinMotor!$R$1:$R$1305,A174,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A174,1),INDEX(LinMotor!$S$1:$S$1305,A174,1))","v":0.3941568090209942},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A174,1),INDEX(LinMotor!$T$1:$T$1305,A174,1))","v":0.50320691129242934},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A174,1),INDEX(LinMotor!$U$1:$U$1305,A174,1))","v":1.0909090909090908},{"$f":"IF(A174<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A174,1),INDEX(LinMotor!$V$1:$V$1305,A174,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A174,1),INDEX(LinMotor!$V$1:$V$1305,A174,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A174,1),INDEX(LinMotor!$V$1:$V$1305,A174,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A174<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A174,1),INDEX(LinMotor!$W$1:$W$1305,A174,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A174,1),INDEX(LinMotor!$X$1:$X$1305,A174,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A174,1),INDEX(LinMotor!$W$1:$W$1305,A174,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A174,1),INDEX(LinMotor!$X$1:$X$1305,A174,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A174,1),INDEX(LinMotor!$W$1:$W$1305,A174,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A174,1),INDEX(LinMotor!$X$1:$X$1305,A174,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A174<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A174,1),INDEX(LinMotor!$X$1:$X$1305,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A174,1),INDEX(LinMotor!$Z$1:$Z$1305,A174,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A174,1),INDEX(LinMotor!$X$1:$X$1305,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A174,1),INDEX(LinMotor!$Z$1:$Z$1305,A174,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A174,1),INDEX(LinMotor!$X$1:$X$1305,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A174,1),INDEX(LinMotor!$Z$1:$Z$1305,A174,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A174<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A174,1),INDEX(LinMotor!$Y$1:$Y$1305,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A174,1),INDEX(LinMotor!$AB$1:$AB$1305,A174,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A174,1),INDEX(LinMotor!$Y$1:$Y$1305,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A174,1),INDEX(LinMotor!$AB$1:$AB$1305,A174,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A174,1),INDEX(LinMotor!$Y$1:$Y$1305,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A174,1),INDEX(LinMotor!$AB$1:$AB$1305,A174,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A174,1),INDEX(LinMotor!$AD$1:$AD$1305,A174,1))","v":0.5537603515335332},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A174,1),INDEX(LinMotor!$AE$1:$AE$1305,A174,1))","v":0.78777551868348883},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A174,1),INDEX(LinMotor!$AF$1:$AF$1305,A174,1))","v":6.6451242184023984},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A174,1),INDEX(LinMotor!$AG$1:$AG$1305,A174,1))","v":18.906612448403731},{"$f":"IF(A174<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A174,1),INDEX(LinMotor!$AI$1:$AI$1305,A174,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A174,1),INDEX(LinMotor!$AI$1:$AI$1305,A174,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A174,1),INDEX(LinMotor!$AI$1:$AI$1305,A174,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A174<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A174,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A174,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A174,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A174,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A174,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A174,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A174<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A174,1),INDEX(LinMotor!$AK$1:$AK$1305,A174,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A174,1),INDEX(LinMotor!$AK$1:$AK$1305,A174,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A174,1),INDEX(LinMotor!$AK$1:$AK$1305,A174,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[600,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A175,1),INDEX(LinMotor!$B$1:$B$1291,A175,1))","v":"AKM2G-71N 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A175,1),INDEX(LinMotor!$R$1:$R$1305,A175,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A175,1),INDEX(LinMotor!$S$1:$S$1305,A175,1))","v":0.39892658525130353},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A175,1),INDEX(LinMotor!$T$1:$T$1305,A175,1))","v":0.50320691129242934},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A175,1),INDEX(LinMotor!$U$1:$U$1305,A175,1))","v":1.0379046726148879},{"$f":"IF(A175<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A175,1),INDEX(LinMotor!$V$1:$V$1305,A175,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A175,1),INDEX(LinMotor!$V$1:$V$1305,A175,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A175,1),INDEX(LinMotor!$V$1:$V$1305,A175,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A175<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A175,1),INDEX(LinMotor!$W$1:$W$1305,A175,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A175,1),INDEX(LinMotor!$X$1:$X$1305,A175,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A175,1),INDEX(LinMotor!$W$1:$W$1305,A175,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A175,1),INDEX(LinMotor!$X$1:$X$1305,A175,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A175,1),INDEX(LinMotor!$W$1:$W$1305,A175,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A175,1),INDEX(LinMotor!$X$1:$X$1305,A175,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A175<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A175,1),INDEX(LinMotor!$X$1:$X$1305,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A175,1),INDEX(LinMotor!$Z$1:$Z$1305,A175,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A175,1),INDEX(LinMotor!$X$1:$X$1305,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A175,1),INDEX(LinMotor!$Z$1:$Z$1305,A175,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A175,1),INDEX(LinMotor!$X$1:$X$1305,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A175,1),INDEX(LinMotor!$Z$1:$Z$1305,A175,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A175<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A175,1),INDEX(LinMotor!$Y$1:$Y$1305,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A175,1),INDEX(LinMotor!$AB$1:$AB$1305,A175,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A175,1),INDEX(LinMotor!$Y$1:$Y$1305,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A175,1),INDEX(LinMotor!$AB$1:$AB$1305,A175,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A175,1),INDEX(LinMotor!$Y$1:$Y$1305,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A175,1),INDEX(LinMotor!$AB$1:$AB$1305,A175,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A175,1),INDEX(LinMotor!$AD$1:$AD$1305,A175,1))","v":0.5537603515335332},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A175,1),INDEX(LinMotor!$AE$1:$AE$1305,A175,1))","v":0.78777551868348883},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A175,1),INDEX(LinMotor!$AF$1:$AF$1305,A175,1))","v":6.6451242184023984},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A175,1),INDEX(LinMotor!$AG$1:$AG$1305,A175,1))","v":18.906612448403731},{"$f":"IF(A175<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A175,1),INDEX(LinMotor!$AI$1:$AI$1305,A175,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A175,1),INDEX(LinMotor!$AI$1:$AI$1305,A175,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A175,1),INDEX(LinMotor!$AI$1:$AI$1305,A175,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A175<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A175,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A175,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A175,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A175,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A175,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A175,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A175<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A175,1),INDEX(LinMotor!$AK$1:$AK$1305,A175,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A175,1),INDEX(LinMotor!$AK$1:$AK$1305,A175,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A175,1),INDEX(LinMotor!$AK$1:$AK$1305,A175,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[601,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A176,1),INDEX(LinMotor!$B$1:$B$1291,A176,1))","v":"AKM2G-71N 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A176,1),INDEX(LinMotor!$R$1:$R$1305,A176,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A176,1),INDEX(LinMotor!$S$1:$S$1305,A176,1))","v":0.40161092754438976},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A176,1),INDEX(LinMotor!$T$1:$T$1305,A176,1))","v":0.50320691129242934},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A176,1),INDEX(LinMotor!$U$1:$U$1305,A176,1))","v":1.0379046726148879},{"$f":"IF(A176<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A176,1),INDEX(LinMotor!$V$1:$V$1305,A176,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A176,1),INDEX(LinMotor!$V$1:$V$1305,A176,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A176,1),INDEX(LinMotor!$V$1:$V$1305,A176,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A176<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A176,1),INDEX(LinMotor!$W$1:$W$1305,A176,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A176,1),INDEX(LinMotor!$X$1:$X$1305,A176,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A176,1),INDEX(LinMotor!$W$1:$W$1305,A176,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A176,1),INDEX(LinMotor!$X$1:$X$1305,A176,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A176,1),INDEX(LinMotor!$W$1:$W$1305,A176,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A176,1),INDEX(LinMotor!$X$1:$X$1305,A176,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A176<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A176,1),INDEX(LinMotor!$X$1:$X$1305,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A176,1),INDEX(LinMotor!$Z$1:$Z$1305,A176,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A176,1),INDEX(LinMotor!$X$1:$X$1305,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A176,1),INDEX(LinMotor!$Z$1:$Z$1305,A176,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A176,1),INDEX(LinMotor!$X$1:$X$1305,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A176,1),INDEX(LinMotor!$Z$1:$Z$1305,A176,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A176<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A176,1),INDEX(LinMotor!$Y$1:$Y$1305,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A176,1),INDEX(LinMotor!$AB$1:$AB$1305,A176,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A176,1),INDEX(LinMotor!$Y$1:$Y$1305,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A176,1),INDEX(LinMotor!$AB$1:$AB$1305,A176,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A176,1),INDEX(LinMotor!$Y$1:$Y$1305,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A176,1),INDEX(LinMotor!$AB$1:$AB$1305,A176,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A176,1),INDEX(LinMotor!$AD$1:$AD$1305,A176,1))","v":0.5537603515335332},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A176,1),INDEX(LinMotor!$AE$1:$AE$1305,A176,1))","v":0.78777551868348883},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A176,1),INDEX(LinMotor!$AF$1:$AF$1305,A176,1))","v":6.6451242184023984},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A176,1),INDEX(LinMotor!$AG$1:$AG$1305,A176,1))","v":18.906612448403731},{"$f":"IF(A176<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A176,1),INDEX(LinMotor!$AI$1:$AI$1305,A176,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A176,1),INDEX(LinMotor!$AI$1:$AI$1305,A176,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A176,1),INDEX(LinMotor!$AI$1:$AI$1305,A176,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A176<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A176,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A176,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A176,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A176,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A176,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A176,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A176<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A176,1),INDEX(LinMotor!$AK$1:$AK$1305,A176,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A176,1),INDEX(LinMotor!$AK$1:$AK$1305,A176,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A176,1),INDEX(LinMotor!$AK$1:$AK$1305,A176,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[603,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A177,1),INDEX(LinMotor!$B$1:$B$1291,A177,1))","v":"AKM2G-71P 240 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A177,1),INDEX(LinMotor!$R$1:$R$1305,A177,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A177,1),INDEX(LinMotor!$S$1:$S$1305,A177,1))","v":0.39057928728011787},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A177,1),INDEX(LinMotor!$T$1:$T$1305,A177,1))","v":0.49815463298920043},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A177,1),INDEX(LinMotor!$U$1:$U$1305,A177,1))","v":0.88888888888888884},{"$f":"IF(A177<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A177,1),INDEX(LinMotor!$V$1:$V$1305,A177,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A177,1),INDEX(LinMotor!$V$1:$V$1305,A177,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A177,1),INDEX(LinMotor!$V$1:$V$1305,A177,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A177<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A177,1),INDEX(LinMotor!$W$1:$W$1305,A177,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A177,1),INDEX(LinMotor!$X$1:$X$1305,A177,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A177,1),INDEX(LinMotor!$W$1:$W$1305,A177,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A177,1),INDEX(LinMotor!$X$1:$X$1305,A177,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A177,1),INDEX(LinMotor!$W$1:$W$1305,A177,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A177,1),INDEX(LinMotor!$X$1:$X$1305,A177,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A177<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A177,1),INDEX(LinMotor!$X$1:$X$1305,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A177,1),INDEX(LinMotor!$Z$1:$Z$1305,A177,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A177,1),INDEX(LinMotor!$X$1:$X$1305,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A177,1),INDEX(LinMotor!$Z$1:$Z$1305,A177,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A177,1),INDEX(LinMotor!$X$1:$X$1305,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A177,1),INDEX(LinMotor!$Z$1:$Z$1305,A177,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A177<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A177,1),INDEX(LinMotor!$Y$1:$Y$1305,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A177,1),INDEX(LinMotor!$AB$1:$AB$1305,A177,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A177,1),INDEX(LinMotor!$Y$1:$Y$1305,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A177,1),INDEX(LinMotor!$AB$1:$AB$1305,A177,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A177,1),INDEX(LinMotor!$Y$1:$Y$1305,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A177,1),INDEX(LinMotor!$AB$1:$AB$1305,A177,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A177,1),INDEX(LinMotor!$AD$1:$AD$1305,A177,1))","v":0.66658612963223807},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A177,1),INDEX(LinMotor!$AE$1:$AE$1305,A177,1))","v":0.94828066430548119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A177,1),INDEX(LinMotor!$AF$1:$AF$1305,A177,1))","v":7.9990335555868572},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A177,1),INDEX(LinMotor!$AG$1:$AG$1305,A177,1))","v":22.758735943331548},{"$f":"IF(A177<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A177,1),INDEX(LinMotor!$AI$1:$AI$1305,A177,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A177,1),INDEX(LinMotor!$AI$1:$AI$1305,A177,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A177,1),INDEX(LinMotor!$AI$1:$AI$1305,A177,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A177<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A177,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A177,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A177,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A177,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A177,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A177,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A177<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A177,1),INDEX(LinMotor!$AK$1:$AK$1305,A177,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A177,1),INDEX(LinMotor!$AK$1:$AK$1305,A177,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A177,1),INDEX(LinMotor!$AK$1:$AK$1305,A177,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[604,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A178,1),INDEX(LinMotor!$B$1:$B$1291,A178,1))","v":"AKM2G-71P 400 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A178,1),INDEX(LinMotor!$R$1:$R$1305,A178,1))","v":0.96525099099107114},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A178,1),INDEX(LinMotor!$S$1:$S$1305,A178,1))","v":0.39650574074176015},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A178,1),INDEX(LinMotor!$T$1:$T$1305,A178,1))","v":0.49815463298920043},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A178,1),INDEX(LinMotor!$U$1:$U$1305,A178,1))","v":0.85737378467475867},{"$f":"IF(A178<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A178,1),INDEX(LinMotor!$V$1:$V$1305,A178,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A178,1),INDEX(LinMotor!$V$1:$V$1305,A178,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A178,1),INDEX(LinMotor!$V$1:$V$1305,A178,1))/1000,\"0.0k\")),\"\")","v":24.808100342800333},{"$f":"IF(A178<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A178,1),INDEX(LinMotor!$W$1:$W$1305,A178,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A178,1),INDEX(LinMotor!$X$1:$X$1305,A178,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A178,1),INDEX(LinMotor!$W$1:$W$1305,A178,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A178,1),INDEX(LinMotor!$X$1:$X$1305,A178,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A178,1),INDEX(LinMotor!$W$1:$W$1305,A178,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A178,1),INDEX(LinMotor!$X$1:$X$1305,A178,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A178<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A178,1),INDEX(LinMotor!$X$1:$X$1305,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A178,1),INDEX(LinMotor!$Z$1:$Z$1305,A178,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A178,1),INDEX(LinMotor!$X$1:$X$1305,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A178,1),INDEX(LinMotor!$Z$1:$Z$1305,A178,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A178,1),INDEX(LinMotor!$X$1:$X$1305,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A178,1),INDEX(LinMotor!$Z$1:$Z$1305,A178,1)))/1000,\"0.0k\")),\"\")","v":-20.094561277668273},{"$f":"IF(A178<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A178,1),INDEX(LinMotor!$Y$1:$Y$1305,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A178,1),INDEX(LinMotor!$AB$1:$AB$1305,A178,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A178,1),INDEX(LinMotor!$Y$1:$Y$1305,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A178,1),INDEX(LinMotor!$AB$1:$AB$1305,A178,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A178,1),INDEX(LinMotor!$Y$1:$Y$1305,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A178,1),INDEX(LinMotor!$AB$1:$AB$1305,A178,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A178,1),INDEX(LinMotor!$AD$1:$AD$1305,A178,1))","v":0.66658612963223807},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A178,1),INDEX(LinMotor!$AE$1:$AE$1305,A178,1))","v":0.94828066430548119},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A178,1),INDEX(LinMotor!$AF$1:$AF$1305,A178,1))","v":7.9990335555868572},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A178,1),INDEX(LinMotor!$AG$1:$AG$1305,A178,1))","v":22.758735943331548},{"$f":"IF(A178<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A178,1),INDEX(LinMotor!$AI$1:$AI$1305,A178,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A178,1),INDEX(LinMotor!$AI$1:$AI$1305,A178,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A178,1),INDEX(LinMotor!$AI$1:$AI$1305,A178,1))/1000,\"0.0k\")),\"\")","v":412.28189586302858},{"$f":"IF(A178<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A178,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A178,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A178,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A178,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A178,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A178,1))/1000,\"0.0k\")),\"\")","v":334.21307738325606},{"$f":"IF(A178<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A178,1),INDEX(LinMotor!$AK$1:$AK$1305,A178,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A178,1),INDEX(LinMotor!$AK$1:$AK$1305,A178,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A178,1),INDEX(LinMotor!$AK$1:$AK$1305,A178,1))/1000,\"0.0k\")),\"\")","v":"3.2k"},""]
[630,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A179,1),INDEX(LinMotor!$B$1:$B$1291,A179,1))","v":"AKM2G-74R 480 V"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A179,1),INDEX(LinMotor!$R$1:$R$1305,A179,1))","v":0.28216702985792697},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A179,1),INDEX(LinMotor!$S$1:$S$1305,A179,1))","v":0.29621825536122692},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A179,1),INDEX(LinMotor!$T$1:$T$1305,A179,1))","v":0.33988579350522558},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A179,1),INDEX(LinMotor!$U$1:$U$1305,A179,1))","v":1.618226291416049},{"$f":"IF(A179<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A179,1),INDEX(LinMotor!$V$1:$V$1305,A179,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A179,1),INDEX(LinMotor!$V$1:$V$1305,A179,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A179,1),INDEX(LinMotor!$V$1:$V$1305,A179,1))/1000,\"0.0k\")),\"\")","v":55.367393687502869},{"$f":"IF(A179<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A179,1),INDEX(LinMotor!$W$1:$W$1305,A179,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A179,1),INDEX(LinMotor!$X$1:$X$1305,A179,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A179,1),INDEX(LinMotor!$W$1:$W$1305,A179,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A179,1),INDEX(LinMotor!$X$1:$X$1305,A179,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A179,1),INDEX(LinMotor!$W$1:$W$1305,A179,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A179,1),INDEX(LinMotor!$X$1:$X$1305,A179,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A179<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A179,1),INDEX(LinMotor!$X$1:$X$1305,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A179,1),INDEX(LinMotor!$Z$1:$Z$1305,A179,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A179,1),INDEX(LinMotor!$X$1:$X$1305,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A179,1),INDEX(LinMotor!$Z$1:$Z$1305,A179,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A179,1),INDEX(LinMotor!$X$1:$X$1305,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A179,1),INDEX(LinMotor!$Z$1:$Z$1305,A179,1)))/1000,\"0.0k\")),\"\")","v":-44.847588886877318},{"$f":"IF(A179<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A179,1),INDEX(LinMotor!$Y$1:$Y$1305,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A179,1),INDEX(LinMotor!$AB$1:$AB$1305,A179,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A179,1),INDEX(LinMotor!$Y$1:$Y$1305,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A179,1),INDEX(LinMotor!$AB$1:$AB$1305,A179,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A179,1),INDEX(LinMotor!$Y$1:$Y$1305,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A179,1),INDEX(LinMotor!$AB$1:$AB$1305,A179,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A179,1),INDEX(LinMotor!$AD$1:$AD$1305,A179,1))","v":0.73918990740070445},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A179,1),INDEX(LinMotor!$AE$1:$AE$1305,A179,1))","v":1.0515662797012792},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A179,1),INDEX(LinMotor!$AF$1:$AF$1305,A179,1))","v":8.8702788888084534},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A179,1),INDEX(LinMotor!$AG$1:$AG$1305,A179,1))","v":25.237590712830702},{"$f":"IF(A179<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A179,1),INDEX(LinMotor!$AI$1:$AI$1305,A179,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A179,1),INDEX(LinMotor!$AI$1:$AI$1305,A179,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A179,1),INDEX(LinMotor!$AI$1:$AI$1305,A179,1))/1000,\"0.0k\")),\"\")","v":920.14195859632116},{"$f":"IF(A179<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A179,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A179,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A179,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A179,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A179,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A179,1))/1000,\"0.0k\")),\"\")","v":745.90584427238775},{"$f":"IF(A179<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A179,1),INDEX(LinMotor!$AK$1:$AK$1305,A179,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A179,1),INDEX(LinMotor!$AK$1:$AK$1305,A179,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A179,1),INDEX(LinMotor!$AK$1:$AK$1305,A179,1))/1000,\"0.0k\")),\"\")","v":"7.2k"},""]
[833,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A180,1),INDEX(LinMotor!$B$1:$B$1291,A180,1))","v":"KBM-25H04-E (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A180,1),INDEX(LinMotor!$R$1:$R$1305,A180,1))","v":2.4509803921568629},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A180,1),INDEX(LinMotor!$S$1:$S$1305,A180,1))","v":0.43334171613244021},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A180,1),INDEX(LinMotor!$T$1:$T$1305,A180,1))","v":0.31888649071937475},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A180,1),INDEX(LinMotor!$U$1:$U$1305,A180,1))","v":0.7373715908494749},{"$f":"IF(A180<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A180,1),INDEX(LinMotor!$V$1:$V$1305,A180,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A180,1),INDEX(LinMotor!$V$1:$V$1305,A180,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A180,1),INDEX(LinMotor!$V$1:$V$1305,A180,1))/1000,\"0.0k\")),\"\")","v":17.156093200702362},{"$f":"IF(A180<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A180,1),INDEX(LinMotor!$W$1:$W$1305,A180,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A180,1),INDEX(LinMotor!$X$1:$X$1305,A180,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A180,1),INDEX(LinMotor!$W$1:$W$1305,A180,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A180,1),INDEX(LinMotor!$X$1:$X$1305,A180,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A180,1),INDEX(LinMotor!$W$1:$W$1305,A180,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A180,1),INDEX(LinMotor!$X$1:$X$1305,A180,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A180<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A180,1),INDEX(LinMotor!$X$1:$X$1305,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A180,1),INDEX(LinMotor!$Z$1:$Z$1305,A180,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A180,1),INDEX(LinMotor!$X$1:$X$1305,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A180,1),INDEX(LinMotor!$Z$1:$Z$1305,A180,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A180,1),INDEX(LinMotor!$X$1:$X$1305,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A180,1),INDEX(LinMotor!$Z$1:$Z$1305,A180,1)))/1000,\"0.0k\")),\"\")","v":-13.89643549256891},{"$f":"IF(A180<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A180,1),INDEX(LinMotor!$Y$1:$Y$1305,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A180,1),INDEX(LinMotor!$AB$1:$AB$1305,A180,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A180,1),INDEX(LinMotor!$Y$1:$Y$1305,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A180,1),INDEX(LinMotor!$AB$1:$AB$1305,A180,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A180,1),INDEX(LinMotor!$Y$1:$Y$1305,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A180,1),INDEX(LinMotor!$AB$1:$AB$1305,A180,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A180,1),INDEX(LinMotor!$AD$1:$AD$1305,A180,1))","v":0.47495532712708094},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A180,1),INDEX(LinMotor!$AE$1:$AE$1305,A180,1))","v":0.67566805413725062},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A180,1),INDEX(LinMotor!$AF$1:$AF$1305,A180,1))","v":5.6994639255249711},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A180,1),INDEX(LinMotor!$AG$1:$AG$1305,A180,1))","v":16.216033299294015},{"$f":"IF(A180<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A180,1),INDEX(LinMotor!$AI$1:$AI$1305,A180,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A180,1),INDEX(LinMotor!$AI$1:$AI$1305,A180,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A180,1),INDEX(LinMotor!$AI$1:$AI$1305,A180,1))/1000,\"0.0k\")),\"\")","v":285.11439943611452},{"$f":"IF(A180<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A180,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A180,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A180,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A180,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A180,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A180,1))/1000,\"0.0k\")),\"\")","v":231.12574623815235},{"$f":"IF(A180<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A180,1),INDEX(LinMotor!$AK$1:$AK$1305,A180,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A180,1),INDEX(LinMotor!$AK$1:$AK$1305,A180,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A180,1),INDEX(LinMotor!$AK$1:$AK$1305,A180,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[834,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A181,1),INDEX(LinMotor!$B$1:$B$1291,A181,1))","v":"KBM-25H04-E (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A181,1),INDEX(LinMotor!$R$1:$R$1305,A181,1))","v":2.4509803921568629},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A181,1),INDEX(LinMotor!$S$1:$S$1305,A181,1))","v":0.44288039114206296},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A181,1),INDEX(LinMotor!$T$1:$T$1305,A181,1))","v":0.31888649071937475},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A181,1),INDEX(LinMotor!$U$1:$U$1305,A181,1))","v":0.7373715908494749},{"$f":"IF(A181<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A181,1),INDEX(LinMotor!$V$1:$V$1305,A181,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A181,1),INDEX(LinMotor!$V$1:$V$1305,A181,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A181,1),INDEX(LinMotor!$V$1:$V$1305,A181,1))/1000,\"0.0k\")),\"\")","v":17.156093200702362},{"$f":"IF(A181<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A181,1),INDEX(LinMotor!$W$1:$W$1305,A181,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A181,1),INDEX(LinMotor!$X$1:$X$1305,A181,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A181,1),INDEX(LinMotor!$W$1:$W$1305,A181,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A181,1),INDEX(LinMotor!$X$1:$X$1305,A181,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A181,1),INDEX(LinMotor!$W$1:$W$1305,A181,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A181,1),INDEX(LinMotor!$X$1:$X$1305,A181,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A181<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A181,1),INDEX(LinMotor!$X$1:$X$1305,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A181,1),INDEX(LinMotor!$Z$1:$Z$1305,A181,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A181,1),INDEX(LinMotor!$X$1:$X$1305,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A181,1),INDEX(LinMotor!$Z$1:$Z$1305,A181,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A181,1),INDEX(LinMotor!$X$1:$X$1305,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A181,1),INDEX(LinMotor!$Z$1:$Z$1305,A181,1)))/1000,\"0.0k\")),\"\")","v":-13.89643549256891},{"$f":"IF(A181<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A181,1),INDEX(LinMotor!$Y$1:$Y$1305,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A181,1),INDEX(LinMotor!$AB$1:$AB$1305,A181,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A181,1),INDEX(LinMotor!$Y$1:$Y$1305,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A181,1),INDEX(LinMotor!$AB$1:$AB$1305,A181,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A181,1),INDEX(LinMotor!$Y$1:$Y$1305,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A181,1),INDEX(LinMotor!$AB$1:$AB$1305,A181,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A181,1),INDEX(LinMotor!$AD$1:$AD$1305,A181,1))","v":0.47495532712708094},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A181,1),INDEX(LinMotor!$AE$1:$AE$1305,A181,1))","v":0.67566805413725062},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A181,1),INDEX(LinMotor!$AF$1:$AF$1305,A181,1))","v":5.6994639255249711},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A181,1),INDEX(LinMotor!$AG$1:$AG$1305,A181,1))","v":16.216033299294015},{"$f":"IF(A181<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A181,1),INDEX(LinMotor!$AI$1:$AI$1305,A181,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A181,1),INDEX(LinMotor!$AI$1:$AI$1305,A181,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A181,1),INDEX(LinMotor!$AI$1:$AI$1305,A181,1))/1000,\"0.0k\")),\"\")","v":285.11439943611452},{"$f":"IF(A181<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A181,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A181,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A181,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A181,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A181,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A181,1))/1000,\"0.0k\")),\"\")","v":231.12574623815235},{"$f":"IF(A181<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A181,1),INDEX(LinMotor!$AK$1:$AK$1305,A181,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A181,1),INDEX(LinMotor!$AK$1:$AK$1305,A181,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A181,1),INDEX(LinMotor!$AK$1:$AK$1305,A181,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[836,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A182,1),INDEX(LinMotor!$B$1:$B$1291,A182,1))","v":"KBM-25H04-F (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A182,1),INDEX(LinMotor!$R$1:$R$1305,A182,1))","v":2.4509803921568629},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A182,1),INDEX(LinMotor!$S$1:$S$1305,A182,1))","v":0.4452679788320843},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A182,1),INDEX(LinMotor!$T$1:$T$1305,A182,1))","v":0.31711817376529317},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A182,1),INDEX(LinMotor!$U$1:$U$1305,A182,1))","v":0.51839144001431858},{"$f":"IF(A182<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A182,1),INDEX(LinMotor!$V$1:$V$1305,A182,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A182,1),INDEX(LinMotor!$V$1:$V$1305,A182,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A182,1),INDEX(LinMotor!$V$1:$V$1305,A182,1))/1000,\"0.0k\")),\"\")","v":17.156093200702362},{"$f":"IF(A182<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A182,1),INDEX(LinMotor!$W$1:$W$1305,A182,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A182,1),INDEX(LinMotor!$X$1:$X$1305,A182,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A182,1),INDEX(LinMotor!$W$1:$W$1305,A182,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A182,1),INDEX(LinMotor!$X$1:$X$1305,A182,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A182,1),INDEX(LinMotor!$W$1:$W$1305,A182,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A182,1),INDEX(LinMotor!$X$1:$X$1305,A182,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A182<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A182,1),INDEX(LinMotor!$X$1:$X$1305,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A182,1),INDEX(LinMotor!$Z$1:$Z$1305,A182,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A182,1),INDEX(LinMotor!$X$1:$X$1305,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A182,1),INDEX(LinMotor!$Z$1:$Z$1305,A182,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A182,1),INDEX(LinMotor!$X$1:$X$1305,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A182,1),INDEX(LinMotor!$Z$1:$Z$1305,A182,1)))/1000,\"0.0k\")),\"\")","v":-13.89643549256891},{"$f":"IF(A182<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A182,1),INDEX(LinMotor!$Y$1:$Y$1305,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A182,1),INDEX(LinMotor!$AB$1:$AB$1305,A182,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A182,1),INDEX(LinMotor!$Y$1:$Y$1305,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A182,1),INDEX(LinMotor!$AB$1:$AB$1305,A182,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A182,1),INDEX(LinMotor!$Y$1:$Y$1305,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A182,1),INDEX(LinMotor!$AB$1:$AB$1305,A182,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A182,1),INDEX(LinMotor!$AD$1:$AD$1305,A182,1))","v":0.67229558648412979},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A182,1),INDEX(LinMotor!$AE$1:$AE$1305,A182,1))","v":0.95640289682076374},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A182,1),INDEX(LinMotor!$AF$1:$AF$1305,A182,1))","v":8.0675470378095575},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A182,1),INDEX(LinMotor!$AG$1:$AG$1305,A182,1))","v":22.953669523698331},{"$f":"IF(A182<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A182,1),INDEX(LinMotor!$AI$1:$AI$1305,A182,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A182,1),INDEX(LinMotor!$AI$1:$AI$1305,A182,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A182,1),INDEX(LinMotor!$AI$1:$AI$1305,A182,1))/1000,\"0.0k\")),\"\")","v":285.11439943611452},{"$f":"IF(A182<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A182,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A182,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A182,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A182,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A182,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A182,1))/1000,\"0.0k\")),\"\")","v":231.12574623815235},{"$f":"IF(A182<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A182,1),INDEX(LinMotor!$AK$1:$AK$1305,A182,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A182,1),INDEX(LinMotor!$AK$1:$AK$1305,A182,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A182,1),INDEX(LinMotor!$AK$1:$AK$1305,A182,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[838,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A183,1),INDEX(LinMotor!$B$1:$B$1291,A183,1))","v":"KBM-25H04-G (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A183,1),INDEX(LinMotor!$R$1:$R$1305,A183,1))","v":2.4509803921568629},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A183,1),INDEX(LinMotor!$S$1:$S$1305,A183,1))","v":0.46024165104719211},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A183,1),INDEX(LinMotor!$T$1:$T$1305,A183,1))","v":0.31479070093031858},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A183,1),INDEX(LinMotor!$U$1:$U$1305,A183,1))","v":0.47840824985681168},{"$f":"IF(A183<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A183,1),INDEX(LinMotor!$V$1:$V$1305,A183,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A183,1),INDEX(LinMotor!$V$1:$V$1305,A183,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A183,1),INDEX(LinMotor!$V$1:$V$1305,A183,1))/1000,\"0.0k\")),\"\")","v":17.156093200702362},{"$f":"IF(A183<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A183,1),INDEX(LinMotor!$W$1:$W$1305,A183,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A183,1),INDEX(LinMotor!$X$1:$X$1305,A183,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A183,1),INDEX(LinMotor!$W$1:$W$1305,A183,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A183,1),INDEX(LinMotor!$X$1:$X$1305,A183,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A183,1),INDEX(LinMotor!$W$1:$W$1305,A183,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A183,1),INDEX(LinMotor!$X$1:$X$1305,A183,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A183<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A183,1),INDEX(LinMotor!$X$1:$X$1305,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A183,1),INDEX(LinMotor!$Z$1:$Z$1305,A183,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A183,1),INDEX(LinMotor!$X$1:$X$1305,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A183,1),INDEX(LinMotor!$Z$1:$Z$1305,A183,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A183,1),INDEX(LinMotor!$X$1:$X$1305,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A183,1),INDEX(LinMotor!$Z$1:$Z$1305,A183,1)))/1000,\"0.0k\")),\"\")","v":-13.89643549256891},{"$f":"IF(A183<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A183,1),INDEX(LinMotor!$Y$1:$Y$1305,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A183,1),INDEX(LinMotor!$AB$1:$AB$1305,A183,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A183,1),INDEX(LinMotor!$Y$1:$Y$1305,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A183,1),INDEX(LinMotor!$AB$1:$AB$1305,A183,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A183,1),INDEX(LinMotor!$Y$1:$Y$1305,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A183,1),INDEX(LinMotor!$AB$1:$AB$1305,A183,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A183,1),INDEX(LinMotor!$AD$1:$AD$1305,A183,1))","v":0.72860900545509433},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A183,1),INDEX(LinMotor!$AE$1:$AE$1305,A183,1))","v":1.036513964209101},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A183,1),INDEX(LinMotor!$AF$1:$AF$1305,A183,1))","v":8.7433080654611324},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A183,1),INDEX(LinMotor!$AG$1:$AG$1305,A183,1))","v":24.876335141018426},{"$f":"IF(A183<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A183,1),INDEX(LinMotor!$AI$1:$AI$1305,A183,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A183,1),INDEX(LinMotor!$AI$1:$AI$1305,A183,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A183,1),INDEX(LinMotor!$AI$1:$AI$1305,A183,1))/1000,\"0.0k\")),\"\")","v":285.11439943611452},{"$f":"IF(A183<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A183,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A183,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A183,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A183,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A183,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A183,1))/1000,\"0.0k\")),\"\")","v":231.12574623815235},{"$f":"IF(A183<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A183,1),INDEX(LinMotor!$AK$1:$AK$1305,A183,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A183,1),INDEX(LinMotor!$AK$1:$AK$1305,A183,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A183,1),INDEX(LinMotor!$AK$1:$AK$1305,A183,1))/1000,\"0.0k\")),\"\")","v":"2.2k"},""]
[848,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A184,1),INDEX(LinMotor!$B$1:$B$1291,A184,1))","v":"KBM-35H01-C (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A184,1),INDEX(LinMotor!$R$1:$R$1305,A184,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A184,1),INDEX(LinMotor!$S$1:$S$1305,A184,1))","v":0.56966940109281294},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A184,1),INDEX(LinMotor!$T$1:$T$1305,A184,1))","v":0.48022152592206641},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A184,1),INDEX(LinMotor!$U$1:$U$1305,A184,1))","v":1.1863915436721184},{"$f":"IF(A184<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A184,1),INDEX(LinMotor!$V$1:$V$1305,A184,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A184,1),INDEX(LinMotor!$V$1:$V$1305,A184,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A184,1),INDEX(LinMotor!$V$1:$V$1305,A184,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A184<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A184,1),INDEX(LinMotor!$W$1:$W$1305,A184,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A184,1),INDEX(LinMotor!$X$1:$X$1305,A184,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A184,1),INDEX(LinMotor!$W$1:$W$1305,A184,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A184,1),INDEX(LinMotor!$X$1:$X$1305,A184,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A184,1),INDEX(LinMotor!$W$1:$W$1305,A184,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A184,1),INDEX(LinMotor!$X$1:$X$1305,A184,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A184<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A184,1),INDEX(LinMotor!$X$1:$X$1305,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A184,1),INDEX(LinMotor!$Z$1:$Z$1305,A184,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A184,1),INDEX(LinMotor!$X$1:$X$1305,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A184,1),INDEX(LinMotor!$Z$1:$Z$1305,A184,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A184,1),INDEX(LinMotor!$X$1:$X$1305,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A184,1),INDEX(LinMotor!$Z$1:$Z$1305,A184,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A184<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A184,1),INDEX(LinMotor!$Y$1:$Y$1305,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A184,1),INDEX(LinMotor!$AB$1:$AB$1305,A184,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A184,1),INDEX(LinMotor!$Y$1:$Y$1305,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A184,1),INDEX(LinMotor!$AB$1:$AB$1305,A184,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A184,1),INDEX(LinMotor!$Y$1:$Y$1305,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A184,1),INDEX(LinMotor!$AB$1:$AB$1305,A184,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A184,1),INDEX(LinMotor!$AD$1:$AD$1305,A184,1))","v":0.38349870075998771},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A184,1),INDEX(LinMotor!$AE$1:$AE$1305,A184,1))","v":0.54556251105555875},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A184,1),INDEX(LinMotor!$AF$1:$AF$1305,A184,1))","v":4.6019844091198525},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A184,1),INDEX(LinMotor!$AG$1:$AG$1305,A184,1))","v":13.093500265333411},{"$f":"IF(A184<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A184,1),INDEX(LinMotor!$AI$1:$AI$1305,A184,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A184,1),INDEX(LinMotor!$AI$1:$AI$1305,A184,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A184,1),INDEX(LinMotor!$AI$1:$AI$1305,A184,1))/1000,\"0.0k\")),\"\")","v":325.61360390147172},{"$f":"IF(A184<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A184,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A184,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A184,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A184,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A184,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A184,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A184<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A184,1),INDEX(LinMotor!$AK$1:$AK$1305,A184,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A184,1),INDEX(LinMotor!$AK$1:$AK$1305,A184,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A184,1),INDEX(LinMotor!$AK$1:$AK$1305,A184,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[849,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A185,1),INDEX(LinMotor!$B$1:$B$1291,A185,1))","v":"KBM-35H01-C (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A185,1),INDEX(LinMotor!$R$1:$R$1305,A185,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A185,1),INDEX(LinMotor!$S$1:$S$1305,A185,1))","v":0.56966630247097405},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A185,1),INDEX(LinMotor!$T$1:$T$1305,A185,1))","v":0.48022152592206641},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A185,1),INDEX(LinMotor!$U$1:$U$1305,A185,1))","v":1.1863915436721184},{"$f":"IF(A185<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A185,1),INDEX(LinMotor!$V$1:$V$1305,A185,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A185,1),INDEX(LinMotor!$V$1:$V$1305,A185,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A185,1),INDEX(LinMotor!$V$1:$V$1305,A185,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A185<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A185,1),INDEX(LinMotor!$W$1:$W$1305,A185,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A185,1),INDEX(LinMotor!$X$1:$X$1305,A185,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A185,1),INDEX(LinMotor!$W$1:$W$1305,A185,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A185,1),INDEX(LinMotor!$X$1:$X$1305,A185,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A185,1),INDEX(LinMotor!$W$1:$W$1305,A185,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A185,1),INDEX(LinMotor!$X$1:$X$1305,A185,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A185<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A185,1),INDEX(LinMotor!$X$1:$X$1305,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A185,1),INDEX(LinMotor!$Z$1:$Z$1305,A185,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A185,1),INDEX(LinMotor!$X$1:$X$1305,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A185,1),INDEX(LinMotor!$Z$1:$Z$1305,A185,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A185,1),INDEX(LinMotor!$X$1:$X$1305,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A185,1),INDEX(LinMotor!$Z$1:$Z$1305,A185,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A185<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A185,1),INDEX(LinMotor!$Y$1:$Y$1305,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A185,1),INDEX(LinMotor!$AB$1:$AB$1305,A185,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A185,1),INDEX(LinMotor!$Y$1:$Y$1305,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A185,1),INDEX(LinMotor!$AB$1:$AB$1305,A185,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A185,1),INDEX(LinMotor!$Y$1:$Y$1305,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A185,1),INDEX(LinMotor!$AB$1:$AB$1305,A185,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A185,1),INDEX(LinMotor!$AD$1:$AD$1305,A185,1))","v":0.38349870075998771},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A185,1),INDEX(LinMotor!$AE$1:$AE$1305,A185,1))","v":0.54556251105555875},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A185,1),INDEX(LinMotor!$AF$1:$AF$1305,A185,1))","v":4.6019844091198525},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A185,1),INDEX(LinMotor!$AG$1:$AG$1305,A185,1))","v":13.093500265333411},{"$f":"IF(A185<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A185,1),INDEX(LinMotor!$AI$1:$AI$1305,A185,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A185,1),INDEX(LinMotor!$AI$1:$AI$1305,A185,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A185,1),INDEX(LinMotor!$AI$1:$AI$1305,A185,1))/1000,\"0.0k\")),\"\")","v":325.61360390147166},{"$f":"IF(A185<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A185,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A185,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A185,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A185,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A185,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A185,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A185<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A185,1),INDEX(LinMotor!$AK$1:$AK$1305,A185,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A185,1),INDEX(LinMotor!$AK$1:$AK$1305,A185,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A185,1),INDEX(LinMotor!$AK$1:$AK$1305,A185,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[850,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A186,1),INDEX(LinMotor!$B$1:$B$1291,A186,1))","v":"KBM-35H01-C (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A186,1),INDEX(LinMotor!$R$1:$R$1305,A186,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A186,1),INDEX(LinMotor!$S$1:$S$1305,A186,1))","v":0.57095659280697675},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A186,1),INDEX(LinMotor!$T$1:$T$1305,A186,1))","v":0.48022152592206641},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A186,1),INDEX(LinMotor!$U$1:$U$1305,A186,1))","v":1.1863915436721184},{"$f":"IF(A186<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A186,1),INDEX(LinMotor!$V$1:$V$1305,A186,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A186,1),INDEX(LinMotor!$V$1:$V$1305,A186,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A186,1),INDEX(LinMotor!$V$1:$V$1305,A186,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A186<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A186,1),INDEX(LinMotor!$W$1:$W$1305,A186,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A186,1),INDEX(LinMotor!$X$1:$X$1305,A186,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A186,1),INDEX(LinMotor!$W$1:$W$1305,A186,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A186,1),INDEX(LinMotor!$X$1:$X$1305,A186,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A186,1),INDEX(LinMotor!$W$1:$W$1305,A186,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A186,1),INDEX(LinMotor!$X$1:$X$1305,A186,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A186<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A186,1),INDEX(LinMotor!$X$1:$X$1305,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A186,1),INDEX(LinMotor!$Z$1:$Z$1305,A186,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A186,1),INDEX(LinMotor!$X$1:$X$1305,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A186,1),INDEX(LinMotor!$Z$1:$Z$1305,A186,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A186,1),INDEX(LinMotor!$X$1:$X$1305,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A186,1),INDEX(LinMotor!$Z$1:$Z$1305,A186,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A186<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A186,1),INDEX(LinMotor!$Y$1:$Y$1305,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A186,1),INDEX(LinMotor!$AB$1:$AB$1305,A186,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A186,1),INDEX(LinMotor!$Y$1:$Y$1305,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A186,1),INDEX(LinMotor!$AB$1:$AB$1305,A186,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A186,1),INDEX(LinMotor!$Y$1:$Y$1305,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A186,1),INDEX(LinMotor!$AB$1:$AB$1305,A186,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A186,1),INDEX(LinMotor!$AD$1:$AD$1305,A186,1))","v":0.38349870075998771},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A186,1),INDEX(LinMotor!$AE$1:$AE$1305,A186,1))","v":0.54556251105555875},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A186,1),INDEX(LinMotor!$AF$1:$AF$1305,A186,1))","v":4.6019844091198525},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A186,1),INDEX(LinMotor!$AG$1:$AG$1305,A186,1))","v":13.093500265333411},{"$f":"IF(A186<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A186,1),INDEX(LinMotor!$AI$1:$AI$1305,A186,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A186,1),INDEX(LinMotor!$AI$1:$AI$1305,A186,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A186,1),INDEX(LinMotor!$AI$1:$AI$1305,A186,1))/1000,\"0.0k\")),\"\")","v":325.61360390147166},{"$f":"IF(A186<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A186,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A186,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A186,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A186,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A186,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A186,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A186<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A186,1),INDEX(LinMotor!$AK$1:$AK$1305,A186,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A186,1),INDEX(LinMotor!$AK$1:$AK$1305,A186,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A186,1),INDEX(LinMotor!$AK$1:$AK$1305,A186,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[852,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A187,1),INDEX(LinMotor!$B$1:$B$1291,A187,1))","v":"KBM-35H01-D (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A187,1),INDEX(LinMotor!$R$1:$R$1305,A187,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A187,1),INDEX(LinMotor!$S$1:$S$1305,A187,1))","v":0.55981358063507658},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A187,1),INDEX(LinMotor!$T$1:$T$1305,A187,1))","v":0.47555918101020161},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A187,1),INDEX(LinMotor!$U$1:$U$1305,A187,1))","v":0.9321740037022429},{"$f":"IF(A187<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A187,1),INDEX(LinMotor!$V$1:$V$1305,A187,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A187,1),INDEX(LinMotor!$V$1:$V$1305,A187,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A187,1),INDEX(LinMotor!$V$1:$V$1305,A187,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A187<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A187,1),INDEX(LinMotor!$W$1:$W$1305,A187,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A187,1),INDEX(LinMotor!$X$1:$X$1305,A187,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A187,1),INDEX(LinMotor!$W$1:$W$1305,A187,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A187,1),INDEX(LinMotor!$X$1:$X$1305,A187,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A187,1),INDEX(LinMotor!$W$1:$W$1305,A187,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A187,1),INDEX(LinMotor!$X$1:$X$1305,A187,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A187<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A187,1),INDEX(LinMotor!$X$1:$X$1305,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A187,1),INDEX(LinMotor!$Z$1:$Z$1305,A187,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A187,1),INDEX(LinMotor!$X$1:$X$1305,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A187,1),INDEX(LinMotor!$Z$1:$Z$1305,A187,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A187,1),INDEX(LinMotor!$X$1:$X$1305,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A187,1),INDEX(LinMotor!$Z$1:$Z$1305,A187,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A187<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A187,1),INDEX(LinMotor!$Y$1:$Y$1305,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A187,1),INDEX(LinMotor!$AB$1:$AB$1305,A187,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A187,1),INDEX(LinMotor!$Y$1:$Y$1305,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A187,1),INDEX(LinMotor!$AB$1:$AB$1305,A187,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A187,1),INDEX(LinMotor!$Y$1:$Y$1305,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A187,1),INDEX(LinMotor!$AB$1:$AB$1305,A187,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A187,1),INDEX(LinMotor!$AD$1:$AD$1305,A187,1))","v":0.47950637327608808},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A187,1),INDEX(LinMotor!$AE$1:$AE$1305,A187,1))","v":0.68214233986510753},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A187,1),INDEX(LinMotor!$AF$1:$AF$1305,A187,1))","v":5.7540764793130572},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A187,1),INDEX(LinMotor!$AG$1:$AG$1305,A187,1))","v":16.371416156762582},{"$f":"IF(A187<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A187,1),INDEX(LinMotor!$AI$1:$AI$1305,A187,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A187,1),INDEX(LinMotor!$AI$1:$AI$1305,A187,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A187,1),INDEX(LinMotor!$AI$1:$AI$1305,A187,1))/1000,\"0.0k\")),\"\")","v":325.61360390147166},{"$f":"IF(A187<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A187,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A187,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A187,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A187,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A187,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A187,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A187<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A187,1),INDEX(LinMotor!$AK$1:$AK$1305,A187,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A187,1),INDEX(LinMotor!$AK$1:$AK$1305,A187,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A187,1),INDEX(LinMotor!$AK$1:$AK$1305,A187,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[853,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A188,1),INDEX(LinMotor!$B$1:$B$1291,A188,1))","v":"KBM-35H01-D (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A188,1),INDEX(LinMotor!$R$1:$R$1305,A188,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A188,1),INDEX(LinMotor!$S$1:$S$1305,A188,1))","v":0.56269892136303423},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A188,1),INDEX(LinMotor!$T$1:$T$1305,A188,1))","v":0.47555918101020161},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A188,1),INDEX(LinMotor!$U$1:$U$1305,A188,1))","v":0.9321740037022429},{"$f":"IF(A188<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A188,1),INDEX(LinMotor!$V$1:$V$1305,A188,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A188,1),INDEX(LinMotor!$V$1:$V$1305,A188,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A188,1),INDEX(LinMotor!$V$1:$V$1305,A188,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A188<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A188,1),INDEX(LinMotor!$W$1:$W$1305,A188,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A188,1),INDEX(LinMotor!$X$1:$X$1305,A188,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A188,1),INDEX(LinMotor!$W$1:$W$1305,A188,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A188,1),INDEX(LinMotor!$X$1:$X$1305,A188,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A188,1),INDEX(LinMotor!$W$1:$W$1305,A188,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A188,1),INDEX(LinMotor!$X$1:$X$1305,A188,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A188<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A188,1),INDEX(LinMotor!$X$1:$X$1305,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A188,1),INDEX(LinMotor!$Z$1:$Z$1305,A188,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A188,1),INDEX(LinMotor!$X$1:$X$1305,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A188,1),INDEX(LinMotor!$Z$1:$Z$1305,A188,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A188,1),INDEX(LinMotor!$X$1:$X$1305,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A188,1),INDEX(LinMotor!$Z$1:$Z$1305,A188,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A188<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A188,1),INDEX(LinMotor!$Y$1:$Y$1305,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A188,1),INDEX(LinMotor!$AB$1:$AB$1305,A188,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A188,1),INDEX(LinMotor!$Y$1:$Y$1305,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A188,1),INDEX(LinMotor!$AB$1:$AB$1305,A188,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A188,1),INDEX(LinMotor!$Y$1:$Y$1305,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A188,1),INDEX(LinMotor!$AB$1:$AB$1305,A188,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A188,1),INDEX(LinMotor!$AD$1:$AD$1305,A188,1))","v":0.47950637327608808},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A188,1),INDEX(LinMotor!$AE$1:$AE$1305,A188,1))","v":0.68214233986510753},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A188,1),INDEX(LinMotor!$AF$1:$AF$1305,A188,1))","v":5.7540764793130572},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A188,1),INDEX(LinMotor!$AG$1:$AG$1305,A188,1))","v":16.371416156762582},{"$f":"IF(A188<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A188,1),INDEX(LinMotor!$AI$1:$AI$1305,A188,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A188,1),INDEX(LinMotor!$AI$1:$AI$1305,A188,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A188,1),INDEX(LinMotor!$AI$1:$AI$1305,A188,1))/1000,\"0.0k\")),\"\")","v":325.61360390147161},{"$f":"IF(A188<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A188,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A188,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A188,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A188,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A188,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A188,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A188<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A188,1),INDEX(LinMotor!$AK$1:$AK$1305,A188,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A188,1),INDEX(LinMotor!$AK$1:$AK$1305,A188,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A188,1),INDEX(LinMotor!$AK$1:$AK$1305,A188,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[854,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A189,1),INDEX(LinMotor!$B$1:$B$1291,A189,1))","v":"KBM-35H01-D (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A189,1),INDEX(LinMotor!$R$1:$R$1305,A189,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A189,1),INDEX(LinMotor!$S$1:$S$1305,A189,1))","v":0.5669755628548554},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A189,1),INDEX(LinMotor!$T$1:$T$1305,A189,1))","v":0.47555918101020161},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A189,1),INDEX(LinMotor!$U$1:$U$1305,A189,1))","v":0.9321740037022429},{"$f":"IF(A189<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A189,1),INDEX(LinMotor!$V$1:$V$1305,A189,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A189,1),INDEX(LinMotor!$V$1:$V$1305,A189,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A189,1),INDEX(LinMotor!$V$1:$V$1305,A189,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A189<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A189,1),INDEX(LinMotor!$W$1:$W$1305,A189,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A189,1),INDEX(LinMotor!$X$1:$X$1305,A189,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A189,1),INDEX(LinMotor!$W$1:$W$1305,A189,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A189,1),INDEX(LinMotor!$X$1:$X$1305,A189,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A189,1),INDEX(LinMotor!$W$1:$W$1305,A189,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A189,1),INDEX(LinMotor!$X$1:$X$1305,A189,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A189<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A189,1),INDEX(LinMotor!$X$1:$X$1305,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A189,1),INDEX(LinMotor!$Z$1:$Z$1305,A189,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A189,1),INDEX(LinMotor!$X$1:$X$1305,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A189,1),INDEX(LinMotor!$Z$1:$Z$1305,A189,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A189,1),INDEX(LinMotor!$X$1:$X$1305,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A189,1),INDEX(LinMotor!$Z$1:$Z$1305,A189,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A189<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A189,1),INDEX(LinMotor!$Y$1:$Y$1305,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A189,1),INDEX(LinMotor!$AB$1:$AB$1305,A189,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A189,1),INDEX(LinMotor!$Y$1:$Y$1305,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A189,1),INDEX(LinMotor!$AB$1:$AB$1305,A189,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A189,1),INDEX(LinMotor!$Y$1:$Y$1305,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A189,1),INDEX(LinMotor!$AB$1:$AB$1305,A189,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A189,1),INDEX(LinMotor!$AD$1:$AD$1305,A189,1))","v":0.47950637327608808},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A189,1),INDEX(LinMotor!$AE$1:$AE$1305,A189,1))","v":0.68214233986510753},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A189,1),INDEX(LinMotor!$AF$1:$AF$1305,A189,1))","v":5.7540764793130572},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A189,1),INDEX(LinMotor!$AG$1:$AG$1305,A189,1))","v":16.371416156762582},{"$f":"IF(A189<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A189,1),INDEX(LinMotor!$AI$1:$AI$1305,A189,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A189,1),INDEX(LinMotor!$AI$1:$AI$1305,A189,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A189,1),INDEX(LinMotor!$AI$1:$AI$1305,A189,1))/1000,\"0.0k\")),\"\")","v":325.61360390147172},{"$f":"IF(A189<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A189,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A189,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A189,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A189,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A189,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A189,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A189<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A189,1),INDEX(LinMotor!$AK$1:$AK$1305,A189,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A189,1),INDEX(LinMotor!$AK$1:$AK$1305,A189,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A189,1),INDEX(LinMotor!$AK$1:$AK$1305,A189,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[856,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A190,1),INDEX(LinMotor!$B$1:$B$1291,A190,1))","v":"KBM-35H01-E (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A190,1),INDEX(LinMotor!$R$1:$R$1305,A190,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A190,1),INDEX(LinMotor!$S$1:$S$1305,A190,1))","v":0.58257385771263459},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A190,1),INDEX(LinMotor!$T$1:$T$1305,A190,1))","v":0.47671625930949652},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A190,1),INDEX(LinMotor!$U$1:$U$1305,A190,1))","v":0.7274857233796207},{"$f":"IF(A190<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A190,1),INDEX(LinMotor!$V$1:$V$1305,A190,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A190,1),INDEX(LinMotor!$V$1:$V$1305,A190,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A190,1),INDEX(LinMotor!$V$1:$V$1305,A190,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A190<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A190,1),INDEX(LinMotor!$W$1:$W$1305,A190,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A190,1),INDEX(LinMotor!$X$1:$X$1305,A190,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A190,1),INDEX(LinMotor!$W$1:$W$1305,A190,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A190,1),INDEX(LinMotor!$X$1:$X$1305,A190,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A190,1),INDEX(LinMotor!$W$1:$W$1305,A190,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A190,1),INDEX(LinMotor!$X$1:$X$1305,A190,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A190<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A190,1),INDEX(LinMotor!$X$1:$X$1305,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A190,1),INDEX(LinMotor!$Z$1:$Z$1305,A190,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A190,1),INDEX(LinMotor!$X$1:$X$1305,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A190,1),INDEX(LinMotor!$Z$1:$Z$1305,A190,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A190,1),INDEX(LinMotor!$X$1:$X$1305,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A190,1),INDEX(LinMotor!$Z$1:$Z$1305,A190,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A190<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A190,1),INDEX(LinMotor!$Y$1:$Y$1305,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A190,1),INDEX(LinMotor!$AB$1:$AB$1305,A190,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A190,1),INDEX(LinMotor!$Y$1:$Y$1305,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A190,1),INDEX(LinMotor!$AB$1:$AB$1305,A190,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A190,1),INDEX(LinMotor!$Y$1:$Y$1305,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A190,1),INDEX(LinMotor!$AB$1:$AB$1305,A190,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A190,1),INDEX(LinMotor!$AD$1:$AD$1305,A190,1))","v":0.60208812414399082},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A190,1),INDEX(LinMotor!$AE$1:$AE$1305,A190,1))","v":0.8565262626282103},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A190,1),INDEX(LinMotor!$AF$1:$AF$1305,A190,1))","v":7.2250574897278899},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A190,1),INDEX(LinMotor!$AG$1:$AG$1305,A190,1))","v":20.556630303077046},{"$f":"IF(A190<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A190,1),INDEX(LinMotor!$AI$1:$AI$1305,A190,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A190,1),INDEX(LinMotor!$AI$1:$AI$1305,A190,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A190,1),INDEX(LinMotor!$AI$1:$AI$1305,A190,1))/1000,\"0.0k\")),\"\")","v":325.61360390147166},{"$f":"IF(A190<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A190,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A190,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A190,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A190,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A190,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A190,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A190<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A190,1),INDEX(LinMotor!$AK$1:$AK$1305,A190,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A190,1),INDEX(LinMotor!$AK$1:$AK$1305,A190,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A190,1),INDEX(LinMotor!$AK$1:$AK$1305,A190,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[857,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A191,1),INDEX(LinMotor!$B$1:$B$1291,A191,1))","v":"KBM-35H01-E (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A191,1),INDEX(LinMotor!$R$1:$R$1305,A191,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A191,1),INDEX(LinMotor!$S$1:$S$1305,A191,1))","v":0.58976914483206866},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A191,1),INDEX(LinMotor!$T$1:$T$1305,A191,1))","v":0.47671625930949652},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A191,1),INDEX(LinMotor!$U$1:$U$1305,A191,1))","v":0.7274857233796207},{"$f":"IF(A191<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A191,1),INDEX(LinMotor!$V$1:$V$1305,A191,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A191,1),INDEX(LinMotor!$V$1:$V$1305,A191,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A191,1),INDEX(LinMotor!$V$1:$V$1305,A191,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A191<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A191,1),INDEX(LinMotor!$W$1:$W$1305,A191,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A191,1),INDEX(LinMotor!$X$1:$X$1305,A191,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A191,1),INDEX(LinMotor!$W$1:$W$1305,A191,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A191,1),INDEX(LinMotor!$X$1:$X$1305,A191,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A191,1),INDEX(LinMotor!$W$1:$W$1305,A191,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A191,1),INDEX(LinMotor!$X$1:$X$1305,A191,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A191<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A191,1),INDEX(LinMotor!$X$1:$X$1305,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A191,1),INDEX(LinMotor!$Z$1:$Z$1305,A191,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A191,1),INDEX(LinMotor!$X$1:$X$1305,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A191,1),INDEX(LinMotor!$Z$1:$Z$1305,A191,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A191,1),INDEX(LinMotor!$X$1:$X$1305,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A191,1),INDEX(LinMotor!$Z$1:$Z$1305,A191,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A191<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A191,1),INDEX(LinMotor!$Y$1:$Y$1305,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A191,1),INDEX(LinMotor!$AB$1:$AB$1305,A191,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A191,1),INDEX(LinMotor!$Y$1:$Y$1305,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A191,1),INDEX(LinMotor!$AB$1:$AB$1305,A191,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A191,1),INDEX(LinMotor!$Y$1:$Y$1305,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A191,1),INDEX(LinMotor!$AB$1:$AB$1305,A191,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A191,1),INDEX(LinMotor!$AD$1:$AD$1305,A191,1))","v":0.60208812414399082},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A191,1),INDEX(LinMotor!$AE$1:$AE$1305,A191,1))","v":0.8565262626282103},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A191,1),INDEX(LinMotor!$AF$1:$AF$1305,A191,1))","v":7.2250574897278899},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A191,1),INDEX(LinMotor!$AG$1:$AG$1305,A191,1))","v":20.556630303077046},{"$f":"IF(A191<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A191,1),INDEX(LinMotor!$AI$1:$AI$1305,A191,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A191,1),INDEX(LinMotor!$AI$1:$AI$1305,A191,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A191,1),INDEX(LinMotor!$AI$1:$AI$1305,A191,1))/1000,\"0.0k\")),\"\")","v":325.61360390147166},{"$f":"IF(A191<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A191,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A191,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A191,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A191,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A191,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A191,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A191<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A191,1),INDEX(LinMotor!$AK$1:$AK$1305,A191,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A191,1),INDEX(LinMotor!$AK$1:$AK$1305,A191,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A191,1),INDEX(LinMotor!$AK$1:$AK$1305,A191,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[859,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A192,1),INDEX(LinMotor!$B$1:$B$1291,A192,1))","v":"KBM-35H01-F (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A192,1),INDEX(LinMotor!$R$1:$R$1305,A192,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A192,1),INDEX(LinMotor!$S$1:$S$1305,A192,1))","v":0.57215959138073869},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A192,1),INDEX(LinMotor!$T$1:$T$1305,A192,1))","v":0.47671625930949652},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A192,1),INDEX(LinMotor!$U$1:$U$1305,A192,1))","v":0.65949394128837768},{"$f":"IF(A192<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A192,1),INDEX(LinMotor!$V$1:$V$1305,A192,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A192,1),INDEX(LinMotor!$V$1:$V$1305,A192,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A192,1),INDEX(LinMotor!$V$1:$V$1305,A192,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A192<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A192,1),INDEX(LinMotor!$W$1:$W$1305,A192,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A192,1),INDEX(LinMotor!$X$1:$X$1305,A192,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A192,1),INDEX(LinMotor!$W$1:$W$1305,A192,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A192,1),INDEX(LinMotor!$X$1:$X$1305,A192,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A192,1),INDEX(LinMotor!$W$1:$W$1305,A192,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A192,1),INDEX(LinMotor!$X$1:$X$1305,A192,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A192<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A192,1),INDEX(LinMotor!$X$1:$X$1305,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A192,1),INDEX(LinMotor!$Z$1:$Z$1305,A192,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A192,1),INDEX(LinMotor!$X$1:$X$1305,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A192,1),INDEX(LinMotor!$Z$1:$Z$1305,A192,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A192,1),INDEX(LinMotor!$X$1:$X$1305,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A192,1),INDEX(LinMotor!$Z$1:$Z$1305,A192,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A192<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A192,1),INDEX(LinMotor!$Y$1:$Y$1305,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A192,1),INDEX(LinMotor!$AB$1:$AB$1305,A192,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A192,1),INDEX(LinMotor!$Y$1:$Y$1305,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A192,1),INDEX(LinMotor!$AB$1:$AB$1305,A192,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A192,1),INDEX(LinMotor!$Y$1:$Y$1305,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A192,1),INDEX(LinMotor!$AB$1:$AB$1305,A192,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A192,1),INDEX(LinMotor!$AD$1:$AD$1305,A192,1))","v":0.67475445545763924},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A192,1),INDEX(LinMotor!$AE$1:$AE$1305,A192,1))","v":0.95990086625034976},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A192,1),INDEX(LinMotor!$AF$1:$AF$1305,A192,1))","v":8.0970534654916708},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A192,1),INDEX(LinMotor!$AG$1:$AG$1305,A192,1))","v":23.037620790008393},{"$f":"IF(A192<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A192,1),INDEX(LinMotor!$AI$1:$AI$1305,A192,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A192,1),INDEX(LinMotor!$AI$1:$AI$1305,A192,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A192,1),INDEX(LinMotor!$AI$1:$AI$1305,A192,1))/1000,\"0.0k\")),\"\")","v":325.61360390147166},{"$f":"IF(A192<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A192,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A192,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A192,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A192,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A192,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A192,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A192<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A192,1),INDEX(LinMotor!$AK$1:$AK$1305,A192,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A192,1),INDEX(LinMotor!$AK$1:$AK$1305,A192,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A192,1),INDEX(LinMotor!$AK$1:$AK$1305,A192,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[860,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A193,1),INDEX(LinMotor!$B$1:$B$1291,A193,1))","v":"KBM-35H01-F (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A193,1),INDEX(LinMotor!$R$1:$R$1305,A193,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A193,1),INDEX(LinMotor!$S$1:$S$1305,A193,1))","v":0.58334289328153066},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A193,1),INDEX(LinMotor!$T$1:$T$1305,A193,1))","v":0.47671625930949652},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A193,1),INDEX(LinMotor!$U$1:$U$1305,A193,1))","v":0.65949394128837768},{"$f":"IF(A193<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A193,1),INDEX(LinMotor!$V$1:$V$1305,A193,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A193,1),INDEX(LinMotor!$V$1:$V$1305,A193,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A193,1),INDEX(LinMotor!$V$1:$V$1305,A193,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A193<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A193,1),INDEX(LinMotor!$W$1:$W$1305,A193,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A193,1),INDEX(LinMotor!$X$1:$X$1305,A193,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A193,1),INDEX(LinMotor!$W$1:$W$1305,A193,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A193,1),INDEX(LinMotor!$X$1:$X$1305,A193,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A193,1),INDEX(LinMotor!$W$1:$W$1305,A193,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A193,1),INDEX(LinMotor!$X$1:$X$1305,A193,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A193<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A193,1),INDEX(LinMotor!$X$1:$X$1305,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A193,1),INDEX(LinMotor!$Z$1:$Z$1305,A193,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A193,1),INDEX(LinMotor!$X$1:$X$1305,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A193,1),INDEX(LinMotor!$Z$1:$Z$1305,A193,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A193,1),INDEX(LinMotor!$X$1:$X$1305,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A193,1),INDEX(LinMotor!$Z$1:$Z$1305,A193,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A193<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A193,1),INDEX(LinMotor!$Y$1:$Y$1305,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A193,1),INDEX(LinMotor!$AB$1:$AB$1305,A193,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A193,1),INDEX(LinMotor!$Y$1:$Y$1305,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A193,1),INDEX(LinMotor!$AB$1:$AB$1305,A193,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A193,1),INDEX(LinMotor!$Y$1:$Y$1305,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A193,1),INDEX(LinMotor!$AB$1:$AB$1305,A193,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A193,1),INDEX(LinMotor!$AD$1:$AD$1305,A193,1))","v":0.67475445545763924},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A193,1),INDEX(LinMotor!$AE$1:$AE$1305,A193,1))","v":0.95990086625034976},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A193,1),INDEX(LinMotor!$AF$1:$AF$1305,A193,1))","v":8.0970534654916708},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A193,1),INDEX(LinMotor!$AG$1:$AG$1305,A193,1))","v":23.037620790008393},{"$f":"IF(A193<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A193,1),INDEX(LinMotor!$AI$1:$AI$1305,A193,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A193,1),INDEX(LinMotor!$AI$1:$AI$1305,A193,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A193,1),INDEX(LinMotor!$AI$1:$AI$1305,A193,1))/1000,\"0.0k\")),\"\")","v":325.61360390147166},{"$f":"IF(A193<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A193,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A193,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A193,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A193,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A193,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A193,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A193<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A193,1),INDEX(LinMotor!$AK$1:$AK$1305,A193,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A193,1),INDEX(LinMotor!$AK$1:$AK$1305,A193,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A193,1),INDEX(LinMotor!$AK$1:$AK$1305,A193,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[862,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A194,1),INDEX(LinMotor!$B$1:$B$1291,A194,1))","v":"KBM-35H01-G (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A194,1),INDEX(LinMotor!$R$1:$R$1305,A194,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A194,1),INDEX(LinMotor!$S$1:$S$1305,A194,1))","v":0.57623498050284605},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A194,1),INDEX(LinMotor!$T$1:$T$1305,A194,1))","v":0.47555918101020161},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A194,1),INDEX(LinMotor!$U$1:$U$1305,A194,1))","v":0.46870212990077026},{"$f":"IF(A194<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A194,1),INDEX(LinMotor!$V$1:$V$1305,A194,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A194,1),INDEX(LinMotor!$V$1:$V$1305,A194,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A194,1),INDEX(LinMotor!$V$1:$V$1305,A194,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A194<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A194,1),INDEX(LinMotor!$W$1:$W$1305,A194,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A194,1),INDEX(LinMotor!$X$1:$X$1305,A194,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A194,1),INDEX(LinMotor!$W$1:$W$1305,A194,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A194,1),INDEX(LinMotor!$X$1:$X$1305,A194,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A194,1),INDEX(LinMotor!$W$1:$W$1305,A194,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A194,1),INDEX(LinMotor!$X$1:$X$1305,A194,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A194<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A194,1),INDEX(LinMotor!$X$1:$X$1305,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A194,1),INDEX(LinMotor!$Z$1:$Z$1305,A194,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A194,1),INDEX(LinMotor!$X$1:$X$1305,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A194,1),INDEX(LinMotor!$Z$1:$Z$1305,A194,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A194,1),INDEX(LinMotor!$X$1:$X$1305,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A194,1),INDEX(LinMotor!$Z$1:$Z$1305,A194,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A194<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A194,1),INDEX(LinMotor!$Y$1:$Y$1305,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A194,1),INDEX(LinMotor!$AB$1:$AB$1305,A194,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A194,1),INDEX(LinMotor!$Y$1:$Y$1305,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A194,1),INDEX(LinMotor!$AB$1:$AB$1305,A194,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A194,1),INDEX(LinMotor!$Y$1:$Y$1305,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A194,1),INDEX(LinMotor!$AB$1:$AB$1305,A194,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A194,1),INDEX(LinMotor!$AD$1:$AD$1305,A194,1))","v":0.93021704764736279},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A194,1),INDEX(LinMotor!$AE$1:$AE$1305,A194,1))","v":1.3233201242545973},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A194,1),INDEX(LinMotor!$AF$1:$AF$1305,A194,1))","v":11.162604571768354},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A194,1),INDEX(LinMotor!$AG$1:$AG$1305,A194,1))","v":31.759682982110338},{"$f":"IF(A194<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A194,1),INDEX(LinMotor!$AI$1:$AI$1305,A194,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A194,1),INDEX(LinMotor!$AI$1:$AI$1305,A194,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A194,1),INDEX(LinMotor!$AI$1:$AI$1305,A194,1))/1000,\"0.0k\")),\"\")","v":325.61360390147166},{"$f":"IF(A194<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A194,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A194,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A194,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A194,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A194,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A194,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A194<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A194,1),INDEX(LinMotor!$AK$1:$AK$1305,A194,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A194,1),INDEX(LinMotor!$AK$1:$AK$1305,A194,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A194,1),INDEX(LinMotor!$AK$1:$AK$1305,A194,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[864,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1452,A195,1),INDEX(LinMotor!$B$1:$B$1291,A195,1))","v":"KBM-35H01-H (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1452,A195,1),INDEX(LinMotor!$R$1:$R$1305,A195,1))","v":1.6447368421052631},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1452,A195,1),INDEX(LinMotor!$S$1:$S$1305,A195,1))","v":0.5871179823273095},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1452,A195,1),INDEX(LinMotor!$T$1:$T$1305,A195,1))","v":0.47326179366232629},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1452,A195,1),INDEX(LinMotor!$U$1:$U$1305,A195,1))","v":0.4241133917172733},{"$f":"IF(A195<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A195,1),INDEX(LinMotor!$V$1:$V$1305,A195,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A195,1),INDEX(LinMotor!$V$1:$V$1305,A195,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1452,A195,1),INDEX(LinMotor!$V$1:$V$1305,A195,1))/1000,\"0.0k\")),\"\")","v":19.593038257620307},{"$f":"IF(A195<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A195,1),INDEX(LinMotor!$W$1:$W$1305,A195,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A195,1),INDEX(LinMotor!$X$1:$X$1305,A195,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A195,1),INDEX(LinMotor!$W$1:$W$1305,A195,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A195,1),INDEX(LinMotor!$X$1:$X$1305,A195,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1452,A195,1),INDEX(LinMotor!$W$1:$W$1305,A195,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A195,1),INDEX(LinMotor!$X$1:$X$1305,A195,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(A195<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A195,1),INDEX(LinMotor!$X$1:$X$1305,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A195,1),INDEX(LinMotor!$Z$1:$Z$1305,A195,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A195,1),INDEX(LinMotor!$X$1:$X$1305,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A195,1),INDEX(LinMotor!$Z$1:$Z$1305,A195,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1452,A195,1),INDEX(LinMotor!$X$1:$X$1305,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1452,A195,1),INDEX(LinMotor!$Z$1:$Z$1305,A195,1)))/1000,\"0.0k\")),\"\")","v":-15.870360988672449},{"$f":"IF(A195<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A195,1),INDEX(LinMotor!$Y$1:$Y$1305,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A195,1),INDEX(LinMotor!$AB$1:$AB$1305,A195,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A195,1),INDEX(LinMotor!$Y$1:$Y$1305,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A195,1),INDEX(LinMotor!$AB$1:$AB$1305,A195,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1452,A195,1),INDEX(LinMotor!$Y$1:$Y$1305,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1452,A195,1),INDEX(LinMotor!$AB$1:$AB$1305,A195,1)))/1000,\"0.0k\")),\"\")","v":0},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1452,A195,1),INDEX(LinMotor!$AD$1:$AD$1305,A195,1))","v":0.9972084556134847},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1452,A195,1),INDEX(LinMotor!$AE$1:$AE$1305,A195,1))","v":1.4186216224779731},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1452,A195,1),INDEX(LinMotor!$AF$1:$AF$1305,A195,1))","v":11.966501467361816},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1452,A195,1),INDEX(LinMotor!$AG$1:$AG$1305,A195,1))","v":34.046918939471354},{"$f":"IF(A195<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A195,1),INDEX(LinMotor!$AI$1:$AI$1305,A195,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A195,1),INDEX(LinMotor!$AI$1:$AI$1305,A195,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1452,A195,1),INDEX(LinMotor!$AI$1:$AI$1305,A195,1))/1000,\"0.0k\")),\"\")","v":325.61360390147166},{"$f":"IF(A195<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A195,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A195,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A195,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A195,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1452,A195,1),INDEX(LinMotor!$AJ$1:$AJ$1305,A195,1))/1000,\"0.0k\")),\"\")","v":263.95610791970807},{"$f":"IF(A195<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A195,1),INDEX(LinMotor!$AK$1:$AK$1305,A195,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A195,1),INDEX(LinMotor!$AK$1:$AK$1305,A195,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1452,A195,1),INDEX(LinMotor!$AK$1:$AK$1305,A195,1))/1000,\"0.0k\")),\"\")","v":"2.5k"},""]
[1," ...",null,null,"Auswahl einschränken",null,null,null,null,null,null,null,null,null,null,null,null,""]
[121,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5]

{"sheet":"Inertia","index":1,"n_rows":54,"n_cols":13,"rows_kept":54,"cut":false,"hidden":false,"merged":[[53,10,54,10],[53,11,54,11],[48,11,49,11],[8,6,9,6],[13,6,14,6],[13,7,14,7],[13,10,14,10],[13,11,14,11],[33,10,34,10],[33,11,34,11],[33,7,34,7],[48,10,49,10],[6,12,7,12],[8,7,9,7],[8,8,9,8],[8,9,9,9],[8,11,9,11],[8,12,9,12],[8,10,9,10],[26,12,27,12],[28,6,29,6],[28,7,29,7],[28,8,29,8],[28,9,29,9],[28,11,29,11],[28,12,29,12],[28,10,29,10],[0,2,0,13],[13,8,14,8],[33,8,34,8],[53,8,54,8],[13,12,14,12],[33,12,34,12],[53,12,54,12],[53,6,54,6],[53,7,54,7],[33,6,34,6],[46,12,47,12],[48,6,49,6],[48,7,49,7],[48,8,49,8],[48,9,49,9],[48,12,49,12]]}
[]
[]
[null,null,{"$f":"IF(deutsch,\"Massenträgheit 1\",\"Inertia 1\")","v":"Massenträgheit 1"}]
[]
[]
[]
[null,null,null,null,null,null,"Gewicht","Durchmesser",null,null,"Last","Reibung"]
[null,null,null,null,null,null,"G [kg]","D [mm]",null,null,"F Last [N]","F Reibung [N]"]
[null,null,null,null,null,null,5,300,null,null,{"$f":"G9*10","v":50},{"$f":"G9*10*0.2","v":10}]
[]
[]
[null,null,null,null,null,null,{"$f":"IF(deutsch,\"Massenträgheit\",\"Inertia\")","v":"Massenträgheit"},{"$f":"IF(deutsch,\"Lastmoment\",\"Load\")","v":"Lastmoment"},{"$f":"IF(deutsch,\"Reibmoment\",\"Friction\")","v":"Reibmoment"},null,{"$f":"IF(deutsch,\"Sum. Massenträgheit\",\"Sum inertia\")","v":"Sum. Massenträgheit"},{"$f":"IF(deutsch,\"Sum. Lastmoment\",\"Sum load\")","v":"Sum. Lastmoment"},{"$f":"IF(deutsch,\"Sum. Reibmoment\",\"Sum friction\")","v":"Sum. Reibmoment"}]
[null,null,null,null,null,null,"[kgcm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"},null,"[kgcm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"}]
[null,null,null,null,null,null,{"$f":"Calc!A72*(1000*G9*(H9/2000)^2)","v":1125},{"$f":"H9*K9/2000","v":7.5},{"$f":"H9*L9/2000","v":1.5},null,{"$f":"G14+G34+G54","v":1125},{"$f":"H14+H34+H54","v":7.5},{"$f":"I14+I34+I54","v":1.5}]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"IF(deutsch,\"Massenträgheit 2\",\"Inertia 2\")","v":"Massenträgheit 2"}]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,5,50,null,null,{"$f":"G29*10","v":50},{"$f":"G29*10*0.2","v":10}]
[]
[]
[null,null,null,null,null,null,{"$f":"IF(deutsch,\"Massenträgheit\",\"Inertia\")","v":"Massenträgheit"},{"$f":"IF(deutsch,\"Lastmoment\",\"Load\")","v":"Lastmoment"},{"$f":"IF(deutsch,\"Reibmoment\",\"Friction\")","v":"Reibmoment"},null,{"$f":"IF(deutsch,\"Sum. Massenträgheit\",\"Sum inertia\")","v":"Sum. Massenträgheit"},{"$f":"IF(deutsch,\"Sum. Lastmoment\",\"Sum load\")","v":"Sum. Lastmoment"},{"$f":"IF(deutsch,\"Sum. Reibmoment\",\"Sum friction\")","v":"Sum. Reibmoment"}]
[null,null,null,null,null,null,"[kgcm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"},null,"[kgcm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"G14+G34+G54","v":1125},{"$f":"H14+H34+H54","v":7.5},{"$f":"I14+I34+I54","v":1.5}]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"IF(deutsch,\"Massenträgheit 3\",\"Inertia 3\")","v":"Massenträgheit 3"}]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,5,50,null,null,{"$f":"G49*10","v":50},{"$f":"G49*10*0.2","v":10}]
[]
[]
[null,null,null,null,null,null,{"$f":"IF(deutsch,\"Massenträgheit\",\"Inertia\")","v":"Massenträgheit"},{"$f":"IF(deutsch,\"Lastmoment\",\"Load\")","v":"Lastmoment"},{"$f":"IF(deutsch,\"Reibmoment\",\"Friction\")","v":"Reibmoment"},null,{"$f":"IF(deutsch,\"Sum. Massenträgheit\",\"Sum inertia\")","v":"Sum. Massenträgheit"},{"$f":"IF(deutsch,\"Sum. Lastmoment\",\"Sum load\")","v":"Sum. Lastmoment"},{"$f":"IF(deutsch,\"Sum. Reibmoment\",\"Sum friction\")","v":"Sum. Reibmoment"}]
[null,null,null,null,null,null,"[kgcm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"},null,"[kgcm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"G14+G34+G54","v":1125},{"$f":"H14+H34+H54","v":7.5},{"$f":"I14+I34+I54","v":1.5}]

{"sheet":"Drives","index":2,"n_rows":50,"n_cols":23,"rows_kept":50,"cut":false,"hidden":true,"merged":[]}
["Selected"]
["S712",480,12,24,2.7,30,100]
[]
[]
[]
[]
[]
[]
["Drives","AC-\nVoltage\n[V]","Icont\n[Arms]","Ipeak\n[Arms]","Lmin \nbei UAC\n[mH]","Lmax \nbei UAC\n[mH]","Brake \nPower\n[W]","AKM","AKM2G","DBK","6SMx7","6SM45100","AKMH","ACC","Goldline BH","DDR","KBM","Sonstige","IC/ICD","IL",null,"ICH","Sonstige"]
["Servostar 303",230,3,9,5.9,null,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 306",230,6,15,3.6,null,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 310",230,10,20,2.7,null,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 341",480,1.5,4.5,35.6,null,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 343",480,3,7.5,17.8,null,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 346",480,6,12,10.7,null,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 403M/A",230,3,9,6.9,43.1,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 406M/A",230,6,12,4.3,23,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 443M/403A",400,3,9,12,75,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 446M/406A",400,6,12,7.5,40,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 601",480,1.5,3,30,180,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 603",480,3,6,14.4,90,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 606",480,6,12,9,48,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 610",480,10,20,4.8,30,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 610/30",480,10,30,4.8,30,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 614",480,14,28,3,18,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 620",480,20,40,2.4,14.4,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 640",480,40,80,1.3,null,"external",1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 670",480,70,140,0.8,null,"external",1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar S20260",230,1.5,4.5,2.5,150,"external",1,null,null,null,null,1,null,null,1,1,1,null,null,null,null,1]
["Servostar S20360",230,3,9,5,300,"external",1,null,null,null,null,1,null,null,1,1,1,null,null,null,null,1]
["Servostar S20330",50,3,9,0.2,15,"external",1,null,null,null,null,1,null,null,1,1,1,null,null,null,null,1]
["Servostar S20630",50,6,18,0.4,30,"external",1,null,null,null,null,1,null,null,1,1,1,null,null,null,null,1]
["S701",480,1.5,4.5,17.8,180,20,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S703",480,3,9,8.9,80,50,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S706",480,6,18,4.4000000000000004,48,50,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S712",480,12,24,2.7,30,100,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S712P",480,12,30,2.7,30,100,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S724",480,24,48,1.7,16,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S724P",480,24,72,1.7,16,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S748",480,48,96,0.85,8,0,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S772",480,72,140,0.57999999999999996,5.5,0,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B00306",230,3,9,2.5,250,"external",1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B00606",230,6,18,1.3,125,"external",1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B01206",230,12,30,1,100,100,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B02406",230,24,48,0.6,60,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B00307",480,3,9,6.3,600,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B00607",480,6,18,3.2,300,100,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B01207",480,12,30,2.5,250,100,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B02407",480,24,48,1.2,120,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B04807",480,48,96,0.6,60,"external",1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]

{"sheet":"Motor","index":3,"n_rows":1452,"n_cols":52,"rows_kept":1452,"cut":false,"hidden":true,"merged":[[0,0,1,0]]}
["Motor\nLinie","Typ","M0","I0","Mn","In","nn","Mmax","nmax","RU-V","LU-V","KE","J","UDCmax","Poles","Nmax","Nmax","Nmax","MnStrich","Jext/Jmot","Trms","Tpk","n","T (t1)","T (t2)","T (t3)","T (t4)","T (t5)","T (t6)","T (t7)","T (t8)","Irms","Ipeak","Irms","Ipeak","Ipeak","P","PbrRMS","PbrPEAK","Koeff","Koeff","Koeff","nmax","Koeff","Koeff","Koeff","nmax","Inenn","Koeff","Koeff","Koeff","nmax"]
[null,"Kein Motor","[Nm]","[A]","[Nm]","[A] ","[min-1]","[Nm]","[min-1] ","[W]","[mH]","[V/1000]","[10-3kgm2]","[V]",null,"bei Mmax","bei Mn","bei M0",null," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," ","trapez"," "," "," ","A","B","C","theo","A","B","C","theo","nmax","A","B","C","theo"]
["Other","power_rotor_test",4.8,4.87,3.01,3.0404040404040402,5000,16.100000000000001,6000,2.61,10.8,63.9,0.21,640,10,{"$f":"IFERROR(IF(AQ3<I3,IF(AQ3<0,0,AQ3),I3),0)","v":1958.3352880669909},{"$f":"IFERROR(IF(AU3<I3,IF(AU3<0,0,AU3),I3),0)","v":3260.319829449963},{"$f":"IFERROR(IF(UAC_V*0.98/L3*1000<I3,IF(UAC_V*0.98/L3*1000<0,0,UAC_V*0.98/L3*1000),I3),0)","v":3527.386541471049},{"$f":"IFERROR(C3+(E3-C3)/G3*Q3,0)","v":3.6328055010569127},{"$f":"IFERROR(IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M3,(inertia/gear^2+gear_inertia)/M3),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M3,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M3)),0)","v":11.904761904761905},{"$f":"IFERROR(IF((C3+(E3-C3)/G3*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X3^2*time1+Y3^2*time2+Z3^2*time3+AA3^2*time4)/time)/(C3+(E3-C3)/G3*mspeed),SQRT((((X3-Y3)*2/PI()+Y3)^2*time1+Y3^2*time2+((Z3-Y3)*2/PI()+Y3)^2*time3+AA3^2*time4)/time)/(C3+(E3-C3)/G3*mspeed)),IF(AccType=1,SQRT((X3^2*time1+Y3^2*time2+Z3^2*time3+AA3^2*time4+AB3^2*time5+AC3^2*time6+AD3^2*time7+AE3^2*time8)/time)/(C3+(E3-C3)/G3*mspeed),SQRT((((X3-Y3)*2/PI()+Y3)^2*time1+Y3^2*time2+((Z3-Y3)*2/PI()+Y3)^2*time3+AA3^2*time4+((AB3-AC3)*2/PI()+AC3)^2*time5+AC3^2*time6+((AD3-AC3)*2/PI()+AC3)^2*time7+AE3^2*time8)/time)/(C3+(E3-C3)/G3*mspeed)))),0)","v":1.0008561413001364},{"$f":"IFERROR(IF(move1,MAX(ABS(X3),ABS(Z3))/H3,MAX(ABS(X3),ABS(Z3),ABS(AB3),ABS(AD3))/H3),0)","v":0.82038771481337158},{"$f":"IFERROR(IF(AZ3>0,speed/(MIN(AZ3,I3)),\"NA\"),0)","v":0.87664905154835027},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M3+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M3+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":13.208242208495284},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M3+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M3+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.698676188881178},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M3+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M3+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M3+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M3+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"AH3/Irms","v":0.39250110498688523},{"$f":"AI3/Ipeak","v":0.55836926697371558},{"$f":"IFERROR(IF(move1,IF(AccType=1,SQRT((X3^2*time1+Y3^2*time2+Z3^2*time3+AA3^2*time4)/time)/(C3/D3),SQRT((((X3-Y3)*2/PI()+Y3)^2*time1+Y3^2*time2+((Z3-AA3)*2/PI()+AA3)^2*time3+AA3^2*time4)/time)/(C3/D3)),IF(AccType=1,SQRT((X3^2*time1+Y3^2*time2+Z3^2*time3+AA3^2*time4+AB3^2*time5+AC3^2*time6+AD3^2*time7+AE3^2*time8)/time)/(C3/D3),SQRT((((X3-Y3)*2/PI()+Y3)^2*time1+Y3^2*time2+((Z3-AA3)*2/PI()+AA3)^2*time3+AA3^2*time4+((AB3-AC3)*2/PI()+AC3)^2*time5+AC3^2*time6+((AD3-AE3)*2/PI()+AE3)^2*time7+AE3^2*time8)/time)/(C3/D3))),0)","v":4.710013259842623},{"$f":"IFERROR(IF(move1,MAX(ABS(X3),ABS(Z3))/(C3/D3),MAX(ABS(X3),ABS(Z3),ABS(AB3),ABS(AD3))/(C3/D3)),0)","v":13.400862407369173},{"$f":"IFERROR(IF(move1,IF(AccType=1,MAX(ABS(X3),ABS(Z3))/(C3/D3),MAX(ABS((X3-Y3)*2/PI()+Y3),ABS((Z3-Y3)*2/PI()+Y3))/(C3/D3)),IF(AccType=1,MAX(ABS(X3),ABS(Z3),ABS(AB3),ABS(AD3))/(C3/D3),MAX(ABS((X3-Y3)*2/PI()+Y3),ABS((Z3-Y3)*2/PI()+Y3),ABS((AB3-AC3)*2/PI()+AC3),ABS((AD3-AC3)*2/PI()+AC3))/(C3/D3))),0)","v":8.5312539753086423},{"$f":"IFERROR(IF((C3+(E3-C3)/G3*mspeed)<0,\"NA\",U3*(C3+(E3-C3)/G3*mspeed)*mspeed/9.55),0)","v":219.50568820223589},{"$f":"IF(move1,IF(speed1>speed2,AM3/2*time1/time,AM3/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z3*-speed/30*PI(),((Z3-AA3)*2/PI()+AA3)*-speed/30*PI()),IF(AccType=1,X3*-speed/30*PI(),((X3-Y3)*2/PI()+Y3)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z3*-speed/30*PI(),((Z3-AA3)*2/PI()+AA3)*-speed/30*PI()),IF(AccType=1,X3*-speed/30*PI(),((X3-Y3)*2/PI()+Y3)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD3*-speed/30*PI(),((AD3-AE3)*2/PI()+AE3)*-speed/30*PI()),IF(AccType=1,AB3*-speed/30*PI(),((AB3-AC3)*2/PI()+AC3)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD3*-speed/30*PI(),((AD3-AE3)*2/PI()+AE3)*-speed/30*PI()),IF(AccType=1,AB3*-speed/30*PI(),((AB3-AC3)*2/PI()+AC3)*-speed/30*PI()),0)/2*time7/time)))","v":177.94056031403207},{"$f":"IF(move1,MAX(IF(AccType=1,Z3*-speed/30*PI(),((Z3-AA3)*2/PI()+AA3)*-speed/30*PI()),IF(AccType=1,X3*-speed/30*PI(),((X3-Y3)*2/PI()+Y3)*-speed/30*PI()),0),MAX(IF(AccType=1,Z3*-speed/30*PI(),((Z3-AA3)*2/PI()+AA3)*-speed/30*PI()),IF(AccType=1,X3*-speed/30*PI(),((X3-Y3)*2/PI()+Y3)*-speed/30*PI()),IF(AccType=1,AD3*-speed/30*PI(),((AD3-AE3)*2/PI()+AE3)*-speed/30*PI()),IF(AccType=1,AB3*-speed/30*PI(),((AB3-AC3)*2/PI()+AC3)*-speed/30*PI()),0))","v":1711.7881902209886},{"$f":"IFERROR((L3^2)/1000000+((K3/1000)^2*(D3/C3*H3)^2*PI()*PI()*(O3/2)^2)/1200,0)","v":1.0482521026179489E-2},{"$f":"IFERROR(SQRT(3)*L3*J3*D3/C3*H3/1000,0)","v":4.7186263950285383},{"$f":"IFERROR(0.75*J3^2*(D3/C3*H3)^2-(UAC_V*0.98)^2,0)","v":-49441.928923478103},{"$f":"IFERROR(-AO3/2/AN3+SQRT((AO3/2/AN3)^2-AP3/AN3),0)","v":1958.3352880669909},{"$f":"IFERROR((L3^2)/1000000+((K3/1000)^2*AV3^2*PI()*PI()*(O3/2)^2)/1200,0)","v":4.4337807862303569E-3},{"$f":"IFERROR(SQRT(3)*L3*J3*AV3/1000,0)","v":1.1044265660464483},{"$f":"IFERROR(0.75*J3^2*AV3^2-(UAC_V*0.98)^2,0)","v":-50730.47868065878},{"$f":"IFERROR(-AS3/2/AR3+SQRT((AS3/2/AR3)^2-AT3/AR3),0)","v":3260.319829449963},{"$f":"IFERROR(D3+(F3-D3)*((0.85*UAC_V-D3*J3)/L3*1000)/G3,0)","v":3.8232689679581418},{"$f":"(L3^2)/1000000+((K3/1000)^2*AJ3^2*PI()*PI()*(O3/2)^2)/1200","v":5.8287578608992568E-3},{"$f":"SQRT(3)*L3*J3*AJ3/1000","v":2.4644207904243345},{"$f":"0.75*J3^2*AJ3^2-(UAC_V*0.98)^2","v":-50433.309799283183},{"$f":"IFERROR(IF(((AX3/2/AW3)^2-AY3/AW3)>0,-AX3/2/AW3+SQRT((AX3/2/AW3)^2-AY3/AW3),-9999),0)","v":2737.697594905379}]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IFERROR(IF(AQ4<I4,IF(AQ4<0,0,AQ4),I4),0)","v":0},{"$f":"IFERROR(IF(AU4<I4,IF(AU4<0,0,AU4),I4),0)","v":0},0,{"$f":"IFERROR(C4+(E4-C4)/G4*Q4,0)","v":0},0,0,0,"NA",12.184725284589746,0,-9.8696274805176927,0,0,0,0,0,0,0,0,0,0,0,164.15180840777867,1579.1403968828308,{"$f":"IFERROR((L4^2)/1000000+((K4/1000)^2*(D4/C4*H4)^2*PI()*PI()*(O4/2)^2)/1200,0)","v":0},{"$f":"IFERROR(SQRT(3)*L4*J4*D4/C4*H4/1000,0)","v":0},0,{"$f":"IFERROR(-AO4/2/AN4+SQRT((AO4/2/AN4)^2-AP4/AN4),0)","v":0},{"$f":"IFERROR((L4^2)/1000000+((K4/1000)^2*AV4^2*PI()*PI()*(O4/2)^2)/1200,0)","v":0},{"$f":"IFERROR(SQRT(3)*L4*J4*AV4/1000,0)","v":0},-50805.16,{"$f":"IFERROR(-AS4/2/AR4+SQRT((AS4/2/AR4)^2-AT4/AR4),0)","v":0},0,0,0,-50805.16,{"$f":"IFERROR(IF(((AX4/2/AW4)^2-AY4/AW4)>0,-AX4/2/AW4+SQRT((AX4/2/AW4)^2-AY4/AW4),-9999),0)","v":0}]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",12.184725284589746,0,-9.8696274805176927,0,0,0,0,0,0,0,0,0,0,0,164.15180840777867,1579.1403968828308,0,0,0,0,0,0,-50805.16,0,0,0,0,-50805.16,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",12.184725284589746,0,-9.8696274805176927,0,0,0,0,0,0,0,0,0,0,0,164.15180840777867,1579.1403968828308,0,0,0,0,0,0,-50805.16,0,0,0,0,-50805.16,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",12.184725284589746,0,-9.8696274805176927,0,0,0,0,0,0,0,0,0,0,0,164.15180840777867,1579.1403968828308,0,0,0,0,0,0,-50805.16,0,0,0,0,-50805.16,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",12.184725284589746,0,-9.8696274805176927,0,0,0,0,0,0,0,0,0,0,0,164.15180840777867,1579.1403968828308,0,0,0,0,0,0,-50805.16,0,0,0,0,-50805.16,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",12.184725284589746,0,-9.8696274805176927,0,0,0,0,0,0,0,0,0,0,0,164.15180840777867,1579.1403968828308,0,0,0,0,0,0,-50805.16,0,0,0,0,-50805.16,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",12.184725284589746,0,-9.8696274805176927,0,0,0,0,0,0,0,0,0,0,0,164.15180840777867,1579.1403968828308,0,0,0,0,0,0,-50805.16,0,0,0,0,-50805.16,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",12.184725284589746,0,-9.8696274805176927,0,0,0,0,0,0,0,0,0,0,0,164.15180840777867,1579.1403968828308,0,0,0,0,0,0,-50805.16,0,0,0,0,-50805.16,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",12.184725284589746,0,-9.8696274805176927,0,0,0,0,0,0,0,0,0,0,0,164.15180840777867,1579.1403968828308,0,0,0,0,0,0,-50805.16,0,0,0,0,-50805.16,0]
["Leerzeile"]
["AKM","AKM11B",0.183,1.1599999999999999,0.16700000000000001,1.0569620253164558,8000,0.61,8000,20.2,12.5,10.199999999999999,1.7000000000000001E-3,320,6,{"$f":"IF(AQ14<I14,IF(AQ14<0,0,AQ14),I14)","v":8000},{"$f":"IF(AU14<I14,IF(AU14<0,0,AU14),I14)","v":8000},{"$f":"IF(UAC_V*0.98/L14*1000<I14,IF(UAC_V*0.98/L14*1000<0,0,UAC_V*0.98/L14*1000),I14)","v":8000},{"$f":"C14+(E14-C14)/G14*Q14","v":0.16700000000000001},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M14,(inertia/gear^2+gear_inertia)/M14),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M14,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M14))","v":1470.5882352941176},{"$f":"IF((C14+(E14-C14)/G14*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X14^2*time1+Y14^2*time2+Z14^2*time3+AA14^2*time4)/time)/(C14+(E14-C14)/G14*mspeed),SQRT((((X14-Y14)*2/PI()+Y14)^2*time1+Y14^2*time2+((Z14-Y14)*2/PI()+Y14)^2*time3+AA14^2*time4)/time)/(C14+(E14-C14)/G14*mspeed)),IF(AccType=1,SQRT((X14^2*time1+Y14^2*time2+Z14^2*time3+AA14^2*time4+AB14^2*time5+AC14^2*time6+AD14^2*time7+AE14^2*time8)/time)/(C14+(E14-C14)/G14*mspeed),SQRT((((X14-Y14)*2/PI()+Y14)^2*time1+Y14^2*time2+((Z14-Y14)*2/PI()+Y14)^2*time3+AA14^2*time4+((AB14-AC14)*2/PI()+AC14)^2*time5+AC14^2*time6+((AD14-AC14)*2/PI()+AC14)^2*time7+AE14^2*time8)/time)/(C14+(E14-C14)/G14*mspeed))))","v":23.534113047270338},{"$f":"IF(move1,MAX(ABS(X14),ABS(Z14))/H14,MAX(ABS(X14),ABS(Z14),ABS(AB14),ABS(AD14))/H14)","v":19.988542455382404},{"$f":"IF(AZ14>0,speed/(MIN(AZ14,I14)),\"NA\")","v":"NA"},12.193010897783266,0,-9.8763388272044441,0,0,0,0,0,2.2637371447429322,3.2203762844782755,{"$f":"IF(move1,IF(AccType=1,SQRT((X14^2*time1+Y14^2*time2+Z14^2*time3+AA14^2*time4)/time)/(C14/D14),SQRT((((X14-Y14)*2/PI()+Y14)^2*time1+Y14^2*time2+((Z14-AA14)*2/PI()+AA14)^2*time3+AA14^2*time4)/time)/(C14/D14)),IF(AccType=1,SQRT((X14^2*time1+Y14^2*time2+Z14^2*time3+AA14^2*time4+AB14^2*time5+AC14^2*time6+AD14^2*time7+AE14^2*time8)/time)/(C14/D14),SQRT((((X14-Y14)*2/PI()+Y14)^2*time1+Y14^2*time2+((Z14-AA14)*2/PI()+AA14)^2*time3+AA14^2*time4+((AB14-AC14)*2/PI()+AC14)^2*time5+AC14^2*time6+((AD14-AE14)*2/PI()+AE14)^2*time7+AE14^2*time8)/time)/(C14/D14)))","v":27.164845736915186},{"$f":"IF(move1,MAX(ABS(X14),ABS(Z14))/(C14/D14),MAX(ABS(X14),ABS(Z14),ABS(AB14),ABS(AD14))/(C14/D14))","v":77.289030827478612},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X14),ABS(Z14))/(C14/D14),MAX(ABS((X14-Y14)*2/PI()+Y14),ABS((Z14-Y14)*2/PI()+Y14))/(C14/D14)),IF(AccType=1,MAX(ABS(X14),ABS(Z14),ABS(AB14),ABS(AD14))/(C14/D14),MAX(ABS((X14-Y14)*2/PI()+Y14),ABS((Z14-Y14)*2/PI()+Y14),ABS((AB14-AC14)*2/PI()+AC14),ABS((AD14-AC14)*2/PI()+AC14))/(C14/D14)))","v":49.203725211900419},{"$f":"IF((C14+(E14-C14)/G14*mspeed)<0,\"NA\",U14*(C14+(E14-C14)/G14*mspeed)*mspeed/9.55)","v":202.63371962196808},164.26343163749593,1580.214212352711,{"$f":"(L14^2)/1000000+((K14/1000)^2*(D14/C14*H14)^2*PI()*PI()*(O14/2)^2)/1200","v":2.7696369377741982E-4},{"$f":"SQRT(3)*L14*J14*D14/C14*H14/1000","v":1.3799040937804334},{"$f":"0.75*J14^2*(D14/C14*H14)^2-(UAC_V*0.98)^2","v":-46229.671466666667},{"$f":"-AO14/2/AN14+SQRT((AO14/2/AN14)^2-AP14/AN14)","v":10666.444514140157},{"$f":"(L14^2)/1000000+((K14/1000)^2*AV14^2*PI()*PI()*(O14/2)^2)/1200","v":1.1431903233866342E-4},{"$f":"SQRT(3)*L14*J14*AV14/1000","v":0.33643236409557697},{"$f":"0.75*J14^2*AV14^2-(UAC_V*0.98)^2","v":-50533.181108201323},{"$f":"-AS14/2/AR14+SQRT((AS14/2/AR14)^2-AT14/AR14)","v":19604.629736266608},{"$f":"D14+(F14-D14)*((0.85*UAC_V-D14*J14)/L14*1000)/G14","v":0.94272624720774412},{"$f":"(L14^2)/1000000+((K14/1000)^2*AJ14^2*PI()*PI()*(O14/2)^2)/1200","v":2.8105263216801291E-2},{"$f":"SQRT(3)*L14*J14*AJ14/1000","v":17.559419443745409},690095.48206407251,{"$f":"IF(((AX14/2/AW14)^2-AY14/AW14)>0,-AX14/2/AW14+SQRT((AX14/2/AW14)^2-AY14/AW14),-9999)","v":-9999}]
["AKM","AKM11C",0.185,1.45,0.17599999999999999,1.3643410852713178,6000,0.61,8000,13.1,8.3000000000000007,8.3000000000000007,1.7000000000000001E-3,320,6,{"$f":"IF(AQ15<I15,IF(AQ15<0,0,AQ15),I15)","v":8000},{"$f":"IF(AU15<I15,IF(AU15<0,0,AU15),I15)","v":8000},{"$f":"IF(UAC_V*0.98/L15*1000<I15,IF(UAC_V*0.98/L15*1000<0,0,UAC_V*0.98/L15*1000),I15)","v":8000},{"$f":"C15+(E15-C15)/G15*Q15","v":0.17299999999999999},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M15,(inertia/gear^2+gear_inertia)/M15),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M15,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M15))","v":1470.5882352941176},{"$f":"IF((C15+(E15-C15)/G15*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X15^2*time1+Y15^2*time2+Z15^2*time3+AA15^2*time4)/time)/(C15+(E15-C15)/G15*mspeed),SQRT((((X15-Y15)*2/PI()+Y15)^2*time1+Y15^2*time2+((Z15-Y15)*2/PI()+Y15)^2*time3+AA15^2*time4)/time)/(C15+(E15-C15)/G15*mspeed)),IF(AccType=1,SQRT((X15^2*time1+Y15^2*time2+Z15^2*time3+AA15^2*time4+AB15^2*time5+AC15^2*time6+AD15^2*time7+AE15^2*time8)/time)/(C15+(E15-C15)/G15*mspeed),SQRT((((X15-Y15)*2/PI()+Y15)^2*time1+Y15^2*time2+((Z15-Y15)*2/PI()+Y15)^2*time3+AA15^2*time4+((AB15-AC15)*2/PI()+AC15)^2*time5+AC15^2*time6+((AD15-AC15)*2/PI()+AC15)^2*time7+AE15^2*time8)/time)/(C15+(E15-C15)/G15*mspeed))))","v":23.249927971966166},{"$f":"IF(move1,MAX(ABS(X15),ABS(Z15))/H15,MAX(ABS(X15),ABS(Z15),ABS(AB15),ABS(AD15))/H15)","v":19.988542455382404},{"$f":"IF(AZ15>0,speed/(MIN(AZ15,I15)),\"NA\")","v":"NA"},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M15+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M15+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.193010897783266},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M15+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M15+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-9.8763388272044441},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M15+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M15+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M15+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M15+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"AH15/Irms","v":2.7990803884321394},{"$f":"AI15/Ipeak","v":3.9819517571589493},33.58896466118567,{"$f":"IF(move1,MAX(ABS(X15),ABS(Z15))/(C15/D15),MAX(ABS(X15),ABS(Z15),ABS(AB15),ABS(AD15))/(C15/D15))","v":95.566842171814784},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X15),ABS(Z15))/(C15/D15),MAX(ABS((X15-Y15)*2/PI()+Y15),ABS((Z15-Y15)*2/PI()+Y15))/(C15/D15)),IF(AccType=1,MAX(ABS(X15),ABS(Z15),ABS(AB15),ABS(AD15))/(C15/D15),MAX(ABS((X15-Y15)*2/PI()+Y15),ABS((Z15-Y15)*2/PI()+Y15),ABS((AB15-AC15)*2/PI()+AC15),ABS((AD15-AC15)*2/PI()+AC15))/(C15/D15)))","v":60.839741309309304},{"$f":"IF((C15+(E15-C15)/G15*mspeed)<0,\"NA\",U15*(C15+(E15-C15)/G15*mspeed)*mspeed/9.55)","v":202.63371962196808},{"$f":"IF(move1,IF(speed1>speed2,AM15/2*time1/time,AM15/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z15*-speed/30*PI(),((Z15-AA15)*2/PI()+AA15)*-speed/30*PI()),IF(AccType=1,X15*-speed/30*PI(),((X15-Y15)*2/PI()+Y15)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z15*-speed/30*PI(),((Z15-AA15)*2/PI()+AA15)*-speed/30*PI()),IF(AccType=1,X15*-speed/30*PI(),((X15-Y15)*2/PI()+Y15)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD15*-speed/30*PI(),((AD15-AE15)*2/PI()+AE15)*-speed/30*PI()),IF(AccType=1,AB15*-speed/30*PI(),((AB15-AC15)*2/PI()+AC15)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD15*-speed/30*PI(),((AD15-AE15)*2/PI()+AE15)*-speed/30*PI()),IF(AccType=1,AB15*-speed/30*PI(),((AB15-AC15)*2/PI()+AC15)*-speed/30*PI()),0)/2*time7/time)))","v":164.26343163749593},{"$f":"IF(move1,MAX(IF(AccType=1,Z15*-speed/30*PI(),((Z15-AA15)*2/PI()+AA15)*-speed/30*PI()),IF(AccType=1,X15*-speed/30*PI(),((X15-Y15)*2/PI()+Y15)*-speed/30*PI()),0),MAX(IF(AccType=1,Z15*-speed/30*PI(),((Z15-AA15)*2/PI()+AA15)*-speed/30*PI()),IF(AccType=1,X15*-speed/30*PI(),((X15-Y15)*2/PI()+Y15)*-speed/30*PI()),IF(AccType=1,AD15*-speed/30*PI(),((AD15-AE15)*2/PI()+AE15)*-speed/30*PI()),IF(AccType=1,AB15*-speed/30*PI(),((AB15-AC15)*2/PI()+AC15)*-speed/30*PI()),0))","v":1580.214212352711},{"$f":"(L15^2)/1000000+((K15/1000)^2*(D15/C15*H15)^2*PI()*PI()*(O15/2)^2)/1200","v":1.8545533367685276E-4},{"$f":"SQRT(3)*L15*J15*D15/C15*H15/1000","v":0.90040132253789007},{"$f":"0.75*J15^2*(D15/C15*H15)^2-(UAC_V*0.98)^2","v":-47863.069197169469},{"$f":"-AO15/2/AN15+SQRT((AO15/2/AN15)^2-AP15/AN15)","v":13819.828030032673},{"$f":"(L15^2)/1000000+((K15/1000)^2*AV15^2*PI()*PI()*(O15/2)^2)/1200","v":7.5591782954334777E-5},{"$f":"SQRT(3)*L15*J15*AV15/1000","v":0.2158969951640469},{"$f":"0.75*J15^2*AV15^2-(UAC_V*0.98)^2","v":-50636.008045721937},{"$f":"-AS15/2/AR15+SQRT((AS15/2/AR15)^2-AT15/AR15)","v":24492.999873019809},{"$f":"D15+(F15-D15)*((0.85*UAC_V-D15*J15)/L15*1000)/G15","v":1.1464010693938547},{"$f":"(L15^2)/1000000+((K15/1000)^2*AJ15^2*PI()*PI()*(O15/2)^2)/1200","v":1.8944105167608704E-2},{"$f":"SQRT(3)*L15*J15*AJ15/1000","v":11.457698083082603},{"$f":"0.75*J15^2*AJ15^2-(UAC_V*0.98)^2","v":425602.32063243852},{"$f":"IF(((AX15/2/AW15)^2-AY15/AW15)>0,-AX15/2/AW15+SQRT((AX15/2/AW15)^2-AY15/AW15),-9999)","v":-9999}]
["AKM","AKM11E",0.185,2.91,0.17599999999999999,2.75,6000,0.61,8000,3.3,2.04,4.0999999999999996,1.7000000000000001E-3,320,6,8000,8000,8000,0.17299999999999999,1470.5882352941176,23.249927971966166,19.988542455382404,"NA",12.193010897783266,0,-9.8763388272044441,0,0,0,0,0,5.6174647795431207,7.9913652505741686,67.409577354517452,191.79276601378004,122.09906704144143,202.63371962196808,164.26343163749593,1580.214212352711,4.517113027776887E-5,0.22485860890062109,-50053.205895349165,30891.786638251931,1.7701222133894292E-5,3.9860315701076496E-2,-50781.530541823478,52447.232327496407,1.7009138211382104,4.6092768982076001E-3,2.8613485872093993,70957.417892998637,-9999]
["AKM","AKM12C",0.31,1.51,0.27900000000000003,1.347826086956522,8000,1.08,8000,12.4,9.1,13.3,3.0999999999999999E-3,320,6,8000,8000,8000,0.27900000000000003,806.45161290322585,13.910410204489052,11.296142911057995,"NA",12.199834343942635,0,-9.8818658185935355,0,0,0,0,0,1.7405132055487893,2.4760416477625511,20.886158466585471,59.424999546301223,37.831129684109911,202.74711739447108,164.35535665020436,1581.0985309749658,3.4652747961446957E-4,1.5027023391151291,-47613.749632000006,9752.4977194217827,1.8632363524879317E-4,0.35436563323387593,-50627.683882049234,15560.368697864978,1.2405596273291928,8.9497745377288274E-3,10.806455353802257,114240.17511464967,-9999]
["AKM","AKM12E",0.31,2.72,0.27900000000000003,2.4910714285714288,8000,1.08,8000,3.9,2.7,7.2,3.0999999999999999E-3,320,6,8000,8000,8000,0.27900000000000003,806.45161290322585,13.910410204489052,11.296142911057995,"NA",12.199834343942635,0,-9.8818658185935355,0,0,0,0,0,3.1352290854918583,4.4601544913338662,37.622749025902301,107.0437077920128,68.146140887933086,202.74711739447108,164.35535665020436,1581.0985309749658,1.0029632443798256E-4,0.46088088535802108,-49780.800477968784,20099.193504118699,5.3966559121643059E-5,9.6549981057102566E-2,-50760.204855120923,29787.486648859485,1.9851551835317465,2.5577823211383808E-3,3.3143548002827274,2170.0895281498742,-9999]
["AKM","AKM13C",0.40899999999999997,1.48,0.40699999999999997,1.464028776978417,8000,1.46,8000,13.5,10.3,17.899999999999999,4.5000000000000005E-3,320,6,7505.1594261272821,8000,8000,0.40699999999999997,555.55555555555554,10.492590677058951,8.3607245137684973,"NA",12.206657790102007,0,-9.8873928099826252,0,0,0,0,0,1.293728997325162,1.8404496260544996,15.524747967901945,44.170791025307992,28.119998927827581,202.86051516697407,164.44728166291267,1581.9828495972199,5.3959861099869843E-4,2.2112542977603922,-46990.01255659639,7505.1594261272821,3.3715917574733483E-4,0.61126061991551017,-50513.627630957606,11367.185237580292,1.4604240987098587,6.5300447784740088E-3,11.769627734732568,57278.340057883746,-9999]
["AKM","AKM13D",0.40100000000000002,2.4,0.36499999999999999,2.1597633136094672,7000,1.44,8000,5.21,3.8,10.9,4.5000000000000005E-3,320,6,8000,8000,8000,0.35985714285714282,555.55555555555554,10.761286952184495,8.4768456875708385,2.4625753759600251,12.206657790102007,0,-9.8873928099826252,0,0,0,0,0,2.1397930575156345,3.0440543117461356,25.677516690187616,73.057303481907255,46.50972391244111,202.86051516697407,164.44728166291267,1581.9828495972199,1.9820386132351152E-4,0.84772347511949153,-49293.008055153892,13776.000346156397,1.2236543940676625E-4,0.17939378307058143,-50737.442363849063,19642.843108686193,1.8238223766353612,2.4309585072749768E-3,4.5747631069279455,-6767.5001133973783,974.58945761786867]
["AKM","AKM21C",0.48,1.58,0.39,1.3,8000,1.47,8000,13,19,19.5,1.1000000000000001E-2,640,6,5920.4767598374192,8000,8000,0.39,227.27272727272725,9.0571467945474318,8.3254000515931583,"NA",12.238338075841941,0,-9.9130538414319709,0,0,0,0,0,1.1799033421754312,1.6785220624852666,14.158840106105176,40.284529499646396,25.645928000000005,203.38700482502375,164.87407636477289,1586.0886146291152,1.0059045097641352E-3,2.12457357423891,-47837.498676953132,5920.4767598374192,4.230766901500468E-4,0.5558552877275883,-50602.020551680005,10299.191559014414,1.2659692307692307,1.795564312319535E-2,11.26048275187471,32560.041712865102,-9999]
["AKM","AKM21E",0.5,3.11,0.41,2.5625,7000,1.49,8000,3.42,5.2,10.199999999999999,1.1000000000000001E-2,640,6,8000,8000,8000,0.39714285714285713,227.27272727272725,8.7039051583990652,8.2136497153301615,1.0805968688069927,12.238338075841941,0,-9.9130538414319709,0,0,0,0,0,2.2295692521512449,3.1717692846557028,26.754831025814941,76.122462831736868,48.461064960000002,203.38700482502375,164.87407636477289,1586.0886146291152,2.7595786227686131E-4,0.55996844974851034,-50051.688583444469,12491.103953011752,1.0977324357665165E-4,0.10225940318445276,-50780.032679883603,21047.178640405484,1.6924519537815126,4.8046433267481033E-3,2.9280592393893974,-30203.634362327903,2220.9947754611421]
["AKM","AKM21G",0.5,4.87,0.46,4.5999999999999996,4000,1.51,8000,1.44,2.1800000000000002,6.6,1.1000000000000001E-2,640,6,8000,8000,8000,0.42000000000000004,227.27272727272725,8.6812414560296496,8.104859652875458,0.57070618840336984,12.238338075841941,0,-9.9130538414319709,0,0,0,0,0,3.4913190540117571,4.9667255357791875,41.895828648141084,119.20141285870051,75.885976320000012,203.38700482502375,164.87407636477289,1586.0886146291152,1.1965319231905482E-4,0.24210455430495473,-50468.758397525249,19550.785492299281,4.660540423578431E-5,4.8434244603799748E-2,-50791.696524045343,32496.953952122865,2.9422899999999967,2.0693622442518088E-3,1.2491902358642555,-41849.258683548018,4205.316235862686]
["AKM","AKM22C",0.84,1.39,0.68,1.1147540983606559,8000,2.73,8000,19.399999999999999,35.5,39,1.6E-2,640,6,2863.9212395452923,5033.7201274268664,5779.4871794871797,0.73932559745146265,156.25,5.186698771742857,4.4918342587586517,13.023662234407601,12.26270752641112,0,-9.9327930963930058,0,0,0,0,0,0.594333239624798,0.84549421933092539,7.1319988754975761,20.291861263942209,12.918200098765432,203.79199686967732,165.20237998158848,1589.2468954228809,3.4247680647328856E-3,5.9200466032473704,-45044.648529812504,2863.9212395452923,1.6647424101895907E-3,1.6267116170397711,-50370.217415349747,5033.7201274268664,1.2413195744010088,1.7088602345633627E-2,16.928909045880719,-3699.972379404644,184.27996340840048]
["AKM","AKM22E",0.87,2.73,0.7,2.1875,8000,2.76,8000,5.09,9.6999999999999993,22.4,1.6E-2,640,6,6156.4691791625019,8000,8000,0.7,156.25,5.0092550697661444,4.4430099733373627,0.99140502675068232,12.26270752641112,0,-9.9327930963930058,0,0,0,0,0,1.1270362896779846,1.6033137714129484,13.524435476135816,38.47953051391076,24.496829956577269,203.79199686967732,165.20237998158848,1589.2468954228809,1.0241675324533163E-3,1.7103260263654887,-49347.682761647426,6156.4691791625019,5.3486591964969964E-4,0.43055339462597264,-50712.797004930675,9343.0775550219223,2.1802213574218752,4.6812592578953302E-3,4.8376708445107983,-39144.675306207238,2420.8067694249748]
["AKM","AKM22G",0.88,4.82,0.74,4.1111111111111116,7000,2.79,8000,1.69,3.19,11.7,1.6E-2,640,6,8000,8000,8000,0.72,156.25,4.9484951216188939,4.3952356725487887,0.470380469749001,12.26270752641112,0,-9.9327930963930058,0,0,0,0,0,1.9672469102296291,2.7985913957055684,23.60696292275555,67.166193496933644,42.75932681481482,203.79199686967732,165.20237998158848,1589.2468954228809,3.1279553846056475E-4,0.52336148984493103,-50304.927607106612,11872.604423923687,1.4459537478402493E-4,0.109536507582846,-50783.24779586996,18365.638573181976,3.1983478551078557,1.5141124496109266E-3,1.4644146096892916,-46888.675689474323,5102.2526536458035]
["AKM","AKM23C",1.1299999999999999,1.41,0.99,1.2375,5500,3.77,8000,20.3,40.700000000000003,51.8,2.2000000000000002E-2,640,6,2168.7944080373672,3776.8211350488227,4351.3513513513517,1.0338627347442118,113.63636363636363,3.8625309341404264,3.2604644209798761,3.2092590349644481,12.291950867094133,0,-9.9564802023462473,0,0,0,0,0,0.4492308991695606,0.63907266676263752,5.3907707900347273,15.3377440023033,9.764311095378563,204.27798732326156,165.59634432176711,1593.0368323753996,5.3966402831604329E-3,8.5677827238047595,-43965.769859504995,2168.7944080373672,2.8933286591653709E-3,2.3840360378791097,-50275.61103774669,3776.8211350488227,1.3089600473850473,1.4373738830812759E-2,17.783941979703279,-21338.117139740341,747.83617459741356]
["AKM","AKM23D",1.1599999999999999,2.19,0.92,1.7692307692307692,8000,3.84,8000,8.36,17.3,33.799999999999997,2.2000000000000002E-2,640,6,3859.2504450767256,6059.9830533650102,6668.6390532544392,0.97820050839904971,113.63636363636363,3.7683727785885979,3.2010288716390973,1.1812920358595744,12.291950867094133,0,-9.9564802023462473,0,0,0,0,0,0.6796965677273854,0.96693147984684458,8.1563588127286248,23.206355516324269,14.773624766283524,204.27798732326156,165.59634432176711,1593.0368323753996,2.3068017093524447E-3,3.5481416950475198,-48050.243004767282,3859.2504450767256,1.2236221670080792E-3,0.93688722572707084,-50613.080399817372,6059.9830533650102,1.9142722883477468,5.9777836330060482E-3,7.2305389392450525,-39364.582518482595,2031.6737327816022]
["AKM","AKM23E",1.1599999999999999,2.78,0.98,2.3333333333333299,6500,3.86,8000,5.44,11.1,27,2.2000000000000002E-2,640,6,4965.6276363877269,7700.3125470769683,8000,0.94676057561940707,113.63636363636363,3.7649506557378798,3.1844432298171332,0.871431739535108,12.291950867094133,0,-9.9564802023462473,0,0,0,0,0,0.86281116816535686,1.2274290018147158,10.353734017984282,29.45829604355318,18.75373372158365,204.27798732326156,165.59634432176711,1593.0368323753996,1.5094681578589752E-3,2.3534089599695966,-48905.800009305494,4965.6276363877269,7.7812785601837347E-4,0.59045079790528499,-50685.60165132134,7700.3125470769683,2.3209213447293413,3.9366166339601764E-3,4.7710177963414075,-42999.052039435388,2754.0883480791663]
["AKM","AKM23F",1.18,4.3099999999999996,0.94,3.481481481481481,8000,3.88,8000,2.23,4.68,17.600000000000001,2.2000000000000002E-2,640,6,8000,8000,8000,0.94,113.63636363636363,3.7037602813868125,3.1680285739933334,0.49545851843914829,12.291950867094133,0,-9.9564802023462473,0,0,0,0,0,1.3149953409216917,1.8707029744765435,15.779944091060301,44.896871387437045,28.582236042686748,204.27798732326156,165.59634432176711,1593.0368323753996,6.3537671593085518E-4,0.96339668294950298,-50056.085580515479,8150.0965274782147,3.2652983750955221E-4,0.2186332587525387,-50766.581340850375,12138.592829262958,3.2161631368371206,1.6342391251620489E-3,1.9430069752594596,-47758.223576715107,4843.9978538682963]
["AKM","AKM24C",1.38,1.42,1.25,1.2886597938144331,4500,4.67,8000,20.399999999999999,43.8,62.4,2.7000000000000003E-2,640,6,1835.0861618368431,3141.3235552466431,3612.1794871794873,1.2892506528484302,92.592592592592581,3.1667673119821229,2.6373276911484611,2.4241838836706884,12.316320317663314,0,-9.976219457307284,0,0,0,0,0,0.37119179595354784,0.52805479622831841,4.4543015514425743,12.673315109479642,8.0680829801395593,204.68297936791518,165.92464793858267,1596.1951131691653,7.1729116881755275E-3,10.595013709748901,-43597.83883037429,1835.0861618368431,4.149549980825124E-3,2.9591197067998554,-50242.953454195223,3141.3235552466431,1.3421070255822833,1.3137547269313462E-2,17.788762660168164,-30488.032276424772,990.02390708329051]
["AKM","AKM24D",1.41,2.21,1.1000000000000001,1.7460317460317463,8000,4.76,8000,8.4,18.7,40.799999999999997,2.7000000000000003E-2,640,6,3276.9205405480579,5036.6336789894885,5524.5098039215691,1.2148304449391574,92.592592592592581,3.1086691600529259,2.5874622516099399,1.0942776486460772,12.316320317663314,0,-9.976219457307284,0,0,0,0,0,0.56540842038713923,0.80434597819255105,6.7849010446456708,19.304303476621225,12.289501285001313,204.68297936791518,165.92464793858267,1596.1951131691653,3.105442486655942E-3,4.4287400565669151,-47859.517325211411,3276.9205405480579,1.7639258090656547E-3,1.1625765405960382,-50602.175538983771,5036.6336789894885,1.9584905423280423,5.574063691499374E-3,7.2951518431046241,-42812.554930142134,2193.2276538495153]
["AKM","AKM24E",1.4,2.79,1.24,2.48,5500,4.79,8000,5.44,11.8,32.4,2.7000000000000003E-2,640,6,{"$f":"IF(AQ33<I33,IF(AQ33<0,0,AQ33),I33)","v":4273.7683777915881},{"$f":"IF(AU33<I33,IF(AU33<0,0,AU33),I33)","v":6416.2352749085685},{"$f":"IF(UAC_V*0.98/L33*1000<I33,IF(UAC_V*0.98/L33*1000<0,0,UAC_V*0.98/L33*1000),I33)","v":6956.7901234567908},{"$f":"C33+(E33-C33)/G33*Q33","v":1.2133458829117507},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M33,(inertia/gear^2+gear_inertia)/M33),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M33,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M33))","v":92.592592592592581},{"$f":"IF((C33+(E33-C33)/G33*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X33^2*time1+Y33^2*time2+Z33^2*time3+AA33^2*time4)/time)/(C33+(E33-C33)/G33*mspeed),SQRT((((X33-Y33)*2/PI()+Y33)^2*time1+Y33^2*time2+((Z33-Y33)*2/PI()+Y33)^2*time3+AA33^2*time4)/time)/(C33+(E33-C33)/G33*mspeed)),IF(AccType=1,SQRT((X33^2*time1+Y33^2*time2+Z33^2*time3+AA33^2*time4+AB33^2*time5+AC33^2*time6+AD33^2*time7+AE33^2*time8)/time)/(C33+(E33-C33)/G33*mspeed),SQRT((((X33-Y33)*2/PI()+Y33)^2*time1+Y33^2*time2+((Z33-Y33)*2/PI()+Y33)^2*time3+AA33^2*time4+((AB33-AC33)*2/PI()+AC33)^2*time5+AC33^2*time6+((AD33-AC33)*2/PI()+AC33)^2*time7+AE33^2*time8)/time)/(C33+(E33-C33)/G33*mspeed))))","v":3.1213075747588963},{"$f":"IF(move1,MAX(ABS(X33),ABS(Z33))/H33,MAX(ABS(X33),ABS(Z33),ABS(AB33),ABS(AD33))/H33)","v":2.5712568512867042},{"$f":"IF(AZ33>0,speed/(MIN(AZ33,I33)),\"NA\")","v":0.81060195626488896},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M33+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M33+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.316320317663314},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M33+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M33+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-9.976219457307284},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M33+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M33+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M33+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M33+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH33/Irms","v":0.71889469455752009},{"$f":"AI33/Ipeak","v":1.0226944549488288},{"$f":"IF(move1,IF(AccType=1,SQRT((X33^2*time1+Y33^2*time2+Z33^2*time3+AA33^2*time4)/time)/(C33/D33),SQRT((((X33-Y33)*2/PI()+Y33)^2*time1+Y33^2*time2+((Z33-AA33)*2/PI()+AA33)^2*time3+AA33^2*time4)/time)/(C33/D33)),IF(AccType=1,SQRT((X33^2*time1+Y33^2*time2+Z33^2*time3+AA33^2*time4+AB33^2*time5+AC33^2*time6+AD33^2*time7+AE33^2*time8)/time)/(C33/D33),SQRT((((X33-Y33)*2/PI()+Y33)^2*time1+Y33^2*time2+((Z33-AA33)*2/PI()+AA33)^2*time3+AA33^2*time4+((AB33-AC33)*2/PI()+AC33)^2*time5+AC33^2*time6+((AD33-AE33)*2/PI()+AE33)^2*time7+AE33^2*time8)/time)/(C33/D33)))","v":8.626736334690241},{"$f":"IF(move1,MAX(ABS(X33),ABS(Z33))/(C33/D33),MAX(ABS(X33),ABS(Z33),ABS(AB33),ABS(AD33))/(C33/D33))","v":24.544666918771892},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X33),ABS(Z33))/(C33/D33),MAX(ABS((X33-Y33)*2/PI()+Y33),ABS((Z33-Y33)*2/PI()+Y33))/(C33/D33)),IF(AccType=1,MAX(ABS(X33),ABS(Z33),ABS(AB33),ABS(AD33))/(C33/D33),MAX(ABS((X33-Y33)*2/PI()+Y33),ABS((Z33-Y33)*2/PI()+Y33),ABS((AB33-AC33)*2/PI()+AC33),ABS((AD33-AC33)*2/PI()+AC33))/(C33/D33)))","v":15.625620266666667},{"$f":"IF((C33+(E33-C33)/G33*mspeed)<0,\"NA\",U33*(C33+(E33-C33)/G33*mspeed)*mspeed/9.55)","v":204.68297936791518},{"$f":"IF(move1,IF(speed1>speed2,AM33/2*time1/time,AM33/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z33*-speed/30*PI(),((Z33-AA33)*2/PI()+AA33)*-speed/30*PI()),IF(AccType=1,X33*-speed/30*PI(),((X33-Y33)*2/PI()+Y33)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z33*-speed/30*PI(),((Z33-AA33)*2/PI()+AA33)*-speed/30*PI()),IF(AccType=1,X33*-speed/30*PI(),((X33-Y33)*2/PI()+Y33)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD33*-speed/30*PI(),((AD33-AE33)*2/PI()+AE33)*-speed/30*PI()),IF(AccType=1,AB33*-speed/30*PI(),((AB33-AC33)*2/PI()+AC33)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD33*-speed/30*PI(),((AD33-AE33)*2/PI()+AE33)*-speed/30*PI()),IF(AccType=1,AB33*-speed/30*PI(),((AB33-AC33)*2/PI()+AC33)*-speed/30*PI()),0)/2*time7/time)))","v":165.92464793858267},{"$f":"IF(move1,MAX(IF(AccType=1,Z33*-speed/30*PI(),((Z33-AA33)*2/PI()+AA33)*-speed/30*PI()),IF(AccType=1,X33*-speed/30*PI(),((X33-Y33)*2/PI()+Y33)*-speed/30*PI()),0),MAX(IF(AccType=1,Z33*-speed/30*PI(),((Z33-AA33)*2/PI()+AA33)*-speed/30*PI()),IF(AccType=1,X33*-speed/30*PI(),((X33-Y33)*2/PI()+Y33)*-speed/30*PI()),IF(AccType=1,AD33*-speed/30*PI(),((AD33-AE33)*2/PI()+AE33)*-speed/30*PI()),IF(AccType=1,AB33*-speed/30*PI(),((AB33-AC33)*2/PI()+AC33)*-speed/30*PI()),0))","v":1596.1951131691653},{"$f":"(L33^2)/1000000+((K33/1000)^2*(D33/C33*H33)^2*PI()*PI()*(O33/2)^2)/1200","v":1.9889390263936883E-3},{"$f":"SQRT(3)*L33*J33*D33/C33*H33/1000","v":2.9141789597131709},{"$f":"0.75*J33^2*(D33/C33*H33)^2-(UAC_V*0.98)^2","v":-48782.688432871575},{"$f":"-AO33/2/AN33+SQRT((AO33/2/AN33)^2-AP33/AN33)","v":4273.7683777915881},{"$f":"(L33^2)/1000000+((K33/1000)^2*AV33^2*PI()*PI()*(O33/2)^2)/1200","v":1.1129625042506414E-3},{"$f":"SQRT(3)*L33*J33*AV33/1000","v":0.75597802038532724},{"$f":"0.75*J33^2*AV33^2-(UAC_V*0.98)^2","v":-50669.056803244144},{"$f":"-AS33/2/AR33+SQRT((AS33/2/AR33)^2-AT33/AR33)","v":6416.2352749085685},{"$f":"D33+(F33-D33)*((0.85*UAC_V-D33*J33)/L33*1000)/G33","v":2.4763078338945004},{"$f":"(L33^2)/1000000+((K33/1000)^2*AJ33^2*PI()*PI()*(O33/2)^2)/1200","v":3.5662751840738142E-3},{"$f":"SQRT(3)*L33*J33*AJ33/1000","v":4.7702572817490738},{"$f":"0.75*J33^2*AJ33^2-(UAC_V*0.98)^2","v":-45385.979774500825},{"$f":"IF(((AX33/2/AW33)^2-AY33/AW33)>0,-AX33/2/AW33+SQRT((AX33/2/AW33)^2-AY33/AW33),-9999)","v":2960.7626547791438}]
["AKM","AKM24F",1.42,3.89,1.1200000000000001,3.1111111111111116,8000,4.82,8000,2.77,6.16,23.4,2.7000000000000003E-2,640,6,{"$f":"IF(AQ34<I34,IF(AQ34<0,0,AQ34),I34)","v":6251.2804138430402},{"$f":"IF(AU34<I34,IF(AU34<0,0,AU34),I34)","v":8000},{"$f":"IF(UAC_V*0.98/L34*1000<I34,IF(UAC_V*0.98/L34*1000<0,0,UAC_V*0.98/L34*1000),I34)","v":8000},{"$f":"C34+(E34-C34)/G34*Q34","v":1.1200000000000001},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M34,(inertia/gear^2+gear_inertia)/M34),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M34,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M34))","v":92.592592592592581},{"$f":"IF((C34+(E34-C34)/G34*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X34^2*time1+Y34^2*time2+Z34^2*time3+AA34^2*time4)/time)/(C34+(E34-C34)/G34*mspeed),SQRT((((X34-Y34)*2/PI()+Y34)^2*time1+Y34^2*time2+((Z34-Y34)*2/PI()+Y34)^2*time3+AA34^2*time4)/time)/(C34+(E34-C34)/G34*mspeed)),IF(AccType=1,SQRT((X34^2*time1+Y34^2*time2+Z34^2*time3+AA34^2*time4+AB34^2*time5+AC34^2*time6+AD34^2*time7+AE34^2*time8)/time)/(C34+(E34-C34)/G34*mspeed),SQRT((((X34-Y34)*2/PI()+Y34)^2*time1+Y34^2*time2+((Z34-Y34)*2/PI()+Y34)^2*time3+AA34^2*time4+((AB34-AC34)*2/PI()+AC34)^2*time5+AC34^2*time6+((AD34-AC34)*2/PI()+AC34)^2*time7+AE34^2*time8)/time)/(C34+(E34-C34)/G34*mspeed))))","v":3.0852623034693978},{"$f":"IF(move1,MAX(ABS(X34),ABS(Z34))/H34,MAX(ABS(X34),ABS(Z34),ABS(AB34),ABS(AD34))/H34)","v":2.5552531779384466},{"$f":"IF(AZ34>0,speed/(MIN(AZ34,I34)),\"NA\")","v":0.53352791813427136},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M34+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M34+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.316320317663314},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M34+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M34+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-9.976219457307284},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M34+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M34+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M34+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M34+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH34/Irms","v":0.98821255655516549},{"$f":"AI34/Ipeak","v":1.4058241207661473},{"$f":"IF(move1,IF(AccType=1,SQRT((X34^2*time1+Y34^2*time2+Z34^2*time3+AA34^2*time4)/time)/(C34/D34),SQRT((((X34-Y34)*2/PI()+Y34)^2*time1+Y34^2*time2+((Z34-AA34)*2/PI()+AA34)^2*time3+AA34^2*time4)/time)/(C34/D34)),IF(AccType=1,SQRT((X34^2*time1+Y34^2*time2+Z34^2*time3+AA34^2*time4+AB34^2*time5+AC34^2*time6+AD34^2*time7+AE34^2*time8)/time)/(C34/D34),SQRT((((X34-Y34)*2/PI()+Y34)^2*time1+Y34^2*time2+((Z34-AA34)*2/PI()+AA34)^2*time3+AA34^2*time4+((AB34-AC34)*2/PI()+AC34)^2*time5+AC34^2*time6+((AD34-AE34)*2/PI()+AE34)^2*time7+AE34^2*time8)/time)/(C34/D34)))","v":11.858550678661986},{"$f":"IF(move1,MAX(ABS(X34),ABS(Z34))/(C34/D34),MAX(ABS(X34),ABS(Z34),ABS(AB34),ABS(AD34))/(C34/D34))","v":33.739778898387534},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X34),ABS(Z34))/(C34/D34),MAX(ABS((X34-Y34)*2/PI()+Y34),ABS((Z34-Y34)*2/PI()+Y34))/(C34/D34)),IF(AccType=1,MAX(ABS(X34),ABS(Z34),ABS(AB34),ABS(AD34))/(C34/D34),MAX(ABS((X34-Y34)*2/PI()+Y34),ABS((Z34-Y34)*2/PI()+Y34),ABS((AB34-AC34)*2/PI()+AC34),ABS((AD34-AC34)*2/PI()+AC34))/(C34/D34)))","v":21.479410362023998},{"$f":"IF((C34+(E34-C34)/G34*mspeed)<0,\"NA\",U34*(C34+(E34-C34)/G34*mspeed)*mspeed/9.55)","v":204.68297936791518},{"$f":"IF(move1,IF(speed1>speed2,AM34/2*time1/time,AM34/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z34*-speed/30*PI(),((Z34-AA34)*2/PI()+AA34)*-speed/30*PI()),IF(AccType=1,X34*-speed/30*PI(),((X34-Y34)*2/PI()+Y34)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z34*-speed/30*PI(),((Z34-AA34)*2/PI()+AA34)*-speed/30*PI()),IF(AccType=1,X34*-speed/30*PI(),((X34-Y34)*2/PI()+Y34)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD34*-speed/30*PI(),((AD34-AE34)*2/PI()+AE34)*-speed/30*PI()),IF(AccType=1,AB34*-speed/30*PI(),((AB34-AC34)*2/PI()+AC34)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD34*-speed/30*PI(),((AD34-AE34)*2/PI()+AE34)*-speed/30*PI()),IF(AccType=1,AB34*-speed/30*PI(),((AB34-AC34)*2/PI()+AC34)*-speed/30*PI()),0)/2*time7/time)))","v":165.92464793858267},{"$f":"IF(move1,MAX(IF(AccType=1,Z34*-speed/30*PI(),((Z34-AA34)*2/PI()+AA34)*-speed/30*PI()),IF(AccType=1,X34*-speed/30*PI(),((X34-Y34)*2/PI()+Y34)*-speed/30*PI()),0),MAX(IF(AccType=1,Z34*-speed/30*PI(),((Z34-AA34)*2/PI()+AA34)*-speed/30*PI()),IF(AccType=1,X34*-speed/30*PI(),((X34-Y34)*2/PI()+Y34)*-speed/30*PI()),IF(AccType=1,AD34*-speed/30*PI(),((AD34-AE34)*2/PI()+AE34)*-speed/30*PI()),IF(AccType=1,AB34*-speed/30*PI(),((AB34-AC34)*2/PI()+AC34)*-speed/30*PI()),0))","v":1596.1951131691653},{"$f":"(L34^2)/1000000+((K34/1000)^2*(D34/C34*H34)^2*PI()*PI()*(O34/2)^2)/1200","v":1.0372700574643808E-3},{"$f":"SQRT(3)*L34*J34*D34/C34*H34/1000","v":1.4823970737534444},{"$f":"0.75*J34^2*(D34/C34*H34)^2-(UAC_V*0.98)^2","v":-49801.844799714745},{"$f":"-AO34/2/AN34+SQRT((AO34/2/AN34)^2-AP34/AN34)","v":6251.2804138430402},{"$f":"(L34^2)/1000000+((K34/1000)^2*AV34^2*PI()*PI()*(O34/2)^2)/1200","v":5.7492680608841544E-4},{"$f":"SQRT(3)*L34*J34*AV34/1000","v":0.35043469301324925},{"$f":"0.75*J34^2*AV34^2-(UAC_V*0.98)^2","v":-50749.091042229491},{"$f":"-AS34/2/AR34+SQRT((AS34/2/AR34)^2-AT34/AR34)","v":9095.4165818214824},{"$f":"D34+(F34-D34)*((0.85*UAC_V-D34*J34)/L34*1000)/G34","v":3.1214101691595446},{"$f":"(L34^2)/1000000+((K34/1000)^2*AJ34^2*PI()*PI()*(O34/2)^2)/1200","v":1.8434470311138249E-3},{"$f":"SQRT(3)*L34*J34*AJ34/1000","v":2.4114519298654691},{"$f":"0.75*J34^2*AJ34^2-(UAC_V*0.98)^2","v":-48150.153968673803},{"$f":"IF(((AX34/2/AW34)^2-AY34/AW34)>0,-AX34/2/AW34+SQRT((AX34/2/AW34)^2-AY34/AW34),-9999)","v":4498.3587895319833}]
["AKM","AKM31C",1.1499999999999999,1.37,1,1.1764705882352942,5000,3.88,8000,21.4,37.5,54.5,3.3000000000000002E-2,640,8,1920.4002794440739,3557.794643069557,4135.7798165137619,1.0432661607079132,75.757575757575751,3.8181126737440185,3.1818463036975073,3.6550442760494204,12.345563658346329,0,-9.9999065632605255,0,0,0,0,0,0.43076636513907646,0.61280515260632151,5.1691963816689173,14.707323662551715,9.362973042190017,205.16896982149947,166.31861227876132,1599.985050121684,6.9240065303963795E-3,9.3373869206654927,-43466.821938707602,1920.4002794440739,3.2603142012980835E-3,2.5291084975301867,-50266.788668270405,3557.794643069557,1.2519775974096061,1.9193152698629028E-2,18.914056235625697,-20694.771709080778,656.62679265654651]
["AKM","AKM31E",1.2,2.99,0.95,2.3170731707317072,6000,4,8000,4.58,8.6,26.1,3.3000000000000002E-2,640,8,4875.9179024572877,8000,8000,0.8666666666666667,75.757575757575751,3.6735196749087176,3.0863909145865822,0.87001490813937798,12.345563658346329,0,-9.9999065632605255,0,0,0,0,0,0.90096724241527637,1.2817095603630391,10.811606908983316,30.761029448712939,19.583079565432097,205.16896982149947,166.31861227876132,1599.985050121684,1.648006905577037E-3,2.0635573647038465,-49242.400719666672,4875.9179024572877,7.2869242628675575E-4,0.45731492131169538,-50728.407993550332,8035.7073446553786,2.2087611715416005,4.4136889005754396E-3,4.0545961265045616,-44771.870064053015,2758.5734193137705]
["AKM","AKM31H",1.23,5.85,0.97,4.6190476190476195,6000,4.0599999999999996,8000,1.25,2.4,13.7,3.3000000000000002E-2,640,8,8000,8000,8000,0.8833333333333333,75.757575757575751,3.5847572615401582,3.0407792261936772,0.41019995349054061,12.345563658346329,0,-9.9999065632605255,0,0,0,0,0,1.7197678010047692,2.446529383513754,20.637213612057231,58.716705204330097,37.380215501355011,205.16896982149947,166.31861227876132,1599.985050121684,4.7031758128761428E-4,0.57275382175689737,-50368.206858733647,9757.6216247594748,1.9465760676802359E-4,8.992957500166078E-2,-50794.38781120468,15924.363287965984,3.0318752896535761,1.2468085316000375E-3,1.1087484056415278,-49167.721901256555,5850.8051489950867]
["AKM","AKM32C",2,1.44,1.86,1.3285714285714287,3000,6.92,8000,23,46.5,89.8,5.9000000000000004E-2,640,8,1158.5766415294784,2143.8695274327356,2510.0222717149222,1.8999527553864723,42.372881355932201,2.2151624220439685,1.8023532949864254,2.3989864608890135,12.472284801306063,0,-10.10255068905791,0,0,0,0,0,0.26301871480621125,0.37416854403918193,3.1562245776745348,8.9800450569403658,5.7168742400000001,207.27492845369801,168.02579108620222,1616.4081102492655,1.5127566349111322E-2,17.823926841575823,-40956.115102720003,1158.5766415294784,8.6003083915569128E-3,4.9111557351383235,-50057.412882711957,2143.8695274327356,1.372836780146357,1.7363584247789991E-2,20.451418636851599,-37838.318185606695,1000.4224863822745]
["AKM","AKM32D",2.04,2.23,1.65,1.793478260869565,5500,7.1,8000,9.57,20.100000000000001,59,5.9000000000000004E-2,640,8,2134.9209029599328,3444.3472775324426,3820.3389830508472,1.7957644657749723,42.372881355932201,2.1831116324976825,1.7566598311698682,1.2206440301201822,12.472284801306063,0,-10.10255068905791,0,0,0,0,0,0.39932716095986587,0.56807996541896488,4.7919259315183904,13.633919170055158,8.679622518518519,207.27492845369801,168.02579108620222,1616.4081102492655,6.6835556530417985E-3,7.5902769260358234,-46667.534043815584,2134.9209029599328,3.6927529320714084E-3,1.9517491308923292,-50531.58023341433,3444.3472775324426,1.9957191189120385,7.4862743797067081E-3,8.4883917513537952,-45630.440485173007,1966.175183573954]
["AKM","AKM32E",2.04,2.82,1.41,1.9315068493150684,7000,7.11,8000,6.3,12.8,47.1,5.9000000000000004E-2,640,8,2802.2198880935462,4405.1444304271081,4785.5626326963911,1.6435370012615602,42.372881355932201,2.1925245959168422,1.7541891422371396,0.92311472982012632,12.472284801306063,0,-10.10255068905791,0,0,0,0,0,0.50497874166225187,0.71837914909483447,6.0597448999470229,17.241099578276028,10.976024888888888,207.27492845369801,168.02579108620222,1616.4081102492655,4.3011521417505635E-3,5.0513868062215588,-47929.619785829804,2802.2198880935462,2.3365708123937079E-3,1.2031772384822332,-50642.021145234459,4405.1444304271081,2.3410329340496339,4.815868321237868E-3,5.6411437546421128,-47218.976330103804,2599.8935153679677]
["AKM","AKM32H",2.1,5.5,1.45,3.7179487179487176,7000,7.26,8000,1.64,3.55,24.8,5.9000000000000004E-2,640,8,5893.0804373080191,8000,8000,1.3571428571428572,42.372881355932201,2.129979211529113,1.7179455649181905,0.42880370696432413,12.472284801306063,0,-10.10255068905791,0,0,0,0,0,0.95674797052523919,1.361062825539352,11.48097564630287,32.665507812944448,20.795508148148148,207.27492845369801,168.02579108620222,1616.4081102492655,1.2146311569246914E-3,1.3394798094697493,-50075.855336897963,5893.0804373080191,6.3636312458953815E-4,0.25260037119648898,-50779.223903352387,8736.5926715231271,3.5857320099255583,1.3322300606420606E-3,1.4649597524023799,-49932.815487383406,5596.9665397497993]
["AKM","AKM33C",2.71,1.47,2.54,1.3655913978494623,2000,9.76,8000,25.4,53.6,120,8.5000000000000006E-2,640,8,783.50085743951092,1586.6170225074115,1878.3333333333335,2.5751375530868699,29.411764705882351,1.6574918011572584,1.2908817565846102,2.5110130167820026,12.599005944265796,0,-10.205194814855295,0,0,0,0,0,0.20016699081821984,0.2847561306591439,2.402003889818638,6.8341471358194541,4.350753193931939,209.38088708589663,169.73296989364314,1632.831170376847,2.4996532743950292E-2,27.949461936413833,-37243.138775433239,783.50085743951092,1.5142274452347948E-2,7.3973099461116645,-49855.156624325653,1586.6170225074115,1.401193861111111,2.1556438718986829E-2,22.968891577236025,-41645.958953353751,955.78954946069064]
["AKM","AKM33E",2.79,2.58,2.34,2.127272727272727,4500,9.9600000000000009,8000,8.36,18.5,70.599999999999994,8.5000000000000006E-2,640,8,1821.3676049194169,2888.5945998480238,3192.6345609065161,2.5011405400151974,29.411764705882351,1.6132734395945771,1.2649604361712645,1.1557682367871673,12.599005944265796,0,-10.205194814855295,0,0,0,0,0,0.34123998888226409,0.48544556953712298,4.0948798665871688,11.650693668890952,7.4170619514137792,209.38088708589663,169.73296989364314,1632.831170376847,8.8049604370576146E-3,9.4155663249074024,-46358.60672040491,1821.3676049194169,5.2293188845915078E-3,2.384115187680941,-50520.06797072589,2888.5945998480238,2.3321454270752855,7.4620430613455118E-3,7.5823444974922607,-47921.542640968393,2076.5408873595438]
["AKM","AKM33H",2.88,5.62,2.27,4.365384615384615,5500,10.220000000000001,8000,1.82,4.0999999999999996,33.4,8.5000000000000006E-2,640,8,{"$f":"IF(AQ44<I44,IF(AQ44<0,0,AQ44),I44)","v":4498.0832303371017},{"$f":"IF(AU44<I44,IF(AU44<0,0,AU44),I44)","v":6426.9288479748921},{"$f":"IF(UAC_V*0.98/L44*1000<I44,IF(UAC_V*0.98/L44*1000<0,0,UAC_V*0.98/L44*1000),I44)","v":6748.5029940119757},{"$f":"C44+(E44-C44)/G44*Q44","v":2.1671951641336937},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M44,(inertia/gear^2+gear_inertia)/M44),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M44,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M44))","v":29.411764705882351},{"$f":"IF((C44+(E44-C44)/G44*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X44^2*time1+Y44^2*time2+Z44^2*time3+AA44^2*time4)/time)/(C44+(E44-C44)/G44*mspeed),SQRT((((X44-Y44)*2/PI()+Y44)^2*time1+Y44^2*time2+((Z44-Y44)*2/PI()+Y44)^2*time3+AA44^2*time4)/time)/(C44+(E44-C44)/G44*mspeed)),IF(AccType=1,SQRT((X44^2*time1+Y44^2*time2+Z44^2*time3+AA44^2*time4+AB44^2*time5+AC44^2*time6+AD44^2*time7+AE44^2*time8)/time)/(C44+(E44-C44)/G44*mspeed),SQRT((((X44-Y44)*2/PI()+Y44)^2*time1+Y44^2*time2+((Z44-Y44)*2/PI()+Y44)^2*time3+AA44^2*time4+((AB44-AC44)*2/PI()+AC44)^2*time5+AC44^2*time6+((AD44-AC44)*2/PI()+AC44)^2*time7+AE44^2*time8)/time)/(C44+(E44-C44)/G44*mspeed))))","v":1.5647746975661452},{"$f":"IF(move1,MAX(ABS(X44),ABS(Z44))/H44,MAX(ABS(X44),ABS(Z44),ABS(AB44),ABS(AD44))/H44)","v":1.2327794466013497},{"$f":"IF(AZ44>0,speed/(MIN(AZ44,I44)),\"NA\")","v":0.47728211811270765},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M44+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M44+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.599005944265796},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M44+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M44+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.205194814855295},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M44+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M44+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M44+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M44+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH44/Irms","v":0.72009242808948681},{"$f":"AI44/Ipeak","v":1.024398342111889},{"$f":"IF(move1,IF(AccType=1,SQRT((X44^2*time1+Y44^2*time2+Z44^2*time3+AA44^2*time4)/time)/(C44/D44),SQRT((((X44-Y44)*2/PI()+Y44)^2*time1+Y44^2*time2+((Z44-AA44)*2/PI()+AA44)^2*time3+AA44^2*time4)/time)/(C44/D44)),IF(AccType=1,SQRT((X44^2*time1+Y44^2*time2+Z44^2*time3+AA44^2*time4+AB44^2*time5+AC44^2*time6+AD44^2*time7+AE44^2*time8)/time)/(C44/D44),SQRT((((X44-Y44)*2/PI()+Y44)^2*time1+Y44^2*time2+((Z44-AA44)*2/PI()+AA44)^2*time3+AA44^2*time4+((AB44-AC44)*2/PI()+AC44)^2*time5+AC44^2*time6+((AD44-AE44)*2/PI()+AE44)^2*time7+AE44^2*time8)/time)/(C44/D44)))","v":8.6411091370738422},{"$f":"IF(move1,MAX(ABS(X44),ABS(Z44))/(C44/D44),MAX(ABS(X44),ABS(Z44),ABS(AB44),ABS(AD44))/(C44/D44))","v":24.585560210685337},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X44),ABS(Z44))/(C44/D44),MAX(ABS((X44-Y44)*2/PI()+Y44),ABS((Z44-Y44)*2/PI()+Y44))/(C44/D44)),IF(AccType=1,MAX(ABS(X44),ABS(Z44),ABS(AB44),ABS(AD44))/(C44/D44),MAX(ABS((X44-Y44)*2/PI()+Y44),ABS((Z44-Y44)*2/PI()+Y44),ABS((AB44-AC44)*2/PI()+AC44),ABS((AD44-AC44)*2/PI()+AC44))/(C44/D44)))","v":15.651653744855965},{"$f":"IF((C44+(E44-C44)/G44*mspeed)<0,\"NA\",U44*(C44+(E44-C44)/G44*mspeed)*mspeed/9.55)","v":209.38088708589663},{"$f":"IF(move1,IF(speed1>speed2,AM44/2*time1/time,AM44/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z44*-speed/30*PI(),((Z44-AA44)*2/PI()+AA44)*-speed/30*PI()),IF(AccType=1,X44*-speed/30*PI(),((X44-Y44)*2/PI()+Y44)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z44*-speed/30*PI(),((Z44-AA44)*2/PI()+AA44)*-speed/30*PI()),IF(AccType=1,X44*-speed/30*PI(),((X44-Y44)*2/PI()+Y44)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD44*-speed/30*PI(),((AD44-AE44)*2/PI()+AE44)*-speed/30*PI()),IF(AccType=1,AB44*-speed/30*PI(),((AB44-AC44)*2/PI()+AC44)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD44*-speed/30*PI(),((AD44-AE44)*2/PI()+AE44)*-speed/30*PI()),IF(AccType=1,AB44*-speed/30*PI(),((AB44-AC44)*2/PI()+AC44)*-speed/30*PI()),0)/2*time7/time)))","v":169.73296989364314},{"$f":"IF(move1,MAX(IF(AccType=1,Z44*-speed/30*PI(),((Z44-AA44)*2/PI()+AA44)*-speed/30*PI()),IF(AccType=1,X44*-speed/30*PI(),((X44-Y44)*2/PI()+Y44)*-speed/30*PI()),0),MAX(IF(AccType=1,Z44*-speed/30*PI(),((Z44-AA44)*2/PI()+AA44)*-speed/30*PI()),IF(AccType=1,X44*-speed/30*PI(),((X44-Y44)*2/PI()+Y44)*-speed/30*PI()),IF(AccType=1,AD44*-speed/30*PI(),((AD44-AE44)*2/PI()+AE44)*-speed/30*PI()),IF(AccType=1,AB44*-speed/30*PI(),((AB44-AC44)*2/PI()+AC44)*-speed/30*PI()),0))","v":1632.831170376847},{"$f":"(L44^2)/1000000+((K44/1000)^2*(D44/C44*H44)^2*PI()*PI()*(O44/2)^2)/1200","v":1.9953836719841093E-3},{"$f":"SQRT(3)*L44*J44*D44/C44*H44/1000","v":2.0997771519020754},{"$f":"0.75*J44^2*(D44/C44*H44)^2-(UAC_V*0.98)^2","v":-49817.076865150695},{"$f":"-AO44/2/AN44+SQRT((AO44/2/AN44)^2-AP44/AN44)","v":4498.0832303371017},{"$f":"(L44^2)/1000000+((K44/1000)^2*AV44^2*PI()*PI()*(O44/2)^2)/1200","v":1.1575081601272776E-3},{"$f":"SQRT(3)*L44*J44*AV44/1000","v":0.45849208523041141},{"$f":"0.75*J44^2*AV44^2-(UAC_V*0.98)^2","v":-50758.050254173038},{"$f":"-AS44/2/AR44+SQRT((AS44/2/AR44)^2-AT44/AR44)","v":6426.9288479748921},{"$f":"D44+(F44-D44)*((0.85*UAC_V-D44*J44)/L44*1000)/G44","v":4.3546510631883084},{"$f":"(L44^2)/1000000+((K44/1000)^2*AJ44^2*PI()*PI()*(O44/2)^2)/1200","v":1.6574693679135498E-3},{"$f":"SQRT(3)*L44*J44*AJ44/1000","v":1.6479298246067231},{"$f":"0.75*J44^2*AJ44^2-(UAC_V*0.98)^2","v":-50196.570433587542},{"$f":"IF(((AX44/2/AW44)^2-AY44/AW44)>0,-AX44/2/AW44+SQRT((AX44/2/AW44)^2-AY44/AW44),-9999)","v":5028.472488117086}]
["AKM","AKM41C",1.95,1.46,1.77,1.3208955223880596,3000,6.12,6000,21.7,66.099999999999994,86.3,8.1000000000000003E-2,640,10,1032.4414369397186,2111.4836164742701,2611.8192352259562,1.8233109830115437,30.864197530864196,2.2992964276435464,2.0554755529102042,3.1388351741372253,12.579510383810451,0,-10.189403410886465,0,0,0,0,0,0.27586088044532325,0.39243771710177899,3.3103305653438793,9.4185052104426958,5.9960066431149093,209.05689345017373,169.47032700019068,1630.3045457418343,2.6310255467470008E-2,14.862806492279299,-43390.007891529473,1032.4414369397186,9.1387474382425126E-3,4.4502009586644231,-50140.380431687619,2111.4836164742701,1.3719821656491586,3.9746434252859175E-2,19.448820239381796,-38108.048254486057,764.61485450878774]
["AKM","AKM41E",2.02,2.85,1.58,2.2253521126760565,6000,6.28,6000,5.7,18.399999999999999,45.6,8.1000000000000003E-2,640,10,2295.0156770095659,4292.0022627960634,4942.9824561403511,1.7052531673949554,30.864197530864196,2.2252573562018028,2.0031067490144028,1.2859177226322107,12.579510383810451,0,-10.189403410886465,0,0,0,0,0,0.51983481726396452,0.7395132960779659,6.2380178071675738,17.748319105871182,11.298930869086908,209.05689345017373,169.47032700019068,1630.3045457418343,7.5444890635392101E-3,3.9889028576125303,-48892.149986405748,2295.0156770095659,2.4940658440737538E-3,1.0988118299491019,-50659.996651946261,4292.0022627960634,2.4407483295239274,1.0966639874311851E-2,5.0867181816944749,-47694.262673421013,1866.3713531277238]
["AKM","AKM41H",2.06,5.6,1.62,4.378378378378379,6000,6.36,6000,1.51,5,23.7,8.1000000000000003E-2,640,10,4647.1284747299542,6000,6000,1.62,30.864197530864196,2.1813425482630717,1.9779104377060457,0.62099189477202144,12.579510383810451,0,-10.189403410886465,0,0,0,0,0,1.0015962277107759,1.4248636357066855,12.019154732529312,34.19672725696045,21.770312722042426,209.05689345017373,169.47032700019068,1630.3045457418343,2.0982671168294923E-3,1.0716768342488578,-50293.983355825432,4647.1284747299542,6.4365440526084855E-4,0.24751373759226925,-50777.892712752189,8691.8126091646554,3.9931294332306999,2.9979736564311292E-3,1.3494307060379067,-49994.675911624756,3864.7847422889281]
["AKM","AKM42C",3.35,1.4,3.1,1.2916666666666667,1500,11.3,6000,27.52,97.4,154,0.15,640,10,538.30447707947155,1186.9784841908117,1463.6363636363635,3.1521702526348649,16.666666666666668,1.3862263435775721,1.1429919293508963,3.2510332324013222,12.915808801665129,0,-10.461805129348754,0,0,0,0,0,0.15809312042286994,0.22490214331257685,1.8971174450744392,5.3976514395018445,3.436251630735212,214.64578366639302,174.00091691224537,1673.8888206958006,6.7217052626439441E-2,34.66501958360795,-38137.935523571403,538.30447707947155,2.7147744602019123E-2,9.7364143212810337,-49805.858222343079,1186.9784841908117,1.3263839826839827,4.674877895372663E-2,25.224045243154041,-44098.16410662968,738.22684310959175]
["AKM","AKM42E",3.42,2.74,2.81,2.2301587301587302,3500,11.3,6000,7.22,26.8,80.900000000000006,0.15,640,10,1370.8415473249308,2451.9625533895596,2786.1557478368354,2.9926579549806767,16.666666666666668,1.3586123584067182,1.1429919293508963,1.4061847150733997,12.915808801665129,0,-10.461805129348754,0,0,0,0,0,0.30307785137041005,0.43115638543570239,3.6369342164449208,10.347753250456858,6.5875843188217456,214.64578366639302,174.00091691224537,1673.8888206958006,1.8648948839048756E-2,9.1590250493864254,-47600.798839962968,1370.8415473249308,7.4122730212747099E-3,2.4519283987339273,-50575.514186274399,2451.9625533895596,2.4236027533782365,1.2953665360331688E-2,6.6645761347889287,-49108.526520326865,1706.7459020664476]
["AKM","AKM42G",3.53,4.8,2.35,3.1756756756756759,6000,11.5,6000,2.38,9.1999999999999993,47.5,0.15,640,10,2539.3646302181492,4359.9226776247651,4745.2631578947367,2.6725485400671296,16.666666666666668,1.3191734875890446,1.123113808840446,0.76674294759636263,12.915808801665129,0,-10.461805129348754,0,0,0,0,0,0.51439445091051172,0.73177386978272685,6.1727334109261411,17.562572874785445,11.180681145734969,214.64578366639302,174.00091691224537,1673.8888206958006,6.5118706479420224E-3,3.061932174934991,-49766.331341395889,2539.3646302181492,2.5011002572328813E-3,0.7344536525690033,-50745.390230717792,4359.9226776247651,3.7508802655286866,4.4318081067274279E-3,2.189270657653744,-50274.090081721479,3130.1233451493508]
["AKM","AKM42H",3.54,6,2.72,4.6101694915254239,4500,11.5,6000,1.65,6,38.299999999999997,0.15,640,10,3179.0677425599206,5452.6606508151544,5885.1174934725859,2.5464040591847943,16.666666666666668,1.3128698829896315,1.123113808840446,0.61355912730789208,12.915808801665129,0,-10.461805129348754,0,0,0,0,0,0.64117669905159125,0.91213338994810245,7.694120388619095,21.891201358754458,13.936371625863151,214.64578366639302,174.00091691224537,1673.8888206958006,4.2791318458289297E-3,2.133482939016313,-50029.411741597243,3179.0677425599206,1.6170059751487375E-3,0.4929198379510466,-50763.750970242203,5452.6606508151544,4.5033214831860668,2.904564090788599E-3,1.5254327431640295,-50408.582026546486,3911.6034513747009]
["AKM","AKM42J",3.56,8.4,2.38,5.5348837209302326,6000,11.6,6000,0.8,3.1,27.5,0.15,640,10,4521.7527780749042,6000,6000,2.38,16.666666666666668,1.3077724503464287,1.1134317932469939,0.43101990613657915,12.915808801665129,0,-10.461805129348754,0,0,0,0,0,0.89260441587069839,1.2698126630850548,10.711252990448381,30.475503914041315,19.401308364544317,214.64578366639302,174.00091691224537,1673.8888206958006,2.2365728753251215E-3,1.0429670435868681,-50445.563221815428,4521.7527780749042,8.0808871268602781E-4,0.1951728771798403,-50792.567453888711,7808.2839873245739,5.1219596899224804,1.5000290346674767E-3,0.73928914005543944,-50624.482832197056,5568.1883036731524]
["AKM","AKM43E",4.7,2.76,3.92,2.2790697674418605,2500,15.9,6000,8.0399999999999991,32.6,111,0.21,640,10,1009.9907746201579,1789.861349226228,2030.6306306306308,4.1415632590414173,11.904761904761905,1.018249019277645,0.83070705713806814,1.6277243226547118,13.208242208495284,0,-10.698676188881178,0,0,0,0,0,0.22717701248924174,0.32318039446318242,2.726124149870901,7.7563294671163785,4.9378326997635931,219.50568820223589,177.94056031403207,1711.7881902209886,3.1371676619625963E-2,14.432713922141241,-46578.570616866135,1009.9907746201579,1.3643016563204925E-2,3.8019924402514431,-50511.856970300119,1789.861349226228,2.4596402658286194,1.7649027416315011E-2,7.6326619207475774,-49623.082084318849,1474.4511503555818]
["AKM","AKM43G",4.8,4.87,3.01,3.0404040404040402,5000,16.100000000000001,6000,2.61,10.8,63.9,0.21,640,10,1958.3352880669909,3260.319829449963,3527.386541471049,3.6328055010569127,11.904761904761905,1.0008561413001364,0.82038771481337158,0.87664905154835027,13.208242208495284,0,-10.698676188881178,0,0,0,0,0,0.39250110498688523,0.55836926697371558,4.710013259842623,13.400862407369173,8.5312539753086423,219.50568820223589,177.94056031403207,1711.7881902209886,1.0482521026179489E-2,4.7186263950285383,-49441.928923478103,1958.3352880669909,4.4337807862303569E-3,1.1044265660464483,-50730.47868065878,3260.319829449963,3.8232689679581418,5.8287578608992568E-3,2.4644207904243345,-50433.309799283183,2737.697594905379]
["AKM","AKM43H",4.82,5.4,2.58,2.898876404494382,6000,16.100000000000001,6000,2.1,6.8,57.4,0.21,640,10,2510.875323227257,3713.569851850476,3926.8292682926831,3.4336005886424892,11.904761904761905,0.99804252902161839,0.82038771481337158,0.73528330000831621,13.208242208495284,0,-10.698676188881178,0,0,0,0,0,0.43341095202484792,0.61656732301067196,5.200931424298175,14.797615752256126,9.4204547717842324,219.50568820223589,177.94056031403207,1711.7881902209886,6.3880563466889549E-3,3.7658620941282166,-49729.078789836611,2510.875323227257,3.4516807996927351E-3,0.84819147692689634,-50750.571139086656,3713.569851850476,4.0625815291860787,4.1385222111194669E-3,1.9668157768155681,-50511.636017985329,3264.0480206375632]
["AKM","AKM43K",4.9000000000000004,9.6,2.62,5.0384615384615383,6000,16.399999999999999,6000,0.7,2.9,33.200000000000003,0.21,640,10,3960.9955573257148,6000,6000,2.62,11.904761904761905,0.98179204715735713,0.80538062246922471,0.43850516294735892,13.208242208495284,0,-10.698676188881178,0,0,0,0,0,0.7579286308425458,1.0782238537547169,9.0951435701105492,25.877372490113206,16.474046984126982,219.50568820223589,177.94056031403207,1711.7881902209886,2.8874631334773106E-3,1.293349061081283,-50425.761730612248,3960.9955573257148,1.1503949088765739E-3,0.21241724989995045,-50794.926047309331,6553.1908052344761,5.2770721346926166,1.5715449169002743E-3,0.66312751953591798,-50705.422622667058,5473.1396635530882]
["AKM","AKM43L",4.7300000000000004,11.2,2.5299999999999998,5.8837209302325579,6000,16,6000,0.56999999999999995,2,27.5,0.21,640,10,4845.4111021425615,6000,6000,2.5299999999999998,11.904761904761905,1.0170633833636205,0.82551513803095522,0.4,13.208242208495284,0,-10.698676188881178,0,0,0,0,0,0.91603072719870748,1.3031387661658489,10.992368726384489,31.275330387980372,19.910493712316967,219.50568820223589,177.94056031403207,1711.7881902209886,1.9367669538243369E-3,1.0285964981878799,-50455.404378153929,4845.4111021425615,7.7769866620069515E-4,0.13864655163204881,-50798.805333461336,7993.3939906716078,5.1067064693446085,1.0822987636257761E-3,0.54056784173432637,-50708.560465614115,6599.7220245770786]
["AKM","AKM44E",5.76,2.9,4.8,2.3529411764705883,2000,19.899999999999999,6000,8.08,33.9,132,0.27,640,10,{"$f":"IF(AQ58<I58,IF(AQ58<0,0,AQ58),I58)","v":854.86230369113048},{"$f":"IF(AU58<I58,IF(AU58<0,0,AU58),I58)","v":1512.8979062637211},{"$f":"IF(UAC_V*0.98/L58*1000<I58,IF(UAC_V*0.98/L58*1000<0,0,UAC_V*0.98/L58*1000),I58)","v":1707.5757575757575},{"$f":"C58+(E58-C58)/G58*Q58","v":5.0338090049934134},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M58,(inertia/gear^2+gear_inertia)/M58),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M58,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M58))","v":9.2592592592592595},{"$f":"IF((C58+(E58-C58)/G58*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X58^2*time1+Y58^2*time2+Z58^2*time3+AA58^2*time4)/time)/(C58+(E58-C58)/G58*mspeed),SQRT((((X58-Y58)*2/PI()+Y58)^2*time1+Y58^2*time2+((Z58-Y58)*2/PI()+Y58)^2*time3+AA58^2*time4)/time)/(C58+(E58-C58)/G58*mspeed)),IF(AccType=1,SQRT((X58^2*time1+Y58^2*time2+Z58^2*time3+AA58^2*time4+AB58^2*time5+AC58^2*time6+AD58^2*time7+AE58^2*time8)/time)/(C58+(E58-C58)/G58*mspeed),SQRT((((X58-Y58)*2/PI()+Y58)^2*time1+Y58^2*time2+((Z58-Y58)*2/PI()+Y58)^2*time3+AA58^2*time4+((AB58-AC58)*2/PI()+AC58)^2*time5+AC58^2*time6+((AD58-AC58)*2/PI()+AC58)^2*time7+AE58^2*time8)/time)/(C58+(E58-C58)/G58*mspeed))))","v":0.85601287399928039},{"$f":"IF(move1,MAX(ABS(X58),ABS(Z58))/H58,MAX(ABS(X58),ABS(Z58),ABS(AB58),ABS(AD58))/H58)","v":0.67842591031786126},{"$f":"IF(AZ58>0,speed/(MIN(AZ58,I58)),\"NA\")","v":1.7921494315212687},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M58+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M58+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":13.500675615325438},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M58+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M58+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.935547248413604},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M58+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M58+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M58+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M58+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH58/Irms","v":0.19908528104389711},{"$f":"AI58/Ipeak","v":0.2832172980645527},{"$f":"IF(move1,IF(AccType=1,SQRT((X58^2*time1+Y58^2*time2+Z58^2*time3+AA58^2*time4)/time)/(C58/D58),SQRT((((X58-Y58)*2/PI()+Y58)^2*time1+Y58^2*time2+((Z58-AA58)*2/PI()+AA58)^2*time3+AA58^2*time4)/time)/(C58/D58)),IF(AccType=1,SQRT((X58^2*time1+Y58^2*time2+Z58^2*time3+AA58^2*time4+AB58^2*time5+AC58^2*time6+AD58^2*time7+AE58^2*time8)/time)/(C58/D58),SQRT((((X58-Y58)*2/PI()+Y58)^2*time1+Y58^2*time2+((Z58-AA58)*2/PI()+AA58)^2*time3+AA58^2*time4+((AB58-AC58)*2/PI()+AC58)^2*time5+AC58^2*time6+((AD58-AE58)*2/PI()+AE58)^2*time7+AE58^2*time8)/time)/(C58/D58)))","v":2.3890233725267653},{"$f":"IF(move1,MAX(ABS(X58),ABS(Z58))/(C58/D58),MAX(ABS(X58),ABS(Z58),ABS(AB58),ABS(AD58))/(C58/D58))","v":6.7972151535492653},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X58),ABS(Z58))/(C58/D58),MAX(ABS((X58-Y58)*2/PI()+Y58),ABS((Z58-Y58)*2/PI()+Y58))/(C58/D58)),IF(AccType=1,MAX(ABS(X58),ABS(Z58),ABS(AB58),ABS(AD58))/(C58/D58),MAX(ABS((X58-Y58)*2/PI()+Y58),ABS((Z58-Y58)*2/PI()+Y58),ABS((AB58-AC58)*2/PI()+AC58),ABS((AD58-AC58)*2/PI()+AC58))/(C58/D58)))","v":4.327241563786008},{"$f":"IF((C58+(E58-C58)/G58*mspeed)<0,\"NA\",U58*(C58+(E58-C58)/G58*mspeed)*mspeed/9.55)","v":224.36559273807876},{"$f":"IF(move1,IF(speed1>speed2,AM58/2*time1/time,AM58/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z58*-speed/30*PI(),((Z58-AA58)*2/PI()+AA58)*-speed/30*PI()),IF(AccType=1,X58*-speed/30*PI(),((X58-Y58)*2/PI()+Y58)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z58*-speed/30*PI(),((Z58-AA58)*2/PI()+AA58)*-speed/30*PI()),IF(AccType=1,X58*-speed/30*PI(),((X58-Y58)*2/PI()+Y58)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD58*-speed/30*PI(),((AD58-AE58)*2/PI()+AE58)*-speed/30*PI()),IF(AccType=1,AB58*-speed/30*PI(),((AB58-AC58)*2/PI()+AC58)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD58*-speed/30*PI(),((AD58-AE58)*2/PI()+AE58)*-speed/30*PI()),IF(AccType=1,AB58*-speed/30*PI(),((AB58-AC58)*2/PI()+AC58)*-speed/30*PI()),0)/2*time7/time)))","v":181.88020371581882},{"$f":"IF(move1,MAX(IF(AccType=1,Z58*-speed/30*PI(),((Z58-AA58)*2/PI()+AA58)*-speed/30*PI()),IF(AccType=1,X58*-speed/30*PI(),((X58-Y58)*2/PI()+Y58)*-speed/30*PI()),0),MAX(IF(AccType=1,Z58*-speed/30*PI(),((Z58-AA58)*2/PI()+AA58)*-speed/30*PI()),IF(AccType=1,X58*-speed/30*PI(),((X58-Y58)*2/PI()+Y58)*-speed/30*PI()),IF(AccType=1,AD58*-speed/30*PI(),((AD58-AE58)*2/PI()+AE58)*-speed/30*PI()),IF(AccType=1,AB58*-speed/30*PI(),((AB58-AC58)*2/PI()+AC58)*-speed/30*PI()),0))","v":1749.6875597461769},{"$f":"(L58^2)/1000000+((K58/1000)^2*(D58/C58*H58)^2*PI()*PI()*(O58/2)^2)/1200","v":4.1144021928728083E-2},{"$f":"SQRT(3)*L58*J58*D58/C58*H58/1000","v":18.508640081405446},{"$f":"0.75*J58^2*(D58/C58*H58)^2-(UAC_V*0.98)^2","v":-45889.960309013317},{"$f":"-AO58/2/AN58+SQRT((AO58/2/AN58)^2-AP58/AN58)","v":854.86230369113048},{"$f":"(L58^2)/1000000+((K58/1000)^2*AV58^2*PI()*PI()*(O58/2)^2)/1200","v":1.895262716885707E-2},{"$f":"SQRT(3)*L58*J58*AV58/1000","v":4.6985922090475514},{"$f":"0.75*J58^2*AV58^2-(UAC_V*0.98)^2","v":-50488.401954388741},{"$f":"-AS58/2/AR58+SQRT((AS58/2/AR58)^2-AT58/AR58)","v":1512.8979062637211},{"$f":"D58+(F58-D58)*((0.85*UAC_V-D58*J58)/L58*1000)/G58","v":2.5434419786096258},{"$f":"(L58^2)/1000000+((K58/1000)^2*AJ58^2*PI()*PI()*(O58/2)^2)/1200","v":2.1848662852870768E-2},{"$f":"SQRT(3)*L58*J58*AJ58/1000","v":7.9938695945350995},{"$f":"0.75*J58^2*AJ58^2-(UAC_V*0.98)^2","v":-49888.293162671711},{"$f":"IF(((AX58/2/AW58)^2-AY58/AW58)>0,-AX58/2/AW58+SQRT((AX58/2/AW58)^2-AY58/AW58),-9999)","v":1339.1740430722657}]
["AKM","AKM44G",5.88,5,3.76,3.1596638655462184,4000,20.3,6000,2.65,11.5,76.599999999999994,0.27,640,10,{"$f":"IF(AQ59<I59,IF(AQ59<0,0,AQ59),I59)","v":1672.6271694944021},{"$f":"IF(AU59<I59,IF(AU59<0,0,AU59),I59)","v":2734.3412834880255},{"$f":"IF(UAC_V*0.98/L59*1000<I59,IF(UAC_V*0.98/L59*1000<0,0,UAC_V*0.98/L59*1000),I59)","v":2942.558746736293},{"$f":"C59+(E59-C59)/G59*Q59","v":4.4307991197513461},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M59,(inertia/gear^2+gear_inertia)/M59),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M59,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M59))","v":9.2592592592592595},{"$f":"IF((C59+(E59-C59)/G59*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X59^2*time1+Y59^2*time2+Z59^2*time3+AA59^2*time4)/time)/(C59+(E59-C59)/G59*mspeed),SQRT((((X59-Y59)*2/PI()+Y59)^2*time1+Y59^2*time2+((Z59-Y59)*2/PI()+Y59)^2*time3+AA59^2*time4)/time)/(C59+(E59-C59)/G59*mspeed)),IF(AccType=1,SQRT((X59^2*time1+Y59^2*time2+Z59^2*time3+AA59^2*time4+AB59^2*time5+AC59^2*time6+AD59^2*time7+AE59^2*time8)/time)/(C59+(E59-C59)/G59*mspeed),SQRT((((X59-Y59)*2/PI()+Y59)^2*time1+Y59^2*time2+((Z59-Y59)*2/PI()+Y59)^2*time3+AA59^2*time4+((AB59-AC59)*2/PI()+AC59)^2*time5+AC59^2*time6+((AD59-AC59)*2/PI()+AC59)^2*time7+AE59^2*time8)/time)/(C59+(E59-C59)/G59*mspeed))))","v":0.84122837764166758},{"$f":"IF(move1,MAX(ABS(X59),ABS(Z59))/H59,MAX(ABS(X59),ABS(Z59),ABS(AB59),ABS(AD59))/H59)","v":0.66505791208499687},{"$f":"IF(AZ59>0,speed/(MIN(AZ59,I59)),\"NA\")","v":0.97659095628395121},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M59+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M59+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":13.500675615325438},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M59+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M59+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.935547248413604},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M59+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M59+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M59+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M59+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH59/Irms","v":0.33624537262867915},{"$f":"AI59/Ipeak","v":0.47834026414843533},{"$f":"IF(move1,IF(AccType=1,SQRT((X59^2*time1+Y59^2*time2+Z59^2*time3+AA59^2*time4)/time)/(C59/D59),SQRT((((X59-Y59)*2/PI()+Y59)^2*time1+Y59^2*time2+((Z59-AA59)*2/PI()+AA59)^2*time3+AA59^2*time4)/time)/(C59/D59)),IF(AccType=1,SQRT((X59^2*time1+Y59^2*time2+Z59^2*time3+AA59^2*time4+AB59^2*time5+AC59^2*time6+AD59^2*time7+AE59^2*time8)/time)/(C59/D59),SQRT((((X59-Y59)*2/PI()+Y59)^2*time1+Y59^2*time2+((Z59-AA59)*2/PI()+AA59)^2*time3+AA59^2*time4+((AB59-AC59)*2/PI()+AC59)^2*time5+AC59^2*time6+((AD59-AE59)*2/PI()+AE59)^2*time7+AE59^2*time8)/time)/(C59/D59)))","v":4.0349444715441498},{"$f":"IF(move1,MAX(ABS(X59),ABS(Z59))/(C59/D59),MAX(ABS(X59),ABS(Z59),ABS(AB59),ABS(AD59))/(C59/D59))","v":11.480166339562448},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X59),ABS(Z59))/(C59/D59),MAX(ABS((X59-Y59)*2/PI()+Y59),ABS((Z59-Y59)*2/PI()+Y59))/(C59/D59)),IF(AccType=1,MAX(ABS(X59),ABS(Z59),ABS(AB59),ABS(AD59))/(C59/D59),MAX(ABS((X59-Y59)*2/PI()+Y59),ABS((Z59-Y59)*2/PI()+Y59),ABS((AB59-AC59)*2/PI()+AC59),ABS((AD59-AC59)*2/PI()+AC59))/(C59/D59)))","v":7.308500881834215},{"$f":"IF((C59+(E59-C59)/G59*mspeed)<0,\"NA\",U59*(C59+(E59-C59)/G59*mspeed)*mspeed/9.55)","v":224.36559273807876},{"$f":"IF(move1,IF(speed1>speed2,AM59/2*time1/time,AM59/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z59*-speed/30*PI(),((Z59-AA59)*2/PI()+AA59)*-speed/30*PI()),IF(AccType=1,X59*-speed/30*PI(),((X59-Y59)*2/PI()+Y59)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z59*-speed/30*PI(),((Z59-AA59)*2/PI()+AA59)*-speed/30*PI()),IF(AccType=1,X59*-speed/30*PI(),((X59-Y59)*2/PI()+Y59)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD59*-speed/30*PI(),((AD59-AE59)*2/PI()+AE59)*-speed/30*PI()),IF(AccType=1,AB59*-speed/30*PI(),((AB59-AC59)*2/PI()+AC59)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD59*-speed/30*PI(),((AD59-AE59)*2/PI()+AE59)*-speed/30*PI()),IF(AccType=1,AB59*-speed/30*PI(),((AB59-AC59)*2/PI()+AC59)*-speed/30*PI()),0)/2*time7/time)))","v":181.88020371581882},{"$f":"IF(move1,MAX(IF(AccType=1,Z59*-speed/30*PI(),((Z59-AA59)*2/PI()+AA59)*-speed/30*PI()),IF(AccType=1,X59*-speed/30*PI(),((X59-Y59)*2/PI()+Y59)*-speed/30*PI()),0),MAX(IF(AccType=1,Z59*-speed/30*PI(),((Z59-AA59)*2/PI()+AA59)*-speed/30*PI()),IF(AccType=1,X59*-speed/30*PI(),((X59-Y59)*2/PI()+Y59)*-speed/30*PI()),IF(AccType=1,AD59*-speed/30*PI(),((AD59-AE59)*2/PI()+AE59)*-speed/30*PI()),IF(AccType=1,AB59*-speed/30*PI(),((AB59-AC59)*2/PI()+AC59)*-speed/30*PI()),0))","v":1749.6875597461769},{"$f":"(L59^2)/1000000+((K59/1000)^2*(D59/C59*H59)^2*PI()*PI()*(O59/2)^2)/1200","v":1.3970294730039598E-2},{"$f":"SQRT(3)*L59*J59*D59/C59*H59/1000","v":6.0690957198951105},{"$f":"0.75*J59^2*(D59/C59*H59)^2-(UAC_V*0.98)^2","v":-49235.77158056973},{"$f":"-AO59/2/AN59+SQRT((AO59/2/AN59)^2-AP59/AN59)","v":1672.6271694944021},{"$f":"(L59^2)/1000000+((K59/1000)^2*AV59^2*PI()*PI()*(O59/2)^2)/1200","v":6.2822979234135783E-3},{"$f":"SQRT(3)*L59*J59*AV59/1000","v":1.3730775011652336},{"$f":"0.75*J59^2*AV59^2-(UAC_V*0.98)^2","v":-50724.830961003972},{"$f":"-AS59/2/AR59+SQRT((AS59/2/AR59)^2-AT59/AR59)","v":2734.3412834880255},{"$f":"D59+(F59-D59)*((0.85*UAC_V-D59*J59)/L59*1000)/G59","v":3.9053483665006472},{"$f":"(L59^2)/1000000+((K59/1000)^2*AJ59^2*PI()*PI()*(O59/2)^2)/1200","v":7.3200421239239151E-3},{"$f":"SQRT(3)*L59*J59*AJ59/1000","v":2.5695884685147119},{"$f":"0.75*J59^2*AJ59^2-(UAC_V*0.98)^2","v":-50523.834163641972},{"$f":"IF(((AX59/2/AW59)^2-AY59/AW59)>0,-AX59/2/AW59+SQRT((AX59/2/AW59)^2-AY59/AW59),-9999)","v":2457.528389503314}]
["AKM","AKM44H",5.89,5.6,3.19,3.0094339622641506,5000,20.2,6000,2.23,9.1,68,0.27,640,10,{"$f":"IF(AQ60<I60,IF(AQ60<0,0,AQ60),I60)","v":1910.3095646499903},{"$f":"IF(AU60<I60,IF(AU60<0,0,AU60),I60)","v":3099.501346770885},{"$f":"IF(UAC_V*0.98/L60*1000<I60,IF(UAC_V*0.98/L60*1000<0,0,UAC_V*0.98/L60*1000),I60)","v":3314.7058823529414},{"$f":"C60+(E60-C60)/G60*Q60","v":4.2162692727437223},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M60,(inertia/gear^2+gear_inertia)/M60),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M60,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M60))","v":9.2592592592592595},{"$f":"IF((C60+(E60-C60)/G60*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X60^2*time1+Y60^2*time2+Z60^2*time3+AA60^2*time4)/time)/(C60+(E60-C60)/G60*mspeed),SQRT((((X60-Y60)*2/PI()+Y60)^2*time1+Y60^2*time2+((Z60-Y60)*2/PI()+Y60)^2*time3+AA60^2*time4)/time)/(C60+(E60-C60)/G60*mspeed)),IF(AccType=1,SQRT((X60^2*time1+Y60^2*time2+Z60^2*time3+AA60^2*time4+AB60^2*time5+AC60^2*time6+AD60^2*time7+AE60^2*time8)/time)/(C60+(E60-C60)/G60*mspeed),SQRT((((X60-Y60)*2/PI()+Y60)^2*time1+Y60^2*time2+((Z60-Y60)*2/PI()+Y60)^2*time3+AA60^2*time4+((AB60-AC60)*2/PI()+AC60)^2*time5+AC60^2*time6+((AD60-AC60)*2/PI()+AC60)^2*time7+AE60^2*time8)/time)/(C60+(E60-C60)/G60*mspeed))))","v":0.84041124868299588},{"$f":"IF(move1,MAX(ABS(X60),ABS(Z60))/H60,MAX(ABS(X60),ABS(Z60),ABS(AB60),ABS(AD60))/H60)","v":0.66835027798640789},{"$f":"IF(AZ60>0,speed/(MIN(AZ60,I60)),\"NA\")","v":0.86270811607252174},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M60+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M60+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":13.500675615325438},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M60+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M60+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.935547248413604},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M60+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M60+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M60+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M60+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH60/Irms","v":0.37595543734862974},{"$f":"AI60/Ipeak","v":0.53483151843394483},{"$f":"IF(move1,IF(AccType=1,SQRT((X60^2*time1+Y60^2*time2+Z60^2*time3+AA60^2*time4)/time)/(C60/D60),SQRT((((X60-Y60)*2/PI()+Y60)^2*time1+Y60^2*time2+((Z60-AA60)*2/PI()+AA60)^2*time3+AA60^2*time4)/time)/(C60/D60)),IF(AccType=1,SQRT((X60^2*time1+Y60^2*time2+Z60^2*time3+AA60^2*time4+AB60^2*time5+AC60^2*time6+AD60^2*time7+AE60^2*time8)/time)/(C60/D60),SQRT((((X60-Y60)*2/PI()+Y60)^2*time1+Y60^2*time2+((Z60-AA60)*2/PI()+AA60)^2*time3+AA60^2*time4+((AB60-AC60)*2/PI()+AC60)^2*time5+AC60^2*time6+((AD60-AE60)*2/PI()+AE60)^2*time7+AE60^2*time8)/time)/(C60/D60)))","v":4.5114652481835567},{"$f":"IF(move1,MAX(ABS(X60),ABS(Z60))/(C60/D60),MAX(ABS(X60),ABS(Z60),ABS(AB60),ABS(AD60))/(C60/D60))","v":12.835956442414677},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X60),ABS(Z60))/(C60/D60),MAX(ABS((X60-Y60)*2/PI()+Y60),ABS((Z60-Y60)*2/PI()+Y60))/(C60/D60)),IF(AccType=1,MAX(ABS(X60),ABS(Z60),ABS(AB60),ABS(AD60))/(C60/D60),MAX(ABS((X60-Y60)*2/PI()+Y60),ABS((Z60-Y60)*2/PI()+Y60),ABS((AB60-AC60)*2/PI()+AC60),ABS((AD60-AC60)*2/PI()+AC60))/(C60/D60)))","v":8.1716236684902217},{"$f":"IF((C60+(E60-C60)/G60*mspeed)<0,\"NA\",U60*(C60+(E60-C60)/G60*mspeed)*mspeed/9.55)","v":224.36559273807876},{"$f":"IF(move1,IF(speed1>speed2,AM60/2*time1/time,AM60/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z60*-speed/30*PI(),((Z60-AA60)*2/PI()+AA60)*-speed/30*PI()),IF(AccType=1,X60*-speed/30*PI(),((X60-Y60)*2/PI()+Y60)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z60*-speed/30*PI(),((Z60-AA60)*2/PI()+AA60)*-speed/30*PI()),IF(AccType=1,X60*-speed/30*PI(),((X60-Y60)*2/PI()+Y60)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD60*-speed/30*PI(),((AD60-AE60)*2/PI()+AE60)*-speed/30*PI()),IF(AccType=1,AB60*-speed/30*PI(),((AB60-AC60)*2/PI()+AC60)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD60*-speed/30*PI(),((AD60-AE60)*2/PI()+AE60)*-speed/30*PI()),IF(AccType=1,AB60*-speed/30*PI(),((AB60-AC60)*2/PI()+AC60)*-speed/30*PI()),0)/2*time7/time)))","v":181.88020371581882},{"$f":"IF(move1,MAX(IF(AccType=1,Z60*-speed/30*PI(),((Z60-AA60)*2/PI()+AA60)*-speed/30*PI()),IF(AccType=1,X60*-speed/30*PI(),((X60-Y60)*2/PI()+Y60)*-speed/30*PI()),0),MAX(IF(AccType=1,Z60*-speed/30*PI(),((Z60-AA60)*2/PI()+AA60)*-speed/30*PI()),IF(AccType=1,X60*-speed/30*PI(),((X60-Y60)*2/PI()+Y60)*-speed/30*PI()),IF(AccType=1,AD60*-speed/30*PI(),((AD60-AE60)*2/PI()+AE60)*-speed/30*PI()),IF(AccType=1,AB60*-speed/30*PI(),((AB60-AC60)*2/PI()+AC60)*-speed/30*PI()),0))","v":1749.6875597461769},{"$f":"(L60^2)/1000000+((K60/1000)^2*(D60/C60*H60)^2*PI()*PI()*(O60/2)^2)/1200","v":1.0904431685355397E-2},{"$f":"SQRT(3)*L60*J60*D60/C60*H60/1000","v":5.0442720927141425},{"$f":"0.75*J60^2*(D60/C60*H60)^2-(UAC_V*0.98)^2","v":-49429.474395256562},{"$f":"-AO60/2/AN60+SQRT((AO60/2/AN60)^2-AP60/AN60)","v":1910.3095646499903},{"$f":"(L60^2)/1000000+((K60/1000)^2*AV60^2*PI()*PI()*(O60/2)^2)/1200","v":4.9251563002120904E-3},{"$f":"SQRT(3)*L60*J60*AV60/1000","v":1.1045865057234143},{"$f":"0.75*J60^2*AV60^2-(UAC_V*0.98)^2","v":-50739.193772241233},{"$f":"-AS60/2/AR60+SQRT((AS60/2/AR60)^2-AT60/AR60)","v":3099.501346770885},{"$f":"D60+(F60-D60)*((0.85*UAC_V-D60*J60)/L60*1000)/G60","v":4.2055744950055489},{"$f":"(L60^2)/1000000+((K60/1000)^2*AJ60^2*PI()*PI()*(O60/2)^2)/1200","v":5.7609935682433038E-3},{"$f":"SQRT(3)*L60*J60*AJ60/1000","v":2.1462621206172341},{"$f":"0.75*J60^2*AJ60^2-(UAC_V*0.98)^2","v":-50556.109335510577},{"$f":"IF(((AX60/2/AW60)^2-AY60/AW60)>0,-AX60/2/AW60+SQRT((AX60/2/AW60)^2-AY60/AW60),-9999)","v":2781.9374308497281}]
["AKM","AKM44J",6,8.8000000000000007,2.75,3.985507246376812,6000,20.399999999999999,6000,0.88,3.8,44.2,0.27,640,10,{"$f":"IF(AQ61<I61,IF(AQ61<0,0,AQ61),I61)","v":3090.8076710665005},{"$f":"IF(AU61<I61,IF(AU61<0,0,AU61),I61)","v":4901.4451647222759},{"$f":"IF(UAC_V*0.98/L61*1000<I61,IF(UAC_V*0.98/L61*1000<0,0,UAC_V*0.98/L61*1000),I61)","v":5099.5475113122166},{"$f":"C61+(E61-C61)/G61*Q61","v":3.3450505357754339},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M61,(inertia/gear^2+gear_inertia)/M61),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M61,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M61))","v":9.2592592592592595},{"$f":"IF((C61+(E61-C61)/G61*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X61^2*time1+Y61^2*time2+Z61^2*time3+AA61^2*time4)/time)/(C61+(E61-C61)/G61*mspeed),SQRT((((X61-Y61)*2/PI()+Y61)^2*time1+Y61^2*time2+((Z61-Y61)*2/PI()+Y61)^2*time3+AA61^2*time4)/time)/(C61+(E61-C61)/G61*mspeed)),IF(AccType=1,SQRT((X61^2*time1+Y61^2*time2+Z61^2*time3+AA61^2*time4+AB61^2*time5+AC61^2*time6+AD61^2*time7+AE61^2*time8)/time)/(C61+(E61-C61)/G61*mspeed),SQRT((((X61-Y61)*2/PI()+Y61)^2*time1+Y61^2*time2+((Z61-Y61)*2/PI()+Y61)^2*time3+AA61^2*time4+((AB61-AC61)*2/PI()+AC61)^2*time5+AC61^2*time6+((AD61-AC61)*2/PI()+AC61)^2*time7+AE61^2*time8)/time)/(C61+(E61-C61)/G61*mspeed))))","v":0.82445881120370512},{"$f":"IF(move1,MAX(ABS(X61),ABS(Z61))/H61,MAX(ABS(X61),ABS(Z61),ABS(AB61),ABS(AD61))/H61)","v":0.66179782428065881},{"$f":"IF(AZ61>0,speed/(MIN(AZ61,I61)),\"NA\")","v":0.54534489205236303},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M61+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M61+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":13.500675615325438},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M61+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M61+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.935547248413604},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M61+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M61+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M61+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M61+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH61/Irms","v":0.57995601870994584},{"$f":"AI61/Ipeak","v":0.82504128760322126},{"$f":"IF(move1,IF(AccType=1,SQRT((X61^2*time1+Y61^2*time2+Z61^2*time3+AA61^2*time4)/time)/(C61/D61),SQRT((((X61-Y61)*2/PI()+Y61)^2*time1+Y61^2*time2+((Z61-AA61)*2/PI()+AA61)^2*time3+AA61^2*time4)/time)/(C61/D61)),IF(AccType=1,SQRT((X61^2*time1+Y61^2*time2+Z61^2*time3+AA61^2*time4+AB61^2*time5+AC61^2*time6+AD61^2*time7+AE61^2*time8)/time)/(C61/D61),SQRT((((X61-Y61)*2/PI()+Y61)^2*time1+Y61^2*time2+((Z61-AA61)*2/PI()+AA61)^2*time3+AA61^2*time4+((AB61-AC61)*2/PI()+AC61)^2*time5+AC61^2*time6+((AD61-AE61)*2/PI()+AE61)^2*time7+AE61^2*time8)/time)/(C61/D61)))","v":6.9594722245193497},{"$f":"IF(move1,MAX(ABS(X61),ABS(Z61))/(C61/D61),MAX(ABS(X61),ABS(Z61),ABS(AB61),ABS(AD61))/(C61/D61))","v":19.800990902477309},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X61),ABS(Z61))/(C61/D61),MAX(ABS((X61-Y61)*2/PI()+Y61),ABS((Z61-Y61)*2/PI()+Y61))/(C61/D61)),IF(AccType=1,MAX(ABS(X61),ABS(Z61),ABS(AB61),ABS(AD61))/(C61/D61),MAX(ABS((X61-Y61)*2/PI()+Y61),ABS((Z61-Y61)*2/PI()+Y61),ABS((AB61-AC61)*2/PI()+AC61),ABS((AD61-AC61)*2/PI()+AC61))/(C61/D61)))","v":12.605702320987655},{"$f":"IF((C61+(E61-C61)/G61*mspeed)<0,\"NA\",U61*(C61+(E61-C61)/G61*mspeed)*mspeed/9.55)","v":224.36559273807876},{"$f":"IF(move1,IF(speed1>speed2,AM61/2*time1/time,AM61/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z61*-speed/30*PI(),((Z61-AA61)*2/PI()+AA61)*-speed/30*PI()),IF(AccType=1,X61*-speed/30*PI(),((X61-Y61)*2/PI()+Y61)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z61*-speed/30*PI(),((Z61-AA61)*2/PI()+AA61)*-speed/30*PI()),IF(AccType=1,X61*-speed/30*PI(),((X61-Y61)*2/PI()+Y61)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD61*-speed/30*PI(),((AD61-AE61)*2/PI()+AE61)*-speed/30*PI()),IF(AccType=1,AB61*-speed/30*PI(),((AB61-AC61)*2/PI()+AC61)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD61*-speed/30*PI(),((AD61-AE61)*2/PI()+AE61)*-speed/30*PI()),IF(AccType=1,AB61*-speed/30*PI(),((AB61-AC61)*2/PI()+AC61)*-speed/30*PI()),0)/2*time7/time)))","v":181.88020371581882},{"$f":"IF(move1,MAX(IF(AccType=1,Z61*-speed/30*PI(),((Z61-AA61)*2/PI()+AA61)*-speed/30*PI()),IF(AccType=1,X61*-speed/30*PI(),((X61-Y61)*2/PI()+Y61)*-speed/30*PI()),0),MAX(IF(AccType=1,Z61*-speed/30*PI(),((Z61-AA61)*2/PI()+AA61)*-speed/30*PI()),IF(AccType=1,X61*-speed/30*PI(),((X61-Y61)*2/PI()+Y61)*-speed/30*PI()),IF(AccType=1,AD61*-speed/30*PI(),((AD61-AE61)*2/PI()+AE61)*-speed/30*PI()),IF(AccType=1,AB61*-speed/30*PI(),((AB61-AC61)*2/PI()+AC61)*-speed/30*PI()),0))","v":1749.6875597461769},{"$f":"(L61^2)/1000000+((K61/1000)^2*(D61/C61*H61)^2*PI()*PI()*(O61/2)^2)/1200","v":4.6116026851181118E-3},{"$f":"SQRT(3)*L61*J61*D61/C61*H61/1000","v":2.015705858479075},{"$f":"0.75*J61^2*(D61/C61*H61)^2-(UAC_V*0.98)^2","v":-50285.224122880005},{"$f":"-AO61/2/AN61+SQRT((AO61/2/AN61)^2-AP61/AN61)","v":3090.8076710665005},{"$f":"(L61^2)/1000000+((K61/1000)^2*AV61^2*PI()*PI()*(O61/2)^2)/1200","v":2.0399448857522742E-3},{"$f":"SQRT(3)*L61*J61*AV61/1000","v":0.36322054792685482},{"$f":"0.75*J61^2*AV61^2-(UAC_V*0.98)^2","v":-50788.277518268944},{"$f":"-AS61/2/AR61+SQRT((AS61/2/AR61)^2-AT61/AR61)","v":4901.4451647222759},{"$f":"D61+(F61-D61)*((0.85*UAC_V-D61*J61)/L61*1000)/G61","v":5.3914407939318441},{"$f":"(L61^2)/1000000+((K61/1000)^2*AJ61^2*PI()*PI()*(O61/2)^2)/1200","v":2.4254420196663873E-3},{"$f":"SQRT(3)*L61*J61*AJ61/1000","v":0.8492442519604978},{"$f":"0.75*J61^2*AJ61^2-(UAC_V*0.98)^2","v":-50712.868713032098},{"$f":"IF(((AX61/2/AW61)^2-AY61/AW61)>0,-AX61/2/AW61+SQRT((AX61/2/AW61)^2-AY61/AW61),-9999)","v":4400.8847152996832}]
["AKM","AKM44K",5.88,10.1,3.18,5.389830508474577,5000,20.100000000000001,6000,0.68,2.8,37.799999999999997,0.27,640,10,{"$f":"IF(AQ62<I62,IF(AQ62<0,0,AQ62),I62)","v":3655.5974674546278},{"$f":"IF(AU62<I62,IF(AU62<0,0,AU62),I62)","v":5785.8132847979941},{"$f":"IF(UAC_V*0.98/L62*1000<I62,IF(UAC_V*0.98/L62*1000<0,0,UAC_V*0.98/L62*1000),I62)","v":5962.9629629629635},{"$f":"C62+(E62-C62)/G62*Q62","v":2.7556608262090836},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M62,(inertia/gear^2+gear_inertia)/M62),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M62,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M62))","v":9.2592592592592595},{"$f":"IF((C62+(E62-C62)/G62*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X62^2*time1+Y62^2*time2+Z62^2*time3+AA62^2*time4)/time)/(C62+(E62-C62)/G62*mspeed),SQRT((((X62-Y62)*2/PI()+Y62)^2*time1+Y62^2*time2+((Z62-Y62)*2/PI()+Y62)^2*time3+AA62^2*time4)/time)/(C62+(E62-C62)/G62*mspeed)),IF(AccType=1,SQRT((X62^2*time1+Y62^2*time2+Z62^2*time3+AA62^2*time4+AB62^2*time5+AC62^2*time6+AD62^2*time7+AE62^2*time8)/time)/(C62+(E62-C62)/G62*mspeed),SQRT((((X62-Y62)*2/PI()+Y62)^2*time1+Y62^2*time2+((Z62-Y62)*2/PI()+Y62)^2*time3+AA62^2*time4+((AB62-AC62)*2/PI()+AC62)^2*time5+AC62^2*time6+((AD62-AC62)*2/PI()+AC62)^2*time7+AE62^2*time8)/time)/(C62+(E62-C62)/G62*mspeed))))","v":0.84190235529864255},{"$f":"IF(move1,MAX(ABS(X62),ABS(Z62))/H62,MAX(ABS(X62),ABS(Z62),ABS(AB62),ABS(AD62))/H62)","v":0.67167540374753421},{"$f":"IF(AZ62>0,speed/(MIN(AZ62,I62)),\"NA\")","v":0.46540271800106253},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M62+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M62+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":13.500675615325438},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M62+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M62+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.935547248413604},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M62+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M62+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M62+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M62+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH62/Irms","v":0.67921565270993189},{"$f":"AI62/Ipeak","v":0.96624733357983938},{"$f":"IF(move1,IF(AccType=1,SQRT((X62^2*time1+Y62^2*time2+Z62^2*time3+AA62^2*time4)/time)/(C62/D62),SQRT((((X62-Y62)*2/PI()+Y62)^2*time1+Y62^2*time2+((Z62-AA62)*2/PI()+AA62)^2*time3+AA62^2*time4)/time)/(C62/D62)),IF(AccType=1,SQRT((X62^2*time1+Y62^2*time2+Z62^2*time3+AA62^2*time4+AB62^2*time5+AC62^2*time6+AD62^2*time7+AE62^2*time8)/time)/(C62/D62),SQRT((((X62-Y62)*2/PI()+Y62)^2*time1+Y62^2*time2+((Z62-AA62)*2/PI()+AA62)^2*time3+AA62^2*time4+((AB62-AC62)*2/PI()+AC62)^2*time5+AC62^2*time6+((AD62-AE62)*2/PI()+AE62)^2*time7+AE62^2*time8)/time)/(C62/D62)))","v":8.1505878325191823},{"$f":"IF(move1,MAX(ABS(X62),ABS(Z62))/(C62/D62),MAX(ABS(X62),ABS(Z62),ABS(AB62),ABS(AD62))/(C62/D62))","v":23.189936005916145},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X62),ABS(Z62))/(C62/D62),MAX(ABS((X62-Y62)*2/PI()+Y62),ABS((Z62-Y62)*2/PI()+Y62))/(C62/D62)),IF(AccType=1,MAX(ABS(X62),ABS(Z62),ABS(AB62),ABS(AD62))/(C62/D62),MAX(ABS((X62-Y62)*2/PI()+Y62),ABS((Z62-Y62)*2/PI()+Y62),ABS((AB62-AC62)*2/PI()+AC62),ABS((AD62-AC62)*2/PI()+AC62))/(C62/D62)))","v":14.763171781305115},{"$f":"IF((C62+(E62-C62)/G62*mspeed)<0,\"NA\",U62*(C62+(E62-C62)/G62*mspeed)*mspeed/9.55)","v":224.36559273807876},{"$f":"IF(move1,IF(speed1>speed2,AM62/2*time1/time,AM62/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z62*-speed/30*PI(),((Z62-AA62)*2/PI()+AA62)*-speed/30*PI()),IF(AccType=1,X62*-speed/30*PI(),((X62-Y62)*2/PI()+Y62)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z62*-speed/30*PI(),((Z62-AA62)*2/PI()+AA62)*-speed/30*PI()),IF(AccType=1,X62*-speed/30*PI(),((X62-Y62)*2/PI()+Y62)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD62*-speed/30*PI(),((AD62-AE62)*2/PI()+AE62)*-speed/30*PI()),IF(AccType=1,AB62*-speed/30*PI(),((AB62-AC62)*2/PI()+AC62)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD62*-speed/30*PI(),((AD62-AE62)*2/PI()+AE62)*-speed/30*PI()),IF(AccType=1,AB62*-speed/30*PI(),((AB62-AC62)*2/PI()+AC62)*-speed/30*PI()),0)/2*time7/time)))","v":181.88020371581882},{"$f":"IF(move1,MAX(IF(AccType=1,Z62*-speed/30*PI(),((Z62-AA62)*2/PI()+AA62)*-speed/30*PI()),IF(AccType=1,X62*-speed/30*PI(),((X62-Y62)*2/PI()+Y62)*-speed/30*PI()),0),MAX(IF(AccType=1,Z62*-speed/30*PI(),((Z62-AA62)*2/PI()+AA62)*-speed/30*PI()),IF(AccType=1,X62*-speed/30*PI(),((X62-Y62)*2/PI()+Y62)*-speed/30*PI()),IF(AccType=1,AD62*-speed/30*PI(),((AD62-AE62)*2/PI()+AE62)*-speed/30*PI()),IF(AccType=1,AB62*-speed/30*PI(),((AB62-AC62)*2/PI()+AC62)*-speed/30*PI()),0))","v":1749.6875597461769},{"$f":"(L62^2)/1000000+((K62/1000)^2*(D62/C62*H62)^2*PI()*PI()*(O62/2)^2)/1200","v":3.3504036779351863E-3},{"$f":"SQRT(3)*L62*J62*D62/C62*H62/1000","v":1.5370976020004949},{"$f":"0.75*J62^2*(D62/C62*H62)^2-(UAC_V*0.98)^2","v":-50391.770635537279},{"$f":"-AO62/2/AN62+SQRT((AO62/2/AN62)^2-AP62/AN62)","v":3655.5974674546278},{"$f":"(L62^2)/1000000+((K62/1000)^2*AV62^2*PI()*PI()*(O62/2)^2)/1200","v":1.4758295718816613E-3},{"$f":"SQRT(3)*L62*J62*AV62/1000","v":0.24036697540182936},{"$f":"0.75*J62^2*AV62^2-(UAC_V*0.98)^2","v":-50795.051050981252},{"$f":"-AS62/2/AR62+SQRT((AS62/2/AR62)^2-AT62/AR62)","v":5785.8132847979941},{"$f":"D62+(F62-D62)*((0.85*UAC_V-D62*J62)/L62*1000)/G62","v":5.3990016321406147},{"$f":"(L62^2)/1000000+((K62/1000)^2*AJ62^2*PI()*PI()*(O62/2)^2)/1200","v":1.7801851128795439E-3},{"$f":"SQRT(3)*L62*J62*AJ62/1000","v":0.65726576693087513},{"$f":"0.75*J62^2*AJ62^2-(UAC_V*0.98)^2","v":-50729.574509605831},{"$f":"IF(((AX62/2/AW62)^2-AY62/AW62)>0,-AX62/2/AW62+SQRT((AX62/2/AW62)^2-AY62/AW62),-9999)","v":5156.8242022912309}]
["AKM","AKM51E",4.7,2.75,3.98,2.3139534883720931,2500,11.6,6000,8.4700000000000006,36.6,110,0.34,640,10,1192.709698280619,1773.7411282548685,2049.0909090909095,4.1891625550625982,7.3529411764705879,1.0645643481827947,1.1932627520080992,1.7209866604979536,13.841847923293949,0,-11.211896817868098,0,0,0,0,0,0.23721221289119451,0.33745639883916984,2.846546554694334,8.0989535721400756,5.155953979511426,230.0354813632288,186.47645435123661,1793.903490858896,2.4788384450708075E-2,10.952910728391561,-48326.518400328205,1192.709698280619,1.3789868665630164E-2,3.9971722160640297,-50475.048724692686,1773.7411282548685,2.4769437103594081,1.9422152055815656E-2,8.3204296924524819,-49374.797391176762,1394.5488684413042]
["AKM","AKM51G",4.75,4.84,2.62,2.6464646464646466,5000,11.7,6000,2.75,12.1,63.6,0.34,640,10,2243.538557205808,3263.2491385615231,3544.0251572327047,3.3598558669727909,7.3529411764705879,1.067440904969311,1.183063925067859,0.92774859781184493,13.841847923293949,0,-11.211896817868098,0,0,0,0,0,0.4130988263233602,0.58767143814686584,4.9571859158803226,14.104114515524781,8.9789581723196878,230.0354813632288,186.47645435123661,1793.903490858896,8.3235874802755263E-3,3.6115035874976238,-49999.035949174518,2243.538557205808,4.4314945023393526E-3,1.0855002935156299,-50732.334132301527,3263.2491385615231,3.5832697922622452,6.4720235361630735E-3,2.7200468556860105,-50347.883852823805,2586.907709330475]
["AKM","AKM51H",4.79,6,1.95,1.9696969696969697,6000,11.7,6000,1.97,7.9,51.3,0.34,640,10,2822.9967621970641,4148.9784779249021,4393.7621832358682,2.8261501871155463,7.3529411764705879,1.0630962317183934,1.183063925067859,0.73955602346108584,13.841847923293949,0,-11.211896817868098,0,0,0,0,0,0.50782952389688252,0.72243465152891184,6.0939542867625907,17.338431636693883,11.037988401762931,230.0354813632288,186.47645435123661,1793.903490858896,5.3879227452663728E-3,2.5653452241739085,-50179.991750776891,2822.9967621970641,2.7975299806122398E-3,0.62926342895959653,-50767.544203399149,4148.9784779249021,3.5949120838009723,4.195170818101948E-3,1.9321202490063853,-50450.531542941942,3245.1902545098856]
["AKM","AKM51I",4.83,7.5,1.97,3.078125,6000,11.8,6000,1.3,5.15,41.4,0.34,640,10,3536.6531226206221,5190.188337850348,5444.4444444444443,2.3560102256246673,7.3529411764705879,1.0542282281311948,1.1730379596011822,0.5892431521224768,13.841847923293949,0,-11.211896817868098,0,0,0,0,0,0.62952987046223274,0.89556469483009504,7.5543584455467929,21.493552675922281,13.683220611916262,230.0354813632288,186.47645435123661,1793.903490858896,3.5448626193285088E-3,1.7080495320925659,-50379.620138497747,3536.6531226206221,1.8098564090257892E-3,0.39090300597927219,-50782.871679373558,5190.188337850348,4.1933845360305959,2.7350161469928626E-3,1.2755357927987019,-50567.845307896539,4073.0214536309954]
["AKM","AKM51K",4.9000000000000004,9.4,2.35,4.5192307692307692,5500,11.9,6000,0.75,3.4,33.5,0.34,640,10,4423.1715618371472,6000,6000,2.1181818181818186,7.3529411764705879,1.0371732006452496,1.163180497755794,0.47022260188431131,13.841847923293949,0,-11.211896817868098,0,0,0,0,0,0.77773918853676971,1.1064062115558089,9.3328702624412365,26.553749077339411,16.90464169312169,230.0354813632288,186.47645435123661,1793.903490858896,2.3609718892966636E-3,0.99344867015983618,-50585.302512755108,4423.1715618371472,1.1684342832021012E-3,0.19182518712951085,-50796.962873152763,6511.935415331126,4.407973071704415,1.8014978650933524E-3,0.73565241969287765,-50684.602084517719,5103.9656332608001]
["AKM","AKM51L",4.8899999999999997,11.9,2,4.8780487804878048,6000,12,6000,0.56000000000000005,2.1,26.6,0.34,640,10,5596.89772905264,6000,6000,2,7.3529411764705879,1.041200197166575,1.1534873269411625,0.4,13.841847923293949,0,-11.211896817868098,0,0,0,0,0,0.98659818308269254,1.40352752460121,11.839178196992311,33.68466059042904,21.444320957358176,230.0354813632288,186.47645435123661,1793.903490858896,1.4808382485152808E-3,0.75344167624931879,-50604.585363393431,5596.89772905264,7.1925791793486413E-4,9.266933092378804E-2,-50802.125767958249,8340.070100531173,3.5917469894247809,1.1245462119664584E-3,0.55327696552245276,-50697.001186409027,6472.8317740128177]
["AKM","AKM52E",8.34,2.99,7.61,2.7275985663082438,1500,21.3,6000,8.59,44.7,179,0.62,640,10,757.88256120530764,1092.4243829215579,1259.217877094972,7.8083534669781756,4.032258064516129,0.65818924492699482,0.71392193216751176,2.2944814378265841,15.206537155168002,0,-12.317295095686081,0,0,0,0,0,0.15967745451184864,0.22715600566522945,1.9161294541421836,5.451744135965507,3.4706881108446574,252.7150358638288,204.8614568929078,1970.7672153097728,5.599858493683528E-2,20.337218904969554,-47578.025447484077,757.88256120530764,3.5317541050903803E-2,7.5210391918411208,-50363.803374697971,1092.4243829215579,2.8240412081055646,3.6989855013007639E-2,9.2432012781535633,-50138.539343119293,1045.9879781260584]
["AKM","AKM52G",8.43,4.72,7.06,3.94413407821229,2500,21.5,6000,3.47,18.5,115,0.62,640,10,1286.8744009714328,1771.2963082089582,1960,7.4593296231014907,4.032258064516129,0.65317759379726126,0.70728079791479082,1.412128821852398,15.206537155168002,0,-12.317295095686081,0,0,0,0,0,0.24937498507750303,0.3547590716310447,2.9924998209300364,8.5142177191450727,5.4203193462501646,252.7150358638288,204.8614568929078,1970.7672153097728,2.3422829172479037E-2,8.3203352657985032,-49496.502553208127,1286.8744009714328,1.4488104080768636E-2,2.9282390585908917,-50643.06956551499,1771.2963082089582,4.2366109728831667,1.5292529494003466E-2,3.7463885453056163,-50539.840016400813,1699.5616567415821]
["AKM","AKM52H",8.48,5.9,6.26,4.3472222222222223,3500,21.6,6000,2.35,11.9,92.7,0.62,640,10,1635.8531987776055,2231.5911371985717,2431.4994606256741,7.0645336215483345,4.032258064516129,0.65229775306196003,0.70400634977629639,1.1241215403882461,15.206537155168002,0,-12.317295095686081,0,0,0,0,0,0.30988076712903162,0.4408341647773743,3.7185692055483797,10.580019954656983,6.7354498951781965,252.7150358638288,204.8614568929078,1970.7672153097728,1.5169448193407913E-2,5.6704579511558819,-49869.718121050646,1635.8531987776055,9.3301962605889296E-3,1.8981832269032253,-50700.336947278149,2231.5911371985717,5.0307172394308317,9.9142377831282942E-3,2.5414105798800235,-50617.258517112597,2135.0004548183415]
["AKM","AKM52I",8.5299999999999994,7.4,5.16,4.4482758620689662,4500,21.8,6000,1.57,7.8,74.900000000000006,0.62,640,10,2047.0795064871616,2804.9004492793633,3009.3457943925232,6.4294412190952324,4.032258064516129,0.65243711160213014,0.69754757592513772,0.90050649286761897,15.206537155168002,0,-12.317295095686081,0,0,0,0,0,0.38638579487911051,0.54966967051701465,4.6366295385493261,13.192072092408351,8.3983339325257269,252.7150358638288,204.8614568929078,1970.7672153097728,1.0084320072970766E-2,3.8519556629686509,-50143.95073167979,2047.0795064871616,6.0293363216598426E-3,1.1792185518116194,-50743.192356763328,2804.9004492793633,5.7896486042692947,6.4923459840828882E-3,1.7105478854520699,-50674.769231158927,2665.1667911436343]
["AKM","AKM52K",8.6,9.3000000000000007,3.9,4.193548387096774,5500,21.9,6000,0.93,5,60.1,0.62,640,10,2615.8573953588602,3563.994335346928,3750.4159733777042,5.5544048407035342,4.032258064516129,0.65066666154640573,0.69436242717662111,0.71289671869106652,15.206537155168002,0,-12.317295095686081,0,0,0,0,0,0.48164045760472912,0.68517827297995371,5.7796854912567497,16.444278551518888,10.468752868217056,252.7150358638288,204.8614568929078,1970.7672153097728,6.4950836773473523E-3,2.2926969860964403,-50441.341830195954,2615.8573953588602,3.8234481655826228E-3,0.62088401765261358,-50778.478390357697,3563.994335346928,6.4134606252531228,4.1753731189165507E-3,1.0134748960705429,-50734.068601791994,3366.5465656884849]
["AKM","AKM52L",8.67,11.6,3.27,4.3600000000000003,6000,22,6000,0.61,3.24,48.3,0.62,640,10,3294.3717315011172,4495.1243300920087,4666.666666666667,4.6243881029171918,4.032258064516129,0.64677108668600702,0.69120623432581829,0.56886277711950228,15.206537155168002,0,-12.317295095686081,0,0,0,0,0,0.59590544642442456,0.84773082948841239,7.1508653570930942,20.345539907721896,12.952372984749456,252.7150358638288,204.8614568929078,1970.7672153097728,4.203019468147929E-3,1.5021011053236613,-50563.366802440905,3294.3717315011172,2.435436560443469E-3,0.35174171596913323,-50791.901527166636,4495.1243300920087,6.8926509316770188,2.6950055816707887E-3,0.66097789438171139,-50758.341271206395,4218.9436478031794]
["AKM","AKM52M",8.6,13.1,5.2,7.8787878787878789,4500,21.9,6000,0.48,2.5,42.4,0.62,640,10,3781.8203765113326,5126.2962177550644,5316.0377358490568,4.7267984132517293,4.032258064516129,0.64714501244776768,0.69436242717662111,0.49790784141216354,15.206537155168002,0,-12.317295095686081,0,0,0,0,0,0.6784397843679516,0.96514358882122497,8.1412774124154197,23.163446131709399,14.746307803617571,252.7150358638288,204.8614568929078,1970.7672153097728,3.2278798802450543E-3,1.1759386929587528,-50612.860720674966,3781.8203765113326,1.8784156641445523E-3,0.27926460457457047,-50794.314737093919,5126.2962177550644,7.9222432501111753,2.0772106441128142E-3,0.51981764352595106,-50767.58401898462,4820.169116423499]
["AKM","AKM53G",11.4,4.7699999999999996,9.85,4.1213389121338908,2000,29.7,6000,3.75,21.3,154,0.91,640,10,984.37291780514533,1324.6384670091488,1463.6363636363635,10.37340518806791,2.7472527472527473,0.52863459612889163,0.55959479084782537,1.8135117654240236,16.619965288180413,0,-13.462171883426134,0,0,0,0,0,0.20368158960345731,0.28975597377419798,2.4441790752414878,6.9541433705807512,4.4271451695906432,276.20457445373597,223.9030666682101,2153.947501348181,3.8122472976757991E-2,12.43032812567473,-49176.375030865871,984.37291780514533,2.551869116976923E-2,4.3970805769426917,-50601.349095967635,1324.6384670091488,4.3959405276992873,2.5544374859527926E-2,4.428293311488658,-50598.445317374608,1323.3991892182996]
["AKM","AKM53H",11.51,6.6,8.83,5.0457142857142854,3000,30,6000,2.1,11.4,112.4,0.91,640,10,1395.6424220762201,1851.1542602258271,2005.3380782918148,9.8563021941982605,2.7472527472527473,0.52594228208393268,0.55399884293934709,1.3041261375085109,16.619965288180413,0,-13.462171883426134,0,0,0,0,0,0.27913022131450971,0.39708865805817672,3.3495626557741165,9.5301277933962414,6.0670677864658753,276.20457445373597,223.9030666682101,2153.947501348181,2.0541419198029605E-2,7.0329268443505155,-49826.392396412746,1395.6424220762201,1.3521177273641853E-2,2.356004236231231,-50695.320253931939,1851.1542602258271,5.7627507202169124,1.3617376726264162E-2,2.4804191783394729,-50683.413202129173,1840.3127818487858]
["AKM","AKM53I",11.58,7.4,8.58,5.5,3250,30.1,6000,1.66,9.11,100.6,0.91,640,10,{"$f":"IF(AQ78<I78,IF(AQ78<0,0,AQ78),I78)","v":1583.8981985116336},{"$f":"IF(AU78<I78,IF(AU78<0,0,AU78),I78)","v":2083.4779657571016},{"$f":"IF(UAC_V*0.98/L78*1000<I78,IF(UAC_V*0.98/L78*1000<0,0,UAC_V*0.98/L78*1000),I78)","v":2240.5566600397619},{"$f":"C78+(E78-C78)/G78*Q78","v":9.6567895700703676},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M78,(inertia/gear^2+gear_inertia)/M78),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M78,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M78))","v":2.7472527472527473},{"$f":"IF((C78+(E78-C78)/G78*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X78^2*time1+Y78^2*time2+Z78^2*time3+AA78^2*time4)/time)/(C78+(E78-C78)/G78*mspeed),SQRT((((X78-Y78)*2/PI()+Y78)^2*time1+Y78^2*time2+((Z78-Y78)*2/PI()+Y78)^2*time3+AA78^2*time4)/time)/(C78+(E78-C78)/G78*mspeed)),IF(AccType=1,SQRT((X78^2*time1+Y78^2*time2+Z78^2*time3+AA78^2*time4+AB78^2*time5+AC78^2*time6+AD78^2*time7+AE78^2*time8)/time)/(C78+(E78-C78)/G78*mspeed),SQRT((((X78-Y78)*2/PI()+Y78)^2*time1+Y78^2*time2+((Z78-Y78)*2/PI()+Y78)^2*time3+AA78^2*time4+((AB78-AC78)*2/PI()+AC78)^2*time5+AC78^2*time6+((AD78-AC78)*2/PI()+AC78)^2*time7+AE78^2*time8)/time)/(C78+(E78-C78)/G78*mspeed))))","v":0.52327708784433868},{"$f":"IF(move1,MAX(ABS(X78),ABS(Z78))/H78,MAX(ABS(X78),ABS(Z78),ABS(AB78),ABS(AD78))/H78)","v":0.55215831522194059},{"$f":"IF(AZ78>0,speed/(MIN(AZ78,I78)),\"NA\")","v":1.1599568282242658},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M78+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M78+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":16.619965288180413},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M78+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M78+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-13.462171883426134},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M78+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M78+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M78+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M78+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH78/Irms","v":0.31107234874969975},{"$f":"AI78/Ipeak","v":0.44252930027538523},{"$f":"IF(move1,IF(AccType=1,SQRT((X78^2*time1+Y78^2*time2+Z78^2*time3+AA78^2*time4)/time)/(C78/D78),SQRT((((X78-Y78)*2/PI()+Y78)^2*time1+Y78^2*time2+((Z78-AA78)*2/PI()+AA78)^2*time3+AA78^2*time4)/time)/(C78/D78)),IF(AccType=1,SQRT((X78^2*time1+Y78^2*time2+Z78^2*time3+AA78^2*time4+AB78^2*time5+AC78^2*time6+AD78^2*time7+AE78^2*time8)/time)/(C78/D78),SQRT((((X78-Y78)*2/PI()+Y78)^2*time1+Y78^2*time2+((Z78-AA78)*2/PI()+AA78)^2*time3+AA78^2*time4+((AB78-AC78)*2/PI()+AC78)^2*time5+AC78^2*time6+((AD78-AE78)*2/PI()+AE78)^2*time7+AE78^2*time8)/time)/(C78/D78)))","v":3.7328681849963967},{"$f":"IF(move1,MAX(ABS(X78),ABS(Z78))/(C78/D78),MAX(ABS(X78),ABS(Z78),ABS(AB78),ABS(AD78))/(C78/D78))","v":10.620703206609246},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X78),ABS(Z78))/(C78/D78),MAX(ABS((X78-Y78)*2/PI()+Y78),ABS((Z78-Y78)*2/PI()+Y78))/(C78/D78)),IF(AccType=1,MAX(ABS(X78),ABS(Z78),ABS(AB78),ABS(AD78))/(C78/D78),MAX(ABS((X78-Y78)*2/PI()+Y78),ABS((Z78-Y78)*2/PI()+Y78),ABS((AB78-AC78)*2/PI()+AC78),ABS((AD78-AC78)*2/PI()+AC78))/(C78/D78)))","v":6.7613496577752192},{"$f":"IF((C78+(E78-C78)/G78*mspeed)<0,\"NA\",U78*(C78+(E78-C78)/G78*mspeed)*mspeed/9.55)","v":276.20457445373597},{"$f":"IF(move1,IF(speed1>speed2,AM78/2*time1/time,AM78/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z78*-speed/30*PI(),((Z78-AA78)*2/PI()+AA78)*-speed/30*PI()),IF(AccType=1,X78*-speed/30*PI(),((X78-Y78)*2/PI()+Y78)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z78*-speed/30*PI(),((Z78-AA78)*2/PI()+AA78)*-speed/30*PI()),IF(AccType=1,X78*-speed/30*PI(),((X78-Y78)*2/PI()+Y78)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD78*-speed/30*PI(),((AD78-AE78)*2/PI()+AE78)*-speed/30*PI()),IF(AccType=1,AB78*-speed/30*PI(),((AB78-AC78)*2/PI()+AC78)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD78*-speed/30*PI(),((AD78-AE78)*2/PI()+AE78)*-speed/30*PI()),IF(AccType=1,AB78*-speed/30*PI(),((AB78-AC78)*2/PI()+AC78)*-speed/30*PI()),0)/2*time7/time)))","v":223.9030666682101},{"$f":"IF(move1,MAX(IF(AccType=1,Z78*-speed/30*PI(),((Z78-AA78)*2/PI()+AA78)*-speed/30*PI()),IF(AccType=1,X78*-speed/30*PI(),((X78-Y78)*2/PI()+Y78)*-speed/30*PI()),0),MAX(IF(AccType=1,Z78*-speed/30*PI(),((Z78-AA78)*2/PI()+AA78)*-speed/30*PI()),IF(AccType=1,X78*-speed/30*PI(),((X78-Y78)*2/PI()+Y78)*-speed/30*PI()),IF(AccType=1,AD78*-speed/30*PI(),((AD78-AE78)*2/PI()+AE78)*-speed/30*PI()),IF(AccType=1,AB78*-speed/30*PI(),((AB78-AC78)*2/PI()+AC78)*-speed/30*PI()),0))","v":2153.947501348181},{"$f":"(L78^2)/1000000+((K78/1000)^2*(D78/C78*H78)^2*PI()*PI()*(O78/2)^2)/1200","v":1.6433923805160251E-2},{"$f":"SQRT(3)*L78*J78*D78/C78*H78/1000","v":5.563605810934404},{"$f":"0.75*J78^2*(D78/C78*H78)^2-(UAC_V*0.98)^2","v":-50040.520461004773},{"$f":"-AO78/2/AN78+SQRT((AO78/2/AN78)^2-AP78/AN78)","v":1583.8981985116336},{"$f":"(L78^2)/1000000+((K78/1000)^2*AV78^2*PI()*PI()*(O78/2)^2)/1200","v":1.0805259435137335E-2},{"$f":"SQRT(3)*L78*J78*AV78/1000","v":1.8324514168049184},{"$f":"0.75*J78^2*AV78^2-(UAC_V*0.98)^2","v":-50722.211414303689},{"$f":"-AS78/2/AR78+SQRT((AS78/2/AR78)^2-AT78/AR78)","v":2083.4779657571016},{"$f":"D78+(F78-D78)*((0.85*UAC_V-D78*J78)/L78*1000)/G78","v":6.3352794005199575},{"$f":"(L78^2)/1000000+((K78/1000)^2*AJ78^2*PI()*PI()*(O78/2)^2)/1200","v":1.0900481151939988E-2},{"$f":"SQRT(3)*L78*J78*AJ78/1000","v":1.9556903455413148},{"$f":"0.75*J78^2*AJ78^2-(UAC_V*0.98)^2","v":-50710.679054469321},{"$f":"IF(((AX78/2/AW78)^2-AY78/AW78)>0,-AX78/2/AW78+SQRT((AX78/2/AW78)^2-AY78/AW78),-9999)","v":2069.0425208962902}]
["AKM","AKM53K",11.6,9.4,7.65,6.1693548387096779,4000,30.3,6000,1,5.7,79.8,0.91,640,10,2043.6607411561649,2667.3306413748819,2824.5614035087724,8.9660109916423032,2.7472527472527473,0.52370357072435314,0.54851370588054171,0.91078975020488373,16.619965288180413,0,-13.462171883426134,0,0,0,0,0,0.39446467038795796,0.56116262108080417,4.7335760446554955,13.467902905939301,8.573933282247765,276.20457445373597,223.9030666682101,2153.947501348181,1.0395518262749932E-2,3.393720029201643,-50353.006133323426,2043.6607411561649,6.7454696130035382E-3,1.0389087281675171,-50762.787019245225,2667.3306413748819,7.5164690961274161,6.8591382865114108E-3,1.1850689476316012,-50750.025751053676,2635.0757674426131]
["AKM","AKM53L",11.6,11.8,5.0599999999999996,5.1111111111111107,5500,30.3,6000,0.69,3.64,63.6,0.91,640,10,2587.3376801016811,3392.2011022354627,3544.0251572327047,7.566364507523649,2.7472527472527473,0.52801276576603051,0.54851370588054171,0.72300891834818359,16.619965288180413,0,-13.462171883426134,0,0,0,0,0,0.49517905431679837,0.70443818390994573,5.9421486518015803,16.906516413838698,10.76302263090677,276.20457445373597,223.9030666682101,2153.947501348181,6.6331405457381084E-3,2.3427906404115633,-50465.931182854714,2587.3376801016811,4.2289198600720165E-3,0.6245938898242781,-50781.048665944421,3392.2011022354627,8.2173332062766029,4.360554758871843E-3,0.81809000591213321,-50763.795483554022,3319.4611284783878]
["AKM","AKM53M",11.4,13.4,8.7200000000000006,10.258823529411766,3000,29.7,6000,0.51,2.7,54.7,0.91,640,10,3069.0707022870351,3949.7324622415053,4120.6581352833637,7.8715723337309225,2.7472527472527473,0.53120332766538225,0.55959479084782537,0.61912451676114066,16.619965288180413,0,-13.462171883426134,0,0,0,0,0,0.57218727477700815,0.81398952800298796,6.8662472973240973,19.535748672071712,12.436843872644575,276.20457445373597,223.9030666682101,2153.947501348181,4.8189229196541833E-3,1.6868424673960098,-50567.41334884557,3069.0707022870351,3.1357136203768333E-3,0.47297484832437442,-50786.468616456441,3949.7324622415053,9.7885850091407676,3.2239396267783487E-3,0.6009361249664763,-50774.986757693645,3876.4415477443035]
["AKM","AKM53P",11.4,19.100000000000001,5.88,9.8000000000000007,5000,29.8,6000,0.27,1.3,38.4,0.91,640,10,4464.9519877309231,5744.6005974395412,5869.791666666667,5.0579609404267458,2.7472527472527473,0.53583871413784223,0.55771695597920845,0.43140258155686817,16.619965288180413,0,-13.462171883426134,0,0,0,0,0,0.81558036927170574,1.1602388048400802,9.7869644312604684,27.845731316161924,17.727143131903837,276.20457445373597,223.9030666682101,2153.947501348181,2.3407930957715564E-3,0.89660342984776231,-50668.86549343283,4464.9519877309231,1.508482046217215E-3,0.17742876528625107,-50799.822650765149,5744.6005974395412,9.8802609374999992,1.5837600193149065E-3,0.31834231280355224,-50787.978293572138,5563.2490453319833]
["AKM","AKM53Q",11.57,21.1,4.99,9.0727272727272723,5500,30.1,6000,0.25,1.1299999999999999,35.5,0.91,640,10,4768.2435937323871,6000,6000,4.3918181818181816,2.7472527472527473,0.52960612727202339,0.55215831522194059,0.4,16.619965288180413,0,-13.462171883426134,0,0,0,0,0,0.88774317957443694,1.262897103070465,10.652918154893243,30.309530473691161,19.295646390729541,276.20457445373597,223.9030666682101,2153.947501348181,2.0513776781260016E-3,0.84380983120192254,-50663.915201104348,4768.2435937323871,1.2833616362079607E-3,0.1442237016570232,-50801.033740107196,6235.6704354452713,9.3822639972063779,1.3580038921974355E-3,0.29661172923343598,-50787.707407673312,6007.2216330513229]
["AKM","AKM54G",14.3,5,12.9,4.479166666666667,1500,38,6000,3.8,22.9,185,1.2,640,10,818.20818510706783,1100.6925900235669,1218.3783783783783,13.272686915978005,2.0833333333333335,0.45669148119637559,0.47456298476823217,2.1418480982760868,18.033393421192823,0,-14.607048671166185,0,0,0,0,0,0.18467986990758986,0.26272426312926606,2.2161584388910782,6.3053823151023849,4.0141310541310533,299.69411304364314,242.94467644351244,2337.1277873865897,5.3260513626125494E-2,16.178323522166078,-48893.266997897212,818.20818510706783,3.6575321206757508E-2,5.6847952286613932,-50569.097934318401,1100.6925900235669,4.6687312312312317,3.5962451007839229E-2,4.8877332905984847,-50630.653522863227,1120.5276424279073]
["AKM","AKM54H",14.19,5.5,12.6,4.9027237354085607,1800,37.5,6000,3.2,18.3,165.6,1.2,640,10,935.18679008872516,1237.1581746914817,1361.1111111111111,13.09717694568919,2.0833333333333335,0.45958645216723243,0.4808904912318086,1.9086193443270401,18.033393421192823,0,-14.607048671166185,0,0,0,0,0,0.20472264648670815,0.29123697385647324,2.456671757840498,6.9896873725553572,4.4497731840367498,299.69411304364314,242.94467644351244,2337.1277873865897,4.1970707427209458E-2,13.340819243414236,-49182.661352082207,935.18679008872516,2.9245089462640442E-2,4.7209840753071983,-50601.978381853063,1237.1581746914817,5.1435337913619934,2.8786801272864811E-2,4.084217036902916,-50653.092302929625,1257.4534608660879]
["AKM","AKM54I",14.42,7.7,11.71,6.262032085561497,2500,38,6000,1.66,9.84,120.3,1.2,640,10,1337.7028270444684,1739.5692299788168,1873.6492103075645,12.534306954702963,2.0833333333333335,0.45498788194256828,0.47456298476823217,1.3657384489335078,18.033393421192823,0,-14.607048671166185,0,0,0,0,0,0.28204022850935817,0.40122841349741317,3.384482742112298,9.6294819239379166,6.1303185904350954,299.69411304364314,242.94467644351244,2337.1277873865897,2.2669314467464279E-2,7.0184854537385366,-49954.22661608069,1337.7028270444684,1.5399835871322624E-2,2.3611550425190075,-50708.853019895316,1739.5692299788168,6.8263753237227789,1.5220284989229669E-2,2.1203980100174258,-50727.491748197986,1757.2910844489568]
["AKM","AKM54K",14.4,9.6999999999999993,10.050000000000001,6.7,3500,38.4,6000,1.02,6.2,96.6,1.2,640,10,1709.708885377142,2201.9077194859933,2333.3333333333335,11.663343262924553,2.0833333333333335,0.45800387049458158,0.46961962034356314,1.0864482518254299,18.033393421192823,0,-14.607048671166185,0,0,0,0,0,0.35579089937335823,0.5061455908147291,4.2694907924802985,12.147494179553499,7.7333349794238675,299.69411304364314,242.94467644351244,2337.1277873865897,1.4619942021052778E-2,4.4144681937662735,-50283.073408000004,1709.708885377142,9.8441471526361859E-3,1.3743610561194199,-50754.555698238626,2201.9077194859933,8.0530967169476479,9.8042490395447886E-3,1.3197897409177899,-50758.494572133925,2209.0329621936112]
["AKM","AKM54L",14.1,12.5,8.1300000000000008,7.1946902654867273,4500,37.5,6000,0.63,3.5,72.900000000000006,1.2,640,10,2338.6515419103889,2960.2863278878667,3091.9067215363511,10.172686805002098,2.0833333333333335,0.46946487992279912,0.4808904912318086,0.81465188506273922,18.033393421192823,0,-14.607048671166185,0,0,0,0,0,0.46824860632598148,0.66612712105469951,5.6189832759117779,15.987050905312788,10.177672708169162,299.69411304364314,242.94467644351244,2337.1277873865897,8.0982157841559786E-3,2.6445444627398884,-50476.16696900464,2338.6515419103889,5.5400926725141233E-3,0.7529749265707697,-50778.488589624991,2960.2863278878667,9.4656798081449391,5.5753205007459186E-3,0.80961246475934645,-50774.325328649196,2946.043634104115]
["AKM","AKM54N",14.1,17.8,9.85,12.3125,3500,37.6,6000,0.33,1.8,51.3,1.2,640,10,3335.5085113749028,4251.2068053268249,4393.7621832358682,8.937820307817427,2.0833333333333335,0.46770688552799916,0.4796115271593836,0.57078840610102743,18.033393421192823,0,-14.607048671166185,0,0,0,0,0,0.6667860154081976,0.94856502038189205,8.0014321848983716,22.765560489165409,14.493005936432887,299.69411304364314,242.94467644351244,2337.1277873865897,4.1326910200517528E-3,1.391812289492631,-50621.139328000005,3335.5085113749028,2.7276953506079546E-3,0.35199613287905301,-50793.389875330889,4251.2068053268249,12.004552074631022,2.7716231009841789E-3,0.42496229860990764,-50788.004393218827,4204.7104922716471]
["AKM","AKM54P",14.36,19.600000000000001,9.23,12.472972972972974,4000,38,6000,0.3,1.5,47.3,1.2,640,10,3634.3802717016069,4624.3507966550824,4765.3276955602541,8.4292701032898574,2.0833333333333335,0.45992819873226665,0.47456298476823217,0.52552930862063052,18.033393421192823,0,-14.607048671166185,0,0,0,0,0,0.72092024982868097,1.0255759954020989,8.6510429979441721,24.613823889650373,15.669646961724958,299.69411304364314,242.94467644351244,2337.1277873865897,3.4818375157741363E-3,1.2747594815155212,-50623.577400547794,3634.3802717016069,2.3090824120614345E-3,0.30616939935482657,-50794.685307280095,4624.3507966550824,12.457151877035599,2.3508850612132602E-3,0.38512546412938009,-50788.586196076409,4566.8242677070439]
["AKM","AKM62G",11.9,4.9000000000000004,10.199999999999999,4.1295546558704448,2000,29.7,6000,3.94,31.7,159,1.7,640,10,823.83671945759215,1231.2933619984151,1417.6100628930819,10.853400642301347,1.4705882352941178,0.62474985410283512,0.6892369857949755,2.0314331828469996,20.470338478110772,0,-16.580974167269723,0,0,0,0,0,0.24687793610985354,0.35120678761464563,2.9625352333182424,8.4289629027514952,5.3660444444444444,340.19331750900022,275.77503812506814,2652.9558667631554,5.6183112435973279E-2,13.269652242253271,-49063.895111048449,823.83671945759215,2.9415263244846758E-2,4.8536060187778531,-50572.203517013608,1231.2933619984151,4.4731199781020035,3.1230569789860246E-2,5.8224831303621931,-50469.91505514663,1181.4319172617156]
["AKM","AKM62H",11.9,5.4,10.199999999999999,4.6363636363636358,2000,29.6,6000,3.3,25.4,142.1,1.7,640,10,940.92778616145711,1387.4688763662537,1586.2068965517242,10.720651455088683,1.4705882352941178,0.62474985410283512,0.69156548912536386,1.8005593650969667,20.470338478110772,0,-16.580974167269723,0,0,0,0,0,0.27206956224351203,0.38704421492226254,3.2648347469221446,9.2890611581343006,5.9135999999999997,340.19331750900022,275.77503812506814,2652.9558667631554,4.4125730697427104E-2,10.90955797792377,-49331.605638810819,940.92778616145711,2.3406895099039936E-2,3.9981711678077407,-50607.246864729263,1387.4688763662537,4.9225794894760408,2.4831468313238975E-2,4.8030885165989421,-50519.537093939201,1332.9191175380943]
["AKM","AKM62I",12.1,7.6,9.4,5.875,3000,30.1,6000,1.75,13.4,103.2,1.7,640,10,1329.0809454803816,1952.0876829700439,2184.1085271317829,10.34312108532696,1.4705882352941178,0.61527078661931878,0.68007769030268339,1.2838157704649211,20.470338478110772,0,-16.580974167269723,0,0,0,0,0,0.37658358140959947,0.5357251116860946,4.5190029769151936,12.85740268046627,8.1852767676767666,340.19331750900022,275.77503812506814,2652.9558667631554,2.3846702861050575E-2,5.9138879387393235,-49984.190929069053,1329.0809454803816,1.2251116887805242E-2,2.0597916264405693,-50705.567372407699,1952.0876829700439,6.5848352713178295,1.3123870585846371E-2,2.5604231315546535,-50651.272232855787,1869.4271056748771]
["AKM","AKM62K",12.2,9.6,9,7.03125,3500,30.2,6000,1.05,8.5,82.1,1.7,640,10,1710.5341003755232,2495.0312257319983,2745.4323995127897,9.9188285936164586,1.4705882352941178,0.61038766545191936,0.67782577742088657,1.0079394058819382,20.470338478110772,0,-16.580974167269723,0,0,0,0,0,0.47178547041133601,0.67115863862658276,5.6614256449360321,16.107807327037985,10.25454863387978,340.19331750900022,275.77503812506814,2652.9558667631554,1.5129851500929416E-2,3.5482272660728231,-50338.20336339694,1710.5341003755232,7.6775513431105074E-3,1.1858983169108439,-50752.998676799638,2495.0312257319983,7.9424477988515747,8.3025841883283078E-3,1.5311214217053846,-50718.209324595795,2381.0955162528057]
["AKM","AKM62L",12.2,12,7.42,7.42,5000,30.1,6000,0.74,5.4,65.5,1.7,640,10,2172.301111109914,3165.0505506846716,3441.2213740458014,9.1742116735454537,1.4705882352941178,0.6113646579493297,0.68007769030268339,0.79974925439794731,20.470338478110772,0,-16.580974167269723,0,0,0,0,0,0.58973183801417006,0.83894829828322848,7.0767820561700407,20.134759158797483,12.818185792349727,340.19331750900022,275.77503812506814,2652.9558667631554,9.5458445014414244E-3,2.4855445864428112,-50445.161637946789,2172.301111109914,4.8189299735879737E-3,0.7883282012474695,-50768.94641379395,3165.0505506846716,9.3901691603053425,5.2753927191101528E-3,1.0761187766089557,-50737.679572206151,3000.9405908189615]
["AKM","AKM62M",12.2,13.4,5.7,6.2637362637362637,6000,30.2,6000,0.55000000000000004,4.4000000000000004,58.8,1.7,640,10,2424.0253358057357,3574.6844366114569,3833.3333333333335,8.3274251936709209,1.4705882352941178,0.61436637821277718,0.67782577742088657,0.71555600968043642,20.470338478110772,0,-16.580974167269723,0,0,0,0,0,0.65853388578248984,0.936825599749605,7.902406629389878,22.483814393990521,14.313640801457193,340.19331750900022,275.77503812506814,2652.9558667631554,7.8373751697600261E-3,1.8580292799096325,-50555.533628681813,2424.0253358057357,3.8238923937638806E-3,0.53743691544081695,-50784.274717964843,3574.6844366114569,9.5945994991403154,4.2730153476548431E-3,0.80177176355847346,-50758.677778989688,3354.0351384538403]
["AKM","AKM62P",12.3,18.8,8.1,12.272727272727272,4500,30.3,6000,0.3,2.2000000000000002,42.2,1.7,640,10,3469.7301981463825,5059.9246512257569,5341.2322274881517,7.5774036588559603,1.4705882352941178,0.60569106791796956,0.67558872865052055,0.50721482397419693,20.470338478110772,0,-16.580974167269723,0,0,0,0,0,0.91640172335318448,1.3036665426439109,10.996820680238214,31.287997023453862,19.918557542908761,340.19331750900028,275.77503812506814,2652.9558667631554,3.9153323484014315E-3,1.01552284900959,-50660.38468935158,3469.7301981463825,1.9307682034429448E-3,0.2691436059282355,-50794.990883092803,5059.9246512257569,12.274102159031067,2.1756786322883288E-3,0.43676941356097676,-50778.379446915169,4731.7229043015768]
["AKM","AKM62Q",12,21.8,6.5,10.833333333333334,5500,40.9,6000,0.27,1.6,35.5,1.7,640,10,3336.7743175279688,6000,6000,6,1.4705882352941178,0.62300431551716573,0.50049727330344185,0.42943298093254384,20.470338478110772,0,-16.580974167269723,0,0,0,0,0,1.0892019419322823,1.5494908986903291,13.070423303187388,37.1877815685679,23.674477037037033,340.19331750900022,275.77503812506814,2652.9558667631554,4.1662498293124628E-3,1.2335344989093444,-50503.313667923132,3336.7743175279688,1.3256894764697893E-3,0.1851072445234184,-50798.362798656017,6120.7678589641173,11.149892274861291,1.5552753009048573E-3,0.39303673092333852,-50774.515708816725,5588.7649681406201]
["AKM","AKM63G",16.5,4.5,14.6,3.9459459459459456,1500,42.1,6000,5.16,43.5,238,2.4,640,10,564.43564704869959,822.55932069940718,947.05882352941182,15.458091527114084,1.0416666666666667,0.52698623056688809,0.56726987073149404,2.9066380033026302,23.8820615577959,0,-19.34446986181468,0,0,0,0,0,0.19076931426670504,0.27138706315677158,{"$f":"IF(move1,IF(AccType=1,SQRT((X99^2*time1+Y99^2*time2+Z99^2*time3+AA99^2*time4)/time)/(C99/D99),SQRT((((X99-Y99)*2/PI()+Y99)^2*time1+Y99^2*time2+((Z99-AA99)*2/PI()+AA99)^2*time3+AA99^2*time4)/time)/(C99/D99)),IF(AccType=1,SQRT((X99^2*time1+Y99^2*time2+Z99^2*time3+AA99^2*time4+AB99^2*time5+AC99^2*time6+AD99^2*time7+AE99^2*time8)/time)/(C99/D99),SQRT((((X99-Y99)*2/PI()+Y99)^2*time1+Y99^2*time2+((Z99-AA99)*2/PI()+AA99)^2*time3+AA99^2*time4+((AB99-AC99)*2/PI()+AC99)^2*time5+AC99^2*time6+((AD99-AE99)*2/PI()+AE99)^2*time7+AE99^2*time8)/time)/(C99/D99)))","v":2.2892317712004604},6.5132895157625184,4.1464888888888884,396.89220376050037,321.73754447924631,3095.1151778903491,0.10793702977506395,24.422940501125932,-48172.57745497521,564.43564704869959,6.3614386531545053E-2,9.0032063893005514,-50447.409288149051,822.55932069940718,4.2326262396850627,6.3333567401101631E-2,8.8199838926448457,-50461.82215368568,825.69621579055615]
["AKM","AKM63H",16.600000000000001,5.6,14.6,4.8666666666666663,1500,58.9,6000,3.43,28.1,191.5,2.4,640,10,{"$f":"IF(AQ100<I100,IF(AQ100<0,0,AQ100),I100)","v":582.21986922690076},{"$f":"IF(AU100<I100,IF(AU100<0,0,AU100),I100)","v":1041.7075781397114},{"$f":"IF(UAC_V*0.98/L100*1000<I100,IF(UAC_V*0.98/L100*1000<0,0,UAC_V*0.98/L100*1000),I100)","v":1177.023498694517},{"$f":"C100+(E100-C100)/G100*Q100","v":15.211056562480385},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M100,(inertia/gear^2+gear_inertia)/M100),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M100,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M100))","v":1.0416666666666667},{"$f":"IF((C100+(E100-C100)/G100*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X100^2*time1+Y100^2*time2+Z100^2*time3+AA100^2*time4)/time)/(C100+(E100-C100)/G100*mspeed),SQRT((((X100-Y100)*2/PI()+Y100)^2*time1+Y100^2*time2+((Z100-Y100)*2/PI()+Y100)^2*time3+AA100^2*time4)/time)/(C100+(E100-C100)/G100*mspeed)),IF(AccType=1,SQRT((X100^2*time1+Y100^2*time2+Z100^2*time3+AA100^2*time4+AB100^2*time5+AC100^2*time6+AD100^2*time7+AE100^2*time8)/time)/(C100+(E100-C100)/G100*mspeed),SQRT((((X100-Y100)*2/PI()+Y100)^2*time1+Y100^2*time2+((Z100-Y100)*2/PI()+Y100)^2*time3+AA100^2*time4+((AB100-AC100)*2/PI()+AC100)^2*time5+AC100^2*time6+((AD100-AC100)*2/PI()+AC100)^2*time7+AE100^2*time8)/time)/(C100+(E100-C100)/G100*mspeed))))","v":0.52468379040163027},{"$f":"IF(move1,MAX(ABS(X100),ABS(Z100))/H100,MAX(ABS(X100),ABS(Z100),ABS(AB100),ABS(AD100))/H100)","v":0.40546793816291854},{"$f":"IF(AZ100>0,speed/(MIN(AZ100,I100)),\"NA\")","v":2.3023420372092596},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M100+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M100+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":23.8820615577959},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M100+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M100+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-19.34446986181468},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M100+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M100+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M100+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M100+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"AH100/Irms","v":0.23597168190419734},{"$f":"AI100/Ipeak","v":0.33569162832243227},2.831660182850368,{"$f":"IF(move1,MAX(ABS(X100),ABS(Z100))/(C100/D100),MAX(ABS(X100),ABS(Z100),ABS(AB100),ABS(AD100))/(C100/D100))","v":8.0565990797383744},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X100),ABS(Z100))/(C100/D100),MAX(ABS((X100-Y100)*2/PI()+Y100),ABS((Z100-Y100)*2/PI()+Y100))/(C100/D100)),IF(AccType=1,MAX(ABS(X100),ABS(Z100),ABS(AB100),ABS(AD100))/(C100/D100),MAX(ABS((X100-Y100)*2/PI()+Y100),ABS((Z100-Y100)*2/PI()+Y100),ABS((AB100-AC100)*2/PI()+AC100),ABS((AD100-AC100)*2/PI()+AC100))/(C100/D100)))","v":5.1289902721999097},{"$f":"IF((C100+(E100-C100)/G100*mspeed)<0,\"NA\",U100*(C100+(E100-C100)/G100*mspeed)*mspeed/9.55)","v":396.89220376050037},{"$f":"IF(move1,IF(speed1>speed2,AM100/2*time1/time,AM100/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z100*-speed/30*PI(),((Z100-AA100)*2/PI()+AA100)*-speed/30*PI()),IF(AccType=1,X100*-speed/30*PI(),((X100-Y100)*2/PI()+Y100)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z100*-speed/30*PI(),((Z100-AA100)*2/PI()+AA100)*-speed/30*PI()),IF(AccType=1,X100*-speed/30*PI(),((X100-Y100)*2/PI()+Y100)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD100*-speed/30*PI(),((AD100-AE100)*2/PI()+AE100)*-speed/30*PI()),IF(AccType=1,AB100*-speed/30*PI(),((AB100-AC100)*2/PI()+AC100)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD100*-speed/30*PI(),((AD100-AE100)*2/PI()+AE100)*-speed/30*PI()),IF(AccType=1,AB100*-speed/30*PI(),((AB100-AC100)*2/PI()+AC100)*-speed/30*PI()),0)/2*time7/time)))","v":321.73754447924631},{"$f":"IF(move1,MAX(IF(AccType=1,Z100*-speed/30*PI(),((Z100-AA100)*2/PI()+AA100)*-speed/30*PI()),IF(AccType=1,X100*-speed/30*PI(),((X100-Y100)*2/PI()+Y100)*-speed/30*PI()),0),MAX(IF(AccType=1,Z100*-speed/30*PI(),((Z100-AA100)*2/PI()+AA100)*-speed/30*PI()),IF(AccType=1,X100*-speed/30*PI(),((X100-Y100)*2/PI()+Y100)*-speed/30*PI()),IF(AccType=1,AD100*-speed/30*PI(),((AD100-AE100)*2/PI()+AE100)*-speed/30*PI()),IF(AccType=1,AB100*-speed/30*PI(),((AB100-AC100)*2/PI()+AC100)*-speed/30*PI()),0))","v":3095.1151778903491},{"$f":"(L100^2)/1000000+((K100/1000)^2*(D100/C100*H100)^2*PI()*PI()*(O100/2)^2)/1200","v":0.10077277925241421},{"$f":"SQRT(3)*L100*J100*D100/C100*H100/1000","v":22.605741624347555},{"$f":"0.75*J100^2*(D100/C100*H100)^2-(UAC_V*0.98)^2","v":-47321.466237095083},{"$f":"-AO100/2/AN100+SQRT((AO100/2/AN100)^2-AP100/AN100)","v":582.21986922690076},{"$f":"(L100^2)/1000000+((K100/1000)^2*AV100^2*PI()*PI()*(O100/2)^2)/1200","v":4.0978258284492232E-2},{"$f":"SQRT(3)*L100*J100*AV100/1000","v":5.8590254209944383},{"$f":"0.75*J100^2*AV100^2-(UAC_V*0.98)^2","v":-50571.139869766252},{"$f":"-AS100/2/AR100+SQRT((AS100/2/AR100)^2-AT100/AR100)","v":1041.7075781397114},{"$f":"D100+(F100-D100)*((0.85*UAC_V-D100*J100)/L100*1000)/G100","v":5.1499362924281984},{"$f":"(L100^2)/1000000+((K100/1000)^2*AJ100^2*PI()*PI()*(O100/2)^2)/1200","v":4.0943302389199271E-2},{"$f":"SQRT(3)*L100*J100*AJ100/1000","v":5.8351953660155758},{"$f":"0.75*J100^2*AJ100^2-(UAC_V*0.98)^2","v":-50573.039629968371},{"$f":"IF(((AX100/2/AW100)^2-AY100/AW100)>0,-AX100/2/AW100+SQRT((AX100/2/AW100)^2-AY100/AW100),-9999)","v":1042.4167917765662}]
["AKM","AKM63I",16.8,7.9,14.1,6.558139534883721,2000,42.5,6000,1.5,14.6,138.19999999999999,2.4,640,10,1076.3470189731315,1486.8253499055104,1630.9696092619395,14.792785777627561,1.0416666666666667,0.51844626535336324,0.56193086018343297,1.6186689876724991,23.8820615577959,0,-19.34446986181468,0,0,0,0,0,0.32892566289239422,0.4679272973873701,3.9471079547087307,11.230255137296883,7.1494024691358025,396.89220376050037,321.73754447924631,3095.1151778903491,3.6604868140016109E-2,7.1757395807340005,-50131.164090601087,1076.3470189731315,2.1252043927352731E-2,2.5164022114777462,-50722.273454646231,1486.8253499055104,7.0084201359674214,2.1339527272205214E-2,2.5670225007985197,-50718.905199814159,1482.6996861482994]
["AKM","AKM63K",16.8,9.9,12.9,7.5438596491228074,3000,42.6,6000,1.0900000000000001,9.3000000000000007,110,2.4,640,10,1360.6494415743739,1879.894942594791,2049.0909090909095,14.356136574626772,1.0416666666666667,0.51772428423383976,0.56061177365718073,1.2840783109714486,23.8820615577959,0,-19.34446986181468,0,0,0,0,0,0.41219798261198765,0.58638990432088145,4.9463757913438515,14.073357703701156,8.9593777777777763,396.89220376050037,321.73754447924631,3095.1151778903491,2.3307156305910369E-2,5.2133312737698443,-50243.614070866395,1360.6494415743739,1.3409548476279776E-2,1.7820849301389581,-50739.543745904375,1879.894942594791,8.5812111270600742,1.352751310428346E-2,1.8606198920862267,-50733.633008619283,1869.0448857315555]
["AKM","AKM63L",16.8,11.1,12.9,8.6,3000,42.6,6000,0.94,7.4,98.2,2.4,640,10,1529.0229158720078,2110.9720321263185,2295.3156822810593,14.055736358235787,1.0416666666666667,0.51772428423383976,0.56061177365718073,1.1448564871142548,23.8820615577959,0,-19.34446986181468,0,0,0,0,0,0.46216137444374367,0.65746746848098836,5.5459364933249242,15.77921924354372,10.045362962962962,396.89220376050037,321.73754447924631,3095.1151778903491,1.8563315695493826E-2,4.5001114006895717,-50280.154850832914,1529.0229158720078,1.0665740447261787E-2,1.5235992434333125,-50744.979120581091,2110.9720321263185,9.529514596062457,1.0779435891173793E-2,1.6060741873156239,-50738.287395585889,2096.3326207370164]
["AKM","AKM63M",17,13.8,11.3,9.112903225806452,4000,43,6000,0.57999999999999996,4.9000000000000004,79.900000000000006,2.4,640,10,1908.2631221861743,2633.0359299604324,2821.026282853567,13.247923799806385,1.0416666666666667,0.51318041295769612,0.55539678041385809,0.92352770223387848,23.8820615577959,0,-19.34446986181468,0,0,0,0,0,0.56781925305266323,0.80777561151368493,6.8138310366319592,19.386614676328438,12.341902222222222,396.89220376050037,321.73754447924631,3095.1151778903491,1.2399180047754694E-2,2.8017799355501998,-50497.752476858135,1908.2631221861743,6.9868428258169826E-3,0.88696914558733808,-50774.352002157582,2633.0359299604324,11.050275667164602,7.1360048579073741E-3,0.99064374488820173,-50766.729020518214,2598.7309251197889]
["AKM","AKM63N",17,17.399999999999999,9.6,9.795918367346939,5000,43,6000,0.38,3.1,63.3,2.4,640,10,2426.9436017493067,3362.0295010682821,3560.8214849921014,12.024196338418943,1.0416666666666667,0.51396081126151738,0.55539678041385809,0.72878192240763806,23.8820615577959,0,-19.34446986181468,0,0,0,0,0,0.71594601471857533,1.018499684082472,8.5913521766229035,24.443992417979331,15.561528888888887,396.89220376050037,321.73754447924631,3095.1151778903491,7.834427555449398E-3,1.8336511555129911,-50595.379062657441,2426.9436017493067,4.3337710768644342E-3,0.53586066185727455,-50787.244194417239,3362.0295010682821,12.861864861205145,4.4853949362352926E-3,0.64833608966482004,-50778.933944058743,3293.1662081727382]
["AKM","AKM63Q",16.7,22.4,11.9,15.866666666666667,3500,51.9,6000,0.23,1.8,48.3,2.4,640,10,2898.7224354255659,4464.5111670935739,4666.666666666667,10.577241827985956,1.0416666666666667,0.52198225484042338,0.4601553286665877,0.55340635830941753,23.8820615577959,0,-19.34446986181468,0,0,0,0,0,0.93823471128375491,1.3347259952460782,11.258816535405058,32.033423885905876,20.393111022399644,396.89220376050037,321.73754447924631,3095.1151778903491,5.5613939960747344E-3,1.3394746509512794,-50612.888574799814,2898.7224354255659,2.4836563797854629E-3,0.28945835411358906,-50796.181207733098,4464.5111670935739,15.043555555555557,2.6099478663806136E-3,0.39239103614833537,-50788.660001580705,4336.7770607690145]
["AKM","AKM64K",20.8,9.1999999999999993,17.2,7.5438596491228074,2000,53.5,6000,1.34,11.8,147,3.2,640,10,1050.861173339488,1410.3970795782511,1533.3333333333335,18.261285256759148,0.78125,0.4885265339556627,0.51927427381055369,1.6931192514444475,27.78117364886462,0,-22.502750655580343,0,0,0,0,0,0.35990113566720999,0.51199278359285749,4.3188136280065201,12.28782680622858,7.8226735042735038,461.69093090507187,374.26612316973547,3600.4401048928553,3.7640681324665193E-2,8.0734848541574209,-50051.062659883508,1050.861173339488,2.3519169341376857E-2,2.7868104750748128,-50715.309560090864,1410.3970795782511,8.1681682300990577,2.3360995278682555E-2,2.6689348028444337,-50722.749742909968,1417.5020442018438]
["AKM","AKM64L",21,12.8,15.6,9.3975903614457827,3000,54.1,6000,0.71,6.2,107,3.2,640,10,1481.085889765287,1968.579474247691,2106.5420560747662,17.456556946354155,0.78125,0.4836865690773991,0.51351522456311682,1.2186474948148369,27.78117364886462,0,-22.502750655580343,0,0,0,0,0,0.4959631385095134,0.70555361647910153,5.951557662114161,16.933286795498436,10.780065185185185,461.69093090507187,374.26612316973547,3600.4401048928553,2.0043443622275666E-2,4.339010427086941,-50394.053975754017,1481.085889765287,1.2375038317496912E-2,1.4242829941736335,-50760.863946906014,1968.579474247691,10.824143347220659,1.2367511632774521E-2,1.4184830177147409,-50761.223977824593,1969.3964088972748]
["AKM","AKM64P",20.399999999999999,18.600000000000001,11.9,10.818181818181818,4500,52.9,6000,0.36,2.8,71,3.2,640,10,2280.2486939897667,3021.6953430143967,3174.6478873239439,14.692353240972807,0.78125,0.49952662514936064,0.52516396311653346,0.80404060459812399,27.78117364886462,0,-22.502750655580343,0,0,0,0,0,0.74189338963624374,1.0554122342093177,8.9027206756349244,25.329893621023626,16.125511111111113,461.69093090507187,374.26612316973547,3600.4401048928553,8.7911744302638373E-3,2.1353050426509146,-50579.037820612459,2280.2486939897667,5.3570241509280237E-3,0.61986102215266881,-50786.104867745285,3021.6953430143967,14.001444757433489,5.4601809604235508E-3,0.71389602810530073,-50779.884879044614,2984.92387856403]
["AKM","AKM64Q",20,20.7,10.7,10.7,5000,53.2,6000,0.32,2.2999999999999998,64.400000000000006,3.2,640,10,2477.6264733005751,3342.7901813639828,3500,13.782410262662992,0.78125,0.50961500176695895,0.52220251219670333,0.7309981239935307,27.78117364886462,0,-22.502750655580343,0,0,0,0,0,0.84216865746127134,1.1980631136072866,10.106023889535257,28.753514726574878,18.305056,461.69093090507187,374.26612316973547,3600.4401048928553,7.4451131528548041E-3,1.965388701719496,-50572.315928780801,2477.6264733005751,4.3867177308003899E-3,0.52949652284581139,-50788.25969669225,3342.7901813639828,14.834285714285713,4.5118253985254085E-3,0.65338255506052578,-50779.426234227474,3283.1821604254073]
["AKM","AKM65K",24.8,9.8000000000000007,20.2,7.9527559055118102,2000,64.5,6000,1.27,11.4,164,4,640,10,964.30780058022788,1269.996923099141,1374.3902439024391,21.879007076871975,0.625,0.46860422033906624,0.49116722077416025,1.8711421007408311,31.680285739933336,0,-25.661031449346002,0,0,0,0,0,0.36666682715240345,0.52161760794917122,4.4000019258288416,12.518822590780109,7.9697299880525687,526.48965804964325,426.79470186022445,4105.7650318953592,4.4255468722552524E-2,9.1948003961653946,-50019.314945667356,964.30780058022788,2.8950826554970107E-2,3.1634551077001873,-50712.14014371622,1269.996923099141,8.7690688400230457,2.8593287553413588E-2,2.8750923841111038,-50728.325561633945,1282.6390892758925]
["AKM","AKM65L",25,12.2,19.2,9.1428571428571423,2500,65.2,6000,0.9,7.6,133.19999999999999,4,640,10,1192.2898168320339,1575.6221628126202,1692.1921921921924,21.34455658227472,0.625,0.4648681079706366,0.48589395306646216,1.5135089867962395,31.680285739933336,0,-25.661031449346002,0,0,0,0,0,0.4528110825438007,0.64416581004531104,5.4337329905256082,15.459979441087466,9.8421285925925908,526.48965804964325,426.79470186022445,4105.7650318953592,2.9765452640752227E-2,6.6065508090154328,-50190.151500620806,1192.2898168320339,1.9053111100069201E-2,2.1814462159475347,-50738.106634795389,1575.6221628126202,10.505993993993993,1.889267944158805E-2,2.0436023652263682,-50746.31299664588,1585.7190283886348]
["AKM","AKM65M",25,13.6,19.2,10.378378378378377,2500,65.2,6000,0.68,6.1,119,4,640,10,1354.4346574708122,1775.4829027848739,1894.1176470588236,20.880879665539091,0.625,0.4648681079706366,0.48589395306646216,1.3450287165054915,31.680285739933336,0,-25.661031449346002,0,0,0,0,0,0.50477301004882702,0.71808647677182214,6.0572761205859242,17.234075442523732,10.971553185185183,526.48965804964325,426.79470186022445,4105.7650318953592,2.3786231172236546E-2,4.9712201572687382,-50368.873193771011,1354.4346574708122,1.5187517476540032E-2,1.6234562381032465,-50758.630620771197,1775.4829027848739,11.583080772200772,1.5081988915841957E-2,1.537746028925101,-50763.413957180375,1784.3485202571892]
["AKM","AKM65N",24.3,17.8,16,11.594202898550726,3500,63.7,6000,0.42,3.4,88.8,4,640,10,1854.687429852733,2411.6850862169376,2538.2882882882886,18.580861081256977,0.625,0.47934143963639209,0.49733572590162217,0.99921838055532497,31.680285739933336,0,-25.661031449346002,0,0,0,0,0,0.67969011580648775,0.96692230139028368,8.1562813896778525,23.206135233366808,14.773484529797287,526.48965804964325,426.79470186022445,4105.7650318953592,1.3060586687251463E-2,3.0142276167439537,-50517.11113634934,1854.687429852733,8.3543642041155417E-3,0.90733160206356245,-50779.059660763916,2411.6850862169376,14.045692425344601,8.4042188063454329E-3,0.95434592902623372,-50776.284751686369,2401.877354043645]
["AKM","AKM65P",24.5,19.8,14.9,11.461538461538462,4000,64.099999999999994,6000,0.37,2.8,80.5,4,640,10,2042.2734396197159,2669.1551892442913,2800.0000000000005,18.094027545813702,0.625,0.47551145225504515,0.49423222683203338,0.90534527903606032,31.680285739933336,0,-25.661031449346002,0,0,0,0,0,0.74988787507253729,1.0667851320589798,8.9986545008704475,25.602843169415515,16.299276190476192,526.48965804964325,426.79470186022445,4105.7650318953592,1.0806273173548962E-2,2.6724855594309678,-50529.623598419545,2042.2734396197159,6.8394398323865912E-3,0.77007489219974057,-50782.282204405834,2669.1551892442913,14.927075585284282,6.9085136445270218E-3,0.84086553214004578,-50777.882701935072,2650.9223117122001]
["AKM","AKM72K",29.7,9.3000000000000007,25.1,7.7708978328173384,1500,79.400000000000006,6000,1.22,20.7,208,6.5,640,10,662.37858336798513,975.93614183095917,1083.6538461538462,26.707129165051725,0.38461538461538464,0.54448724474084653,0.55245605824336375,2.4755917010304218,43.865011024523085,0,-35.530658929863698,0,0,0,0,0,0.4023026355284256,0.57231285427618506,4.8276316263411072,13.735508502628441,8.7442962962962962,728.98568037642917,590.94651026800329,5684.9054287781919,9.7725951898429461E-2,10.927751102046958,-50115.118948847266,662.37858336798513,4.947692077616013E-2,3.6908984930784787,-50726.441367382766,975.93614183095917,8.397467049694372,5.0000726701033976E-2,3.8433386915410823,-50719.804668212048,969.46519856284942]
["AKM","AKM72L",30,11.5,24.3,9.3461538461538467,1800,79.5,6000,0.92,13.6,168.5,6.5,640,10,825.88765498684268,1211.0185968065659,1337.6854599406529,26.165107776779209,0.38461538461538464,0.53963043531729471,0.55176114496255457,1.9974889362985826,43.865011024523085,0,-35.530658929863698,0,0,0,0,0,0.49249629091302416,0.70062170386391032,5.9099554909562899,16.814920892733848,10.704711111111111,728.98568037642917,590.94651026800329,5684.9054287781919,6.3712498734618539E-2,8.1826141808697521,-50215.604973250003,825.88765498684268,3.2338759032075878E-2,2.7351852644573502,-50739.286051731506,1211.0185968065659,10.186814273757895,3.2750239982813401E-2,2.8742418684131836,-50732.417734785558,1201.5085322311145]
["AKM","AKM72M",30,13,23.6,10.128755364806867,2000,79.8,6000,0.64,10.8,150,6.5,640,10,938.15115872325771,1374.5608486849603,1502.6666666666665,25.601405284208127,0.38461538461538464,0.53991488640792018,0.54968685494389835,1.7662768645723679,43.865011024523085,0,-35.530658929863698,0,0,0,0,0,0.5567349375538535,0.79200714349833357,6.680819250646242,19.008171443960006,12.100977777777778,728.98568037642917,590.94651026800329,5684.9054287781919,5.1178471248985856E-2,5.749854424870251,-50437.817489920002,938.15115872325771,2.5513031730417083E-2,1.8637201621978396,-50766.566079522418,1374.5608486849603,11.208534763948498,2.6011938853569731E-2,2.0121127999078121,-50760.175578671639,1358.7903732074656]
["AKM","AKM72P",29.4,18.7,20.100000000000001,12.721518987341772,3000,78.5,6000,0.33,5,102,6.5,640,10,1414.8890780863314,2058.4735653447601,2209.8039215686276,23.018731947431245,0.38461538461538464,0.55061370055845582,0.55878994935698201,1.1926760422323004,43.865011024523085,0,-35.530658929863698,0,0,0,0,0,0.81718550488673936,1.1625222592950422,9.8062260586408723,27.90053422308101,17.762031746031745,728.98568037642917,590.94651026800329,5684.9054287781919,2.3219229332493312E-2,2.9109763151971055,-50601.541605448903,1414.8890780863314,1.156074554433627E-2,0.87456964249400293,-50786.780721367453,2058.4735653447601,15.00098094233474,1.2025749604027738E-2,1.0355411965263381,-50779.392372892566,2012.2815542668091]
["AKM","AKM72Q",29.5,23.5,16.3,12.538461538461538,4000,78.400000000000006,6000,0.26,3.2,81.2,6.5,640,10,1773.2732443290879,2611.1548368737572,2775.8620689655172,20.883189038316601,0.38461538461538464,0.55042325230185751,0.55950269163932498,0.95005832323097761,43.865011024523085,0,-35.530658929863698,0,0,0,0,0,1.0234631837691439,1.4559714111247068,12.281558205229727,34.943313866992966,22.245604519774012,728.98568037642929,590.94651026800329,5684.9054287781919,1.4806070480668291E-2,2.2837676329099583,-50607.403040009194,1773.2732443290879,7.2097157141783746E-3,0.62560224576836532,-50790.320319578612,2611.1548368737572,17.108356621826452,7.63539002368613E-3,0.81345628067459463,-50780.070247133182,2526.1607012062495]
["AKM","AKM73L",42,12.1,34.4,9.8285714285714274,1400,113,6000,0.95,15.7,224.7,9.1999999999999993,640,10,637.95080081852791,913.95305686412621,1003.1152647975078,37.038540548451884,0.27173913043478265,0.50677945733699858,0.50464171975115046,2.6154436608492455,57.024514331880006,0,-46.189856608822794,0,0,0,0,0,0.48117805317154466,0.68452045973784525,5.7741366380585362,16.428491033708287,10.458702222222222,947.68138448935781,768.2304633484041,7390.377057411647,0.10420401143845166,12.036544574152712,-50087.799398713862,637.95080081852791,5.6370414509700269E-2,3.9825299033150756,-50726.627042191853,913.95305686412621,10.77138974414866,5.6033964737185471E-2,3.8669192499040794,-50731.120398935323,917.62634230121785]
["AKM","AKM73M",42,13.6,33.799999999999997,10.903225806451612,1500,112,6000,0.68,12.4,200,9.1999999999999993,640,10,734.97446929007333,1036.9216903116042,1127,36.331494759629898,0.27173913043478265,0.50699998415339564,0.5091474493917858,2.3103087240722009,57.024514331880006,0,-46.189856608822794,0,0,0,0,0,0.54082822505231465,0.76937836796980952,6.4899387006277758,18.465080831275429,11.755235555555554,947.68138448935781,768.2304633484041,7390.377057411647,8.1583128435069471E-2,8.5429364631450539,-50349.023978666672,734.97446929007333,4.4496474829383882E-2,2.8092130671258593,-50755.837012146811,1036.9216903116042,11.925734709677419,4.436882401215226E-2,2.769050472254083,-50757.237246763187,1038.8222037138428]
["AKM","AKM73P",41.6,19.5,28.5,13.380281690140846,2400,111,6000,0.35,5.9,137,9.1999999999999993,640,10,1095.9825924792574,1538.2236176084566,1645.2554744525546,33.203862753887172,0.27173913043478265,0.51213326455691122,0.51373436335027034,1.5713400040539485,57.024514331880006,0,-46.189856608822794,0,0,0,0,0,0.78290850593510619,1.1137600455445313,9.3949020712212743,26.730241093068752,17.016999999999999,947.68138448935781,768.2304633484041,7390.377057411647,3.8146201272721239E-2,4.3212908534742045,-50556.431316528324,1095.9825924792574,2.0598652500168547E-2,1.3278599736510588,-50781.674304043576,1538.2236176084566,15.98832770038724,2.084166220928213E-2,1.4132930970055599,-50778.554994698126,1527.3588108290796]
["AKM","AKM73Q",41.5,24.5,25.2,14.823529411764707,3000,111,6000,0.27,3.7,109.2,9.1999999999999993,640,10,1383.2013115406792,1944.6641959837484,2064.1025641025644,30.933991201821634,0.27173913043478265,0.51329679601192901,0.51373436335027034,1.250586405228143,57.024514331880006,0,-46.189856608822794,0,0,0,0,0,0.98602452795682449,1.4027114469187349,11.832294335481894,33.665074726049639,21.431852208835338,947.68138448935781,768.2304633484041,7390.377057411647,2.4012346016058402E-2,3.3464781700042439,-50570.3747959537,1383.2013115406792,1.2932364355963389E-2,0.96624426545730258,-50785.586495463824,1944.6641959837484,18.920817621920563,1.3217588919907571E-2,1.094477242406481,-50780.04644449339,1919.0997039202348]
["AKM","AKM74L",53,12.9,43.5,10.507246376811596,1200,143,6000,0.85,16.399999999999999,266,12,640,10,555.91729810040817,777.65983960281744,847.36842105263156,46.843526269811029,0.20833333333333334,0.50255670220647741,0.49420564091343017,3.0671070884646676,70.671406650620511,0,-57.243839387002616,0,0,0,0,0,0.50380875698813865,0.71671473725865142,6.0457050838576638,17.201153694207633,10.950594549266244,1174.4769294953578,952.08048876511634,9159.0143019204188,0.13775155055908794,13.630477426409692,-50148.714204336509,555.91729810040817,7.8091047310583875E-2,4.5101350592149565,-50733.288645442226,777.65983960281744,11.516708051832481,7.7387650082935425E-2,4.2884355645392445,-50740.180777067653,782.49631681474546]
["AKM","AKM74P",52.5,18.5,39.6,13.943661971830988,1800,142,6000,0.43,7.7,183,12,640,10,836.15841287705314,1148.9431877009254,1231.6939890710382,44.265907154810037,0.20833333333333334,0.50420248903420817,0.49768596232831347,2.0881400279648652,70.671406650620511,0,-57.243839387002616,0,0,0,0,0,0.72939754333978579,1.0376357325686345,8.7527705200774299,24.903257581647228,15.853906172839503,1174.4769294953578,952.08048876511634,9159.0143019204188,6.4013003671322732E-2,6.81994609582918,-50457.944013034015,836.15841287705314,3.6573273108288763E-2,2.1678868305449881,-50770.07584318694,1148.9431877009254,15.905833589881732,3.6553167666797157E-2,2.1608093791864076,-50770.304546170541,1149.3482083857559]
["AKM","AKM74Q",52.2,26.1,31.5,15.75,2500,141,6000,0.26,3.8,129,12,640,10,1205.3391266194242,1655.1732186215388,1747.2868217054265,38.495165749813658,0.20833333333333334,0.51255437458818542,0.50121565000440083,1.4658037483845343,70.671406650620511,0,-57.243839387002616,0,0,0,0,0,1.0349559736578042,1.4723209718879273,12.419471683893651,35.335703325310256,22.495407407407402,1174.4769294953578,952.08048876511634,9159.0143019204188,3.1398199050083078E-2,4.09555537805314,-50553.168325000006,1205.3391266194242,1.7833825829106264E-2,1.1643923737033908,-50784.791488493203,1655.1732186215388,20.043597209302327,1.814349635515819E-2,1.3068253445234583,-50779.503601930643,1637.3269632070771]
["AKM","AKM82T",75,48,47.5,30.06,2500,210,4000,9.1999999999999998E-2,2.73,108.4,17.2,640,10,{"$f":"IF(AQ128<I128,IF(AQ128<0,0,AQ128),I128)","v":1104.7565579367881},{"$f":"IF(AU128<I128,IF(AU128<0,0,AU128),I128)","v":1905.7835656585598},{"$f":"IF(UAC_V*0.98/L128*1000<I128,IF(UAC_V*0.98/L128*1000<0,0,UAC_V*0.98/L128*1000),I128)","v":2079.3357933579337},{"$f":"C128+(E128-C128)/G128*Q128","v":54.036380777755838},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M128,(inertia/gear^2+gear_inertia)/M128),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M128,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M128))","v":0.14534883720930233},{"$f":"IF((C128+(E128-C128)/G128*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X128^2*time1+Y128^2*time2+Z128^2*time3+AA128^2*time4)/time)/(C128+(E128-C128)/G128*mspeed),SQRT((((X128-Y128)*2/PI()+Y128)^2*time1+Y128^2*time2+((Z128-Y128)*2/PI()+Y128)^2*time3+AA128^2*time4)/time)/(C128+(E128-C128)/G128*mspeed)),IF(AccType=1,SQRT((X128^2*time1+Y128^2*time2+Z128^2*time3+AA128^2*time4+AB128^2*time5+AC128^2*time6+AD128^2*time7+AE128^2*time8)/time)/(C128+(E128-C128)/G128*mspeed),SQRT((((X128-Y128)*2/PI()+Y128)^2*time1+Y128^2*time2+((Z128-Y128)*2/PI()+Y128)^2*time3+AA128^2*time4+((AB128-AC128)*2/PI()+AC128)^2*time5+AC128^2*time6+((AD128-AC128)*2/PI()+AC128)^2*time7+AE128^2*time8)/time)/(C128+(E128-C128)/G128*mspeed))))","v":0.48186962575685155},{"$f":"IF(move1,MAX(ABS(X128),ABS(Z128))/H128,MAX(ABS(X128),ABS(Z128),ABS(AB128),ABS(AD128))/H128)","v":0.45721731067889138},{"$f":"IF(AZ128>0,speed/(MIN(AZ128,I128)),\"NA\")","v":1.2803460526065469},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M128+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M128+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":96.015635242567186},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M128+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M128+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-77.772664546479419},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M128+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M128+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M128+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M128+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH128/Irms","v":1.7998241263279446},{"$f":"AI128/Ipeak","v":2.5604169398017915},{"$f":"IF(move1,IF(AccType=1,SQRT((X128^2*time1+Y128^2*time2+Z128^2*time3+AA128^2*time4)/time)/(C128/D128),SQRT((((X128-Y128)*2/PI()+Y128)^2*time1+Y128^2*time2+((Z128-AA128)*2/PI()+AA128)^2*time3+AA128^2*time4)/time)/(C128/D128)),IF(AccType=1,SQRT((X128^2*time1+Y128^2*time2+Z128^2*time3+AA128^2*time4+AB128^2*time5+AC128^2*time6+AD128^2*time7+AE128^2*time8)/time)/(C128/D128),SQRT((((X128-Y128)*2/PI()+Y128)^2*time1+Y128^2*time2+((Z128-AA128)*2/PI()+AA128)^2*time3+AA128^2*time4+((AB128-AC128)*2/PI()+AC128)^2*time5+AC128^2*time6+((AD128-AE128)*2/PI()+AE128)^2*time7+AE128^2*time8)/time)/(C128/D128)))","v":21.597889515935336},{"$f":"IF(move1,MAX(ABS(X128),ABS(Z128))/(C128/D128),MAX(ABS(X128),ABS(Z128),ABS(AB128),ABS(AD128))/(C128/D128))","v":61.450006555243},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X128),ABS(Z128))/(C128/D128),MAX(ABS((X128-Y128)*2/PI()+Y128),ABS((Z128-Y128)*2/PI()+Y128))/(C128/D128)),IF(AccType=1,MAX(ABS(X128),ABS(Z128),ABS(AB128),ABS(AD128))/(C128/D128),MAX(ABS((X128-Y128)*2/PI()+Y128),ABS((Z128-Y128)*2/PI()+Y128),ABS((AB128-AC128)*2/PI()+AC128),ABS((AD128-AC128)*2/PI()+AC128))/(C128/D128)))","v":39.120289185185179},{"$f":"IF((C128+(E128-C128)/G128*mspeed)<0,\"NA\",U128*(C128+(E128-C128)/G128*mspeed)*mspeed/9.55)","v":1595.6686559350728},{"$f":"IF(move1,IF(speed1>speed2,AM128/2*time1/time,AM128/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z128*-speed/30*PI(),((Z128-AA128)*2/PI()+AA128)*-speed/30*PI()),IF(AccType=1,X128*-speed/30*PI(),((X128-Y128)*2/PI()+Y128)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z128*-speed/30*PI(),((Z128-AA128)*2/PI()+AA128)*-speed/30*PI()),IF(AccType=1,X128*-speed/30*PI(),((X128-Y128)*2/PI()+Y128)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD128*-speed/30*PI(),((AD128-AE128)*2/PI()+AE128)*-speed/30*PI()),IF(AccType=1,AB128*-speed/30*PI(),((AB128-AC128)*2/PI()+AC128)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD128*-speed/30*PI(),((AD128-AE128)*2/PI()+AE128)*-speed/30*PI()),IF(AccType=1,AB128*-speed/30*PI(),((AB128-AC128)*2/PI()+AC128)*-speed/30*PI()),0)/2*time7/time)))","v":1293.5162502532958},{"$f":"IF(move1,MAX(IF(AccType=1,Z128*-speed/30*PI(),((Z128-AA128)*2/PI()+AA128)*-speed/30*PI()),IF(AccType=1,X128*-speed/30*PI(),((X128-Y128)*2/PI()+Y128)*-speed/30*PI()),0),MAX(IF(AccType=1,Z128*-speed/30*PI(),((Z128-AA128)*2/PI()+AA128)*-speed/30*PI()),IF(AccType=1,X128*-speed/30*PI(),((X128-Y128)*2/PI()+Y128)*-speed/30*PI()),IF(AccType=1,AD128*-speed/30*PI(),((AD128-AE128)*2/PI()+AE128)*-speed/30*PI()),IF(AccType=1,AB128*-speed/30*PI(),((AB128-AC128)*2/PI()+AC128)*-speed/30*PI()),0))","v":12443.626327436707},3.9431595960855534E-2,2.3215444618763579,{"$f":"0.75*J128^2*(D128/C128*H128)^2-(UAC_V*0.98)^2","v":-50690.49379072},{"$f":"-AO128/2/AN128+SQRT((AO128/2/AN128)^2-AP128/AN128)","v":1104.7565579367881},{"$f":"(L128^2)/1000000+((K128/1000)^2*AV128^2*PI()*PI()*(O128/2)^2)/1200","v":1.3665574121182503E-2},{"$f":"SQRT(3)*L128*J128*AV128/1000","v":0.61062112669806423},{"$f":"0.75*J128^2*AV128^2-(UAC_V*0.98)^2","v":-50797.227225724353},{"$f":"-AS128/2/AR128+SQRT((AS128/2/AR128)^2-AT128/AR128)","v":1905.7835656585598},{"$f":"D128+(F128-D128)*((0.85*UAC_V-D128*J128)/L128*1000)/G128","v":35.350380221402212},{"$f":"(L128^2)/1000000+((K128/1000)^2*AJ128^2*PI()*PI()*(O128/2)^2)/1200","v":1.4095803360549997E-2},{"$f":"SQRT(3)*L128*J128*AJ128/1000","v":0.67574025822074579},{"$f":"0.75*J128^2*AJ128^2-(UAC_V*0.98)^2","v":-50795.445039679384},{"$f":"IF(((AX128/2/AW128)^2-AY128/AW128)>0,-AX128/2/AW128+SQRT((AX128/2/AW128)^2-AY128/AW128),-9999)","v":1874.493224010841}]
["AKM","AKM83T",130,62,70,33.33,2200,456,4000,6.0999999999999999E-2,2.36,140.1,33.4,640,10,{"$f":"IF(AQ129<I129,IF(AQ129<0,0,AQ129),I129)","v":807.15113744956625},{"$f":"IF(AU129<I129,IF(AU129<0,0,AU129),I129)","v":1509.4759428914622},{"$f":"IF(UAC_V*0.98/L129*1000<I129,IF(UAC_V*0.98/L129*1000<0,0,UAC_V*0.98/L129*1000),I129)","v":1608.8508208422556},{"$f":"C129+(E129-C129)/G129*Q129","v":88.8324742847783},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M129,(inertia/gear^2+gear_inertia)/M129),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M129,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M129))","v":7.4850299401197612E-2},{"$f":"IF((C129+(E129-C129)/G129*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X129^2*time1+Y129^2*time2+Z129^2*time3+AA129^2*time4)/time)/(C129+(E129-C129)/G129*mspeed),SQRT((((X129-Y129)*2/PI()+Y129)^2*time1+Y129^2*time2+((Z129-Y129)*2/PI()+Y129)^2*time3+AA129^2*time4)/time)/(C129+(E129-C129)/G129*mspeed)),IF(AccType=1,SQRT((X129^2*time1+Y129^2*time2+Z129^2*time3+AA129^2*time4+AB129^2*time5+AC129^2*time6+AD129^2*time7+AE129^2*time8)/time)/(C129+(E129-C129)/G129*mspeed),SQRT((((X129-Y129)*2/PI()+Y129)^2*time1+Y129^2*time2+((Z129-Y129)*2/PI()+Y129)^2*time3+AA129^2*time4+((AB129-AC129)*2/PI()+AC129)^2*time5+AC129^2*time6+((AD129-AC129)*2/PI()+AC129)^2*time7+AE129^2*time8)/time)/(C129+(E129-C129)/G129*mspeed))))","v":0.52256387448122554},{"$f":"IF(move1,MAX(ABS(X129),ABS(Z129))/H129,MAX(ABS(X129),ABS(Z129),ABS(AB129),ABS(AD129))/H129)","v":0.38371196290944898},{"$f":"IF(AZ129>0,speed/(MIN(AZ129,I129)),\"NA\")","v":1.6286983955675944},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M129+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M129+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":174.97265508670873},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M129+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M129+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-141.72785062023405},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M129+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M129+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M129+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M129+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH129/Irms","v":2.4441432426180807},{"$f":"AI129/Ipeak","v":3.4770207100563915},{"$f":"IF(move1,IF(AccType=1,SQRT((X129^2*time1+Y129^2*time2+Z129^2*time3+AA129^2*time4)/time)/(C129/D129),SQRT((((X129-Y129)*2/PI()+Y129)^2*time1+Y129^2*time2+((Z129-AA129)*2/PI()+AA129)^2*time3+AA129^2*time4)/time)/(C129/D129)),IF(AccType=1,SQRT((X129^2*time1+Y129^2*time2+Z129^2*time3+AA129^2*time4+AB129^2*time5+AC129^2*time6+AD129^2*time7+AE129^2*time8)/time)/(C129/D129),SQRT((((X129-Y129)*2/PI()+Y129)^2*time1+Y129^2*time2+((Z129-AA129)*2/PI()+AA129)^2*time3+AA129^2*time4+((AB129-AC129)*2/PI()+AC129)^2*time5+AC129^2*time6+((AD129-AE129)*2/PI()+AE129)^2*time7+AE129^2*time8)/time)/(C129/D129)))","v":29.329718911416968},{"$f":"IF(move1,MAX(ABS(X129),ABS(Z129))/(C129/D129),MAX(ABS(X129),ABS(Z129),ABS(AB129),ABS(AD129))/(C129/D129))","v":83.448497041353392},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X129),ABS(Z129))/(C129/D129),MAX(ABS((X129-Y129)*2/PI()+Y129),ABS((Z129-Y129)*2/PI()+Y129))/(C129/D129)),IF(AccType=1,MAX(ABS(X129),ABS(Z129),ABS(AB129),ABS(AD129))/(C129/D129),MAX(ABS((X129-Y129)*2/PI()+Y129),ABS((Z129-Y129)*2/PI()+Y129),ABS((AB129-AC129)*2/PI()+AC129),ABS((AD129-AC129)*2/PI()+AC129))/(C129/D129)))","v":53.124963190883186},{"$f":"IF((C129+(E129-C129)/G129*mspeed)<0,\"NA\",U129*(C129+(E129-C129)/G129*mspeed)*mspeed/9.55)","v":2907.8428806126449},{"$f":"IF(move1,IF(speed1>speed2,AM129/2*time1/time,AM129/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z129*-speed/30*PI(),((Z129-AA129)*2/PI()+AA129)*-speed/30*PI()),IF(AccType=1,X129*-speed/30*PI(),((X129-Y129)*2/PI()+Y129)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z129*-speed/30*PI(),((Z129-AA129)*2/PI()+AA129)*-speed/30*PI()),IF(AccType=1,X129*-speed/30*PI(),((X129-Y129)*2/PI()+Y129)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD129*-speed/30*PI(),((AD129-AE129)*2/PI()+AE129)*-speed/30*PI()),IF(AccType=1,AB129*-speed/30*PI(),((AB129-AC129)*2/PI()+AC129)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD129*-speed/30*PI(),((AD129-AE129)*2/PI()+AE129)*-speed/30*PI()),IF(AccType=1,AB129*-speed/30*PI(),((AB129-AC129)*2/PI()+AC129)*-speed/30*PI()),0)/2*time7/time)))","v":2357.2199687357011},{"$f":"IF(move1,MAX(IF(AccType=1,Z129*-speed/30*PI(),((Z129-AA129)*2/PI()+AA129)*-speed/30*PI()),IF(AccType=1,X129*-speed/30*PI(),((X129-Y129)*2/PI()+Y129)*-speed/30*PI()),0),MAX(IF(AccType=1,Z129*-speed/30*PI(),((Z129-AA129)*2/PI()+AA129)*-speed/30*PI()),IF(AccType=1,X129*-speed/30*PI(),((X129-Y129)*2/PI()+Y129)*-speed/30*PI()),IF(AccType=1,AD129*-speed/30*PI(),((AD129-AE129)*2/PI()+AE129)*-speed/30*PI()),IF(AccType=1,AB129*-speed/30*PI(),((AB129-AC129)*2/PI()+AC129)*-speed/30*PI()),0))","v":22676.456099237446},7.3791778556152918E-2,3.2191541798645242,{"$f":"0.75*J129^2*(D129/C129*H129)^2-(UAC_V*0.98)^2","v":-50673.168096162844},{"$f":"-AO129/2/AN129+SQRT((AO129/2/AN129)^2-AP129/AN129)","v":807.15113744956625},{"$f":"(L129^2)/1000000+((K129/1000)^2*AV129^2*PI()*PI()*(O129/2)^2)/1200","v":2.1861962787268287E-2},{"$f":"SQRT(3)*L129*J129*AV129/1000","v":0.65376901845167001},{"$f":"0.75*J129^2*AV129^2-(UAC_V*0.98)^2","v":-50799.716071533905},{"$f":"-AS129/2/AR129+SQRT((AS129/2/AR129)^2-AT129/AR129)","v":1509.4759428914622},{"$f":"D129+(F129-D129)*((0.85*UAC_V-D129*J129)/L129*1000)/G129","v":44.166780027253267},{"$f":"(L129^2)/1000000+((K129/1000)^2*AJ129^2*PI()*PI()*(O129/2)^2)/1200","v":2.2860072856413588E-2},{"$f":"SQRT(3)*L129*J129*AJ129/1000","v":0.78637054861490097},{"$f":"0.75*J129^2*AJ129^2-(UAC_V*0.98)^2","v":-50797.28377312157},{"$f":"IF(((AX129/2/AW129)^2-AY129/AW129)>0,-AX129/2/AW129+SQRT((AX129/2/AW129)^2-AY129/AW129),-9999)","v":1473.5693278334754}]
["AKM","AKM84T",180,67,105,39.18,1800,668,4000,5.8000000000000003E-2,2.5,177.4,49.5,640,10,{"$f":"IF(AQ130<I130,IF(AQ130<0,0,AQ130),I130)","v":656.05966749167544},{"$f":"IF(AU130<I130,IF(AU130<0,0,AU130),I130)","v":1196.6933749076138},{"$f":"IF(UAC_V*0.98/L130*1000<I130,IF(UAC_V*0.98/L130*1000<0,0,UAC_V*0.98/L130*1000),I130)","v":1270.5749718151071},{"$f":"C130+(E130-C130)/G130*Q130","v":130.13777604551609},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M130,(inertia/gear^2+gear_inertia)/M130),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M130,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M130))","v":5.0505050505050504E-2},{"$f":"IF((C130+(E130-C130)/G130*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X130^2*time1+Y130^2*time2+Z130^2*time3+AA130^2*time4)/time)/(C130+(E130-C130)/G130*mspeed),SQRT((((X130-Y130)*2/PI()+Y130)^2*time1+Y130^2*time2+((Z130-Y130)*2/PI()+Y130)^2*time3+AA130^2*time4)/time)/(C130+(E130-C130)/G130*mspeed)),IF(AccType=1,SQRT((X130^2*time1+Y130^2*time2+Z130^2*time3+AA130^2*time4+AB130^2*time5+AC130^2*time6+AD130^2*time7+AE130^2*time8)/time)/(C130+(E130-C130)/G130*mspeed),SQRT((((X130-Y130)*2/PI()+Y130)^2*time1+Y130^2*time2+((Z130-Y130)*2/PI()+Y130)^2*time3+AA130^2*time4+((AB130-AC130)*2/PI()+AC130)^2*time5+AC130^2*time6+((AD130-AC130)*2/PI()+AC130)^2*time7+AE130^2*time8)/time)/(C130+(E130-C130)/G130*mspeed))))","v":0.55264182631425973},{"$f":"IF(move1,MAX(ABS(X130),ABS(Z130))/H130,MAX(ABS(X130),ABS(Z130),ABS(AB130),ABS(AD130))/H130)","v":0.37940461963992017},{"$f":"IF(AZ130>0,speed/(MIN(AZ130,I130)),\"NA\")","v":2.0488587370594309},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M130+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M130+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":253.44228591946668},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M130+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M130+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-205.28825159476801},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M130+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M130+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M130+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M130+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH130/Irms","v":2.7630548752672723},{"$f":"AI130/Ipeak","v":3.9307021195843213},{"$f":"IF(move1,IF(AccType=1,SQRT((X130^2*time1+Y130^2*time2+Z130^2*time3+AA130^2*time4)/time)/(C130/D130),SQRT((((X130-Y130)*2/PI()+Y130)^2*time1+Y130^2*time2+((Z130-AA130)*2/PI()+AA130)^2*time3+AA130^2*time4)/time)/(C130/D130)),IF(AccType=1,SQRT((X130^2*time1+Y130^2*time2+Z130^2*time3+AA130^2*time4+AB130^2*time5+AC130^2*time6+AD130^2*time7+AE130^2*time8)/time)/(C130/D130),SQRT((((X130-Y130)*2/PI()+Y130)^2*time1+Y130^2*time2+((Z130-AA130)*2/PI()+AA130)^2*time3+AA130^2*time4+((AB130-AC130)*2/PI()+AC130)^2*time5+AC130^2*time6+((AD130-AE130)*2/PI()+AE130)^2*time7+AE130^2*time8)/time)/(C130/D130)))","v":33.156658503207268},{"$f":"IF(move1,MAX(ABS(X130),ABS(Z130))/(C130/D130),MAX(ABS(X130),ABS(Z130),ABS(AB130),ABS(AD130))/(C130/D130))","v":94.33685087002371},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X130),ABS(Z130))/(C130/D130),MAX(ABS((X130-Y130)*2/PI()+Y130),ABS((Z130-Y130)*2/PI()+Y130))/(C130/D130)),IF(AccType=1,MAX(ABS(X130),ABS(Z130),ABS(AB130),ABS(AD130))/(C130/D130),MAX(ABS((X130-Y130)*2/PI()+Y130),ABS((Z130-Y130)*2/PI()+Y130),ABS((AB130-AC130)*2/PI()+AC130),ABS((AD130-AC130)*2/PI()+AC130))/(C130/D130)))","v":60.056704526748959},{"$f":"IF((C130+(E130-C130)/G130*mspeed)<0,\"NA\",U130*(C130+(E130-C130)/G130*mspeed)*mspeed/9.55)","v":4211.9172643971469},{"$f":"IF(move1,IF(speed1>speed2,AM130/2*time1/time,AM130/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z130*-speed/30*PI(),((Z130-AA130)*2/PI()+AA130)*-speed/30*PI()),IF(AccType=1,X130*-speed/30*PI(),((X130-Y130)*2/PI()+Y130)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z130*-speed/30*PI(),((Z130-AA130)*2/PI()+AA130)*-speed/30*PI()),IF(AccType=1,X130*-speed/30*PI(),((X130-Y130)*2/PI()+Y130)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD130*-speed/30*PI(),((AD130-AE130)*2/PI()+AE130)*-speed/30*PI()),IF(AccType=1,AB130*-speed/30*PI(),((AB130-AC130)*2/PI()+AC130)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD130*-speed/30*PI(),((AD130-AE130)*2/PI()+AE130)*-speed/30*PI()),IF(AccType=1,AB130*-speed/30*PI(),((AB130-AC130)*2/PI()+AC130)*-speed/30*PI()),0)/2*time7/time)))","v":3414.3576148817956},{"$f":"IF(move1,MAX(IF(AccType=1,Z130*-speed/30*PI(),((Z130-AA130)*2/PI()+AA130)*-speed/30*PI()),IF(AccType=1,X130*-speed/30*PI(),((X130-Y130)*2/PI()+Y130)*-speed/30*PI()),0),MAX(IF(AccType=1,Z130*-speed/30*PI(),((Z130-AA130)*2/PI()+AA130)*-speed/30*PI()),IF(AccType=1,X130*-speed/30*PI(),((X130-Y130)*2/PI()+Y130)*-speed/30*PI()),IF(AccType=1,AD130*-speed/30*PI(),((AD130-AE130)*2/PI()+AE130)*-speed/30*PI()),IF(AccType=1,AB130*-speed/30*PI(),((AB130-AC130)*2/PI()+AC130)*-speed/30*PI()),0))","v":32846.120255162874},0.11092115221774389,4.4311963712577898,{"$f":"0.75*J130^2*(D130/C130*H130)^2-(UAC_V*0.98)^2","v":-50649.177897242967},{"$f":"-AO130/2/AN130+SQRT((AO130/2/AN130)^2-AP130/AN130)","v":656.05966749167544},{"$f":"(L130^2)/1000000+((K130/1000)^2*AV130^2*PI()*PI()*(O130/2)^2)/1200","v":3.4722977157122234E-2},{"$f":"SQRT(3)*L130*J130*AV130/1000","v":0.89652569667566362},{"$f":"0.75*J130^2*AV130^2-(UAC_V*0.98)^2","v":-50798.775038810636},{"$f":"-AS130/2/AR130+SQRT((AS130/2/AR130)^2-AT130/AR130)","v":1196.6933749076138},{"$f":"D130+(F130-D130)*((0.85*UAC_V-D130*J130)/L130*1000)/G130","v":50.306083302016788},{"$f":"(L130^2)/1000000+((K130/1000)^2*AJ130^2*PI()*PI()*(O130/2)^2)/1200","v":3.6105885745871404E-2},{"$f":"SQRT(3)*L130*J130*AJ130/1000","v":1.0702955851808389},{"$f":"0.75*J130^2*AJ130^2-(UAC_V*0.98)^2","v":-50796.060024025021},{"$f":"IF(((AX130/2/AW130)^2-AY130/AW130)>0,-AX130/2/AW130+SQRT((AX130/2/AW130)^2-AY130/AW130),-9999)","v":1171.383832662146}]
["DBK","DBK4N00100",1,1.1000000000000001,0.9,1.06,3000,4.6500000000000004,9000,38,70,56,7.9000000000000001E-2,670,6,782.17007945006355,3227.1562998161967,4025.0000000000005,0.89242812333946009,31.645569620253163,4.4854202926546236,2.7031747534586623,"NA",12.569762603582781,0,-10.181507708902052,0,0,0,0,0,0.40497470367859661,0.57611411933087753,4.8596964441431592,13.82673886394106,8.8023753481481464,208.89489663231234,169.33900555346449,1629.0412334243283,1.2625610012295903E-2,18.852888066161114,-22470.387324999992,782.17007945006355,3.5461609310796487E-3,3.9195016510680714,-49580.471448284014,3227.1562998161967,1.063404761904762,3.1239270018907854E-2,32.443831310845148,33107.642146570157,-9999]
["DBK","DBK4H00100",1,1.9,0.9,1.85,3000,4.6109999999999998,9000,13,24,32,7.9000000000000001E-2,670,6,2443.4594991423692,6043.1816969322444,7043.75,0.79856061010225854,31.645569620253163,4.4854202926546236,2.7260383004950728,2.4245488858436071,12.569762603582781,0,-10.181507708902052,0,0,0,0,0,0.6995017608993942,0.99510620611697032,8.3940211307927299,23.882548946807287,15.204102874074072,208.89489663231234,169.33900555346449,1629.0412334243283,4.2965096701362369E-3,6.3125187507325524,-41076.670503332505,2443.4594991423692,1.1638428855461906E-3,1.3049155314170084,-50389.436234342451,6043.1816969322444,1.8110416666666669,1.0880099771718037E-2,10.955059923142519,-21505.028671962071,989.8748645626647]
["DBK","DBK4N00160",1.6,1.1000000000000001,1.4,1,3000,7.3010000000000002,9000,25,68,90,0.128,670,6,1050.328336050979,2210.0171924422875,2504.4444444444448,1.4526655205038475,19.53125,2.8676066526107897,1.7543601176771317,2.6080122138959809,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.25791816626292935,0.3669125401322087,3.0950179951551524,8.8059009631730092,5.6060106666666663,212.86381866991732,172.55638099825697,1659.9923852032321,1.6723606596990688E-2,19.561321744687135,-38995.119617309574,1050.328336050979,8.4686273615242856E-3,4.0443386356733289,-50300.324351851858,2210.0171924422875,1.0377777777777779,1.8856888666779873E-2,21.847264430489414,-36073.587064946674,920.24108906098957]
["DBK","DBK4H00160",1.6,1.9,1.4,1.7,3000,5.9639999999999995,9000,7.6,18,51,0.128,670,6,3004.8149212927783,4154.8433511207149,4419.6078431372553,1.3230104432586187,19.53125,2.8676066526107897,2.147649768470949,0.95774844728497066,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.44549501445415074,0.63375802386472413,5.3459401734498089,15.210192572753378,9.6831093333333307,212.86381866991732,172.55638099825697,1659.9923852032321,3.8039526276768109E-3,4.7546182040462526,-48632.303957492506,3004.8149212927783,2.6673525739450378E-3,1.1166582363220239,-50685.309402465806,4154.8433511207149,1.6633202614379083,4.8497215927343516E-3,6.5006866332079269,-46743.36389242905,2505.8772027284722]
["DBK","DBK5N00210",2.1,1.5,1.9,1.5,3000,9.52,9000,22,60,83,0.41299999999999998,670,6,883.92274622253603,2286.2473685756404,2715.6626506024099,1.947583508761624,6.053268765133172,2.4107771360355099,1.4913489392441144,2.5245786974998947,14.197641901603969,0,-11.500089940299215,0,0,0,0,0,0.29702726613450087,0.4225488661191657,3.5643271936140102,10.141172786859977,6.4560711111111093,235.94836521517087,191.26968715674369,1840.0143904478743,1.9211003702672039E-2,21.50652846742123,-34020.040000000008,883.92274622253603,7.4885784673661788E-3,4.7440871619311551,-49988.41,2286.2473685756404,1.5,1.799608563323853E-2,20.418776049824544,-35675.009928404397,950.65366842266951]
["DBK","DBK5H00210",2.1,4,1.9,3.94,3000,7.5919999999999996,9000,3.1,10,32,0.41299999999999998,670,6,3921.6121893355003,6393.6217261753918,7043.75,1.6737585515883069,6.053268765133172,2.4107771360355099,1.8700792810331888,0.69436254470831782,14.197641901603969,0,-11.500089940299215,0,0,0,0,0,0.79207270969200227,1.1267969763177754,9.5048725163040277,27.043127431626608,17.216189629629625,235.94836521517087,191.26968715674369,1840.0143904478743,2.571942416235185E-3,2.4846727415646495,-49297.933771319731,3921.6121893355003,1.135755474511879E-3,0.66761517326564701,-50696.344077252317,6393.6217261753918,3.8855624999999998,3.2179922238495867E-3,2.9580760630048855,-48668.877286493538,3456.4076335773161]
["DBK","DBK5N00430",4.3,2.9,3.9,2.8,3000,19.37,9000,7.1,32,90,0.57799999999999996,670,6,1148.5139209245676,2234.594961141644,2504.4444444444448,4.0020540051811135,4.3252595155709344,1.2436242136820375,0.77448806248770741,1.3337652220469247,15.001833770386893,0,-12.151485354013383,0,0,0,0,0,0.29633437087616016,0.42156315827637586,3.5560124505139221,10.11751579863302,6.4410106046511624,249.31310268873881,202.10370651165709,1944.2376566421412,2.1035382980776021E-2,14.458413748527679,-44353.131354209443,1148.5139209245676,8.7093040139034263E-3,3.1379644732412766,-50501.245770514681,2234.594961141644,2.8352185185185186,1.1244625948741286E-2,7.1287847187619331,-49236.654704739085,1799.4171390349559]
["DBK","DBK5H00430",4.3,5,3.9,4.8,3000,19.574999999999999,9000,2.2000000000000002,10,53,0.57799999999999996,670,6,2389.6328615458665,3968.9969927131433,4252.8301886792451,3.7708004009715808,4.3252595155709344,1.2436242136820375,0.76637720410661014,0.70809924875742092,15.001833770386893,0,-12.151485354013383,0,0,0,0,0,0.51092132909682786,0.72683303151099288,6.1310559491619347,17.443992756263828,11.105190697674418,249.31310268873881,202.10370651165709,1944.2376566421412,6.6440201286967655E-3,4.5968729133506345,-48924.487110938346,2389.6328615458665,2.9772750597434065E-3,0.96291632595984167,-50722.638831363482,3968.9969927131433,4.7679245283018865,3.7218786498417547E-3,2.2427723765788179,-50357.48930463288,3389.3553823302909]
["DBK","DBK6N00350",3.5,2.8,3,2.7,3000,16.510000000000002,9000,12,56,77,0.8,670,6,632.77397642876235,2285.7115684665587,2927.272727272727,3.11904807192224,3.125,1.6506364566338978,0.97418760603624832,2.0857431014949932,16.083837375658462,0,-13.027908274283355,0,0,0,0,0,0.37686672695953155,0.53612791252194869,4.5224007235143784,12.867069900526769,8.1914311111111111,267.29474947135736,216.68038709826786,2084.4653238853366,4.6424911928584042E-2,21.138280609325626,-31964.423488000004,632.77397642876235,7.6589550136484151E-3,4.3689942390440386,-50000.297853735879,2285.7115684665587,2.7299134199134198,2.1505024774579953E-2,13.109688780937816,-43558.409286007474,1150.6690341105564]
["DBK","DBK6N00700",7,5,6,4.5999999999999996,3000,31.97,9000,4.4000000000000004,34,84,1.135,670,6,784.08643535648525,2210.1323873304837,2683.3333333333335,6.263289204223172,2.2026431718061672,0.90910053331276042,0.55416298291502941,1.3373937567157552,17.716590563793488,0,-14.350438356672724,0,0,0,0,0,0.37064679450700683,0.52727948106528244,4.4477615340840817,12.654707545566778,8.056237037037036,294.42921646314664,238.67672942491015,2296.0701370676356,5.1677898505634819E-2,14.618647379945928,-43233.417822448981,784.08643535648525,8.9660710301453696E-3,3.0245302141875414,-50481.046372713536,2210.1323873304837,4.7246031746031747,1.2609711487853441E-2,5.1573288656611442,-49862.76909054062,1794.5350708782225]
["DBK","DBK7N00650",6.5,4.5,5,3.8,3000,30.03,9000,4.1500000000000004,22,87,3.2360000000000002,670,6,1146.6901693687569,2341.9830830574756,2590.8045977011493,5.3290084584712627,0.77255871446229907,1.5660819678177467,0.93095683293249132,1.4422382363786521,27.956633692962715,0,-22.644873291299799,0,0,0,0,0,0.5668813494335333,0.80644135652777071,6.8025761932023991,19.354592556666496,12.32151630769231,464.60687362657762,376.62990921080745,3623.179726607968,2.3054147593009295E-2,13.001170867272332,-45222.1753283125,1146.6901693687569,8.1496326058212547E-3,2.5175349106071758,-50595.819861734519,2341.9830830574756,4.0257567049808429,1.3008195674061959E-2,7.705345784520933,-48844.123084323081,1664.0801356273935]
["DBK","DBK7N01200",12,7.5,10,6.8,3000,55.545000000000002,9000,1.65,11.5,98,5.3109999999999999,670,6,1292.8740617970877,2145.5241865818257,2300.0000000000005,10.569650542278783,0.47072114479382415,1.1437325426331142,0.68538942621608057,1.2699986601750832,38.069955679172196,0,-30.836664100129479,0,0,0,0,0,0.69690009571044043,0.99140509581177583,8.3628011485252856,23.793722299482621,15.147554074074071,632.67857215780987,512.87591018926366,4933.8662560207167,2.1401953126759649E-2,9.7228958953793914,-48344.344074542241,1292.8740617970877,1.009249104517893E-2,1.9784296222867759,-50703.270584903643,2145.5241865818257,7.0639880952380949,1.1850165293781478E-2,4.242415089224294,-50336.655059629375,1889.7657731931258]
["DBK","DBK7N01950",19.5,11.8,15,10,3000,90.75,9000,0.9,7,100,6.9160000000000004,670,6,1338.5382250437397,2128.6157096356987,2254,16.307076435546453,0.36148062463851938,0.85694024924290424,0.50570302272042778,1.192849385138804,45.892549311878817,0,-37.172964942621839,0,0,0,0,0,0.81338791360530693,1.1571198330772865,9.7606549632636828,27.770875993854876,17.679488753656219,762.68101849160632,618.26137118705776,5947.6743908194949,2.0938182070613345E-2,8.5604612643929183,-48973.122573520712,1338.5382250437397,1.041454434875908E-2,1.6665183188543473,-50735.727917323078,2128.6157096356987,10.690720000000001,1.1133695683595115E-2,2.7559595495857625,-50615.277174026181,2011.9891328281383]
["DBL","DBL1X00010",0.1,0.6,0.09,0.59,6000,0.47599999999999998,14000,38.200000000000003,6.5,10,6.0000000000000001E-3,330,6,12228.967865330673,14000,14000,7.6666666666666647E-2,416.66666666666669,43.254075897497493,25.659597952253698,"NA",12.213968625272759,0,-9.8933145864709342,0,0,0,0,0,2.1464273130922407,3.0534921563181894,25.757127757106886,73.283811751636549,46.653923555555544,202.98201278037013,164.5457727479573,1582.9303338353493,1.2550962816545679E-4,1.8896535746511842,-41878.183419520006,12228.967865330673,1.0102051613264825E-4,0.3779549751885482,-50448.035091825564,20554.380208685936,0.57123666666666661,6.907130379696493E-3,30.868261000790838,2331318.6830323623,-9999]
["DBL","DBL1X00020",0.2,0.93,0.18,0.89,6000,0.96399999999999997,14000,22,4.7,13,1.2E-2,330,6,10177.995692166689,14000,14000,0.15333333333333329,208.33333333333334,21.678818566343523,12.700427350576533,"NA",12.243211965955776,0,-9.9170016924241775,0,0,0,0,0,1.6674639637382185,2.3721223184039317,20.009567564858621,56.930935641694361,36.24335928888889,203.46800323395448,164.93973708813601,1586.7202707878685,2.0185615194266189E-4,2.2205300117023588,-43511.145898119998,10177.995692166689,1.7015440763018744E-4,0.41622474170483104,-50548.88332010762,16056.170096667194,0.84023589743589744,2.3168978006747765E-3,17.953747161444085,426024.77659328631,-9999]
["DBL","DBL2H00040",0.4,0.93,0.34,0.7,6000,1.849,14000,26.5,20,26,8.0000000000000002E-3,560,6,4065.3139473018764,7996.0975524897149,8669.2307692307695,0.32003902447510291,312.5,10.863337734770356,6.6109877801516674,"NA",12.223716405500433,0,-9.9012102884553492,0,0,0,0,0,0.83240438317186538,1.1841725267828545,9.988852598062385,28.420140642788507,18.092823466666665,203.14400959823161,164.67709419468358,1584.193646152856,1.2231932568670474E-3,5.1302640408524161,-41071.576742284262,4065.3139473018764,6.8961464858804684E-4,0.80923110417721511,-50562.979903858039,7996.0975524897149,0.67809839743589739,1.036845272987055E-2,21.59166806318574,121606.13058831179,-9999]
["DBL","DBL2H00060",0.6,1.5,0.52,1.27,6000,2.7879999999999998,14000,14.8,13.2,25,1.0999999999999999E-2,560,6,4331.1377694096454,8263.3598594740979,9016,0.48982186854034537,227.27272727272728,7.2417008992965952,4.3896478033866364,"NA",12.238338075841941,0,-9.9130538414319709,0,0,0,0,0,0.89612912063956796,1.2748268829002023,10.753549447674816,30.595845189604855,19.477920000000005,203.38700482502375,164.87407636477289,1586.0886146291152,1.2515769687817988E-3,4.4667858276393773,-42824.289748000003,4331.1377694096454,6.4464859782250509E-4,0.79099492579147013,-50554.890810948862,8263.3598594740979,1.2342733333333333,5.5182119391105483E-3,12.482596414331939,11520.92529723703,-9999]
["DBL","DBL2M00080",0.8,0.83,0.72,0.83,4500,3.6480000000000001,12000,47.7,43,58,1.2999999999999999E-2,560,6,1098.9204595487065,3256.6197595059562,3886.2068965517242,0.74210453760878303,192.30769230769232,5.4356016606727415,3.3574796754576783,"NA",12.248085856069611,0,-9.9209495434163841,0,0,0,0,0,0.37218979660270884,0.52947454481967582,4.4662775592325064,12.70738907567222,8.0897751407407394,203.54900164288517,165.00539781149911,1587.3519269466215,5.3245764876220167E-3,18.136351949220067,-26360.506163348804,1098.9204595487065,3.4582874965192181E-3,3.977270164302646,-49629.574539250003,3256.6197595059562,0.83,1.2321170078074893E-2,38.765326871307693,60873.687164040603,-9999]
["DBL","DBL2H00080",0.8,1.49,0.69,1.1000000000000001,6000,3.6720000000000002,12000,14.7,13,33,1.2999999999999999E-2,560,6,3647.0569499578364,6342.6721472219178,6830.30303030303,0.68371767730093147,192.30769230769232,5.4373239950522123,3.33553536385338,2.3186115334885469,12.248085856069611,0,-9.9209495434163841,0,0,0,0,0,0.66814794811811595,0.95050249612206883,8.0177753774173919,22.812059906929651,14.522608385185183,203.54900164288517,165.00539781149911,1587.3519269466215,1.6741209138648699E-3,5.7463338757192943,-43224.730015785331,3647.0569499578364,1.1054885252680103E-3,0.96462597528829075,-50591.545842010819,6342.6721472219178,1.1480665151515153,3.7273776913905494E-3,12.202154746617929,-16624.126836453055,1035.102243448689]
["DBL","DBL3N00065",0.65,0.67,0.6,0.65,3000,2.94,9000,79,82.8,59,0.05,670,6,291.33432104264466,2988.5204377217497,3820.3389830508472,0.60019132603797076,50,6.7990734049388175,4.2273536701637893,"NA",12.42841979028154,0,-10.067020030128045,0,0,0,0,0,0.37521958217386925,0.53378469612106605,4.5026349860864308,12.810832706905586,8.1556294017094011,206.5459427733216,167.43484457593422,1610.7232048204874,8.1415721461795734E-3,24.46518514764908,-7818.5696302248543,291.33432104264466,3.697985942618877E-3,5.2789152373848038,-48803.799321783008,2988.5204377217497,0.65389039548022598,3.7235886193957839E-2,65.841120494710196,260531.60730816916,-9999]
["DBL","DBL3H00065",0.65,1.08,0.48,0.95,6000,3,9000,30.3,31,36.5,0.05,670,6,2098.9162467611077,5347.6388900428765,6175.3424657534251,0.49848356478211853,50,6.8552857274752119,4.1428065967605132,"NA",12.42841979028154,0,-10.067020030128045,0,0,0,0,0,0.60483156529519222,0.86042906240410655,7.2579787835423071,20.650297497698556,13.146387692307691,206.5459427733216,167.43484457593422,1610.7232048204874,3.0997023068686652E-3,9.5483377748366021,-33696.742986982252,2098.9162467611077,1.4010395870955772E-3,1.8837153354522798,-50139.297086692051,5347.6388900428765,0.98337497716894973,1.3626364901813815E-2,25.182715318926089,68198.246048803674,-9999]
["DBL","DBL3N00130",1.3,1,1.2,0.95,3000,5.76,9000,35.5,61,77.5,0.08,670,6,993.66315006227057,2479.7833752979263,2908.3870967741937,1.2173405541567357,31.25,3.4395312519102257,2.183096613488996,5.798446418111225,12.574636493696616,0,-10.185455559894258,0,0,0,0,0,0.2833089031339136,0.4030332209518146,3.399706837606963,9.6727973028435503,6.1578940170940157,208.97589504124306,169.40466627682758,1629.6728895830813,1.1413531023714129E-2,21.113965813619622,-32249.507455621308,993.66315006227057,6.2630573533420403E-3,4.6013373078740196,-49923.898604752001,2479.7833752979263,0.96559139784946235,1.6450688545297614E-2,29.344241821017469,-14963.972568143574,413.90397132992246]
["DBL","DBL3H00130",1.3,1.75,1.1000000000000001,1.5,6000,5.55,9000,13,22,45,0.08,670,6,2487.3381843801048,4519.0523361942051,5008.8888888888896,1.1493649221268598,31.25,3.4395312519102257,2.2657002691345256,1.4210142609836001,12.574636493696616,0,-10.185455559894258,0,0,0,0,0,0.49579058048434876,0.7053081366656756,5.9494869658121852,16.927395279976214,10.776314529914528,208.97589504124306,169.40466627682758,1629.6728895830813,4.0247777381230533E-3,7.570144560830725,-43730.210781250003,2487.3381843801048,2.1155786637554845E-3,1.6111139683695628,-50484.70466431167,4519.0523361942051,1.5900462962962962,6.1855130432054246E-3,10.91909770623049,-36085.814973060755,1688.9344927043617]
["DBL","DBL3M00190",1.9,1.5,1.6,1.32,3000,8.7629999999999999,9000,21.3,40,77,0.1,670,6,1074.7929224468467,2556.1536969530339,2927.272727272727,1.6443846303046967,25,2.4012150459629535,1.4460931525702767,2.0062543185605954,12.672114295973335,0,-10.2644125797384,0,0,0,0,0,0.29301838818623865,0.41684586499912291,3.5162206582348636,10.00430075997895,6.3689356725146204,210.59586321985731,170.71788074408983,1642.3060127581441,1.1597418816597087E-2,19.652663848384286,-34519.648263721087,1074.7929224468467,6.1521221477408164E-3,3.8990769038000299,-50164.124382621572,2556.1536969530339,1.3725584415584415,1.0733129617413538E-2,18.092468218907907,-37002.773161907884,1196.2591072311814]
["DBL","DBL3H00250",2.5,3,1.8,2.4,6000,11.536999999999999,9000,5.0999999999999996,11,50,0.14000000000000001,670,6,2693.6508557382062,4225.1327414236166,4508,2.0070678468339116,17.857142857142854,1.8479006660185668,1.1152873277738382,0.74492790495543826,12.86706990052677,0,-10.422326619426684,0,0,0,0,0,0.45224007235143793,0.64335349502633854,5.4268808682172551,15.440483880632124,9.829717333333333,213.83579957708594,173.34430967861428,1667.5722591082695,4.2167009854839343E-3,6.1146970710781732,-47066.207972894801,2693.6508557382062,2.5624054642661904E-3,1.1658399344729962,-50669.241724718806,4225.1327414236166,2.6396000000000002,3.3654230091590596E-3,4.3415203105703162,-48920.280139290546,3221.7882885506465]
["DBL","DBL3N00300",3,2.1,2.6,1.9,3000,13.87,9000,11.5,25,88,0.17,670,6,1276.6432417833648,2314.0342178030519,2561.3636363636365,2.6914621042929263,14.705882352941176,1.555821461371536,0.93823263186314698,1.3498905361804892,13.013286603941848,0,-10.540762149192895,0,0,0,0,0,0.26680451238157737,0.37955419261497059,3.2016541485789287,9.1093006227592941,5.7991608888888893,216.26575184500729,175.31413137950764,1686.5219438708634,1.2105039580304146E-2,17.018279066174461,-41455.2819533125,1276.6432417833648,7.9235795916842815E-3,3.4534177484064004,-50420.149212777367,2314.0342178030519,1.970189393939394,9.2998629594213036E-3,10.16497459643171,-47469.457890428013,1777.9219393527953]
["DBL","DBL4N00260",2.6,1.9,2.2999999999999998,1.76,3000,11.696,9000,9.5,40,82,0.21,670,6,1392.2567767897524,2502.554858435552,2748.7804878048782,2.3497445141564448,11.904761904761905,1.8170630879670882,1.129295674460951,1.3805452562855141,13.208242208495284,0,-10.698676188881178,0,0,0,0,0,0.2827049500458374,0.40217404160482434,3.3924594005500488,9.6521769985157846,6.1447667236467236,219.50568820223589,177.94056031403207,1711.7881902209886,1.5375994140163426E-2,11.532293788348614,-45860.417286556214,1392.2567767897524,7.1073091673648937E-3,2.4273488292766552,-50586.093137307013,2502.554858435552,1.7990121951219511,1.1195896998912505E-2,8.2909345213254291,-48249.404674416059,1738.4435526999123]
["DBL","DBL4H00260",2.6,3,2.2999999999999998,2.8,3000,11.18,9000,3.8,15,52,0.21,670,6,2615.4382785739972,4068.8803104740705,4334.6153846153848,2.1931119689525929,11.904761904761905,1.8170630879670882,1.1814170132822257,0.78759415045654668,13.208242208495284,0,-10.698676188881178,0,0,0,0,0,0.44637623691448014,0.63501164463919635,5.3565148429737617,15.240279471340711,9.7022632478632485,219.50568820223589,177.94056031403207,1711.7881902209886,5.4755514654001598E-3,4.4150667905253691,-49002.939700000003,2615.4382785739972,2.8312364509114839E-3,0.9459791784628947,-50722.423627395961,4068.8803104740705,2.7639743589743588,4.2717962989608418E-3,3.3206310277965772,-49785.689731623032,3047.2547296203074]
["DBL","DBL4N00530",5.3,3.2,4.5999999999999996,2.77,3000,24.75,9000,6.14,30,100,0.28000000000000003,670,6,1055.5410659037598,2042.9898387212424,2254,4.8233023709650436,8.928571428571427,0.91675814132263977,0.54745109157429483,1.3061831465155112,13.549414516463797,0,-10.975025758335676,0,0,0,0,0,0.23960880524814129,0.34086577399908924,2.8753056629776954,8.1807785759781417,5.2080453948287921,225.17557682738587,182.53681094944989,1756.0041213337079,2.487654712052445E-2,15.891991002095363,-44491.275549733007,1055.5410659037598,1.0578951800538996E-2,3.1350786742923327,-50559.442042649942,2042.9898387212424,2.9479454666666669,1.1806978728947941E-2,5.5386479284287091,-50038.244478122811,1837.4146124932408]
["DBL","DBL4H00530",5.3,6.5,4.5999999999999996,6,3000,24.3,9000,1.65,9.3000000000000007,49,0.28000000000000003,670,6,2216.763754935012,4245.0474706157411,4600.0000000000009,4.3094889235229932,8.928571428571427,0.91675814132263977,0.55758907475159658,0.63203593290644666,13.549414516463797,0,-10.975025758335676,0,0,0,0,0,0.48670538566028693,0.69238360343564997,5.8404646279234429,16.6172064824556,10.578842208245982,225.17557682738587,182.53681094944989,1756.0041213337079,8.0870991348324494E-3,4.1733461916485854,-48991.663703108316,2216.763754935012,2.6217125604729974E-3,0.82222508645628567,-50734.76702907143,4245.0474706157411,5.8715136054421766,3.1174785361076807E-3,1.4814220035563397,-50576.649884150269,3797.2524583586383]
["DBL","DBL4N00750",7.5,4.0999999999999996,6.5,3.7,3000,35.15,9000,3.8,22.6,112,0.43,670,6,1088.3007971707984,1858.8671572623571,2012.5000000000002,6.880377614245881,5.8139534883720927,0.68292986993537097,0.40627305927565244,1.3294465089962053,14.280498033539182,0,-11.567203407166737,0,0,0,0,0,0.22865151469519454,0.32527801076394802,2.7438181763423346,7.8066722583347525,4.9698819160493821,237.32533816699305,192.38591945391664,1850.7525451466781,2.650362437423711E-2,14.164790947695316,-46806.40954974667,1088.3007971707984,1.3114874841188673E-2,2.8644665493178398,-50641.632245452791,1858.8671572623571,3.8858095238095238,1.3477834741964395E-2,3.6636022469332277,-50537.661964609892,1805.2625538218253]
["DBL","DBL4H00750",7.5,9.3000000000000007,6.4,8.4,3000,34.506,9000,0.86,5.3,49,0.43,670,6,2591.6831195154459,4355.8322810661357,4600.0000000000009,5.9028614969424176,5.8139534883720927,0.68433140294924677,0.4138555043626958,0.56988741048744895,14.280498033539182,0,-11.567203407166737,0,0,0,0,0,0.51864855772324625,0.73782573173285781,6.223782692678955,17.707817561588588,11.273146785185185,237.32533816699305,192.38591945391664,1850.7525451466781,6.2076710937708952E-3,3.1229962430446174,-49789.634642433281,2591.6831195154459,2.5391796646121695E-3,0.59500532403349704,-50768.297095415641,4355.8322810661357,8.1520285714285716,2.6652427447149294E-3,0.82281143853018179,-50734.66659481715,4211.3581662510805]
["DBL","DBL4N00950",9.5,6.1,8,5.6,3000,42.625,9000,1.61,10,94,0.65,670,6,1619.7176018609425,2281.7926350816037,2397.8723404255315,8.3591036824591978,3.8461538461538458,0.5818328765217925,0.36018190870576133,1.0576913388515867,15.352753858583077,0,-12.435730625452292,0,0,0,0,0,0.28873581174351659,0.41075350235682789,3.4648297409221991,9.8580840565638699,6.2758512280701737,255.14498813175015,206.8312785938011,1989.7169000723666,1.4381008959703933E-2,7.1743899582798347,-49348.848567409848,1619.7176018609425,9.0825076110847055E-3,1.5126868066171379,-50740.4185622761,2281.7926350816037,5.7707819148936164,9.1275454637988369E-3,1.6450799030357612,-50728.590062036783,2269.0929875684305]
["DBL","DBL5N01050",10.5,6.5,8.5,5.7,3000,48,9000,2.25,19.8,97,0.81,670,6,1014.5300609720957,2095.6223830234935,2323.7113402061859,9.1029184113176704,3.0864197530864197,0.55595187477603958,0.33609533909993378,1.1553957105024342,16.132576276796822,0,-13.067386784205427,0,0,0,0,0,0.29250676877829446,0.41611803888563231,3.5100812253395333,9.986832933255176,6.3578153086419755,268.10473356066456,217.33699433189901,2090.7818854728685,3.5031528165451201E-2,11.232596922913823,-47452.7518367347,1014.5300609720957,1.0454663088419407E-2,2.2691597629959861,-50668.347213572117,2095.6223830234935,6.0027491408934708,1.0582024828950628E-2,2.4033819072410756,-50651.683419277986,2077.2104121421212]
["DBL","DBL5H01050",10.5,14.1,8.5,13,3000,52.54,9000,0.52,4.5,45,0.81,670,6,2145.3292999478244,4626.7673505539351,5008.8888888888896,7.4154884329640431,3.0864197530864197,0.55595187477603958,0.30705322186518502,0.52534631288178257,16.132576276796822,0,-13.067386784205427,0,0,0,0,0,0.63451468304214653,0.90265605358267942,7.6141761965057579,21.663745285984305,13.791568592592593,268.10473356066456,217.33699433189901,2090.7818854728685,9.4864941083723058E-3,2.8595412566499929,-49795.656765619337,2145.3292999478244,2.2617194861894916E-3,0.50933142385023178,-50773.133024775154,4626.7673505539351,12.56677925925926,2.3101105998382244E-3,0.55897212193153267,-50766.585946531282,4568.4150457530022]
["DBL","DBL5N01350",13.5,8.6999999999999993,10.7,7.3,3000,62,9000,1.71,16.5,94,0.91,670,6,946.92001782914576,2138.6162129591667,2397.8723404255315,11.503958201238111,2.7472527472527473,0.44664252808821603,0.2680639562609744,1.0995612122889404,16.619965288180413,0,-13.462171883426134,0,0,0,0,0,0.31370665512649892,0.44627684570114062,3.7644798615179873,10.710644296827375,6.8186079341563781,276.20457445373597,223.9030666682101,2153.947501348181,4.1008384057811431E-2,11.12402010137558,-47304.033268000007,946.92001782914576,1.0063112555187863E-2,2.1725127932486257,-50671.620733453237,2138.6162129591667,7.8032900709219852,9.7729584584851908E-3,1.8983675903965269,-50703.196455741629,2182.6888518593296]
["DBL","DBL5H01350",13.5,18.600000000000001,10.7,15.7,3000,62.05,9000,0.38,3.1,44,0.91,670,6,2479.7365626435808,4836.0835765922457,5122.727272727273,8.9863219951805693,2.7472527472527473,0.44664252808821603,0.2678479498498052,0.49663618015182237,16.619965288180413,0,-13.462171883426134,0,0,0,0,0,0.67068319371872198,0.95410911839554247,8.0481983246246642,22.898618841493018,14.577713514403294,276.20457445373597,223.9030666682101,2153.947501348181,7.1350778384935646E-3,2.4758131312281417,-50013.624532442969,2479.7365626435808,2.0847419120649199E-3,0.41876596969927887,-50782.514734326171,4836.0835765922457,14.460206060606058,2.0871691665396725E-3,0.422168972576973,-50782.145196099344,4832.5113954974377]
["DBL","DBL5N01700",17,10.4,14,9.1,3000,78.72,9000,1.25,12.6,99,1.1299999999999999,670,6,1008.370973984159,2065.7312100652111,2276.7676767676771,14.934268789934789,2.2123893805309738,0.37576355919926657,0.22474874381636573,1.1197936774640813,17.69222111322431,0,-14.330699101711689,0,0,0,0,0,0.31701142326595888,0.45097818523905103,3.8041370791915066,10.823476445737224,6.8904391111111112,294.02422441849308,238.34842580809465,2292.9118562738704,3.7055681155040154E-2,10.322272936996173,-48087.342466435992,1008.370973984159,1.0884306084657954E-2,2.0579289501345968,-50697.133483221049,2065.7312100652111,9.6011784511784519,1.0358950791086641E-2,1.4769055900793917,-50749.521541628208,2143.2519653398231]
["DBL","DBL5H01700",17,20,14,17.3,3000,78.260000000000005,9000,0.36,3.3,52,1.1299999999999999,670,6,2138.0730817377889,4071.4304577411681,4334.6153846153848,12.928569542258831,2.2123893805309738,0.37576355919926657,0.22606978166655134,0.57832617266101727,17.69222111322431,0,-14.330699101711689,0,0,0,0,0,0.60963735243453632,0.86726574084432884,7.3156482292144354,20.814377780263893,13.250844444444445,294.02422441849308,238.34842580809465,2292.9118562738704,9.5373037198183477E-3,2.9852959351416128,-49981.196259211079,2138.0730817377889,2.9299174023572996E-3,0.54280878822465661,-50777.918748097829,4071.4304577411681,16.740961538461541,2.8455389599213966E-3,0.4296452625685504,-50788.093149810695,4149.9072901318386]
["DBL","DBL5N02200",22,13.7,17,11.3,3000,100.8,9000,0.94,9,97,1.31,670,6,1067.1020569071663,2127.2121039751146,2323.7113402061859,18.45464649337481,1.9083969465648853,0.3071738714166995,0.1842214418027259,1.0787244889898164,18.569521333714771,0,-15.041312280308965,0,0,0,0,0,0.3386933978496327,0.48182280733312949,4.0643207741955925,11.563747375995108,7.3617102222222215,308.60393802602169,250.16735601345474,2406.6099648494346,3.3033512994437991E-2,9.9133087769103838,-48193.998056478682,1067.1020569071663,1.0300511507325364E-2,1.9257534209875415,-50706.623326643501,2127.2121039751146,12.193839175257732,9.7339402157032764E-3,1.162623062433801,-50769.245121019696,2224.8498337582996]
["DBL","DBL6N02200",22,15.1,16,12,3000,101.61599999999999,9000,0.72,8.5,88,2.5099999999999998,670,6,1095.6644183813385,2342.837273936002,2561.3636363636365,17.314325452127996,0.99601593625498019,0.40680340326523634,0.24029866822466789,1.0016354604464737,24.418189470317849,0,-19.778733470957459,0,0,0,0,0,0.49088059161872449,0.69832322159431726,5.8905670994246941,16.759757318263613,10.669592888888888,405.80202874287892,328.96022404918853,3164.5973553531935,3.3759464464858925E-2,7.6540652075951332,-48913.866282214673,1095.6644183813385,8.6383995562094584E-3,1.419195264514346,-50740.138202517439,2342.837273936002,12.932019696969697,8.3528279161831694E-3,1.1709103494294295,-50760.898925413196,2396.0813038010983]
["DBL","DBL6N02900",29,17.5,20,13.5,3000,133.65,9000,0.55000000000000004,6.5,100,3.82,670,6,1154.714519144738,2111.5371020338871,2254,22.66538869389834,0.65445026178010479,0.39161609877898862,0.23047501323937802,1.1151485015716609,30.802985519442874,0,-24.950418270748727,0,0,0,0,0,0.54442868340810058,0.77450035429633657,6.5331442008972074,18.588008503112079,11.833493742017877,511.90994444211469,414.97577165486456,3992.0669233197968,3.0342566754982293E-2,7.6830264927722824,-49329.437597783981,1154.714519144738,1.0705706249520464E-2,1.4310059434566766,-50753.965549744797,2111.5371020338871,15.021666666666667,1.0437939071191664E-2,1.1272916815722827,-50773.390336616452,2152.1797290831701]
["DBL","DBL7N02600",26,17,20,14.1,3000,116.28,9000,0.46,4.5,92.5,9.74,670,6,1547.1108643049336,2327.5414128885577,2436.7567567567567,21.344917174222886,0.25667351129363447,0.83546213764335819,0.51304106461430499,1.0819628185927828,59.65641499335139,0,-48.32169614461462,0,0,0,0,0,1.142459623335363,1.6252548956522015,13.709515480024356,39.006117495652838,24.83206564102564,991.42052531194349,803.6872539644844,7731.4713831383397,1.7220824282653806E-2,5.6032601730168201,-49887.803548093019,1547.1108643049336,8.8952535816080678E-3,1.1083305822272547,-50769.268205127832,2327.5414128885577,15.03865945945946,9.4805474002664387E-3,1.8300924922208848,-50707.300583489174,2218.1908275937581]
["DBL","DBL7N03200",32,20,23,15.8,3000,143.68,9000,0.36,3.6,97,11.41,670,6,1557.0138027779988,2235.1930033954509,2323.7113402061859,25.294420989813649,0.21910604732690622,0.77754951103319248,0.47185280820891801,1.1104891437093274,67.795811483457342,0,-54.914607301600448,0,0,0,0,0,1.2410549649637981,1.7655159240483682,14.892659579565578,42.372382177160837,26.975096296296293,1126.6878682262366,913.34066198088067,8786.3371682560719,1.7145039590367294E-2,5.4313926351874064,-50021.335312000003,1557.0138027779988,9.6955282738817906E-3,1.0452871198052334,-50776.128616143302,2235.1930033954509,17.282268041237113,1.0107058818307637E-2,1.6315405273627479,-50734.4318542771,2161.2097818294428]
["DBL","DBL7N04000",40,23.4,26,17,3000,160.74,9000,0.3,2.9,103.5,13.94,670,6,1610.5407080689699,2106.1333219633416,2177.7777777777778,30.171377830837738,0.1793400286944046,0.74320925210740008,0.49848670817134588,1.1694528027121964,80.126753471462138,0,-64.902670311884336,0,0,0,0,0,1.3729083560078019,1.9530896158668893,16.474900272093624,46.874150780805344,29.841011199999986,1331.6138428209438,1079.4622920895524,10384.427249901495,1.6216734646880525E-2,5.0571060598934992,-50208.312425937329,1610.5407080689699,1.0949331165942388E-2,1.0495237160805464,-50779.453448374166,2106.1333219633416,19.515066022544282,1.1266600030681688E-2,1.6048548813539698,-50745.052198412901,2052.2418642581529]
["DBL","DBL8N04000",40,23,32,20,3000,139.19999999999999,9000,0.35,7.5,105,7.11,670,6,1088.5369729447914,1932.1546059584409,2146.6666666666665,34.847587717444156,0.35161744022503516,0.42432959304214962,0.33648048846237771,1.2048265107756182,46.838083993962975,0,-37.938848035110006,0,0,0,0,0,0.78881489261236037,1.1221624290220296,9.4657787113483245,26.931898296528711,17.145378962962962,778.39470982416492,630.9995515195011,6070.2156856176007,3.769958647680717E-2,5.0947754889396242,-50216.571853000001,1088.5369729447914,1.2898958028106644E-2,1.3503804217400182,-50763.810174979168,1932.1546059584409,21.214761904761904,1.224898955862958E-2,1.0913525298486355,-50778.152055682382,1991.9880402158296]
["DBL","DBL8N06800",68,37,50,28.6,3000,259,9000,0.12,3.4,112,11.36,670,6,1254.352979043704,1916.8652924788701,2012.5000000000002,56.498808245126781,0.22007042253521128,0.363644806751028,0.26081898447013724,1.2276204326635509,67.55211697776555,0,-54.717214751990085,0,0,0,0,0,1.0765641428218971,1.531512455991008,12.918769713862766,36.756298943784195,23.399786666666664,1122.6379477797011,910.05762581272484,8754.7543603184131,2.9538327907066585E-2,3.2805938886360808,-50590.669082785469,1254.352979043704,1.3432513975299211E-2,0.75012321481703048,-50793.945777315705,1916.8652924788701,32.223500000000001,1.3012535647577147E-2,0.54471808464110605,-50799.246459826711,1955.0016732718871]
["DBL","DBL8L09300",93,34,70,32,2000,319.77999999999997,6000,0.16,4.4000000000000004,164,15.3,670,6,987.16930256412013,1310.2696002034775,1374.3902439024391,77.931899597660006,0.16339869281045752,0.34726070185339991,0.27129665403176872,1.7870417807818741,86.755244026278987,0,-70.271747661285971,0,0,0,0,0,0.92896604413452455,1.3215404555974397,11.147592529614295,31.716970934338555,20.191650816407805,1441.7716789667154,1168.7608758633842,11243.479625805756,4.6482683024047539E-2,5.3133903752165814,-50542.740706429919,987.16930256412013,2.8441616294781855E-2,1.4925954762428031,-50784.452076371024,1310.2696002034775,32.841097560975612,2.7480265195241011E-2,0.91769060429505578,-50797.332106956324,1343.0016163080093]
["DBL","DBL8L11500",115,43,85,32.5,2000,395.66,6000,0.11,3.9,164,19,670,6,947.08964683714476,1316.5504520723864,1374.3902439024391,95.2517432189142,0.13157894736842105,0.34030592836628337,0.26484516364421928,1.7874288216884284,104.7886374474718,0,-84.878796332452154,0,0,0,0,0,1.1476063539989687,1.6325765979135101,13.771276247987625,39.181838349924242,24.94393301127214,1741.4657920103584,1411.7055523068964,13580.607413192343,5.1537988275487841E-2,4.6226383980461767,-50606.535801614642,947.08964683714476,2.8428424039033721E-2,1.1527669778939784,-50792.808054493951,1316.5504520723864,36.893033536585364,2.7596519269091638E-2,0.77940303406276668,-50799.513536868813,1342.7108094480254]
["AKMH","AKMH21C",0.317,1.33,0.255,0.85,8000,1.39,8000,13,19,19.5,1.0699999999999999E-2,675,6,5094.0240573600786,8000,8000,0.255,233.64485981308411,13.718979794383719,8.8035078480631572,"NA",12.236875908807788,0,-9.9118694861343091,0,0,0,0,0,1.5037341763834762,2.1392014929961038,18.044810116601713,51.340835831906489,32.684591220469677,203.36270530234452,164.85437814776398,1585.8991177814896,1.2890798205684537E-3,2.5606237543721759,-46494.315811009168,5094.0240573600786,3.9657697383858073E-4,0.34320794598074211,-50727.716414080001,10885.465540819092,0.78166153846153841,2.8926845821040315E-2,14.350982958782941,84599.647286836553,-9999]
["AKMH","AKMH22C",0.63300000000000001,1.18,0.4,0.65573769999999998,8000,2.65,8000,20,35.5,39,1.61E-2,675,6,2617.4048744979032,5265.6705389884537,5779.4871794871797,0.4796373455519613,155.27950310559007,6.9535658630239361,4.6276207228009447,"NA",12.263194915422503,0,-9.9331878814922252,0,0,0,0,0,0.66956086852493835,0.95251250659548126,8.0347304222992602,22.860300158291551,14.553319083026151,203.80009671057039,165.20894605392476,1589.3100610387562,3.7974916272172253E-3,6.6738954861120785,-43484.173648989621,2617.4048744979032,1.5950834046424515E-3,1.2039455312814635,-50566.914628157036,5265.6705389884537,0.89115163663461527,2.1278947071692533E-2,19.661528695039138,12734.568899711943,-9999]
["AKMH","AKMH22E",0.65400000000000003,2.31,0.41,1.28125,8000,2.68,8000,5.24,9.6999999999999993,20.399999999999999,1.61E-2,675,6,6069.5645354160179,8000,8000,0.41,155.27950310559007,6.7322266224298239,4.5758189982919779,1.1574334628291092,12.263194915422503,0,-9.9331878814922252,0,0,0,0,0,1.2686621945566019,1.8047897715740306,{"$f":"IF(move1,IF(AccType=1,SQRT((X182^2*time1+Y182^2*time2+Z182^2*time3+AA182^2*time4)/time)/(C182/D182),SQRT((((X182-Y182)*2/PI()+Y182)^2*time1+Y182^2*time2+((Z182-AA182)*2/PI()+AA182)^2*time3+AA182^2*time4)/time)/(C182/D182)),IF(AccType=1,SQRT((X182^2*time1+Y182^2*time2+Z182^2*time3+AA182^2*time4+AB182^2*time5+AC182^2*time6+AD182^2*time7+AE182^2*time8)/time)/(C182/D182),SQRT((((X182-Y182)*2/PI()+Y182)^2*time1+Y182^2*time2+((Z182-AA182)*2/PI()+AA182)^2*time3+AA182^2*time4+((AB182-AC182)*2/PI()+AC182)^2*time5+AC182^2*time6+((AD182-AE182)*2/PI()+AE182)^2*time7+AE182^2*time8)/time)/(C182/D182)))","v":15.223946334679223},43.314954517776734,27.575156485219164,203.80009671057039,165.20894605392476,1589.3100610387562,1.040243252813512E-3,1.7526334950943647,-48959.881640639003,6069.5645354160179,4.2543415772550505E-4,0.21365205870716597,-50777.738333940186,10676.762560495665,1.1539447089460786,5.7120682036224954E-3,5.1055210068254926,-35146.311990138172,2073.5533204074568]
["AKMH","AKMH23D",0.89700000000000002,1.89,0.57999999999999996,1.1153846199999999,8000,3.75,8000,8.7899999999999991,17.3,33.799999999999997,2.1600000000000001E-2,675,6,{"$f":"IF(AQ183<I183,IF(AQ183<0,0,AQ183),I183)","v":3591.8476468360468},{"$f":"IF(AU183<I183,IF(AU183<0,0,AU183),I183)","v":6249.7396399388699},{"$f":"IF(UAC_V*0.98/L183*1000<I183,IF(UAC_V*0.98/L183*1000<0,0,UAC_V*0.98/L183*1000),I183)","v":6668.6390532544392},{"$f":"C183+(E183-C183)/G183*Q183","v":0.64935406676742224},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M183,(inertia/gear^2+gear_inertia)/M183),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M183,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M183))","v":115.74074074074073},{"$f":"IF((C183+(E183-C183)/G183*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X183^2*time1+Y183^2*time2+Z183^2*time3+AA183^2*time4)/time)/(C183+(E183-C183)/G183*mspeed),SQRT((((X183-Y183)*2/PI()+Y183)^2*time1+Y183^2*time2+((Z183-Y183)*2/PI()+Y183)^2*time3+AA183^2*time4)/time)/(C183+(E183-C183)/G183*mspeed)),IF(AccType=1,SQRT((X183^2*time1+Y183^2*time2+Z183^2*time3+AA183^2*time4+AB183^2*time5+AC183^2*time6+AD183^2*time7+AE183^2*time8)/time)/(C183+(E183-C183)/G183*mspeed),SQRT((((X183-Y183)*2/PI()+Y183)^2*time1+Y183^2*time2+((Z183-Y183)*2/PI()+Y183)^2*time3+AA183^2*time4+((AB183-AC183)*2/PI()+AC183)^2*time5+AC183^2*time6+((AD183-AC183)*2/PI()+AC183)^2*time7+AE183^2*time8)/time)/(C183+(E183-C183)/G183*mspeed))))","v":4.9135976358378697},{"$f":"IF(move1,MAX(ABS(X183),ABS(Z183))/H183,MAX(ABS(X183),ABS(Z183),ABS(AB183),ABS(AD183))/H183)","v":3.2773336829462933},{"$f":"IF(AZ183>0,speed/(MIN(AZ183,I183)),\"NA\")","v":1.4134612470957963},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M183+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M183+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.2900013110486},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M183+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M183+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-9.9549010619493661},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M183+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M183+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M183+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M183+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"AH183/Irms","v":0.7584543141047525},{"$f":"AI183/Ipeak","v":1.0789716870067749},9.1014517692570305,{"$f":"IF(move1,MAX(ABS(X183),ABS(Z183))/(C183/D183),MAX(ABS(X183),ABS(Z183),ABS(AB183),ABS(AD183))/(C183/D183))","v":25.8953204881626},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X183),ABS(Z183))/(C183/D183),MAX(ABS((X183-Y183)*2/PI()+Y183),ABS((Z183-Y183)*2/PI()+Y183))/(C183/D183)),IF(AccType=1,MAX(ABS(X183),ABS(Z183),ABS(AB183),ABS(AD183))/(C183/D183),MAX(ABS((X183-Y183)*2/PI()+Y183),ABS((Z183-Y183)*2/PI()+Y183),ABS((AB183-AC183)*2/PI()+AC183),ABS((AD183-AC183)*2/PI()+AC183))/(C183/D183)))","v":16.485473034559643},{"$f":"IF((C183+(E183-C183)/G183*mspeed)<0,\"NA\",U183*(C183+(E183-C183)/G183*mspeed)*mspeed/9.55)","v":204.24558795968932},{"$f":"IF(move1,IF(speed1>speed2,AM183/2*time1/time,AM183/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z183*-speed/30*PI(),((Z183-AA183)*2/PI()+AA183)*-speed/30*PI()),IF(AccType=1,X183*-speed/30*PI(),((X183-Y183)*2/PI()+Y183)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z183*-speed/30*PI(),((Z183-AA183)*2/PI()+AA183)*-speed/30*PI()),IF(AccType=1,X183*-speed/30*PI(),((X183-Y183)*2/PI()+Y183)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD183*-speed/30*PI(),((AD183-AE183)*2/PI()+AE183)*-speed/30*PI()),IF(AccType=1,AB183*-speed/30*PI(),((AB183-AC183)*2/PI()+AC183)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD183*-speed/30*PI(),((AD183-AE183)*2/PI()+AE183)*-speed/30*PI()),IF(AccType=1,AB183*-speed/30*PI(),((AB183-AC183)*2/PI()+AC183)*-speed/30*PI()),0)/2*time7/time)))","v":165.57008003242188},{"$f":"IF(move1,MAX(IF(AccType=1,Z183*-speed/30*PI(),((Z183-AA183)*2/PI()+AA183)*-speed/30*PI()),IF(AccType=1,X183*-speed/30*PI(),((X183-Y183)*2/PI()+Y183)*-speed/30*PI()),0),MAX(IF(AccType=1,Z183*-speed/30*PI(),((Z183-AA183)*2/PI()+AA183)*-speed/30*PI()),IF(AccType=1,X183*-speed/30*PI(),((X183-Y183)*2/PI()+Y183)*-speed/30*PI()),IF(AccType=1,AD183*-speed/30*PI(),((AD183-AE183)*2/PI()+AE183)*-speed/30*PI()),IF(AccType=1,AB183*-speed/30*PI(),((AB183-AC183)*2/PI()+AC183)*-speed/30*PI()),0))","v":1592.7841699118985},{"$f":"(L183^2)/1000000+((K183/1000)^2*(D183/C183*H183)^2*PI()*PI()*(O183/2)^2)/1200","v":2.5255428389403568E-3},{"$f":"SQRT(3)*L183*J183*D183/C183*H183/1000","v":4.065994918759702},{"$f":"0.75*J183^2*(D183/C183*H183)^2-(UAC_V*0.98)^2","v":-47187.395679908856},{"$f":"-AO183/2/AN183+SQRT((AO183/2/AN183)^2-AP183/AN183)","v":3591.8476468360468},{"$f":"(L183^2)/1000000+((K183/1000)^2*AV183^2*PI()*PI()*(O183/2)^2)/1200","v":1.1844800422913973E-3},{"$f":"SQRT(3)*L183*J183*AV183/1000","v":0.70887745983371131},{"$f":"0.75*J183^2*AV183^2-(UAC_V*0.98)^2","v":-50695.196401679677},{"$f":"-AS183/2/AR183+SQRT((AS183/2/AR183)^2-AT183/AR183)","v":6249.7396399388699},{"$f":"D183+(F183-D183)*((0.85*UAC_V-D183*J183)/L183*1000)/G183","v":1.3775423667880102},{"$f":"(L183^2)/1000000+((K183/1000)^2*AJ183^2*PI()*PI()*(O183/2)^2)/1200","v":7.1632655182880508E-3},{"$f":"SQRT(3)*L183*J183*AJ183/1000","v":8.4833545091932319},{"$f":"0.75*J183^2*AJ183^2-(UAC_V*0.98)^2","v":-35056.564071844223},{"$f":"IF(((AX183/2/AW183)^2-AY183/AW183)>0,-AX183/2/AW183+SQRT((AX183/2/AW183)^2-AY183/AW183),-9999)","v":1697.9595336845778}]
["AKMH","AKMH23E",0.90400000000000003,2.36,0.57999999999999996,1.3809523800000001,8000,3.78,8000,5.46,11.1,27,2.1600000000000001E-2,675,6,4759.6458331260937,7967.3670752164326,8000,0.58132163345373444,115.74074074074073,4.8769562038333198,3.2513230981610057,0.95861728004667868,12.2900013110486,0,-9.9549010619493661,0,0,0,0,0,0.93973118100308606,1.3368548623743868,11.276774172037033,32.084516696985283,20.425637716158636,204.24558795968932,165.57008003242188,1592.7841699118985,1.6171323941706118E-3,2.5197207159359865,-48627.864908670454,4759.6458331260937,7.5041319462648042E-4,0.39124993934506958,-50752.664624472731,7967.3670752164326,1.5322768810290373,4.5340311432295602E-3,5.2154604800697166,-41476.961090819947,2503.6060270926214]
["AKMH","AKMH23F",0.91700000000000004,3.71,0.59,2.1851851899999999,8000,3.8,8000,2.36,4.68,17.600000000000001,2.1600000000000001E-2,675,6,7718.2766129457559,8000,8000,0.59,115.74074074074073,4.8073161016077881,3.2342108713285791,0.5509835052748705,12.2900013110486,0,-9.9549010619493661,0,0,0,0,0,1.4563462396241384,2.071787752816717,17.476154875489662,49.722906067601208,31.654585142210912,204.24558795968932,165.57008003242188,1592.7841699118985,6.9296313733870345E-4,1.106046711138674,-49817.831643190962,7718.2766129457559,3.1437746685214165E-4,0.12141178212498729,-50793.26303070219,12519.298633911632,1.6876233891721304,1.9342833842414453E-3,2.2773087995825216,-46619.552296732967,4355.8472749609919]
["AKMH","AKMH24D",1.1200000000000001,2.41,0.83,1.3174603199999999,8000,4.68,8000,9.0399999999999991,18.7,40.799999999999997,2.7E-2,675,6,2560.2627987431292,5052.2002620216472,5524.5098039215691,0.93685774050171533,92.592592592592595,3.9223511825996962,2.6316923755690844,1.6954170868397793,12.316320317663314,0,-9.976219457307284,0,0,0,0,0,0.7762259022776089,1.104253421338117,9.3147108273313073,26.50208211211481,16.87174948148148,204.68297936791518,165.92464793858267,1596.1951131691653,4.2896681669379755E-3,6.4333042936442517,-44589.491126456538,2560.2627987431292,1.7511870934003935E-3,1.1681358525505576,-50600.229599130442,5052.2002620216472,1.8285386000133332,9.0328917895980149E-3,10.778276960861582,-33358.256428501118,1415.5808730661952]
["AKMH","AKMH24E",1.1200000000000001,2.41,0.83,1.66,8000,4.72,8000,5.46,11.8,32.4,2.7E-2,675,6,4110.8044111403251,6573.1834377354771,6956.7901234567908,0.88172210038208898,92.592592592592595,3.9223511825996962,2.6093898978100243,0.87158382708087401,12.316320317663314,0,-9.976219457307284,0,0,0,0,0,0.7762259022776089,1.104253421338117,9.3147108273313073,26.50208211211481,16.87174948148148,204.68297936791518,165.92464793858267,1596.1951131691653,2.1129406418444094E-3,3.1119979254913699,-48498.792094892502,4110.8044111403251,1.0862812017594745E-3,0.57677748438985843,-50725.934208747931,6573.1834377354771,1.8823917824074075,3.9836596802414366E-3,5.169617352844269,-44440.623445256875,2753.6077717712224]
["AKMH","AKMH24F",1.1299999999999999,3.38,0.84,2.3333333299999999,8000,4.74,8000,2.96,6.16,23.4,2.7E-2,675,6,5949.3181936822521,8000,8000,0.84,92.592592592592595,3.8871298995791324,2.5983798138530196,0.58196794941911212,12.316320317663314,0,-9.976219457307284,0,0,0,0,0,1.0790147158455243,1.5349986236615782,12.948176590146293,36.839966967877878,23.453051385119632,204.68297936791518,165.92464793858267,1596.1951131691653,1.1121791840143496E-3,1.7009235504694538,-49484.235843495873,5949.3181936822521,5.629776086978574E-4,0.28107064401706827,-50769.0905706552,9249.9453511736065,2.3428651533921792,2.092533886534311E-3,2.8136336602371768,-47190.700226632856,4123.9384443688796]
["AKMH","AKMH31C",1,1.29,0.82,0.96470588000000002,6000,3.8,8000,21.4,37.5,54.5,3.3000000000000002E-2,675,8,1818.9415504061485,3627.0010828321901,4135.7798165137619,0.89118996751503432,75.757575757575751,4.3986945888573441,3.2488325416700867,4.8549430008804872,12.345563658346329,0,-9.9999065632605255,0,0,0,0,0,0.46645394356483205,0.66357404663611519,5.5974473227779846,15.925777119266765,10.138664604444443,205.16896982149947,166.31861227876132,1599.985050121684,7.4170503511531453E-3,9.9024853803648831,-42551.711914120009,1818.9415504061485,3.2036207926418548E-3,2.2685253927360063,-50372.014014183318,3627.0010828321901,1.1229818624364527,2.199252826394206E-2,20.481023668285193,-15499.013168852944,494.34154006849076]
["AKMH","AKMH31E",1.04,2.76,0.74,1.8048780499999999,8000,3.92,8000,4.76,8.6,26.1,3.3000000000000002E-2,675,8,4706.9592971846423,8000,8000,0.74,75.757575757575751,4.2412749637760756,3.1493784842720229,0.94111301447844142,12.345563658346329,0,-9.9999065632605255,0,0,0,0,0,0.95961008067899234,1.3651344429902188,11.515320968147908,32.763226631765249,20.857717880341873,205.16896982149947,166.31861227876132,1599.985050121684,1.7345267829895459E-3,2.2385659686787025,-48966.087762317635,4706.9592971846423,7.173063615415297E-4,0.41440225417143445,-50742.136399251933,8126.7967573881124,1.9258125905427201,4.915386547692452E-3,4.488227644232845,-43412.363583896338,2550.1719379898959]
["AKMH","AKMH31H",1.08,5.59,0.76,3.6190476199999999,8000,3.98,8000,1.31,2.4,13.7,3.3000000000000002E-2,675,8,8000,8000,8000,0.76,75.757575757575751,4.0860275871575666,3.101900416669932,0.44544080059419217,12.345563658346329,0,-9.9999065632605255,0,0,0,0,0,1.8715744649206221,2.6624884587251532,22.458893579047466,63.899723009403679,40.679827116598069,205.16896982149947,166.31861227876132,1599.985050121684,5.0935456003155808E-4,0.64035914287776985,-50258.967033050307,9324.6423848780141,1.9137863653210933E-4,6.8573282509906824E-2,-50798.896620126034,16114.054418299338,2.2059844607071355,1.4420412373284393E-3,1.2645371384105073,-48675.246080212804,5387.921350712686]
["AKMH","AKMH32C",1.72,1.3,1.57,1.12142857,3000,6.84,8000,23.8,46.5,89.8,5.8999999999999997E-2,675,8,1089.5301282670614,2188.4669591407501,2510.0222717149222,1.6105766520429625,42.372881355932208,2.5825311266889499,1.8234334504833427,2.6308637835914239,12.472284801306063,0,-10.10255068905791,0,0,0,0,0,0.27610168705432381,0.39278028686283628,3.3132202446518857,9.4267268847080707,6.0012407235142122,207.27492845369801,168.02579108620222,1616.4081102492655,1.5668815573745158E-2,19.13748785975347,-39450.942957977284,1089.5301282670614,8.4676024497336716E-3,4.4085635138629202,-50202.626026465543,2188.4669591407501,1.1909216239020044,1.8311741889793808E-2,22.215442528374211,-35504.954187172378,912.24791453236355]
["AKMH","AKMH32E",1.77,2.56,1.1000000000000001,1.5068493199999999,7000,7.04,8000,6.32,12.8,47.1,5.8999999999999997E-2,675,8,2735.8950346437082,4473.6996390829281,4785.5626326963911,1.3418030345449199,42.372881355932208,2.5386250424187171,1.7716313638218839,0.95492954439361721,12.472284801306063,0,-10.10255068905791,0,0,0,0,0,0.52834895629621836,0.75162544941957454,6.3401874755546208,18.039010786069788,11.483990940364093,207.27492845369801,168.02579108620222,1616.4081102492655,4.4537167907113609E-3,5.2497421263607684,-47699.355347874509,2735.8950346437082,2.3035516428352868E-3,1.0245671210690841,-50686.861558145727,4473.6996390829281,1.9872010237848226,5.0618502302574994E-3,5.9209508224500285,-46854.395866919142,2513.2744233230383]
["AKMH","AKMH32H",1.82,4.92,0.95,2.4358974400000002,8000,7.18,8000,1.71,3.53,24.8,5.8999999999999997E-2,675,8,5815.1361535417846,8000,8000,0.95,42.372881355932208,2.4753869469240826,1.7370870196805104,0.43796895517799611,12.472284801306063,0,-10.10255068905791,0,0,0,0,0,0.98752447866800919,1.4048452660811774,11.85029374401611,33.716286385948258,21.464454564102564,207.27492845369801,168.02579108620222,1616.4081102492655,1.2328062965436394E-3,1.4256948394533626,-49978.951226894213,5815.1361535417846,6.2593433859671119E-4,0.18932802595758652,-50790.58976822118,8858.0095330482563,2.5775463769041935,1.3705280632642942E-3,1.5766245167463373,-49794.760324041687,5479.8404581544137]
["AKMH","AKMH33C",2.25,1.27,2.14,1.1505376300000001,2000,9.68,8000,26.6,53.6,120,8.5000000000000006E-2,675,8,718.47088894984131,1623.7308567924947,1878.3333333333335,2.1606948028764128,29.411764705882351,1.9900481770539327,1.3015502008539046,2.6915885408486635,12.599005944265796,0,-10.205194814855295,0,0,0,0,0,0.2082886567797633,0.29630995461514004,2.4994638813571597,7.1114389107633604,4.5272826205761314,209.38088708589663,169.73296989364314,1632.831170376847,2.5686549267685453E-2,30.207867674181582,-34962.881016998879,718.47088894984131,1.4934932939053082E-2,6.5764140692136124,-50054.30545121961,1623.7308567924947,1.18950326853475,2.2148957423603698E-2,25.030015392844085,-39928.394886006739,891.66674756434918]
["AKMH","AKMH33E",2.3199999999999998,2.2000000000000002,1.82,1.6545454500000001,4500,9.8800000000000008,8000,9.0299999999999994,18.5,70.599999999999994,8.5000000000000006E-2,675,8,1749.0626447946142,2938.0135401903694,3192.6345609065161,1.993554051089959,29.411764705882351,1.9508907638490418,1.2752030307961331,1.1982858964558181,12.599005944265796,0,-10.205194814855295,0,0,0,0,0,0.34992833663447881,0.49780555095877793,4.1991400396137459,11.94733322301067,7.605908556832695,209.38088708589663,169.73296989364314,1632.831170376847,8.937709586860642E-3,10.34533883045432,-45437.066828714924,1749.0626447946142,5.1466841912059707E-3,2.0963014423344033,-50584.746559902713,2938.0135401903694,1.8984565173600882,7.5898183692389987E-3,8.3985474158361999,-47267.313681914588,2002.8609258429092]
["AKMH","AKMH33H",2.38,4.78,0.88,1.69230769,8000,10.1,8000,1.98,4.0999999999999996,33.4,8.5000000000000006E-2,675,8,4407.5657999228006,6569.4607315660251,6748.5029940119757,1.1482261128313702,29.411764705882351,1.9292123346151526,1.2474263311154254,0.48745761964521711,12.599005944265796,0,-10.205194814855295,0,0,0,0,0,0.74113164284601163,1.0543285786693015,8.8935797141521391,25.303885888063238,16.108954074074074,209.38088708589663,169.73296989364314,1632.831170376847,2.0257893228701127E-3,2.3235102772473386,-49595.296790384651,4407.5657999228006,1.130863508011878E-3,0.30127610245397984,-50784.818805911418,6569.4607315660251,2.6302219629257633,1.6895983165769214E-3,1.8451837778164646,-50042.156850479347,4923.5049433564609]
["AKMH","AKMH41C",1.85,1.39,1.68,1.2537313400000001,3000,5.65,6000,21.3,66.099999999999994,86.3,8.1000000000000003E-2,675,10,1118.2597919067316,2146.1675279765282,2611.8192352259562,1.7283838400813301,30.864197530864196,2.4234289108250238,2.2264620148337082,3.11519072840805,12.579510383810451,0,-10.189403410886465,0,0,0,0,0,0.27683114270531234,0.39381800525893068,3.3219737124637478,9.4516321262143368,6.0170958926926916,209.05689345017373,169.47032700019068,1630.3045457418343,2.3637601186047311E-2,13.515824570424,-44673.140749115599,1118.2597919067316,8.972233537044922E-3,4.1475366141009316,-50227.730623733405,2146.1675279765282,1.3026843692028582,3.997403712458359E-2,19.157461404691979,-38485.62443017021,770.41831760537741]
["AKMH","AKMH41E",1.92,2.71,1.44,2.02816901,6000,5.77,6000,6.04,18.399999999999999,45.6,8.1000000000000003E-2,675,10,2430.1862020565118,4344.2275032010912,4942.9824561403511,1.5724617997439125,30.864197530864196,2.3469345415995839,2.1801577788233018,1.3007298427958265,12.579510383810451,0,-10.189403410886465,0,0,0,0,0,0.5200438151802621,0.73981061502010259,6.2405257821631457,17.755454760482461,11.303473567901234,209.05689345017373,169.47032700019068,1630.3045457418343,6.696594209071819E-3,3.8851365188560734,-48990.384567877969,2430.1862020565118,2.4360493216280805E-3,1.0798424236740558,-50664.965461780761,4344.2275032010912,2.2635910958761549,1.0973787515443431E-2,5.3923035462257829,-47309.260115583747,1845.1179645739276]
["AKMH","AKMH41H",1.96,5.32,1.47,3.9729729699999998,6000,5.84,6000,1.58,5,23.7,8.1000000000000003E-2,675,10,4941.469910615805,6000,6000,1.47,30.864197530864196,2.2990379183016332,2.1540257506524747,0.62228173422529653,12.579510383810451,0,-10.189403410886465,0,0,0,0,0,1.0000631722601983,1.4226827219785629,12.00075806712238,34.144385327485509,21.736990814814813,209.05689345017373,169.47032700019068,1630.3045457418343,1.8533116999373655E-3,1.028097891283325,-50334.711320986127,4941.469910615805,6.2638817459066253E-4,0.23009798513341945,-50781.594918388058,8822.1178479654263,3.5476989172881011,2.9905213528996005E-3,1.4098258916446718,-49920.504298121879,3856.773978731444]
["AKMH","AKMH42C",3.22,1.35,2.98,1.2416666700000001,1500,10.5,6000,27.5,97.4,154,0.14499999999999999,675,10,583.75663369082076,1199.0562807777842,1463.6363636363635,3.0281509950755545,17.241379310344829,1.4394297921548536,1.2277561286758047,3.2534789342374495,12.891439351095951,0,-10.442065874387719,0,0,0,0,0,0.15830237922204352,0.22519983338482832,1.8996285506645221,5.40479600123588,3.4407999999999999,214.2407916217395,173.67261329542984,1670.7305399020352,6.1517654942725743E-2,32.290980911651616,-39813.556776051511,583.75663369082076,2.6890616314348591E-2,9.3577503134094471,-49882.075469217889,1199.0562807777842,1.2757260123863636,4.6809793645659639E-2,25.239077173122475,-44090.167837000001,737.67190398683556]
["AKMH","AKMH42E",3.28,2.63,2.72,2.1587301600000002,3500,10.7,6000,7.8,26.8,80.900000000000006,0.14499999999999999,675,10,1403.1602973065428,2454.1175192813389,2786.1557478368354,2.8873411969149858,17.241379310344829,1.4125056947234835,1.2048074159902757,1.4248224584666926,12.891439351095951,0,-10.442065874387719,0,0,0,0,0,0.30275508777773208,0.43069722425536522,3.633061053332785,10.336733382128765,6.5805688527551949,214.2407916217395,173.67261329542984,1670.7305399020352,1.7415558819135809E-2,9.377119144317879,-47446.377871613811,1403.1602973065428,7.3525992614083572E-3,2.5561641602600402,-50555.573869379026,2454.1175192813389,2.3387564039475897,1.2940022372430977E-2,7.1922899824642483,-48829.203662388383,1684.4203891779853]
["AKMH","AKMH42H",3.4,5.76,2.21,3.7457627100000002,6000,10.8,6000,1.67,6,38.299999999999997,0.14499999999999999,675,10,3316.2303126400748,5503.2519570601116,5885.1174934725859,2.308521695183078,17.241379310344829,1.3686896158869344,1.1936517917681435,0.61331503819918276,12.891439351095951,0,-10.442065874387719,0,0,0,0,0,0.6396657707858574,0.90998395419500833,7.6759892494302884,21.8396149006802,13.903530666666667,214.2407916217395,173.67261329542984,1670.7305399020352,3.9448577651210112E-3,2.0269507398631794,-50104.949128388653,3316.2303126400748,1.593192802128357E-3,0.45761669582231862,-50769.470030013275,5503.2519570601116,4.1307221981939426,2.8977963370300378E-3,1.5402845939933025,-50400.822143975842,3913.1602040068774]
["AKMH","AKMH42J",3.42,8.06,2.23,5.1860465099999997,6000,11,6000,0.82,3.1,27.5,0.14499999999999999,675,10,4683.818215187498,6000,6000,2.23,17.241379310344829,1.3604703457105907,1.1719490319178136,0.4308242277044676,12.891439351095951,0,-10.442065874387719,0,0,0,0,0,0.88985343479002388,1.2658991370593735,10.678241217480286,30.381579289424963,19.341514091401347,214.2407916217395,173.67261329542984,1670.7305399020352,2.0842104397634257E-3,1.0125320861721425,-50466.243892387407,4683.818215187498,8.0120768025186608E-4,0.18630228125841061,-50793.686102478649,7846.7712819975468,4.7699189461279268,1.4954514883957926E-3,0.75543593904145245,-50616.504311406468,5570.7173498290986]
["AKMH","AKMH43E",4.5599999999999996,2.68,3.83,2.2267441899999998,2500,15.2,6000,8.6300000000000008,32.6,111,0.20899999999999999,675,10,1023.5262872796286,1787.242575284874,2030.6306306306308,4.0381251680168164,11.961722488038278,1.0479783632315876,0.86864265252509532,1.6467826024312318,13.203368318381449,0,-10.694728337888971,0,0,0,0,0,0.22728083979045674,0.32332809843989663,2.7273700774854808,7.7598743625575191,4.9400894502923984,219.42468979330516,177.87489959066897,1711.1565340622356,2.9759968241241282E-2,14.822038642177127,-46347.469278666671,1023.5262872796286,1.3578063625352651E-2,3.9794786372906219,-50483.833601480153,1787.242575284874,2.3984561110666811,1.7653898693698059E-2,8.1965145591095698,-49441.982276647694,1457.3872692465623]
["AKMH","AKMH43H",4.68,5.24,2.44,2.7415730300000001,6000,15.4,6000,2.12,8.8000000000000007,57.4,0.20899999999999999,675,10,2274.5211886486709,3673.4531269172476,3926.8292682926831,3.3085774992842274,11.961722488038278,1.0286344465018378,0.85736157911567845,0.7811676738041099,13.203368318381449,0,-10.694728337888971,0,0,0,0,0,0.43299044028966466,0.61596910602135679,5.1958852834759757,14.783258544512563,9.4113146894586901,219.42468979330516,177.87489959066897,1711.1565340622356,8.0288462037590366E-3,3.6342477935022752,-49802.981007859744,2274.5211886486709,3.5372397398580032E-3,0.82249673614499008,-50753.82842494073,3673.4531269172476,3.9023462627448779,4.7051020115446585E-3,1.9836209023307882,-50506.598656824506,3072.323753890817]
["AKMH","AKMH43L",4.59,10.9,2.39,5.69047619,6000,15.3,6000,0.56999999999999995,2,27.5,0.20899999999999999,675,10,4974.2395447337476,6000,6000,2.39,11.961722488038278,1.0488586424046311,0.86296524956741494,0.4,13.203368318381449,0,-10.694728337888971,0,0,0,0,0,0.9183467353546696,1.3064335028173366,11.020160824256035,31.354404067616077,19.960833580246913,219.42468979330516,177.87489959066897,1711.1565340622356,1.8419978693457655E-3,0.98644623618066496,-50483.481925,4974.2395447337476,7.7618864511689884E-4,0.13367701799654264,-50799.252712350266,8004.2818732119586,4.923665858039576,1.0839495514784465E-3,0.5419345639338492,-50708.071381293834,6594.2373870043202]
["AKMH","AKMH44E",5.64,2.79,4.76,2.3333333299999999,2000,19.3,6000,8.66,33.9,132,0.27300000000000002,675,10,{"$f":"IF(AQ208<I208,IF(AQ208<0,0,AQ208),I208)","v":867.01349623312308},{"$f":"IF(AU208<I208,IF(AU208<0,0,AU208),I208)","v":1508.733859949039},{"$f":"IF(UAC_V*0.98/L208*1000<I208,IF(UAC_V*0.98/L208*1000<0,0,UAC_V*0.98/L208*1000),I208)","v":1707.5757575757575},{"$f":"C208+(E208-C208)/G208*Q208","v":4.9761571016224222},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M208,(inertia/gear^2+gear_inertia)/M208),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M208,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M208))","v":9.1575091575091569},{"$f":"IF((C208+(E208-C208)/G208*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X208^2*time1+Y208^2*time2+Z208^2*time3+AA208^2*time4)/time)/(C208+(E208-C208)/G208*mspeed),SQRT((((X208-Y208)*2/PI()+Y208)^2*time1+Y208^2*time2+((Z208-Y208)*2/PI()+Y208)^2*time3+AA208^2*time4)/time)/(C208+(E208-C208)/G208*mspeed)),IF(AccType=1,SQRT((X208^2*time1+Y208^2*time2+Z208^2*time3+AA208^2*time4+AB208^2*time5+AC208^2*time6+AD208^2*time7+AE208^2*time8)/time)/(C208+(E208-C208)/G208*mspeed),SQRT((((X208-Y208)*2/PI()+Y208)^2*time1+Y208^2*time2+((Z208-Y208)*2/PI()+Y208)^2*time3+AA208^2*time4+((AB208-AC208)*2/PI()+AC208)^2*time5+AC208^2*time6+((AD208-AC208)*2/PI()+AC208)^2*time7+AE208^2*time8)/time)/(C208+(E208-C208)/G208*mspeed))))","v":0.87299388566359049},{"$f":"IF(move1,MAX(ABS(X208),ABS(Z208))/H208,MAX(ABS(X208),ABS(Z208),ABS(AB208),ABS(AD208))/H208)","v":0.70027447075994542},{"$f":"IF(AZ208>0,speed/(MIN(AZ208,I208)),\"NA\")","v":1.800739227768632},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M208+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M208+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":13.515297285666946},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M208+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M208+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.947390801390226},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M208+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M208+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M208+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M208+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH208/Irms","v":0.19582080784346115},{"$f":"AI208/Ipeak","v":0.27857328181893309},2.3498496941215339,{"$f":"IF(move1,MAX(ABS(X208),ABS(Z208))/(C208/D208),MAX(ABS(X208),ABS(Z208),ABS(AB208),ABS(AD208))/(C208/D208))","v":6.6857587636543938},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X208),ABS(Z208))/(C208/D208),MAX(ABS((X208-Y208)*2/PI()+Y208),ABS((Z208-Y208)*2/PI()+Y208))/(C208/D208)),IF(AccType=1,MAX(ABS(X208),ABS(Z208),ABS(AB208),ABS(AD208))/(C208/D208),MAX(ABS((X208-Y208)*2/PI()+Y208),ABS((Z208-Y208)*2/PI()+Y208),ABS((AB208-AC208)*2/PI()+AC208),ABS((AD208-AC208)*2/PI()+AC208))/(C208/D208)))","v":4.2562862222222222},{"$f":"IF((C208+(E208-C208)/G208*mspeed)<0,\"NA\",U208*(C208+(E208-C208)/G208*mspeed)*mspeed/9.55)","v":224.60858796487094},{"$f":"IF(move1,IF(speed1>speed2,AM208/2*time1/time,AM208/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z208*-speed/30*PI(),((Z208-AA208)*2/PI()+AA208)*-speed/30*PI()),IF(AccType=1,X208*-speed/30*PI(),((X208-Y208)*2/PI()+Y208)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z208*-speed/30*PI(),((Z208-AA208)*2/PI()+AA208)*-speed/30*PI()),IF(AccType=1,X208*-speed/30*PI(),((X208-Y208)*2/PI()+Y208)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD208*-speed/30*PI(),((AD208-AE208)*2/PI()+AE208)*-speed/30*PI()),IF(AccType=1,AB208*-speed/30*PI(),((AB208-AC208)*2/PI()+AC208)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD208*-speed/30*PI(),((AD208-AE208)*2/PI()+AE208)*-speed/30*PI()),IF(AccType=1,AB208*-speed/30*PI(),((AB208-AC208)*2/PI()+AC208)*-speed/30*PI()),0)/2*time7/time)))","v":182.07718588590811},{"$f":"IF(move1,MAX(IF(AccType=1,Z208*-speed/30*PI(),((Z208-AA208)*2/PI()+AA208)*-speed/30*PI()),IF(AccType=1,X208*-speed/30*PI(),((X208-Y208)*2/PI()+Y208)*-speed/30*PI()),0),MAX(IF(AccType=1,Z208*-speed/30*PI(),((Z208-AA208)*2/PI()+AA208)*-speed/30*PI()),IF(AccType=1,X208*-speed/30*PI(),((X208-Y208)*2/PI()+Y208)*-speed/30*PI()),IF(AccType=1,AD208*-speed/30*PI(),((AD208-AE208)*2/PI()+AE208)*-speed/30*PI()),IF(AccType=1,AB208*-speed/30*PI(),((AB208-AC208)*2/PI()+AC208)*-speed/30*PI()),0))","v":1751.5825282224359},{"$f":"(L208^2)/1000000+((K208/1000)^2*(D208/C208*H208)^2*PI()*PI()*(O208/2)^2)/1200","v":3.8962860377216191E-2},{"$f":"SQRT(3)*L208*J208*D208/C208*H208/1000","v":18.903179524888234},{"$f":"0.75*J208^2*(D208/C208*H208)^2-(UAC_V*0.98)^2","v":-45678.177158084349},{"$f":"-AO208/2/AN208+SQRT((AO208/2/AN208)^2-AP208/AN208)","v":867.01349623312308},{"$f":"(L208^2)/1000000+((K208/1000)^2*AV208^2*PI()*PI()*(O208/2)^2)/1200","v":1.8893325592774353E-2},{"$f":"SQRT(3)*L208*J208*AV208/1000","v":4.9372204592104474},{"$f":"0.75*J208^2*AV208^2-(UAC_V*0.98)^2","v":-50455.410432408658},{"$f":"-AS208/2/AR208+SQRT((AS208/2/AR208)^2-AT208/AR208)","v":1508.733859949039},{"$f":"D208+(F208-D208)*((0.85*UAC_V-D208*J208)/L208*1000)/G208","v":2.4936188336952196},{"$f":"(L208^2)/1000000+((K208/1000)^2*AJ208^2*PI()*PI()*(O208/2)^2)/1200","v":2.1704746940012877E-2},{"$f":"SQRT(3)*L208*J208*AJ208/1000","v":8.4271995112704321},{"$f":"0.75*J208^2*AJ208^2-(UAC_V*0.98)^2","v":-49786.196334900764},{"$f":"IF(((AX208/2/AW208)^2-AY208/AW208)>0,-AX208/2/AW208+SQRT((AX208/2/AW208)^2-AY208/AW208),-9999)","v":1332.7859819958139}]
["AKMH","AKMH44H",5.77,5.49,3.31,3.1226415099999998,5000,19.5,6000,2.25,9.1,68,0.27300000000000002,675,10,1950.8620662242822,3097.8449187436645,3314.7058823529414,4.2458602999781174,9.1575091575091569,0.85623231993737503,0.69309216849574085,0.86363519645060804,13.515297285666946,0,-10.947390801390226,0,0,0,0,0,0.3766433204587934,0.53581009603055707,4.519719845505521,12.859442304733369,8.1865752328134018,224.60858796487094,182.07718588590811,1751.5825282224359,1.0485429934784497E-2,4.9168074485711939,-49498.120884173601,1950.8620662242822,4.9264757166072159E-3,1.1169318338308891,-50737.710999057919,3097.8449187436645,4.2147770910374263,5.7651580734628107E-3,2.1694733292123267,-50550.693384182334,2778.9511241130363]
["AKMH","AKMH44K",5.76,9.9,2.5499999999999998,4.3220339000000001,6000,18.600000000000001,6000,0.7,2.8,37.799999999999997,0.27300000000000002,675,10,3817.6591392808427,5790.0883273330664,5962.9629629629635,2.6623027448768091,9.1575091575091569,0.86079664201984685,0.72662888632617983,0.46607809068785649,13.515297285666946,0,-10.947390801390226,0,0,0,0,0,0.68037202725181067,0.96789238373916942,8.1644643270217276,23.229417209740067,14.788306296296296,224.60858796487094,182.07718588590811,1751.5825282224359,3.0763417382458158E-3,1.465129870273211,-50429.574641113286,3817.6591392808427,1.4734796618091186E-3,0.24117019232788225,-50794.983377413242,5790.0883273330664,5.2622704255864203,1.7813824716173894E-3,0.67774902945698856,-50724.78995385595,5149.3516815132525]
["AKMH","AKMH51E",3.47,2.38,2.98,1.7325581400000001,2500,11,6000,9,36.6,110,0.34200000000000003,675,10,1093.2921333405873,1835.5189834712228,2049.0909090909095,3.1102382792396406,7.3099415204678353,1.4397282217125005,1.2592359730474201,1.8977443070851918,13.851595703521621,0,-11.219792519852513,0,0,0,0,0,0.27826297555728674,0.39585492044166015,3.3391557066874409,9.5005180905998436,6.0482176642117613,230.19747818109019,186.60777579796277,1795.166803176402,2.7778373766452223E-2,12.937071827300191,-47347.147035852802,1093.2921333405873,1.3169110475724033E-2,3.3782888130943425,-50569.357617671936,1835.5189834712228,1.9701575309498183,2.2175706384583035E-2,10.371062086753826,-48582.868082493747,1264.6593068621764]
["AKMH","AKMH51H",3.39,5.0199999999999996,1.41,1.7625,5500,11.1,6000,2,7.9,51.3,0.34200000000000003,675,10,2633.6430386794641,4214.1227482257973,4393.7621832358682,1.8729158106387129,7.3099415204678353,1.5084509416667089,1.2478915048217678,0.8003995787721303,13.851595703521621,0,-11.219792519852513,0,0,0,0,0,0.6007751513872488,0.85465843696753352,7.2093018166469856,20.511802487220805,13.058219030263299,230.19747818109019,186.60777579796277,1795.166803176402,6.098792539119444E-3,2.9210230622990006,-49994.61851045501,2633.6430386794641,2.7380405059582273E-3,0.51158926523855042,-50780.297309456349,4214.1227482257973,2.8788128654970757,4.8198576263298017E-3,2.3205553786015076,-50293.608747273014,2998.5023276521088]
["AKMH","AKMH51L",3.47,10,1.45,3.5365853700000001,5500,11.4,6000,0.57999999999999996,2.1,26.6,0.34200000000000003,675,10,5220.1310842150669,6000,6000,1.2663636363636361,7.3099415204678353,1.4734276952148853,1.215052254694879,0.4,13.851595703521621,0,-11.219792519852513,0,0,0,0,0,1.1691721662070871,1.6632559682422696,14.030065994485046,39.918143237814469,25.412679261393954,230.19747818109019,186.60777579796277,1795.166803176402,1.6862560839250975E-3,0.87790118269327966,-50532.847232681946,5220.1310842150669,7.0993740295562612E-4,4.3268626359797724E-2,-50804.498510505451,8429.0104522608217,1.6192087811961731,1.2931558736363426E-3,0.67907964465850945,-50642.223583374725,6000.8725889614807]
["AKMH","AKMH52E",6.15,2.4300000000000002,5.39,1.9318996399999999,1500,20.7,6000,8.98,44.7,179,0.622,675,10,715.43613917910716,1137.9982663742426,1259.217877094972,5.5734142117037173,4.019292604501608,0.90320753367113693,0.73508622876307594,2.3673806112849745,15.216284935395672,0,-12.325190797670494,0,0,0,0,0,0.17609536520136779,0.25051200808273361,2.1131443824164133,6.012288193985607,3.8275415414634137,252.8770326816902,204.99277833963399,1972.0305276272788,5.9524786161286723E-2,22.771492605033828,-46759.243241307151,715.43613917910716,3.3866300576516101E-2,5.8684095253977384,-50536.455602838716,1137.9982663742426,2.1078049415854898,3.805984806010515E-2,10.656385132052993,-49919.119114239256,1013.778683731519]
["AKMH","AKMH52H",6.29,4.8099999999999996,3.44,2.38888889,3500,21,6000,2.37,11.9,92.7,0.622,675,10,1577.6464152237447,2311.0722212157225,2431.4994606256741,4.4081269055814829,4.019292604501608,0.90304102785586571,0.72458499692360345,1.1463108136925315,15.216284935395672,0,-12.325190797670494,0,0,0,0,0,0.34080911275355491,0.48483260823564639,4.0897093530426591,11.635982597655513,7.4076965925925906,252.8770326816902,204.99277833963399,1972.0305276272788,1.6102251577923055E-2,6.1108613936221428,-49718.770882093428,1577.6464152237447,8.9370940243398145E-3,1.3075790993106837,-50755.418774551013,2311.0722212157225,3.4362065597647309,1.0191076704028561E-2,2.8188495278270547,-50573.993803452147,2093.6729997940492]
["AKMH","AKMH52L",6.45,9.5,1.19,1.5866666700000001,4500,21.4,6000,0.63,3.24,48.3,0.622,675,10,3178.3641474767646,4622.9510753841523,4666.666666666667,1.0462838541065249,4.019292604501608,0.90305998842359547,0.71104135212129316,0.57902869503649379,15.216284935395672,0,-12.325190797670494,0,0,0,0,0,0.65641826725938124,0.9338159359577447,7.8770192071125749,22.411582462985873,14.267656525983345,252.8770326816902,204.99277833963399,1972.0305276272788,4.4772804104774569E-3,1.6612154882139947,-50509.428429042731,3178.3641474767646,2.3474823555113852E-3,0.13703665344463761,-50803.147577169599,4622.9510753841523,2.6000903334025764,2.7722836941276147E-3,0.75197075951575265,-50744.563484179853,4144.8723017928114]
["AKMH","AKMH52M",6.39,10.7,1.18,1.7878787899999999,4500,21.3,6000,0.51,2.5,42.4,0.622,675,10,3648.1394777270698,5290.785448316763,5316.0377358490568,0.26444618094881456,4.019292604501608,0.91152274721911231,0.71437957443172162,0.50691479705041731,15.216284935395672,0,-12.325190797670494,0,0,0,0,0,0.74627636463069258,1.0616474231138084,8.9553163755683105,25.479538154731404,16.22077778009621,252.8770326816902,204.99277833963399,1972.0305276272788,3.4325560183459496E-3,1.3358545776423418,-50557.002925000001,3648.1394777270698,1.8020319395586741E-3,6.8287300871921044E-2,-50804.511532537668,5290.785448316763,1.8232376776099048,2.135888575301257E-3,0.60753084814375813,-50753.833108278326,4734.5234622561202]
["AKMH","AKMH53H",8.6,5.29,4.0599999999999996,2.3199999999999998,3000,29.4,6000,2.12,11.4,112,0.91200000000000003,675,10,1363.3993809437798,1925.9973240243467,2012.5000000000002,5.685324049643155,2.7412280701754383,0.73830060271003328,0.56563649892544499,1.3120526164827166,16.629713068408083,0,-13.470067585410547,0,0,0,0,0,0.29960572810612779,0.42621696769321105,3.5952687372735332,10.229207224637065,6.5121155748492674,276.36657127159731,224.03438811493632,2155.2108136656875,2.1283313385066813E-2,7.4373644261315057,-49702.752681618978,1363.3993809437798,1.2902162111117773E-2,1.505636818114122,-50759.980188375703,1925.9973240243467,3.6610504642857142,1.3677215249214662E-2,2.6781605631924661,-50662.212295873738,1829.1949346008676]
["AKMH","AKMH53L",8.68,9.43,2.14,2.1616161599999999,3500,29.7,6000,0.71,3.64,63.9,0.91200000000000003,675,10,2522.1405849787443,3483.2166468455152,3527.386541471049,2.1713608941800944,2.7412280701754383,0.74587663492566814,0.55992299893629915,0.73182160805390961,16.629713068408083,0,-13.470067585410547,0,0,0,0,0,0.52915738193859274,0.75277550996106102,6.3498885832631125,18.066612239065464,11.501562571087215,276.36657127159731,224.03438811493632,2155.2108136656875,6.9195488201411852E-3,2.5355270674118846,-50411.54214115988,2522.1405849787443,4.1127711870782759E-3,0.25885116952511239,-50801.057594786675,3483.2166468455152,3.2940508365926755,4.4436018558179852E-3,0.90380903956289715,-50755.14599263842,3279.487751642343]
["AKMH","AKMH53P",8.49,15.2,2.09,3.4833333299999998,3500,29.2,6000,0.3,1.3,38.4,0.91200000000000003,675,10,{"$f":"IF(AQ220<I220,IF(AQ220<0,0,AQ220),I220)","v":4359.4881984417152},{"$f":"IF(AU220<I220,IF(AU220<0,0,AU220),I220)","v":5878.1231246252928},{"$f":"IF(UAC_V*0.98/L220*1000<I220,IF(UAC_V*0.98/L220*1000<0,0,UAC_V*0.98/L220*1000),I220)","v":5869.791666666667},{"$f":"C220+(E220-C220)/G220*Q220","v":-2.2585679993148222},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M220,(inertia/gear^2+gear_inertia)/M220),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M220,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M220))","v":2.7412280701754383},{"$f":"IF((C220+(E220-C220)/G220*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X220^2*time1+Y220^2*time2+Z220^2*time3+AA220^2*time4)/time)/(C220+(E220-C220)/G220*mspeed),SQRT((((X220-Y220)*2/PI()+Y220)^2*time1+Y220^2*time2+((Z220-Y220)*2/PI()+Y220)^2*time3+AA220^2*time4)/time)/(C220+(E220-C220)/G220*mspeed)),IF(AccType=1,SQRT((X220^2*time1+Y220^2*time2+Z220^2*time3+AA220^2*time4+AB220^2*time5+AC220^2*time6+AD220^2*time7+AE220^2*time8)/time)/(C220+(E220-C220)/G220*mspeed),SQRT((((X220-Y220)*2/PI()+Y220)^2*time1+Y220^2*time2+((Z220-Y220)*2/PI()+Y220)^2*time3+AA220^2*time4+((AB220-AC220)*2/PI()+AC220)^2*time5+AC220^2*time6+((AD220-AC220)*2/PI()+AC220)^2*time7+AE220^2*time8)/time)/(C220+(E220-C220)/G220*mspeed))))","v":0.76260933073365755},{"$f":"IF(move1,MAX(ABS(X220),ABS(Z220))/H220,MAX(ABS(X220),ABS(Z220),ABS(AB220),ABS(AD220))/H220)","v":0.56951072152082483},{"$f":"IF(AZ220>0,speed/(MIN(AZ220,I220)),\"NA\")","v":0.43496183271728861},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M220+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M220+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":16.629713068408083},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M220+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M220+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-13.470067585410547},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M220+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M220+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M220+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M220+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH220/Irms","v":0.87202470554779266},{"$f":"AI220/Ipeak","v":1.2405361142510938},10.464296466573511,{"$f":"IF(move1,MAX(ABS(X220),ABS(Z220))/(C220/D220),MAX(ABS(X220),ABS(Z220),ABS(AB220),ABS(AD220))/(C220/D220))","v":29.772866742026249},18.953995648039083,{"$f":"IF((C220+(E220-C220)/G220*mspeed)<0,\"NA\",U220*(C220+(E220-C220)/G220*mspeed)*mspeed/9.55)","v":276.36657127159731},{"$f":"IF(move1,IF(speed1>speed2,AM220/2*time1/time,AM220/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z220*-speed/30*PI(),((Z220-AA220)*2/PI()+AA220)*-speed/30*PI()),IF(AccType=1,X220*-speed/30*PI(),((X220-Y220)*2/PI()+Y220)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z220*-speed/30*PI(),((Z220-AA220)*2/PI()+AA220)*-speed/30*PI()),IF(AccType=1,X220*-speed/30*PI(),((X220-Y220)*2/PI()+Y220)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD220*-speed/30*PI(),((AD220-AE220)*2/PI()+AE220)*-speed/30*PI()),IF(AccType=1,AB220*-speed/30*PI(),((AB220-AC220)*2/PI()+AC220)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD220*-speed/30*PI(),((AD220-AE220)*2/PI()+AE220)*-speed/30*PI()),IF(AccType=1,AB220*-speed/30*PI(),((AB220-AC220)*2/PI()+AC220)*-speed/30*PI()),0)/2*time7/time)))","v":224.03438811493632},{"$f":"IF(move1,MAX(IF(AccType=1,Z220*-speed/30*PI(),((Z220-AA220)*2/PI()+AA220)*-speed/30*PI()),IF(AccType=1,X220*-speed/30*PI(),((X220-Y220)*2/PI()+Y220)*-speed/30*PI()),0),MAX(IF(AccType=1,Z220*-speed/30*PI(),((Z220-AA220)*2/PI()+AA220)*-speed/30*PI()),IF(AccType=1,X220*-speed/30*PI(),((X220-Y220)*2/PI()+Y220)*-speed/30*PI()),IF(AccType=1,AD220*-speed/30*PI(),((AD220-AE220)*2/PI()+AE220)*-speed/30*PI()),IF(AccType=1,AB220*-speed/30*PI(),((AB220-AC220)*2/PI()+AC220)*-speed/30*PI()),0))","v":2155.2108136656875},{"$f":"(L220^2)/1000000+((K220/1000)^2*(D220/C220*H220)^2*PI()*PI()*(O220/2)^2)/1200","v":2.4242518497887833E-3},{"$f":"SQRT(3)*L220*J220*D220/C220*H220/1000","v":1.0431141953556402},{"$f":"0.75*J220^2*(D220/C220*H220)^2-(UAC_V*0.98)^2","v":-50620.683406210592},{"$f":"-AO220/2/AN220+SQRT((AO220/2/AN220)^2-AP220/AN220)","v":4359.4881984417152},{"$f":"(L220^2)/1000000+((K220/1000)^2*AV220^2*PI()*PI()*(O220/2)^2)/1200","v":1.4752862627492849E-3},{"$f":"SQRT(3)*L220*J220*AV220/1000","v":-2.8846118602568145E-2},{"$f":"0.75*J220^2*AV220^2-(UAC_V*0.98)^2","v":-50805.018924262418},{"$f":"-AS220/2/AR220+SQRT((AS220/2/AR220)^2-AT220/AR220)","v":5878.1231246252928},{"$f":"D220+(F220-D220)*((0.85*UAC_V-D220*J220)/L220*1000)/G220","v":-1.4456870087038709},1.5993979894937487E-3,0.3781933455610722,-50780.910358305759,{"$f":"IF(((AX220/2/AW220)^2-AY220/AW220)>0,-AX220/2/AW220+SQRT((AX220/2/AW220)^2-AY220/AW220),-9999)","v":5517.7255094010143}]
["AKMH","AKMH54H",10.5,4.12,7.62,2.96498054,1800,36.9,6000,3.22,18.3,166,1.1919999999999999,675,10,934.25533952669525,1282.6758609119674,1357.831325301205,8.4477186225408527,2.0973154362416109,0.64684280528181348,0.48765317886943449,1.9156779981869121,17.994402300282133,0,-14.57546586322853,0,0,0,0,0,0.20680140182000406,0.29419419633794597,2.4816168218400487,7.0606607121107032,4.4949562153086413,299.04612577219734,242.41939065660756,2332.0745381165648,4.1991414331982974E-2,13.404754674944323,-49174.957431635201,934.25533952669525,2.8359317723440747E-2,3.1621896856830141,-50714.440704671943,1282.6758609119674,3.4155711035279248,2.8947270635366756E-2,4.1615014739304588,-50648.042725018822,1252.8201515450264]
["AKMH","AKMH54L",10.4,9.2899999999999991,2.4700000000000002,2.1858407099999999,3000,36.9,6000,0.67,3.5,72.900000000000006,1.1919999999999999,675,10,2335.7987912930839,3059.8105939623697,3091.9067215363511,2.3119006632928034,2.0973154362416109,0.68697034063526952,0.48765317886943449,0.81624917577067735,17.994402300282133,0,-14.57546586322853,0,0,0,0,0,0.47079076597582831,0.66974357920521221,5.6494891917099395,16.073845900925093,10.232928118518513,299.0461257721974,242.41939065660756,2332.0745381165648,8.0510147624700979E-3,2.7885067444048564,-50439.372929394267,2335.7987912930839,5.339270477560624E-3,0.26577883506405431,-50801.837035213321,3059.8105939623697,3.1416473592763934,5.5781611995893267E-3,0.86569095879063751,-50769.90581204067,2940.278619863835]
["AKMH","AKMH54P",10.6,14.5,2.52,3.4054054100000002,3000,35.299999999999997,6000,0.32,1.5,47.3,1.1919999999999999,675,10,3721.0932229188984,4767.7155051686304,4765.3276955602541,-2.2410470939208444,2.0973154362416109,0.67398160770369597,0.50975643910147683,0.52616068918383263,17.994402300282133,0,-14.57546586322853,0,0,0,0,0,0.72095423674426673,1.0256243449453259,8.6514508409312008,24.614984278687821,15.670385688329835,299.0461257721974,242.41939065660756,2332.0745381165648,3.31602485349098E-3,1.2659267845101987,-50626.085022712716,3721.0932229188984,2.2373726156095252E-3,-1.1078533850921687E-2,-50805.146285426534,4767.7155051686304,-0.42258156058773899,2.3508957720700086E-3,0.41081986176516067,-50786.300916150707,4561.3441850299005]
["AKMH","AKMH62H",10.6,5.3,9.93,4.5136363599999996,1800,28.6,6000,3.32,25.4,142.1,1.69,675,10,902.78012288853279,1396.0701011353804,1586.2068965517242,10.080351684577385,1.4792899408284024,0.68804193140069769,0.71404194325078363,1.8470889864082625,20.421599576972412,0,-16.541495657347653,0,0,0,0,0,0.29906658825008275,0.42544999118692522,3.5887990590009928,10.210799788486206,6.5003970370370361,339.38333341969309,275.11843089143701,2646.6393051756245,4.7319175692311227E-2,11.685002952313896,-49114.682068000002,902.78012288853279,2.3189307396722789E-2,3.8838795754787481,-50618.400215546077,1396.0701011353804,4.7530563882611618,2.5797798376327168E-2,5.3116894104188992,-50455.845029761724,1299.3418387854149]
["AKMH","AKMH62L",10.8,11.9,4.95,4.95,5000,29.1,6000,0.75700000000000001,5.4,65.5,1.69,675,10,2067.1046306520248,3225.7542722113644,3441.2213740458014,7.0258675015127041,1.4792899408284024,0.69877577375220612,0.70177318133925815,0.82146634205749525,20.421599576972412,0,-16.541495657347653,0,0,0,0,0,0.65905414818073782,0.93756572131933524,7.9086497781688543,22.501577311664047,14.324949026063099,339.38333341969309,275.11843089143701,2646.6393051756245,1.0454474076696639E-2,2.753683369635795,-50363.299263434026,2067.1046306520248,4.6684734324832855E-3,0.68210150670191516,-50778.048382644076,3225.7542722113644,7.9423898778625954,5.5206099850760894E-3,1.2302429702349611,-50716.965969010402,2921.6047902690839]
["AKMH","AKMH62M",10.9,13.1,3.33,3.6593406599999998,5500,29.3,6000,0.58699999999999997,4.4000000000000004,58.8,1.69,675,10,2330.2829932237091,3649.5958337959305,3833.3333333333335,5.8768290069390554,1.4792899408284024,0.69831248869323259,0.69698292071578194,0.73151167907919057,20.421599576972412,0,-16.541495657347653,0,0,0,0,0,0.71885730386717128,1.0226412632199486,8.6262876464060554,24.543390317278767,15.62480755691471,339.38333341969303,275.11843089143701,2646.6393051756245,8.3935939613951453E-3,2.1051763031600932,-50484.708505007555,2330.2829932237091,3.6884253080962221E-3,0.45539294988299905,-50790.164603203302,3649.5958337959305,7.6174611538552801,4.4292765200029524E-3,0.93409432105818757,-50742.069085867501,3280.8772144568666]
["AKMH","AKMH63H",14.6,5.2,13.6,4.5333333299999996,1500,41.1,6000,3.45,28.1,194.5,2.42,675,10,711.70338241777836,1038.3848072440014,1158.8688946015425,13.907743461837333,1.0330578512396695,0.58942119882697075,0.58344378005042863,2.3593131105203744,23.979539360072618,0,-19.42342688165882,0,0,0,0,0,0.25014939659953966,0.35586074392801836,3.0017927591944757,8.5406578542724407,5.4371516590563163,398.51217193911464,323.05075894650844,3107.7483010654109,7.262035722555038E-2,17.013420568752341,-48892.296091823046,711.70338241777836,4.1562022221254775E-2,5.5721309985488547,-50599.976027749035,1038.3848072440014,4.7942644938296484,4.2629949432907613E-2,6.31932621619677,-50541.258202981007,1017.2452267137412]
["AKMH","AKMH63L",14.8,10.6,11.1,7.4,3000,41.6,6000,0.95699999999999996,7.4,98.2,2.42,675,10,1480.0225482972678,2135.6571454923001,2295.3156822810593,12.16602285389283,1.0330578512396695,0.5917338286379259,0.57643123461713019,1.1599993811810669,23.979539360072618,0,-19.42342688165882,0,0,0,0,0,0.50302911405593487,0.71560562279495976,6.0363493686712184,17.174534947079035,10.933648528528527,398.51217193911464,323.05075894650844,3107.7483010654109,1.9638564737897685E-2,4.8497743631161478,-50195.398359380808,1480.0225482972678,1.0473410944895198E-2,1.397677081700579,-50754.515682718906,2135.6571454923001,8.5866308214528182,1.0989262022459043E-2,1.779709677224482,-50723.046350044009,2068.9666209618249]
["AKMH","AKMH63M",15,13,7.9,6.3709677400000002,4000,42,6000,0.627,4.9000000000000004,79.900000000000006,2.42,675,10,1856.5603062527932,2676.3236044877358,2821.026282853567,10.249525602034268,1.0330578512396695,0.5935923463009779,0.57094141333506232,0.93451824355498381,23.979539360072618,0,-19.42342688165882,0,0,0,0,0,0.60869686505887977,0.86592781022484466,7.3043623807065572,20.782267445396272,13.230402370370371,398.51217193911464,323.05075894650844,3107.7483010654109,1.2925149863435192E-2,3.1584669087615391,-50414.499850120003,1856.5603062527932,6.7940966065741532E-3,0.79083777616685291,-50780.668168525248,2676.3236044877358,9.1140720748474973,7.2481751992107667E-3,1.1480161559454685,-50753.548979093401,2568.1681621005105]
["AKMH","AKMH64K",18.7,8.6999999999999993,15.6,6.8421052600000003,2000,52.5,6000,1.43,11.8,147,3.16,675,10,1026.4369107141893,1419.4293448800515,1533.3333333333335,16.499884515435919,0.79113924050632911,0.53865045956141566,0.52545177227259399,1.7065411803790795,27.586218044311185,0,-22.344836615892056,0,0,0,0,0,0.37590486487079189,0.53475957438838528,4.5108583784495027,12.834229785321247,8.1705244444444443,458.45099454784332,371.63969423521092,3575.1738585427292,3.8689336465423503E-2,8.8930544020493461,-49890.189193879763,1026.4369107141893,2.3238040005670334E-2,2.746430498215112,-50717.8945031986,1419.4293448800515,7.5431824720759861,2.3520271526696761E-2,2.9748421974019377,-50702.77573766205,1406.3534051178772]
["AKMH","AKMH64L",19,12.1,12.5,7.5301204799999999,3000,53.1,6000,0.76700000000000002,6.2,107,3.16,675,10,1453.9765957318239,1989.178916888111,2106.5420560747662,14.690112346742428,0.79113924050632911,0.53800669384212996,0.51951446411132174,1.2263128446090781,27.586218044311185,0,-22.344836615892056,0,0,0,0,0,0.5145553162390446,0.73200271564948538,6.1746637948685352,17.568065175587648,11.184177653021441,458.45099454784332,371.63969423521092,3575.1738585427292,2.0487460572760574E-2,4.8069107587352695,-50300.609579822587,1453.9765957318239,1.2154676000248709E-2,1.343140668766645,-50765.767326926049,1989.178916888111,9.4489103884774579,1.2437666914557204E-2,1.5898048806561631,-50749.970036715917,1957.0862447951183]
["AKMH","AKMH65K",21.9,9.1,17.7,6.9685039399999997,2000,59.8,6000,1.35,11.4,164,4,675,10,{"$f":"IF(AQ232<I232,IF(AQ232<0,0,AQ232),I232)","v":968.80064975779442},{"$f":"IF(AU232<I232,IF(AU232<0,0,AU232),I232)","v":1280.4206612339042},{"$f":"IF(UAC_V*0.98/L232*1000<I232,IF(UAC_V*0.98/L232*1000<0,0,UAC_V*0.98/L232*1000),I232)","v":1374.3902439024391},{"$f":"C232+(E232-C232)/G232*Q232","v":19.211116611408801},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M232,(inertia/gear^2+gear_inertia)/M232),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M232,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M232))","v":0.625},{"$f":"IF((C232+(E232-C232)/G232*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X232^2*time1+Y232^2*time2+Z232^2*time3+AA232^2*time4)/time)/(C232+(E232-C232)/G232*mspeed),SQRT((((X232-Y232)*2/PI()+Y232)^2*time1+Y232^2*time2+((Z232-Y232)*2/PI()+Y232)^2*time3+AA232^2*time4)/time)/(C232+(E232-C232)/G232*mspeed)),IF(AccType=1,SQRT((X232^2*time1+Y232^2*time2+Z232^2*time3+AA232^2*time4+AB232^2*time5+AC232^2*time6+AD232^2*time7+AE232^2*time8)/time)/(C232+(E232-C232)/G232*mspeed),SQRT((((X232-Y232)*2/PI()+Y232)^2*time1+Y232^2*time2+((Z232-Y232)*2/PI()+Y232)^2*time3+AA232^2*time4+((AB232-AC232)*2/PI()+AC232)^2*time5+AC232^2*time6+((AD232-AC232)*2/PI()+AC232)^2*time7+AE232^2*time8)/time)/(C232+(E232-C232)/G232*mspeed))))","v":0.53144542739254774},{"$f":"IF(move1,MAX(ABS(X232),ABS(Z232))/H232,MAX(ABS(X232),ABS(Z232),ABS(AB232),ABS(AD232))/H232)","v":0.5297706645473802},{"$f":"IF(AZ232>0,speed/(MIN(AZ232,I232)),\"NA\")","v":1.8854829058277836},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M232+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M232+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":31.680285739933336},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M232+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M232+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-25.661031449346002},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M232+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M232+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M232+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M232+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH232/Irms","v":0.38556224746880258},{"$f":"AI232/Ipeak","v":0.54849809785653225},4.6267469696256311,{"$f":"IF(move1,MAX(ABS(X232),ABS(Z232))/(C232/D232),MAX(ABS(X232),ABS(Z232),ABS(AB232),ABS(AD232))/(C232/D232))","v":13.163954348556775},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X232),ABS(Z232))/(C232/D232),MAX(ABS((X232-Y232)*2/PI()+Y232),ABS((Z232-Y232)*2/PI()+Y232))/(C232/D232)),IF(AccType=1,MAX(ABS(X232),ABS(Z232),ABS(AB232),ABS(AD232))/(C232/D232),MAX(ABS((X232-Y232)*2/PI()+Y232),ABS((Z232-Y232)*2/PI()+Y232),ABS((AB232-AC232)*2/PI()+AC232),ABS((AD232-AC232)*2/PI()+AC232))/(C232/D232)))","v":8.3804336208354471},{"$f":"IF((C232+(E232-C232)/G232*mspeed)<0,\"NA\",U232*(C232+(E232-C232)/G232*mspeed)*mspeed/9.55)","v":526.48965804964325},{"$f":"IF(move1,IF(speed1>speed2,AM232/2*time1/time,AM232/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z232*-speed/30*PI(),((Z232-AA232)*2/PI()+AA232)*-speed/30*PI()),IF(AccType=1,X232*-speed/30*PI(),((X232-Y232)*2/PI()+Y232)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z232*-speed/30*PI(),((Z232-AA232)*2/PI()+AA232)*-speed/30*PI()),IF(AccType=1,X232*-speed/30*PI(),((X232-Y232)*2/PI()+Y232)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD232*-speed/30*PI(),((AD232-AE232)*2/PI()+AE232)*-speed/30*PI()),IF(AccType=1,AB232*-speed/30*PI(),((AB232-AC232)*2/PI()+AC232)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD232*-speed/30*PI(),((AD232-AE232)*2/PI()+AE232)*-speed/30*PI()),IF(AccType=1,AB232*-speed/30*PI(),((AB232-AC232)*2/PI()+AC232)*-speed/30*PI()),0)/2*time7/time)))","v":426.79470186022445},{"$f":"IF(move1,MAX(IF(AccType=1,Z232*-speed/30*PI(),((Z232-AA232)*2/PI()+AA232)*-speed/30*PI()),IF(AccType=1,X232*-speed/30*PI(),((X232-Y232)*2/PI()+Y232)*-speed/30*PI()),0),MAX(IF(AccType=1,Z232*-speed/30*PI(),((Z232-AA232)*2/PI()+AA232)*-speed/30*PI()),IF(AccType=1,X232*-speed/30*PI(),((X232-Y232)*2/PI()+Y232)*-speed/30*PI()),IF(AccType=1,AD232*-speed/30*PI(),((AD232-AE232)*2/PI()+AE232)*-speed/30*PI()),IF(AccType=1,AB232*-speed/30*PI(),((AB232-AC232)*2/PI()+AC232)*-speed/30*PI()),0))","v":4105.7650318953592},{"$f":"(L232^2)/1000000+((K232/1000)^2*(D232/C232*H232)^2*PI()*PI()*(O232/2)^2)/1200","v":4.3395285351257522E-2},{"$f":"SQRT(3)*L232*J232*D232/C232*H232/1000","v":9.5287669513091746},{"$f":"0.75*J232^2*(D232/C232*H232)^2-(UAC_V*0.98)^2","v":-49961.192499141493},{"$f":"-AO232/2/AN232+SQRT((AO232/2/AN232)^2-AP232/AN232)","v":968.80064975779442},{"$f":"(L232^2)/1000000+((K232/1000)^2*AV232^2*PI()*PI()*(O232/2)^2)/1200","v":2.8567681482907639E-2},{"$f":"SQRT(3)*L232*J232*AV232/1000","v":3.0330593216501063},{"$f":"0.75*J232^2*AV232^2-(UAC_V*0.98)^2","v":-50719.650548328296},{"$f":"-AS232/2/AR232+SQRT((AS232/2/AR232)^2-AT232/AR232)","v":1280.4206612339042},{"$f":"D232+(F232-D232)*((0.85*UAC_V-D232*J232)/L232*1000)/G232","v":7.9093839919728657},{"$f":"(L232^2)/1000000+((K232/1000)^2*AJ232^2*PI()*PI()*(O232/2)^2)/1200","v":2.8772727387004305E-2},{"$f":"SQRT(3)*L232*J232*AJ232/1000","v":3.2136955721130329},{"$f":"0.75*J232^2*AJ232^2-(UAC_V*0.98)^2","v":-50709.162089249156},{"$f":"IF(((AX232/2/AW232)^2-AY232/AW232)>0,-AX232/2/AW232+SQRT((AX232/2/AW232)^2-AY232/AW232),-9999)","v":1272.8834573794918}]
["AKMH","AKMH65L",22.2,11.1,16,7.6190476199999999,2500,64.2,6000,1.07,7.6,133,4,675,10,{"$f":"IF(AQ233<I233,IF(AQ233<0,0,AQ233),I233)","v":1166.1003387527028},{"$f":"IF(AU233<I233,IF(AU233<0,0,AU233),I233)","v":1588.1745597324837},{"$f":"IF(UAC_V*0.98/L233*1000<I233,IF(UAC_V*0.98/L233*1000<0,0,UAC_V*0.98/L233*1000),I233)","v":1694.7368421052631},{"$f":"C233+(E233-C233)/G233*Q233","v":18.261327091863439},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M233,(inertia/gear^2+gear_inertia)/M233),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M233,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M233))","v":0.625},{"$f":"IF((C233+(E233-C233)/G233*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X233^2*time1+Y233^2*time2+Z233^2*time3+AA233^2*time4)/time)/(C233+(E233-C233)/G233*mspeed),SQRT((((X233-Y233)*2/PI()+Y233)^2*time1+Y233^2*time2+((Z233-Y233)*2/PI()+Y233)^2*time3+AA233^2*time4)/time)/(C233+(E233-C233)/G233*mspeed)),IF(AccType=1,SQRT((X233^2*time1+Y233^2*time2+Z233^2*time3+AA233^2*time4+AB233^2*time5+AC233^2*time6+AD233^2*time7+AE233^2*time8)/time)/(C233+(E233-C233)/G233*mspeed),SQRT((((X233-Y233)*2/PI()+Y233)^2*time1+Y233^2*time2+((Z233-Y233)*2/PI()+Y233)^2*time3+AA233^2*time4+((AB233-AC233)*2/PI()+AC233)^2*time5+AC233^2*time6+((AD233-AC233)*2/PI()+AC233)^2*time7+AE233^2*time8)/time)/(C233+(E233-C233)/G233*mspeed))))","v":0.52820818167642147},{"$f":"IF(move1,MAX(ABS(X233),ABS(Z233))/H233,MAX(ABS(X233),ABS(Z233),ABS(AB233),ABS(AD233))/H233)","v":0.49346239470301145},{"$f":"IF(AZ233>0,speed/(MIN(AZ233,I233)),\"NA\")","v":1.5249446861472877},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M233+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M233+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":31.680285739933336},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M233+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M233+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-25.661031449346002},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M233+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M233+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M233+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M233+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH233/Irms","v":0.46394578129487779},{"$f":"AI233/Ipeak","v":0.66000595291527786},5.5673493755385337,{"$f":"IF(move1,MAX(ABS(X233),ABS(Z233))/(C233/D233),MAX(ABS(X233),ABS(Z233),ABS(AB233),ABS(AD233))/(C233/D233))","v":15.840142869966668},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X233),ABS(Z233))/(C233/D233),MAX(ABS((X233-Y233)*2/PI()+Y233),ABS((Z233-Y233)*2/PI()+Y233))/(C233/D233)),IF(AccType=1,MAX(ABS(X233),ABS(Z233),ABS(AB233),ABS(AD233))/(C233/D233),MAX(ABS((X233-Y233)*2/PI()+Y233),ABS((Z233-Y233)*2/PI()+Y233),ABS((AB233-AC233)*2/PI()+AC233),ABS((AD233-AC233)*2/PI()+AC233))/(C233/D233)))","v":10.084148148148147},{"$f":"IF((C233+(E233-C233)/G233*mspeed)<0,\"NA\",U233*(C233+(E233-C233)/G233*mspeed)*mspeed/9.55)","v":526.48965804964325},{"$f":"IF(move1,IF(speed1>speed2,AM233/2*time1/time,AM233/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z233*-speed/30*PI(),((Z233-AA233)*2/PI()+AA233)*-speed/30*PI()),IF(AccType=1,X233*-speed/30*PI(),((X233-Y233)*2/PI()+Y233)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z233*-speed/30*PI(),((Z233-AA233)*2/PI()+AA233)*-speed/30*PI()),IF(AccType=1,X233*-speed/30*PI(),((X233-Y233)*2/PI()+Y233)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD233*-speed/30*PI(),((AD233-AE233)*2/PI()+AE233)*-speed/30*PI()),IF(AccType=1,AB233*-speed/30*PI(),((AB233-AC233)*2/PI()+AC233)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD233*-speed/30*PI(),((AD233-AE233)*2/PI()+AE233)*-speed/30*PI()),IF(AccType=1,AB233*-speed/30*PI(),((AB233-AC233)*2/PI()+AC233)*-speed/30*PI()),0)/2*time7/time)))","v":426.79470186022445},{"$f":"IF(move1,MAX(IF(AccType=1,Z233*-speed/30*PI(),((Z233-AA233)*2/PI()+AA233)*-speed/30*PI()),IF(AccType=1,X233*-speed/30*PI(),((X233-Y233)*2/PI()+Y233)*-speed/30*PI()),0),MAX(IF(AccType=1,Z233*-speed/30*PI(),((Z233-AA233)*2/PI()+AA233)*-speed/30*PI()),IF(AccType=1,X233*-speed/30*PI(),((X233-Y233)*2/PI()+Y233)*-speed/30*PI()),IF(AccType=1,AD233*-speed/30*PI(),((AD233-AE233)*2/PI()+AE233)*-speed/30*PI()),IF(AccType=1,AB233*-speed/30*PI(),((AB233-AC233)*2/PI()+AC233)*-speed/30*PI()),0))","v":4105.7650318953592},{"$f":"(L233^2)/1000000+((K233/1000)^2*(D233/C233*H233)^2*PI()*PI()*(O233/2)^2)/1200","v":2.9926586015348207E-2},{"$f":"SQRT(3)*L233*J233*D233/C233*H233/1000","v":7.9122696286465741},{"$f":"0.75*J233^2*(D233/C233*H233)^2-(UAC_V*0.98)^2","v":-49920.372693250007},{"$f":"-AO233/2/AN233+SQRT((AO233/2/AN233)^2-AP233/AN233)","v":1166.1003387527028},{"$f":"(L233^2)/1000000+((K233/1000)^2*AV233^2*PI()*PI()*(O233/2)^2)/1200","v":1.8689341383947428E-2},{"$f":"SQRT(3)*L233*J233*AV233/1000","v":2.2621808292489072},{"$f":"0.75*J233^2*AV233^2-(UAC_V*0.98)^2","v":-50732.834513762493},{"$f":"-AS233/2/AR233+SQRT((AS233/2/AR233)^2-AT233/AR233)","v":1588.1745597324837},{"$f":"D233+(F233-D233)*((0.85*UAC_V-D233*J233)/L233*1000)/G233","v":9.1776453567737146},{"$f":"(L233^2)/1000000+((K233/1000)^2*AJ233^2*PI()*PI()*(O233/2)^2)/1200","v":1.8896714073825135E-2},{"$f":"SQRT(3)*L233*J233*AJ233/1000","v":2.4856230256500056},{"$f":"0.75*J233^2*AJ233^2-(UAC_V*0.98)^2","v":-50717.841301576671},{"$f":"IF(((AX233/2/AW233)^2-AY233/AW233)>0,-AX233/2/AW233+SQRT((AX233/2/AW233)^2-AY233/AW233),-9999)","v":1573.8275766995228}]
["AKMH","AKMH65M",22.2,12.6,16.100000000000001,8.7027026999999997,2500,64.2,6000,0.747,6.1,119,4,675,10,{"$f":"IF(AQ234<I234,IF(AQ234<0,0,AQ234),I234)","v":1326.715846367518},{"$f":"IF(AU234<I234,IF(AU234<0,0,AU234),I234)","v":1791.0220949323375},{"$f":"IF(UAC_V*0.98/L234*1000<I234,IF(UAC_V*0.98/L234*1000<0,0,UAC_V*0.98/L234*1000),I234)","v":1894.1176470588236},{"$f":"C234+(E234-C234)/G234*Q234","v":17.829906088365099},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M234,(inertia/gear^2+gear_inertia)/M234),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M234,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M234))","v":0.625},{"$f":"IF((C234+(E234-C234)/G234*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X234^2*time1+Y234^2*time2+Z234^2*time3+AA234^2*time4)/time)/(C234+(E234-C234)/G234*mspeed),SQRT((((X234-Y234)*2/PI()+Y234)^2*time1+Y234^2*time2+((Z234-Y234)*2/PI()+Y234)^2*time3+AA234^2*time4)/time)/(C234+(E234-C234)/G234*mspeed)),IF(AccType=1,SQRT((X234^2*time1+Y234^2*time2+Z234^2*time3+AA234^2*time4+AB234^2*time5+AC234^2*time6+AD234^2*time7+AE234^2*time8)/time)/(C234+(E234-C234)/G234*mspeed),SQRT((((X234-Y234)*2/PI()+Y234)^2*time1+Y234^2*time2+((Z234-Y234)*2/PI()+Y234)^2*time3+AA234^2*time4+((AB234-AC234)*2/PI()+AC234)^2*time5+AC234^2*time6+((AD234-AC234)*2/PI()+AC234)^2*time7+AE234^2*time8)/time)/(C234+(E234-C234)/G234*mspeed))))","v":0.52775597752082037},{"$f":"IF(move1,MAX(ABS(X234),ABS(Z234))/H234,MAX(ABS(X234),ABS(Z234),ABS(AB234),ABS(AD234))/H234)","v":0.49346239470301145},{"$f":"IF(AZ234>0,speed/(MIN(AZ234,I234)),\"NA\")","v":1.3542080334669699},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M234+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M234+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":31.680285739933336},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M234+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M234+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-25.661031449346002},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M234+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M234+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M234+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M234+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH234/Irms","v":0.52664115714553705},{"$f":"AI234/Ipeak","v":0.74919594655247757},6.3196938857464442,{"$f":"IF(move1,MAX(ABS(X234),ABS(Z234))/(C234/D234),MAX(ABS(X234),ABS(Z234),ABS(AB234),ABS(AD234))/(C234/D234))","v":17.980702717259462},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X234),ABS(Z234))/(C234/D234),MAX(ABS((X234-Y234)*2/PI()+Y234),ABS((Z234-Y234)*2/PI()+Y234))/(C234/D234)),IF(AccType=1,MAX(ABS(X234),ABS(Z234),ABS(AB234),ABS(AD234))/(C234/D234),MAX(ABS((X234-Y234)*2/PI()+Y234),ABS((Z234-Y234)*2/PI()+Y234),ABS((AB234-AC234)*2/PI()+AC234),ABS((AD234-AC234)*2/PI()+AC234))/(C234/D234)))","v":11.446870870870869},{"$f":"IF((C234+(E234-C234)/G234*mspeed)<0,\"NA\",U234*(C234+(E234-C234)/G234*mspeed)*mspeed/9.55)","v":526.48965804964325},{"$f":"IF(move1,IF(speed1>speed2,AM234/2*time1/time,AM234/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z234*-speed/30*PI(),((Z234-AA234)*2/PI()+AA234)*-speed/30*PI()),IF(AccType=1,X234*-speed/30*PI(),((X234-Y234)*2/PI()+Y234)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z234*-speed/30*PI(),((Z234-AA234)*2/PI()+AA234)*-speed/30*PI()),IF(AccType=1,X234*-speed/30*PI(),((X234-Y234)*2/PI()+Y234)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD234*-speed/30*PI(),((AD234-AE234)*2/PI()+AE234)*-speed/30*PI()),IF(AccType=1,AB234*-speed/30*PI(),((AB234-AC234)*2/PI()+AC234)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD234*-speed/30*PI(),((AD234-AE234)*2/PI()+AE234)*-speed/30*PI()),IF(AccType=1,AB234*-speed/30*PI(),((AB234-AC234)*2/PI()+AC234)*-speed/30*PI()),0)/2*time7/time)))","v":426.79470186022445},{"$f":"IF(move1,MAX(IF(AccType=1,Z234*-speed/30*PI(),((Z234-AA234)*2/PI()+AA234)*-speed/30*PI()),IF(AccType=1,X234*-speed/30*PI(),((X234-Y234)*2/PI()+Y234)*-speed/30*PI()),0),MAX(IF(AccType=1,Z234*-speed/30*PI(),((Z234-AA234)*2/PI()+AA234)*-speed/30*PI()),IF(AccType=1,X234*-speed/30*PI(),((X234-Y234)*2/PI()+Y234)*-speed/30*PI()),IF(AccType=1,AD234*-speed/30*PI(),((AD234-AE234)*2/PI()+AE234)*-speed/30*PI()),IF(AccType=1,AB234*-speed/30*PI(),((AB234-AC234)*2/PI()+AC234)*-speed/30*PI()),0))","v":4105.7650318953592},{"$f":"(L234^2)/1000000+((K234/1000)^2*(D234/C234*H234)^2*PI()*PI()*(O234/2)^2)/1200","v":2.4319354757466882E-2},{"$f":"SQRT(3)*L234*J234*D234/C234*H234/1000","v":5.6102315903746023},{"$f":"0.75*J234^2*(D234/C234*H234)^2-(UAC_V*0.98)^2","v":-50249.50188091171},{"$f":"-AO234/2/AN234+SQRT((AO234/2/AN234)^2-AP234/AN234)","v":1326.715846367518},{"$f":"(L234^2)/1000000+((K234/1000)^2*AV234^2*PI()*PI()*(O234/2)^2)/1200","v":1.4951124235767414E-2},{"$f":"SQRT(3)*L234*J234*AV234/1000","v":1.5646485182966525},{"$f":"0.75*J234^2*AV234^2-(UAC_V*0.98)^2","v":-50761.940506570725},{"$f":"-AS234/2/AR234+SQRT((AS234/2/AR234)^2-AT234/AR234)","v":1791.0220949323375},{"$f":"D234+(F234-D234)*((0.85*UAC_V-D234*J234)/L234*1000)/G234","v":10.162220233603563},{"$f":"(L234^2)/1000000+((K234/1000)^2*AJ234^2*PI()*PI()*(O234/2)^2)/1200","v":1.516351699903187E-2},{"$f":"SQRT(3)*L234*J234*AJ234/1000","v":1.7624425701793855},{"$f":"0.75*J234^2*AJ234^2-(UAC_V*0.98)^2","v":-50750.322703672406},{"$f":"IF(((AX234/2/AW234)^2-AY234/AW234)>0,-AX234/2/AW234+SQRT((AX234/2/AW234)^2-AY234/AW234),-9999)","v":1772.2535538765414}]
["ACC","AHD55 C4-22",0.4,1.6,0.36,1.39,3000,1.4,8000,9.1999999999999993,8.4,22,2.4E-2,560,6,{"$f":"IF(AQ235<I235,IF(AQ235<0,0,AQ235),I235)","v":7296.7028009036821},{"$f":"IF(AU235<I235,IF(AU235<0,0,AU235),I235)","v":8000},{"$f":"IF(UAC_V*0.98/L235*1000<I235,IF(UAC_V*0.98/L235*1000<0,0,UAC_V*0.98/L235*1000),I235)","v":8000},{"$f":"C235+(E235-C235)/G235*Q235","v":0.29333333333333328},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M235,(inertia/gear^2+gear_inertia)/M235),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M235,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M235))","v":104.16666666666667},{"$f":"IF((C235+(E235-C235)/G235*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X235^2*time1+Y235^2*time2+Z235^2*time3+AA235^2*time4)/time)/(C235+(E235-C235)/G235*mspeed),SQRT((((X235-Y235)*2/PI()+Y235)^2*time1+Y235^2*time2+((Z235-Y235)*2/PI()+Y235)^2*time3+AA235^2*time4)/time)/(C235+(E235-C235)/G235*mspeed)),IF(AccType=1,SQRT((X235^2*time1+Y235^2*time2+Z235^2*time3+AA235^2*time4+AB235^2*time5+AC235^2*time6+AD235^2*time7+AE235^2*time8)/time)/(C235+(E235-C235)/G235*mspeed),SQRT((((X235-Y235)*2/PI()+Y235)^2*time1+Y235^2*time2+((Z235-Y235)*2/PI()+Y235)^2*time3+AA235^2*time4+((AB235-AC235)*2/PI()+AC235)^2*time5+AC235^2*time6+((AD235-AC235)*2/PI()+AC235)^2*time7+AE235^2*time8)/time)/(C235+(E235-C235)/G235*mspeed))))","v":10.974409479120073},{"$f":"IF(move1,MAX(ABS(X235),ABS(Z235))/H235,MAX(ABS(X235),ABS(Z235),ABS(AB235),ABS(AD235))/H235)","v":8.7869276052298613},{"$f":"IF(AZ235>0,speed/(MIN(AZ235,I235)),\"NA\")","v":"NA"},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M235+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M235+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.301698647321805},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M235+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M235+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-9.9643759043306623},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M235+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M235+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M235+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M235+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH235/Irms","v":1.4412297255240265},{"$f":"AI235/Ipeak","v":2.0502831078869677},{"$f":"IF(move1,IF(AccType=1,SQRT((X235^2*time1+Y235^2*time2+Z235^2*time3+AA235^2*time4)/time)/(C235/D235),SQRT((((X235-Y235)*2/PI()+Y235)^2*time1+Y235^2*time2+((Z235-AA235)*2/PI()+AA235)^2*time3+AA235^2*time4)/time)/(C235/D235)),IF(AccType=1,SQRT((X235^2*time1+Y235^2*time2+Z235^2*time3+AA235^2*time4+AB235^2*time5+AC235^2*time6+AD235^2*time7+AE235^2*time8)/time)/(C235/D235),SQRT((((X235-Y235)*2/PI()+Y235)^2*time1+Y235^2*time2+((Z235-AA235)*2/PI()+AA235)^2*time3+AA235^2*time4+((AB235-AC235)*2/PI()+AC235)^2*time5+AC235^2*time6+((AD235-AE235)*2/PI()+AE235)^2*time7+AE235^2*time8)/time)/(C235/D235)))","v":17.294756706288318},{"$f":"IF(move1,MAX(ABS(X235),ABS(Z235))/(C235/D235),MAX(ABS(X235),ABS(Z235),ABS(AB235),ABS(AD235))/(C235/D235))","v":49.20679458928722},31.326018370370363,{"$f":"IF((C235+(E235-C235)/G235*mspeed)<0,\"NA\",U235*(C235+(E235-C235)/G235*mspeed)*mspeed/9.55)","v":204.43998414112301},{"$f":"IF(move1,IF(speed1>speed2,AM235/2*time1/time,AM235/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z235*-speed/30*PI(),((Z235-AA235)*2/PI()+AA235)*-speed/30*PI()),IF(AccType=1,X235*-speed/30*PI(),((X235-Y235)*2/PI()+Y235)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z235*-speed/30*PI(),((Z235-AA235)*2/PI()+AA235)*-speed/30*PI()),IF(AccType=1,X235*-speed/30*PI(),((X235-Y235)*2/PI()+Y235)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD235*-speed/30*PI(),((AD235-AE235)*2/PI()+AE235)*-speed/30*PI()),IF(AccType=1,AB235*-speed/30*PI(),((AB235-AC235)*2/PI()+AC235)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD235*-speed/30*PI(),((AD235-AE235)*2/PI()+AE235)*-speed/30*PI()),IF(AccType=1,AB235*-speed/30*PI(),((AB235-AC235)*2/PI()+AC235)*-speed/30*PI()),0)/2*time7/time)))","v":165.72766576849332},{"$f":"IF(move1,MAX(IF(AccType=1,Z235*-speed/30*PI(),((Z235-AA235)*2/PI()+AA235)*-speed/30*PI()),IF(AccType=1,X235*-speed/30*PI(),((X235-Y235)*2/PI()+Y235)*-speed/30*PI()),0),MAX(IF(AccType=1,Z235*-speed/30*PI(),((Z235-AA235)*2/PI()+AA235)*-speed/30*PI()),IF(AccType=1,X235*-speed/30*PI(),((X235-Y235)*2/PI()+Y235)*-speed/30*PI()),IF(AccType=1,AD235*-speed/30*PI(),((AD235-AE235)*2/PI()+AE235)*-speed/30*PI()),IF(AccType=1,AB235*-speed/30*PI(),((AB235-AC235)*2/PI()+AC235)*-speed/30*PI()),0))","v":1594.3001446929059},{"$f":"(L235^2)/1000000+((K235/1000)^2*(D235/C235*H235)^2*PI()*PI()*(O235/2)^2)/1200","v":6.4779311219441155E-4},{"$f":"SQRT(3)*L235*J235*D235/C235*H235/1000","v":1.963175667330868},{"$f":"0.75*J235^2*(D235/C235*H235)^2-(UAC_V*0.98)^2","v":-48814.427200000006},{"$f":"-AO235/2/AN235+SQRT((AO235/2/AN235)^2-AP235/AN235)","v":7296.7028009036821},{"$f":"(L235^2)/1000000+((K235/1000)^2*AV235^2*PI()*PI()*(O235/2)^2)/1200","v":4.894851702160754E-4},{"$f":"SQRT(3)*L235*J235*AV235/1000","v":0.35925796014806277},{"$f":"0.75*J235^2*AV235^2-(UAC_V*0.98)^2","v":-50738.493532061082},{"$f":"-AS235/2/AR235+SQRT((AS235/2/AR235)^2-AT235/AR235)","v":9820.8373111378278},{"$f":"D235+(F235-D235)*((0.85*UAC_V-D235*J235)/L235*1000)/G235","v":1.0247909090909086},5.6094261159268816E-3,10.981870896262656,11488.997222200793,{"$f":"IF(((AX235/2/AW235)^2-AY235/AW235)>0,-AX235/2/AW235+SQRT((AX235/2/AW235)^2-AY235/AW235),-9999)","v":-9999}]
["ACC","AHD55 G4-44",0.8,1.6,0.65,1.27,3000,2.9,8000,13.4,15,44,3.5000000000000003E-2,560,6,3279.610948742773,4789.3047986141846,5122.727272727273,0.56053476006929071,71.428571428571416,5.5858109287975273,4.2604522201979318,2.8954558072951007,12.355311438574001,0,-10.007802265244942,0,0,0,0,0,0.72375541882000949,1.0296092865478335,8.6850650258401139,24.710622877148001,15.731271111111109,205.33096663936089,166.4499337254876,1601.2483624391907,2.4962727678388402E-3,5.9230595056271387,-46274.861199999999,3279.610948742773,1.9585987040607565E-3,1.1895648043327192,-50622.429573384929,4789.3047986141846,1.1648499999999999,6.0576504600922537E-3,16.065043946597285,-17477.985799831862,828.88503908545249]
["ACC","AHD70 C4-44",1.2,2.2999999999999998,1.2,2.35,3000,4.7,8000,4.7,12.1,44,0.06,560,6,3657.3210814914219,4831.3479464332841,5122.727272727273,1.2,41.666666666666671,3.6544652311227299,2.6547146151957235,0.89095587347063254,12.4771586914199,0,-10.106498540050117,0,0,0,0,0,0.70043916929852335,0.99643975660645046,8.4052700315822797,23.914554158554811,15.224478024691358,207.35592686262873,168.09145180956534,1617.0397664080185,2.8154692215574704E-3,3.2266778639389044,-49460.706224479167,3657.3210814914219,1.996871383237737E-3,0.84889088909796928,-50712.105281302487,4831.3479464332841,2.3699583333333334,4.4479822872161463E-3,5.4532269638071309,-46965.066467097997,2693.7361001404388]
["ACC","AHD70 E4-44",1.8,3.5,1.8,3.53,3000,7,8000,2.6,7.6,44,0.08,560,6,3809.5349061610827,4876.7136458454106,5122.727272727273,1.8,31.25,2.4553438271605845,1.7963766419566594,0.66699208033992863,12.574636493696616,0,-10.185455559894258,0,0,0,0,0,0.71614194958850375,1.0187784196281979,8.5937033950620449,24.450682071076752,15.565787654320983,208.97589504124306,169.40466627682758,1629.6728895830813,2.7280914981752417E-3,2.6969955574744717,-49865.879907407412,3809.5349061610827,1.9896505866776235E-3,0.70190735438438012,-50741.539915529589,4876.7136458454106,3.5423636363636359,2.9719299673621868E-3,3.0843080928216495,-49576.730711331984,3598.2436234877841]
["ACC","AHR92 E4-64",2.2000000000000002,2.9,2,3.92,3000,7.4,6000,2.8,30,64,0.13,560,6,2054.0584859008518,3035.1644725833016,3521.875,1.9976557018277799,19.23076923076923,2.0762609425273237,1.7322068918092446,1.2473627647725714,12.81833099938841,0,-10.382848109504613,0,0,0,0,0,0.49489712922182272,0.70403711928459067,5.9387655506618726,16.896890862830176,10.75689481481481,213.02581548777871,172.68770244498319,1661.2556975207381,1.0434953877449355E-2,3.0276500050966888,-50245.671196694217,2054.0584859008518,5.1069278952198495E-3,1.209085363344182,-50715.933473153498,3035.1644725833016,3.8954562500000001,1.1804632862420632E-2,3.3387627124872754,-50124.7805779849,1924.0593576942199]
["ACC","AHR92 G4-64",3,4,2.4,4.7,3000,9.1999999999999993,6000,1.5,19,64,0.16,560,6,2373.09637961821,3209.9955062689905,3521.875,2.3580008987462016,15.625,1.5660308255180271,1.4091899676960316,0.95800398378187834,12.96454770280349,0,-10.501283639270826,0,0,0,0,0,0.50629570389512824,0.72025265015574946,6.0755484467415384,17.286063603737986,11.00464987654321,215.45576775570015,174.65752414587649,1680.205382283332,8.1168820967928174E-3,2.0396630309931099,-50551.240000000005,2373.09637961821,4.6840007228739758E-3,0.77998577991845475,-50768.027564888005,3209.9955062689905,4.6908854166666671,7.3320905849021054E-3,1.8298188197452236,-50600.799836847305,2505.2087889296713]
["ACC","AHR92 J4-64",3.8,5.0999999999999996,3.4,3.33,3000,11.4,6000,5,15,64,0.2,560,6,1936.8451411614681,3207.911625341414,3521.875,3.3722784499544778,12.5,1.2367485771192537,1.1543423953821863,1.0269446855777267,13.159503307356925,0,-10.659197678959108,0,0,0,0,0,0.5172901545287828,0.73589327705614382,6.2074818543453931,17.661438649347453,11.243621052631578,218.69570411292875,177.28395308040098,1705.4716286334572,7.9947589840485764E-3,8.4801207538572232,-46415.972500000003,1936.8451411614681,4.3038665957418117E-3,1.9580834379566157,-50571.145671997074,3207.911625341414,3.5328124999999999,6.2015033023614819E-3,6.2318473357468651,-48434.80348046538,2337.0294755942341]
["ACC","AHR115 A6-44",3.7,7.2,3.2,6.27,3000,11,6000,1.29,6.9,44,0.27,560,6,3476.6045176431603,4827.5996626272909,5122.727272727273,2.8954000562287852,9.2592592592592595,1.3090854889565686,1.227334146847767,0.61796570849148047,13.500675615325438,0,-10.935547248413604,0,0,0,0,0,0.76947481597879763,1.0946493742155758,9.2336977917455716,26.27158498117382,16.725010450450448,224.36559273807876,181.88020371581882,1749.6875597461769,3.5507530194128292E-3,2.1043911740374783,-50233.302792695402,3476.6045176431603,2.0581806516248228E-3,0.57886146250367976,-50761.890295354875,4827.5996626272909,5.8880518181818173,2.9218072002133253E-3,1.6442559115803823,-50456.041004291452,3883.7106444929664]
["ACC","AHR115 A6-88",3.7,3.6,3.2,3.14,3000,11,6000,5.5,28,88,0.27,560,6,1544.8355899847402,2297.8565377653895,2561.3636363636365,3.317023910372435,9.2592592592592595,1.3090854889565686,1.227334146847767,1.3585362815818418,13.500675615325438,0,-10.935547248413604,0,0,0,0,0,0.38473740798939882,0.54732468710778792,4.6168488958727858,13.13579249058691,8.3625052252252239,224.36559273807876,181.88020371581882,1749.6875597461769,1.4391586469332376E-2,8.972210431942738,-48206.355763330903,1544.8355899847402,8.3736312939195826E-3,2.76128100809757,-50559.012246717451,2297.8565377653895,3.2938560606060605,1.1802353523247463E-2,7.0103934214667483,-49218.58923799896,1766.6072172952988]
["ACC","AHR115 C6-64",6.8,9.1,5.2,6.93,3000,22,6000,0.9,6.7,64,0.51,560,6,2482.3406190306305,3372.3718339220213,3521.875,5.001401688574922,4.9019607843137258,0.78610911067490741,0.66683678375663868,0.7541305285643195,14.670409242646052,0,-11.883031486543301,0,0,0,0,0,0.57501985952253387,0.81801914281911203,6.900238314270406,19.632459427658688,12.498411851851849,243.80521088145017,197.63877732296544,1901.2850378469277,6.9761886528627113E-3,2.9372321365436265,-50278.58940527682,2482.3406190306305,4.2580300404653918E-3,0.69666753696081485,-50775.536851986391,3372.3718339220213,6.9830067708333328,4.6150632448627073E-3,1.246918138060517,-50710.262243467761,3182.4729394910114]
["ACC","AHR115 C6-88",6.8,6.6,5.2,5.09,3000,22,6000,1.7,12.6,88,0.51,560,6,1750.1741098782968,2414.8811533023481,2561.3636363636365,5.5120633849054146,4.9019607843137258,0.78610911067490741,0.66683678375663868,1.0526805660711034,14.670409242646052,0,-11.883031486543301,0,0,0,0,0,0.41704737064271685,0.59328860907759773,5.004568447712602,14.238926617862345,9.0647822222222203,243.80521088145017,197.63877732296544,1901.2850378469277,1.3102182558134706E-2,5.5328630996980221,-49816.892500000002,1750.1741098782968,8.1054579618875331E-3,1.4370440111359264,-50738.492402829885,2414.8811533023481,5.5459742424242426,8.7096435603368563E-3,2.3488192399180257,-50627.055925174041,2279.8938988277018]
["ACC","AHR115 E6-88",9.8000000000000007,9.5,8,7.84,3000,33,6000,1.01,8.1,88,0.75,560,6,1799.3009144392217,2427.9667976529399,2561.3636363636365,8.3432199214082363,3.3333333333333335,0.58424931485116871,0.48000432939292931,1.0016160935495615,15.840142869966668,0,-12.830515724673001,0,0,0,0,0,0.44974335941850391,0.63980168905052437,5.3969203130220471,15.355240537212584,9.7754497354497332,263.24482902482163,213.39735093011222,2052.8825159476796,1.2713972497676246E-2,4.92465876081656,-50022.222761154211,1799.3009144392217,8.0810782464105831E-3,1.2825210826915443,-50752.058878888551,2427.9667976529399,8.331051893939394,8.2080924897523187E-3,1.5048784400954502,-50732.049878633006,2396.1276335874331]
["ACC","AHR142 C6-64",11.3,15,9.75,13,2000,30,6000,0.43,4.7,64,1.1499999999999999,560,6,2611.7345412299524,3357.8047590126666,3521.875,8.6977013117651829,2.1739130434782612,0.57100802409467233,0.59298996385003422,0.72889014142788322,17.789698915501027,0,-14.40965612155583,0,0,0,0,0,0.69165504495288122,0.98394352408744601,8.2998605394345741,23.614644578098705,15.033549655850539,295.64419259710741,239.66164027535686,2305.5449794489327,6.6891334372540679E-3,1.8982050620294668,-50585.23919570836,2611.7345412299524,4.3332734812526153E-3,0.5741895651409471,-50785.037096147666,3357.8047590126666,12.046093750000001,4.4655556083270358E-3,0.71658975254261625,-50773.818393954527,3292.6772686188915]
["ACC","AHR142 C6-130",11.3,7.4,9.75,6.37,2000,30,6000,1.7,19,130,1.1499999999999999,560,6,1223.9040199294702,1605.0867242277186,1733.8461538461538,10.056057788723518,2.1739130434782612,0.57100802409467233,0.59298996385003422,1.5136164945791599,17.789698915501027,0,-14.40965612155583,0,0,0,0,0,0.34121648884342143,0.48541213854980686,4.0945978661210569,11.649891325195364,7.4165511635529331,295.64419259710741,239.66164027535686,2305.5449794489327,2.7213765970660598E-2,7.5201660814994913,-49968.578670216935,1223.9040199294702,1.809074014054831E-2,2.5552140853258449,-50708.575399085101,1605.0867242277186,6.6753553846153846,1.8369847252236376E-2,2.8389313985179139,-50685.936161457241,1585.6063993721782]
["ACC","AHR142 G6-64",21,28,17,22.66,2000,60,6000,0.15,2.1,64,2.2000000000000002,560,6,2757.4448647758572,3427.5599229375766,3521.875,14.144880154124847,1.1363636363636362,0.40062154486837193,0.38178805891714535,0.6993688351159566,22.907283535028721,0,-18.554899663373263,0,0,0,0,0,0.89458263470191823,1.2726268630571511,10.734991616423018,30.543044713371629,19.444306172839507,380.69252197435748,308.60539980662395,2968.783946139722,6.1851978596225952E-3,1.3302150202128977,-50697.16,2757.4448647758572,4.2268257311511848E-3,0.33287305861959976,-50798.397031667802,3427.5599229375766,20.019203125000001,4.2194197038820276E-3,0.32331385160911846,-50798.779882407085,3431.6656383495779]
["ACC","AHR142 G6-130",21,13.8,17,11.11,2000,60,5400,0.6,8.4,130,2.2000000000000002,560,6,1316.6289225750356,1651.8609217589142,1733.8461538461538,17.696278156482173,1.1363636363636362,0.40062154486837193,0.38178805891714535,1.4349836884738454,22.907283535028721,0,-18.554899663373263,0,0,0,0,0,0.44090144138880261,0.62722323964959592,5.2908172966656313,15.053357751590303,9.5832651851851853,380.69252197435748,308.60539980662395,2968.783946139722,2.5019731436459733E-2,5.3267985407632557,-50385.414693877552,1316.6289225750356,1.7635035195531824E-2,1.6026899256473521,-50767.162736719358,1651.8609217589142,11.862993076923077,1.7379674457291699E-2,1.2946987718454432,-50780.363477665414,1672.4928786838566]
["ACC","AHR142 J6-88",25,24,21,20.59,2000,76,6000,0.21,3,88,2.7,560,6,2016.720495841636,2476.5462580787594,2561.3636363636365,20.046907483842482,0.92592592592592582,0.36966439005870755,0.3334766919992983,0.95847958114573084,25.344228591946671,0,-20.528825159476799,0,0,0,0,0,0.71262072006893229,1.0137691436778666,8.5514486408271875,24.330459448268801,15.489251555555555,421.19172643971461,341.43576148817965,3284.6120255162882,1.1290281192967216E-2,2.3353254894857631,-50629.096430080004,2016.720495841636,8.0187998019786554E-3,0.65008334979528248,-50791.516909811435,2476.5462580787594,20.3098375,7.9038322393802408E-3,0.49578459389728469,-50797.224748077679,2503.9657048626214]
["ACC","AHR142 J6-130",25,16,21,13.73,2000,76,5400,0.43,6.3,130,2.7,560,6,1359.3964298340993,1663.8976194947124,1733.8461538461538,21.672204761010576,0.92592592592592582,0.36966439005870755,0.3334766919992983,1.4210010158739563,25.344228591946671,0,-20.528825159476799,0,0,0,0,0,0.47508048004595488,0.67584609578524457,5.7009657605514583,16.22030629884587,10.326167703703705,421.19172643971461,341.43576148817965,3284.6120255162882,2.3850711138215745E-2,4.709404576560396,-50477.07580672,1359.3964298340993,1.7505256859649525E-2,1.3897005887365006,-50776.59095079387,1663.8976194947124,14.353202307692309,1.721327118918527E-2,0.99979649346530386,-50790.373120882468,1688.9502352142454]
["ACC","AHD190 E8-180",45,21,32,15.238095238095237,2000,130,3900,0.36,5.8,180,7.8,560,6,1022.8163463116446,1206.5142707339546,1252.2222222222224,37.157657240229298,0.32051282051282054,0.41945255263976738,0.38616206286545962,1.9732757802789485,50.20106817250975,0,-40.6628652197329,0,0,0,0,0,0.68616391448945013,0.976131881132134,8.233966973873402,23.427165147171216,14.914196543209876,834.28361198635798,676.30545064004821,6506.0584351572643,4.1564679092293201E-2,6.8090381347147693,-50447.420800000007,1022.8163463116446,3.3206072714302301E-2,2.019362306810752,-50773.695307668459,1206.5142707339546,17.991965608465609,3.2953881321847692E-2,1.6739230716156139,-50783.539487270937,1216.2516886822218]
["ACC","AHD190 G8-130",56,37,40,26.143790849673202,2000,170,4000,0.123,2.2000000000000002,130,10,560,6,1467.0132688202782,1695.1958185453555,1733.8461538461538,42.438433451637152,0.25,0.40874009241643466,0.35837427307616893,1.4107764107401333,60.923626422948722,0,-49.348137402588463,0,0,0,0,0,1.1789830980707745,1.6772129297984393,14.147797176849295,40.253110315162544,25.62592592592592,1012.4801116339294,820.75904203889343,7895.7019844141541,2.1419928941999539E-2,3.1107972728202813,-50662.008229695479,1467.0132688202782,1.7201863368298813E-2,0.8039168152933569,-50795.599611746875,1695.1958185453555,29.026991226747107,1.713526943163448E-2,0.70972263705825656,-50797.708724533244,1701.1909057516009]
["ACC","AHD190 J8-180",67,32,44,20.952380952380953,2000,220,3900,0.18,3.2,180,13,560,6,1043.4016213998964,1219.9883021106061,1252.2222222222224,52.970134525728028,0.19230769230769232,0.42959445486206815,0.34338771256571105,1.959323561917454,75.545296764456424,0,-61.191690379209696,0,0,0,0,0,1.0567949828806402,1.5033889903374413,12.681539794567682,36.08133576809859,22.970091763405197,1255.4753384260725,1017.7412121282277,9790.6704606735511,4.0768674538928566E-2,5.8966247910929948,-50536.871543773676,1043.4016213998964,3.2919410072525662E-2,1.4690288960320252,-50788.508411285671,1219.9883021106061,26.177291005291004,3.2799932249336916E-2,1.2890458580350848,-50792.338709690455,1224.9125395354745]
["6SMx7","6SM27M-4000",0.32,0.8,0.3,0.75,4000,1.4350000000000001,9000,31,21,25,8.0000000000000002E-3,670,6,4407.5927779354934,8149.7619664280446,9000,0.27925119016785976,312.5,13.52127805730332,8.5182692721257371,"NA",12.223716405500433,0,-9.9012102884553492,0,0,0,0,0,0.89505847652888759,1.2733037922396286,10.740701718346651,30.559291013751086,19.45464888888889,203.14400959823161,164.67709419468358,1584.193646152856,1.0451297326641933E-3,4.8156425109188437,-41528.994882812505,4407.5927779354934,6.4167194981536808E-4,0.95930283496255109,-50437.055228333127,8149.7619664280446,0.71465000000000001,1.2980103635891182E-2,26.114741247200946,221986.72416330341,-9999]
["6SMx7","6SM27LL-4500",0.8,0.82,0.72,0.79,4000,3.6259999999999999,9000,37,42,59,1.4E-2,670,6,{"$f":"IF(AQ257<I257,IF(AQ257<0,0,AQ257),I257)","v":1619.5928747917071},{"$f":"IF(AU257<I257,IF(AU257<0,0,AU257),I257)","v":3351.0400680129405},{"$f":"IF(UAC_V*0.98/L257*1000<I257,IF(UAC_V*0.98/L257*1000<0,0,UAC_V*0.98/L257*1000),I257)","v":3820.3389830508472},{"$f":"C257+(E257-C257)/G257*Q257","v":0.73297919863974115},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M257,(inertia/gear^2+gear_inertia)/M257),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M257,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M257))","v":178.57142857142856},{"$f":"IF((C257+(E257-C257)/G257*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X257^2*time1+Y257^2*time2+Z257^2*time3+AA257^2*time4)/time)/(C257+(E257-C257)/G257*mspeed),SQRT((((X257-Y257)*2/PI()+Y257)^2*time1+Y257^2*time2+((Z257-Y257)*2/PI()+Y257)^2*time3+AA257^2*time4)/time)/(C257+(E257-C257)/G257*mspeed)),IF(AccType=1,SQRT((X257^2*time1+Y257^2*time2+Z257^2*time3+AA257^2*time4+AB257^2*time5+AC257^2*time6+AD257^2*time7+AE257^2*time8)/time)/(C257+(E257-C257)/G257*mspeed),SQRT((((X257-Y257)*2/PI()+Y257)^2*time1+Y257^2*time2+((Z257-Y257)*2/PI()+Y257)^2*time3+AA257^2*time4+((AB257-AC257)*2/PI()+AC257)^2*time5+AC257^2*time6+((AD257-AC257)*2/PI()+AC257)^2*time7+AE257^2*time8)/time)/(C257+(E257-C257)/G257*mspeed))))","v":5.4446632905128922},{"$f":"IF(move1,MAX(ABS(X257),ABS(Z257))/H257,MAX(ABS(X257),ABS(Z257),ABS(AB257),ABS(AD257))/H257)","v":3.3791946349099411},{"$f":"IF(AZ257>0,speed/(MIN(AZ257,I257)),\"NA\")","v":"NA"},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M257+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M257+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.252959746183446},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M257+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M257+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-9.9248973944085908},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M257+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M257+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M257+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M257+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH257/Irms","v":0.36785190354760172},{"$f":"AI257/Ipeak","v":0.52330348915991798},4.4142228425712204,{"$f":"IF(move1,MAX(ABS(X257),ABS(Z257))/(C257/D257),MAX(ABS(X257),ABS(Z257),ABS(AB257),ABS(AD257))/(C257/D257))","v":12.559283739838031},7.9954883555555529,{"$f":"IF((C257+(E257-C257)/G257*mspeed)<0,\"NA\",U257*(C257+(E257-C257)/G257*mspeed)*mspeed/9.55)","v":203.63000005181584},{"$f":"IF(move1,IF(speed1>speed2,AM257/2*time1/time,AM257/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z257*-speed/30*PI(),((Z257-AA257)*2/PI()+AA257)*-speed/30*PI()),IF(AccType=1,X257*-speed/30*PI(),((X257-Y257)*2/PI()+Y257)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z257*-speed/30*PI(),((Z257-AA257)*2/PI()+AA257)*-speed/30*PI()),IF(AccType=1,X257*-speed/30*PI(),((X257-Y257)*2/PI()+Y257)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD257*-speed/30*PI(),((AD257-AE257)*2/PI()+AE257)*-speed/30*PI()),IF(AccType=1,AB257*-speed/30*PI(),((AB257-AC257)*2/PI()+AC257)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD257*-speed/30*PI(),((AD257-AE257)*2/PI()+AE257)*-speed/30*PI()),IF(AccType=1,AB257*-speed/30*PI(),((AB257-AC257)*2/PI()+AC257)*-speed/30*PI()),0)/2*time7/time)))","v":165.0710585348622},{"$f":"IF(move1,MAX(IF(AccType=1,Z257*-speed/30*PI(),((Z257-AA257)*2/PI()+AA257)*-speed/30*PI()),IF(AccType=1,X257*-speed/30*PI(),((X257-Y257)*2/PI()+Y257)*-speed/30*PI()),0),MAX(IF(AccType=1,Z257*-speed/30*PI(),((Z257-AA257)*2/PI()+AA257)*-speed/30*PI()),IF(AccType=1,X257*-speed/30*PI(),((X257-Y257)*2/PI()+Y257)*-speed/30*PI()),IF(AccType=1,AD257*-speed/30*PI(),((AD257-AE257)*2/PI()+AE257)*-speed/30*PI()),IF(AccType=1,AB257*-speed/30*PI(),((AB257-AC257)*2/PI()+AC257)*-speed/30*PI()),0))","v":1587.9835831053745},{"$f":"(L257^2)/1000000+((K257/1000)^2*(D257/C257*H257)^2*PI()*PI()*(O257/2)^2)/1200","v":5.2846942461981915E-3},{"$f":"SQRT(3)*L257*J257*D257/C257*H257/1000","v":14.052902341914743},{"$f":"0.75*J257^2*(D257/C257*H257)^2-(UAC_V*0.98)^2","v":-36622.161994298134},{"$f":"-AO257/2/AN257+SQRT((AO257/2/AN257)^2-AP257/AN257)","v":1619.5928747917071},{"$f":"(L257^2)/1000000+((K257/1000)^2*AV257^2*PI()*PI()*(O257/2)^2)/1200","v":3.5643601861533002E-3},{"$f":"SQRT(3)*L257*J257*AV257/1000","v":3.0210916891893285},{"$f":"0.75*J257^2*AV257^2-(UAC_V*0.98)^2","v":-50149.673430444644},{"$f":"-AS257/2/AR257+SQRT((AS257/2/AR257)^2-AT257/AR257)","v":3351.0400680129405},{"$f":"D257+(F257-D257)*((0.85*UAC_V-D257*J257)/L257*1000)/G257","v":0.79900508474576271},1.1828368378416656E-2,30.231476473851099,14832.743604496747,{"$f":"IF(((AX257/2/AW257)^2-AY257/AW257)>0,-AX257/2/AW257+SQRT((AX257/2/AW257)^2-AY257/AW257),-9999)","v":-662.22086953736448}]
["6SMx7","6SM37S-6000",0.5,1,0.4,0.95,4500,2,9000,36,32,30,4.4999999999999998E-2,670,6,2681.3481874294775,6333.7246995481728,7513.3333333333339,0.35925056223226287,55.555555555555557,8.8979002678439549,6.2020251698561797,"NA",12.404050339712359,0,-10.047280775167012,0,0,0,0,0,0.72661046978182409,1.0336708616426966,8.719325637381889,24.808100679424719,15.793327407407405,206.14095072866803,167.10654095911869,1607.5649240267219,2.1127769888058603E-3,7.4824594886975495,-35253.160000000003,2681.3481874294775,9.6710761983646865E-4,1.7601100306514927,-49944.60796666667,6333.7246995481728,0.94092592592592583,1.9806373918324936E-2,29.54323312941565,191640.01326083406,-9999]
["6SMx7","6SM37M-6000",1,1.6,0.8,1.5,6000,4.03,9000,12.8,21,38,7.0000000000000007E-2,670,6,3184.0689897517441,5358.8673293163147,5931.5789473684208,0.82137108902278955,35.714285714285708,4.4697674106717251,3.108163174332073,1.6183871827387455,12.525897592558255,0,-10.145977049972187,0,0,0,0,0,0.58699847774908831,0.83505983950388363,7.0439817329890602,20.041436148093208,12.758774518518516,208.16591095193584,168.74805904319646,1623.3563279955499,2.8012181407337847E-3,5.4322434185440853,-45696.214612480006,3184.0689897517441,1.5197415989163035E-3,1.2832806002497192,-50520.047621368205,5358.8673293163147,1.5232368421052631,6.7579507248772264E-3,10.748878552560511,-30801.976111894848,1482.957864222921]
["6SMx7","6SM37L-4000",1.5,1.6,1.2,1.5,4000,6.1440000000000001,9000,15.5,30,58,0.1,670,6,1935.3250108665932,3461.1535460297105,3886.2068965517242,1.2404134840477716,25,3.0378412667251284,2.0625186028602434,1.6374746205967881,12.672114295973335,0,-10.2644125797384,0,0,0,0,0,0.39590040003829574,0.56320507982103718,4.7508048004595489,13.516921915704891,8.6051397530864211,210.59586321985731,170.71788074408983,1642.3060127581441,6.2252998985817109E-3,10.204700187062571,-43066.165803520002,1935.3250108665932,3.5192218971947095E-3,2.3768132158769197,-50385.329362130862,3461.1535460297105,1.5264224137931035,8.2970938080321084E-3,13.39918079346017,-37462.558488716415,1465.6715712181876]
["6SMx7","6SM37VL-6000",3,3.8,2,2.8,6000,12,9000,3.65,8,48,0.16,670,6,3159.4135010284954,4443.4955927933088,4695.8333333333339,2.259417401201115,15.625,1.5579713549630436,1.0803789752336241,0.65347386593070156,12.96454770280349,0,-10.501283639270826,0,0,0,0,0,0.48098091870037174,0.68424001764796205,5.7717710244044609,16.421760423551088,10.454417382716048,215.45576775570015,174.65752414587649,1680.205382283332,3.3985312323972887E-3,4.612520582588223,-48496.637200000005,3159.4135010284954,2.3515859476658414E-3,0.96175310950499182,-50704.794435368654,4443.4955927933088,3.1693402777777777,2.8217744935843366E-3,3.1724483787332809,-49713.099592477498,3672.6793910600109]
["6SMx7","6SM47L-3000",3,2.2999999999999998,2.2000000000000002,2,3000,11.97,6000,11,25,81,0.16,670,6,1464.3501077272053,2502.0679857364253,2782.7160493827164,2.3327818704702867,15.625,1.5824025342666197,1.0830866919635329,1.2919923536032045,12.96454770280349,0,-10.501283639270826,0,0,0,0,0,0.29112002973969869,0.41414527383955591,3.4934403568763845,9.9394865721493417,{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X262),ABS(Z262))/(C262/D262),MAX(ABS((X262-Y262)*2/PI()+Y262),ABS((Z262-Y262)*2/PI()+Y262))/(C262/D262)),IF(AccType=1,MAX(ABS(X262),ABS(Z262),ABS(AB262),ABS(AD262))/(C262/D262),MAX(ABS((X262-Y262)*2/PI()+Y262),ABS((Z262-Y262)*2/PI()+Y262),ABS((AB262-AC262)*2/PI()+AC262),ABS((AD262-AC262)*2/PI()+AC262))/(C262/D262)))","v":6.3276736790123458},215.45576775570015,174.65752414587649,1680.205382283332,1.0457211191936206E-2,14.162471962604092,-43162.437393250002,1464.3501077272053,6.763060902804225E-3,3.2252171677578554,-50408.801755098313,2502.0679857364253,2.0898765432098765,{"$f":"(L262^2)/1000000+((K262/1000)^2*AJ262^2*PI()*PI()*(O262/2)^2)/1200","v":8.4133761247113213E-3},{"$f":"SQRT(3)*L262*J262*AJ262/1000","v":9.765228404437206},{"$f":"0.75*J262^2*AJ262^2-(UAC_V*0.98)^2","v":-47171.579532433047},1857.5961330627856]
["6SMx7","6SM57S-3000",4.5999999999999996,2.8,3,2.7,3000,18.149999999999999,6000,6.3,35,97,0.31,670,6,1258.8837933242057,2100.0127429366657,2323.7113402061859,3.4799932037671115,8.064516129032258,1.1042509673491319,0.75458023250021344,1.3169631352741666,13.695631219878873,0,-11.093461288101887,0,0,0,0,0,0.24416892356040795,0.34735296572156565,2.9300270827248953,8.3364711773175753,5.3071623832528179,227.60552909530733,184.50663265034322,1774.9538060963018,2.0476531215102099E-2,11.69364055413944,-47171.903824810972,1258.8837933242057,1.0089210011486905E-2,2.8989843589217728,-50581.860225494929,2100.0127429366657,2.7388797250859107,1.1963005624616566E-2,5.6173991863864421,-49966.729411754306,1822.3744732994107]
["6SMx7","6SM57M-3000",8,4.3,6,4,3000,31.45,6000,3.9,24,112,0.45,670,6,1151.9416376707641,1838.1189804871251,2012.5000000000002,6.7745873463419164,5.5555555555555554,0.6563795467055854,0.45716934295122097,1.3355539291267808,14.377975835815899,0,-11.646160427010878,0,0,0,0,0,0.22635200906636635,0.3220067504896269,2.7162241087963963,7.7281620117510457,4.91990074074074,238.94530634560732,193.69913392117886,1863.3856683217405,2.4727771036915383E-2,12.78917044650211,-47545.376822590828,1151.9416376707641,1.3274923984063582E-2,3.132475026881822,-50609.600374002752,1838.1189804871251,4.1404196428571431,1.3576039154020187E-2,3.7221990847461268,-50529.03663371961,1797.0071800613707]
["6SMx7","6SM77K-3000",11,6,8.5,5,3000,44.4,6000,2.2000000000000002,18,112,1.2,670,6,1172.1468156723388,1869.5884681850955,2012.5000000000002,9.4420096098457531,2.0833333333333335,0.59661066889332715,0.40615750948632484,1.3030964569530634,18.033393421192823,0,-14.607048671166185,0,0,0,0,0,0.28810059705584024,0.40984985048165506,3.4572071646700828,9.836396411559722,6.2620444444444443,299.69411304364314,242.94467644351244,2337.1277873865897,2.6610598435494747E-2,10.335770707054216,-48676.091200000003,1172.1468156723388,1.3258305565900257E-2,2.3291118149486367,-50697.045326719286,1869.5884681850955,5.4574404761904765,1.3484455629231153E-2,2.6724985393647342,-50662.816081734163,1841.7669599161884]
["6SMx7","6SM77S-3000",17,10,12,8,3000,68,6000,1.1000000000000001,8.3000000000000007,103,1.8,670,6,1425.9228698601162,2070.1027146303572,2188.3495145631068,13.549828808949405,1.3888888888888888,0.453366748892223,0.30820187484550532,1.1504599708004231,20.95772748949436,0,-16.975759266490428,0,0,0,0,0,0.36107997458243885,0.51366979140917557,4.3329596949892659,12.328074993820213,7.8482962962962954,348.2931584020717,282.34111046137929,2716.1214826384689,1.8768004566292549E-2,7.8496542599021524,-49353.16,1425.9228698601162,1.1004418804049393E-2,1.7280670907114688,-50734.790128428693,2070.1027146303572,8.8058252427184467,1.0923100027691163E-2,1.5401603113799125,-50749.261852560332,2086.1221258573819]
["6SMx7","6SM107K-3000",26,16,20,14,3000,112,6000,0.45,4.4000000000000004,97,8.1999999999999993,670,6,1604.0537817428224,2229.1394792015622,2323.7113402061859,21.541721041596876,0.30487804878048785,0.73034680333202073,0.46563057337539376,1.1029772013016863,52.150624218044101,0,-42.242005616615721,0,0,0,0,0,0.93997062435127898,1.3371954927703615,11.279647492215348,32.092691826488675,20.430842165242158,866.68297555864353,702.56973998529281,6758.7208986585165,1.62166258145609E-2,5.210861531103216,-50083.694437869824,1604.0537817428224,9.7189175345253568E-3,1.111820733886538,-50772.315241144119,2229.1394792015622,14.705841924398625,1.0007189656523521E-2,1.5446537537162108,-50741.764442053631,2175.9289286919288]
["6SMx7","6SM107S-3000",32,20,23,16,3000,136,6000,0.37,3.6,97,10.4,670,6,1596.1466860345406,2232.7764009030457,2323.7113402061859,25.301670797290864,0.24038461538461536,0.72109192611992701,0.46230281226825798,1.1033584376340679,62.873182468483087,0,-50.927277799471298,0,0,0,0,0,1.1509424189815241,1.6373224601167469,13.811309027778288,39.295739042801927,25.016444444444446,1044.8794752062154,847.02333138413815,8148.3644479154082,1.6340127082753023E-2,5.2838807961099956,-50063.333125000005,1596.1466860345406,9.6999274412496988E-3,1.0825386829337786,-50774.022525240514,2232.7764009030457,17.41443298969072,1.0009367505570492E-2,1.5551048280817952,-50740.903675567992,2175.1770939879893]
["6SM45100","6SM45S-3000",0.85,1.3,0.8,1.4,3000,3.2,8000,25.4,54,41.012193308819754,0.15,560,6,1833.2036089396472,4271.9813660384234,5495.926499291304,0.77880031056602639,16.666666666666668,5.3883336008839748,4.0361902505203524,"NA",12.915808801665129,0,-10.461805129348754,0,0,0,0,0,0.57856768020302407,0.82306624716493471,6.9428121624362893,19.753589931958434,12.575525925925923,214.64578366639302,174.00091691224537,1673.8888206958006,6.8520808926598887E-3,8.8304278132491891,-39215.318239446366,1833.2036089396472,2.1246596314443067E-3,2.5838543821086586,-49812.84378895034,4271.9813660384234,1.4320582871347014,3.5817073493693327E-2,22.689947792584771,25715.905818998595,-9999]
["6SM45100","6SM45M-3000",1.7,1.3,1.6,1.3,3000,7.6,8000,34,99,82.024386617639507,0.21,560,6,494.52328583060807,2126.9534645838867,2747.963249645652,1.6291015511805371,11.904761904761905,2.7551668034708627,1.7379266063809584,7.003069150463058,13.208242208495284,0,-10.698676188881178,0,0,0,0,0,0.29583366289626328,0.42085085468244771,3.5500039547551596,10.100420512378745,6.4301274074074071,219.50568820223589,177.94056031403207,1711.7881902209886,3.1232590220516127E-2,28.073112044089445,-21520.840000000004,494.52328583060807,7.9540780079170974E-3,6.2795119045989551,-49339.93,2126.9534645838867,1.3,3.672449794573892E-2,31.060047386848328,-14957.711141748521,342.70688300162033]
["6SM45100","6SM45L-3000",3.2,2.4,2.9,2.2999999999999998,3000,13.1,8000,11.9,47,82.024386617639507,0.34,560,6,1023.0108963640904,2322.0481426247734,2747.963249645652,2.9677951857375224,7.3529411764705879,1.5420752099048136,1.0566296124651871,1.6376068515580706,13.841847923293949,0,-11.211896817868098,0,0,0,0,0,0.30406292743325841,0.43255774760293586,3.6487551291991007,10.381385942470461,6.6089955555555546,230.0354813632288,186.47645435123661,1793.903490858896,2.251217338009889E-2,16.610516586107426,-40552.883645312511,1023.0108963640904,7.6173502031355199E-3,3.9428351729386439,-50227.501364411342,2322.0481426247734,2.332158387326849,1.3870128246713898E-2,11.173417841533418,-46166.141485527005,1465.5532234226821]
["6SM45100","6SM56S-3000",3.8,2.8,3.6,2.9,3000,16.5,8000,9.4,54,80.610173055266415,0.52,560,6,846.3007390214168,2247.2623580615045,2796.1731312183829,3.6501825094625664,4.8076923076923075,1.3722798385782449,0.89206958447178253,1.6710199471489575,14.719148143784412,0,-11.922509996465372,0,0,0,0,0,0.31766198596190171,0.45190367108110036,3.8119438315428207,10.845688105946408,6.904579493177387,244.6151949707573,198.29538455659664,1907.6015994344596,3.8403480263062589E-2,15.956466082438178,-41009.499418282554,846.3007390214168,8.2758685049424685E-3,3.7666380431420459,-50259.316580946259,2247.2623580615045,2.8699580849363393,1.6788180588993569E-2,9.0618228633388753,-47645.855844624071,1436.2485642944034]
["6SM45100","6SM56M-3000",7,4.8,6.4,4.7,3000,28.4,8000,4,30,87.681240867131891,1,560,6,1018.768960700905,2194.865510977339,2570.6752980556098,6.5610268978045321,2.5,0.86771021932173942,0.60065547177555079,1.2568805331441721,17.058615398425641,0,-13.817478472724769,0,0,0,0,0,0.34260611541775593,0.4873890113835897,4.1112733850130709,11.697336273206153,7.446755555555554,283.49443125750025,229.81253177089013,2210.7965556359632,3.2953424124805994E-2,11.830111650082614,-46254.186351020413,1018.768960700905,9.1803555047657234E-3,2.8751578488258422,-50536.347153496856,2194.865510977339,4.7329769217617264,1.1382347248988539E-2,4.5237063348860502,-50139.709980349631,1909.489356157213]
["6SM45100","6SM56L-3000",10,7.6,8.4,6.7,3000,37.4,8000,1.8,15.8,79.903066274079862,1.5,560,6,1356.762921373203,2524.8762412594501,2820.9180261849174,8.6533993379949603,1.6666666666666667,0.70212153618939532,0.521271669928973,1.0134625970151545,19.49556045534359,0,-15.791403968828309,0,0,0,0,0,0.43396774619582407,0.6173594144192136,5.207612954349889,14.816625946061126,9.432557037037034,323.99363572285733,262.64289345244595,2526.6246350125298,2.1314010606039917E-2,7.0807909488499812,-48841.905224320006,1356.762921373203,7.2687079462231746E-3,1.7232020139626001,-50688.885225901613,2524.8762412594501,6.9173478497946652,8.0286220832233926E-3,2.3497735889516966,-50588.955288615602,2368.1189686412395]
["6SM45100","6SM71K-3000",10.5,8,9.5,7.6,3000,41.9,6000,1.65,19.600000000000001,79.195959492893323,2,560,6,1077.6289891668646,2417.0956795341026,2846.1047942758541,9.6943014401553,1.25,0.74483330670510106,0.52344881890839001,1.0983432732186267,21.932505512261542,0,-17.765329464931849,0,0,0,0,0,0.48943730773965138,0.69627001626227125,5.8732476928758164,16.71048039029451,10.638222222222222,364.49284018821459,295.47325513400165,2842.4527143890959,3.5252279737932046E-2,7.2254068636721058,-48724.224718367353,1077.6289891668646,7.9549603062707454E-3,1.7411971881769674,-50684.314669638261,2417.0956795341026,7.6930819852135528,9.4901869368966846E-3,2.4077791782458013,-50574.077387946672,2185.1092081321253]
["6SM45100","6SM71S-3000",16.5,12.3,13.4,10.5,3000,59.4,6000,0.8,12,81.317279836452954,3.1,560,6,1258.6431382407568,2459.8930158145185,2771.8585822512669,13.958110550324998,0.80645161290322576,0.59831214519160081,0.45949132386331693,1.0118425385754748,27.293784637481025,0,-22.10796555635963,0,0,0,0,0,0.59592700075694516,0.84776149252781974,7.1511240090833414,20.346275820667675,12.95284148148148,453.59109001200028,367.7000508334242,3537.2744890175413,2.7512136145931836E-2,4.9893166672801996,-49864.015168000005,1258.6431382407568,7.8859218601717816E-3,1.2315664710587679,-50747.815728822832,2459.8930158145185,10.930106660920755,8.4008544598093635E-3,1.459481208044126,-50724.627470826701,2371.9105577225941]
["6SM45100","6SM71M-3000",22,15.6,16.3,12.2,3000,71.900000000000006,6000,0.56999999999999995,9,85.559920523572245,4.2,560,6,1388.9668984614173,2399.5975279223039,2634.4110492470713,17.440764696947625,0.59523809523809523,0.54286654769286546,0.45417334857719766,1.0191685143394631,32.655063762700514,0,-26.450601647787419,0,0,0,0,0,0.67820437847469417,0.96480870207978786,8.1384525416963296,23.15540884991491,14.741191111111108,542.6893398357862,439.92684653284687,4232.0962636459872,2.2905530031985463E-2,4.30662109571192,-50171.76797547876,1388.9668984614173,8.3538675201331302E-3,1.1089456080002618,-50763.162856310941,2399.5975279223039,13.128175980383242,8.6234002903863224E-3,1.2451980506496798,-50752.20876083117,2354.8608166682548]
["6SM45100","6SM100K-3000",25,18.8,19.899999999999999,15.7,3000,95.8,6000,0.46,10.5,80.610173055266415,7.4,560,6,965.23504430508376,2356.4932876059338,2796.1731312183829,20.993961411069911,0.33783783783783783,0.69984971422190057,0.50366922888283283,1.1458223799581833,48.251512126975385,0,-39.083724822850058,0,0,0,0,0,1.062764170025879,1.5118807133118954,12.753170040310547,36.285137119485491,23.099835733333329,801.88424841407209,650.04116129480349,6253.3959716560094,4.8853158010250253E-2,4.6269165018517153,-49981.508248880134,965.23504430508376,8.6942388684382709E-3,1.0536061469855365,-50762.451246808036,2356.4932876059338,16.404763856943664,1.0852691463891898E-2,1.4836012962597149,-50720.477297389065,2094.5654771445361]
["6SM45100","6SM100S-3000",36,26.7,24.6,19.2,3000,152.6,6000,0.22,7,82.024386617639507,10.8,560,6,940.17040731685256,2432.3968139668582,2747.963249645652,26.756892106925939,0.23148148148148145,0.66454488793703881,0.42478858790312873,1.0946543661990507,64.822738514017445,0,-52.506418196354126,0,0,0,0,0,1.4081349264583254,2.0032026832456782,16.897619117499904,48.076864397896273,30.606682469135801,1077.2788387785008,873.28762072938252,8401.0269114166604,5.3188478384638596E-2,3.5374441658835698,-50340.18113455917,940.17040731685256,8.3154448590824527E-3,0.65387853290845577,-50789.272769924253,2432.3968139668582,20.920438340979299,1.0125735788790547E-2,0.9566268308495034,-50771.155284872882,2192.4728700744859]
["6SM45100","6SM100M-3000",46,35,27.1,21.8,3000,198,6000,0.16,5,79.903066274079862,14.1,560,6,986.41200181245893,2566.558523092795,2820.9180261849174,29.830681304515394,0.1773049645390071,0.6589315522295921,0.40861907014987831,1.0437855403165681,80.906575889675906,0,-65.534326470637481,0,0,0,0,0,1.8030267487111977,2.5649729675168991,21.636320984534372,61.559351220405581,39.189900161030593,1344.5735882498582,1089.9680078276504,10485.492235301997,4.8384744955270238E-2,3.3359494307410067,-50369.395311909269,986.41200181245893,7.4991801633690373E-3,0.54346137497303737,-50793.594870934001,2566.558523092795,24.542829343571121,9.2266652920079371E-3,0.86779713652487689,-50775.671713127078,2299.3229042740982]
["6SM45100","6SM100L-3000",57,42,28,22.5,3000,243,6000,0.12,4,81.317279836452954,17.5,560,6,1030.4650728503389,2579.0332364888145,2771.8585822512669,32.069345380608127,0.14285714285714285,0.65091021003713112,0.40114321924575297,1.0337556296815134,97.477802276717966,0,-78.957019844141541,0,0,0,0,0,2.103721761337098,2.9927395435834465,25.244661136045174,71.825749046002713,45.725692007797271,1619.9681786142871,1313.2144672622294,12633.123175062647,4.458265832959514E-2,3.0262543328496712,-50458.913675346266,1030.4650728503389,7.4616142207498447E-3,0.4525507379471016,-50797.417006789554,2579.0332364888145,26.775806538415061,9.0887903484892906E-3,0.77283183352785878,-50782.578939776409,2321.6318548508498]
["Goldline BH","BH-122-A",0.7,1,0.6,0.85,6000,2.52,9000,34.9,120,42.6,0.03,670,4,1705.9976185610185,4266.3007524985442,5291.0798122065726,0.62889498745835759,83.333333333333343,6.2586714908630023,4.8932309476209603,"NA",12.33094198800482,0,-9.9880630102839039,0,0,0,0,0,0.51594849524221575,0.73398464214314407,6.1913819429065891,17.615631411435459,11.214459259259257,204.92597459470727,166.12163010867201,1598.0900816454246,7.9544435058296684E-3,9.2703931835218292,-38966.102800000008,1705.9976185610185,2.2034101088993356E-3,2.3324081963105749,-50055.731977256393,4266.3007524985442,0.90575117370892022,6.1394370244521899E-2,28.8784574094223,64081.285362998096,-9999]
["Goldline BH","BH-124-B",1.3,1.8,1.2,1.6,6000,4.6619999999999999,9000,12.4,58,44.9,4.5999999999999999E-2,670,4,2206.4467972913549,4325.8150911189523,5020.0445434298445,1.2279030818146841,54.347826086956523,3.3744398782298344,2.6617169090146278,1.9205117702592565,12.408924229826194,0,-10.051228626159219,0,0,0,0,0,0.50323567491554222,0.71589947479766503,6.0388280989865066,17.181587395143961,10.938138256410253,206.2219491375987,167.17220168248178,1608.1965801854749,6.6274580635321944E-3,6.2248669819393676,-46000.004154686867,2206.4467972913549,2.3251906641910658E-3,1.6118238493930448,-50482.991940135194,4325.8150911189523,1.6714328136599852,1.525702552510249E-2,10.548047139887608,-37007.944402695037,1249.6669050229334]
["Goldline BH","BH-126-B",1.9,2.6,1.7,2.2999999999999998,6000,6.66,9000,8.1999999999999993,38,44.9,7.5999999999999998E-2,670,4,{"$f":"IF(AQ284<I284,IF(AQ284<0,0,AQ284),I284)","v":2351.0224653277655},{"$f":"IF(AU284<I284,IF(AU284<0,0,AU284),I284)","v":4372.6312179277402},{"$f":"IF(UAC_V*0.98/L284*1000<I284,IF(UAC_V*0.98/L284*1000<0,0,UAC_V*0.98/L284*1000),I284)","v":5020.0445434298445},{"$f":"C284+(E284-C284)/G284*Q284","v":1.7542456260690753},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M284,(inertia/gear^2+gear_inertia)/M284),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M284,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M284))","v":32.894736842105267},{"$f":"IF((C284+(E284-C284)/G284*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X284^2*time1+Y284^2*time2+Z284^2*time3+AA284^2*time4)/time)/(C284+(E284-C284)/G284*mspeed),SQRT((((X284-Y284)*2/PI()+Y284)^2*time1+Y284^2*time2+((Z284-Y284)*2/PI()+Y284)^2*time3+AA284^2*time4)/time)/(C284+(E284-C284)/G284*mspeed)),IF(AccType=1,SQRT((X284^2*time1+Y284^2*time2+Z284^2*time3+AA284^2*time4+AB284^2*time5+AC284^2*time6+AD284^2*time7+AE284^2*time8)/time)/(C284+(E284-C284)/G284*mspeed),SQRT((((X284-Y284)*2/PI()+Y284)^2*time1+Y284^2*time2+((Z284-Y284)*2/PI()+Y284)^2*time3+AA284^2*time4+((AB284-AC284)*2/PI()+AC284)^2*time5+AC284^2*time6+((AD284-AC284)*2/PI()+AC284)^2*time7+AE284^2*time8)/time)/(C284+(E284-C284)/G284*mspeed))))","v":2.3410548769387809},{"$f":"IF(move1,MAX(ABS(X284),ABS(Z284))/H284,MAX(ABS(X284),ABS(Z284),ABS(AB284),ABS(AD284))/H284)","v":1.8851562962824733},{"$f":"IF(AZ284>0,speed/(MIN(AZ284,I284)),\"NA\")","v":1.1995930849297756},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M284+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M284+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.555140933241272},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M284+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M284+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.169664155925432},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M284+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M284+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M284+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M284+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"AH284/Irms","v":0.50321024531183378},{"$f":"AI284/Ipeak","v":0.71586329882516031},6.0385229437420058,{"$f":"IF(move1,MAX(ABS(X284),ABS(Z284))/(C284/D284),MAX(ABS(X284),ABS(Z284),ABS(AB284),ABS(AD284))/(C284/D284))","v":17.180719171803847},10.937585528265107,{"$f":"IF((C284+(E284-C284)/G284*mspeed)<0,\"NA\",U284*(C284+(E284-C284)/G284*mspeed)*mspeed/9.55)","v":208.65190140552016},{"$f":"IF(move1,IF(speed1>speed2,AM284/2*time1/time,AM284/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z284*-speed/30*PI(),((Z284-AA284)*2/PI()+AA284)*-speed/30*PI()),IF(AccType=1,X284*-speed/30*PI(),((X284-Y284)*2/PI()+Y284)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z284*-speed/30*PI(),((Z284-AA284)*2/PI()+AA284)*-speed/30*PI()),IF(AccType=1,X284*-speed/30*PI(),((X284-Y284)*2/PI()+Y284)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD284*-speed/30*PI(),((AD284-AE284)*2/PI()+AE284)*-speed/30*PI()),IF(AccType=1,AB284*-speed/30*PI(),((AB284-AC284)*2/PI()+AC284)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD284*-speed/30*PI(),((AD284-AE284)*2/PI()+AE284)*-speed/30*PI()),IF(AccType=1,AB284*-speed/30*PI(),((AB284-AC284)*2/PI()+AC284)*-speed/30*PI()),0)/2*time7/time)))","v":169.14202338337515},{"$f":"IF(move1,MAX(IF(AccType=1,Z284*-speed/30*PI(),((Z284-AA284)*2/PI()+AA284)*-speed/30*PI()),IF(AccType=1,X284*-speed/30*PI(),((X284-Y284)*2/PI()+Y284)*-speed/30*PI()),0),MAX(IF(AccType=1,Z284*-speed/30*PI(),((Z284-AA284)*2/PI()+AA284)*-speed/30*PI()),IF(AccType=1,X284*-speed/30*PI(),((X284-Y284)*2/PI()+Y284)*-speed/30*PI()),IF(AccType=1,AD284*-speed/30*PI(),((AD284-AE284)*2/PI()+AE284)*-speed/30*PI()),IF(AccType=1,AB284*-speed/30*PI(),((AB284-AC284)*2/PI()+AC284)*-speed/30*PI()),0))","v":1627.1462649480691},{"$f":"(L284^2)/1000000+((K284/1000)^2*(D284/C284*H284)^2*PI()*PI()*(O284/2)^2)/1200","v":5.961796987756271E-3},{"$f":"SQRT(3)*L284*J284*D284/C284*H284/1000","v":5.811855353148716},{"$f":"0.75*J284^2*(D284/C284*H284)^2-(UAC_V*0.98)^2","v":-46616.482532387818},{"$f":"-AO284/2/AN284+SQRT((AO284/2/AN284)^2-AP284/AN284)","v":2351.0224653277655},{"$f":"(L284^2)/1000000+((K284/1000)^2*AV284^2*PI()*PI()*(O284/2)^2)/1200","v":2.2910208284152938E-3},{"$f":"SQRT(3)*L284*J284*AV284/1000","v":1.5343444824982815},{"$f":"0.75*J284^2*AV284^2-(UAC_V*0.98)^2","v":-50513.220353002602},{"$f":"-AS284/2/AR284+SQRT((AS284/2/AR284)^2-AT284/AR284)","v":4372.6312179277402},{"$f":"D284+(F284-D284)*((0.85*UAC_V-D284*J284)/L284*1000)/G284","v":2.4060356347438754},7.6991533154666756E-3,6.9749690174198431,-44772.179906403398,{"$f":"IF(((AX284/2/AW284)^2-AY284/AW284)>0,-AX284/2/AW284+SQRT((AX284/2/AW284)^2-AY284/AW284),-9999)","v":2000.6784218337641}]
["Goldline BH","BH-222-B",2.1,1.3,2,1.2,3000,7.452,6000,35.4,272,98,0.1,670,4,517.66506827765829,1659.0046335469629,2300.0000000000005,2.0446998455484344,25,2.1362064891482637,1.7004984294113439,5.3818217509205111,12.672114295973335,0,-10.2644125797384,0,0,0,0,0,0.22976362502222522,0.32686009096756619,2.7571635002667025,7.8446421832215885,4.9940543209876544,210.59586321985731,170.71788074408983,1642.3060127581441,6.1401655913551671E-2,27.719594246423824,-30803.704742128986,517.66506827765829,1.3401956419819573E-2,7.5059696535391653,-49338.594495005971,1659.0046335469629,1.249156462585034,7.030877064199953E-2,30.008426729736222,-27364.258427895998,445.94565020469179]
["Goldline BH","BH-224-B",3.8,2.2000000000000002,3.5,2,3000,13.6,6000,12.5,152,103,0.17,670,4,729.58498483037692,1739.8877141382425,2188.3495145631068,3.6260112285861759,14.705882352941176,1.218104280672953,0.95685930911337125,2.1201240121078602,13.013286603941848,0,-10.540762149192895,0,0,0,0,0,0.220665386180252,0.31391700141087797,2.647984634163024,7.5340080338610713,4.7962984795321644,216.26575184500729,175.31413137950764,1686.5219438708634,5.7730776135057928E-2,17.558437160307445,-43540.132299168981,729.58498483037692,1.3933165325728037E-2,4.6635467993792021,-50292.654845178622,1739.8877141382425,2.0912621359223302,2.8094500600828774E-2,10.695819543074393,-48109.322604910645,1132.0092533709303]
["Goldline BH","BH-226-C",5.5,4.4000000000000004,4.8,3.8,4000,20,6000,3.9,44,75.400000000000006,0.25,670,4,1301.9471699443873,2594.1739655146885,2989.389920424403,5.0460195560349295,10,0.86900091499648457,0.67015989065243597,1.0821317910116721,13.403197813048719,0,-10.856590228569461,0,0,0,0,0,0.31405560579960962,0.4467732604349573,3.7686672695953156,10.722558250438976,6.8261925925925926,222.74562455946449,180.56698924855652,1737.0544365711139,2.1990272849501009E-2,8.1492297675792642,-47884.840000000004,1301.9471699443873,6.727396937383283E-3,2.0603352305865252,-50618.490615919516,2594.1739655146885,4.0452122015915117,8.6530029669377902E-3,3.4767632421740391,-50273.605802662874,2217.8444621391895]
["Goldline BH","BH-226-E",5.6,3,3.9,2.6,2500,21.39,6000,8.5,92,112,0.25,670,4,770.26900435891969,1705.4144296471818,2012.5000000000002,4.4403181878399156,10,0.89002224586794465,0.62661046344313787,1.6526063771359072,13.403197813048719,0,-10.856590228569461,0,0,0,0,0,0.21030509316938148,0.29917852261269468,2.5236611180325776,7.1802845427046718,4.5711111111111116,222.74562455946449,180.56698924855652,1737.0544365711139,4.9107029253663552E-2,18.894769054688123,-43689.959552973538,770.26900435891969,1.4660765182082588E-2,4.5462869597067881,-50393.23547193878,1705.4144296471818,2.7571428571428571,1.8362321312941594E-2,7.5373616502956891,-49672.909110185188,1452.2514454769216]
["Goldline BH","BH-422-D",5.8,4,5.2,3.4,3600,20.88,6000,6.1,89,87.4,0.32,670,4,753.33152415535017,1979.506774888534,2578.9473684210525,5.4700822041852444,7.8125,0.84383677199838847,0.65825527399507822,1.5483581672605773,13.744370121017232,0,-11.132939798023957,0,0,0,0,0,0.27762909352818155,0.39495316439704692,{"$f":"IF(move1,IF(AccType=1,SQRT((X289^2*time1+Y289^2*time2+Z289^2*time3+AA289^2*time4)/time)/(C289/D289),SQRT((((X289-Y289)*2/PI()+Y289)^2*time1+Y289^2*time2+((Z289-AA289)*2/PI()+AA289)^2*time3+AA289^2*time4)/time)/(C289/D289)),IF(AccType=1,SQRT((X289^2*time1+Y289^2*time2+Z289^2*time3+AA289^2*time4+AB289^2*time5+AC289^2*time6+AD289^2*time7+AE289^2*time8)/time)/(C289/D289),SQRT((((X289-Y289)*2/PI()+Y289)^2*time1+Y289^2*time2+((Z289-AA289)*2/PI()+AA289)^2*time3+AA289^2*time4+((AB289-AC289)*2/PI()+AC289)^2*time5+AC289^2*time6+((AD289-AE289)*2/PI()+AE289)^2*time7+AE289^2*time8)/time)/(C289/D289)))","v":3.3315491223381786},9.4788759455291256,6.0344398467432949,228.41551318461447,185.16323988397431,1781.270367683833,6.1674796721863108E-2,13.297328172680706,-45018.260800000004,753.33152415535017,1.1155750252247885E-2,3.3924091454611327,-50428.513796617248,1979.506774888534,3.6737223493516398,1.712802180639704E-2,5.5723560403087946,-49788.923338553446,1550.0289601896081]
["Goldline BH","BH-424-B",11.3,4.2,10.8,4,2000,37.659999999999997,6000,6.3,134,162,0.7,670,4,482.36826164063848,1083.716414797595,1391.3580246913582,11.029070896300603,3.5714285714285716,0.49000123847891647,0.41413829963555165,2.1410056304979901,15.596448364274874,0,-12.633123175062646,0,0,0,0,0,0.16978710144596754,0.2415379171458498,2.0374452173516104,5.7969100115003949,3.6904275319567352,259.19490857828589,210.11431476195671,2021.2997080100233,0.14198584808355877,24.743854540325753,-44972.795102187178,482.36826164063848,3.6153110611384508E-2,7.2400153304979362,-50305.828514842964,1083.716414797595,4.0956543209876548,3.4289285319677607E-2,6.5236833515322843,-50399.748815814477,1120.9685606673388]
["Goldline BH","BH-424-D",11.1,6.3,10,5.6,3000,39.375,6000,3.3,60,106,0.66,670,4,724.24472880473536,1699.5973618266596,2126.4150943396226,10.476814300663557,3.7878787878787876,0.49505803940934268,0.39114902246911587,1.3856251111579261,15.401492759721437,0,-12.475209135374364,0,0,0,0,0,0.2560286240892149,0.36422449093935833,3.0723434890705787,8.7413877825445994,5.5649403003003002,255.95497222105735,207.48788582743228,1996.0334616598984,7.0386342865758539E-2,13.539997057450774,-46726.049989414038,724.24472880473536,1.5380306848890506E-2,3.5839825672972609,-50519.361427494427,1699.5973618266596,5.91541823899371,1.490376929751136E-2,3.3716380175544622,-50552.224281741313,1732.0702264080583]
["Goldline BH","BH-426-B",15.8,8.1,14.4,7.2,2500,52.65,6000,2.1,48,118,1,670,4,757.01444128764535,1578.8672716698568,1910.1694915254236,14.91583432786488,2.5,0.3856408383081204,0.32400029246772349,1.4174064794961436,17.058615398425641,0,-13.817478472724769,0,0,0,0,0,0.25614143913748361,0.36438498082080084,3.0736972696498035,8.7452395396992202,5.5673924050632895,283.49443125750025,229.81253177089013,2210.7965556359632,6.9146184205421249E-2,11.584791899217443,-48395.518313915294,757.01444128764535,1.8250952466400981E-2,3.2428175059620146,-50616.351730519724,1578.8672716698568,7.555454237288135,1.6273441472718395E-2,2.3895370134859424,-50702.641199030106,1693.2334053200791]
["Goldline BH","BH-426-H",15.7,9.1,13,7.5,3000,51.034999999999997,6000,1.9,39.700000000000003,105,1,670,4,840.54207705646866,1772.9891677454721,2146.6666666666665,14.104309749029074,2.5,0.39203381309000557,0.33425326537524525,1.2715888506090247,17.058615398425641,0,-13.817478472724769,0,0,0,0,0,0.28959672972546513,0.41197823812545997,3.4751607567055816,9.8874777150110393,6.2945638122198622,283.49443125750025,229.81253177089013,2210.7965556359632,5.6396090971919492E-2,10.221470660891582,-48436.033866860154,840.54207705646866,1.4507065166990303E-2,2.8316672805251768,-50623.338240644065,1772.9891677454721,8.194806349206349,1.3079427337727849E-2,2.1750496146827234,-50697.884697815614,1887.4025191794701]
["Goldline BH","BH-622-B",14.9,8.4,12.7,6.7,3000,66.728999999999999,6000,1.91,32,107,1.03,670,6,575.166034470976,1716.4957346537788,2106.5420560747662,13.641236461253895,2.4271844660194173,0.4150633178962832,0.25783140916004621,1.3291143971751105,17.204832101840722,0,-13.935914002490984,0,0,0,0,0,0.28408715140848156,0.40414035138552035,3.409045816901779,9.6993684332524879,6.1748097240865034,285.92438352542172,231.78235347178349,2229.7462403985573,0.11871849445291584,13.316356288955962,-46933.089408367174,575.166034470976,1.5655569187229254E-2,2.6370071524696712,-50653.316897498124,1716.4957346537788,7.4496099688473523,1.4339068418682106E-2,2.1857543516569891,-50700.838179627317,1805.7136429346801]
["Goldline BH","BH-624-D",25.8,12.4,23.7,11.1,2500,91.08,6000,1.01,23,125,2.0299999999999998,670,6,686.80595215675226,1496.8253688956274,1803.2,24.542666690127675,1.2315270935960592,0.30526427270074941,0.24241021317167999,1.4408502638515035,22.078722215676613,0,-17.883764994698055,0,0,0,0,0,0.31080217563382079,0.44214495393150838,3.7296261076058492,10.611478894356202,6.7554772782084394,366.92279245613594,297.4430768348949,2861.4023991516888,9.0660483117783408E-2,9.572315740883953,-49339.092341709205,686.80595215675226,2.0929379307617221E-2,2.5450771970063597,-50701.521312980454,1496.8253688956274,11.63881984,1.7412017296243577E-2,1.4772297717483087,-50770.244675223374,1665.6831457174569]
["Goldline BH","BH-624-C",27.6,19,18.399999999999999,12.2,3600,91.76,6000,0.53,10,90,2.0299999999999998,670,6,1084.9492208276172,2214.1516170410223,2504.4444444444448,21.941612534228497,1.2315270935960592,0.29342902671817117,0.24061379921182011,1.0177131864659374,22.078722215676613,0,-17.883764994698055,0,0,0,0,0,0.4451707179046836,0.63329668191101396,5.3420486148562034,15.199120365864335,9.6760605475040222,366.92279245613594,297.4430768348949,2861.4023991516888,3.7636352085199179E-2,5.2188754231707986,-49964.522324611848,1084.9492208276172,9.789623208391043E-3,1.2482266054507904,-50757.071430291508,2214.1516170410223,15.108259259259258,8.7930397796880961E-3,0.7994247387530885,-50785.435311329311,2358.2282630473978]
["Goldline BH","BH-626-E",35.4,20,24.9,14.4,3000,133.19999999999999,6000,0.43,10.7,108,3.04,670,6,{"$f":"IF(AQ297<I297,IF(AQ297<0,0,AQ297),I297)","v":866.33446881065015},1853.6326562018869,2087.037037037037,28.912285703293392,0.82236842105263153,0.28061258852116866,0.20271284707695855,1.2074566395262021,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.4468074104082787,0.63562502897012418,5.3616889248993447,15.25500069528298,9.711635070098346,448.73118547615752,363.76040743163765,3499.3751194923539,5.9658390536391909E-2,6.0531829050090504,-50019.815708129849,866.33446881065015,1.4047282401496924E-2,1.3488892991997823,-50766.161750225147,1853.6326562018869,16.76962962962963,1.2463306369228081E-2,0.78116934679602146,-50792.080748705986,1987.6490148265234]
["Goldline BH","BH-822-D",34.700000000000003,18.100000000000001,30,15.1,3000,128.256,6000,0.58299999999999996,20.8,116,4.88,670,6,{"$f":"IF(AQ298<I298,IF(AQ298<0,0,AQ298),I298)","v":538.38010636793388},{"$f":"IF(AU298<I298,IF(AU298<0,0,AU298),I298)","v":1469.4534878819925},{"$f":"IF(UAC_V*0.98/L298*1000<I298,IF(UAC_V*0.98/L298*1000<0,0,UAC_V*0.98/L298*1000),I298)","v":1943.1034482758621},{"$f":"C298+(E298-C298)/G298*Q298","v":32.397856202318216},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M298,(inertia/gear^2+gear_inertia)/M298),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M298,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M298))","v":0.51229508196721307},{"$f":"IF((C298+(E298-C298)/G298*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X298^2*time1+Y298^2*time2+Z298^2*time3+AA298^2*time4)/time)/(C298+(E298-C298)/G298*mspeed),SQRT((((X298-Y298)*2/PI()+Y298)^2*time1+Y298^2*time2+((Z298-Y298)*2/PI()+Y298)^2*time3+AA298^2*time4)/time)/(C298+(E298-C298)/G298*mspeed)),IF(AccType=1,SQRT((X298^2*time1+Y298^2*time2+Z298^2*time3+AA298^2*time4+AB298^2*time5+AC298^2*time6+AD298^2*time7+AE298^2*time8)/time)/(C298+(E298-C298)/G298*mspeed),SQRT((((X298-Y298)*2/PI()+Y298)^2*time1+Y298^2*time2+((Z298-Y298)*2/PI()+Y298)^2*time3+AA298^2*time4+((AB298-AC298)*2/PI()+AC298)^2*time5+AC298^2*time6+((AD298-AC298)*2/PI()+AC298)^2*time7+AE298^2*time8)/time)/(C298+(E298-C298)/G298*mspeed))))","v":0.37190981527925321},{"$f":"IF(move1,MAX(ABS(X298),ABS(Z298))/H298,MAX(ABS(X298),ABS(Z298),ABS(AB298),ABS(AD298))/H298)","v":0.28044932821941215},{"$f":"IF(AZ298>0,speed/(MIN(AZ298,I298)),\"NA\")","v":1.4634952015332208},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M298+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M298+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":35.969309040108925},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M298+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M298+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-29.135140322488226},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M298+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M298+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M298+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M298+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH298/Irms","v":0.54952737374247118},{"$f":"AI298/Ipeak","v":0.78175371472859212},{"$f":"IF(move1,IF(AccType=1,SQRT((X298^2*time1+Y298^2*time2+Z298^2*time3+AA298^2*time4)/time)/(C298/D298),SQRT((((X298-Y298)*2/PI()+Y298)^2*time1+Y298^2*time2+((Z298-AA298)*2/PI()+AA298)^2*time3+AA298^2*time4)/time)/(C298/D298)),IF(AccType=1,SQRT((X298^2*time1+Y298^2*time2+Z298^2*time3+AA298^2*time4+AB298^2*time5+AC298^2*time6+AD298^2*time7+AE298^2*time8)/time)/(C298/D298),SQRT((((X298-Y298)*2/PI()+Y298)^2*time1+Y298^2*time2+((Z298-AA298)*2/PI()+AA298)^2*time3+AA298^2*time4+((AB298-AC298)*2/PI()+AC298)^2*time5+AC298^2*time6+((AD298-AE298)*2/PI()+AE298)^2*time7+AE298^2*time8)/time)/(C298/D298)))","v":6.5943284849096537},{"$f":"IF(move1,MAX(ABS(X298),ABS(Z298))/(C298/D298),MAX(ABS(X298),ABS(Z298),ABS(AB298),ABS(AD298))/(C298/D298))","v":18.762089153486212},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X298),ABS(Z298))/(C298/D298),MAX(ABS((X298-Y298)*2/PI()+Y298),ABS((Z298-Y298)*2/PI()+Y298))/(C298/D298)),IF(AccType=1,MAX(ABS(X298),ABS(Z298),ABS(AB298),ABS(AD298))/(C298/D298),MAX(ABS((X298-Y298)*2/PI()+Y298),ABS((Z298-Y298)*2/PI()+Y298),ABS((AB298-AC298)*2/PI()+AC298),ABS((AD298-AC298)*2/PI()+AC298))/(C298/D298)))","v":11.944316926032659},{"$f":"IF((C298+(E298-C298)/G298*mspeed)<0,\"NA\",U298*(C298+(E298-C298)/G298*mspeed)*mspeed/9.55)","v":597.7682579086719},{"$f":"IF(move1,IF(speed1>speed2,AM298/2*time1/time,AM298/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z298*-speed/30*PI(),((Z298-AA298)*2/PI()+AA298)*-speed/30*PI()),IF(AccType=1,X298*-speed/30*PI(),((X298-Y298)*2/PI()+Y298)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z298*-speed/30*PI(),((Z298-AA298)*2/PI()+AA298)*-speed/30*PI()),IF(AccType=1,X298*-speed/30*PI(),((X298-Y298)*2/PI()+Y298)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD298*-speed/30*PI(),((AD298-AE298)*2/PI()+AE298)*-speed/30*PI()),IF(AccType=1,AB298*-speed/30*PI(),((AB298-AC298)*2/PI()+AC298)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD298*-speed/30*PI(),((AD298-AE298)*2/PI()+AE298)*-speed/30*PI()),IF(AccType=1,AB298*-speed/30*PI(),((AB298-AC298)*2/PI()+AC298)*-speed/30*PI()),0)/2*time7/time)))","v":484.57613841976257},{"$f":"IF(move1,MAX(IF(AccType=1,Z298*-speed/30*PI(),((Z298-AA298)*2/PI()+AA298)*-speed/30*PI()),IF(AccType=1,X298*-speed/30*PI(),((X298-Y298)*2/PI()+Y298)*-speed/30*PI()),0),MAX(IF(AccType=1,Z298*-speed/30*PI(),((Z298-AA298)*2/PI()+AA298)*-speed/30*PI()),IF(AccType=1,X298*-speed/30*PI(),((X298-Y298)*2/PI()+Y298)*-speed/30*PI()),IF(AccType=1,AD298*-speed/30*PI(),((AD298-AE298)*2/PI()+AE298)*-speed/30*PI()),IF(AccType=1,AB298*-speed/30*PI(),((AB298-AC298)*2/PI()+AC298)*-speed/30*PI()),0))","v":4661.6224515981157},{"$f":"(L298^2)/1000000+((K298/1000)^2*(D298/C298*H298)^2*PI()*PI()*(O298/2)^2)/1200","v":0.15678737304472865},{"$f":"SQRT(3)*L298*J298*D298/C298*H298/1000","v":7.8363524841025223},{"$f":"0.75*J298^2*(D298/C298*H298)^2-(UAC_V*0.98)^2","v":-49664.24850596203},{"$f":"-AO298/2/AN298+SQRT((AO298/2/AN298)^2-AP298/AN298)","v":538.38010636793388},{"$f":"(L298^2)/1000000+((K298/1000)^2*AV298^2*PI()*PI()*(O298/2)^2)/1200","v":2.2180720756393289E-2},{"$f":"SQRT(3)*L298*J298*AV298/1000","v":1.9333883613958787},{"$f":"0.75*J298^2*AV298^2-(UAC_V*0.98)^2","v":-50735.711602333889},{"$f":"-AS298/2/AR298+SQRT((AS298/2/AR298)^2-AT298/AR298)","v":1469.4534878819925},{"$f":"D298+(F298-D298)*((0.85*UAC_V-D298*J298)/L298*1000)/G298","v":16.505623275862071},{"$f":"(L298^2)/1000000+((K298/1000)^2*AJ298^2*PI()*PI()*(O298/2)^2)/1200","v":1.8024885929664152E-2},{"$f":"SQRT(3)*L298*J298*AJ298/1000","v":1.3990991399510915},{"$f":"0.75*J298^2*AJ298^2-(UAC_V*0.98)^2","v":-50768.791866761821},{"$f":"IF(((AX298/2/AW298)^2-AY298/AW298)>0,-AX298/2/AW298+SQRT((AX298/2/AW298)^2-AY298/AW298),-9999)","v":1639.9097157856454}]
["Goldline BH","BH-824-D",66,32,48.1,23,2500,245.44,6000,0.23300000000000001,11,126,8.4,670,6,572.43442085511879,1481.305332203234,1788.8888888888889,55.393853821424841,0.29761904761904762,0.29748246927740363,0.2164496505900069,1.4597727732033874,53.12540224081129,0,-43.031575815057138,0,0,0,0,0,0.75442558748556365,1.0732404493093191,9.0531070498267638,25.757770783423656,16.397906172839505,882.88265734478648,715.70188465791489,6885.0521304091417,0.14271393101646412,6.051157801239528,-50228.558357024725,572.43442085511879,2.222640038349738E-2,1.3539868854607724,-50776.291259668687,1481.305332203234,26.627314285714284,1.8284369803304959E-2,0.83382611061727463,-50794.211619067355,1644.0914942764264]
["Goldline BH","BH-824-A",66,37,43.9,22.5,3000,246.6,6000,0.155,7.3,108,8.4,670,6,738.67653291883289,1820.5783005974899,2087.037037037037,52.588406518931819,0.29761904761904762,0.29792542724195092,0.21543147705114069,1.2309864895615636,53.12540224081129,0,-43.031575815057138,0,0,0,0,0,0.87230458553018286,1.2409342695139001,10.467655026362195,29.782422468333603,18.960079012345677,882.88265734478648,715.70188465791489,6885.0521304091417,8.7053081232037838E-2,4.0083620508901507,-50460.789150998455,738.67653291883289,1.4869700014120453E-2,0.82655956525286201,-50790.516637626228,1820.5783005974899,28.507430555555558,1.3082035210437177E-2,0.54973858956047694,-50798.682536933047,1949.6558413527348]
["Goldline BH","BH-826-C",93,39.700000000000003,55.1,20.3,2500,339.3,6000,0.16700000000000001,9,141,12.6,670,6,568.09139835298834,1400.7663529581991,1598.5815602836878,71.764382089153699,0.19841269841269843,0.30023740167900337,0.21690462929243165,1.6088303803836164,73.595740718922059,0,-59.612549982326861,0,0,0,0,0,0.92017064520377312,1.3090281839342321,11.042047742445277,31.416676414421573,20.000477387495025,1223.0759748537869,991.47692278298302,9538.0079971722971,0.14566600268378169,5.9072809859540962,-50366.349469254383,568.09139835298834,2.5030235174600988E-2,1.1952109435690885,-50787.19650219271,1400.7663529581991,29.305446978723403,2.2279428363336188E-2,0.8157114773746913,-50796.792900579443,1491.7669564567359]
["Goldline BH","BH-826-D",93,52,47.5,24,3000,360,6000,8.7999999999999995E-2,4.7,103,12.6,670,6,790.83465921632626,1988.1169032540815,2188.3495145631068,62.846893633979761,0.19841269841269843,0.30024789290359555,0.20443261310811683,1.1630637229947174,73.595740718922059,0,-59.612549982326861,0,0,0,0,0,1.2052612985036826,1.7145961099390441,14.46313558204419,41.15030663853706,26.197098845081641,1223.0759748537866,991.47692278298302,9538.0079971722971,7.6861537463285862E-2,3.160118876244479,-50569.832652653487,790.83465921632626,1.2577800635122337E-2,0.54475726686353487,-50798.16686964369,1988.1169032540815,34.699443365695792,1.1731181544942518E-2,0.41127633709274569,-50801.174039366284,2063.5154829009321]
["Goldline BH","BH-828-B",124,50,75.7,35,2500,437.5,6000,0.112,4.7,150,12.6,670,6,795.40042054557432,1388.8907135514125,1502.6666666666665,97.16663141418671,0.19841269841269843,0.22439006995806487,0.16821883592896469,1.630832485575632,73.595740718922059,0,-59.612549982326861,0,0,0,0,0,0.8691788210363095,1.2364875792829648,10.430145852435714,29.675701902791154,18.892138590203107,1223.0759748537866,991.47692278298302,9538.0079971722971,7.3387308109770732E-2,5.1332957401738906,-50512.374164932364,795.40042054557432,2.5440156015768454E-2,1.2338908250617313,-50788.243482575876,1388.8907135514125,42.403999999999996,2.3083604954724633E-2,0.54973201755132262,-50801.802163431988,1471.6410307174353]
["Cart. DDR","C041A (240 V)",4.57,2.73,4.2344309430620841,2.5204946089655262,1750,12.3,1750,8.4700000000000006,34.4,102,0.58600000000000008,325,10,1211.9218110636559,1750,1750,4.2344309430620841,4.2662116040955622,1.1791047914504555,1.2228312919754132,1.6929105766250048,15.040824891297582,0,-12.183068161951041,0,0,0,0,0,0.2631638538520425,0.37437501780855581,3.1579662462245102,8.985000427405339,5.7200289268174087,249.96108996018449,202.62899229856203,1949.2909059121666,2.3540464906972931E-2,10.9950135234466,-47900.259904345119,1211.9218110636559,1.1958604858094189E-2,3.782391885328936,-50461.386250139323,1902.1173048008586,2.5276812894128269,1.8365077345397159E-2,8.5593825009745537,-49044.706597510827,1417.6767710818208]
["Cart. DDR","C041B (240 V)",4.51,4.6900000000000004,4.0107045659157627,4.1347469751708896,2500,12.2,2500,2.87,11.4,58.7,0.58600000000000008,325,10,2308.0112950990879,2500,2500,4.0107045659157627,4.2662116040955622,1.1960708467031758,1.2328544992866872,0.96,15.040824891297582,0,-12.183068161951041,0,0,0,0,0,0.45811666616042362,0.65171349538235102,5.4973999939250833,15.641123889176423,9.9574487299006336,249.96108996018449,202.62899229856203,1949.2909059121666,7.7467992475345167E-3,3.7020029189874455,-49810.814483413225,2308.0112950990879,3.8735026492182426E-3,1.1675441997467055,-50706.25677173787,3470.5140643357668,4.0012225276730238,6.0951927130744044E-3,2.9055523476800569,-50192.638672986468,2641.1661210527545]
["Cart. DDR","C042A (240 V)",8.26,4.68,7.4933892029854734,4.2097692151603781,1700,22.2,1700,3.7,18.3,108,0.88700000000000001,325,10,1296.1320507065986,1700,1700,7.4933892029854734,2.818489289740699,0.72017971179736795,0.74359755925955784,1.411764705882353,16.507865815562184,0,-13.371371310605369,0,0,0,0,0,0.27394594191209215,0.38971353922937357,3.2873513029451056,9.3531249415049658,5.9543842711864388,274.34161104832947,222.39287003085852,2139.419409696859,2.2558272844647256E-2,8.7057238524199949,-49180.725247886781,1296.1320507065986,1.2892385216204326E-2,2.9232977592548872,-50621.996638604585,1871.4083152807027,4.2236405110791768,1.410537450527841E-2,4.1211931157593629,-50441.128949387385,1750.585655899723]
["Cart. DDR","C042B (240 V)",8.4600000000000009,9.19,7.2612851236246332,7.8078334662630464,2500,22.8,2500,0.96,5,56.1,0.88700000000000001,325,10,2500,2500,2500,7.2612851236246332,2.818489289740699,0.70383284393941781,0.72402920243693791,0.96,16.507865815562184,0,-13.371371310605369,0,0,0,0,0,0.52522357809959808,0.7471793087323505,6.3026829371951765,17.932303409576413,11.416058914630938,274.34161104832947,222.39287003085852,2139.419409696859,6.300460747672005E-3,2.3103337210129227,-50381.162085779994,2650.3862776551841,3.4249300874275978E-3,0.68564467897345693,-50767.816716122805,3751.2726937091488,7.3502885467498507,3.8171423032773038E-3,1.0649051394214044,-50715.078391530427,3508.1936918312922]
["Cart. DDR","C043A (240 V)",11.1,4.7300000000000004,10.259764251475941,4.3290144520995533,1250,30,1250,3.97,20.6,143,1.19,325,10,1019.287975018324,1250,1250,10.259764251475941,2.1008403361344539,0.58547697298506862,0.59948848400181542,1.92,17.984654520054463,0,-14.567570161244113,0,0,0,0,0,0.22446487825326153,0.3193221316811472,2.6935785390391382,7.6637311603475329,4.8788827867867868,298.88412895433595,242.28806920988129,2330.8112257990579,3.470874574802256E-2,12.570327371767856,-48873.364677081816,1019.287975018324,2.2087639374890708E-2,4.2612046313768674,-50583.170356124167,1419.9215347952349,4.3335640397342212,2.2525986710457829E-2,4.7974179535317969,-50523.786595177407,1394.9298565363524]
["Cart. DDR","C043B (240 V)",11.2,9.15,9.2284402202404596,7.5027969270247636,2500,30.2,2500,1.06,5.5,74.5,1.19,325,10,2147.2150842495507,2500,2500,9.2284402202404596,2.1008403361344539,0.58291656188662189,0.59551836159120741,0.96,17.984654520054463,0,-14.567570161244113,0,0,0,0,0,0.43034157655905519,0.61220085140810399,5.1640989187086621,14.692820433794497,9.3537400000000002,298.88412895433595,242.28806920988129,2330.8112257990579,9.3364531782374194E-3,3.3746814147138804,-50292.188753172595,2147.2150842495507,5.9007514861446429E-3,1.0267761061087566,-50757.672536729166,2847.1858898023479,7.5067679024865939,6.0944449093389003E-3,1.2794050461547317,-50731.430110710055,2782.1143130521264]
["Cart. DDR","C044A (240 V)",14.1,5,13.159840151655576,4.617487772510728,1050,38.1,1050,4.08,22.1,173,1.49,325,10,846.11965598810775,1050,1050,13.159840151655576,1.6778523489932886,0.49906195931400671,0.51041526388990122,2.2857142857142856,19.446821554205236,0,-15.751925458906239,0,0,0,0,0,0.20197966910709905,0.28733483383872988,2.4237560292851885,6.8960360121295166,4.3901528762805366,323.18365163355026,261.98628621881483,2520.3080734249988,4.8260364377784776E-2,16.517440876152222,-48526.217727478499,846.11965598810775,3.2082997687023045E-2,5.6619754530866206,-50537.376528857007,1169.9312521850482,4.631280533810231,3.1864540855527132E-2,5.3671846564534942,-50564.534927858687,1178.2992916816188]
["Cart. DDR","C044B (240 V)",14.4,9.5299999999999994,12.080970563998754,8.1080339355696331,2150,38.799999999999997,2100,1.08,6,90,1.49,325,10,1807.6105514404683,2100,2100,12.134901481115062,1.6778523489932886,0.49126870722333421,0.50120674108776386,1.1428571428571428,19.446821554205236,0,-15.751925458906239,0,0,0,0,0,0.37695297329066974,0.53625060593627283,4.5234356794880366,12.870014542470548,8.1933057283950621,323.18365163355026,261.98628621881483,2520.3080734249988,1.2980735548661795E-2,4.323037734966813,-50228.349652532503,1807.6105514404683,8.593964594523839E-3,1.3752900426767394,-50746.782756126988,2351.3088577138219,8.1689719789426682,8.5969118229702098E-3,1.3793867593026667,-50746.434449637673,2350.6802951086615]
["Cart. DDR","C051A (240 V)",11.7,4.75,10.941902337567806,4.3943382881798412,1200,30,1200,4.13,24,151,2.74,325,10,949.73146406182479,1200,1200,10.941902337567806,0.91240875912408748,0.78637703591147934,0.85130613988333692,2,25.539184196500109,0,-20.686739199165086,0,0,0,0,0,0.30368469418618044,0.43201967568865934,3.6442163302341655,10.368472216527824,6.6007744222855349,424.43166279694327,344.06219042270408,3309.8782718664133,4.0369674500952947E-2,13.155780805999616,-48907.495767998029,949.73146406182479,2.5098886414062299E-2,4.7578572670107464,-50556.955910560428,1327.6432924520898,4.4047755461964178,2.7961250373035651E-2,7.1298848769011611,-50247.780297817379,1219.0945932618001]
["Cart. DDR","C051B (240 V)",11.8,9.2899999999999991,10.161231101401743,7.8769233344199554,2450,30.5,2450,1.08,6.4,78,2.74,325,10,1990.1026388403718,2450,2450,10.161231101401743,0.91240875912408748,0.78068468335973451,0.83735030152459378,0.97959183673469385,25.539184196500109,0,-20.686739199165086,0,0,0,0,0,0.58890991017267624,0.83777902960976691,7.0669189220721149,20.106696710634406,12.800320682988071,424.43166279694327,344.06219042270408,3309.8782718664133,1.0940076816301277E-2,3.5035839775074273,-50300.759084177895,1990.1026388403718,6.6120959267218166E-3,1.1553835141222923,-50750.306652502237,2684.4548273192372,7.9185776697027679,7.4639398489205295E-3,1.867668678579514,-50661.825586253006,2483.1812769933154]
["Cart. DDR","C052A (240 V)",16.8,9.84,14.907226237277634,8.6168937787731981,1850,26.6,1850,1.1399999999999999,7,105,3.59,325,10,{"$f":"IF(AQ314<I314,IF(AQ314<0,0,AQ314),I314)","v":1821.3313921108877},{"$f":"IF(AU314<I314,IF(AU314<0,0,AU314),I314)","v":1850},{"$f":"IF(UAC_V*0.98/L314*1000<I314,IF(UAC_V*0.98/L314*1000<0,0,UAC_V*0.98/L314*1000),I314)","v":1850},{"$f":"C314+(E314-C314)/G314*Q314","v":14.907226237277634},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M314,(inertia/gear^2+gear_inertia)/M314),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M314,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M314))","v":0.69637883008356549},{"$f":"IF((C314+(E314-C314)/G314*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X314^2*time1+Y314^2*time2+Z314^2*time3+AA314^2*time4)/time)/(C314+(E314-C314)/G314*mspeed),SQRT((((X314-Y314)*2/PI()+Y314)^2*time1+Y314^2*time2+((Z314-Y314)*2/PI()+Y314)^2*time3+AA314^2*time4)/time)/(C314+(E314-C314)/G314*mspeed)),IF(AccType=1,SQRT((X314^2*time1+Y314^2*time2+Z314^2*time3+AA314^2*time4+AB314^2*time5+AC314^2*time6+AD314^2*time7+AE314^2*time8)/time)/(C314+(E314-C314)/G314*mspeed),SQRT((((X314-Y314)*2/PI()+Y314)^2*time1+Y314^2*time2+((Z314-Y314)*2/PI()+Y314)^2*time3+AA314^2*time4+((AB314-AC314)*2/PI()+AC314)^2*time5+AC314^2*time6+((AD314-AC314)*2/PI()+AC314)^2*time7+AE314^2*time8)/time)/(C314+(E314-C314)/G314*mspeed))))","v":0.63853323804378848},{"$f":"IF(move1,MAX(ABS(X314),ABS(Z314))/H314,MAX(ABS(X314),ABS(Z314),ABS(AB314),ABS(AD314))/H314)","v":1.1158643155361134},{"$f":"IF(AZ314>0,speed/(MIN(AZ314,I314)),\"NA\")","v":1.2972972972972974},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M314+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M314+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.681990793260617},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M314+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M314+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-24.042412542541101},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M314+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M314+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M314+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M314+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH314/Irms","v":0.50919833903963974},{"$f":"AI314/Ipeak","v":0.72438191816886022},{"$f":"IF(move1,IF(AccType=1,SQRT((X314^2*time1+Y314^2*time2+Z314^2*time3+AA314^2*time4)/time)/(C314/D314),SQRT((((X314-Y314)*2/PI()+Y314)^2*time1+Y314^2*time2+((Z314-AA314)*2/PI()+AA314)^2*time3+AA314^2*time4)/time)/(C314/D314)),IF(AccType=1,SQRT((X314^2*time1+Y314^2*time2+Z314^2*time3+AA314^2*time4+AB314^2*time5+AC314^2*time6+AD314^2*time7+AE314^2*time8)/time)/(C314/D314),SQRT((((X314-Y314)*2/PI()+Y314)^2*time1+Y314^2*time2+((Z314-AA314)*2/PI()+AA314)^2*time3+AA314^2*time4+((AB314-AC314)*2/PI()+AC314)^2*time5+AC314^2*time6+((AD314-AE314)*2/PI()+AE314)^2*time7+AE314^2*time8)/time)/(C314/D314)))","v":6.1103800684756768},{"$f":"IF(move1,MAX(ABS(X314),ABS(Z314))/(C314/D314),MAX(ABS(X314),ABS(Z314),ABS(AB314),ABS(AD314))/(C314/D314))","v":17.385166036052645},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X314),ABS(Z314))/(C314/D314),MAX(ABS((X314-Y314)*2/PI()+Y314),ABS((Z314-Y314)*2/PI()+Y314))/(C314/D314)),IF(AccType=1,MAX(ABS(X314),ABS(Z314),ABS(AB314),ABS(AD314))/(C314/D314),MAX(ABS((X314-Y314)*2/PI()+Y314),ABS((Z314-Y314)*2/PI()+Y314),ABS((AB314-AC314)*2/PI()+AC314),ABS((AD314-AC314)*2/PI()+AC314))/(C314/D314)))","v":11.067740444444443},{"$f":"IF((C314+(E314-C314)/G314*mspeed)<0,\"NA\",U314*(C314+(E314-C314)/G314*mspeed)*mspeed/9.55)","v":493.28031038805045},{"$f":"IF(move1,IF(speed1>speed2,AM314/2*time1/time,AM314/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z314*-speed/30*PI(),((Z314-AA314)*2/PI()+AA314)*-speed/30*PI()),IF(AccType=1,X314*-speed/30*PI(),((X314-Y314)*2/PI()+Y314)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z314*-speed/30*PI(),((Z314-AA314)*2/PI()+AA314)*-speed/30*PI()),IF(AccType=1,X314*-speed/30*PI(),((X314-Y314)*2/PI()+Y314)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD314*-speed/30*PI(),((AD314-AE314)*2/PI()+AE314)*-speed/30*PI()),IF(AccType=1,AB314*-speed/30*PI(),((AB314-AC314)*2/PI()+AC314)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD314*-speed/30*PI(),((AD314-AE314)*2/PI()+AE314)*-speed/30*PI()),IF(AccType=1,AB314*-speed/30*PI(),((AB314-AC314)*2/PI()+AC314)*-speed/30*PI()),0)/2*time7/time)))","v":399.87380528134889},{"$f":"IF(move1,MAX(IF(AccType=1,Z314*-speed/30*PI(),((Z314-AA314)*2/PI()+AA314)*-speed/30*PI()),IF(AccType=1,X314*-speed/30*PI(),((X314-Y314)*2/PI()+Y314)*-speed/30*PI()),0),MAX(IF(AccType=1,Z314*-speed/30*PI(),((Z314-AA314)*2/PI()+AA314)*-speed/30*PI()),IF(AccType=1,X314*-speed/30*PI(),((X314-Y314)*2/PI()+Y314)*-speed/30*PI()),IF(AccType=1,AD314*-speed/30*PI(),((AD314-AE314)*2/PI()+AE314)*-speed/30*PI()),IF(AccType=1,AB314*-speed/30*PI(),((AB314-AC314)*2/PI()+AC314)*-speed/30*PI()),0))","v":3846.7860068065766},{"$f":"(L314^2)/1000000+((K314/1000)^2*(D314/C314*H314)^2*PI()*PI()*(O314/2)^2)/1200","v":1.3470622913447599E-2},{"$f":"SQRT(3)*L314*J314*D314/C314*H314/1000","v":3.2301465843561949},{"$f":"0.75*J314^2*(D314/C314*H314)^2-(UAC_V*0.98)^2","v":-50568.564830920004},{"$f":"-AO314/2/AN314+SQRT((AO314/2/AN314)^2-AP314/AN314)","v":1821.3313921108877},{"$f":"(L314^2)/1000000+((K314/1000)^2*AV314^2*PI()*PI()*(O314/2)^2)/1200","v":1.1784031061105926E-2},{"$f":"SQRT(3)*L314*J314*AV314/1000","v":1.7995224040384126},{"$f":"0.75*J314^2*AV314^2-(UAC_V*0.98)^2","v":-50731.729594498051},{"$f":"-AS314/2/AR314+SQRT((AS314/2/AR314)^2-AT314/AR314)","v":1999.9297134818182},{"$f":"D314+(F314-D314)*((0.85*UAC_V-D314*J314)/L314*1000)/G314","v":8.6796553415567264},{"$f":"(L314^2)/1000000+((K314/1000)^2*AJ314^2*PI()*PI()*(O314/2)^2)/1200","v":1.2259162992246234E-2},{"$f":"SQRT(3)*L314*J314*AJ314/1000","v":2.2946356863390975},{"$f":"0.75*J314^2*AJ314^2-(UAC_V*0.98)^2","v":-50685.764241881618},{"$f":"IF(((AX314/2/AW314)^2-AY314/AW314)>0,-AX314/2/AW314+SQRT((AX314/2/AW314)^2-AY314/AW314),-9999)","v":1941.9161612654059}]
["Cart. DDR","C052B (240 V)",16.5,13.5,13.819742018555456,11.055793614844365,2500,42.4,2500,0.61,3.7,75.400000000000006,3.59,325,10,{"$f":"IF(AQ315<I315,IF(AQ315<0,0,AQ315),I315)","v":2211.1522519952623},{"$f":"IF(AU315<I315,IF(AU315<0,0,AU315),I315)","v":2500},{"$f":"IF(UAC_V*0.98/L315*1000<I315,IF(UAC_V*0.98/L315*1000<0,0,UAC_V*0.98/L315*1000),I315)","v":2500},{"$f":"C315+(E315-C315)/G315*Q315","v":13.819742018555456},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M315,(inertia/gear^2+gear_inertia)/M315),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M315,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M315))","v":0.69637883008356549},{"$f":"IF((C315+(E315-C315)/G315*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X315^2*time1+Y315^2*time2+Z315^2*time3+AA315^2*time4)/time)/(C315+(E315-C315)/G315*mspeed),SQRT((((X315-Y315)*2/PI()+Y315)^2*time1+Y315^2*time2+((Z315-Y315)*2/PI()+Y315)^2*time3+AA315^2*time4)/time)/(C315+(E315-C315)/G315*mspeed)),IF(AccType=1,SQRT((X315^2*time1+Y315^2*time2+Z315^2*time3+AA315^2*time4+AB315^2*time5+AC315^2*time6+AD315^2*time7+AE315^2*time8)/time)/(C315+(E315-C315)/G315*mspeed),SQRT((((X315-Y315)*2/PI()+Y315)^2*time1+Y315^2*time2+((Z315-Y315)*2/PI()+Y315)^2*time3+AA315^2*time4+((AB315-AC315)*2/PI()+AC315)^2*time5+AC315^2*time6+((AD315-AC315)*2/PI()+AC315)^2*time7+AE315^2*time8)/time)/(C315+(E315-C315)/G315*mspeed))))","v":0.65137569629520042},{"$f":"IF(move1,MAX(ABS(X315),ABS(Z315))/H315,MAX(ABS(X315),ABS(Z315),ABS(AB315),ABS(AD315))/H315)","v":0.70004695267124095},{"$f":"IF(AZ315>0,speed/(MIN(AZ315,I315)),\"NA\")","v":0.96},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M315+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M315+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.681990793260617},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M315+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M315+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-24.042412542541101},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M315+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M315+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M315+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M315+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH315/Irms","v":0.7112970146230001},{"$f":"AI315/Ipeak","v":1.0118860497702482},{"$f":"IF(move1,IF(AccType=1,SQRT((X315^2*time1+Y315^2*time2+Z315^2*time3+AA315^2*time4)/time)/(C315/D315),SQRT((((X315-Y315)*2/PI()+Y315)^2*time1+Y315^2*time2+((Z315-AA315)*2/PI()+AA315)^2*time3+AA315^2*time4)/time)/(C315/D315)),IF(AccType=1,SQRT((X315^2*time1+Y315^2*time2+Z315^2*time3+AA315^2*time4+AB315^2*time5+AC315^2*time6+AD315^2*time7+AE315^2*time8)/time)/(C315/D315),SQRT((((X315-Y315)*2/PI()+Y315)^2*time1+Y315^2*time2+((Z315-AA315)*2/PI()+AA315)^2*time3+AA315^2*time4+((AB315-AC315)*2/PI()+AC315)^2*time5+AC315^2*time6+((AD315-AE315)*2/PI()+AE315)^2*time7+AE315^2*time8)/time)/(C315/D315)))","v":8.5355641754760008},{"$f":"IF(move1,MAX(ABS(X315),ABS(Z315))/(C315/D315),MAX(ABS(X315),ABS(Z315),ABS(AB315),ABS(AD315))/(C315/D315))","v":24.285265194485959},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X315),ABS(Z315))/(C315/D315),MAX(ABS((X315-Y315)*2/PI()+Y315),ABS((Z315-Y315)*2/PI()+Y315))/(C315/D315)),IF(AccType=1,MAX(ABS(X315),ABS(Z315),ABS(AB315),ABS(AD315))/(C315/D315),MAX(ABS((X315-Y315)*2/PI()+Y315),ABS((Z315-Y315)*2/PI()+Y315),ABS((AB315-AC315)*2/PI()+AC315),ABS((AD315-AC315)*2/PI()+AC315))/(C315/D315)))","v":15.460479999999997},{"$f":"IF((C315+(E315-C315)/G315*mspeed)<0,\"NA\",U315*(C315+(E315-C315)/G315*mspeed)*mspeed/9.55)","v":493.28031038805045},{"$f":"IF(move1,IF(speed1>speed2,AM315/2*time1/time,AM315/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z315*-speed/30*PI(),((Z315-AA315)*2/PI()+AA315)*-speed/30*PI()),IF(AccType=1,X315*-speed/30*PI(),((X315-Y315)*2/PI()+Y315)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z315*-speed/30*PI(),((Z315-AA315)*2/PI()+AA315)*-speed/30*PI()),IF(AccType=1,X315*-speed/30*PI(),((X315-Y315)*2/PI()+Y315)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD315*-speed/30*PI(),((AD315-AE315)*2/PI()+AE315)*-speed/30*PI()),IF(AccType=1,AB315*-speed/30*PI(),((AB315-AC315)*2/PI()+AC315)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD315*-speed/30*PI(),((AD315-AE315)*2/PI()+AE315)*-speed/30*PI()),IF(AccType=1,AB315*-speed/30*PI(),((AB315-AC315)*2/PI()+AC315)*-speed/30*PI()),0)/2*time7/time)))","v":399.87380528134889},{"$f":"IF(move1,MAX(IF(AccType=1,Z315*-speed/30*PI(),((Z315-AA315)*2/PI()+AA315)*-speed/30*PI()),IF(AccType=1,X315*-speed/30*PI(),((X315-Y315)*2/PI()+Y315)*-speed/30*PI()),0),MAX(IF(AccType=1,Z315*-speed/30*PI(),((Z315-AA315)*2/PI()+AA315)*-speed/30*PI()),IF(AccType=1,X315*-speed/30*PI(),((X315-Y315)*2/PI()+Y315)*-speed/30*PI()),IF(AccType=1,AD315*-speed/30*PI(),((AD315-AE315)*2/PI()+AE315)*-speed/30*PI()),IF(AccType=1,AB315*-speed/30*PI(),((AB315-AC315)*2/PI()+AC315)*-speed/30*PI()),0))","v":3846.7860068065766},{"$f":"(L315^2)/1000000+((K315/1000)^2*(D315/C315*H315)^2*PI()*PI()*(O315/2)^2)/1200","v":9.0727693111543883E-3},{"$f":"SQRT(3)*L315*J315*D315/C315*H315/1000","v":2.7636146683829121},{"$f":"0.75*J315^2*(D315/C315*H315)^2-(UAC_V*0.98)^2","v":-50469.304631140498},{"$f":"-AO315/2/AN315+SQRT((AO315/2/AN315)^2-AP315/AN315)","v":2211.1522519952623},{"$f":"(L315^2)/1000000+((K315/1000)^2*AV315^2*PI()*PI()*(O315/2)^2)/1200","v":6.0302234812098171E-3},{"$f":"SQRT(3)*L315*J315*AV315/1000","v":0.88202385250122761},{"$f":"0.75*J315^2*AV315^2-(UAC_V*0.98)^2","v":-50770.949613819968},{"$f":"-AS315/2/AR315+SQRT((AS315/2/AR315)^2-AT315/AR315)","v":2829.4105969216548},{"$f":"D315+(F315-D315)*((0.85*UAC_V-D315*J315)/L315*1000)/G315","v":11.071807380816075},{"$f":"(L315^2)/1000000+((K315/1000)^2*AJ315^2*PI()*PI()*(O315/2)^2)/1200","v":6.3579939587671292E-3},{"$f":"SQRT(3)*L315*J315*AJ315/1000","v":1.2316428259712973},{"$f":"0.75*J315^2*AJ315^2-(UAC_V*0.98)^2","v":-50738.453695746182},{"$f":"IF(((AX315/2/AW315)^2-AY315/AW315)>0,-AX315/2/AW315+SQRT((AX315/2/AW315)^2-AY315/AW315),-9999)","v":2729.7378079470527}]
["Cart. DDR","C052C (240 V)",16.899999999999999,5.74,5.6263423125459218,1.8817198369718799,1850,43.1,950,3.36,90,181,3.59,325,10,335.34404173572756,919.68133912973894,950,11.295582378979436,0.69637883008356549,0.73735981511489501,0.68867728058609323,3.5662658187679037,29.681990793260617,0,-24.042412542541101,0,0,0,0,0,0.29527477648452488,0.42005578686714978,3.5432973178142988,10.081338884811595,6.417979666009205,493.28031038805045,399.87380528134889,3846.7860068065766,0.38966255715719988,15.419877996977307,-48990.711132126125,335.34404173572756,5.5680033321296646E-2,3.9075528821922294,-50688.642116486611,919.68133912973894,3.70959403513283,0.10136354075452966,6.760468855689056,-50456.392111743073,672.97282983498053]
["Cart. DDR","C052D (240 V)",16.5,10.9,14.207490041861877,9.4716600279079177,2050,42.3,2050,0.94,5.59,92.7,3.59,325,10,1773.4887316803552,2050,2050,14.207490041861877,0.69637883008356549,0.65222517067269048,0.70170191000616122,1.1707317073170731,29.681990793260617,0,-24.042412542541101,0,0,0,0,0,0.57430647847338534,0.81700429203671898,6.8916777416806241,19.608103008881255,12.482906074074073,493.28031038805045,399.87380528134889,3846.7860068065766,1.3610334648499825E-2,4.2174615920284708,-50287.692816877032,1773.4887316803552,9.1740857993205267E-3,1.4349569978362864,-50745.255656447087,2274.9791710463455,9.5075949525616519,9.5944731441732281E-3,1.8840130983387644,-50701.896134975315,2202.7153602587055]
["Cart. DDR","C053A (240 V)",20.9,9.2100000000000009,18.971269216553925,8.2483779202408378,1350,53.7,1350,1.41,9.1,139,4.43,325,10,1184.0940851443713,1350,1350,18.971269216553925,0.56433408577878108,0.58609640828038689,0.62897688061234214,1.7777777777777777,33.776058488882775,0,-27.358607375995042,0,0,0,0,0,0.43594374199308022,0.62017045191907971,5.2313249039169625,14.884090846057914,9.4755065263157903,561.31897388985044,455.02881290636242,4377.3771801592065,2.8855908992907277E-2,8.0330814429213415,-49970.182547117038,1184.0940851443713,2.0486857876003246E-2,2.8089674030442264,-50703.065156677127,1506.1213471261974,8.2746981289477439,2.0849784119631495E-2,3.2165993906944581,-50671.2834972282,1483.7125306517526]
["Cart. DDR","C053B (240 V)",20,18.2,16.123032354981365,14.525254373857084,2500,51.4,2500,0.36,2.2000000000000002,67.400000000000006,4.43,325,10,2500,2500,2500,16.123032354981365,0.56433408577878108,0.6151020392019857,0.65712176048410065,0.96,33.776058488882775,0,-27.358607375995042,0,0,0,0,0,0.900240394024581,1.2806755510368051,10.802884728294972,30.736213224883322,19.567281066666663,561.31897388985055,455.02881290636242,4377.3771801592065,6.7200330265574249E-3,1.9657466126983718,-50592.505152212805,2601.4664418395128,4.7400326003599605E-3,0.59170395817714716,-50785.89233154941,3211.4422609733233,14.079312542620464,4.9237949707068825E-3,0.82234396195572279,-50767.944210933165,3128.6118372720694]
["Cart. DDR","C054A (240 V)",24.8,9.7899999999999991,22.631832907667519,8.8061606644620696,1200,63.5,1200,1.35,9,156,5.28,325,10,1073.8020505359475,1200,1200,22.631832907667519,0.47348484848484845,0.55567508200547755,0.59714748166367382,2,37.91886508564329,0,-30.714280719371061,0,0,0,0,0,0.43842415840275328,0.62369907457736518,5.2610899008330394,14.968777789856764,9.52941990919952,630.16762148095779,510.84042776500723,4914.2849150993698,3.4801331736585325E-2,9.1437370939317208,-49946.268563003963,1073.8020505359475,2.5635156908008157E-2,3.2216476064023856,-50698.537986318232,1344.8722892788039,8.8319995858999558,2.5848434082524237E-2,3.4760455480419483,-50681.034294747886,1334.6245678626296]
["Cart. DDR","C054B (240 V)",24,17.399999999999999,18.692240124835369,13.447654766068611,2350,60.9,2300,0.43,2.7,84.3,5.28,325,10,2110.8273944066705,2300,2300,18.805171186009083,0.47348484848484845,0.57995303105910745,0.62264146281844479,1.0434782608695652,37.91886508564329,0,-30.714280719371061,0,0,0,0,0,0.80519574750577172,1.1454657161288078,9.6623489700692602,27.491177187091385,17.501426962962963,630.16762148095768,510.84042776500723,4914.2849150993698,1.0028600499499269E-2,2.7721195570696691,-50534.820956439537,2110.8273944066705,7.385732307293935E-3,0.85694756345341627,-50779.325898829498,2564.712488461983,13.648898078325576,7.5656171300527231E-3,1.0988290121885751,-50762.683855024516,2518.6980958072972]
["Cart. DDR","C061A (240 V)",33.4,9.89,31.300472141406086,9.2060212180606129,900,85.7,900,1.36,18.100000000000001,206,9.41,325,10,694.26248634850731,900,900,31.300472141406086,0.26567481402763016,0.63073692548989257,0.67733992130438203,2.6666666666666665,58.048031255785546,0,-47.018905317186288,0,0,0,0,0,0.50343737617821771,0.7161864135725039,6.041248514138613,17.188473925740094,10.942522357950766,964.69105036480801,782.01921525465764,7523.0248507498063,8.581474180151874E-2,12.313950481271291,-49911.853747907429,694.26248634850731,4.8160334655882382E-2,4.4732321231849266,-50687.277744203668,980.50888708789387,9.2183815336539769,5.0501857462986542E-2,5.3098737930900626,-50639.058342807148,950.16541511241599]
["Cart. DDR","C061B (240 V)",32.299999999999997,19.5,26.963295897353099,16.145686166079702,1950,83,1950,0.35,4.3,101,9.41,325,10,1524.555917260986,1950,1950,26.963295897353099,0.26567481402763016,0.6567754405691254,0.69937387055163303,1.2307692307692308,58.048031255785546,0,-47.018905317186288,0,0,0,0,0,1.0264261774406183,1.4601865447469276,12.31711412928742,35.044477073926259,22.31000701754386,964.69105036480801,782.01921525465764,7523.0248507498063,1.9746875854117676E-2,3.0680344149528032,-50574.475871695555,1524.555917260986,1.120945692803586E-2,0.99719711381249043,-50780.789789143324,2084.4050863400153,16.286620144123319,1.2093321104490634E-2,1.3659970214912072,-50759.430467044338,1993.0349886930276]
["Cart. DDR","C062A (240 V)",47.3,14.6,43.635259450226378,13.344116039824581,950,121.5,950,0.76,11.1,198,12.6,325,10,756.28181745859104,950,950,43.635259450226378,0.19841269841269843,0.56777580966779839,0.60572626106108696,2.5263157894736841,73.595740718922059,0,-59.612549982326861,0,0,0,0,0,0.66535363112225576,0.94652732073314139,7.9842435734670687,22.716655697595392,14.4618721791559,1223.0759748537866,991.47692278298302,9538.0079971722971,7.4836020663870462E-2,9.7747892578686457,-50195.869461816757,756.28181745859104,4.3731817012814901E-2,3.484428927676678,-50727.736491225194,1037.9184816078166,13.36879305798943,4.4502506885158166E-2,3.7693279827754234,-50714.558062431555,1026.0053278067126]
["Cart. DDR","C062B (240 V)",46,20.6,39.843616787833106,17.708274127925826,1450,117.8,1450,0.38,5.2,136,12.6,325,10,1151.8008495468489,1450,1450,39.843616787833106,0.19841269841269843,0.58677703278572479,0.62475161900612952,1.6551724137931034,73.595740718922059,0,-59.612549982326861,0,0,0,0,0,0.96531755671963004,1.3732538576175675,11.58381068063556,32.958092582821621,20.981773397745574,1223.0759748537866,991.47692278298302,9538.0079971722971,3.3969000998377616E-2,4.7221286133868929,-50503.763770526508,1151.8008495468489,2.0267103414957546E-2,1.5976163443822515,-50770.660946368982,1543.8202500197492,17.84799199866174,2.0943651486292469E-2,1.8781285937867116,-50757.48256954478,1512.5756941372524]
["Cart. DDR","C062C (240 V)",48.4,11.8,44.745275429264296,10.808037543300555,700,124.2,700,1.19,17.8,250.4,12.6,325,10,577.33440435114846,700,700,44.745275429264296,0.19841269841269843,0.56180315273703518,0.59255829886410671,3.4285714285714284,73.595740718922059,0,-59.612549982326861,0,0,0,0,0,0.52552993840509432,0.74761513471356789,6.3063592608611314,17.942763233125628,11.422717845117846,1223.0759748537866,991.47692278298302,9538.0079971722971,0.12243325195315058,15.627883130453613,-49831.355742008011,577.33440435114846,7.0261135467313579E-2,5.5600867989730833,-50681.896497912792,810.66897031256894,10.773074375469147,7.1200521806924266E-2,5.8953740116797624,-50666.58206520052,803.18177391227323]
["Cart. DDR","C063A (240 V)",60.2,13.9,56.231715036410804,12.897182347800642,700,154.4,700,0.93,14.4,264,15.7,325,10,576.92451007275145,700,700,56.231715036410804,0.15923566878980894,0.54089332810730628,0.57451295383298795,3.4285714285714284,88.704800071813338,0,-71.850888058168806,0,0,0,0,0,0.59989268465105139,0.85340304609510342,7.1987122158126162,20.481673106282482,13.039038070628768,1474.1710425390011,1195.025165208629,11496.14208930701,0.12388544489239156,15.160485444035794,-49980.721298715776,576.92451007275145,7.6801369545473591E-2,5.4897060665100668,-50697.058843919753,777.51524594978116,12.909267168750036,7.6944941566259584E-2,5.5448915466761841,-50694.874537906049,776.46113649388406]
["Cart. DDR","C063B (240 V)",59,19.8,52.313537816292559,17.437845938764188,1150,149,1150,0.47,7.1,181,15.7,325,10,866.0456742528454,1150,1150,52.313537816292559,0.15923566878980894,0.55303658149417378,0.59533422866988817,2.1020885324897529,88.704800071813338,0,-71.850888058168806,0,0,0,0,0,0.87190352932162796,1.240363729817729,10.462842351859535,29.768729515625495,18.951361807909603,1474.1710425390011,1195.025165208629,11496.14208930701,5.8677365697970815E-2,7.3677775864762527,-50390.916337079288,866.0456742528454,3.6003530259308067E-2,2.6061024003876363,-50753.331837540783,1151.6571764249886,17.687009784877535,3.6483682960340262E-2,2.7923990600398576,-50745.657142101045,1141.7216558226476]
["Cart. DDR","C063C (240 V)",61.8,11.3,58.163897384492664,10.536937931973309,550,158.9,550,1.45,23.1,333.8,15.7,325,10,436.32799364763662,550,550,58.163897384492664,0.15923566878980894,0.53009123995514884,0.55824292052745961,4.3636363636363633,88.704800071813338,0,-71.850888058168806,0,0,0,0,0,0.47505645696342835,0.6758119207197214,5.7006774835611402,16.219486097273315,10.325645547165289,1474.1710425390008,1195.025165208629,11496.14208930701,0.20404359640555086,24.357282183837658,-49474.016122287634,436.32799364763662,0.12364727982048261,8.8490228536589477,-50629.465576451708,605.11239013661839,10.555537543904348,0.12312058212085314,8.6562975164076938,-50637.035233811599,607.12019313083806]
["Cart. DDR","C091A (230 V)",50,12.8,42.016904976260371,10.426031011478999,600,120,600,0.91600000000000004,7.8,244,28,325,38,442.08949414561317,600,600,42.016904976260371,8.9285714285714288E-2,1.1876594062119945,1.2387804039332906,4.5771713639187945,148.65364847199487,0,-120.40945526231586,0,0,0,0,0,1.1146118954924324,1.5856389170346119,13.37534274590919,38.055334008830684,24.226778074074073,2470.4514723867878,2002.6520625749001,19265.51284197054,0.23000967725837071,11.89233511510654,-50211.285560627206,442.08949414561317,7.6955476030398928E-2,3.8015089544183716,-50744.476252643268,787.71090999570106,9.8199684039669073,0.16556049893675479,9.3786772010483173,-50435.80538245153,524.34130365292117]
["Cart. DDR","C092A (230 V)",101,15.3,89.524655489191119,13.165390513116341,400,227,400,0.92100000000000004,11,441,47,325,38,265.43095493177839,400,400,89.524655489191119,5.3191489361702128E-2,0.96308168729994115,1.0628086371580483,7.0638611088354573,241.25756063487694,0,-195.41862411425032,0,0,0,0,0,1.070432101945699,1.5227890584627133,12.845185223348389,36.546937403105119,23.266502970297029,4009.4212420703602,3250.2058064740177,31266.979858280047,0.61929899024442847,24.191052348087272,-50052.892408682732,265.43095493177839,0.25617892654397639,9.2191014858058882,-50695.905327042761,427.22144666220765,13.104780430707303,0.38896026130647987,16.367786796363401,-50460.776172516591,339.75752963178832]
["Cart. DDR","C092C (230 V)",101.6,18.100000000000001,87.004702223569467,15.344744660241529,450,231.2,450,0.64,7.35,343,47,325,38,339.65491121542971,450,450,87.004702223569467,5.3191489361702128E-2,0.97516948403070347,1.0435015598394333,5.4561194730559155,241.25756063487694,0,-195.41862411425032,0,0,0,0,0,1.2588498569083764,1.7908308101588226,15.106198282900516,42.979939443811745,27.361879265091865,4009.4212420703602,3250.2058064740177,31266.979858280047,0.38975979599526256,15.660564698073852,-50284.00536489355,339.65491121542971,0.15286331424762997,5.6337056138730039,-50737.716505062126,557.98851367732425,14.816970903355887,0.23773495712059384,10.40352807785769,-50575.167827378958,439.8730658028984]
["Cart. DDR","C093A (230 V)",145,15.5,132.09860276627313,15.450128978511476,300,309,300,0.86699999999999999,11,517,66,325,38,{"$f":"IF(AQ333<I333,IF(AQ333<0,0,AQ333),I333)","v":257.15331937344519},{"$f":"IF(AU333<I333,IF(AU333<0,0,AU333),I333)","v":300},{"$f":"IF(UAC_V*0.98/L333*1000<I333,IF(UAC_V*0.98/L333*1000<0,0,UAC_V*0.98/L333*1000),I333)","v":300},{"$f":"C333+(E333-C333)/G333*Q333","v":132.09860276627313},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M333,(inertia/gear^2+gear_inertia)/M333),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M333,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M333))","v":3.787878787878788E-2},{"$f":"IF((C333+(E333-C333)/G333*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X333^2*time1+Y333^2*time2+Z333^2*time3+AA333^2*time4)/time)/(C333+(E333-C333)/G333*mspeed),SQRT((((X333-Y333)*2/PI()+Y333)^2*time1+Y333^2*time2+((Z333-Y333)*2/PI()+Y333)^2*time3+AA333^2*time4)/time)/(C333+(E333-C333)/G333*mspeed)),IF(AccType=1,SQRT((X333^2*time1+Y333^2*time2+Z333^2*time3+AA333^2*time4+AB333^2*time5+AC333^2*time6+AD333^2*time7+AE333^2*time8)/time)/(C333+(E333-C333)/G333*mspeed),SQRT((((X333-Y333)*2/PI()+Y333)^2*time1+Y333^2*time2+((Z333-Y333)*2/PI()+Y333)^2*time3+AA333^2*time4+((AB333-AC333)*2/PI()+AC333)^2*time5+AC333^2*time6+((AD333-AC333)*2/PI()+AC333)^2*time7+AE333^2*time8)/time)/(C333+(E333-C333)/G333*mspeed))))","v":0.93439879885631616},{"$f":"IF(move1,MAX(ABS(X333),ABS(Z333))/H333,MAX(ABS(X333),ABS(Z333),ABS(AB333),ABS(AD333))/H333)","v":1.0804578407694467},{"$f":"IF(AZ333>0,speed/(MIN(AZ333,I333)),\"NA\")","v":8},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M333+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M333+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":333.86147279775901},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M333+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M333+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-270.42779296618477},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M333+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M333+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M333+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M333+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},{"$f":"AH333/Irms","v":1.0452932271402366},{"$f":"AI333/Ipeak","v":1.4870266748176046},{"$f":"IF(move1,IF(AccType=1,SQRT((X333^2*time1+Y333^2*time2+Z333^2*time3+AA333^2*time4)/time)/(C333/D333),SQRT((((X333-Y333)*2/PI()+Y333)^2*time1+Y333^2*time2+((Z333-AA333)*2/PI()+AA333)^2*time3+AA333^2*time4)/time)/(C333/D333)),IF(AccType=1,SQRT((X333^2*time1+Y333^2*time2+Z333^2*time3+AA333^2*time4+AB333^2*time5+AC333^2*time6+AD333^2*time7+AE333^2*time8)/time)/(C333/D333),SQRT((((X333-Y333)*2/PI()+Y333)^2*time1+Y333^2*time2+((Z333-AA333)*2/PI()+AA333)^2*time3+AA333^2*time4+((AB333-AC333)*2/PI()+AC333)^2*time5+AC333^2*time6+((AD333-AE333)*2/PI()+AE333)^2*time7+AE333^2*time8)/time)/(C333/D333)))","v":12.543518725682839},{"$f":"IF(move1,MAX(ABS(X333),ABS(Z333))/(C333/D333),MAX(ABS(X333),ABS(Z333),ABS(AB333),ABS(AD333))/(C333/D333))","v":35.688640195622511},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X333),ABS(Z333))/(C333/D333),MAX(ABS((X333-Y333)*2/PI()+Y333),ABS((Z333-Y333)*2/PI()+Y333))/(C333/D333)),IF(AccType=1,MAX(ABS(X333),ABS(Z333),ABS(AB333),ABS(AD333))/(C333/D333),MAX(ABS((X333-Y333)*2/PI()+Y333),ABS((Z333-Y333)*2/PI()+Y333),ABS((AB333-AC333)*2/PI()+AC333),ABS((AD333-AC333)*2/PI()+AC333))/(C333/D333)))","v":22.720093997445719},{"$f":"IF((C333+(E333-C333)/G333*mspeed)<0,\"NA\",U333*(C333+(E333-C333)/G333*mspeed)*mspeed/9.55)","v":5548.3910117539326},{"$f":"IF(move1,IF(speed1>speed2,AM333/2*time1/time,AM333/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z333*-speed/30*PI(),((Z333-AA333)*2/PI()+AA333)*-speed/30*PI()),IF(AccType=1,X333*-speed/30*PI(),((X333-Y333)*2/PI()+Y333)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z333*-speed/30*PI(),((Z333-AA333)*2/PI()+AA333)*-speed/30*PI()),IF(AccType=1,X333*-speed/30*PI(),((X333-Y333)*2/PI()+Y333)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD333*-speed/30*PI(),((AD333-AE333)*2/PI()+AE333)*-speed/30*PI()),IF(AccType=1,AB333*-speed/30*PI(),((AB333-AC333)*2/PI()+AC333)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD333*-speed/30*PI(),((AD333-AE333)*2/PI()+AE333)*-speed/30*PI()),IF(AccType=1,AB333*-speed/30*PI(),((AB333-AC333)*2/PI()+AC333)*-speed/30*PI()),0)/2*time7/time)))","v":4497.7595503731354},{"$f":"IF(move1,MAX(IF(AccType=1,Z333*-speed/30*PI(),((Z333-AA333)*2/PI()+AA333)*-speed/30*PI()),IF(AccType=1,X333*-speed/30*PI(),((X333-Y333)*2/PI()+Y333)*-speed/30*PI()),0),MAX(IF(AccType=1,Z333*-speed/30*PI(),((Z333-AA333)*2/PI()+AA333)*-speed/30*PI()),IF(AccType=1,X333*-speed/30*PI(),((X333-Y333)*2/PI()+Y333)*-speed/30*PI()),IF(AccType=1,AD333*-speed/30*PI(),((AD333-AE333)*2/PI()+AE333)*-speed/30*PI()),IF(AccType=1,AB333*-speed/30*PI(),((AB333-AC333)*2/PI()+AC333)*-speed/30*PI()),0))","v":43268.446874589565},{"$f":"(L333^2)/1000000+((K333/1000)^2*(D333/C333*H333)^2*PI()*PI()*(O333/2)^2)/1200","v":0.6592613406265776},{"$f":"SQRT(3)*L333*J333*D333/C333*H333/1000","v":25.644394149670696},{"$f":"0.75*J333^2*(D333/C333*H333)^2-(UAC_V*0.98)^2","v":-50190.062716438333},{"$f":"-AO333/2/AN333+SQRT((AO333/2/AN333)^2-AP333/AN333)","v":257.15331937344519},{"$f":"(L333^2)/1000000+((K333/1000)^2*AV333^2*PI()*PI()*(O333/2)^2)/1200","v":0.35295091499831255},{"$f":"SQRT(3)*L333*J333*AV333/1000","v":11.988328135719922},{"$f":"0.75*J333^2*AV333^2-(UAC_V*0.98)^2","v":-50670.736200769868},{"$f":"-AS333/2/AR333+SQRT((AS333/2/AR333)^2-AT333/AR333)","v":362.294668258277},{"$f":"D333+(F333-D333)*((0.85*UAC_V-D333*J333)/L333*1000)/G333","v":15.441459748686441},{"$f":"(L333^2)/1000000+((K333/1000)^2*AJ333^2*PI()*PI()*(O333/2)^2)/1200","v":0.45274091367703173},{"$f":"SQRT(3)*L333*J333*AJ333/1000","v":17.639261219390221},{"$f":"0.75*J333^2*AJ333^2-(UAC_V*0.98)^2","v":-50514.142097686512},{"$f":"IF(((AX333/2/AW333)^2-AY333/AW333)>0,-AX333/2/AW333+SQRT((AX333/2/AW333)^2-AY333/AW333),-9999)","v":315.11408265509073}]
["Cart. DDR","C093C (230 V)",139.4,20,128.50624833648465,18.227836643473001,350,316.60000000000002,350,0.59,7.54,426,66,325,38,{"$f":"IF(AQ334<I334,IF(AQ334<0,0,AQ334),I334)","v":289.93803130745482},{"$f":"IF(AU334<I334,IF(AU334<0,0,AU334),I334)","v":350},{"$f":"IF(UAC_V*0.98/L334*1000<I334,IF(UAC_V*0.98/L334*1000<0,0,UAC_V*0.98/L334*1000),I334)","v":350},{"$f":"C334+(E334-C334)/G334*Q334","v":128.50624833648465},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M334,(inertia/gear^2+gear_inertia)/M334),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M334,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M334))","v":3.787878787878788E-2},{"$f":"IF((C334+(E334-C334)/G334*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X334^2*time1+Y334^2*time2+Z334^2*time3+AA334^2*time4)/time)/(C334+(E334-C334)/G334*mspeed),SQRT((((X334-Y334)*2/PI()+Y334)^2*time1+Y334^2*time2+((Z334-Y334)*2/PI()+Y334)^2*time3+AA334^2*time4)/time)/(C334+(E334-C334)/G334*mspeed)),IF(AccType=1,SQRT((X334^2*time1+Y334^2*time2+Z334^2*time3+AA334^2*time4+AB334^2*time5+AC334^2*time6+AD334^2*time7+AE334^2*time8)/time)/(C334+(E334-C334)/G334*mspeed),SQRT((((X334-Y334)*2/PI()+Y334)^2*time1+Y334^2*time2+((Z334-Y334)*2/PI()+Y334)^2*time3+AA334^2*time4+((AB334-AC334)*2/PI()+AC334)^2*time5+AC334^2*time6+((AD334-AC334)*2/PI()+AC334)^2*time7+AE334^2*time8)/time)/(C334+(E334-C334)/G334*mspeed))))","v":0.93615534868991335},{"$f":"IF(move1,MAX(ABS(X334),ABS(Z334))/H334,MAX(ABS(X334),ABS(Z334),ABS(AB334),ABS(AD334))/H334)","v":1.0545213922860359},{"$f":"IF(AZ334>0,speed/(MIN(AZ334,I334)),\"NA\")","v":6.8571428571428568},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M334+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M334+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":333.86147279775901},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M334+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M334+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-270.42779296618477},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M334+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M334+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M334+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M334+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH334/Irms","v":1.4029482846793568},{"$f":"AI334/Ipeak","v":1.9958242037168759},{"$f":"IF(move1,IF(AccType=1,SQRT((X334^2*time1+Y334^2*time2+Z334^2*time3+AA334^2*time4)/time)/(C334/D334),SQRT((((X334-Y334)*2/PI()+Y334)^2*time1+Y334^2*time2+((Z334-AA334)*2/PI()+AA334)^2*time3+AA334^2*time4)/time)/(C334/D334)),IF(AccType=1,SQRT((X334^2*time1+Y334^2*time2+Z334^2*time3+AA334^2*time4+AB334^2*time5+AC334^2*time6+AD334^2*time7+AE334^2*time8)/time)/(C334/D334),SQRT((((X334-Y334)*2/PI()+Y334)^2*time1+Y334^2*time2+((Z334-AA334)*2/PI()+AA334)^2*time3+AA334^2*time4+((AB334-AC334)*2/PI()+AC334)^2*time5+AC334^2*time6+((AD334-AE334)*2/PI()+AE334)^2*time7+AE334^2*time8)/time)/(C334/D334)))","v":16.835379416152282},{"$f":"IF(move1,MAX(ABS(X334),ABS(Z334))/(C334/D334),MAX(ABS(X334),ABS(Z334),ABS(AB334),ABS(AD334))/(C334/D334))","v":47.899780889205019},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X334),ABS(Z334))/(C334/D334),MAX(ABS((X334-Y334)*2/PI()+Y334),ABS((Z334-Y334)*2/PI()+Y334))/(C334/D334)),IF(AccType=1,MAX(ABS(X334),ABS(Z334),ABS(AB334),ABS(AD334))/(C334/D334),MAX(ABS((X334-Y334)*2/PI()+Y334),ABS((Z334-Y334)*2/PI()+Y334),ABS((AB334-AC334)*2/PI()+AC334),ABS((AD334-AC334)*2/PI()+AC334))/(C334/D334)))","v":30.493947606142722},{"$f":"IF((C334+(E334-C334)/G334*mspeed)<0,\"NA\",U334*(C334+(E334-C334)/G334*mspeed)*mspeed/9.55)","v":5548.3910117539326},{"$f":"IF(move1,IF(speed1>speed2,AM334/2*time1/time,AM334/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z334*-speed/30*PI(),((Z334-AA334)*2/PI()+AA334)*-speed/30*PI()),IF(AccType=1,X334*-speed/30*PI(),((X334-Y334)*2/PI()+Y334)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z334*-speed/30*PI(),((Z334-AA334)*2/PI()+AA334)*-speed/30*PI()),IF(AccType=1,X334*-speed/30*PI(),((X334-Y334)*2/PI()+Y334)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD334*-speed/30*PI(),((AD334-AE334)*2/PI()+AE334)*-speed/30*PI()),IF(AccType=1,AB334*-speed/30*PI(),((AB334-AC334)*2/PI()+AC334)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD334*-speed/30*PI(),((AD334-AE334)*2/PI()+AE334)*-speed/30*PI()),IF(AccType=1,AB334*-speed/30*PI(),((AB334-AC334)*2/PI()+AC334)*-speed/30*PI()),0)/2*time7/time)))","v":4497.7595503731354},{"$f":"IF(move1,MAX(IF(AccType=1,Z334*-speed/30*PI(),((Z334-AA334)*2/PI()+AA334)*-speed/30*PI()),IF(AccType=1,X334*-speed/30*PI(),((X334-Y334)*2/PI()+Y334)*-speed/30*PI()),0),MAX(IF(AccType=1,Z334*-speed/30*PI(),((Z334-AA334)*2/PI()+AA334)*-speed/30*PI()),IF(AccType=1,X334*-speed/30*PI(),((X334-Y334)*2/PI()+Y334)*-speed/30*PI()),IF(AccType=1,AD334*-speed/30*PI(),((AD334-AE334)*2/PI()+AE334)*-speed/30*PI()),IF(AccType=1,AB334*-speed/30*PI(),((AB334-AC334)*2/PI()+AC334)*-speed/30*PI()),0))","v":43268.446874589565},{"$f":"(L334^2)/1000000+((K334/1000)^2*(D334/C334*H334)^2*PI()*PI()*(O334/2)^2)/1200","v":0.5297528901178814},{"$f":"SQRT(3)*L334*J334*D334/C334*H334/1000","v":19.774265937142449},{"$f":"0.75*J334^2*(D334/C334*H334)^2-(UAC_V*0.98)^2","v":-50266.491535088899},{"$f":"-AO334/2/AN334+SQRT((AO334/2/AN334)^2-AP334/AN334)","v":289.93803130745482},{"$f":"(L334^2)/1000000+((K334/1000)^2*AV334^2*PI()*PI()*(O334/2)^2)/1200","v":0.23505783372539343},{"$f":"SQRT(3)*L334*J334*AV334/1000","v":7.7561612202164394},{"$f":"0.75*J334^2*AV334^2-(UAC_V*0.98)^2","v":-50722.28673180753},{"$f":"-AS334/2/AR334+SQRT((AS334/2/AR334)^2-AT334/AR334)","v":448.32264151597803},{"$f":"D334+(F334-D334)*((0.85*UAC_V-D334*J334)/L334*1000)/G334","v":17.816590150274919},{"$f":"(L334^2)/1000000+((K334/1000)^2*AJ334^2*PI()*PI()*(O334/2)^2)/1200","v":0.33843842239082211},{"$f":"SQRT(3)*L334*J334*AJ334/1000","v":13.275041513509056},{"$f":"0.75*J334^2*AJ334^2-(UAC_V*0.98)^2","v":-50562.391359538749},{"$f":"IF(((AX334/2/AW334)^2-AY334/AW334)>0,-AX334/2/AW334+SQRT((AX334/2/AW334)^2-AY334/AW334),-9999)","v":367.40682833297762}]
["Cart. DDR","C131A (230 V)",188,13.8,168.91644626819826,13.845610349852317,225,389,225,0.93,13,738,123,325,46,{"$f":"IF(AQ335<I335,IF(AQ335<0,0,AQ335),I335)","v":195.31276231739977},{"$f":"IF(AU335<I335,IF(AU335<0,0,AU335),I335)","v":225},{"$f":"IF(UAC_V*0.98/L335*1000<I335,IF(UAC_V*0.98/L335*1000<0,0,UAC_V*0.98/L335*1000),I335)","v":225},{"$f":"C335+(E335-C335)/G335*Q335","v":168.91644626819826},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M335,(inertia/gear^2+gear_inertia)/M335),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M335,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M335))","v":2.032520325203252E-2},{"$f":"IF((C335+(E335-C335)/G335*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X335^2*time1+Y335^2*time2+Z335^2*time3+AA335^2*time4)/time)/(C335+(E335-C335)/G335*mspeed),SQRT((((X335-Y335)*2/PI()+Y335)^2*time1+Y335^2*time2+((Z335-Y335)*2/PI()+Y335)^2*time3+AA335^2*time4)/time)/(C335+(E335-C335)/G335*mspeed)),IF(AccType=1,SQRT((X335^2*time1+Y335^2*time2+Z335^2*time3+AA335^2*time4+AB335^2*time5+AC335^2*time6+AD335^2*time7+AE335^2*time8)/time)/(C335+(E335-C335)/G335*mspeed),SQRT((((X335-Y335)*2/PI()+Y335)^2*time1+Y335^2*time2+((Z335-Y335)*2/PI()+Y335)^2*time3+AA335^2*time4+((AB335-AC335)*2/PI()+AC335)^2*time5+AC335^2*time6+((AD335-AC335)*2/PI()+AC335)^2*time7+AE335^2*time8)/time)/(C335+(E335-C335)/G335*mspeed))))","v":1.436101626387396},{"$f":"IF(move1,MAX(ABS(X335),ABS(Z335))/H335,MAX(ABS(X335),ABS(Z335),ABS(AB335),ABS(AD335))/H335)","v":1.5724247025357463},{"$f":"IF(AZ335>0,speed/(MIN(AZ335,I335)),\"NA\")","v":12.295231365395864},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M335+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M335+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":611.67320928640527},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M335+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M335+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-495.4552995219882},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M335+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M335+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M335+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M335+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH335/Irms","v":1.3150698831826499},{"$f":"AI335/Ipeak","v":1.8708090177642713},{"$f":"IF(move1,IF(AccType=1,SQRT((X335^2*time1+Y335^2*time2+Z335^2*time3+AA335^2*time4)/time)/(C335/D335),SQRT((((X335-Y335)*2/PI()+Y335)^2*time1+Y335^2*time2+((Z335-AA335)*2/PI()+AA335)^2*time3+AA335^2*time4)/time)/(C335/D335)),IF(AccType=1,SQRT((X335^2*time1+Y335^2*time2+Z335^2*time3+AA335^2*time4+AB335^2*time5+AC335^2*time6+AD335^2*time7+AE335^2*time8)/time)/(C335/D335),SQRT((((X335-Y335)*2/PI()+Y335)^2*time1+Y335^2*time2+((Z335-AA335)*2/PI()+AA335)^2*time3+AA335^2*time4+((AB335-AC335)*2/PI()+AC335)^2*time5+AC335^2*time6+((AD335-AE335)*2/PI()+AE335)^2*time7+AE335^2*time8)/time)/(C335/D335)))","v":15.780838598191799},{"$f":"IF(move1,MAX(ABS(X335),ABS(Z335))/(C335/D335),MAX(ABS(X335),ABS(Z335),ABS(AB335),ABS(AD335))/(C335/D335))","v":44.899416426342512},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X335),ABS(Z335))/(C335/D335),MAX(ABS((X335-Y335)*2/PI()+Y335),ABS((Z335-Y335)*2/PI()+Y335))/(C335/D335)),IF(AccType=1,MAX(ABS(X335),ABS(Z335),ABS(AB335),ABS(AD335))/(C335/D335),MAX(ABS((X335-Y335)*2/PI()+Y335),ABS((Z335-Y335)*2/PI()+Y335),ABS((AB335-AC335)*2/PI()+AC335),ABS((AD335-AC335)*2/PI()+AC335))/(C335/D335)))","v":28.583856264775417},{"$f":"IF((C335+(E335-C335)/G335*mspeed)<0,\"NA\",U335*(C335+(E335-C335)/G335*mspeed)*mspeed/9.55)","v":10165.300320804654},{"$f":"IF(move1,IF(speed1>speed2,AM335/2*time1/time,AM335/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z335*-speed/30*PI(),((Z335-AA335)*2/PI()+AA335)*-speed/30*PI()),IF(AccType=1,X335*-speed/30*PI(),((X335-Y335)*2/PI()+Y335)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z335*-speed/30*PI(),((Z335-AA335)*2/PI()+AA335)*-speed/30*PI()),IF(AccType=1,X335*-speed/30*PI(),((X335-Y335)*2/PI()+Y335)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD335*-speed/30*PI(),((AD335-AE335)*2/PI()+AE335)*-speed/30*PI()),IF(AccType=1,AB335*-speed/30*PI(),((AB335-AC335)*2/PI()+AC335)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD335*-speed/30*PI(),((AD335-AE335)*2/PI()+AE335)*-speed/30*PI()),IF(AccType=1,AB335*-speed/30*PI(),((AB335-AC335)*2/PI()+AC335)*-speed/30*PI()),0)/2*time7/time)))","v":8240.4207820704905},{"$f":"IF(move1,MAX(IF(AccType=1,Z335*-speed/30*PI(),((Z335-AA335)*2/PI()+AA335)*-speed/30*PI()),IF(AccType=1,X335*-speed/30*PI(),((X335-Y335)*2/PI()+Y335)*-speed/30*PI()),0),MAX(IF(AccType=1,Z335*-speed/30*PI(),((Z335-AA335)*2/PI()+AA335)*-speed/30*PI()),IF(AccType=1,X335*-speed/30*PI(),((X335-Y335)*2/PI()+Y335)*-speed/30*PI()),IF(AccType=1,AD335*-speed/30*PI(),((AD335-AE335)*2/PI()+AE335)*-speed/30*PI()),IF(AccType=1,AB335*-speed/30*PI(),((AB335-AC335)*2/PI()+AC335)*-speed/30*PI()),0))","v":79272.847923518115},{"$f":"(L335^2)/1000000+((K335/1000)^2*(D335/C335*H335)^2*PI()*PI()*(O335/2)^2)/1200","v":1.1441624499909331},{"$f":"SQRT(3)*L335*J335*D335/C335*H335/1000","v":33.944606318885967},{"$f":"0.75*J335^2*(D335/C335*H335)^2-(UAC_V*0.98)^2","v":-50276.26575984306},{"$f":"-AO335/2/AN335+SQRT((AO335/2/AN335)^2-AP335/AN335)","v":195.31276231739977},{"$f":"(L335^2)/1000000+((K335/1000)^2*AV335^2*PI()*PI()*(O335/2)^2)/1200","v":0.68569343811537475},{"$f":"SQRT(3)*L335*J335*AV335/1000","v":16.464751485025872},{"$f":"0.75*J335^2*AV335^2-(UAC_V*0.98)^2","v":-50680.726406008485},{"$f":"-AS335/2/AR335+SQRT((AS335/2/AR335)^2-AT335/AR335)","v":260.1260067644522},{"$f":"D335+(F335-D335)*((0.85*UAC_V-D335*J335)/L335*1000)/G335","v":13.85017440630005},{"$f":"(L335^2)/1000000+((K335/1000)^2*AJ335^2*PI()*PI()*(O335/2)^2)/1200","v":1.1454060832956339},{"$f":"SQRT(3)*L335*J335*AJ335/1000","v":33.97979520526129},{"$f":"0.75*J335^2*AJ335^2-(UAC_V*0.98)^2","v":-50275.168628484163},{"$f":"IF(((AX335/2/AW335)^2-AY335/AW335)>0,-AX335/2/AW335+SQRT((AX335/2/AW335)^2-AY335/AW335),-9999)","v":195.1976281434317}]
["Cart. DDR","C131B (230 V)",190,25.9,133.26573901561372,20.253151826081112,450,396,450,0.26100000000000001,3.6,398,123,325,46,{"$f":"IF(AQ336<I336,IF(AQ336<0,0,AQ336),I336)","v":381.43203828573849},{"$f":"IF(AU336<I336,IF(AU336<0,0,AU336),I336)","v":450},{"$f":"IF(UAC_V*0.98/L336*1000<I336,IF(UAC_V*0.98/L336*1000<0,0,UAC_V*0.98/L336*1000),I336)","v":450},{"$f":"C336+(E336-C336)/G336*Q336","v":133.26573901561372},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M336,(inertia/gear^2+gear_inertia)/M336),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M336,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M336))","v":2.032520325203252E-2},{"$f":"IF((C336+(E336-C336)/G336*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X336^2*time1+Y336^2*time2+Z336^2*time3+AA336^2*time4)/time)/(C336+(E336-C336)/G336*mspeed),SQRT((((X336-Y336)*2/PI()+Y336)^2*time1+Y336^2*time2+((Z336-Y336)*2/PI()+Y336)^2*time3+AA336^2*time4)/time)/(C336+(E336-C336)/G336*mspeed)),IF(AccType=1,SQRT((X336^2*time1+Y336^2*time2+Z336^2*time3+AA336^2*time4+AB336^2*time5+AC336^2*time6+AD336^2*time7+AE336^2*time8)/time)/(C336+(E336-C336)/G336*mspeed),SQRT((((X336-Y336)*2/PI()+Y336)^2*time1+Y336^2*time2+((Z336-Y336)*2/PI()+Y336)^2*time3+AA336^2*time4+((AB336-AC336)*2/PI()+AC336)^2*time5+AC336^2*time6+((AD336-AC336)*2/PI()+AC336)^2*time7+AE336^2*time8)/time)/(C336+(E336-C336)/G336*mspeed))))","v":1.6155910666394122},{"$f":"IF(move1,MAX(ABS(X336),ABS(Z336))/H336,MAX(ABS(X336),ABS(Z336),ABS(AB336),ABS(AD336))/H336)","v":1.5446293163798113},{"$f":"IF(AZ336>0,speed/(MIN(AZ336,I336)),\"NA\")","v":6.2366556735068048},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M336+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M336+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":611.67320928640527},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M336+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M336+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-495.4552995219882},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M336+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M336+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M336+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M336+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH336/Irms","v":2.442157999692204},{"$f":"AI336/Ipeak","v":3.474196517657433},{"$f":"IF(move1,IF(AccType=1,SQRT((X336^2*time1+Y336^2*time2+Z336^2*time3+AA336^2*time4)/time)/(C336/D336),SQRT((((X336-Y336)*2/PI()+Y336)^2*time1+Y336^2*time2+((Z336-AA336)*2/PI()+AA336)^2*time3+AA336^2*time4)/time)/(C336/D336)),IF(AccType=1,SQRT((X336^2*time1+Y336^2*time2+Z336^2*time3+AA336^2*time4+AB336^2*time5+AC336^2*time6+AD336^2*time7+AE336^2*time8)/time)/(C336/D336),SQRT((((X336-Y336)*2/PI()+Y336)^2*time1+Y336^2*time2+((Z336-AA336)*2/PI()+AA336)^2*time3+AA336^2*time4+((AB336-AC336)*2/PI()+AC336)^2*time5+AC336^2*time6+((AD336-AE336)*2/PI()+AE336)^2*time7+AE336^2*time8)/time)/(C336/D336)))","v":29.305895996306447},{"$f":"IF(move1,MAX(ABS(X336),ABS(Z336))/(C336/D336),MAX(ABS(X336),ABS(Z336),ABS(AB336),ABS(AD336))/(C336/D336))","v":83.380716423778395},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X336),ABS(Z336))/(C336/D336),MAX(ABS((X336-Y336)*2/PI()+Y336),ABS((Z336-Y336)*2/PI()+Y336))/(C336/D336)),IF(AccType=1,MAX(ABS(X336),ABS(Z336),ABS(AB336),ABS(AD336))/(C336/D336),MAX(ABS((X336-Y336)*2/PI()+Y336),ABS((Z336-Y336)*2/PI()+Y336),ABS((AB336-AC336)*2/PI()+AC336),ABS((AD336-AC336)*2/PI()+AC336))/(C336/D336)))","v":53.081812709551656},{"$f":"IF((C336+(E336-C336)/G336*mspeed)<0,\"NA\",U336*(C336+(E336-C336)/G336*mspeed)*mspeed/9.55)","v":10165.300320804652},{"$f":"IF(move1,IF(speed1>speed2,AM336/2*time1/time,AM336/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z336*-speed/30*PI(),((Z336-AA336)*2/PI()+AA336)*-speed/30*PI()),IF(AccType=1,X336*-speed/30*PI(),((X336-Y336)*2/PI()+Y336)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z336*-speed/30*PI(),((Z336-AA336)*2/PI()+AA336)*-speed/30*PI()),IF(AccType=1,X336*-speed/30*PI(),((X336-Y336)*2/PI()+Y336)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD336*-speed/30*PI(),((AD336-AE336)*2/PI()+AE336)*-speed/30*PI()),IF(AccType=1,AB336*-speed/30*PI(),((AB336-AC336)*2/PI()+AC336)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD336*-speed/30*PI(),((AD336-AE336)*2/PI()+AE336)*-speed/30*PI()),IF(AccType=1,AB336*-speed/30*PI(),((AB336-AC336)*2/PI()+AC336)*-speed/30*PI()),0)/2*time7/time)))","v":8240.4207820704905},{"$f":"IF(move1,MAX(IF(AccType=1,Z336*-speed/30*PI(),((Z336-AA336)*2/PI()+AA336)*-speed/30*PI()),IF(AccType=1,X336*-speed/30*PI(),((X336-Y336)*2/PI()+Y336)*-speed/30*PI()),0),MAX(IF(AccType=1,Z336*-speed/30*PI(),((Z336-AA336)*2/PI()+AA336)*-speed/30*PI()),IF(AccType=1,X336*-speed/30*PI(),((X336-Y336)*2/PI()+Y336)*-speed/30*PI()),IF(AccType=1,AD336*-speed/30*PI(),((AD336-AE336)*2/PI()+AE336)*-speed/30*PI()),IF(AccType=1,AB336*-speed/30*PI(),((AB336-AC336)*2/PI()+AC336)*-speed/30*PI()),0))","v":79272.847923518115},{"$f":"(L336^2)/1000000+((K336/1000)^2*(D336/C336*H336)^2*PI()*PI()*(O336/2)^2)/1200","v":0.32271319617415239},{"$f":"SQRT(3)*L336*J336*D336/C336*H336/1000","v":9.7123775366621334},{"$f":"0.75*J336^2*(D336/C336*H336)^2-(UAC_V*0.98)^2","v":-50656.283902466705},{"$f":"-AO336/2/AN336+SQRT((AO336/2/AN336)^2-AP336/AN336)","v":381.43203828573849},{"$f":"(L336^2)/1000000+((K336/1000)^2*AV336^2*PI()*PI()*(O336/2)^2)/1200","v":0.18084439661269713},{"$f":"SQRT(3)*L336*J336*AV336/1000","v":3.5893010377757708},{"$f":"0.75*J336^2*AV336^2-(UAC_V*0.98)^2","v":-50784.827366449434},{"$f":"-AS336/2/AR336+SQRT((AS336/2/AR336)^2-AT336/AR336)","v":520.09424852323514},{"$f":"D336+(F336-D336)*((0.85*UAC_V-D336*J336)/L336*1000)/G336","v":19.949208883136414},{"$f":"(L336^2)/1000000+((K336/1000)^2*AJ336^2*PI()*PI()*(O336/2)^2)/1200","v":0.31728452402301699},{"$f":"SQRT(3)*L336*J336*AJ336/1000","v":9.5505845149814412},{"$f":"0.75*J336^2*AJ336^2-(UAC_V*0.98)^2","v":-50661.202674778098},{"$f":"IF(((AX336/2/AW336)^2-AY336/AW336)>0,-AX336/2/AW336+SQRT((AX336/2/AW336)^2-AY336/AW336),-9999)","v":384.82162967488404}]
["Cart. DDR","C131C (230 V)",188.8,18.8,166.15776058793875,16.289976528229289,250,394.5,250,0.65,8.67,617,123,325,46,{"$f":"IF(AQ337<I337,IF(AQ337<0,0,AQ337),I337)","v":223.47909154984697},{"$f":"IF(AU337<I337,IF(AU337<0,0,AU337),I337)","v":250},{"$f":"IF(UAC_V*0.98/L337*1000<I337,IF(UAC_V*0.98/L337*1000<0,0,UAC_V*0.98/L337*1000),I337)","v":250},{"$f":"C337+(E337-C337)/G337*Q337","v":166.15776058793875},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M337,(inertia/gear^2+gear_inertia)/M337),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M337,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M337))","v":2.032520325203252E-2},{"$f":"IF((C337+(E337-C337)/G337*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X337^2*time1+Y337^2*time2+Z337^2*time3+AA337^2*time4)/time)/(C337+(E337-C337)/G337*mspeed),SQRT((((X337-Y337)*2/PI()+Y337)^2*time1+Y337^2*time2+((Z337-Y337)*2/PI()+Y337)^2*time3+AA337^2*time4)/time)/(C337+(E337-C337)/G337*mspeed)),IF(AccType=1,SQRT((X337^2*time1+Y337^2*time2+Z337^2*time3+AA337^2*time4+AB337^2*time5+AC337^2*time6+AD337^2*time7+AE337^2*time8)/time)/(C337+(E337-C337)/G337*mspeed),SQRT((((X337-Y337)*2/PI()+Y337)^2*time1+Y337^2*time2+((Z337-Y337)*2/PI()+Y337)^2*time3+AA337^2*time4+((AB337-AC337)*2/PI()+AC337)^2*time5+AC337^2*time6+((AD337-AC337)*2/PI()+AC337)^2*time7+AE337^2*time8)/time)/(C337+(E337-C337)/G337*mspeed))))","v":1.4535587640253325},{"$f":"IF(move1,MAX(ABS(X337),ABS(Z337))/H337,MAX(ABS(X337),ABS(Z337),ABS(AB337),ABS(AD337))/H337)","v":1.5505024316512175},{"$f":"IF(AZ337>0,speed/(MIN(AZ337,I337)),\"NA\")","v":10.655116340171208},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M337+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M337+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":611.67320928640527},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M337+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M337+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-495.4552995219882},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M337+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M337+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M337+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M337+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH337/Irms","v":1.7839531883753832},{"$f":"AI337/Ipeak","v":2.5378390568909825},{"$f":"IF(move1,IF(AccType=1,SQRT((X337^2*time1+Y337^2*time2+Z337^2*time3+AA337^2*time4)/time)/(C337/D337),SQRT((((X337-Y337)*2/PI()+Y337)^2*time1+Y337^2*time2+((Z337-AA337)*2/PI()+AA337)^2*time3+AA337^2*time4)/time)/(C337/D337)),IF(AccType=1,SQRT((X337^2*time1+Y337^2*time2+Z337^2*time3+AA337^2*time4+AB337^2*time5+AC337^2*time6+AD337^2*time7+AE337^2*time8)/time)/(C337/D337),SQRT((((X337-Y337)*2/PI()+Y337)^2*time1+Y337^2*time2+((Z337-AA337)*2/PI()+AA337)^2*time3+AA337^2*time4+((AB337-AC337)*2/PI()+AC337)^2*time5+AC337^2*time6+((AD337-AE337)*2/PI()+AE337)^2*time7+AE337^2*time8)/time)/(C337/D337)))","v":21.407438260504598},{"$f":"IF(move1,MAX(ABS(X337),ABS(Z337))/(C337/D337),MAX(ABS(X337),ABS(Z337),ABS(AB337),ABS(AD337))/(C337/D337))","v":60.908137365383581},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X337),ABS(Z337))/(C337/D337),MAX(ABS((X337-Y337)*2/PI()+Y337),ABS((Z337-Y337)*2/PI()+Y337))/(C337/D337)),IF(AccType=1,MAX(ABS(X337),ABS(Z337),ABS(AB337),ABS(AD337))/(C337/D337),MAX(ABS((X337-Y337)*2/PI()+Y337),ABS((Z337-Y337)*2/PI()+Y337),ABS((AB337-AC337)*2/PI()+AC337),ABS((AD337-AC337)*2/PI()+AC337))/(C337/D337)))","v":38.775324544883873},{"$f":"IF((C337+(E337-C337)/G337*mspeed)<0,\"NA\",U337*(C337+(E337-C337)/G337*mspeed)*mspeed/9.55)","v":10165.300320804654},{"$f":"IF(move1,IF(speed1>speed2,AM337/2*time1/time,AM337/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z337*-speed/30*PI(),((Z337-AA337)*2/PI()+AA337)*-speed/30*PI()),IF(AccType=1,X337*-speed/30*PI(),((X337-Y337)*2/PI()+Y337)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z337*-speed/30*PI(),((Z337-AA337)*2/PI()+AA337)*-speed/30*PI()),IF(AccType=1,X337*-speed/30*PI(),((X337-Y337)*2/PI()+Y337)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD337*-speed/30*PI(),((AD337-AE337)*2/PI()+AE337)*-speed/30*PI()),IF(AccType=1,AB337*-speed/30*PI(),((AB337-AC337)*2/PI()+AC337)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD337*-speed/30*PI(),((AD337-AE337)*2/PI()+AE337)*-speed/30*PI()),IF(AccType=1,AB337*-speed/30*PI(),((AB337-AC337)*2/PI()+AC337)*-speed/30*PI()),0)/2*time7/time)))","v":8240.4207820704905},{"$f":"IF(move1,MAX(IF(AccType=1,Z337*-speed/30*PI(),((Z337-AA337)*2/PI()+AA337)*-speed/30*PI()),IF(AccType=1,X337*-speed/30*PI(),((X337-Y337)*2/PI()+Y337)*-speed/30*PI()),0),MAX(IF(AccType=1,Z337*-speed/30*PI(),((Z337-AA337)*2/PI()+AA337)*-speed/30*PI()),IF(AccType=1,X337*-speed/30*PI(),((X337-Y337)*2/PI()+Y337)*-speed/30*PI()),IF(AccType=1,AD337*-speed/30*PI(),((AD337-AE337)*2/PI()+AE337)*-speed/30*PI()),IF(AccType=1,AB337*-speed/30*PI(),((AB337-AC337)*2/PI()+AC337)*-speed/30*PI()),0))","v":79272.847923518115},{"$f":"(L337^2)/1000000+((K337/1000)^2*(D337/C337*H337)^2*PI()*PI()*(O337/2)^2)/1200","v":0.88537133069084861},{"$f":"SQRT(3)*L337*J337*D337/C337*H337/1000","v":27.287391060309954},{"$f":"0.75*J337^2*(D337/C337*H337)^2-(UAC_V*0.98)^2","v":-50316.177056653672},{"$f":"-AO337/2/AN337+SQRT((AO337/2/AN337)^2-AP337/AN337)","v":223.47909154984697},{"$f":"(L337^2)/1000000+((K337/1000)^2*AV337^2*PI()*PI()*(O337/2)^2)/1200","v":0.46251529114577017},{"$f":"SQRT(3)*L337*J337*AV337/1000","v":10.987512907802127},{"$f":"0.75*J337^2*AV337^2-(UAC_V*0.98)^2","v":-50725.879117245895},{"$f":"-AS337/2/AR337+SQRT((AS337/2/AR337)^2-AT337/AR337)","v":319.50552035270994},{"$f":"D337+(F337-D337)*((0.85*UAC_V-D337*J337)/L337*1000)/G337","v":15.817587669976428},{"$f":"(L337^2)/1000000+((K337/1000)^2*AJ337^2*PI()*PI()*(O337/2)^2)/1200","v":0.87241508730682193},{"$f":"SQRT(3)*L337*J337*AJ337/1000","v":26.934851750485862},{"$f":"0.75*J337^2*AJ337^2-(UAC_V*0.98)^2","v":-50328.730264165337},{"$f":"IF(((AX337/2/AW337)^2-AY337/AW337)>0,-AX337/2/AW337+SQRT((AX337/2/AW337)^2-AY337/AW337),-9999)","v":225.24390380907246}]
["Cart. DDR","C132A (230 V)",361,12.4,340.30220559285254,12.988633801253915,110,836,110,1.66,29,1584,225,325,46,83.16719770134516,110,110,340.30220559285254,1.1111111111111112E-2,1.4118359334811261,1.3263277522699362,26.090839838962935,1108.8100008976667,0,-898.13610072711003,0,0,0,0,0,1.1155261444984872,1.5869395211370112,13.386313733981847,38.086548507288271,24.246649840976705,18427.138031737511,14937.814565107861,143701.77611633763,5.5263087275935305,130.78099985935009,-49100.966278914129,83.16719770134516,3.1265742803573455,59.164843261062579,-50456.375568912561,117.92533132801952,12.990917527434171,4.6602206296615041,110.42709142120093,-49590.147011076449,91.986306872956362]
["Cart. DDR","C132B (230 V)",361,26.3,307.27514346275262,24.981718980711594,225,742,225,0.36899999999999999,6.5,746,225,325,46,203.43646858155745,225,225,307.27514346275262,1.1111111111111112E-2,1.5392905283665019,1.4943531009402515,11.499314583195229,1108.8100008976667,0,-898.13610072711003,0,0,0,0,0,2.3659949677669529,3.3658475327341453,28.391939613203434,80.780340785619487,51.426362162716721,18427.138031737511,14937.814565107861,143701.77611633763,1.0936786261416498,25.773789240834859,-50506.746202449271,203.43646858155745,0.66994687203025749,11.843798609392868,-50742.144935967764,266.51257237261336,24.840777971623503,1.0426684654655554,24.519500853181647,-50535.084242030251,208.70809148114719]
["Cart. DDR","C132C (230 V)",361.7,16.899999999999999,337.40847935481816,15.548777850452449,120,818.3,120,1.1399999999999999,19.899999999999999,1313,225,325,46,96.832509542640537,120,120,337.40847935481816,1.1111111111111112E-2,1.4418320498170889,1.3550164987140005,22.578494883173082,1108.8100008976667,0,-898.13610072711003,0,0,0,0,0,1.5174118309976234,2.1586592267038252,18.20894197197148,51.807821440891807,32.98188349256084,18427.138031737511,14937.814565107861,143701.77611633763,4.2427001788958059,99.124486792586126,-49380.299129257321,96.832509542640537,2.1319879196280778,39.896077006162656,-50574.341325116395,144.94584687273996,15.388631097338392,3.5982350158472372,85.5077852802047,-49744.876818642682,106.29583647706434]
["Cart. DDR","C133A (230 V)",504,16.8,475.34276336779408,15.6362751107827,90,1016,90,1.41,26,1837,302,325,46,74.77853509571014,90,90,475.34276336779408,8.2781456953642391E-3,1.4480641759577011,1.460727893369125,30.759896043399802,1484.099539663031,0,-1202.1206271270551,0,0,0,0,0,1.4489383631209263,2.0612493606430986,17.387260357451115,49.469984655434367,31.493570370370371,24664.015519402525,19993.690264067445,192339.3003403288,6.7479529459279668,151.93623122948432,-49094.969872000001,74.77853509571014,4.0894755718864895,69.944425497963266,-50442.726852371365,102.83899042868644,15.590649605841634,6.2917586535079808,141.28979498133745,-49326.244754388761,78.023670711168464]
["Cart. DDR","C133B (230 V)",510,32.700000000000003,443.08736156783669,28.043503896698525,175,1017,175,0.37,7,954,302,325,46,155.90147926985603,175,175,443.08736156783669,8.2781456953642391E-3,1.5462547512520892,1.4592915827561761,14.813120127639099,1484.099539663031,0,-1202.1206271270551,0,0,0,0,0,2.7870755572973116,3.9648737701781962,33.444906687567737,95.156970484276712,60.578808888888894,24664.015519402525,19993.690264067445,192339.3003403288,1.8166149604095208,39.866605225854315,-50368.582076901708,155.90147926985603,1.0723364181972392,16.8646898519461,-50727.033210721951,209.7760462641472,27.584659827244121,1.6924851391729179,37.036629413221775,-50428.364097529244,162.01853352434196]
["Cart. DDR","C133C (230 V)",498.7,20,481.2845479098915,18.948210547633526,100,1072.5999999999999,100,0.94,18.100000000000001,1536,302,325,46,89.425778976902876,100,100,481.2845479098915,8.2781456953642391E-3,1.2417729804991522,1.3836467832025277,24.95754304428101,1484.099539663031,0,-1202.1206271270551,0,0,0,0,0,1.743258507865562,2.4799470952192886,20.919102094386744,59.518730285262926,37.890800525811557,24664.015519402525,19993.690264067445,192339.3003403288,4.9967698431443646,107.57419794181133,-49578.924709597275,89.425778976902876,2.8625489473013963,46.990189843486121,-50571.183642060299,124.96076485645386,18.790031274523724,4.4057353718619297,94.757474536171543,-49853.713150974574,96.163312059275682]
["Cart. DDR","CH041A (400 V)",4.57,2.73,4.0794595013314616,2.4282497031734893,2500,12.3,2500,8.4700000000000006,34.4,102,0.58600000000000008,565,10,1211.9218110636559,1902.3723918129983,2209.8039215686276,4.1967237193067168,4.2662116040955622,1.1796349763734761,1.2228312919754132,1.6929105766250048,15.040824891297582,0,-12.183068161951041,0,0,0,0,0,0.2631638538520425,0.37437501780855581,3.1579662462245102,8.985000427405339,5.7200289268174087,249.96108996018449,202.62899229856203,1949.2909059121666,2.3540464906972931E-2,10.9950135234466,-47900.259904345119,1211.9218110636559,1.1956562612252987E-2,3.779906651663151,-50461.837857187449,1902.3723918129983,2.5260204676822204,1.8365077345397159E-2,8.5593825009745537,-49044.706597510827,1417.6767710818208]
["Cart. DDR","CH041A (480 V)",4.57,2.73,4.0794595013314616,2.4282497031734893,2500,12.3,2500,8.4700000000000006,34.4,102,0.58600000000000008,679,10,1211.9218110636559,1902.3723918129983,2209.8039215686276,4.1967237193067168,4.2662116040955622,1.1796349763734761,1.2228312919754132,1.6929105766250048,15.040824891297582,0,-12.183068161951041,0,0,0,0,0,0.2631638538520425,0.37437501780855581,3.1579662462245102,8.985000427405339,5.7200289268174087,249.96108996018449,202.62899229856203,1949.2909059121666,2.3540464906972931E-2,10.9950135234466,-47900.259904345119,1211.9218110636559,1.1956562612252987E-2,3.779906651663151,-50461.837857187449,1902.3723918129983,2.5260204676822204,1.8365077345397159E-2,8.5593825009745537,-49044.706597510827,1417.6767710818208]
["Cart. DDR","CH042A (400 V)",8.26,4.68,7.1008569409880025,3.98924547246517,2500,22.2,2500,3.7,18.3,108,0.88700000000000001,565,10,1296.1320507065986,1871.3747475279577,2087.037037037037,7.392323580237055,2.818489289740699,0.72069311769289224,0.74359755925955784,1.3709697619831731,16.507865815562184,0,-13.371371310605369,0,0,0,0,0,0.27394594191209215,0.38971353922937357,3.2873513029451056,9.3531249415049658,5.9543842711864388,274.34161104832947,222.39287003085852,2139.419409696859,2.2558272844647256E-2,8.7057238524199949,-49180.725247886781,1296.1320507065986,1.2892677485224236E-2,2.9236455078864565,-50621.953058646592,1871.3747475279577,4.2241429454286434,1.410537450527841E-2,4.1211931157593629,-50441.128949387385,1750.585655899723]
["Cart. DDR","CH042A (480 V)",8.26,4.68,7.1008569409880025,3.98924547246517,2500,22.2,2500,3.7,18.3,108,0.88700000000000001,679,10,1296.1320507065986,1871.3747475279577,2087.037037037037,7.392323580237055,2.818489289740699,0.72069311769289224,0.74359755925955784,1.3709697619831731,16.507865815562184,0,-13.371371310605369,0,0,0,0,0,0.27394594191209215,0.38971353922937357,3.2873513029451056,9.3531249415049658,5.9543842711864388,274.34161104832947,222.39287003085852,2139.419409696859,2.2558272844647256E-2,8.7057238524199949,-49180.725247886781,1296.1320507065986,1.2892677485224236E-2,2.9236455078864565,-50621.953058646592,1871.3747475279577,4.2241429454286434,1.410537450527841E-2,4.1211931157593629,-50441.128949387385,1750.585655899723]
["Cart. DDR","CH043A (400 V)",11.1,4.7300000000000004,9.3922637083297165,3.9629804676496692,2250,30,2250,3.97,20.6,143,1.19,565,10,1019.287975018324,1421.0423362960305,1576.2237762237762,10.021437524581041,2.1008403361344539,0.58761035587915245,0.59948848400181542,1.7205166186343328,17.984654520054463,0,-14.567570161244113,0,0,0,0,0,0.22446487825326153,0.3193221316811472,2.6935785390391382,7.6637311603475329,4.8788827867867868,298.88412895433601,242.28806920988129,2330.8112257990579,3.470874574802256E-2,12.570327371767856,-48873.364677081816,1019.287975018324,2.2068899409901119E-2,4.2367683665674551,-50585.709095408747,1421.0423362960305,4.308712823328479,2.2525986710457829E-2,4.7974179535317969,-50523.786595177407,1394.9298565363524]
["Cart. DDR","CH043A (480 V)",11.1,4.7300000000000004,9.1749641593615827,3.8712928942453932,2500,30,2500,3.97,20.6,143,1.19,679,10,1019.287975018324,1421.1863058127833,1576.2237762237762,10.005666170034353,2.1008403361344539,0.58788231372594901,0.59948848400181542,1.7205166186343328,17.984654520054463,0,-14.567570161244113,0,0,0,0,0,0.22446487825326153,0.3193221316811472,2.6935785390391382,7.6637311603475329,4.8788827867867868,298.88412895433595,242.28806920988129,2330.8112257990579,3.470874574802256E-2,12.570327371767856,-48873.364677081816,1019.287975018324,2.2066497979040069E-2,4.2336267888298789,-50586.034421889854,1421.1863058127833,4.3055178985385876,2.2525986710457829E-2,4.7974179535317969,-50523.786595177407,1394.9298565363524]
["Cart. DDR","CH044A (400 V)",14.1,5,12.316011704343641,4.3214076155591723,1850,38.1,1850,4.08,22.1,173,1.49,565,10,846.11965598810775,1170.0199356498563,1302.8901734104045,12.971728718441108,1.6778523489932886,0.50019871555035156,0.51041526388990122,2.0368339495263736,19.446821554205236,0,-15.751925458906239,0,0,0,0,0,0.20197966910709905,0.28733483383872988,2.4237560292851885,6.8960360121295166,4.3901528762805366,323.18365163355031,261.98628621881483,2520.3080734249988,4.8260364377784776E-2,16.517440876152222,-48526.217727478499,846.11965598810775,3.2080635829538448E-2,5.6588704249325126,-50537.670153311374,1170.0199356498563,4.6287407388983315,3.1864540855527132E-2,5.3671846564534942,-50564.534927858687,1178.2992916816188]
["Cart. DDR","CH044A (480 V)",14.2,5,11.756245129721334,4.1249982911302929,2250,38.1,2250,4.08,22.1,173,1.49,679,10,849.33677298171335,1170.7998922570887,1302.8901734104045,12.928378693855556,1.6778523489932886,0.49855679139447517,0.51041526388990122,2.0349943597437679,19.446821554205236,0,-15.751925458906239,0,0,0,0,0,0.20055727707113355,0.28531134909338668,2.4066873248536025,6.8474723782412807,4.3592363067292652,323.18365163355026,261.98628621881483,2520.3080734249988,4.8003085260600042E-2,16.401120869982137,-48558.202485617934,849.33677298171335,3.2059906593198614E-2,5.6315451773134706,-50540.247197332668,1170.7998922570887,4.6063897258238002,3.1837375706642281E-2,5.3293875814080467,-50567.912079982074,1179.3644481167953]
["Cart. DDR","CH051A (400 V)",11.7,4.75,10.27231475555976,4.1254276126746019,2100,30,2100,4.13,24,151,2.74,565,10,949.73146406182479,1327.7002168922265,1492.7152317880793,10.797362853001363,0.91240875912408748,0.78787627502238589,0.85130613988333692,1.9686741400259831,25.539184196500109,0,-20.686739199165086,0,0,0,0,0,0.30368469418618044,0.43201967568865934,3.6442163302341655,10.368472216527824,6.6007744222855349,424.43166279694327,344.06219042270408,3309.8782718664133,4.0369674500952947E-2,13.155780805999616,-48907.495767998029,949.73146406182479,2.5097634029171492E-2,4.7565605361037875,-50557.091185763566,1327.7002168922265,4.403575045998867,2.7961250373035651E-2,7.1298848769011611,-50247.780297817379,1219.0945932618001]
["Cart. DDR","CH051A (480 V)",11.7,4.75,10.030581133423611,4.0283458367163094,2500,30,2500,4.13,24,151,2.74,679,10,949.73146406182479,1327.216616497142,1492.7152317880793,10.813727816154396,0.91240875912408748,0.78749914963390466,0.85130613988333692,1.9686741400259831,25.539184196500109,0,-20.686739199165086,0,0,0,0,0,0.30368469418618044,0.43201967568865934,3.6442163302341655,10.368472216527824,6.6007744222855349,424.43166279694327,344.06219042270408,3309.8782718664133,4.0369674500952947E-2,13.155780805999616,-48907.495767998029,949.73146406182479,2.510828180922664E-2,4.7675740982507788,-50555.941075585375,1327.216616497142,4.4137712890761751,2.7961250373035651E-2,7.1298848769011611,-50247.780297817379,1219.0945932618001]
["Cart. DDR","CH052A (400 V)",16.8,9.84,14.090942041584047,8.1450532032277732,2500,26.6,2500,1.1399999999999999,7,105,3.59,565,10,1821.3313921108877,2000.6124171236843,2146.6666666666665,14.632090003874122,0.69637883008356549,0.63960277938010213,1.1158643155361134,1.2358926960245771,29.681990793260617,0,-24.042412542541101,0,0,0,0,0,0.50919833903963974,0.72438191816886022,6.1103800684756768,17.385166036052645,11.067740444444443,493.28031038805045,399.87380528134889,3846.7860068065766,1.3470622913447599E-2,3.2301465843561949,-50568.564830920004,1821.3313921108877,1.1778870590016402E-2,1.7933947093506295,-50732.228830305517,2000.6124171236843,8.6500995673085779,1.2259162992246234E-2,2.2946356863390975,-50685.764241881618,1941.9161612654059]
["Cart. DDR","CH052A (480 V)",16.8,9.84,14.090942041584047,8.1450532032277732,2500,26.6,2500,1.1399999999999999,7,105,3.59,679,10,1821.3313921108877,2000.6124171236843,2146.6666666666665,14.632090003874122,0.69637883008356549,0.63960277938010213,1.1158643155361134,1.2358926960245771,29.681990793260617,0,-24.042412542541101,0,0,0,0,0,0.50919833903963974,0.72438191816886022,6.1103800684756768,17.385166036052645,11.067740444444443,493.28031038805045,399.87380528134889,3846.7860068065766,1.3470622913447599E-2,3.2301465843561949,-50568.564830920004,1821.3313921108877,1.1778870590016402E-2,1.7933947093506295,-50732.228830305517,2000.6124171236843,8.6500995673085779,1.2259162992246234E-2,2.2946356863390975,-50685.764241881618,1941.9161612654059]
["Cart. DDR","CH052C (400 V)",16.899999999999999,5.74,10.504226244065093,3.5131191451722716,2500,43.1,1750,3.36,90,181,3.59,565,10,335.34404173572756,801.83077278903488,1245.3038674033151,14.848668714677952,0.69637883008356549,0.66259177517775869,0.68867728058609323,3.5662658187679037,29.681990793260617,0,-24.042412542541101,0,0,0,0,0,0.29527477648452488,0.42005578686714978,3.5432973178142988,10.081338884811595,6.417979666009205,493.28031038805045,399.87380528134889,3846.7860068065766,0.38966255715719988,15.419877996977307,-48990.711132126125,335.34404173572756,7.2306877348061488E-2,5.1328352368179413,-50604.113041968201,801.83077278903488,4.8728028901651461,0.10136354075452966,6.760468855689056,-50456.392111743073,672.97282983498053]
["Cart. DDR","CH052C (480 V)",16.899999999999999,5.74,12.108508070431398,4.0496682509804005,2500,43.1,2100,3.36,90,181,3.59,679,10,335.34404173572756,782.52232345314428,1245.3038674033151,15.400220240986794,0.69637883008356549,0.65061762078038421,0.68867728058609323,3.5662658187679037,29.681990793260617,0,-24.042412542541101,0,0,0,0,0,0.29527477648452488,0.42005578686714978,3.5432973178142988,10.081338884811595,6.417979666009205,493.28031038805045,399.87380528134889,3846.7860068065766,0.38966255715719988,15.419877996977307,-48990.711132126125,335.34404173572756,7.5771017656359019E-2,5.3529295368023408,-50586.50172777105,782.52232345314428,5.0817470879800224,0.10136354075452966,6.760468855689056,-50456.392111743073,672.97282983498053]
["Cart. DDR","CH053A (400 V)",20.9,9.2100000000000009,16.93679496528561,7.3638238979502662,2350,53.7,2350,1.41,9.1,139,4.43,565,10,1184.0940851443713,1507.8705825984821,1621.5827338129495,18.357021155467223,0.56433408577878108,0.58948413267379884,0.62897688061234214,1.6175640162220295,33.776058488882775,0,-27.358607375995042,0,0,0,0,0,0.43594374199308022,0.62017045191907971,5.2313249039169625,14.884090846057914,9.4755065263157903,561.31897388985067,455.02881290636242,4377.3771801592065,2.8855908992907277E-2,8.0330814429213415,-49970.182547117038,1184.0940851443713,2.0459896546824074E-2,2.7762976918096935,-50705.426175747278,1507.8705825984821,8.1784592056577541,2.0849784119631495E-2,3.2165993906944581,-50671.2834972282,1483.7125306517526]
["Cart. DDR","CH053A (480 V)",20.9,9.2100000000000009,16.810581709138354,7.3089485691905898,2500,53.7,2500,1.41,9.1,139,4.43,679,10,1184.0940851443713,1507.2703115677714,1621.5827338129495,18.434456487440809,0.56433408577878108,0.58881471054922296,0.62897688061234214,1.6175640162220295,33.776058488882775,0,-27.358607375995042,0,0,0,0,0,0.43594374199308022,0.62017045191907971,5.2313249039169625,14.884090846057914,9.4755065263157903,561.31897388985044,455.02881290636242,4377.3771801592065,2.8855908992907277E-2,8.0330814429213415,-49970.182547117038,1184.0940851443713,2.0469125769550477E-2,2.7875240709646296,-50704.61796741619,1507.2703115677714,8.2115300410428613,2.0849784119631495E-2,3.2165993906944581,-50671.2834972282,1483.7125306517526]
["Cart. DDR","CH054A (400 V)",24.8,9.7899999999999991,20.326359874879206,7.9090894454782905,2100,63.5,2100,1.35,9,155.5,5.28,565,10,1076.3264530306933,1350.3256115986253,1449.5176848874598,21.923394839035293,0.47348484848484845,0.55908024515632848,0.59714748166367382,1.7928164218474258,37.91886508564329,0,-30.714280719371061,0,0,0,0,0,0.43842415840275328,0.62369907457736518,5.2610899008330394,14.968777789856764,9.52941990919952,630.16762148095768,510.84042776500723,4914.2849150993698,3.4645581736585329E-2,9.1144302442716825,-49946.268563003963,1076.3264530306933,2.5452498755765243E-2,3.1778913375197346,-50700.746342644488,1350.3256115986253,8.7400567782417458,2.5692684082524238E-2,3.4649043764136085,-50681.034294747886,1338.6758235552616]
["Cart. DDR","CH054A (480 V)",24.8,9.7899999999999991,19.251381916395662,7.4908100842006471,2500,63.5,2500,1.35,9,156,5.28,679,10,1073.8020505359475,1346.5600427611087,1444.8717948717949,21.811381038430675,0.47348484848484845,0.56002590877141711,0.59714748166367382,1.7982585198798973,37.91886508564329,0,-30.714280719371061,0,0,0,0,0,0.43842415840275328,0.62369907457736518,5.2610899008330394,14.968777789856764,9.52941990919952,630.16762148095768,510.84042776500723,4914.2849150993698,3.4801331736585325E-2,9.1437370939317208,-49946.268563003963,1073.8020505359475,2.5601072809504855E-2,3.1791058739217277,-50701.335273693257,1346.5600427611087,8.7153733717522783,2.5848434082524237E-2,3.4760455480419483,-50681.034294747886,1334.6245678626296]
["Cart. DDR","CH061A (400 V)",33.4,9.89,29.131322896182791,8.5680361459361158,1600,85.7,1600,1.36,18.100000000000001,206,9.41,565,10,694.26248634850731,981.5113166244389,1094.1747572815534,30.781403197242359,0.26567481402763016,0.63370151135141384,0.67733992130438203,2.5258759809901639,58.048031255785546,0,-47.018905317186288,0,0,0,0,0,0.50343737617821771,0.7161864135725039,6.041248514138613,17.188473925740094,10.942522357950766,964.69105036480801,782.01921525465764,7523.0248507498063,8.581474180151874E-2,12.313950481271291,-49911.853747907429,694.26248634850731,4.8087852045967265E-2,4.4448214450167285,-50688.770391659913,981.5113166244389,9.1598331588386266,5.0501857462986542E-2,5.3098737930900626,-50639.058342807148,950.16541511241599]
["Cart. DDR","CH061A (480 V)",33.4,9.89,27.893997920842708,8.204117035541973,1900,85.7,1900,1.36,18.100000000000001,206,9.41,679,10,694.26248634850731,982.43361545967196,1094.1747572815534,30.553009721392122,0.26567481402763016,0.63575213807826736,0.67733992130438203,2.5258759809901639,58.048031255785546,0,-47.018905317186288,0,0,0,0,0,0.50343737617821771,0.7161864135725039,6.041248514138613,17.188473925740094,10.942522357950766,964.69105036480801,782.01921525465764,7523.0248507498063,8.581474180151874E-2,12.313950481271291,-49911.853747907429,694.26248634850731,4.8021436603023326E-2,4.4186285120884294,-50690.138096852672,982.43361545967196,9.1058550860337313,5.0501857462986542E-2,5.3098737930900626,-50639.058342807148,950.16541511241599]
["Cart. DDR","CH062A (400 V)",47.3,14.6,39.701923985832799,12.141261157747033,1650,121.5,1650,0.76,11.1,198,12.6,565,10,756.28181745859104,1039.5956607375051,1138.3838383838386,42.512771603465488,0.19841269841269843,0.57201257480328338,0.60572626106108696,2.3391691397260774,73.595740718922059,0,-59.612549982326861,0,0,0,0,0,0.66535363112225576,0.94652732073314139,7.9842435734670687,22.716655697595392,14.4618721791559,1223.0759748537866,991.47692278298302,9538.0079971722971,7.4836020663870462E-2,9.7747892578686457,-50195.869461816757,756.28181745859104,4.3626352247665298E-2,3.4436090702839133,-50729.53988834723,1039.5956607375051,13.212178520150548,4.4502506885158166E-2,3.7693279827754234,-50714.558062431555,1026.0053278067126]
["Cart. DDR","CH062A (480 V)",47.3,14.6,37.543059525947193,11.481057959005257,2000,121.5,2000,0.76,11.1,198,12.6,679,10,756.28181745859104,1040.2848064813709,1138.3838383838386,42.225001533549857,0.19841269841269843,0.57357950400611779,0.60572626106108696,2.3391691397260774,73.595740718922059,0,-59.612549982326861,0,0,0,0,0,0.66535363112225576,0.94652732073314139,7.9842435734670687,22.716655697595392,14.4618721791559,1223.0759748537866,991.47692278298302,9538.0079971722971,7.4836020663870462E-2,9.7747892578686457,-50195.869461816757,756.28181745859104,4.3583235162129835E-2,3.4267806877244356,-50730.27716992041,1040.2848064813709,13.147612656243448,4.4502506885158166E-2,3.7693279827754234,-50714.558062431555,1026.0053278067126]
["Cart. DDR","CH062C (400 V)",48.4,11.8,40.489017522578173,9.7799559233280622,1250,124.2,1250,1.19,17.8,250.4,12.6,565,10,577.33440435114846,812.31087329319405,900.15974440894558,43.259058332126656,0.19841269841269843,0.5679737502947837,0.59255829886410671,2.9881156146132093,73.595740718922059,0,-59.612549982326861,0,0,0,0,0,0.52552993840509432,0.74761513471356789,6.3063592608611314,17.942763233125628,11.422717845117846,1223.0759748537864,991.47692278298302,9538.0079971722971,0.12243325195315058,15.627883130453613,-49831.355742008011,577.33440435114846,7.0060119981801824E-2,5.4856789067888085,-50685.173571463027,812.31087329319405,10.628903648355475,7.1200521806924266E-2,5.8953740116797624,-50666.58206520052,803.18177391227323]
["Cart. DDR","CH062C (480 V)",48.4,11.8,37.889144516715724,9.1519672745690155,1550,124.2,1550,1.19,17.8,250.4,12.6,679,10,577.33440435114846,813.07067288834628,900.15974440894558,42.886407522305731,0.19841269841269843,0.57053301367414178,0.59255829886410671,2.9881156146132093,73.595740718922059,0,-59.612549982326861,0,0,0,0,0,0.52552993840509432,0.74761513471356789,6.3063592608611314,17.942763233125628,11.422717845117846,1223.0759748537866,991.47692278298302,9538.0079971722971,0.12243325195315058,15.627883130453613,-49831.355742008011,577.33440435114846,6.9967706816924782E-2,5.451130460946275,-50686.680145633378,813.07067288834628,10.561963510534744,7.1200521806924266E-2,5.8953740116797624,-50666.58206520052,803.18177391227323]
["Cart. DDR","CH063A (400 V)",60.2,13.9,52.437097410372942,12.026857204213977,1250,154.4,1250,0.93,14.4,264,15.7,565,10,576.92451007275145,777.88463410193299,853.78787878787875,55.369085887599205,0.15923566878980894,0.54319699772897856,0.57451295383298795,3.0909467160677448,88.704800071813338,0,-71.850888058168806,0,0,0,0,0,0.59989268465105139,0.85340304609510342,7.1987122158126162,20.481673106282482,13.039038070628768,1474.1710425390011,1195.025165208629,11496.14208930701,0.12388544489239156,15.160485444035794,-49980.721298715776,576.92451007275145,7.6751276026513035E-2,5.4703203680664343,-50697.820967167121,777.88463410193299,12.863680910136237,7.6944941566259584E-2,5.5448915466761841,-50694.874537906049,776.46113649388406]
["Cart. DDR","CH063A (480 V)",60.2,13.9,50.674933880459477,11.622691256986117,1500,154.4,1500,0.93,14.4,264,15.7,679,10,576.92451007275145,777.99488991477097,853.78787878787875,55.259698155264772,0.15923566878980894,0.54379476956146922,0.57451295383298795,3.0909467160677448,88.704800071813338,0,-71.850888058168806,0,0,0,0,0,0.59989268465105139,0.85340304609510342,7.1987122158126162,20.481673106282482,13.039038070628768,1474.1710425390013,1195.025165208629,11496.14208930701,0.12388544489239156,15.160485444035794,-49980.721298715776,576.92451007275145,7.6736345942216178E-2,5.4645292694893586,-50698.048113603705,777.99488991477097,12.850062906216481,7.6944941566259584E-2,5.5448915466761841,-50694.874537906049,776.46113649388406]
["Cart. DDR","CH063B (400 V)",58,19.5,45.800491136899048,15.266830378966349,1850,149,1850,0.47,7.1,181,15.7,565,10,865.27286689511084,1155.8269272553721,1245.3038674033151,50.378096841479646,0.15923566878980894,0.56662796144575633,0.59533422866988817,2.1025976755732052,88.704800071813338,0,-71.850888058168806,0,0,0,0,0,0.87349791926552856,1.24263189755773,10.481975031186343,29.823165541385517,18.986016858237544,1474.1710425390011,1195.025165208629,11496.14208930701,5.877223530614345E-2,7.3812505339959316,-50389.399954171007,865.27286689511084,3.5807614588113559E-2,2.5261446554741749,-50756.463326971243,1155.8269272553721,17.144355199834834,3.6497310236553067E-2,2.7975053279134929,-50745.439325572297,1141.4451884361176]
["Cart. DDR","CH063B (480 V)",58,19.5,41.73910725740906,13.913035752469687,2200,149,2200,0.47,7.1,181,15.7,679,10,865.27286689511084,1157.7940437195543,1245.3038674033151,49.442379653211674,0.15923566878980894,0.57035852762479866,0.59533422866988817,2.1025976755732052,88.704800071813338,0,-71.850888058168806,0,0,0,0,0,0.87349791926552856,1.24263189755773,10.481975031186343,29.823165541385517,18.986016858237544,1474.1710425390011,1195.025165208629,11496.14208930701,5.877223530614345E-2,7.3812505339959316,-50389.399954171007,865.27286689511084,3.5716351327323204E-2,2.4880208511549178,-50757.922066513682,1157.7940437195543,16.885617822542539,3.6497310236553067E-2,2.7975053279134929,-50745.439325572297,1141.4451884361176]
["Cart. DDR","CH063C (400 V)",61.8,11.3,54.07917434743559,9.7969518745354343,950,158.9,950,1.45,23.1,333.8,15.7,565,10,436.32799364763662,606.02680031057946,675.25464349910123,56.874708141074258,0.15923566878980894,0.53633417917246229,0.55824292052745961,3.9530887411659283,88.704800071813338,0,-71.850888058168806,0,0,0,0,0,0.47505645696342835,0.6758119207197214,5.7006774835611402,16.219486097273315,10.325645547165289,1474.1710425390011,1195.025165208629,11496.14208930701,0.20404359640555086,24.357282183837658,-49474.016122287634,436.32799364763662,0.12340639695216517,8.7614068547399597,-50632.927525836174,606.02680031057946,10.451024991351311,0.12312058212085314,8.6562975164076938,-50637.035233811599,607.12019313083806]
["Cart. DDR","CH063C (480 V)",61.8,11.3,51.89835100822674,9.4018751826497731,1150,158.9,1150,1.45,23.1,333.8,15.7,679,10,436.32799364763662,606.34722469644908,675.25464349910123,56.579271838191204,0.15923566878980894,0.53835384213655135,0.55824292052745961,3.9530887411659283,88.704800071813338,0,-71.850888058168806,0,0,0,0,0,0.47505645696342835,0.6758119207197214,5.7006774835611402,16.219486097273315,10.325645547165289,1474.1710425390013,1195.025165208629,11496.14208930701,0.20404359640555086,24.357282183837658,-49474.016122287634,436.32799364763662,0.12332238715736213,8.7306432894146297,-50634.134907911284,606.34722469644908,10.414328739782515,0.12312058212085314,8.6562975164076938,-50637.035233811599,607.12019313083806]
["Cart. DDR","CH091A (400 V)",50,12.8,28.842332447196419,7.1569063144407981,884,120,1200,0.91600000000000004,7.8,244,28,565,38,442.08949414561317,823.6514486576059,923.77049180327879,30.28671546370736,8.9285714285714288E-2,1.3331019780947915,1.2387804039332906,4.5771713639187945,148.65364847199487,0,-120.40945526231586,0,0,0,0,0,1.1146118954924324,1.5856389170346119,13.37534274590919,38.055334008830684,24.226778074074073,2470.4514723867878,2002.6520625749001,19265.51284197054,0.23000967725837071,11.89233511510654,-50211.285560627206,442.08949414561317,7.1073951996628804E-2,3.0938755325472691,-50764.9655554165,823.6514486576059,7.9920264136452257,0.16556049893675479,9.3786772010483173,-50435.80538245153,524.34130365292117]
["Cart. DDR","CH091A (480 V)",50,12.8,28.842332447196419,7.1569063144407981,884,120,1500,0.91600000000000004,7.8,244,28,679,38,442.08949414561317,823.6514486576059,923.77049180327879,30.28671546370736,8.9285714285714288E-2,1.3331019780947915,1.2387804039332906,4.5771713639187945,148.65364847199487,0,-120.40945526231586,0,0,0,0,0,1.1146118954924324,1.5856389170346119,13.37534274590919,38.055334008830684,24.226778074074073,2470.4514723867878,2002.6520625749001,19265.51284197054,0.23000967725837071,11.89233511510654,-50211.285560627206,442.08949414561317,7.1073951996628804E-2,3.0938755325472691,-50764.9655554165,823.6514486576059,7.9920264136452257,0.16556049893675479,9.3786772010483173,-50435.80538245153,524.34130365292117]
["Cart. DDR","CH092A (400 V)",101,15.3,69.437028028949783,10.211327651316145,700,227,700,0.92100000000000004,11,441,47,565,38,265.43095493177839,434.28958096573155,511.11111111111109,81.417900183799247,5.3191489361702128E-2,1.0515357487263428,1.0628086371580483,7.0638611088354573,241.25756063487694,0,-195.41862411425032,0,0,0,0,0,1.070432101945699,1.5227890584627133,12.845185223348389,36.546937403105119,23.266502970297029,4009.4212420703602,3250.2058064740177,31266.979858280047,0.61929899024442847,24.191052348087272,-50052.892408682732,265.43095493177839,0.24891879970284223,8.6597148749337105,-50708.761557844795,434.28958096573155,12.309622819887641,0.38896026130647987,16.367786796363401,-50460.776172516591,339.75752963178832]
["Cart. DDR","CH092A (480 V)",101,15.3,67.944370989854903,9.9918192632139569,721,227,800,0.92100000000000004,11,441,47,679,38,265.43095493177839,434.62690854259625,511.11111111111109,81.073695080984294,5.3191489361702128E-2,1.0560119542081723,1.0628086371580483,7.0638611088354573,241.25756063487694,0,-195.41862411425032,0,0,0,0,0,1.070432101945699,1.5227890584627133,12.845185223348389,36.546937403105119,23.266502970297029,4009.4212420703602,3250.2058064740177,31266.979858280047,0.61929899024442847,24.191052348087272,-50052.892408682732,265.43095493177839,0.24858198845666307,8.6328841173011579,-50709.357983115638,434.62690854259625,12.271483399456542,0.38896026130647987,16.367786796363401,-50460.776172516591,339.75752963178832]
["Cart. DDR","CH092C (400 V)",101.6,18.100000000000001,60.041202281417512,10.589277298309966,800,231.2,800,0.59,7.35,343,47,565,38,341.4192002573426,576.25663883424374,657.14285714285711,71.664333640871774,5.3191489361702128E-2,1.0851376099336425,1.0435015598394333,5.4340206093593526,241.25756063487694,0,-195.41862411425032,0,0,0,0,0,1.2588498569083764,1.7908308101588226,15.106198282900516,42.979939443811745,27.361879265091865,4009.4212420703611,3250.2058064740177,31266.979858280047,0.38975979599526256,14.437083081036832,-50362.25490117052,341.4192002573426,0.1449283729369534,4.5711319826232186,-50760.758331472091,576.25663883424374,13.041183380287706,0.23773495712059384,9.5907524467750562,-50609.700343531775,441.66192448117152]
["Cart. DDR","CH092C (480 V)",101.6,18.100000000000001,42.207890907970643,7.4440724705415597,1000,231.2,1000,0.64,7.35,343,47,679,38,339.65491121542971,581.00723576188807,657.14285714285711,67.092754870371522,5.3191489361702128E-2,1.1339120557267122,1.0435015598394333,5.4561194730559155,241.25756063487694,0,-195.41862411425032,0,0,0,0,0,1.2588498569083764,1.7908308101588226,15.106198282900516,42.979939443811745,27.361879265091865,4009.4212420703602,3250.2058064740177,31266.979858280047,0.38975979599526256,15.660564698073852,-50284.00536489355,339.65491121542971,0.14225745174720519,4.7095203412850788,-50758.029166238186,581.00723576188807,12.386310298810852,0.23773495712059384,10.40352807785769,-50575.167827378958,439.8730658028984]
["Cart. DDR","CH093A (400 V)",145,15.5,109.38285179770261,12.793315999731298,550,309,550,0.86699999999999999,11,517,66,565,38,257.15331937344519,373.19355259134835,435.97678916827851,120.83256350765834,3.787878787878788E-2,1.0136912880719222,1.0804578407694467,7.6162892492079726,333.86147279775901,0,-270.42779296618477,0,0,0,0,0,1.0452932271402366,1.4870266748176046,12.543518725682839,35.688640195622511,22.720093997445719,5548.3910117539326,4497.7595503731354,43268.446874589565,0.6592613406265776,25.644394149670696,-50190.062716438333,257.15331937344519,0.33537984445876767,10.688311251775701,-50698.309365092813,373.19355259134835,13.766984529224828,0.45274091367703173,17.639261219390221,-50514.142097686512,315.11408265509073]
["Cart. DDR","CH093A (480 V)",145,15.5,96.52771935511548,11.289791737440407,646,309,650,0.86699999999999999,11,517,66,679,38,257.15331937344519,376.80216795852022,435.97678916827851,116.72684143516051,3.787878787878788E-2,1.0560228026197265,1.0804578407694467,7.6162892492079726,333.86147279775901,0,-270.42779296618477,0,0,0,0,0,1.0452932271402366,1.4870266748176046,12.543518725682839,35.688640195622511,22.720093997445719,5548.3910117539326,4497.7595503731354,43268.446874589565,0.6592613406265776,25.644394149670696,-50190.062716438333,257.15331937344519,0.32993341243492613,10.251936375341943,-50706.856104736769,376.80216795852022,13.204915739189557,0.45274091367703173,17.639261219390221,-50514.142097686512,315.11408265509073]
["Cart. DDR","CH093C (400 V)",139.4,20,87.853528586726242,12.461493416556914,700,316.60000000000002,700,0.65,7.54,426,66,565,38,287.8084498922816,462.26576020432674,529.10798122065728,105.35975886613201,3.787878787878788E-2,1.1054604380714865,1.0545213922860359,6.5695739323002718,333.86147279775901,0,-270.42779296618477,0,0,0,0,0,1.4029482846793568,1.9958242037168759,16.835379416152282,47.899780889205019,30.493947606142722,5548.3910117539326,4497.7595503731354,43268.446874589565,0.5297528901178814,21.785208235834901,-50151.361015728406,287.8084498922816,0.22143752603449493,7.3793892440103006,-50730.142662150072,462.26576020432674,15.386393522876045,0.33843842239082211,14.625045735221843,-50510.504008632925,365.3204948649788]
["Cart. DDR","CH093C (480 V)",139.4,20,67.322540927871728,9.5492965855137211,800,316.60000000000002,800,0.59,7.54,426,66,679,38,289.93803130745482,470.13042017724047,529.10798122065728,97.042742351390601,3.787878787878788E-2,1.1886893626697075,1.0545213922860359,6.5322683600885636,333.86147279775901,0,-270.42779296618477,0,0,0,0,0,1.4029482846793568,1.9958242037168759,16.835379416152282,47.899780889205019,30.493947606142722,5548.3910117539326,4497.7595503731354,43268.446874589565,0.5297528901178814,19.774265937142449,-50266.491535088899,289.93803130745482,0.21631683427541901,6.2543519202875437,-50751.272822159954,470.13042017724047,14.36680100574786,0.33843842239082211,13.275041513509056,-50562.391359538749,367.40682833297762]
["Cart. DDR","CH131A (400 V)",188,13.8,142.7619839534301,11.70180196339591,400,389,400,0.93,13,738,123,565,46,195.31276231739977,266.22533114444195,305.42005420054204,157.89123549421089,2.032520325203252E-2,1.5700280634022441,1.5724247025357463,12.295231365395864,611.67320928640527,0,-495.4552995219882,0,0,0,0,0,1.3150698831826499,1.8708090177642713,15.780838598191799,44.899416426342512,28.583856264775417,10165.300320804654,8240.4207820704905,79272.847923518115,1.1441624499909331,33.944606318885967,-50276.26575984306,195.31276231739977,0.65956419827735369,14.861672374561662,-50703.77758058071,266.22533114444195,12.501661779965032,1.1454060832956339,33.97979520526129,-50275.168628484163,195.1976281434317]
["Cart. DDR","CH131A (480 V)",188,13.8,121.08508070431398,9.9250066151077032,500,389,500,0.93,13,738,123,679,46,195.31276231739977,268.97666756743018,305.42005420054204,152.00289599460569,2.032520325203252E-2,1.6852620477007743,1.5724247025357463,12.295231365395864,611.67320928640527,0,-495.4552995219882,0,0,0,0,0,1.3150698831826499,1.8708090177642713,15.780838598191799,44.899416426342512,28.583856264775417,10165.300320804654,8240.4207820704905,79272.847923518115,1.1441624499909331,33.944606318885967,-50276.26575984306,195.31276231739977,0.64845004130971207,14.124751451120177,-50713.58247249767,268.97666756743018,11.881762759770362,1.1454060832956339,33.97979520526129,-50275.168628484163,195.1976281434317]
["Cart. DDR","CH131B (400 V)",190,25.9,123.9498696799681,18.837366212761111,500,396,800,0.26100000000000001,3.6,398,123,565,46,381.43203828573849,522.8155158472299,566.3316582914573,120.93593408991153,2.032520325203252E-2,1.6493068134073563,1.5446293163798113,6.2366556735068048,611.67320928640527,0,-495.4552995219882,0,0,0,0,0,2.442157999692204,3.474196517657433,29.305895996306447,83.380716423778395,53.081812709551656,10165.300320804654,8240.4207820704905,79272.847923518115,0.32271319617415239,9.7123775366621334,-50656.283902466705,381.43203828573849,0.17919375280061484,3.4547711402410246,-50786.322969951136,522.8155158472299,19.201496445895241,0.31728452402301699,9.5505845149814412,-50661.202674778098,384.82162967488404]
["Cart. DDR","CH131B (480 V)",190,25.9,123.9498696799681,18.837366212761111,500,396,1000,0.26100000000000001,3.6,398,123,679,46,381.43203828573849,522.8155158472299,566.3316582914573,120.93593408991153,2.032520325203252E-2,1.6493068134073563,1.5446293163798113,6.2366556735068048,611.67320928640527,0,-495.4552995219882,0,0,0,0,0,2.442157999692204,3.474196517657433,29.305895996306447,83.380716423778395,53.081812709551656,10165.300320804654,8240.4207820704905,79272.847923518115,0.32271319617415239,9.7123775366621334,-50656.283902466705,381.43203828573849,0.17919375280061484,3.4547711402410246,-50786.322969951136,522.8155158472299,19.201496445895241,0.31728452402301699,9.5505845149814412,-50661.202674778098,384.82162967488404]
["Cart. DDR","CH131C (400 V)",188.8,18.8,121.27606663602425,11.889810454512183,500,394.5,500,1.1399999999999999,8.67,617,123,565,46,210.49037082974857,314.64077157555232,365.31604538087521,146.30843501308499,2.032520325203252E-2,1.681965987082644,1.5505024316512175,11.306053472903594,611.67320928640527,0,-495.4552995219882,0,0,0,0,0,1.7839531883753832,2.5378390568909825,21.407438260504598,60.908137365383581,38.775324544883873,10165.300320804654,8240.4207820704905,79272.847923518115,0.88537133069084861,47.857885859620531,-49301.060039827484,210.49037082974857,0.45330677468735786,18.153732330355115,-50588.737935321107,314.64077157555232,14.900995546826667,0.87241508730682193,47.239586147005966,-49339.673409016024,212.27566327648347]
["Cart. DDR","CH131C (480 V)",188.8,18.8,91.35493733474793,8.9563664053674454,600,394.5,600,0.65,8.67,617,123,679,46,223.47909154984697,327.30314034836385,365.31604538087521,135.64320829703314,2.032520325203252E-2,1.8619419046819186,1.5505024316512175,10.655116340171208,611.67320928640527,0,-495.4552995219882,0,0,0,0,0,1.7839531883753832,2.5378390568909825,21.407438260504598,60.908137365383581,38.775324544883873,10165.300320804654,8240.4207820704905,79272.847923518115,0.88537133069084861,27.287391060309954,-50316.177056653672,223.47909154984697,0.44411993902708907,9.6739432468148649,-50743.702236614015,327.30314034836385,13.926577079351015,0.87241508730682193,26.934851750485862,-50328.730264165337,225.24390380907246]
["Cart. DDR","CH132A (400 V)",361,12.4,315.60425215122842,12.045963822565971,200,836,200,1.66,29,1584,225,565,46,83.16719770134516,119.80790852095123,142.29797979797982,333.80615197247101,1.1111111111111112E-2,1.5075664911153634,1.3263277522699362,26.090839838962935,1108.8100008976667,0,-898.13610072711003,0,0,0,0,0,1.1155261444984872,1.5869395211370112,13.386313733981847,38.086548507288271,24.246649840976705,18427.138031737511,14937.814565107861,143701.77611633763,5.5263087275935305,130.78099985935009,-49100.966278914129,83.16719770134516,3.0540753289804687,55.583355544881428,-50497.32416317246,119.80790852095123,12.204524646426608,4.6602206296615041,110.42709142120093,-49590.147011076449,91.986306872956362]
["Cart. DDR","CH132A (480 V)",361,12.4,298.70199719486919,11.400839587590427,250,836,250,1.66,29,1584,225,679,46,83.16719770134516,120.39353858729615,142.29797979797982,330.99889198147599,1.1111111111111112E-2,1.56842495438711,1.3263277522699362,26.090839838962935,1108.8100008976667,0,-898.13610072711003,0,0,0,0,0,1.1155261444984872,1.5869395211370112,13.386313733981847,38.086548507288271,24.246649840976705,18427.138031737511,14937.814565107861,143701.77611633763,5.5263087275935305,130.78099985935009,-49100.966278914129,83.16719770134516,3.0323376178266126,54.463625584911583,-50509.601978192855,120.39353858729615,11.958663781068099,4.6602206296615041,110.42709142120093,-49590.147011076449,91.986306872956362]
["Cart. DDR","CH132B (400 V)",361,26.3,232.08417017957396,18.868631721916582,395,742,400,0.36899999999999999,6.5,746,225,565,46,203.43646858155745,273.18552784446752,302.14477211796248,271.84066071645407,1.1111111111111112E-2,1.824292593900658,1.4943531009402515,11.499314583195229,1108.8100008976667,0,-898.13610072711003,0,0,0,0,0,2.3659949677669529,3.3658475327341453,28.391939613203434,80.780340785619487,51.426362162716721,18427.138031737511,14937.814565107861,143701.77611633763,1.0936786261416498,25.773789240834859,-50506.746202449271,203.43646858155745,0.64239485078701142,10.305486310857656,-50757.451107486908,273.18552784446752,21.614374389530688,1.0426684654655554,24.519500853181647,-50535.084242030251,208.70809148114719]
["Cart. DDR","CH132B (480 V)",361,26.3,232.08417017957396,18.868631721916582,395,742,500,0.36899999999999999,6.5,746,225,679,46,203.43646858155745,273.18552784446752,302.14477211796248,271.84066071645407,1.1111111111111112E-2,1.824292593900658,1.4943531009402515,11.499314583195229,1108.8100008976667,0,-898.13610072711003,0,0,0,0,0,2.3659949677669529,3.3658475327341453,28.391939613203434,80.780340785619487,51.426362162716721,18427.138031737511,14937.814565107861,143701.77611633763,1.0936786261416498,25.773789240834859,-50506.746202449271,203.43646858155745,0.64239485078701142,10.305486310857656,-50757.451107486908,273.18552784446752,21.614374389530688,1.0426684654655554,24.519500853181647,-50535.084242030251,208.70809148114719]
["Cart. DDR","CH132C (400 V)",361.7,16.899999999999999,298.70199719486919,13.765068995155262,250,818.3,250,0.94,19.899999999999999,1313,225,565,46,99.175605603117617,147.06516101864608,171.66793602437167,324.64075429444131,1.1111111111111112E-2,1.5719954564003493,1.3550164987140005,22.101875648117968,1108.8100008976667,0,-898.13610072711003,0,0,0,0,0,1.5174118309976234,2.1586592267038252,18.20894197197148,51.807821440891807,32.98188349256084,18427.138031737511,14937.814565107861,143701.77611633763,4.2427001788958059,81.734225951781568,-49836.394945069071,99.175605603117617,2.1212405648169139,32.460618119550752,-50652.35972796737,147.06516101864608,15.184607776072557,3.5982350158472372,70.506419441572305,-50084.271865922339,108.58806909468638]
["Cart. DDR","CH132C (480 V)",361.7,16.899999999999999,279.15777018318443,12.864413372496978,300,818.3,300,1.1399999999999999,19.899999999999999,1313,225,679,46,96.832509542640537,145.62446211942597,171.66793602437167,321.63277393596064,1.1111111111111112E-2,1.6411956829498557,1.3550164987140005,22.578494883173082,1108.8100008976667,0,-898.13610072711003,0,0,0,0,0,1.5174118309976234,2.1586592267038252,18.20894197197148,51.807821440891807,32.98188349256084,18427.138031737511,14937.814565107861,143701.77611633763,4.2427001788958059,99.124486792586126,-49380.299129257321,96.832509542640537,2.116536825003978,39.133383018266329,-50583.082099171399,145.62446211942597,15.094446372908433,3.5982350158472372,85.5077852802047,-49744.876818642682,106.29583647706434]
["Cart. DDR","CH133A (400 V)",504,16.8,445.23595329957726,14.645919516433462,160,1016,160,1.41,26,1837,302,565,46,74.77853509571014,102.91979344856111,122.70005443658138,466.20010282119307,8.2781456953642391E-3,1.5425476802025124,1.460727893369125,30.759896043399802,1484.099539663031,0,-1202.1206271270551,0,0,0,0,0,1.4489383631209263,2.0612493606430986,17.387260357451115,49.469984655434367,31.493570370370371,24664.015519402525,19993.690264067445,192339.3003403288,6.7479529459279668,151.93623122948432,-49094.969872000001,74.77853509571014,4.0849134259876436,69.720894624982478,-50445.039704096445,102.91979344856111,15.540824455489474,6.2917586535079808,141.28979498133745,-49326.244754388761,78.023670711168464]
["Cart. DDR","CH133A (480 V)",504,16.8,424.94369805536053,13.978411120242123,200,1016,200,1.41,26,1837,302,679,46,74.77853509571014,103.01757610582676,122.70005443658138,463.2790569888644,8.2781456953642391E-3,1.6024781251311357,1.460727893369125,30.759896043399802,1484.099539663031,0,-1202.1206271270551,0,0,0,0,0,1.4489383631209263,2.0612493606430986,17.387260357451115,49.469984655434367,31.493570370370371,24664.015519402525,19993.690264067445,192339.3003403288,6.7479529459279668,151.93623122948432,-49094.969872000001,74.77853509571014,4.0794098389809541,69.45027862304029,-50447.829834220465,103.01757610582676,15.480504004874904,6.2917586535079808,141.28979498133745,-49326.244754388761,78.023670711168464]
["Cart. DDR","CH133B (400 V)",510,32.700000000000003,326.68646213599573,20.676358363037703,342,1017,350,0.37,7,954,302,565,46,155.90147926985603,212.0464548982649,236.26834381551362,396.34214666982177,8.2781456953642391E-3,1.9466095964168435,1.4592915827561761,14.813120127639099,1484.099539663031,0,-1202.1206271270551,0,0,0,0,0,2.7870755572973116,3.9648737701781962,33.444906687567737,95.156970484276712,60.578808888888894,24664.015519402525,19993.690264067445,192339.3003403288,1.8166149604095208,39.866605225854315,-50368.582076901708,155.90147926985603,1.0535835513247684,15.859972990818912,-50736.064757396452,212.0464548982649,25.941298871294389,1.6924851391729179,37.036629413221775,-50428.364097529244,162.01853352434196]
["Cart. DDR","CH133B (480 V)",510,32.700000000000003,326.68646213599573,20.676358363037703,342,1017,400,0.37,7,954,302,679,46,155.90147926985603,212.0464548982649,236.26834381551362,396.34214666982177,8.2781456953642391E-3,1.9466095964168435,1.4592915827561761,14.813120127639099,1484.099539663031,0,-1202.1206271270551,0,0,0,0,0,2.7870755572973116,3.9648737701781962,33.444906687567737,95.156970484276712,60.578808888888894,24664.015519402525,19993.690264067445,192339.3003403288,1.8166149604095208,39.866605225854315,-50368.582076901708,155.90147926985603,1.0535835513247684,15.859972990818912,-50736.064757396452,212.0464548982649,25.941298871294389,1.6924851391729179,37.036629413221775,-50428.364097529244,162.01853352434196]
["Cart. DDR","CH133C (400 V)",498.7,20,433.53806498232291,17.068427755209566,200,1072.5999999999999,200,0.94,18.100000000000001,1536,302,565,46,89.425778976902876,125.6924181061205,146.74479166666669,457.7481940957714,8.2781456953642391E-3,1.4836490456586826,1.3836467832025277,24.95754304428101,1484.099539663031,0,-1202.1206271270551,0,0,0,0,0,1.743258507865562,2.4799470952192886,20.919102094386744,59.518730285262926,37.890800525811557,24664.015519402525,19993.690264067445,192339.3003403288,4.9967698431443646,107.57419794181133,-49578.924709597275,89.425778976902876,2.837361048038169,45.799162098838977,-50582.89420027037,125.6924181061205,18.313773386541438,4.4057353718619297,94.757474536171543,-49853.713150974574,96.163312059275682]
["Cart. DDR","CH133C (480 V)",498.7,20,377.00622919608168,14.842764928979594,250,1072.5999999999999,250,0.94,18.100000000000001,1536,302,679,46,{"$f":"IF(AQ401<I401,IF(AQ401<0,0,AQ401),I401)","v":89.425778976902876},{"$f":"IF(AU401<I401,IF(AU401<0,0,AU401),I401)","v":126.74136481252448},{"$f":"IF(UAC_V*0.98/L401*1000<I401,IF(UAC_V*0.98/L401*1000<0,0,UAC_V*0.98/L401*1000),I401)","v":146.74479166666669},{"$f":"C401+(E401-C401)/G401*Q401","v":437.00546159651537},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M401,(inertia/gear^2+gear_inertia)/M401),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M401,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M401))","v":8.2781456953642391E-3},{"$f":"IF((C401+(E401-C401)/G401*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X401^2*time1+Y401^2*time2+Z401^2*time3+AA401^2*time4)/time)/(C401+(E401-C401)/G401*mspeed),SQRT((((X401-Y401)*2/PI()+Y401)^2*time1+Y401^2*time2+((Z401-Y401)*2/PI()+Y401)^2*time3+AA401^2*time4)/time)/(C401+(E401-C401)/G401*mspeed)),IF(AccType=1,SQRT((X401^2*time1+Y401^2*time2+Z401^2*time3+AA401^2*time4+AB401^2*time5+AC401^2*time6+AD401^2*time7+AE401^2*time8)/time)/(C401+(E401-C401)/G401*mspeed),SQRT((((X401-Y401)*2/PI()+Y401)^2*time1+Y401^2*time2+((Z401-Y401)*2/PI()+Y401)^2*time3+AA401^2*time4+((AB401-AC401)*2/PI()+AC401)^2*time5+AC401^2*time6+((AD401-AC401)*2/PI()+AC401)^2*time7+AE401^2*time8)/time)/(C401+(E401-C401)/G401*mspeed))))","v":1.8703204902721613},{"$f":"IF(move1,MAX(ABS(X401),ABS(Z401))/H401,MAX(ABS(X401),ABS(Z401),ABS(AB401),ABS(AD401))/H401)","v":1.3836467832025277},{"$f":"IF(AZ401>0,speed/(MIN(AZ401,I401)),\"NA\")","v":24.95754304428101},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M401+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M401+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":1484.099539663031},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M401+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M401+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-1202.1206271270551},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M401+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M401+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M401+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M401+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH401/Irms","v":1.743258507865562},{"$f":"AI401/Ipeak","v":2.4799470952192886},{"$f":"IF(move1,IF(AccType=1,SQRT((X401^2*time1+Y401^2*time2+Z401^2*time3+AA401^2*time4)/time)/(C401/D401),SQRT((((X401-Y401)*2/PI()+Y401)^2*time1+Y401^2*time2+((Z401-AA401)*2/PI()+AA401)^2*time3+AA401^2*time4)/time)/(C401/D401)),IF(AccType=1,SQRT((X401^2*time1+Y401^2*time2+Z401^2*time3+AA401^2*time4+AB401^2*time5+AC401^2*time6+AD401^2*time7+AE401^2*time8)/time)/(C401/D401),SQRT((((X401-Y401)*2/PI()+Y401)^2*time1+Y401^2*time2+((Z401-AA401)*2/PI()+AA401)^2*time3+AA401^2*time4+((AB401-AC401)*2/PI()+AC401)^2*time5+AC401^2*time6+((AD401-AE401)*2/PI()+AE401)^2*time7+AE401^2*time8)/time)/(C401/D401)))","v":20.919102094386744},{"$f":"IF(move1,MAX(ABS(X401),ABS(Z401))/(C401/D401),MAX(ABS(X401),ABS(Z401),ABS(AB401),ABS(AD401))/(C401/D401))","v":59.518730285262926},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X401),ABS(Z401))/(C401/D401),MAX(ABS((X401-Y401)*2/PI()+Y401),ABS((Z401-Y401)*2/PI()+Y401))/(C401/D401)),IF(AccType=1,MAX(ABS(X401),ABS(Z401),ABS(AB401),ABS(AD401))/(C401/D401),MAX(ABS((X401-Y401)*2/PI()+Y401),ABS((Z401-Y401)*2/PI()+Y401),ABS((AB401-AC401)*2/PI()+AC401),ABS((AD401-AC401)*2/PI()+AC401))/(C401/D401)))","v":37.890800525811557},{"$f":"IF((C401+(E401-C401)/G401*mspeed)<0,\"NA\",U401*(C401+(E401-C401)/G401*mspeed)*mspeed/9.55)","v":24664.015519402525},{"$f":"IF(move1,IF(speed1>speed2,AM401/2*time1/time,AM401/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z401*-speed/30*PI(),((Z401-AA401)*2/PI()+AA401)*-speed/30*PI()),IF(AccType=1,X401*-speed/30*PI(),((X401-Y401)*2/PI()+Y401)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z401*-speed/30*PI(),((Z401-AA401)*2/PI()+AA401)*-speed/30*PI()),IF(AccType=1,X401*-speed/30*PI(),((X401-Y401)*2/PI()+Y401)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD401*-speed/30*PI(),((AD401-AE401)*2/PI()+AE401)*-speed/30*PI()),IF(AccType=1,AB401*-speed/30*PI(),((AB401-AC401)*2/PI()+AC401)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD401*-speed/30*PI(),((AD401-AE401)*2/PI()+AE401)*-speed/30*PI()),IF(AccType=1,AB401*-speed/30*PI(),((AB401-AC401)*2/PI()+AC401)*-speed/30*PI()),0)/2*time7/time)))","v":19993.690264067445},{"$f":"IF(move1,MAX(IF(AccType=1,Z401*-speed/30*PI(),((Z401-AA401)*2/PI()+AA401)*-speed/30*PI()),IF(AccType=1,X401*-speed/30*PI(),((X401-Y401)*2/PI()+Y401)*-speed/30*PI()),0),MAX(IF(AccType=1,Z401*-speed/30*PI(),((Z401-AA401)*2/PI()+AA401)*-speed/30*PI()),IF(AccType=1,X401*-speed/30*PI(),((X401-Y401)*2/PI()+Y401)*-speed/30*PI()),IF(AccType=1,AD401*-speed/30*PI(),((AD401-AE401)*2/PI()+AE401)*-speed/30*PI()),IF(AccType=1,AB401*-speed/30*PI(),((AB401-AC401)*2/PI()+AC401)*-speed/30*PI()),0))","v":192339.3003403288},{"$f":"(L401^2)/1000000+((K401/1000)^2*(D401/C401*H401)^2*PI()*PI()*(O401/2)^2)/1200","v":4.9967698431443646},{"$f":"SQRT(3)*L401*J401*D401/C401*H401/1000","v":107.57419794181133},{"$f":"0.75*J401^2*(D401/C401*H401)^2-(UAC_V*0.98)^2","v":-49578.924709597275},{"$f":"-AO401/2/AN401+SQRT((AO401/2/AN401)^2-AP401/AN401)","v":89.425778976902876},{"$f":"(L401^2)/1000000+((K401/1000)^2*AV401^2*PI()*PI()*(O401/2)^2)/1200","v":2.8021713714064878},{"$f":"SQRT(3)*L401*J401*AV401/1000","v":44.081341318879083},{"$f":"0.75*J401^2*AV401^2-(UAC_V*0.98)^2","v":-50599.254864265495},{"$f":"-AS401/2/AR401+SQRT((AS401/2/AR401)^2-AT401/AR401)","v":126.74136481252448},{"$f":"D401+(F401-D401)*((0.85*UAC_V-D401*J401)/L401*1000)/G401","v":17.626866049350767},{"$f":"(L401^2)/1000000+((K401/1000)^2*AJ401^2*PI()*PI()*(O401/2)^2)/1200","v":4.4057353718619297},{"$f":"SQRT(3)*L401*J401*AJ401/1000","v":94.757474536171543},{"$f":"0.75*J401^2*AJ401^2-(UAC_V*0.98)^2","v":-49853.713150974574},{"$f":"IF(((AX401/2/AW401)^2-AY401/AW401)>0,-AX401/2/AW401+SQRT((AX401/2/AW401)^2-AY401/AW401),-9999)","v":96.163312059275682}]
["AKM2G","AKM2G-21D 120 V",0.63599997758865401,2.1700000762939502,0.58294791666666701,1.96941861200652,4800,1.7799999713897701,4800,7.3000001907348597,16.299999237060501,19.5,9.2999998742015998E-3,168,6,{"$f":"IF(AQ402<I402,IF(AQ402<0,0,AQ402),I402)","v":4800},{"$f":"IF(AU402<I402,IF(AU402<0,0,AU402),I402)","v":4800},{"$f":"IF(UAC_V*0.98/L402*1000<I402,IF(UAC_V*0.98/L402*1000<0,0,UAC_V*0.98/L402*1000),I402)","v":4800},{"$f":"C402+(E402-C402)/G402*Q402","v":0.58294791666666701},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M402,(inertia/gear^2+gear_inertia)/M402),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M402,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M402))","v":268.81720793728761},{"$f":"IF((C402+(E402-C402)/G402*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X402^2*time1+Y402^2*time2+Z402^2*time3+AA402^2*time4)/time)/(C402+(E402-C402)/G402*mspeed),SQRT((((X402-Y402)*2/PI()+Y402)^2*time1+Y402^2*time2+((Z402-Y402)*2/PI()+Y402)^2*time3+AA402^2*time4)/time)/(C402+(E402-C402)/G402*mspeed)),IF(AccType=1,SQRT((X402^2*time1+Y402^2*time2+Z402^2*time3+AA402^2*time4+AB402^2*time5+AC402^2*time6+AD402^2*time7+AE402^2*time8)/time)/(C402+(E402-C402)/G402*mspeed),SQRT((((X402-Y402)*2/PI()+Y402)^2*time1+Y402^2*time2+((Z402-Y402)*2/PI()+Y402)^2*time3+AA402^2*time4+((AB402-AC402)*2/PI()+AC402)^2*time5+AC402^2*time6+((AD402-AC402)*2/PI()+AC402)^2*time7+AE402^2*time8)/time)/(C402+(E402-C402)/G402*mspeed))))","v":6.812116555453815},{"$f":"IF(move1,MAX(ABS(X402),ABS(Z402))/H402,MAX(ABS(X402),ABS(Z402),ABS(AB402),ABS(AD402))/H402)","v":6.8708161003432142},{"$f":"IF(AZ402>0,speed/(MIN(AZ402,I402)),\"NA\")","v":2.2856056380738652},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M402+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M402+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.230052462035292},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M402+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M402+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-9.9063424942485856},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M402+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M402+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M402+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M402+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH402/Irms","v":1.2221910648528196},{"$f":"AI402/Ipeak","v":1.7386802745599821},{"$f":"IF(move1,IF(AccType=1,SQRT((X402^2*time1+Y402^2*time2+Z402^2*time3+AA402^2*time4)/time)/(C402/D402),SQRT((((X402-Y402)*2/PI()+Y402)^2*time1+Y402^2*time2+((Z402-AA402)*2/PI()+AA402)^2*time3+AA402^2*time4)/time)/(C402/D402)),IF(AccType=1,SQRT((X402^2*time1+Y402^2*time2+Z402^2*time3+AA402^2*time4+AB402^2*time5+AC402^2*time6+AD402^2*time7+AE402^2*time8)/time)/(C402/D402),SQRT((((X402-Y402)*2/PI()+Y402)^2*time1+Y402^2*time2+((Z402-AA402)*2/PI()+AA402)^2*time3+AA402^2*time4+((AB402-AC402)*2/PI()+AC402)^2*time5+AC402^2*time6+((AD402-AE402)*2/PI()+AE402)^2*time7+AE402^2*time8)/time)/(C402/D402)))","v":14.666292778233835},{"$f":"IF(move1,MAX(ABS(X402),ABS(Z402))/(C402/D402),MAX(ABS(X402),ABS(Z402),ABS(AB402),ABS(AD402))/(C402/D402))","v":41.728326589439568},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X402),ABS(Z402))/(C402/D402),MAX(ABS((X402-Y402)*2/PI()+Y402),ABS((Z402-Y402)*2/PI()+Y402))/(C402/D402)),IF(AccType=1,MAX(ABS(X402),ABS(Z402),ABS(AB402),ABS(AD402))/(C402/D402),MAX(ABS((X402-Y402)*2/PI()+Y402),ABS((Z402-Y402)*2/PI()+Y402),ABS((AB402-AC402)*2/PI()+AC402),ABS((AD402-AC402)*2/PI()+AC402))/(C402/D402)))","v":26.565077774649112},{"$f":"IF((C402+(E402-C402)/G402*mspeed)<0,\"NA\",U402*(C402+(E402-C402)/G402*mspeed)*mspeed/9.55)","v":203.24930751965204},{"$f":"IF(move1,IF(speed1>speed2,AM402/2*time1/time,AM402/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z402*-speed/30*PI(),((Z402-AA402)*2/PI()+AA402)*-speed/30*PI()),IF(AccType=1,X402*-speed/30*PI(),((X402-Y402)*2/PI()+Y402)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z402*-speed/30*PI(),((Z402-AA402)*2/PI()+AA402)*-speed/30*PI()),IF(AccType=1,X402*-speed/30*PI(),((X402-Y402)*2/PI()+Y402)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD402*-speed/30*PI(),((AD402-AE402)*2/PI()+AE402)*-speed/30*PI()),IF(AccType=1,AB402*-speed/30*PI(),((AB402-AC402)*2/PI()+AC402)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD402*-speed/30*PI(),((AD402-AE402)*2/PI()+AE402)*-speed/30*PI()),IF(AccType=1,AB402*-speed/30*PI(),((AB402-AC402)*2/PI()+AC402)*-speed/30*PI()),0)/2*time7/time)))","v":164.76245312679561},{"$f":"IF(move1,MAX(IF(AccType=1,Z402*-speed/30*PI(),((Z402-AA402)*2/PI()+AA402)*-speed/30*PI()),IF(AccType=1,X402*-speed/30*PI(),((X402-Y402)*2/PI()+Y402)*-speed/30*PI()),0),MAX(IF(AccType=1,Z402*-speed/30*PI(),((Z402-AA402)*2/PI()+AA402)*-speed/30*PI()),IF(AccType=1,X402*-speed/30*PI(),((X402-Y402)*2/PI()+Y402)*-speed/30*PI()),IF(AccType=1,AD402*-speed/30*PI(),((AD402-AE402)*2/PI()+AE402)*-speed/30*PI()),IF(AccType=1,AB402*-speed/30*PI(),((AB402-AC402)*2/PI()+AC402)*-speed/30*PI()),0))","v":1585.0147990797736},{"$f":"(L402^2)/1000000+((K402/1000)^2*(D402/C402*H402)^2*PI()*PI()*(O402/2)^2)/1200","v":1.1056565373826505E-3},{"$f":"SQRT(3)*L402*J402*D402/C402*H402/1000","v":1.4974100868367155},{"$f":"0.75*J402^2*(D402/C402*H402)^2-(UAC_V*0.98)^2","v":-49330.97395913193},{"$f":"-AO402/2/AN402+SQRT((AO402/2/AN402)^2-AP402/AN402)","v":6036.6665107754516},{"$f":"(L402^2)/1000000+((K402/1000)^2*AV402^2*PI()*PI()*(O402/2)^2)/1200","v":4.4291301353685661E-4},{"$f":"SQRT(3)*L402*J402*AV402/1000","v":0.44010434893655426},{"$f":"0.75*J402^2*AV402^2-(UAC_V*0.98)^2","v":-50677.814938887008},{"$f":"-AS402/2/AR402+SQRT((AS402/2/AR402)^2-AT402/AR402)","v":10211.400216156302},{"$f":"D402+(F402-D402)*((0.85*UAC_V-D402*J402)/L402*1000)/G402","v":1.7849972440537492},{"$f":"(L402^2)/1000000+((K402/1000)^2*AJ402^2*PI()*PI()*(O402/2)^2)/1200","v":1.4259255900464273E-2},{"$f":"SQRT(3)*L402*J402*AJ402/1000","v":6.5498175402834562},{"$f":"0.75*J402^2*AJ402^2-(UAC_V*0.98)^2","v":-22599.959598287434},{"$f":"IF(((AX402/2/AW402)^2-AY402/AW402)>0,-AX402/2/AW402+SQRT((AX402/2/AW402)^2-AY402/AW402),-9999)","v":1050.0499123823206}]
["AKM2G","AKM2G-21D 240 V",0.63599997758865401,2.1700000762939502,0.53480000000000005,1.8067567334721999,8000,1.7799999713897701,8000,7.3000001907348597,16.299999237060501,19.5,9.2999998742015998E-3,336,6,6036.6665107754516,8000,8000,0.53480000000000005,268.81720793728761,6.8199129642001797,6.8708161003432142,2.2856056380738652,12.230052462035292,0,-9.9063424942485856,0,0,0,0,0,1.2221910648528196,1.7386802745599821,14.666292778233835,41.728326589439568,26.565077774649112,203.24930751965204,164.76245312679561,1585.0147990797736,1.1056565373826505E-3,1.4974100868367155,-49330.97395913193,6036.6665107754516,4.4059473041680065E-4,0.43188656808880338,-50682.526201383618,10246.37568799926,1.7516671572211202,1.4259255900464273E-2,6.5498175402834562,-22599.959598287434,1050.0499123823206]
["AKM2G","AKM2G-21D 400 V",0.63599997758865401,2.1700000762939502,0.52405625,1.7704602812372601,8000,1.7799999713897701,8000,7.3000001907348597,16.299999237060501,19.5,9.2999998742015998E-3,560,6,6036.6665107754516,8000,8000,0.52405625,268.81720793728761,6.8264810477859079,6.8708161003432142,2.2856056380738652,12.230052462035292,0,-9.9063424942485856,0,0,0,0,0,1.2221910648528196,1.7386802745599821,14.666292778233835,41.728326589439568,26.565077774649112,203.24930751965204,164.76245312679561,1585.0147990797736,1.1056565373826505E-3,1.4974100868367155,-49330.97395913193,6036.6665107754516,4.3774900348135781E-4,0.4215801758939231,-50688.309346017915,10289.95653186484,1.7098659759593318,1.4259255900464273E-2,6.5498175402834562,-22599.959598287434,1050.0499123823206]
["AKM2G","AKM2G-21D 480 V",0.63599997758865401,2.1700000762939502,0.51928125000000003,1.7543285246883999,8000,1.7799999713897701,8000,7.3000001907348597,16.299999237060501,19.5,9.2999998742015998E-3,672,6,6036.6665107754516,8000,8000,0.51928125000000003,268.81720793728761,6.8294042586340948,6.8708161003432142,2.2856056380738652,12.230052462035292,0,-9.9063424942485856,0,0,0,0,0,1.2221910648528196,1.7386802745599821,14.666292778233835,41.728326589439568,26.565077774649112,203.24930751965204,164.76245312679561,1585.0147990797736,1.1056565373826505E-3,1.4974100868367155,-49330.97395913193,6036.6665107754516,4.3650629728043608E-4,0.41699955714064357,-50690.83479904307,10309.219779691666,1.6912876731763169,1.4259255900464273E-2,6.5498175402834562,-22599.959598287434,1050.0499123823206]
["AKM2G","AKM2G-21E 120 V",0.64200001955032304,2.7300000190734899,0.56837903225806496,2.3881471393376299,6200,1.78999996185303,6200,4.6300001144409197,10.5,15.6000003814697,9.2999998742015998E-3,168,6,6200,6200,6200,0.56837903225806496,268.81720793728761,6.7518861870721825,6.8324316886434966,1.4216256348418328,12.230052462035292,0,-9.9063424942485856,0,0,0,0,0,1.5232250189508527,2.1669290263425642,18.278700227410233,52.006296632221542,33.108236723685792,203.24930751965204,164.76245312679561,1585.0147990797736,7.1618548734715356E-4,0.95224098229650755,-49873.656420921128,7706.5711642034685,2.787927893674748E-4,0.26067479036914454,-50735.354626262801,13030.673834549338,2.0836885001715455,9.1890060585877852E-3,4.1419255645593278,-33181.529839605355,1688.2081619659448]
["AKM2G","AKM2G-21E 240 V",0.64200001955032304,2.7300000190734899,0.53480000000000005,2.2470587717561599,8000,1.78999996185303,8000,4.6300001144409197,10.5,15.6000003814697,9.2999998742015998E-3,336,6,7706.5711642034685,8000,8000,0.53480000000000005,268.81720793728761,6.7592004791512021,6.8324316886434966,1.4216256348418328,12.230052462035292,0,-9.9063424942485856,0,0,0,0,0,1.5232250189508527,2.1669290263425642,18.278700227410233,52.006296632221542,33.108236723685792,203.24930751965204,164.76245312679561,1585.0147990797736,7.1618548734715356E-4,0.95224098229650755,-49873.656420921128,7706.5711642034685,2.7673846063254058E-4,0.2530052359918894,-50739.401816333077,13091.19410971355,2.0223823714327591,9.1890060585877852E-3,4.1419255645593278,-33181.529839605355,1688.2081619659448]
["AKM2G","AKM2G-21G 120 V",0.64899998903274503,4.1799998283386204,0.54435,3.4671973363938,8000,1.78999996185303,8000,1.9700000286102299,4.5500001907348597,10.300000190734901,9.2999998742015998E-3,168,6,8000,8000,8000,0.54435,268.81720793728761,6.6841147782115042,6.8324316886434966,0.77447874632655311,12.230052462035292,0,-9.9063424942485856,0,0,0,0,0,2.3071085575339936,3.2820761463641901,27.685302690407923,78.769827512740562,50.146429660594542,203.24930751965204,164.76245312679561,1585.0147990797736,3.0977218221492857E-4,0.40518064250790664,-50418.291899842385,12120.467977552613,1.1613346278026359E-4,8.9973336457946779E-2,-50786.08374169677,20528.125792132683,2.5600575776224401,3.959665514526701E-3,1.7623984817590088,-43485.788962505532,3098.8584404459025]
["AKM2G","AKM2G-22C 120 V",1.1100000143051101,1.6499999761581401,1.0929444444444401,1.6167817248318499,1800,3.3299999237060498,1800,14.699999809265099,37.900001525878899,44.200000762939503,1.5499999790336E-2,168,6,1800,1800,1800,1.0929444444444401,161.29032476237256,3.8971196733181976,3.6817630213899601,2.4177745162265145,12.260270580332323,0,-9.9308191700691797,0,0,0,0,0,0.53378841535579469,0.75936358500502876,6.4054609842695358,18.224726040120689,11.602220943123166,203.7514976482295,165.16954960614018,1588.9310672110687,4.5588925469898251E-3,5.5706440679239924,-46834.101583377334,2651.9189297266507,2.2185688725224165E-3,1.7764177001319814,-50401.34203246222,4382.7675550802942,1.5785009895784767,1.6266345288133716E-2,13.056938690744671,-28989.006296093026,992.64839789350754]
["AKM2G","AKM2G-22C 240 V",1.1100000143051101,1.6499999761581401,1.04181818181818,1.54115115870997,4400,3.3299999237060498,4400,14.699999809265099,37.900001525878899,44.200000762939503,1.5499999790336E-2,336,6,2651.9189297266507,4396.3909259136526,4400,1.0418741075647229,161.29032476237256,3.9067251383298149,3.6817630213899601,2.4177745162265145,12.260270580332323,0,-9.9308191700691797,0,0,0,0,0,0.53378841535579469,0.75936358500502876,6.4054609842695358,18.224726040120689,11.602220943123166,203.7514976482295,165.16954960614018,1588.9310672110687,4.5588925469898251E-3,5.5706440679239924,-46834.101583377334,2651.9189297266507,2.2104598390671809E-3,1.749019812904153,-50413.70223394208,4396.3909259136526,1.5541555937302629,1.6266345288133716E-2,13.056938690744671,-28989.006296093026,992.64839789350754]
["AKM2G","AKM2G-22C 400 V",1.1100000143051101,1.6499999761581401,0.95622435897435898,1.41453307740142,7800,3.3299999237060498,7800,14.699999809265099,37.900001525878899,44.200000762939503,1.5499999790336E-2,560,6,2651.9189297266507,4408.1763881357074,5099.5474232885481,1.023093576753942,161.29032476237256,3.913484518004593,3.6817630213899601,2.4177745162265145,12.260270580332323,0,-9.9308191700691797,0,0,0,0,0,0.53378841535579469,0.75936358500502876,6.4054609842695358,18.224726040120689,11.602220943123166,203.7514976482295,165.16954960614018,1588.9310672110687,4.5588925469898251E-3,5.5706440679239924,-46834.101583377334,2651.9189297266507,2.2035292239756762E-3,1.7252586242775778,-50424.266230179514,4408.1763881357074,1.5330417195790298,1.6266345288133716E-2,13.056938690744671,-28989.006296093026,992.64839789350754]
["AKM2G","AKM2G-22C 480 V",1.1100000143051101,1.6499999761581401,0.94425625000000002,1.3968287741599399,8000,3.3299999237060498,8000,14.699999809265099,37.900001525878899,44.200000762939503,1.5499999790336E-2,672,6,2651.9189297266507,4411.325339638649,5099.5474232885481,1.0186063058843315,161.29032476237256,3.9150951416316664,3.6817630213899601,2.4177745162265145,12.260270580332323,0,-9.9308191700691797,0,0,0,0,0,0.53378841535579469,0.75936358500502876,6.4054609842695358,18.224726040120689,11.602220943123166,203.7514976482295,165.16954960614018,1588.9310672110687,4.5588925469898251E-3,5.5706440679239924,-46834.101583377334,2651.9189297266507,2.2016906728713169E-3,1.7189001408150115,-50427.068643340877,4411.325339638649,1.5273916562875338,1.6266345288133716E-2,13.056938690744671,-28989.006296093026,992.64839789350754]
["AKM2G","AKM2G-22D 120 V",1.1100000143051101,2.3699998855590798,1.07355172413793,2.27447397803095,2900,3.3299999237060498,2900,7.1100001335143999,18.5,30.899999618530298,1.5499999790336E-2,168,6,2900,2900,2900,1.07355172413793,161.29032476237256,3.9020485729212004,3.6817630213899601,1.2745223191127888,12.260270580332323,0,-9.9308191700691797,0,0,0,0,0,0.76671424338538763,1.0907222033724222,9.2005709206246511,26.177332880938135,16.665007699853238,203.7514976482295,165.16954960614018,1588.9310672110687,2.2354987248258038E-3,2.7055668838506168,-48888.524139533896,4110.3024487437651,1.0751584833211447E-3,0.82938624937680372,-50625.0504578818,6487.0606297162449,2.1795564443142927,7.9906426564527698E-3,6.3415325939701761,-40275.568606602545,1883.0584321745505]
["AKM2G","AKM2G-22D 240 V",1.1100000143051101,2.3699998855590798,0.99117424242424301,2.0999454161361202,6600,3.3299999237060498,6600,7.1100001335143999,18.5,30.899999618530298,1.5499999790336E-2,336,6,4110.3024487437651,6509.71460140405,6600,0.99279973214814232,161.29032476237256,3.9107405544378251,3.6817630213899601,1.2745223191127888,12.260270580332323,0,-9.9308191700691797,0,0,0,0,0,0.76671424338538763,1.0907222033724222,9.2005709206246511,26.177332880938135,16.665007699853238,203.7514976482295,165.16954960614018,1588.9310672110687,2.2354987248258038E-3,2.7055668838506168,-48888.524139533896,4110.3024487437651,1.07011900064831E-3,0.81183566408165508,-50632.592378759153,6509.71460140405,2.1334350005234515,7.9906426564527698E-3,6.3415325939701761,-40275.568606602545,1883.0584321745505]
["AKM2G","AKM2G-22D 400 V",1.1100000143051101,2.3699998855590798,0.93828750000000005,1.98789723371309,8000,3.3299999237060498,8000,7.1100001335143999,18.5,30.899999618530298,1.5499999790336E-2,560,6,4110.3024487437651,6529.0411841574123,7294.498471929779,0.96986025458844982,161.29032476237256,3.9162939128514189,3.6817630213899601,1.2745223191127888,12.260270580332323,0,-9.9308191700691797,0,0,0,0,0,0.76671424338538763,1.0907222033724222,9.2005709206246511,26.177332880938135,16.665007699853238,203.7514976482295,165.16954960614018,1588.9310672110687,2.2354987248258038E-3,2.7055668838506168,-48888.524139533896,4110.3024487437651,1.0658804828495112E-3,0.79677528351924731,-50638.935602449179,6529.0411841574123,2.0938576027389018,7.9906426564527698E-3,6.3415325939701761,-40275.568606602545,1883.0584321745505]
["AKM2G","AKM2G-22D 480 V",1.1100000143051101,2.3699998855590798,0.92754375,1.96513505164768,8000,3.3299999237060498,8000,7.1100001335143999,18.5,30.899999618530298,1.5499999790336E-2,672,6,4110.3024487437651,6537.0423719076261,7294.498471929779,0.96090947295729989,161.29032476237256,3.9184535520207127,3.6817630213899601,1.2745223191127888,12.260270580332323,0,-9.9308191700691797,0,0,0,0,0,0.76671424338538763,1.0907222033724222,9.2005709206246511,26.177332880938135,16.665007699853238,203.7514976482295,165.16954960614018,1588.9310672110687,2.2354987248258038E-3,2.7055668838506168,-48888.524139533896,4110.3024487437651,1.0641421256651364E-3,0.79051555552532049,-50641.537169552837,6537.0423719076261,2.0774075705626154,7.9906426564527698E-3,6.3415325939701761,-40275.568606602545,1883.0584321745505]
["AKM2G","AKM2G-22E 120 V",1.1100000143051101,2.9300000667571999,1.06055263157895,2.7618557873965099,3800,3.3399999141693102,3800,4.6900000572204599,12.199999809265099,25.100000381469702,1.5499999790336E-2,168,6,3800,3800,3800,1.06055263157895,161.29032476237256,3.9027572749281227,3.6707397890402547,0.95832637753331595,12.260270580332323,0,-9.9308191700691797,0,0,0,0,0,0.94787885771266278,1.3484456890346512,11.374546292551953,32.362696536831628,20.602732502478865,203.7514976482295,165.16954960614018,1588.9310672110687,1.4863828087891635E-3,1.7976217121721001,-49522.861416703861,5199.0401018194516,7.0503779202474076E-4,0.53208118580150343,-50692.816394470523,8110.4864430215921,2.6095805047314728,5.3066108694051857E-3,4.2008002132121085,-43802.603733062468,2504.3660033416586]
["AKM2G","AKM2G-22E 240 V",1.1100000143051101,2.9300000667571999,0.95499999999999996,2.48697914504899,8000,3.3399999141693102,8000,4.6900000572204599,12.199999809265099,25.100000381469702,1.5499999790336E-2,336,6,5199.0401018194516,8000,8000,0.95499999999999996,161.29032476237256,3.9129392018050178,3.6707397890402547,0.95832637753331595,12.260270580332323,0,-9.9308191700691797,0,0,0,0,0,0.94787885771266278,1.3484456890346512,11.374546292551953,32.362696536831628,20.602732502478865,203.7514976482295,165.16954960614018,1588.9310672110687,1.4863828087891635E-3,1.7976217121721001,-49522.861416703861,5199.0401018194516,7.0047527614787691E-4,0.5156492557819915,-50699.648124431995,8147.4678766485058,2.5289904643799481,5.3066108694051857E-3,4.2008002132121085,-43802.603733062468,2504.3660033416586]
["AKM2G","AKM2G-23D 120 V",1.4800000190734901,2.1099998950958301,1.44841666666667,2.0400235358321499,1800,4.6900000572204599,1800,9.6000003814697301,26.5,46.099998474121101,2.1699999706470401E-2,168,6,1800,1800,1800,1.44841666666667,115.2073748302661,2.9344590863593654,2.6205732513174729,1.3530559074712203,12.290488698629353,0,-9.9552958458897756,0,0,0,0,0,0.51321341517401786,0.73009373678417688,6.1585609820882148,17.522249682820245,11.155010604444948,204.25368777680694,165.57664608548484,1592.8473353423642,4.4492299499220168E-3,5.1253832987660362,-47714.929422988913,2749.0816407158845,2.3253560318270612E-3,1.5041115804812475,-50539.027265317025,4349.7511921617333,1.9622180497976007,8.5935482454943726E-3,8.5507217876562827,-42204.263155687666,1773.762626324477]
["AKM2G","AKM2G-23D 240 V",1.4800000190734901,2.1099998950958301,1.36587209302326,1.92376356944048,4300,4.6900000572204599,4300,9.6000003814697301,26.5,46.099998474121101,2.1699999706470401E-2,336,6,2749.0816407158845,4300,4300,1.36587209302326,115.2073748302661,2.9425783550562965,2.6205732513174729,1.3530559074712203,12.290488698629353,0,-9.9552958458897756,0,0,0,0,0,0.51321341517401786,0.73009373678417688,6.1585609820882148,17.522249682820245,11.155010604444948,204.25368777680694,165.57664608548484,1592.8473353423642,4.4492299499220168E-3,5.1253832987660362,-47714.929422988913,2749.0816407158845,2.3219315257075792E-3,1.4911883690968499,-50543.580803199227,4355.5361874154696,1.9453588227502956,8.5935482454943726E-3,8.5507217876562827,-42204.263155687666,1773.762626324477]
["AKM2G","AKM2G-23D 400 V",1.4800000190734901,2.1099998950958301,1.2276776315789499,1.72912347701678,7600,4.6900000572204599,7600,9.6000003814697301,26.5,46.099998474121101,2.1699999706470401E-2,560,6,2749.0816407158845,4364.3884198892974,4889.3710945897656,1.3351009524866491,115.2073748302661,2.9486179469300975,2.6205732513174729,1.3530559074712203,12.290488698629353,0,-9.9552958458897756,0,0,0,0,0,0.51321341517401786,0.73009373678417688,6.1585609820882148,17.522249682820245,11.155010604444948,204.25368777680694,165.57664608548484,1592.8473353423642,4.4492299499220168E-3,5.1253832987660362,-47714.929422988913,2749.0816407158845,2.316734835519836E-3,1.4713605882131018,-50550.490799796215,4364.3884198892974,1.9194921051194971,8.5935482454943726E-3,8.5507217876562827,-42204.263155687666,1773.762626324477]
["AKM2G","AKM2G-23D 480 V",1.4800000190734901,2.1099998950958301,1.1937500000000001,1.6813380789825401,8000,4.6900000572204599,8000,9.6000003814697301,26.5,46.099998474121101,2.1699999706470401E-2,672,6,2749.0816407158845,4368.8881055949623,4889.3710945897656,1.3236757311289273,115.2073748302661,2.950965505632821,2.6205732513174729,1.3530559074712203,12.290488698629353,0,-9.9552958458897756,0,0,0,0,0,0.51321341517401786,0.73009373678417688,6.1585609820882148,17.522249682820245,11.155010604444948,204.25368777680694,165.57664608548484,1592.8473353423642,4.4492299499220168E-3,5.1253832987660362,-47714.929422988913,2749.0816407158845,2.3141134995472725E-3,1.4612568964520345,-50553.976368878757,4368.8881055949623,1.906311137297406,8.5935482454943726E-3,8.5507217876562827,-42204.263155687666,1773.762626324477]
["AKM2G","AKM2G-23E 120 V",1.4800000190734901,2.9200000762939502,1.4188571428571399,2.77120522551767,2800,4.6900000572204599,2800,4.9899997711181596,13.800000190734901,33.299999237060497,2.1699999706470401E-2,168,6,2800,2800,2800,1.4188571428571399,115.2073748302661,2.9383261877890021,2.6205732513174729,0.86897581238027111,12.290488698629353,0,-9.9552958458897756,0,0,0,0,0,0.71022904548303301,1.0103667645038952,8.5227485457963965,24.248802348093484,15.437267031029746,204.25368777680694,165.57664608548484,1592.8473353423642,2.3158896799516469E-3,2.6631729219113454,-49206.153259702216,4070.2118757567287,1.2064898824037428E-3,0.75730450454487319,-50675.861751552584,6174.6993799176653,2.6312684806840552,4.4682768676394197E-3,4.4429946796693409,-46354.717975067542,2761.8720404035134]
["AKM2G","AKM2G-23E 240 V",1.4800000190734901,2.9200000762939502,1.2923306451612899,2.52408317144313,6200,4.6900000572204599,6200,4.9899997711181596,13.800000190734901,33.299999237060497,2.1699999706470401E-2,336,6,4070.2118757567287,6192.1263040577742,6200,1.2925689760625565,115.2073748302661,2.9459564511036596,2.6205732513174729,0.86897581238027111,12.290488698629353,0,-9.9552958458897756,0,0,0,0,0,0.71022904548303301,1.0103667645038952,8.5227485457963965,24.248802348093484,15.437267031029746,204.25368777680694,165.57664608548484,1592.8473353423642,2.3158896799516469E-3,2.6631729219113454,-49206.153259702216,4070.2118757567287,1.2022181727627498E-3,0.74054640768286395,-50681.520818687772,6192.1263040577742,2.5730421637869232,4.4682768676394197E-3,4.4429946796693409,-46354.717975067542,2761.8720404035134]
["AKM2G","AKM2G-23E 400 V",1.4800000190734901,2.9200000762939502,1.18539375,2.3152220580015999,8000,4.6900000572204599,8000,4.9899997711181596,13.800000190734901,33.299999237060497,2.1699999706470401E-2,560,6,4070.2118757567287,6211.0613208184977,6768.7689238486855,1.2512728187343649,115.2073748302661,2.9519166487556872,2.6205732513174729,0.86897581238027111,12.290488698629353,0,-9.9552958458897756,0,0,0,0,0,0.71022904548303301,1.0103667645038952,8.5227485457963965,24.248802348093484,15.437267031029746,204.25368777680694,165.57664608548484,1592.8473353423642,2.3158896799516469E-3,2.6631729219113454,-49206.153259702216,4070.2118757567287,1.1976483394328863E-3,0.72218836673349729,-50687.574833539838,6211.0613208184977,2.5092568116237191,4.4682768676394197E-3,4.4429946796693409,-46354.717975067542,2761.8720404035134]
["AKM2G","AKM2G-23E 480 V",1.4800000190734901,2.9200000762939502,1.1674875,2.28024891513149,8000,4.6900000572204599,8000,4.9899997711181596,13.800000190734901,33.299999237060497,2.1699999706470401E-2,672,6,4070.2118757567287,6218.0697046999867,6768.7689238486855,1.237096940674697,115.2073748302661,2.953956878662781,2.6205732513174729,0.86897581238027111,12.290488698629353,0,-9.9552958458897756,0,0,0,0,0,0.71022904548303301,1.0103667645038952,8.5227485457963965,24.248802348093484,15.437267031029746,204.25368777680694,165.57664608548484,1592.8473353423642,2.3158896799516469E-3,2.6631729219113454,-49206.153259702216,4070.2118757567287,1.1959759283673098E-3,0.71535217095595582,-50689.790406997105,6218.0697046999867,2.4855043232002667,4.4682768676394197E-3,4.4429946796693409,-46354.717975067542,2761.8720404035134]
["AKM2G","AKM2G-23F 120 V",1.5,4.0700001716613796,1.3952317073170699,3.7405676205845202,4100,5.9299998283386204,4100,2.5699999332428001,7.3200001716613796,24.200000762939499,2.1699999706470401E-2,168,6,4100,4100,4100,1.3952317073170699,115.2073748302661,2.9021577546774324,2.0725951187881773,0.59001101655571508,12.290488698629353,0,-9.9552958458897756,0,0,0,0,0,0.9767433338279915,1.3895080864784364,11.720920005935898,33.348194075482475,21.230119721203579,204.25368777680694,165.57664608548484,1592.8473353423642,1.6124708437304527E-3,1.7332729860240028,-49522.701896619525,5030.410751643818,6.3300275240133527E-4,0.37225095491456928,-50746.006439494602,8664.4001692075071,3.455625748995649,2.3733130242287819E-3,2.2869757645096804,-48572.449709688561,4067.7206571673678]
["AKM2G","AKM2G-23F 240 V",1.5,4.0700001716613796,1.217625,3.2644102231395,8000,5.9299998283386204,8000,2.5699999332428001,7.3200001716613796,24.200000762939499,2.1699999706470401E-2,336,6,5030.410751643818,8000,8000,1.217625,115.2073748302661,2.9107618420613401,2.0725951187881773,0.59001101655571508,12.290488698629353,0,-9.9552958458897756,0,0,0,0,0,0.9767433338279915,1.3895080864784364,11.720920005935898,33.348194075482475,21.230119721203579,204.25368777680694,165.57664608548484,1592.8473353423642,1.6124708437304527E-3,1.7332729860240028,-49522.701896619525,5030.410751643818,6.2883356466255898E-4,0.35548956843604279,-50751.213537455318,8705.490109413191,3.3000288917159781,2.3733130242287819E-3,2.2869757645096804,-48572.449709688561,4067.7206571673678]
["AKM2G","AKM2G-24D 120 V",1.79999995231628,2.1099998950958301,1.7635666666666701,2.0435303781722598,1500,5.9299998283386204,1500,9.8400001525878906,28.399999618530298,55.700000762939503,2.7899999622604799E-2,168,6,1500,1500,1500,1.7635666666666701,89.605735979095869,2.4205099557778316,2.0776909230329972,1.6,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.42301298507398072,0.60177524953468353,5.0761558208877684,14.442605988832405,9.1944485370051527,204.75587790538441,165.98374256482944,1596.7636034736593,5.9873645458768075E-3,6.5989608916247935,-47296.181433085956,2313.0166249269951,3.334423947796295E-3,1.8710878368132871,-50523.050339923502,3622.0787375518021,1.9709846497516434,8.1496730645443348E-3,8.7284397805755756,-44666.08631111955,1866.0514685342639]
["AKM2G","AKM2G-24D 240 V",1.79999995231628,2.1099998950958301,1.6685972222222201,1.93348466887839,3600,5.9299998283386204,3600,9.8400001525878906,28.399999618530298,55.700000762939503,2.7899999622604799E-2,336,6,2313.0166249269951,3600,3600,1.6685972222222201,89.605735979095869,2.4279938472147307,2.0776909230329972,1.2861381588178482,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.42301298507398072,0.60177524953468353,5.0761558208877684,14.442605988832405,9.1944485370051527,204.75587790538441,165.98374256482944,1596.7636034736593,5.9873645458768075E-3,6.5989608916247935,-47296.181433085956,2313.0166249269951,3.3309529236985394E-3,1.8570341034367817,-50527.272273782117,3625.9504328259191,1.9561805918064157,8.1496730645443348E-3,8.7284397805755756,-44666.08631111955,1866.0514685342639]
["AKM2G","AKM2G-24D 400 V",1.79999995231628,2.1099998950958301,1.5143571428571401,1.75475919528458,6300,5.9299998283386204,6300,9.8400001525878906,28.399999618530298,55.700000762939503,2.7899999622604799E-2,560,6,2313.0166249269951,3631.9718871285754,4046.6785801190131,1.6353258802978641,89.605735979095869,2.4334398675628299,2.0776909230329972,1.2861381588178482,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.42301298507398072,0.60177524953468353,5.0761558208877684,14.442605988832405,9.1944485370051527,204.75587790538441,165.98374256482944,1596.7636034736593,5.9873645458768075E-3,6.5989608916247935,-47296.181433085956,2313.0166249269951,3.3255948907262153E-3,1.835128828212292,-50533.789445713039,3631.9718871285754,1.9331058005718218,8.1496730645443348E-3,8.7284397805755756,-44666.08631111955,1866.0514685342639]
["AKM2G","AKM2G-24D 480 V",1.79999995231628,2.1099998950958301,1.41993421052632,1.6453467561286199,7600,5.9299998283386204,7600,9.8400001525878906,28.399999618530298,55.700000762939503,2.7899999622604799E-2,672,6,2313.0166249269951,3635.8526629463495,4046.6785801190131,1.6181758681871081,89.605735979095869,2.4363260591437177,2.0776909230329972,1.2861381588178482,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.42301298507398072,0.60177524953468353,5.0761558208877684,14.442605988832405,9.1944485370051527,204.75587790538441,165.98374256482944,1596.7636034736593,5.9873645458768075E-3,6.5989608916247935,-47296.181433085956,2313.0166249269951,3.3221677144785293E-3,1.8209793118220325,-50537.95804582414,3635.8526629463495,1.9182008457867443,8.1496730645443348E-3,8.7284397805755756,-44666.08631111955,1866.0514685342639]
["AKM2G","AKM2G-24E 120 V",1.8099999427795399,2.9200000762939502,1.73976086956522,2.7747383429226899,2300,5.9499998092651403,2300,5.1500000953674299,15,40.5,2.7899999622604799E-2,168,6,2300,2300,2300,1.73976086956522,89.605735979095869,2.4108373973176125,2.0707070944340185,1.0434782608695652,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.58216763885996525,0.82818752262345618,6.986011666319583,19.876500542962948,12.65377325112518,204.75587790538441,165.98374256482944,1596.7636034736593,3.1748176328809776E-3,3.4677209412160699,-48972.346629149761,3419.1582495364046,1.756203606699251E-3,0.95322023961916547,-50666.670619536715,5106.6950884737962,2.6385806148863544,4.3070080983822435E-3,4.571333808212505,-47620.11308853732,2836.5169206102651]
["AKM2G","AKM2G-24E 240 V",1.8099999427795399,2.9200000762939502,1.59728431372549,2.5475029973232401,5100,5.9499998092651403,5100,5.1500000953674299,15,40.5,2.7899999622604799E-2,336,6,3419.1582495364046,5100,5100,1.59728431372549,89.605735979095869,2.4176264403112242,2.0707070944340185,0.84610812033641947,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.58216763885996525,0.82818752262345618,6.986011666319583,19.876500542962948,12.65377325112518,204.75587790538441,165.98374256482944,1596.7636034736593,3.1748176328809776E-3,3.4677209412160699,-48972.346629149761,3419.1582495364046,1.7523660663456499E-3,0.93731388417292549,-50671.253992156177,5116.5554246031088,2.5945507051241479,4.3070080983822435E-3,4.571333808212505,-47620.11308853732,2836.5169206102651]
["AKM2G","AKM2G-24E 400 V",1.8099999427795399,2.9200000762939502,1.3847499999999999,2.2085327860733099,8000,5.9499998092651403,8000,5.1500000953674299,15,40.5,2.7899999622604799E-2,560,6,3419.1582495364046,5132.3016077683715,5565.4320987654328,1.5371860721506847,89.605735979095869,2.4246236709460538,2.0707070944340185,0.84610812033641947,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.58216763885996525,0.82818752262345618,6.986011666319583,19.876500542962948,12.65377325112518,204.75587790538441,165.98374256482944,1596.7636034736593,3.1748176328809776E-3,3.4677209412160699,-48972.346629149761,3419.1582495364046,1.7463286346599408E-3,0.91172756390530951,-50678.464808598583,5132.3016077683715,2.5237259724355323,4.3070080983822435E-3,4.571333808212505,-47620.11308853732,2836.5169206102651]
["AKM2G","AKM2G-24E 480 V",1.8099999427795399,2.9200000762939502,1.3608750000000001,2.1704546345892899,8000,5.9499998092651403,8000,5.1500000953674299,15,40.5,2.7899999622604799E-2,672,6,3419.1582495364046,5136.9887790784333,5565.4320987654328,1.5216062188466974,89.605735979095869,2.4264545499089216,2.0707070944340185,0.84610812033641947,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.58216763885996525,0.82818752262345618,6.986011666319583,19.876500542962948,12.65377325112518,204.75587790538441,165.98374256482944,1596.7636034736593,3.1748176328809776E-3,3.4677209412160699,-48972.346629149761,3419.1582495364046,1.7445532043487166E-3,0.90406561062847601,-50680.585296704616,5136.9887790784333,2.502517147288791,4.3070080983822435E-3,4.571333808212505,-47620.11308853732,2836.5169206102651]
["AKM2G","AKM2G-24F 120 V",1.83000004291534,4.1100001335143999,1.71338235294118,3.79907391113084,3400,6,3400,2.5799999237060498,7.75,29.100000381469702,2.7899999622604799E-2,168,6,3400,3400,3400,1.71338235294118,89.605735979095869,2.386520624644406,2.0534511361543974,0.70588235294117652,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.81046542991640669,1.1529623286667743,9.7255851589968803,27.671095888002583,17.615966765381721,204.75587790538441,165.98374256482944,1596.7636034736593,1.6541349951399347E-3,1.7523276010195468,-49898.624903346376,4988.1587551601569,9.0217759478008845E-4,0.45890083727217884,-50742.988446485077,7249.6490108233693,3.5289502423091452,2.2264868758608281E-3,2.2907610884031189,-49255.938147824956,4217.0941834966634]
["AKM2G","AKM2G-24F 240 V",1.83000004291534,4.1100001335143999,1.4782876712328801,3.27779967809672,7300,6,7300,2.5799999237060498,7.75,29.100000381469702,2.7899999622604799E-2,336,6,4988.1587551601569,7277.2068933510382,7300,1.4793858380270606,89.605735979095869,2.3947929316605663,2.0534511361543974,0.56911225966739165,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.81046542991640669,1.1529623286667743,9.7255851589968803,27.671095888002583,17.615966765381721,204.75587790538441,165.98374256482944,1596.7636034736593,1.6541349951399347E-3,1.7523276010195468,-49898.624903346376,4988.1587551601569,8.9777269011232983E-4,0.44026806606338675,-50747.934658744816,7277.2068933510382,3.3856641178753426,2.2264868758608281E-3,2.2907610884031189,-49255.938147824956,4217.0941834966634]
["AKM2G","AKM2G-24F 400 V",1.83000004291534,4.1100001335143999,1.3608750000000001,3.0174611638408102,8000,6,8000,2.5799999237060498,7.75,29.100000381469702,2.7899999622604799E-2,560,6,4988.1587551601569,7304.2830897857948,7745.7043658160992,1.4016722781701458,89.605735979095869,2.4010652600550593,2.0534511361543974,0.56911225966739165,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.81046542991640669,1.1529623286667743,9.7255851589968803,27.671095888002583,17.615966765381721,204.75587790538441,165.98374256482944,1596.7636034736593,1.6541349951399347E-3,1.7523276010195468,-49898.624903346376,4988.1587551601569,8.9354738847347026E-4,0.42162196309938382,-50752.679197013749,7304.2830897857948,3.2422754721625173,2.2264868758608281E-3,2.2907610884031189,-49255.938147824956,4217.0941834966634]
["AKM2G","AKM2G-24F 480 V",1.83000004291534,4.1100001335143999,1.3250625,2.93805429110816,8000,6,8000,2.5799999237060498,7.75,29.100000381469702,2.7899999622604799E-2,672,6,4988.1587551601569,7316.0285766322204,7745.7043658160992,1.3682328562424544,89.605735979095869,2.4037594571408687,2.0534511361543974,0.56911225966739165,12.320706816926384,0,-9.9797725217103714,0,0,0,0,0,0.81046542991640669,1.1529623286667743,9.7255851589968803,27.671095888002583,17.615966765381721,204.75587790538441,165.98374256482944,1596.7636034736593,1.6541349951399347E-3,1.7523276010195468,-49898.624903346376,4988.1587551601569,8.9174684794154154E-4,0.41342078182085157,-50754.701001417001,7316.0285766322204,3.1792083380249254,2.2264868758608281E-3,2.2907610884031189,-49255.938147824956,4217.0941834966634]
["AKM2G","AKM2G-31C 120 V",1.6799999475479099,1.4800000190734901,1.6712499999999999,1.4407328000772801,1000,5.9899997711181596,1000,21.399999618530298,46.900001525878899,75.599998474121094,4.2600000597303699E-2,168,8,1000,1000,1000,1.6712499999999999,58.685445186548513,2.5987020629303923,2.0688403138347788,2.6279218514835097,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.31975280619559115,0.45487805700365197,3.8370336743470941,10.917073368087648,6.9500247625121432,205.94655459561494,166.94895526226662,1606.0489496230048,1.3775502137619453E-2,14.786842202127394,-41240.989451822577,1274.8790885384556,6.2785750008214746E-3,3.9087804502613062,-50136.848413980166,2531.6560715269979,1.3949064993685298,1.9696960618358239E-2,19.475227144498554,-34214.582694263649,913.26916690660209]
["AKM2G","AKM2G-31C 240 V",1.6799999475479099,1.4800000190734901,1.6394166666666701,1.4132902705520001,2400,5.9899997711181596,2400,21.399999618530298,46.900001525878899,75.599998474121094,4.2600000597303699E-2,336,8,1274.8790885384556,2400,2400,1.6394166666666701,58.685445186548513,2.6044276150512369,2.0688403138347788,2.6279218514835097,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.31975280619559115,0.45487805700365197,3.8370336743470941,10.917073368087648,6.9500247625121432,205.94655459561494,166.94895526226662,1606.0489496230048,1.3775502137619453E-2,14.786842202127394,-41240.989451822577,1274.8790885384556,6.29882841302067E-3,3.9784402738961648,-50112.815700958039,2522.4361093664629,1.4197656445596172,1.9696960618358239E-2,19.475227144498554,-34214.582694263649,913.26916690660209]
["AKM2G","AKM2G-31C 400 V",1.6799999475479099,1.4800000190734901,1.58352325581395,1.3651062942924901,4300,5.9899997711181596,4300,21.399999618530298,46.900001525878899,75.599998474121094,4.2600000597303699E-2,560,8,1274.8790885384556,2521.5702319695602,2981.4815416584629,1.6234248884885478,58.685445186548513,2.6083199817394762,2.0688403138347788,2.6279218514835097,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.31975280619559115,0.45487805700365197,3.8370336743470941,10.917073368087648,6.9500247625121432,205.94655459561494,166.94895526226662,1606.0489496230048,1.3775502137619453E-2,14.786842202127394,-41240.989451822577,1274.8790885384556,6.3007469493398405E-3,3.9849757733524305,-50110.539164425441,2521.5702319695602,1.4220979348440601,1.9696960618358239E-2,19.475227144498554,-34214.582694263649,913.26916690660209]
["AKM2G","AKM2G-31C 480 V",1.6799999475479099,1.4800000190734901,1.5500384615384599,1.3362400915002499,5200,5.9899997711181596,5200,21.399999618530298,46.900001525878899,75.599998474121094,4.2600000597303699E-2,672,8,1274.8790885384556,2522.3157700078432,2981.4815416584629,1.6169607349218929,58.685445186548513,2.6101241646174644,2.0688403138347788,2.6279218514835097,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.31975280619559115,0.45487805700365197,3.8370336743470941,10.917073368087648,6.9500247625121432,205.94655459561494,166.94895526226662,1606.0489496230048,1.3775502137619453E-2,14.786842202127394,-41240.989451822577,1274.8790885384556,6.2990948812074185E-3,3.9793486404088156,-50112.499509622045,2522.3157700078432,1.4200898086738285,1.9696960618358239E-2,19.475227144498554,-34214.582694263649,913.26916690660209]
["AKM2G","AKM2G-31D 120 V",1.6799999475479099,2.0599999427795401,1.6744333333333301,2.0029106252572202,1500,6,1500,10.8999996185303,24.200000762939499,54.400001525878899,4.2600000597303699E-2,168,8,1500,1500,1500,1.6744333333333301,58.685445186548513,2.5951789329995276,2.0653921677250575,1.6,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.44506132025516387,0.63314105359660944,5.3407358430619665,15.195385286318626,9.6736827220138579,205.94655459561494,166.94895526226662,1606.0489496230048,7.1308157369254499E-3,7.5560567753974315,-45981.989551816718,2064.2251404059011,3.2490910301947295E-3,1.9913554280221777,-50470.163901328749,3646.7197767743278,1.9389328123465028,1.0171313699126687E-2,9.9352285312731432,-42466.468489740051,1612.4744392260366]
["AKM2G","AKM2G-31D 240 V",1.6799999475479099,2.0599999427795401,1.6207714285714301,1.93872174590351,3500,6,3500,10.8999996185303,24.200000762939499,54.400001525878899,4.2600000597303699E-2,336,8,2064.2251404059011,3500,3500,1.6207714285714301,58.685445186548513,2.604436569724756,2.0653921677250575,1.4883956865399763,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.44506132025516387,0.63314105359660944,5.3407358430619665,15.195385286318626,9.6736827220138579,205.94655459561494,166.94895526226662,1606.0489496230048,7.1308157369254499E-3,7.5560567753974315,-45981.989551816718,2064.2251404059011,3.2523405362536234E-3,2.0024914158400628,-50466.406718415492,3643.3135763730311,1.9497756442559395,1.0171313699126687E-2,9.9352285312731432,-42466.468489740051,1612.4744392260366]
["AKM2G","AKM2G-31D 400 V",1.6799999475479099,2.0599999427795401,1.5217377049180301,1.8202603575547101,6100,6,6100,10.8999996185303,24.200000762939499,54.400001525878899,4.2600000597303699E-2,560,8,2064.2251404059011,3647.9599472284176,4143.3822367224357,1.5853549766835906,58.685445186548513,2.6107967685600797,2.0653921677250575,1.4883956865399763,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.44506132025516387,0.63314105359660944,5.3407358430619665,15.195385286318626,9.6736827220138579,205.94655459561494,166.94895526226662,1606.0489496230048,7.1308157369254499E-3,7.5560567753974315,-45981.989551816718,2064.2251404059011,3.2479114899561534E-3,1.9872977322504619,-50471.527723506508,3647.9599472284176,1.9349819357909734,1.0171313699126687E-2,9.9352285312731432,-42466.468489740051,1612.4744392260366]
["AKM2G","AKM2G-31D 480 V",1.6799999475479099,2.0599999427795401,1.4652054794520499,1.7526380803334201,7300,6,7300,10.8999996185303,24.200000762939499,54.400001525878899,4.2600000597303699E-2,672,8,2064.2251404059011,3650.7566311615246,4143.3822367224357,1.5725804504605436,58.685445186548513,2.6132577878281169,2.0653921677250575,1.4883956865399763,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.44506132025516387,0.63314105359660944,5.3407358430619665,15.195385286318626,9.6736827220138579,205.94655459561494,166.94895526226662,1606.0489496230048,7.1308157369254499E-3,7.5560567753974315,-45981.989551816718,2064.2251404059011,3.245258545218583E-3,1.9781410159221555,-50474.595143125727,3650.7566311615246,1.9260662708662362,1.0171313699126687E-2,9.9352285312731432,-42466.468489740051,1612.4744392260366]
["AKM2G","AKM2G-31E 120 V",1.70000004768372,2.9000000953674299,1.67747826086957,2.7911451418608402,2300,6.0599999427795401,2300,5.4899997711181596,12.5,39.099998474121101,4.2600000597303699E-2,168,8,2300,2300,2300,1.67747826086957,58.685445186548513,2.568770452149975,2.0449427596308434,1.0434782608695652,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.61917154634506877,0.88082901696602833,7.4300585561408248,21.139896407184679,13.458076038616161,205.94655459561494,166.94895526226662,1606.0489496230048,3.7261733762823678E-3,3.8435398909216527,-48389.424878218335,3124.6296025306783,1.6767820918494041E-3,0.99740265959558161,-50642.482469271286,5206.2776738073289,2.6826303136051237,5.252936714897103E-3,5.0037162280166401,-46710.933437400563,2543.5212175691177]
["AKM2G","AKM2G-31E 240 V",1.70000004768372,2.9000000953674299,1.5891200000000001,2.6441264076558899,5000,6.0599999427795401,5000,5.4899997711181596,12.5,39.099998474121101,4.2600000597303699E-2,336,8,3124.6296025306783,5000,5000,1.5891200000000001,58.685445186548513,2.577270381105873,2.0449427596308434,0.94357380761058363,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.61917154634506877,0.88082901696602833,7.4300585561408248,21.139896407184679,13.458076038616161,205.94655459561494,166.94895526226662,1606.0489496230048,3.7261733762823678E-3,3.8435398909216527,-48389.424878218335,3124.6296025306783,1.6748395912538753E-3,0.99083434586743224,-50644.618013491476,5211.1037279365537,2.6649640708426006,5.252936714897103E-3,5.0037162280166401,-46710.933437400563,2543.5212175691177]
["AKM2G","AKM2G-31E 400 V",1.70000004768372,2.9000000953674299,1.4325000000000001,2.3835274107475,8000,6.0599999427795401,8000,5.4899997711181596,12.5,39.099998474121101,4.2600000597303699E-2,560,8,3124.6296025306783,5227.8187224383619,5764.7061073208033,1.5251948279919569,58.685445186548513,2.5850488914588938,2.0449427596308434,0.94357380761058363,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.61917154634506877,0.88082901696602833,7.4300585561408248,21.139896407184679,13.458076038616161,205.94655459561494,166.94895526226662,1606.0489496230048,3.7261733762823678E-3,3.8435398909216527,-48389.424878218335,3124.6296025306783,1.6681804546773249E-3,0.96797910913689111,-50651.938927914998,5227.8187224383619,2.6034922567381229,5.252936714897103E-3,5.0037162280166401,-46710.933437400563,2543.5212175691177]
["AKM2G","AKM2G-31E 480 V",1.70000004768372,2.9000000953674299,1.3847499999999999,2.3040764970559202,8000,6.0599999427795401,8000,5.4899997711181596,12.5,39.099998474121101,4.2600000597303699E-2,672,8,3124.6296025306783,5240.1413316185299,5764.7061073208033,1.4935056971009482,58.685445186548513,2.5891906785660632,2.0449427596308434,0.94357380761058363,12.392353006350346,0,-10.03780593514378,0,0,0,0,0,0.61917154634506877,0.88082901696602833,7.4300585561408248,21.139896407184679,13.458076038616161,205.94655459561494,166.94895526226662,1606.0489496230048,3.7261733762823678E-3,3.8435398909216527,-48389.424878218335,3124.6296025306783,1.6633397191644494E-3,0.9510202195807328,-50657.260730528491,5240.1413316185299,2.5578793532926096,5.252936714897103E-3,5.0037162280166401,-46710.933437400563,2543.5212175691177]
["AKM2G","AKM2G-32D 240 V",2.8099999427795401,2.1700000762939502,2.7260909090909098,2.0496923467125199,2200,10.300000190734901,2200,11.1000003814697,24.700000762939499,86.099998474121094,8.1300000601913794E-2,336,8,1441.9113810991914,2200,2200,2.7260909090909098,30.750307275411636,1.5833148929582619,1.2214536233790709,1.4197113132703325,12.580972553778265,0,-10.190587768560393,0,0,0,0,0,0.28456126877631943,0.40481482736476132,3.4147352253158334,9.7155558567542712,6.1851149579514253,209.08119302160696,169.49002525672171,1630.4940429696626,1.2492625436727755E-2,13.166715014640925,-44958.759101418735,1441.9113810991914,7.754279229628948E-3,3.4118662241390494,-50412.58945552526,2339.2314361665331,2.0611292653197122,1.0484550241742321E-2,10.23845770982167,-47270.05105288748,1690.4845214422878]
["AKM2G","AKM2G-32D 400 V",2.8099999427795401,2.1700000762939502,2.5956410256410298,1.9516097307421201,3900,10.300000190734901,3900,11.1000003814697,24.700000762939499,86.099998474121094,8.1300000601913794E-2,560,8,1441.9113810991914,2339.6305383225235,2617.8862252564159,2.6814048995233848,30.750307275411636,1.5876334762793936,1.2214536233790709,1.4197113132703325,12.580972553778265,0,-10.190587768560393,0,0,0,0,0,0.28456126877631943,0.40481482736476132,3.4147352253158334,9.7155558567542712,6.1851149579514253,209.08119302160696,169.49002525672171,1630.4940429696626,1.2492625436727755E-2,13.166715014640925,-44958.759101418735,1441.9113810991914,7.7534151960692403E-3,3.4075418322199433,-50413.583957034636,2339.6305383225235,2.0585168736977546,1.0484550241742321E-2,10.23845770982167,-47270.05105288748,1690.4845214422878]
["AKM2G","AKM2G-32D 480 V",2.8099999427795401,2.1700000762939502,2.4992553191489399,1.8791392770714499,4700,10.300000190734901,4700,11.1000003814697,24.700000762939499,86.099998474121094,8.1300000601913794E-2,672,8,1441.9113810991914,2341.4203431961309,2617.8862252564159,2.6551948825013461,30.750307275411636,1.5905092346622838,1.2214536233790709,1.4197113132703325,12.580972553778265,0,-10.190587768560393,0,0,0,0,0,0.28456126877631943,0.40481482736476132,3.4147352253158334,9.7155558567542712,6.1851149579514253,209.08119302160696,169.49002525672171,1630.4940429696626,1.2492625436727755E-2,13.166715014640925,-44958.759101418735,1441.9113810991914,7.7495518047312256E-3,3.3881384751374357,-50418.030715466404,2341.4203431961309,2.0467951869430823,1.0484550241742321E-2,10.23845770982167,-47270.05105288748,1690.4845214422878]
["AKM2G","AKM2G-32E 120 V",2.7999999523162802,2.75,2.77684615384615,2.6446155047154698,1300,10.3999996185303,1300,6.9000000953674299,15.300000190734901,67.699996948242202,8.1300000601913794E-2,168,8,1300,1300,1300,2.77684615384615,30.750307275411636,1.5837798321116343,1.2097089437736128,1.8461538461538463,12.580972553778265,0,-10.190587768560393,0,0,0,0,0,0.36190703091304705,0.51484635583460092,4.3428843709565648,12.356312540030421,7.8662728765368568,209.08119302160696,169.49002525672171,1630.4940429696626,7.7972264502591737E-3,8.264305565350778,-47079.738270468159,1983.782578227429,4.7818162789208451E-3,2.0539844395500557,-50575.038599310443,3044.4718426025543,2.5386263056352321,6.489449666568347E-3,6.3645452856907978,-48595.642363893057,2289.7093105410454]
["AKM2G","AKM2G-32E 240 V",2.7999999523162802,2.75,2.67070689655172,2.54353049317782,2900,10.3999996185303,2900,6.9000000953674299,15.300000190734901,67.699996948242202,8.1300000601913794E-2,336,8,1983.782578227429,2900,2900,2.67070689655172,30.750307275411636,1.5906677137300305,1.2097089437736128,1.0481679875044458,12.580972553778265,0,-10.190587768560393,0,0,0,0,0,0.36190703091304705,0.51484635583460092,4.3428843709565648,12.356312540030421,7.8662728765368568,209.08119302160696,169.49002525672171,1630.4940429696626,7.7972264502591737E-3,8.264305565350778,-47079.738270468159,1983.782578227429,4.7858612868591074E-3,2.0748040278489093,-50570.349844954188,3041.0882634680765,2.5643583187460726,6.489449666568347E-3,6.3645452856907978,-48595.642363893057,2289.7093105410454]
["AKM2G","AKM2G-32E 400 V",2.7999999523162802,2.75,2.4639000000000002,2.3465715351364298,5000,10.3999996185303,5000,6.9000000953674299,15.300000190734901,67.699996948242202,8.1300000601913794E-2,560,8,1983.782578227429,3044.3419284486745,3329.3945370828028,2.5953593169190698,30.750307275411636,1.596538185817012,1.2097089437736128,1.0481679875044458,12.580972553778265,0,-10.190587768560393,0,0,0,0,0,0.36190703091304705,0.51484635583460092,4.3428843709565648,12.356312540030421,7.8662728765368568,209.08119302160696,169.49002525672171,1630.4940429696626,7.7972264502591737E-3,8.264305565350778,-47079.738270468159,1983.782578227429,4.7819709962721498E-3,2.0547846471638427,-50574.859259327437,3044.3419284486745,2.5396153238863994,6.489449666568347E-3,6.3645452856907978,-48595.642363893057,2289.7093105410454]
["AKM2G","AKM2G-32E 480 V",2.7999999523162802,2.75,2.3327049180327899,2.2216238323505402,6100,10.3999996185303,6100,6.9000000953674299,15.300000190734901,67.699996948242202,8.1300000601913794E-2,672,8,1983.782578227429,3046.3729026107981,3329.3945370828028,2.5666302916661476,30.750307275411636,1.5989850167776307,1.2097089437736128,1.0481679875044458,12.580972553778265,0,-10.190587768560393,0,0,0,0,0,0.36190703091304705,0.51484635583460092,4.3428843709565648,12.356312540030421,7.8662728765368568,209.08119302160696,169.49002525672171,1630.4940429696626,7.7972264502591737E-3,8.264305565350778,-47079.738270468159,1983.782578227429,4.7795576922061737E-3,2.0422671939355608,-50577.656630834499,3046.3729026107981,2.5241443517441589,6.489449666568347E-3,6.3645452856907978,-48595.642363893057,2289.7093105410454]
["AKM2G","AKM2G-32G 120 V",2.9000000953674299,4.2399997711181596,2.8234782608695701,4.02778653458014,2300,10.6000003814697,2300,2.8699998855590798,6.8000001907348597,45.400001525878899,8.1300000601913794E-2,168,8,2300,2300,2300,2.8234782608695701,30.750307275411636,1.5327146495013058,1.1868841604733886,1.0434782608695652,12.580972553778265,0,-10.190587768560393,0,0,0,0,0,0.53875358302205723,0.76642699704384398,6.4650429962646871,18.394247929052256,11.710141929466101,209.08119302160696,169.49002525672171,1630.4940429696626,3.5226766814413727E-3,3.4976155902220412,-49321.370047418808,3278.1513476513755,2.15217197482477E-3,0.87280886120230583,-50712.761149718375,4655.6870818273028,3.8674149574313406,2.8955723465281607E-3,2.6427770886946855,-49958.031408448216,3722.3483294838538]
["AKM2G","AKM2G-32G 240 V",2.9000000953674299,4.2399997711181596,2.6008510638297899,3.7102013635181201,4700,10.6000003814697,4700,2.8699998855590798,6.8000001907348597,45.400001525878899,8.1300000601913794E-2,336,8,3278.1513476513755,4664.02548373429,4700,2.6031407961065818,30.750307275411636,1.5400372969225233,1.1868841604733886,0.64475427541000374,12.580972553778265,0,-10.190587768560393,0,0,0,0,0,0.53875358302205723,0.76642699704384398,6.4650429962646871,18.394247929052256,11.710141929466101,209.08119302160696,169.49002525672171,1630.4940429696626,3.5226766814413727E-3,3.4976155902220412,-49321.370047418808,3278.1513476513755,2.1483255734309507E-3,0.85416615457147338,-50716.66616999988,4664.02548373429,3.7848091479855381,2.8955723465281607E-3,2.6427770886946855,-49958.031408448216,3722.3483294838538]
["AKM2G","AKM2G-32G 400 V",2.9000000953674299,4.2399997711181596,2.1613157894736799,3.0831895376933098,7600,10.6000003814697,7600,2.8699998855590798,6.8000001907348597,45.400001525878899,8.1300000601913794E-2,560,8,3278.1513476513755,4679.9465893443785,4964.7575423872522,2.4451312666872096,30.750307275411636,1.5482053606636972,1.1868841604733886,0.64475427541000374,12.580972553778265,0,-10.190587768560393,0,0,0,0,0,0.53875358302205723,0.76642699704384398,6.4650429962646871,18.394247929052256,11.710141929466101,209.08119302160696,169.49002525672171,1630.4940429696626,3.5226766814413727E-3,3.4976155902220412,-49321.370047418808,3278.1513476513755,2.1411354177887773E-3,0.81817855262751848,-50723.965903110147,4679.9465893443785,3.6253481293973269,2.8955723465281607E-3,2.6427770886946855,-49958.031408448216,3722.3483294838538]
["AKM2G","AKM2G-33E 240 V",3.8599998950958301,2.9900000095367401,3.6456086956521698,2.7410590812170499,2300,14.6000003814697,2300,6.3499999046325701,15.1000003814697,85.599998474121094,0.11999999696854501,336,8,1628.2468415410428,2300,2300,3.6456086956521698,20.833333859627615,1.1755494319841915,0.87462957190619128,1.1481737439319071,12.769592083475073,0,-10.343369587614809,0,0,0,0,0,0.28971371603582546,0.41214466201454442,3.4765645924299053,9.8914718883490664,6.2971065819411134,212.21583115292856,172.03109501230452,1654.9391340183695,1.1165014710527429E-2,10.647431801701089,-46937.197732089255,1628.2468415410428,7.5570546705503215E-3,2.6048793330932329,-50573.651087448794,2420.3243236796716,2.7668110853689543,8.5171611688619944E-3,5.9285590116089946,-49605.96229416877,2090.2759819095227]
["AKM2G","AKM2G-33E 400 V",3.8599998950958301,2.9900000095367401,3.3186249999999999,2.4952066864040199,4000,14.6000003814697,4000,6.3499999046325701,15.1000003814697,85.599998474121094,0.11999999696854501,560,8,1628.2468415410428,2423.1032311688036,2633.1776170316612,3.5320480807007355,20.833333859627615,1.1814364136472899,0.87462957190619128,1.1481737439319071,12.769592083475073,0,-10.343369587614809,0,0,0,0,0,0.28971371603582546,0.41214466201454442,3.4765645924299053,9.8914718883490664,6.2971065819411134,212.21583115292856,172.03109501230452,1654.9391340183695,1.1165014710527429E-2,10.647431801701089,-46937.197732089255,1628.2468415410428,7.5517909341337756E-3,2.5748593744894666,-50578.95639342269,2423.1032311688036,2.7349249426244508,8.5171611688619944E-3,5.9285590116089946,-49605.96229416877,2090.2759819095227]
["AKM2G","AKM2G-33E 480 V",3.8599998950958301,2.9900000095367401,3.1435416666666698,2.3635650866417,4800,14.6000003814697,4800,6.3499999046325701,15.1000003814697,85.599998474121094,0.11999999696854501,672,8,1628.2468415410428,2424.3250307337248,2633.1776170316612,3.4981399749591731,20.833333859627615,1.1833942558439252,0.87462957190619128,1.1481737439319071,12.769592083475073,0,-10.343369587614809,0,0,0,0,0,0.28971371603582546,0.41214466201454442,3.4765645924299053,9.8914718883490664,6.2971065819411134,212.21583115292856,172.03109501230452,1654.9391340183695,1.1165014710527429E-2,10.647431801701089,-46937.197732089255,1628.2468415410428,7.5494924814477624E-3,2.5616405727849458,-50581.272997789027,2424.3250307337248,2.7208843970119481,8.5171611688619944E-3,5.9285590116089946,-49605.96229416877,2090.2759819095227]
["AKM2G","AKM2G-33G 120 V",3.8099999427795401,4.2399997711181596,3.7125625000000002,4.0179246757288096,1600,14.3999996185303,1600,3.1400001049041699,7.3000001907348597,59.700000762939503,0.11999999696854501,168,8,{"$f":"IF(AQ466<I466,IF(AQ466<0,0,AQ466),I466)","v":1600},{"$f":"IF(AU466<I466,IF(AU466<0,0,AU466),I466)","v":1600},{"$f":"IF(UAC_V*0.98/L466*1000<I466,IF(UAC_V*0.98/L466*1000<0,0,UAC_V*0.98/L466*1000),I466)","v":1600},{"$f":"C466+(E466-C466)/G466*Q466","v":3.7125625000000002},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M466,(inertia/gear^2+gear_inertia)/M466),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M466,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M466))","v":20.833333859627615},{"$f":"IF((C466+(E466-C466)/G466*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X466^2*time1+Y466^2*time2+Z466^2*time3+AA466^2*time4)/time)/(C466+(E466-C466)/G466*mspeed),SQRT((((X466-Y466)*2/PI()+Y466)^2*time1+Y466^2*time2+((Z466-Y466)*2/PI()+Y466)^2*time3+AA466^2*time4)/time)/(C466+(E466-C466)/G466*mspeed)),IF(AccType=1,SQRT((X466^2*time1+Y466^2*time2+Z466^2*time3+AA466^2*time4+AB466^2*time5+AC466^2*time6+AD466^2*time7+AE466^2*time8)/time)/(C466+(E466-C466)/G466*mspeed),SQRT((((X466-Y466)*2/PI()+Y466)^2*time1+Y466^2*time2+((Z466-Y466)*2/PI()+Y466)^2*time3+AA466^2*time4+((AB466-AC466)*2/PI()+AC466)^2*time5+AC466^2*time6+((AD466-AC466)*2/PI()+AC466)^2*time7+AE466^2*time8)/time)/(C466+(E466-C466)/G466*mspeed))))","v":1.1865536732292818},{"$f":"IF(move1,MAX(ABS(X466),ABS(Z466))/H466,MAX(ABS(X466),ABS(Z466),ABS(AB466),ABS(AD466))/H466)","v":0.88677725151067532},{"$f":"IF(AZ466>0,speed/(MIN(AZ466,I466)),\"NA\")","v":1.5},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M466+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M466+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.769592083475073},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M466+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M466+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.343369587614809},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M466+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M466+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M466+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M466+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH466/Irms","v":0.4162229508156054},{"$f":"AI466/Ipeak","v":0.59211579532320535},{"$f":"IF(move1,IF(AccType=1,SQRT((X466^2*time1+Y466^2*time2+Z466^2*time3+AA466^2*time4)/time)/(C466/D466),SQRT((((X466-Y466)*2/PI()+Y466)^2*time1+Y466^2*time2+((Z466-AA466)*2/PI()+AA466)^2*time3+AA466^2*time4)/time)/(C466/D466)),IF(AccType=1,SQRT((X466^2*time1+Y466^2*time2+Z466^2*time3+AA466^2*time4+AB466^2*time5+AC466^2*time6+AD466^2*time7+AE466^2*time8)/time)/(C466/D466),SQRT((((X466-Y466)*2/PI()+Y466)^2*time1+Y466^2*time2+((Z466-AA466)*2/PI()+AA466)^2*time3+AA466^2*time4+((AB466-AC466)*2/PI()+AC466)^2*time5+AC466^2*time6+((AD466-AE466)*2/PI()+AE466)^2*time7+AE466^2*time8)/time)/(C466/D466)))","v":4.9946754097872645},{"$f":"IF(move1,MAX(ABS(X466),ABS(Z466))/(C466/D466),MAX(ABS(X466),ABS(Z466),ABS(AB466),ABS(AD466))/(C466/D466))","v":14.210779087756928},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X466),ABS(Z466))/(C466/D466),MAX(ABS((X466-Y466)*2/PI()+Y466),ABS((Z466-Y466)*2/PI()+Y466))/(C466/D466)),IF(AccType=1,MAX(ABS(X466),ABS(Z466),ABS(AB466),ABS(AD466))/(C466/D466),MAX(ABS((X466-Y466)*2/PI()+Y466),ABS((Z466-Y466)*2/PI()+Y466),ABS((AB466-AC466)*2/PI()+AC466),ABS((AD466-AC466)*2/PI()+AC466))/(C466/D466)))","v":9.0468629480138016},{"$f":"IF((C466+(E466-C466)/G466*mspeed)<0,\"NA\",U466*(C466+(E466-C466)/G466*mspeed)*mspeed/9.55)","v":212.21583115292856},{"$f":"IF(move1,IF(speed1>speed2,AM466/2*time1/time,AM466/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z466*-speed/30*PI(),((Z466-AA466)*2/PI()+AA466)*-speed/30*PI()),IF(AccType=1,X466*-speed/30*PI(),((X466-Y466)*2/PI()+Y466)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z466*-speed/30*PI(),((Z466-AA466)*2/PI()+AA466)*-speed/30*PI()),IF(AccType=1,X466*-speed/30*PI(),((X466-Y466)*2/PI()+Y466)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD466*-speed/30*PI(),((AD466-AE466)*2/PI()+AE466)*-speed/30*PI()),IF(AccType=1,AB466*-speed/30*PI(),((AB466-AC466)*2/PI()+AC466)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD466*-speed/30*PI(),((AD466-AE466)*2/PI()+AE466)*-speed/30*PI()),IF(AccType=1,AB466*-speed/30*PI(),((AB466-AC466)*2/PI()+AC466)*-speed/30*PI()),0)/2*time7/time)))","v":172.03109501230452},{"$f":"IF(move1,MAX(IF(AccType=1,Z466*-speed/30*PI(),((Z466-AA466)*2/PI()+AA466)*-speed/30*PI()),IF(AccType=1,X466*-speed/30*PI(),((X466-Y466)*2/PI()+Y466)*-speed/30*PI()),0),MAX(IF(AccType=1,Z466*-speed/30*PI(),((Z466-AA466)*2/PI()+AA466)*-speed/30*PI()),IF(AccType=1,X466*-speed/30*PI(),((X466-Y466)*2/PI()+Y466)*-speed/30*PI()),IF(AccType=1,AD466*-speed/30*PI(),((AD466-AE466)*2/PI()+AE466)*-speed/30*PI()),IF(AccType=1,AB466*-speed/30*PI(),((AB466-AC466)*2/PI()+AC466)*-speed/30*PI()),0))","v":1654.9391340183695},{"$f":"(L466^2)/1000000+((K466/1000)^2*(D466/C466*H466)^2*PI()*PI()*(O466/2)^2)/1200","v":5.3649955483124736E-3},{"$f":"SQRT(3)*L466*J466*D466/C466*H466/1000","v":5.2031694685499481},{"$f":"0.75*J466^2*(D466/C466*H466)^2-(UAC_V*0.98)^2","v":-48906.149886163847},{"$f":"-AO466/2/AN466+SQRT((AO466/2/AN466)^2-AP466/AN466)","v":2573.0109483038673},{"$f":"(L466^2)/1000000+((K466/1000)^2*AV466^2*PI()*PI()*(O466/2)^2)/1200","v":3.6662309713435914E-3},{"$f":"SQRT(3)*L466*J466*AV466/1000","v":1.239145523482104},{"$f":"0.75*J466^2*AV466^2-(UAC_V*0.98)^2","v":-50697.454976479261},{"$f":"-AS466/2/AR466+SQRT((AS466/2/AR466)^2-AT466/AR466)","v":3553.4752625180517},{"$f":"D466+(F466-D466)*((0.85*UAC_V-D466*J466)/L466*1000)/G466","v":3.8164333797611794},{"$f":"(L466^2)/1000000+((K466/1000)^2*AJ466^2*PI()*PI()*(O466/2)^2)/1200","v":4.1380482678161305E-3},{"$f":"SQRT(3)*L466*J466*AJ466/1000","v":2.9373969379465295},{"$f":"0.75*J466^2*AJ466^2-(UAC_V*0.98)^2","v":-50199.935345843827},{"$f":"IF(((AX466/2/AW466)^2-AY466/AW466)>0,-AX466/2/AW466+SQRT((AX466/2/AW466)^2-AY466/AW466),-9999)","v":3146.1143506423032}]
["AKM2G","AKM2G-33G 240 V",3.8099999427795401,4.2399997711181596,3.4494029850746299,3.7331200135388798,3350,14.3999996185303,3350,3.1400001049041699,7.3000001907348597,59.700000762939503,0.11999999696854501,336,8,2573.0109483038673,3350,3350,3.4494029850746299,20.833333859627615,1.1932119999319537,0.88677725151067532,0.76284576226862888,12.769592083475073,0,-10.343369587614809,0,0,0,0,0,0.4162229508156054,0.59211579532320535,4.9946754097872645,14.210779087756928,9.0468629480138016,212.21583115292856,172.03109501230452,1654.9391340183695,5.3649955483124736E-3,5.2031694685499481,-48906.149886163847,2573.0109483038673,3.6641976363009105E-3,1.2267495860813784,-50699.599077823055,3556.1099467125578,3.7782552413802901,4.1380482678161305E-3,2.9373969379465295,-50199.935345843827,3146.1143506423032]
["AKM2G","AKM2G-33G 400 V",3.8099999427795401,4.2399997711181596,2.83206896551724,3.0650096206912298,5800,14.3999996185303,5800,3.1400001049041699,7.3000001907348597,59.700000762939503,0.11999999696854501,560,8,2573.0109483038673,3566.8356491255681,3775.5443403599343,3.2086001027651645,20.833333859627615,1.2020098235138572,0.88677725151067532,0.76284576226862888,12.769592083475073,0,-10.343369587614809,0,0,0,0,0,0.4162229508156054,0.59211579532320535,4.9946754097872645,14.210779087756928,9.0468629480138016,212.21583115292856,172.03109501230452,1654.9391340183695,5.3649955483124736E-3,5.2031694685499481,-48906.149886163847,2573.0109483038673,3.6560771352327393E-3,1.1759418485793864,-50708.161944683205,3566.8356491255681,3.6217729383107864,4.1380482678161305E-3,2.9373969379465295,-50199.935345843827,3146.1143506423032]
["AKM2G","AKM2G-33G 480 V",3.8099999427795401,4.2399997711181596,2.4147857142857099,2.6134043825594802,7000,14.3999996185303,7000,3.1400001049041699,7.3000001907348597,59.700000762939503,0.11999999696854501,672,8,2573.0109483038673,3573.0111958908433,3775.5443403599343,3.0978405057688745,20.833333859627615,1.2064903089147474,0.88677725151067532,0.76284576226862888,12.769592083475073,0,-10.343369587614809,0,0,0,0,0,0.4162229508156054,0.59211579532320535,4.9946754097872645,14.210779087756928,9.0468629480138016,212.21583115292856,172.03109501230452,1654.9391340183695,5.3649955483124736E-3,5.2031694685499481,-48906.149886163847,2573.0109483038673,3.6515177253219266E-3,1.1464282451794916,-50712.969729289034,3573.0111958908433,3.5308742512414311,4.1380482678161305E-3,2.9373969379465295,-50199.935345843827,3146.1143506423032]
["AKM2G","AKM2G-33H 120 V",3.8499999046325701,5.8000001907348597,3.6756888888888901,5.3816818996836302,2250,14.6000003814697,2250,1.66999995708466,4,44.099998474121101,0.11999999696854501,168,8,2250,2250,2250,3.6756888888888901,20.833333859627615,1.1764404247527418,0.87462957190619128,1.0666666666666667,12.769592083475073,0,-10.343369587614809,0,0,0,0,0,0.56344619307748045,0.80155452764474522,6.761354316929765,19.237308663473886,12.246851062305648,212.21583115292856,172.03109501230452,1654.9391340183695,2.9633983853040169E-3,2.8056650228969899,-49793.26722314264,3652.9743545804258,1.9977985935876884E-3,0.63992367419142748,-50752.519595908016,4882.6468409688068,5.0166351356203114,2.2606063834878986E-3,1.5622124625766227,-50491.439386274891,4393.1140318965263]
["AKM2G","AKM2G-33H 240 V",3.8499999046325701,5.8000001907348597,3.1971739130434802,4.6810743504377399,4600,14.6000003814697,4600,1.66999995708466,4,44.099998474121101,0.11999999696854501,336,8,3652.9743545804258,4600,4600,3.1971739130434802,20.833333859627615,1.1854835259644148,0.87462957190619128,0.54630951588659526,12.769592083475073,0,-10.343369587614809,0,0,0,0,0,0.56344619307748045,0.80155452764474522,6.761354316929765,19.237308663473886,12.246851062305648,212.21583115292856,172.03109501230452,1654.9391340183695,2.9633983853040169E-3,2.8056650228969899,-49793.26722314264,3652.9743545804258,1.9928188646460014E-3,0.60911284209822469,-50757.466590350246,4896.2860252066712,4.7750958566871473,2.2606063834878986E-3,1.5622124625766227,-50491.439386274891,4393.1140318965263]
["AKM2G","AKM2G-33H 400 V",3.8499999046325701,5.8000001907348597,1.8741874999999999,2.7440518635439402,8000,14.6000003814697,8000,1.66999995708466,4,44.099998474121101,0.11999999696854501,560,8,3652.9743545804258,4928.3116991529778,5111.1112879577522,2.6328224809972864,20.833333859627615,1.2005268663373092,0.87462957190619128,0.54630951588659526,12.769592083475073,0,-10.343369587614809,0,0,0,0,0,0.56344619307748045,0.80155452764474522,6.761354316929765,19.237308663473886,12.246851062305648,212.21583115292856,172.03109501230452,1654.9391340183695,2.9633983853040169E-3,2.8056650228969899,-49793.26722314264,3652.9743545804258,1.9817830137336067E-3,0.53453930657013105,-50768.429896539848,4928.3116991529778,4.1904820447503299,2.2606063834878986E-3,1.5622124625766227,-50491.439386274891,4393.1140318965263]
["AKM2G","AKM2G-41D 120 V",2.8499999046325701,2.3199999332428001,2.8331666666666702,2.2848118103846802,900,7.25,900,9.6099996566772496,56.5,82.199996948242202,7.7400000009220093E-2,168,10,900,900,900,2.8331666666666702,32.299741598219555,1.553785294872865,1.7326847419924938,2.6666666666666665,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.2995082710477836,0.42607832597848039,3.594099252573403,10.225879823483529,6.5099972854843271,208.76529917876999,169.23394839668893,1628.0305835761476,2.9619021124197675E-2,8.074895941276937,-48392.643597954993,1149.1513825232396,1.0043286102905388E-2,3.0615502316811627,-50458.359923445067,2094.2063445014496,2.237616153046909,3.457427044288057E-2,8.9071057475515367,-47869.744232830613,1054.8866324326543]
["AKM2G","AKM2G-41D 240 V",2.8499999046325701,2.3199999332428001,2.76040476190476,2.2261328553828301,2100,7.25,2100,9.6099996566772496,56.5,82.199996948242202,7.7400000009220093E-2,336,10,1149.1513825232396,2098.407722618068,2100,2.7604726953901393,32.299741598219555,1.5597242103053885,1.7326847419924938,2.2751259957341623,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.2995082710477836,0.42607832597848039,3.594099252573403,10.225879823483529,6.5099972854843271,208.76529917876999,169.23394839668893,1628.0305835761476,2.9619021124197675E-2,8.074895941276937,-48392.643597954993,1149.1513825232396,1.000871173755217E-2,3.0454034568667807,-50462.008360189633,2098.407722618068,2.225814849324895,3.457427044288057E-2,8.9071057475515367,-47869.744232830613,1054.8866324326543]
["AKM2G","AKM2G-41D 400 V",2.8499999046325701,2.3199999332428001,2.6136842105263201,2.1078098309876401,3800,7.25,3800,9.6099996566772496,56.5,82.199996948242202,7.7400000009220093E-2,560,10,1149.1513825232396,2106.7764889519131,2742.0925592238727,2.7189829708658859,32.299741598219555,1.5645971007438171,1.7326847419924938,2.2751259957341623,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.2995082710477836,0.42607832597848039,3.594099252573403,10.225879823483529,6.5099972854843271,208.76529917876999,169.23394839668893,1628.0305835761476,2.9619021124197675E-2,8.074895941276937,-48392.643597954993,1149.1513825232396,9.9404800255467052E-3,3.013284317919442,-50469.208465894604,2106.7764889519131,2.2023397146082395,3.457427044288057E-2,8.9071057475515367,-47869.744232830613,1054.8866324326543]
["AKM2G","AKM2G-41D 480 V",2.8499999046325701,2.3199999332428001,2.5328260869565198,2.0426016673199601,4600,7.25,4600,9.6099996566772496,56.5,82.199996948242202,7.7400000009220093E-2,672,10,1149.1513825232396,2110.1341833016186,2742.0925592238727,2.704504401431155,32.299741598219555,1.5662920225149501,1.7326847419924938,2.2751259957341623,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.2995082710477836,0.42607832597848039,3.594099252573403,10.225879823483529,6.5099972854843271,208.76529917876999,169.23394839668893,1628.0305835761476,2.9619021124197675E-2,8.074895941276937,-48392.643597954993,1149.1513825232396,9.9133406876973709E-3,3.0004132713781271,-50472.072326342117,2110.1341833016186,2.1929325648089528,3.457427044288057E-2,8.9071057475515367,-47869.744232830613,1054.8866324326543]
["AKM2G","AKM2G-41E 120 V",2.8699998855590798,2.9200000762939502,2.8411249999999999,2.8698232046780099,1200,7.2600002288818404,1200,6.03999996185303,36,65.599998474121094,7.7400000009220093E-2,168,10,1200,1200,1200,2.8411249999999999,32.299741598219555,1.5442314248433642,1.7302980693404648,2,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.37434037974418005,0.53253394902774653,4.4920845569301608,12.780814776665917,8.1365193937932769,208.76529917876999,169.23394839668893,1628.0305835761476,1.8842500690974824E-2,5.0691951453388757,-49312.329942965647,1488.8070302823946,6.4024608089804039E-3,1.9261331529076797,-50589.631372641299,2664.5774947571363,2.8066283900432265,2.1945076246192411E-2,5.5839311713868023,-48993.767926288187,1372.3579134730871]
["AKM2G","AKM2G-41E 240 V",2.8699998855590798,2.9200000762939502,2.73412962962963,2.7617470740318799,2700,7.2600002288818404,2700,6.03999996185303,36,65.599998474121094,7.7400000009220093E-2,336,10,1488.8070302823946,2680.5192145745564,2700,2.7351099478894305,32.299741598219555,1.550662606518338,1.7302980693404648,1.7488149238897988,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.37434037974418005,0.53253394902774653,4.4920845569301608,12.780814776665917,8.1365193937932769,208.76529917876999,169.23394839668893,1628.0305835761476,1.8842500690974824E-2,5.0691951453388757,-49312.329942965647,1488.8070302823946,6.3348860819916961E-3,1.8948762844610143,-50596.569718194158,2680.5192145745564,2.7610830370473414,2.1945076246192411E-2,5.5839311713868023,-48993.767926288187,1372.3579134730871]
["AKM2G","AKM2G-41E 400 V",2.8699998855590798,2.9200000762939502,2.5267708333333299,2.5522937464573401,4800,7.2600002288818404,4800,6.03999996185303,36,65.599998474121094,7.7400000009220093E-2,560,10,1488.8070302823946,2697.6315285879946,3435.9756896780918,2.6771029037233385,32.299741598219555,1.5558897749237808,1.7302980693404648,1.7488149238897988,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.37434037974418005,0.53253394902774653,4.4920845569301608,12.780814776665917,8.1365193937932769,208.76529917876999,169.23394839668893,1628.0305835761476,1.8842500690974824E-2,5.0691951453388757,-49312.329942965647,1488.8070302823946,6.2637301147730647E-3,1.8613956580009241,-50603.875773441607,2697.6315285879946,2.712297377241077,2.1945076246192411E-2,5.5839311713868023,-48993.767926288187,1372.3579134730871]
["AKM2G","AKM2G-41E 480 V",2.8699998855590798,2.9200000762939502,2.3794067796610201,2.4034411684242598,5900,7.2600002288818404,5900,6.03999996185303,36,65.599998474121094,7.7400000009220093E-2,672,10,1488.8070302823946,2708.0585189571402,3435.9756896780918,2.644821099157574,32.299741598219555,1.5587783420986132,1.7302980693404648,1.7488149238897988,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.37434037974418005,0.53253394902774653,4.4920845569301608,12.780814776665917,8.1365193937932769,208.76529917876999,169.23394839668893,1628.0305835761476,1.8842500690974824E-2,5.0691951453388757,-49312.329942965647,1488.8070302823946,6.2210603393759124E-3,1.8410264708093966,-50608.256962379564,2708.0585189571402,2.6826168024752337,2.1945076246192411E-2,5.5839311713868023,-48993.767926288187,1372.3579134730871]
["AKM2G","AKM2G-41G 120 V",2.8599998950958301,4.5300002098083496,2.7876904761904799,4.3557664664065898,2100,7.2600002288818404,2100,2.4900000095367401,14.8999996185303,42.200000762939503,7.7400000009220093E-2,168,10,2100,2100,2100,2.7876904761904799,32.299741598219555,1.5522026912956677,1.7302980693404648,1.1428571428571428,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.5827709543287215,0.82904579489775865,6.9932514519446585,19.897099077546208,12.66688668552268,208.76529917876999,169.23394839668893,1628.0305835761476,7.8171106742660409E-3,2.0928652849103586,-50190.269703509774,2403.5526161282573,2.573791560628016E-3,0.75854305266650324,-50724.385261401418,4294.4597042930209,4.167808923408538,9.1052188079623758E-3,2.3053789343008289,-50059.055375420445,2221.5662868235299]
["AKM2G","AKM2G-41G 240 V",2.8599998950958301,4.5300002098083496,2.56788888888889,4.0123264785713699,4500,7.2600002288818404,4500,2.4900000095367401,14.8999996185303,42.200000762939503,7.7400000009220093E-2,336,10,2403.5526161282573,4342.4692297688325,4500,2.5781147715112858,32.299741598219555,1.5597500211110806,1.7302980693404648,1.0803188787274949,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.5827709543287215,0.82904579489775865,6.9932514519446585,19.897099077546208,12.66688668552268,208.76529917876999,169.23394839668893,1628.0305835761476,7.8171106742660409E-3,2.0928652849103586,-50190.269703509774,2403.5526161282573,2.521414770991489E-3,0.7330631035990991,-50729.720671589319,4342.4692297688325,4.0278095407527834,9.1052188079623758E-3,2.3053789343008289,-50059.055375420445,2221.5662868235299]
["AKM2G","AKM2G-41G 400 V",2.8599998950958301,4.5300002098083496,2.2760833333333301,3.5563802878246298,6000,7.2600002288818404,6000,2.4900000095367401,14.8999996185303,42.200000762939503,7.7400000009220093E-2,560,10,2403.5526161282573,4413.141218052052,5341.2321309232939,2.4305155206596094,32.299741598219555,1.5678550093537611,1.7302980693404648,1.0803188787274949,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.5827709543287215,0.82904579489775865,6.9932514519446585,19.897099077546208,12.66688668552268,208.76529917876999,169.23394839668893,1628.0305835761476,7.8171106742660409E-3,2.0928652849103586,-50190.269703509774,2403.5526161282573,2.4475350806106716E-3,0.69553746467450117,-50737.246494677587,4413.141218052052,3.8216252085428248,9.1052188079623758E-3,2.3053789343008289,-50059.055375420445,2221.5662868235299]
["AKM2G","AKM2G-41G 480 V",2.8599998950958301,4.5300002098083496,2.1805833333333302,3.40716153448933,6000,7.2600002288818404,6000,2.4900000095367401,14.8999996185303,42.200000762939503,7.7400000009220093E-2,672,10,2403.5526161282573,4450.2703114014312,5341.2321309232939,2.3560686694481485,32.299741598219555,1.5718668305999546,1.7302980693404648,1.0803188787274949,12.56196437944558,0,-10.175191147350921,0,0,0,0,0,0.5827709543287215,0.82904579489775865,6.9932514519446585,19.897099077546208,12.66688668552268,208.76529917876999,169.23394839668893,1628.0305835761476,7.8171106742660409E-3,2.0928652849103586,-50190.269703509774,2403.5526161282573,2.4101934547379475E-3,0.67577825285448034,-50741.050333983061,4450.2703114014312,3.713058372351381,9.1052188079623758E-3,2.3053789343008289,-50059.055375420445,2221.5662868235299]
["AKM2G","AKM2G-42D 240 V",5.03999996185303,2.2699999809265101,4.9341666666666697,2.20275296681231,1200,14.3999996185303,1200,12.199999809265099,81.900001525878906,149,0.136000002385117,336,10,641.49228058379038,1200,1200,4.9341666666666697,18.382352618793664,0.90307812075056182,0.89219268694727083,2.4872028287036643,12.847574351696224,0,-10.406535224873942,0,0,0,0,0,0.16948239625443118,0.24110444571792367,2.0337887550531741,5.786506697230168,3.6838045763941549,213.51180613455372,173.08166694177032,1665.0456359798304,8.0216218155620675E-2,20.420412964646264,-46109.501407518881,641.49228058379038,2.8918177852600702E-2,6.9484346845559521,-50261.482411540695,1203.6776160642471,2.2068878305058646,4.0917278282676925E-2,11.598539416421453,-49290.294491753957,964.93939790623563]
["AKM2G","AKM2G-42D 400 V",5.03999996185303,2.2699999809265101,4.7750000000000004,2.1316964194957899,2100,14.3999996185303,2100,12.199999809265099,81.900001525878906,149,0.136000002385117,560,10,641.49228058379038,1205.5702516105109,1512.7516778523491,4.8878684996206809,18.382352618793664,0.90618758845794867,0.89219268694727083,2.4872028287036643,12.847574351696224,0,-10.406535224873942,0,0,0,0,0,0.16948239625443118,0.24110444571792367,2.0337887550531741,5.786506697230168,3.6838045763941549,213.51180613455372,173.08166694177032,1665.0456359798304,8.0216218155620675E-2,20.420412964646264,-46109.501407518881,641.49228058379038,2.8851024956837629E-2,6.9136150343098581,-50266.917659084786,1205.5702516105109,2.1958287839897661,4.0917278282676925E-2,11.598539416421453,-49290.294491753957,964.93939790623563]
["AKM2G","AKM2G-42D 480 V",5.03999996185303,2.2699999809265101,4.7015384615384601,2.09890108996508,2600,14.3999996185303,2600,12.199999809265099,81.900001525878906,149,0.136000002385117,672,10,641.49228058379038,1205.5603107767809,1512.7516778523491,4.8830631343510271,18.382352618793664,0.90651511628520809,0.89219268694727083,2.4872028287036643,12.847574351696224,0,-10.406535224873942,0,0,0,0,0,0.16948239625443118,0.24110444571792367,2.0337887550531741,5.786506697230168,3.6838045763941549,213.51180613455372,173.08166694177032,1665.0456359798304,8.0216218155620675E-2,20.420412964646264,-46109.501407518881,641.49228058379038,2.8851376763727763E-2,6.9137979077015341,-50266.889184400054,1205.5603107767809,2.1958868662890083,4.0917278282676925E-2,11.598539416421453,-49290.294491753957,964.93939790623563]
["AKM2G","AKM2G-42E 240 V",5.0799999237060502,2.8800001144409202,4.9540625,2.7989053973925899,1600,14.3999996185303,1600,7.5199999809265101,51.400001525878899,118,0.136000002385117,336,10,861.13749011893913,1551.0669322729254,1600,4.9579140653022389,18.382352618793664,0.89515052716749843,0.89219268694727083,1.8992036559169507,12.847574351696224,0,-10.406535224873942,0,0,0,0,0,0.2133330166554486,0.3034860249251386,2.5599961998653833,7.2836645982033259,4.6369248985100127,213.51180613455372,173.08166694177032,1665.0456359798304,5.0128898266617455E-2,12.547342531110361,-47978.461411357894,861.13749011893913,1.819916334133815E-2,4.3116593812526283,-50471.376485565503,1551.0669322729254,2.8053300923346303,2.560405521131303E-2,7.1267337820435595,-49893.239316286257,1263.6875421563259]
["AKM2G","AKM2G-42E 400 V",5.0799999237060502,2.8800001144409202,4.7042592592592598,2.6577736214419598,2700,14.3999996185303,2700,7.5199999809265101,51.400001525878899,118,0.136000002385117,560,10,861.13749011893913,1558.6967349140612,1910.1694915254236,4.8630866841328455,18.382352618793664,0.9000209411379565,0.89219268694727083,1.8992036559169507,12.847574351696224,0,-10.406535224873942,0,0,0,0,0,0.2133330166554486,0.3034860249251386,2.5599961998653833,7.2836645982033259,4.6369248985100127,213.51180613455372,173.08166694177032,1665.0456359798304,5.0128898266617455E-2,12.547342531110361,-47978.461411357894,861.13749011893913,1.805835141717016E-2,4.240057855435448,-50482.370381042812,1558.6967349140612,2.758743407888872,2.560405521131303E-2,7.1267337820435595,-49893.239316286257,1263.6875421563259]
["AKM2G","AKM2G-42E 480 V",5.0799999237060502,2.8800001144409202,4.5724242424242396,2.5832905602805698,3300,14.3999996185303,3300,7.5199999809265101,51.400001525878899,118,0.136000002385117,672,10,861.13749011893913,1560.5312801247749,1910.1694915254236,4.8399733395633504,18.382352618793664,0.90120903005980724,0.89219268694727083,1.8992036559169507,12.847574351696224,0,-10.406535224873942,0,0,0,0,0,0.2133330166554486,0.3034860249251386,2.5599961998653833,7.2836645982033259,4.6369248985100127,213.51180613455372,173.08166694177032,1665.0456359798304,5.0128898266617455E-2,12.547342531110361,-47978.461411357894,861.13749011893913,1.8024834334116238E-2,4.2228358585842614,-50484.987228372862,1560.5312801247749,2.7475381196820168,2.560405521131303E-2,7.1267337820435595,-49893.239316286257,1263.6875421563259]
["AKM2G","AKM2G-42H 120 V",5.1199998855590803,5.6399998664856001,5.0296666666666701,5.5089449451974604,1500,14.3999996185303,1500,1.9400000572204601,13.6000003814697,60.799999237060497,0.136000002385117,168,10,1500,1500,1500,5.0296666666666701,18.382352618793664,0.88665238553419101,0.89219268694727083,1.6,12.847574351696224,0,-10.406535224873942,0,0,0,0,0,0.41451325032881398,0.58968358762894613,4.9741590039457675,14.152406103094707,9.0097015518057226,213.51180613455372,173.08166694177032,1665.0456359798304,1.3265927240393396E-2,3.2406905816414691,-50094.915310937293,1824.9385620545554,4.7952892227524201E-3,1.0980631420162494,-50723.616849049766,3139.8739249870669,5.3747883875357472,6.7837858387306367E-3,1.8406717588262766,-50576.028098545568,2598.1643241137845]
["AKM2G","AKM2G-42H 240 V",5.1199998855590803,5.6399998664856001,4.6556249999999997,5.0992607483235997,3200,14.3999996185303,3200,1.9400000572204601,13.6000003814697,60.799999237060497,0.136000002385117,336,10,1824.9385620545554,3177.0462434883079,3200,4.6589559837666457,18.382352618793664,0.89337711122786845,0.89219268694727083,0.9237291027843757,12.847574351696224,0,-10.406535224873942,0,0,0,0,0,0.41451325032881398,0.58968358762894613,4.9741590039457675,14.152406103094707,9.0097015518057226,213.51180613455372,173.08166694177032,1665.0456359798304,1.3265927240393396E-2,3.2406905816414691,-50094.915310937293,1824.9385620545554,4.6963471281071742E-3,1.0474521291313432,-50730.96045728305,3177.0462434883079,5.1270581123570995,6.7837858387306367E-3,1.8406717588262766,-50576.028098545568,2598.1643241137845]
["AKM2G","AKM2G-42H 400 V",5.1199998855590803,5.6399998664856001,3.8711607142857098,4.2400446515364703,5600,14.3999996185303,5600,1.9400000572204601,13.6000003814697,60.799999237060497,0.136000002385117,560,10,1824.9385620545554,3213.5881755627288,3707.2368886249583,4.4033472437762837,18.382352618793664,0.89963729851920249,0.89219268694727083,0.9237291027843757,12.847574351696224,0,-10.406535224873942,0,0,0,0,0,0.41451325032881398,0.58968358762894613,4.9741590039457675,14.152406103094707,9.0097015518057226,213.51180613455372,173.08166694177032,1665.0456359798304,1.3265927240393396E-2,3.2406905816414691,-50094.915310937293,1824.9385620545554,4.6027490295536579E-3,0.9972132049320005,-50737.907427322672,3213.5881755627288,4.8811491331219869,6.7837858387306367E-3,1.8406717588262766,-50576.028098545568,2598.1643241137845]
["AKM2G","AKM2G-42H 480 V",5.1199998855590803,5.6399998664856001,3.5494166666666702,3.8876415277817502,6000,14.3999996185303,6000,1.9400000572204601,13.6000003814697,60.799999237060497,0.136000002385117,672,10,1824.9385620545554,3232.3929327705455,3707.2368886249583,4.2738762027131072,18.382352618793664,0.90278508163385796,0.89219268694727083,0.9237291027843757,12.847574351696224,0,-10.406535224873942,0,0,0,0,0,0.41451325032881398,0.58968358762894613,4.9741590039457675,14.152406103094707,9.0097015518057226,213.51180613455372,173.08166694177032,1665.0456359798304,1.3265927240393396E-2,3.2406905816414691,-50094.915310937293,1824.9385620545554,4.5559594291496837E-3,0.97112494183212617,-50741.38021103511,3232.3929327705455,4.7534525661443237,6.7837858387306367E-3,1.8406717588262766,-50576.028098545568,2598.1643241137845]
["AKM2G","AKM2G-43D 400 V",6.9699997901916504,2.3299999237060498,6.6849999999999996,2.2209302395948298,1600,21.100000381469702,1600,13.199999809265099,95.5,202,0.19500000053085401,560,10,466.01341805620171,897.69811909803468,1115.841584158416,6.8100974304426636,12.820512785611177,0.6700882902498223,0.62251818113285518,2.8632897878118131,13.135133859375069,0,-10.639458426093805,0,0,0,0,0,0.12860734729717863,0.18295589318190361,1.5432881675661436,4.3909414363656865,2.7953601376985042,218.29071211127351,176.95564949844169,1702.313348175009,0.13410288659956074,32.57553272315932,-44303.55885674429,466.01341805620171,5.0504642579030437E-2,10.503971815624251,-50129.163627687063,897.69811909803468,2.2744040815107138,5.5457480364477001E-2,12.909924115771641,-49784.021504540106,838.19668208788994]
["AKM2G","AKM2G-43D 480 V",6.9699997901916504,2.3299999237060498,6.58447368421053,2.1875327923828798,1900,21.100000381469702,1900,13.199999809265099,95.5,202,0.19500000053085401,672,10,466.01341805620171,898.33604969208886,1115.841584158416,6.7877197906652009,12.820512785611177,0.67117853870623112,0.62251818113285518,2.8632897878118131,13.135133859375069,0,-10.639458426093805,0,0,0,0,0,0.12860734729717863,0.18295589318190361,1.5432881675661436,4.3909414363656865,2.7953601376985042,218.29071211127351,176.95564949844169,1702.313348175009,0.13410288659956074,32.57553272315932,-44303.55885674429,466.01341805620171,5.0457294564459548E-2,10.478305960842087,-50132.463108708595,898.33604969208886,2.2688467051299832,5.5457480364477001E-2,12.909924115771641,-49784.021504540106,838.19668208788994]
["AKM2G","AKM2G-43G 240 V",6.9699997901916504,4.5199999809265101,6.6347368421052604,4.2804755136866097,1900,21.100000381469702,1900,3.46000003814697,25.299999237060501,104,0.19500000053085401,336,10,1062.9064559570616,1856.2647950438316,1900,6.6424541019730325,12.820512785611177,0.67001492302177379,0.62251818113285518,1.3764651070410712,13.135133859375069,0,-10.639458426093805,0,0,0,0,0,0.24948722161571771,0.3549187385282187,2.9938466593886126,8.5180497246772493,5.4227588767397688,218.29071211127351,176.95564949844169,1702.313348175009,3.5457990532328634E-2,8.5282161933330514,-49124.07476885568,1062.9064559570616,1.3251768318009475E-2,2.6812560952906832,-50638.991031607497,1856.2647950438316,4.3019784107248418,1.468625973800641E-2,3.3797950392550549,-50541.129524145414,1743.5966867036525]
["AKM2G","AKM2G-43G 400 V",6.9699997901916504,4.5199999809265101,6.1179687500000002,3.9470767343298601,3200,21.100000381469702,3200,3.46000003814697,25.299999237060501,104,0.19500000053085401,560,10,1062.9064559570616,1865.3155257929538,2167.3076923076924,6.4733414377769609,12.820512785611177,0.67398159592890838,0.62251818113285518,1.3764651070410712,13.135133859375069,0,-10.639458426093805,0,0,0,0,0,0.24948722161571771,0.3549187385282187,2.9938466593886126,8.5180497246772493,5.4227588767397688,218.29071211127351,176.95564949844169,1702.313348175009,3.5457990532328634E-2,8.5282161933330514,-49124.07476885568,1062.9064559570616,1.3149130722638978E-2,2.6241571790410112,-50645.993004338197,1865.3155257929538,4.2103652651497843,1.468625973800641E-2,3.3797950392550549,-50541.129524145414,1743.5966867036525]
["AKM2G","AKM2G-43G 480 V",6.9699997901916504,4.5199999809265101,5.7544871794871799,3.7125724880751201,3900,21.100000381469702,3900,3.46000003814697,25.299999237060501,104,0.19500000053085401,672,10,1062.9064559570616,1870.0822402140645,2167.3076923076924,6.3871514450545579,12.820512785611177,0.67600527854238368,0.62251818113285518,1.3764651070410712,13.135133859375069,0,-10.639458426093805,0,0,0,0,0,0.24948722161571771,0.3549187385282187,2.9938466593886126,8.5180497246772493,5.4227588767397688,218.29071211127351,176.95564949844169,1702.313348175009,3.5457990532328634E-2,8.5282161933330514,-49124.07476885568,1062.9064559570616,1.3095782981820885E-2,2.5939826195416931,-50649.63240591521,1870.0822402140645,4.1619512759947774,1.468625973800641E-2,3.3797950392550549,-50541.129524145414,1743.5966867036525]
["AKM2G","AKM2G-43I 120 V",6.9800000190734899,7.1399998664856001,6.8214285714285703,6.93939848127778,1400,21.100000381469702,1400,1.3600000143051101,10.199999809265099,65.900001525878906,0.19500000053085401,168,10,1400,1400,1400,6.8214285714285703,12.820512785611177,0.66628873915689857,0.62251818113285518,1.7142857142857142,13.135133859375069,0,-10.639458426093805,0,0,0,0,0,0.39353686214839967,0.55984272770972277,4.722442345780796,13.436225465033347,8.553766797029029,218.29071211127351,176.95564949844169,1702.313348175009,1.4308544895207444E-2,3.3505045183414399,-50158.926339791062,1758.8806397359813,5.3134714965083329E-3,1.0456573720669962,-50742.216923447959,2993.4330130409689,6.7360366075414833,5.9080239242317277E-3,1.3278296766145088,-50703.662837537828,2819.3134280234403]
["AKM2G","AKM2G-43I 240 V",6.9800000190734899,7.1399998664856001,6.2074999999999996,6.3148526179627797,3000,21.100000381469702,3000,1.3600000143051101,10.199999809265099,65.900001525878906,0.19500000053085401,336,10,1758.8806397359813,3000,3000,6.2074999999999996,12.820512785611177,0.67261121462131612,0.62251818113285518,0.85127108470610457,13.135133859375069,0,-10.639458426093805,0,0,0,0,0,0.39353686214839967,0.55984272770972277,4.722442345780796,13.436225465033347,8.553766797029029,218.29071211127351,176.95564949844169,1702.313348175009,1.4308544895207444E-2,3.3505045183414399,-50158.926339791062,1758.8806397359813,5.2093650967359418E-3,0.98799236254095868,-50748.967761378248,3027.8089295123791,6.3645634792319843,5.9080239242317277E-3,1.3278296766145088,-50703.662837537828,2819.3134280234403]
["AKM2G","AKM2G-43I 400 V",6.9800000190734899,7.1399998664856001,4.8290566037735898,4.9125703965573999,5300,21.100000381469702,5300,1.3600000143051101,10.199999809265099,65.900001525878906,0.19500000053085401,560,10,1758.8806397359813,3064.9458979954111,3420.3337599542469,5.7361273402916657,12.820512785611177,0.67923996567656231,0.62251818113285518,0.85127108470610457,13.135133859375069,0,-10.639458426093805,0,0,0,0,0,0.39353686214839967,0.55984272770972277,4.722442345780796,13.436225465033347,8.553766797029029,218.29071211127351,176.95564949844169,1702.313348175009,1.4308544895207444E-2,3.3505045183414399,-50158.926339791062,1758.8806397359813,5.1014645467131973E-3,0.9244374314616558,-50755.964633111253,3064.9458979954111,5.9551479729904901,5.9080239242317277E-3,1.3278296766145088,-50703.662837537828,2819.3134280234403]
["AKM2G","AKM2G-43I 480 V",6.9800000190734899,7.1399998664856001,4.0269166666666703,4.0965582367809796,6000,21.100000381469702,6000,1.3600000143051101,10.199999809265099,65.900001525878906,0.19500000053085401,672,10,1758.8806397359813,3086.7504799239268,3420.3337599542469,5.4607614431906377,12.820512785611177,0.68315881685441837,0.62251818113285518,0.85127108470610457,13.135133859375069,0,-10.639458426093805,0,0,0,0,0,0.39353686214839967,0.55984272770972277,4.722442345780796,13.436225465033347,8.553766797029029,218.29071211127351,176.95564949844169,1702.313348175009,1.4308544895207444E-2,3.3505045183414399,-50158.926339791062,1758.8806397359813,5.0402780411620334E-3,0.88637529094606859,-50759.932306408955,3086.7504799239268,5.709954873679604,5.9080239242317277E-3,1.3278296766145088,-50703.662837537828,2819.3134280234403]
["AKM2G","AKM2G-44E 240 V",8.4799995422363299,2.9900000095367401,8.3085000000000004,2.9152632554460198,900,26.899999618530298,900,8.4499998092651403,63.599998474121101,192,0.25300000561401198,336,10,533.36238482580848,900,900,8.3085000000000004,9.8814227056346819,0.56182985372718153,0.49880370635802251,2.6666666666666665,13.417819510752304,0,-10.868433803709365,0,0,0,0,0,0.138568795590604,0.19712697833536411,1.6628255470872482,4.7310474800487388,3.0118783698088478,222.98862024098261,180.76397178726594,1738.9494085934984,0.11168577175787631,26.65300556356134,-45987.568952018017,533.36238482580848,4.3937898272345552E-2,8.1952385747743275,-50349.688976118516,981.27581025241648,2.9163728451799336,4.440879731990028E-2,8.4636166598454921,-50319.368937141837,973.43385254629186]
["AKM2G","AKM2G-44E 400 V",8.4799995422363299,2.9900000095367401,7.9770588235294104,2.7989681019157202,1700,26.899999618530298,1700,8.4499998092651403,63.599998474121101,192,0.25300000561401198,560,10,533.36238482580848,983.40675609948698,1173.9583333333335,8.1890611300634379,9.8814227056346819,0.56503034887263925,0.49880370635802251,2.4654988047951285,13.417819510752304,0,-10.868433803709365,0,0,0,0,0,0.138568795590604,0.19712697833536411,1.6628255470872482,4.7310474800487388,3.0118783698088478,222.98862024098261,180.76397178726594,1738.9494085934984,0.11168577175787631,26.65300556356134,-45987.568952018017,533.36238482580848,4.3812302095441132E-2,8.1221600302496686,-50357.775807040845,983.40675609948698,2.8903669783741757,4.440879731990028E-2,8.4636166598454921,-50319.368937141837,973.43385254629186]
["AKM2G","AKM2G-44E 480 V",8.4799995422363299,2.9900000095367401,7.8219047619047597,2.7445280784713502,2100,26.899999618530298,2100,8.4499998092651403,63.599998474121101,192,0.25300000561401198,672,10,533.36238482580848,983.73493555202708,1173.9583333333335,8.1717181963712804,9.8814227056346819,0.56556676941432427,0.49880370635802251,2.4654988047951285,13.417819510752304,0,-10.868433803709365,0,0,0,0,0,0.138568795590604,0.19712697833536411,1.6628255470872482,4.7310474800487388,3.0118783698088478,222.98862024098261,180.76397178726594,1738.9494085934984,0.11168577175787631,26.65300556356134,-45987.568952018017,533.36238482580848,4.3793048621970122E-2,8.1108991300006945,-50359.015491149592,983.73493555202708,2.8863596534624305,4.440879731990028E-2,8.4636166598454921,-50319.368937141837,973.43385254629186]
["AKM2G","AKM2G-44H 120 V",8.5100002288818395,5.8699998855590803,8.3827777777777808,5.7416284648986498,900,27,900,2.1800000667571999,16.700000762939499,98.5,0.25300000561401198,168,10,900,900,900,8.3827777777777808,9.8814227056346819,0.55835650661852732,0.49695627817601129,2.6666666666666665,13.417819510752304,0,-10.868433803709365,0,0,0,0,0,0.27108070242189669,0.38563747000684728,3.2529684290627601,9.2552992801643352,5.8921065209320593,222.98862024098261,180.76397178726594,1738.9494085934984,2.9592308494454725E-2,6.926688380540571,-49568.874295108981,1182.4864178112657,1.1504063144886004E-2,2.0847908641487178,-50693.166572000366,2010.5207473220221,5.6054325420823412,1.1693073090853604E-2,2.1914115910254051,-50681.418477124367,1990.3030912673385]
["AKM2G","AKM2G-44H 240 V",8.5100002288818395,5.8699998855590803,7.9264999999999999,5.4291094471889796,2000,27,2000,2.1800000667571999,16.700000762939499,98.5,0.25300000561401198,336,10,1182.4864178112657,2000,2000,7.9264999999999999,9.8814227056346819,0.5628823223518622,0.49695627817601129,1.205846491687748,13.417819510752304,0,-10.868433803709365,0,0,0,0,0,0.27108070242189669,0.38563747000684728,3.2529684290627601,9.2552992801643352,5.8921065209320593,222.98862024098261,180.76397178726594,1738.9494085934984,2.9592308494454725E-2,6.926688380540571,-49568.874295108981,1182.4864178112657,1.1412472566214161E-2,2.0311122995441666,-50698.859472458462,2020.59320802551,5.4611055604071392,1.1693073090853604E-2,2.1914115910254051,-50681.418477124367,1990.3030912673385]
["AKM2G","AKM2G-44H 400 V",8.5100002288818395,5.8699998855590803,6.9851428571428604,4.7843442976949397,3500,27,3500,2.1800000667571999,16.700000762939499,98.5,0.25300000561401198,560,10,1182.4864178112657,2032.1120474274421,2288.3248730964469,7.6246627901048898,9.8814227056346819,0.56728272131836077,0.49695627817601129,1.205846491687748,13.417819510752304,0,-10.868433803709365,0,0,0,0,0,0.27108070242189669,0.38563747000684728,3.2529684290627601,9.2552992801643352,5.8921065209320593,222.98862024098261,180.76397178726594,1738.9494085934984,2.9592308494454725E-2,6.926688380540571,-49568.874295108981,1182.4864178112657,1.130980367505041E-2,1.9692024211725638,-50705.240956078444,2032.1120474274421,5.2946468268870053,1.1693073090853604E-2,2.1914115910254051,-50681.418477124367,1990.3030912673385]
["AKM2G","AKM2G-44H 480 V",8.5100002288818395,5.8699998855590803,6.3296511627907002,4.3353773954857404,4300,27,4300,2.1800000667571999,16.700000762939499,98.5,0.25300000561401198,672,10,1182.4864178112657,2038.0619868538561,2288.3248730964469,7.47658475221378,9.8814227056346819,0.56949089380768925,0.49695627817601129,1.205846491687748,13.417819510752304,0,-10.868433803709365,0,0,0,0,0,0.27108070242189669,0.38563747000684728,3.2529684290627601,9.2552992801643352,5.8921065209320593,222.98862024098261,180.76397178726594,1738.9494085934984,2.9592308494454725E-2,6.926688380540571,-49568.874295108981,1182.4864178112657,1.125763213056127E-2,1.9369846198943061,-50708.483728575666,2038.0619868538561,5.2080219692933252,1.1693073090853604E-2,2.1914115910254051,-50681.418477124367,1990.3030912673385]
["AKM2G","AKM2G-44J 120 V",8.4700002670288104,7.3000001907348597,8.2766666666666708,7.0740743335495804,1200,26.899999618530298,1200,1.3899999856948899,10.699999809265099,78.800003051757798,0.25300000561401198,168,10,1200,1200,1200,8.2766666666666708,9.8814227056346819,0.56160930970269451,0.49880370635802251,2,13.417819510752304,0,-10.868433803709365,0,0,0,0,0,0.3387111775782386,0.48184810064798284,4.0645341309388634,11.564354415551588,7.3620966756064865,222.98862024098261,180.76397178726594,1738.9494085934984,1.8862906131610895E-2,4.398386390864478,-50026.27328296523,1516.1060566927617,7.31635271389856E-3,1.3009039340100121,-50737.023786652244,2545.986393240998,6.8571487340006421,7.4853770363949128E-3,1.396700129949028,-50726.619459230584,2511.5974827681471]
["AKM2G","AKM2G-44J 240 V",8.4700002670288104,7.3000001907348597,7.5665384615384603,6.46712712741662,2600,26.899999618530298,2600,1.3899999856948899,10.699999809265099,78.800003051757798,0.25300000561401198,336,10,1516.1060566927617,2566.7332708890704,2600,7.5780981612097369,9.8814227056346819,0.5672948511276763,0.49880370635802251,0.95556713066731125,13.417819510752304,0,-10.868433803709365,0,0,0,0,0,0.3387111775782386,0.48184810064798284,4.0645341309388634,11.564354415551588,7.3620966756064865,222.98862024098261,180.76397178726594,1738.9494085934984,1.8862906131610895E-2,4.398386390864478,-50026.27328296523,1516.1060566927617,7.2183342300943193E-3,1.2419706967008428,-50743.057334864796,2566.7332708890704,6.5465078303641562,7.4853770363949128E-3,1.396700129949028,-50726.619459230584,2511.5974827681471]
["AKM2G","AKM2G-44J 400 V",8.4700002670288104,7.3000001907348597,6.0271111111111102,5.1513772069950798,4500,26.899999618530298,4500,1.3899999856948899,10.699999809265099,78.800003051757798,0.25300000561401198,560,10,1516.1060566927617,2590.9504554731602,2860.4059805930679,7.0634658734298306,9.8814227056346819,0.57338001921028414,0.49880370635802251,0.95556713066731125,13.417819510752304,0,-10.868433803709365,0,0,0,0,0,0.3387111775782386,0.48184810064798284,4.0645341309388634,11.564354415551588,7.3620966756064865,222.98862024098267,180.76397178726594,1738.9494085934984,1.8862906131610895E-2,4.398386390864478,-50026.27328296523,1516.1060566927617,7.1076264117214353E-3,1.1718492798996751,-50749.871977713105,2590.9504554731602,6.1768933093577516,7.4853770363949128E-3,1.396700129949028,-50726.619459230584,2511.5974827681471]
["AKM2G","AKM2G-44J 480 V",8.4700002670288104,7.3000001907348597,4.9164814814814797,4.2021210784760301,5400,26.899999618530298,5400,1.3899999856948899,10.699999809265099,78.800003051757798,0.25300000561401198,672,10,1516.1060566927617,2605.5003233019543,2860.4059805930679,6.7554272402504516,9.8814227056346819,0.57702937904444207,0.49880370635802251,0.95556713066731125,13.417819510752304,0,-10.868433803709365,0,0,0,0,0,0.3387111775782386,0.48184810064798284,4.0645341309388634,11.564354415551588,7.3620966756064865,222.98862024098261,180.76397178726594,1738.9494085934984,1.8862906131610895E-2,4.398386390864478,-50026.27328296523,1516.1060566927617,7.0430181200273907E-3,1.1289160864040646,-50753.848954582536,2605.5003233019543,5.9505896709964228,7.4853770363949128E-3,1.396700129949028,-50726.619459230584,2511.5974827681471]
["AKM2G","AKM2G-51H 120 V",6.8200001716613796,5.7800002098083496,6.7718181818181797,5.6906032405035702,1100,15.699999809265099,1100,2.3099999427795401,20.799999237060501,80.199996948242202,0.251999997999519,168,10,1100,1100,1100,6.7718181818181797,9.9206349993890548,0.69325101396067079,0.8543277545526361,2.1818181818181817,13.412945583526268,0,-10.864485922656275,0,0,0,0,0,0.33294750659494515,0.4736487434968053,3.9953700791393416,11.367569843923327,7.2368197264110501,222.90762121529011,180.69831056392974,1738.3177476250039,2.2181706573483215E-2,4.2696282565670671,-50096.608481483898,1409.6554904426634,9.2172038385906208E-3,1.7954767564862169,-50679.860055176105,2249.4902241792497,5.5954219095342888,1.1090910179380083E-2,2.322173701952968,-50595.565100386877,2033.7351900887911]
["AKM2G","AKM2G-51H 240 V",6.8200001716613796,5.7800002098083496,6.44625,5.4170165462486004,2400,15.699999809265099,2400,2.3099999427795401,20.799999237060501,80.199996948242202,0.251999997999519,336,10,1409.6554904426634,2270.8214098616763,2400,6.4663668834329888,9.9206349993890548,0.698442105117974,0.8543277545526361,1.1800946414735627,13.412945583526268,0,-10.864485922656275,0,0,0,0,0,0.33294750659494515,0.4736487434968053,3.9953700791393416,11.367569843923327,7.2368197264110501,222.90762121529011,180.69831056392974,1738.3177476250039,2.2181706573483215E-2,4.2696282565670671,-50096.608481483898,1409.6554904426634,9.0612418576345184E-3,1.7444815510013783,-50686.876527206608,2270.8214098616763,5.4365005038294978,1.1090910179380083E-2,2.322173701952968,-50595.565100386877,2033.7351900887911]
["AKM2G","AKM2G-51H 400 V",6.8200001716613796,5.7800002098083496,5.8891666666666698,4.9488793138567404,4200,15.699999809265099,4200,2.3099999427795401,20.799999237060501,80.199996948242202,0.251999997999519,560,10,1409.6554904426634,2285.0460325673534,2810.4739224050591,6.3135722174783018,9.9206349993890548,0.70153490432769927,0.8543277545526361,1.1800946414735627,13.412945583526268,0,-10.864485922656275,0,0,0,0,0,0.33294750659494515,0.4736487434968053,3.9953700791393416,11.367569843923327,7.2368197264110501,222.90762121529011,180.69831056392974,1738.3177476250039,2.2181706573483215E-2,4.2696282565670671,-50096.608481483898,1409.6554904426634,8.9597766601079293E-3,1.7104891780308069,-50691.441278924627,2285.0460325673534,5.3305667078115393,1.1090910179380083E-2,2.322173701952968,-50595.565100386877,2033.7351900887911]
["AKM2G","AKM2G-51H 480 V",6.8200001716613796,5.7800002098083496,5.5427450980392203,4.6577687659828104,5100,15.699999809265099,5100,2.3099999427795401,20.799999237060501,80.199996948242202,0.251999997999519,672,10,1409.6554904426634,2291.8034617009139,2810.4739224050591,6.2460359365236702,9.9206349993890548,0.70289591751717451,0.8543277545526361,1.1800946414735627,13.412945583526268,0,-10.864485922656275,0,0,0,0,0,0.33294750659494515,0.4736487434968053,3.9953700791393416,11.367569843923327,7.2368197264110501,222.90762121529011,180.69831056392974,1738.3177476250039,2.2181706573483215E-2,4.2696282565670671,-50096.608481483898,1409.6554904426634,8.9122712496470281E-3,1.6943397730240946,-50693.578468909989,2291.8034617009139,5.2802387187278255,1.1090910179380083E-2,2.322173701952968,-50595.565100386877,2033.7351900887911]
["AKM2G","AKM2G-51I 120 V",6.8299999237060502,6.3499999046325701,6.7645833333333298,6.2635028375305097,1200,15.699999809265099,1200,1.9099999666214,17.200000762939499,73.099998474121094,0.251999997999519,168,10,1200,1200,1200,6.7645833333333298,9.9206349993890548,0.69272510580825775,0.8543277545526361,2,13.412945583526268,0,-10.864485922656275,0,0,0,0,0,0.3652458736430802,0.51959616964154898,4.3829504837169626,12.470308071397175,7.9388446857664823,222.90762121529011,180.69831056392974,1738.3177476250039,1.8304080474469298E-2,3.5299131650123341,-50222.207301696988,1562.8131839879236,7.6587164458263492E-3,1.4918980205618062,-50701.028158572735,2477.388473614883,6.1691848418729176,9.17741505967333E-3,1.9198560224444332,-50632.718181604207,2246.5817929166683]
["AKM2G","AKM2G-51I 240 V",6.8299999237060502,6.3499999046325701,6.3666666666666698,5.8950614941463604,2700,15.699999809265099,2700,1.9099999666214,17.200000762939499,73.099998474121094,0.251999997999519,336,10,1562.8131839879236,2509.5303288480336,2700,6.3993521974452108,9.9206349993890548,0.69814928784932739,0.8543277545526361,1.0682896156138404,13.412945583526268,0,-10.864485922656275,0,0,0,0,0,0.3652458736430802,0.51959616964154898,4.3829504837169626,12.470308071397175,7.9388446857664823,222.90762121529011,180.69831056392974,1738.3177476250039,1.8304080474469298E-2,3.5299131650123341,-50222.207301696988,1562.8131839879236,7.4807517357195945E-3,1.4334096378278345,-50709.032883893327,2509.5303288480336,5.927328066667731,9.17741505967333E-3,1.9198560224444332,-50632.718181604207,2246.5817929166683]
["AKM2G","AKM2G-51I 400 V",6.8299999237060502,6.3499999046325701,5.7507608695652204,5.3247783713430801,4600,15.699999809265099,4600,1.9099999666214,17.200000762939499,73.099998474121094,0.251999997999519,560,10,1562.8131839879236,2527.6559628862419,3083.4473967847789,6.2369683953193595,9.9206349993890548,0.70110360328134758,0.8543277545526361,1.0682896156138404,13.412945583526268,0,-10.864485922656275,0,0,0,0,0,0.3652458736430802,0.51959616964154898,4.3829504837169626,12.470308071397175,7.9388446857664823,222.90762121529011,180.69831056392974,1738.3177476250039,1.8304080474469298E-2,3.5299131650123341,-50222.207301696988,1562.8131839879236,7.3835172975599411E-3,1.4004218373676343,-50713.406419347084,2527.6559628862419,5.7909193874141982,9.17741505967333E-3,1.9198560224444332,-50632.718181604207,2246.5817929166683]
["AKM2G","AKM2G-51I 480 V",6.8299999237060502,6.3499999046325701,5.29438596491228,4.9022090319743503,5700,15.699999809265099,5700,1.9099999666214,17.200000762939499,73.099998474121094,0.251999997999519,672,10,1562.8131839879236,2538.0239803967056,3083.4473967847789,6.1462411426445573,9.9206349993890548,0.70274540426865029,0.8543277545526361,1.0682896156138404,13.412945583526268,0,-10.864485922656275,0,0,0,0,0,0.3652458736430802,0.51959616964154898,4.3829504837169626,12.470308071397175,7.9388446857664823,222.90762121529011,180.69831056392974,1738.3177476250039,1.8304080474469298E-2,3.5299131650123341,-50222.207301696988,1562.8131839879236,7.3288827440322248E-3,1.3815409084188608,-50715.863842471816,2538.0239803967056,5.7128443855937716,9.17741505967333E-3,1.9198560224444332,-50632.718181604207,2246.5817929166683]
["AKM2G","AKM2G-51K 120 V",6.8099999427795401,10.199999809265099,6.5485714285714298,9.7159809905912606,2100,15.699999809265099,2100,0.74000000953674305,6.6999998092651403,45.599998474121101,0.251999997999519,168,10,2100,2100,2100,6.5485714285714298,9.9206349993890548,0.69801745841443341,0.8543277545526361,1.1428571428571428,13.412945583526268,0,-10.864485922656275,0,0,0,0,0,0.58841719262137471,0.83707809314245551,7.0610063114564969,20.089874235418932,12.789611162645738,222.90762121529011,180.69831056392974,1738.3177476250039,7.1833930966590989E-3,1.3743896732136114,-50578.053209899554,2559.5420886401521,2.8691127696356417E-3,0.54062827236738009,-50770.019506237069,4113.426516549458,9.2499965921310405,3.5891715057629805E-3,0.74750572265008364,-50737.980093347272,3657.1493281451521]
["AKM2G","AKM2G-51K 240 V",6.8099999427795401,10.199999809265099,5.7724444444444396,8.5644573176323,4500,15.699999809265099,4500,0.74000000953674305,6.6999998092651403,45.599998474121101,0.251999997999519,336,10,2559.5420886401521,4184.4036316248921,4500,5.8452108327249244,9.9206349993890548,0.70300344091176503,0.8543277545526361,0.65624883882366425,13.412945583526268,0,-10.864485922656275,0,0,0,0,0,0.58841719262137471,0.83707809314245551,7.0610063114564969,20.089874235418932,12.789611162645738,222.90762121529011,180.69831056392974,1738.3177476250039,7.1833930966590989E-3,1.3743896732136114,-50578.053209899554,2559.5420886401521,2.7782991753733839E-3,0.50859591933617776,-50774.060307489235,4184.4036316248921,8.7019321058268329,3.5891715057629805E-3,0.74750572265008364,-50737.980093347272,3657.1493281451521]
["AKM2G","AKM2G-51K 400 V",6.8099999427795401,10.199999809265099,4.6635833333333299,6.9192628512856498,6000,15.699999809265099,6000,0.74000000953674305,6.6999998092651403,45.599998474121101,0.251999997999519,560,10,2559.5420886401521,4281.0573792198866,4942.9826215437033,5.2785111653212358,9.9206349993890548,0.70907541130390095,0.8543277545526361,0.65624883882366425,13.412945583526268,0,-10.864485922656275,0,0,0,0,0,0.58841719262137471,0.83707809314245551,7.0610063114564969,20.089874235418932,12.789611162645738,222.90762121529011,180.69831056392974,1738.3177476250039,7.1833930966590989E-3,1.3743896732136114,-50578.053209899554,2559.5420886401521,2.66217990161015E-3,0.46443011719361305,-50779.22709898818,4281.0573792198866,7.9462677423659418,3.5891715057629805E-3,0.74750572265008364,-50737.980093347272,3657.1493281451521]
["AKM2G","AKM2G-52H 240 V",12,6.3000001907348597,11.46,6.0000001048542497,1500,29,1500,2.3199999332428001,24.5,129,0.45799999497830901,336,10,966.21122086194259,1476.8640634891235,1500,11.468328937143916,5.4585153436920901,0.42806088208156123,0.49713679076729023,1.6,14.416966932251416,0,-11.677743215123646,0,0,0,0,0,0.22168757589282481,0.31537116119097947,2.6602509107138976,7.5689078685835067,4.8185164043688271,239.59329321030404,194.22441937835589,1868.4389144197837,4.5250173114021935E-2,7.8921553344621795,-49869.427234191462,966.21122086194259,2.1113188939912146E-2,3.1203480822081509,-50658.886155968095,1476.8640634891235,6.0195598004100646,1.9506611823786997E-2,2.4977654380037126,-50711.433177944753,1549.6070850892243]
["AKM2G","AKM2G-52H 400 V",12,6.3000001907348597,10.681851851851899,5.5925926903271099,2700,29,2700,2.3199999332428001,24.5,129,0.45799999497830901,560,10,966.21122086194259,1482.2418893454337,1747.2868217054265,11.27636503646362,5.4585153436920901,0.4301646117440282,0.49713679076729023,1.5487797023474574,14.416966932251416,0,-11.677743215123646,0,0,0,0,0,0.22168757589282481,0.31537116119097947,2.6602509107138976,7.5689078685835067,4.8185164043688271,239.59329321030404,194.22441937835589,1868.4389144197837,4.5250173114021935E-2,7.8921553344621795,-49869.427234191462,966.21122086194259,2.0984938469843752E-2,3.0752809939423993,-50663.080900310932,1482.2418893454337,5.9326194893617936,1.9506611823786997E-2,2.4977654380037126,-50711.433177944753,1549.6070850892243]
["AKM2G","AKM2G-52H 480 V",12,6.3000001907348597,10.266249999999999,5.3750000939319298,3200,29,3200,2.3199999332428001,24.5,129,0.45799999497830901,672,10,966.21122086194259,1484.5849966875173,1747.2868217054265,11.195656488122818,5.4585153436920901,0.43105019419055324,0.49713679076729023,1.5487797023474574,14.416966932251416,0,-11.677743215123646,0,0,0,0,0,0.22168757589282481,0.31537116119097947,2.6602509107138976,7.5689078685835067,4.8185164043688271,239.59329321030404,194.22441937835589,1868.4389144197837,4.5250173114021935E-2,7.8921553344621795,-49869.427234191462,966.21122086194259,2.0929551144480599E-2,3.0556124337070911,-50664.892477840498,1484.5849966875173,5.8946762627072147,1.9506611823786997E-2,2.4977654380037126,-50711.433177944753,1549.6070850892243]
["AKM2G","AKM2G-52K 120 V",11.8999996185303,10,11.69875,9.7489579459445501,1200,29,1200,0.90200001001357999,9.6000003814697301,80.900001525878906,0.45799999497830901,168,10,1200,1200,1200,11.69875,5.4585153436920901,0.42853763042427873,0.49713679076729023,2,14.416966932251416,0,-11.677743215123646,0,0,0,0,0,0.35484205888375997,0.50479577711504631,4.2581047066051196,12.11509865076111,7.71271134525833,239.59329321030404,194.22441937835589,1868.4389144197837,1.7798711741695006E-2,3.0801137107509997,-50442.769796415858,1599.1650573855136,8.2614214918541908E-3,1.2029599586346651,-50749.882894648988,2406.7701309316071,9.5177758412428588,7.6720470621116721E-3,0.9748162885543975,-50768.861514612938,2509.6811261976368]
["AKM2G","AKM2G-52K 240 V",11.8999996185303,10,10.810600000000001,9.0088329753544691,2500,29,2500,0.90200001001357999,9.6000003814697301,80.900001525878906,0.45799999497830901,336,10,{"$f":"IF(AQ530<I530,IF(AQ530<0,0,AQ530),I530)","v":1599.1650573855136},{"$f":"IF(AU530<I530,IF(AU530<0,0,AU530),I530)","v":2431.9686968661704},{"$f":"IF(UAC_V*0.98/L530*1000<I530,IF(UAC_V*0.98/L530*1000<0,0,UAC_V*0.98/L530*1000),I530)","v":2500},{"$f":"C530+(E530-C530)/G530*Q530","v":10.840245310272847},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M530,(inertia/gear^2+gear_inertia)/M530),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M530,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M530))","v":5.4585153436920901},{"$f":"IF((C530+(E530-C530)/G530*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X530^2*time1+Y530^2*time2+Z530^2*time3+AA530^2*time4)/time)/(C530+(E530-C530)/G530*mspeed),SQRT((((X530-Y530)*2/PI()+Y530)^2*time1+Y530^2*time2+((Z530-Y530)*2/PI()+Y530)^2*time3+AA530^2*time4)/time)/(C530+(E530-C530)/G530*mspeed)),IF(AccType=1,SQRT((X530^2*time1+Y530^2*time2+Z530^2*time3+AA530^2*time4+AB530^2*time5+AC530^2*time6+AD530^2*time7+AE530^2*time8)/time)/(C530+(E530-C530)/G530*mspeed),SQRT((((X530-Y530)*2/PI()+Y530)^2*time1+Y530^2*time2+((Z530-Y530)*2/PI()+Y530)^2*time3+AA530^2*time4+((AB530-AC530)*2/PI()+AC530)^2*time5+AC530^2*time6+((AD530-AC530)*2/PI()+AC530)^2*time7+AE530^2*time8)/time)/(C530+(E530-C530)/G530*mspeed))))","v":0.43296980454629619},{"$f":"IF(move1,MAX(ABS(X530),ABS(Z530))/H530,MAX(ABS(X530),ABS(Z530),ABS(AB530),ABS(AD530))/H530)","v":0.49713679076729023},{"$f":"IF(AZ530>0,speed/(MIN(AZ530,I530)),\"NA\")","v":0.96},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M530+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M530+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":14.416966932251416},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M530+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M530+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-11.677743215123646},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M530+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M530+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M530+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M530+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH530/Irms","v":0.35484205888375997},{"$f":"AI530/Ipeak","v":0.50479577711504631},{"$f":"IF(move1,IF(AccType=1,SQRT((X530^2*time1+Y530^2*time2+Z530^2*time3+AA530^2*time4)/time)/(C530/D530),SQRT((((X530-Y530)*2/PI()+Y530)^2*time1+Y530^2*time2+((Z530-AA530)*2/PI()+AA530)^2*time3+AA530^2*time4)/time)/(C530/D530)),IF(AccType=1,SQRT((X530^2*time1+Y530^2*time2+Z530^2*time3+AA530^2*time4+AB530^2*time5+AC530^2*time6+AD530^2*time7+AE530^2*time8)/time)/(C530/D530),SQRT((((X530-Y530)*2/PI()+Y530)^2*time1+Y530^2*time2+((Z530-AA530)*2/PI()+AA530)^2*time3+AA530^2*time4+((AB530-AC530)*2/PI()+AC530)^2*time5+AC530^2*time6+((AD530-AE530)*2/PI()+AE530)^2*time7+AE530^2*time8)/time)/(C530/D530)))","v":4.2581047066051196},{"$f":"IF(move1,MAX(ABS(X530),ABS(Z530))/(C530/D530),MAX(ABS(X530),ABS(Z530),ABS(AB530),ABS(AD530))/(C530/D530))","v":12.11509865076111},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X530),ABS(Z530))/(C530/D530),MAX(ABS((X530-Y530)*2/PI()+Y530),ABS((Z530-Y530)*2/PI()+Y530))/(C530/D530)),IF(AccType=1,MAX(ABS(X530),ABS(Z530),ABS(AB530),ABS(AD530))/(C530/D530),MAX(ABS((X530-Y530)*2/PI()+Y530),ABS((Z530-Y530)*2/PI()+Y530),ABS((AB530-AC530)*2/PI()+AC530),ABS((AD530-AC530)*2/PI()+AC530))/(C530/D530)))","v":7.71271134525833},{"$f":"IF((C530+(E530-C530)/G530*mspeed)<0,\"NA\",U530*(C530+(E530-C530)/G530*mspeed)*mspeed/9.55)","v":239.59329321030404},{"$f":"IF(move1,IF(speed1>speed2,AM530/2*time1/time,AM530/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z530*-speed/30*PI(),((Z530-AA530)*2/PI()+AA530)*-speed/30*PI()),IF(AccType=1,X530*-speed/30*PI(),((X530-Y530)*2/PI()+Y530)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z530*-speed/30*PI(),((Z530-AA530)*2/PI()+AA530)*-speed/30*PI()),IF(AccType=1,X530*-speed/30*PI(),((X530-Y530)*2/PI()+Y530)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD530*-speed/30*PI(),((AD530-AE530)*2/PI()+AE530)*-speed/30*PI()),IF(AccType=1,AB530*-speed/30*PI(),((AB530-AC530)*2/PI()+AC530)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD530*-speed/30*PI(),((AD530-AE530)*2/PI()+AE530)*-speed/30*PI()),IF(AccType=1,AB530*-speed/30*PI(),((AB530-AC530)*2/PI()+AC530)*-speed/30*PI()),0)/2*time7/time)))","v":194.22441937835589},{"$f":"IF(move1,MAX(IF(AccType=1,Z530*-speed/30*PI(),((Z530-AA530)*2/PI()+AA530)*-speed/30*PI()),IF(AccType=1,X530*-speed/30*PI(),((X530-Y530)*2/PI()+Y530)*-speed/30*PI()),0),MAX(IF(AccType=1,Z530*-speed/30*PI(),((Z530-AA530)*2/PI()+AA530)*-speed/30*PI()),IF(AccType=1,X530*-speed/30*PI(),((X530-Y530)*2/PI()+Y530)*-speed/30*PI()),IF(AccType=1,AD530*-speed/30*PI(),((AD530-AE530)*2/PI()+AE530)*-speed/30*PI()),IF(AccType=1,AB530*-speed/30*PI(),((AB530-AC530)*2/PI()+AC530)*-speed/30*PI()),0))","v":1868.4389144197837},{"$f":"(L530^2)/1000000+((K530/1000)^2*(D530/C530*H530)^2*PI()*PI()*(O530/2)^2)/1200","v":1.7798711741695006E-2},{"$f":"SQRT(3)*L530*J530*D530/C530*H530/1000","v":3.0801137107509997},{"$f":"0.75*J530^2*(D530/C530*H530)^2-(UAC_V*0.98)^2","v":-50442.769796415858},{"$f":"-AO530/2/AN530+SQRT((AO530/2/AN530)^2-AP530/AN530)","v":1599.1650573855136},{"$f":"(L530^2)/1000000+((K530/1000)^2*AV530^2*PI()*PI()*(O530/2)^2)/1200","v":8.1092457552980057E-3},{"$f":"SQRT(3)*L530*J530*AV530/1000","v":1.1484022311048647},{"$f":"0.75*J530^2*AV530^2-(UAC_V*0.98)^2","v":-50754.783150455973},{"$f":"-AS530/2/AR530+SQRT((AS530/2/AR530)^2-AT530/AR530)","v":2431.9686968661704},{"$f":"D530+(F530-D530)*((0.85*UAC_V-D530*J530)/L530*1000)/G530","v":9.0861170671423466},{"$f":"(L530^2)/1000000+((K530/1000)^2*AJ530^2*PI()*PI()*(O530/2)^2)/1200","v":7.6720470621116721E-3},{"$f":"SQRT(3)*L530*J530*AJ530/1000","v":0.9748162885543975},{"$f":"0.75*J530^2*AJ530^2-(UAC_V*0.98)^2","v":-50768.861514612938},{"$f":"IF(((AX530/2/AW530)^2-AY530/AW530)>0,-AX530/2/AW530+SQRT((AX530/2/AW530)^2-AY530/AW530),-9999)","v":2509.6811261976368}]
["AKM2G","AKM2G-52K 400 V",11.8999996185303,10,8.9856818181818205,7.4880678842690997,4400,29,4400,0.90200001001357999,9.6000003814697301,80.900001525878906,0.45799999497830901,560,10,1599.1650573855136,2455.14782405511,2786.1556952863261,10.2738448444097,5.4585153436920901,0.43678846986743158,0.49713679076729023,0.95629678804501661,14.416966932251416,0,-11.677743215123646,0,0,0,0,0,0.35484205888375997,0.50479577711504631,4.2581047066051196,12.11509865076111,7.71271134525833,239.59329321030404,194.22441937835589,1868.4389144197837,1.7798711741695006E-2,3.0801137107509997,-50442.769796415858,1599.1650573855136,7.9738548079411088E-3,1.0975847920645776,-50759.142914311982,2455.14782405511,8.6840513207808208,7.6720470621116721E-3,0.9748162885543975,-50768.861514612938,2509.6811261976368]
["AKM2G","AKM2G-52K 480 V",11.8999996185303,10,7.8201886792452804,6.51682364041576,5300,29,5300,0.90200001001357999,9.6000003814697301,80.900001525878906,0.45799999497830901,672,10,1599.1650573855136,2466.4978848782639,2786.1556952863261,10.001349608634129,5.4585153436920901,0.43862265033100262,0.49713679076729023,0.95629678804501661,14.416966932251416,0,-11.677743215123646,0,0,0,0,0,0.35484205888375997,0.50479577711504631,4.2581047066051196,12.11509865076111,7.71271134525833,239.59329321030404,194.22441937835589,1868.4389144197837,1.7798711741695006E-2,3.0801137107509997,-50442.769796415858,1599.1650573855136,7.9091268594685526E-3,1.0724394441749008,-50761.227238084975,2466.4978848782639,8.4851022344490978,7.6720470621116721E-3,0.9748162885543975,-50768.861514612938,2509.6811261976368]
["AKM2G","AKM2G-52L 120 V",11.8999996185303,12.5,11.46,11.987448069451601,1500,28.899999618530298,1500,0.57800000905990601,6.0999999046325701,64.699996948242202,0.45799999497830901,168,10,1500,1500,1500,11.46,5.4585153436920901,0.4306034587734528,0.49885699385987003,1.6,14.416966932251416,0,-11.677743215123646,0,0,0,0,0,0.44355257360469991,0.63099472139380774,5.3226308832563989,15.143873313451387,9.640889181572911,239.59329321030404,194.22441937835589,1868.4389144197837,1.1236915154901654E-2,1.9663174589303025,-50574.252117343764,2035.8007226691984,5.1989304796042201E-3,0.74525390496144372,-50771.990417211855,3054.184519447992,11.505659771069734,4.8972250836441852E-3,0.62446747538405056,-50781.870984200083,3157.0476666524405]
["AKM2G","AKM2G-52L 240 V",11.8999996185303,12.5,10.2065625,10.676320936855401,3200,28.899999618530298,3200,0.57800000905990601,6.0999999046325701,64.699996948242202,0.45799999497830901,336,10,2035.8007226691984,3091.5543211586073,3200,10.263951855591948,5.4585153436920901,0.43453642796345021,0.49885699385987003,0.76020391625725048,14.416966932251416,0,-11.677743215123646,0,0,0,0,0,0.44355257360469991,0.63099472139380774,5.3226308832563989,15.143873313451387,9.640889181572911,239.59329321030404,194.22441937835589,1868.4389144197837,1.1236915154901654E-2,1.9663174589303025,-50574.252117343764,2035.8007226691984,5.085391848524445E-3,0.70224149642698774,-50775.708700229516,3091.5543211586073,10.841609391411126,4.8972250836441852E-3,0.62446747538405056,-50781.870984200083,3157.0476666524405]
["AKM2G","AKM2G-52L 400 V",11.8999996185303,12.5,7.4183035714285701,7.7597320092432396,5600,28.899999618530298,5600,0.57800000905990601,6.0999999046325701,64.699996948242202,0.45799999497830901,560,10,2035.8007226691984,3135.7879071213538,3483.7714162538887,9.3904195706918756,5.4585153436920901,0.43914666000879665,0.49885699385987003,0.76020391625725048,14.416966932251416,0,-11.677743215123646,0,0,0,0,0,0.44355257360469991,0.63099472139380774,5.3226308832563989,15.143873313451387,9.640889181572911,239.59329321030404,194.22441937835589,1868.4389144197837,1.1236915154901654E-2,1.9663174589303025,-50574.252117343764,2035.8007226691984,4.9568279102821366E-3,0.65011041310091189,-50779.919047876865,3135.7879071213538,10.03677964915282,4.8972250836441852E-3,0.62446747538405056,-50781.870984200083,3157.0476666524405]
["AKM2G","AKM2G-53H 240 V",16.200000762939499,5.6900000572204599,15.7575,5.4904183373966999,1000,41.799999237060497,1000,3.1500000953674299,35.5,194,0.66399999195709802,336,10,647.07771467521536,992.27410043544978,1000,15.760918716451707,3.7650602865692933,0.33874786946688484,0.368923171350302,2.4,15.420988280976562,0,-12.491000507591014,0,0,0,0,0,0.15864178160264339,0.22568266478595531,1.9037013792317208,5.4163839548629271,3.4481771204002567,256.278965205318,207.75052819278193,1998.5600812145622,9.3491022790420958E-2,15.539836096264029,-49201.067469585301,647.07771467521536,4.5495500568296959E-2,5.8292514849551234,-50579.44411046039,992.27410043544978,5.5073143710039174,4.0717018782364361E-2,3.64974472953819,-50716.676655656876,1072.1407740953598]
["AKM2G","AKM2G-53H 400 V",16.200000762939499,5.6900000572204599,14.908611111111099,5.1946382249443497,1800,41.799999237060497,1800,3.1500000953674299,35.5,194,0.66399999195709802,560,10,647.07771467521536,995.11003232918188,1161.855670103093,15.486070319505872,3.7650602865692933,0.34139688155752368,0.368923171350302,2.2385120107245693,15.420988280976562,0,-12.491000507591014,0,0,0,0,0,0.15864178160264339,0.22568266478595531,1.9037013792317208,5.4163839548629271,3.4481771204002567,256.278965205318,207.75052819278193,1998.5600812145622,9.3491022790420958E-2,15.539836096264029,-49201.067469585301,647.07771467521536,4.5299180951937648E-2,5.7559877042307086,-50585.082185864238,995.11003232918188,5.438096792469346,4.0717018782364361E-2,3.64974472953819,-50716.676655656876,1072.1407740953598]
["AKM2G","AKM2G-53H 480 V",16.200000762939499,5.6900000572204599,14.4118181818182,5.0215396364068896,2200,41.799999237060497,2200,3.1500000953674299,35.5,194,0.66399999195709802,672,10,647.07771467521536,996.1825561448361,1161.855670103093,15.390293356341733,3.7650602865692933,0.34232548623148634,0.368923171350302,2.2385120107245693,15.420988280976562,0,-12.491000507591014,0,0,0,0,0,0.15864178160264339,0.22568266478595531,1.9037013792317208,5.4163839548629271,3.4481771204002567,256.278965205318,207.75052819278193,1998.5600812145622,9.3491022790420958E-2,15.539836096264029,-49201.067469585301,647.07771467521536,4.5225463408566029E-2,5.728235347498738,-50587.199269606674,996.1825561448361,5.4118771391478715,4.0717018782364361E-2,3.64974472953819,-50716.676655656876,1072.1407740953598]
["AKM2G","AKM2G-53L 120 V",16,12.5,15.6272727272727,12.1141652630942,1100,41.400001525878899,1100,0.63499999046325695,7.1500000953674299,87.099998474121094,0.66399999195709802,168,10,1100,1100,1100,15.6272727272727,3.7650602865692933,0.34202255057488867,0.37248762590834672,2.1818181818181817,15.420988280976562,0,-12.491000507591014,0,0,0,0,0,0.35286645391478927,0.50198529560470584,4.2343974469774714,12.047647094512939,7.6697703508737805,256.278965205318,207.75052819278193,1998.5600812145622,1.8582831231125398E-2,3.098438504434208,-50488.794238654031,1567.0587469118527,9.0363572082696065E-3,1.1251057048808391,-50763.445180622068,2308.7295224071254,11.744670398135009,8.2047610995849302E-3,0.73474197949942399,-50787.37010348263,2443.5961144970906]
["AKM2G","AKM2G-53L 240 V",16,12.5,14.0464583333333,10.888727712174701,2400,41.400001525878899,2400,0.63499999046325695,7.1500000953674299,87.099998474121094,0.66399999195709802,336,10,1567.0587469118527,2333.336925721479,2400,14.100720455512961,3.7650602865692933,0.34671670751584893,0.37248762590834672,1,15.420988280976562,0,-12.491000507591014,0,0,0,0,0,0.35286645391478927,0.50198529560470584,4.2343974469774714,12.047647094512939,7.6697703508737805,256.278965205318,207.75052819278193,1998.5600812145622,1.8582831231125398E-2,3.098438504434208,-50488.794238654031,1567.0587469118527,8.8709010307022312E-3,1.0589678491404426,-50768.205335514278,2333.336925721479,11.054275430674929,8.2047610995849302E-3,0.73474197949942399,-50787.37010348263,2443.5961144970906]
["AKM2G","AKM2G-53L 400 V",16,12.5,10.846071428571401,8.4078075575998703,4200,41.400001525878899,4200,0.63499999046325695,7.1500000953674299,87.099998474121094,0.66399999195709802,560,10,1567.0587469118527,2356.0355158212369,2587.8301257028174,13.108847914216287,3.7650602865692933,0.35090449639973936,0.37248762590834672,0.98215903428621099,15.420988280976562,0,-12.491000507591014,0,0,0,0,0,0.35286645391478927,0.50198529560470584,4.2343974469774714,12.047647094512939,7.6697703508737805,256.278965205318,207.75052819278193,1998.5600812145622,1.8582831231125398E-2,3.098438504434208,-50488.794238654031,1567.0587469118527,8.7237555830692003E-3,0.99646824958355817,-50772.438692846212,2356.0355158212369,10.40185922335619,8.2047610995849302E-3,0.73474197949942399,-50787.37010348263,2443.5961144970906]
["AKM2G","AKM2G-53L 480 V",16,12.5,8.6324509803921607,6.6918226633061497,5100,41.400001525878899,5100,0.63499999046325695,7.1500000953674299,87.099998474121094,0.66399999195709802,672,10,1567.0587469118527,2368.1101695113407,2587.8301257028174,12.578986714175169,3.7650602865692933,0.35314994817840761,0.37248762590834672,0.98215903428621099,15.420988280976562,0,-12.491000507591014,0,0,0,0,0,0.35286645391478927,0.50198529560470584,4.2343974469774714,12.047647094512939,7.6697703508737805,256.278965205318,207.75052819278193,1998.5600812145622,1.8582831231125398E-2,3.098438504434208,-50488.794238654031,1567.0587469118527,8.6475974810966451E-3,0.96252785210833414,-50774.629752539578,2368.1101695113407,10.047564707028574,8.2047610995849302E-3,0.73474197949942399,-50787.37010348263,2443.5961144970906]
["AKM2G","AKM2G-53M 120 V",16.100000381469702,14.199999809265099,15.353461538461501,13.4679488869492,1300,41.400001525878899,1300,0.5,5.5999999046325701,77.099998474121094,0.66399999195709802,168,10,1300,1300,1300,15.353461538461501,3.7650602865692933,0.3421586766982081,0.37248762590834672,1.8461538461538463,15.420988280976562,0,-12.491000507591014,0,0,0,0,0,0.3983664862261746,0.56671331640820777,4.780397834714095,13.601119593796986,8.6587416597472888,256.278965205318,207.75052819278193,1998.5600812145622,1.4541671843068146E-2,2.4380792062760661,-50555.167551154824,1782.6095514610188,7.0048354972149229E-3,0.85626433744852026,-50774.324784873228,2631.8720211630357,12.823980687608316,6.4278514685653428E-3,0.57814900622750098,-50791.102411163083,2766.3879152503173]
["AKM2G","AKM2G-53M 240 V",16.100000381469702,14.199999809265099,13.540535714285699,11.8776630563132,2800,41.400001525878899,2800,0.5,5.5999999046325701,77.099998474121094,0.66399999195709802,336,10,1782.6095514610188,2654.5036832254036,2800,13.673533100710696,3.7650602865692933,0.34550573005757335,0.37248762590834672,0.8675572889721922,15.420988280976562,0,-12.491000507591014,0,0,0,0,0,0.3983664862261746,0.56671331640820777,4.780397834714095,13.601119593796986,8.6587416597472888,256.278965205318,207.75052819278193,1998.5600812145622,1.4541671843068146E-2,2.4380792062760661,-50555.167551154824,1782.6095514610188,6.8999517550678551E-3,0.81281669586020722,-50777.374609724953,2654.5036832254036,12.173280089343411,6.4278514685653428E-3,0.57814900622750098,-50791.102411163083,2766.3879152503173]
["AKM2G","AKM2G-53M 400 V",16.100000381469702,14.199999809265099,9.7489583333333307,8.5517179435672297,4800,41.400001525878899,4800,0.5,5.5999999046325701,77.099998474121094,0.66399999195709802,560,10,1782.6095514610188,2683.2377440579835,2923.4760630463093,12.549717936124111,3.7650602865692933,0.34962227127797246,0.37248762590834672,0.8675572889721922,15.420988280976562,0,-12.491000507591014,0,0,0,0,0,0.3983664862261746,0.56671331640820777,4.780397834714095,13.601119593796986,8.6587416597472888,256.278965205318,207.75052819278193,1998.5600812145622,1.4541671843068146E-2,2.4380792062760661,-50555.167551154824,1782.6095514610188,6.7713584404063727E-3,0.75614834432442746,-50781.113865006962,2683.2377440579835,11.324577400336317,6.4278514685653428E-3,0.57814900622750098,-50791.102411163083,2766.3879152503173]
["AKM2G","AKM2G-54L 240 V",20.100000381469702,10.6000003814697,18.443437500000002,9.6562501687497999,1600,54.799999237060497,1600,0.99099999666214,11.6000003814697,130,0.86999998893588804,336,10,1042.3526545224552,1556.7454117640571,1600,18.488221215828077,2.8735632549349721,0.2940491319990205,0.29972645726961428,1.5,16.425009629701709,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-13.304257800058384,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.25370182054186802,0.36091439684123511,3.0444218465024164,8.6619455241896421,5.5143657878700001,272.96463720033194,221.27663700720805,2128.6812480093413,4.0007621773030737E-2,6.4486380332879838,-50189.99827685846,1042.3526545224552,1.9535906739581374E-2,2.1779875628297001,-50734.98796118579,1556.7454117640571,9.7606280363792095,1.7741328608962027E-2,1.2304761597420484,-50782.762491424655,1657.53972584187]
["AKM2G","AKM2G-54L 400 V",20.100000381469702,10.6000003814697,15.893928571428599,8.32142871685142,2800,54.799999237060497,2800,0.99099999666214,11.6000003814697,130,0.86999998893588804,560,10,1042.3526545224552,1565.1444246427784,1733.8461538461538,17.74888972320792,2.8735632549349721,0.29724062713884475,0.29972645726961428,1.4479290979171144,16.425009629701709,0,-13.304257800058384,0,0,0,0,0,0.25370182054186802,0.36091439684123511,3.0444218465024164,8.6619455241896421,5.5143657878700001,272.96463720033188,221.27663700720805,2128.6812480093413,4.0007621773030737E-2,6.4486380332879838,-50189.99827685846,1042.3526545224552,1.9366602612737531E-2,2.1068808161983448,-50739.495106898459,1565.1444246427784,9.4419639096456329,1.7741328608962027E-2,1.2304761597420484,-50782.762491424655,1657.53972584187]
["AKM2G","AKM2G-54L 480 V",20.100000381469702,10.6000003814697,14.268823529411801,7.47058836584793,3400,54.799999237060497,3400,0.99099999666214,11.6000003814697,130,0.86999998893588804,672,10,1042.3526545224552,1569.1069201891059,1733.8461538461538,17.408900395760707,2.8735632549349721,0.29871916692036082,0.29972645726961428,1.4479290979171144,16.425009629701709,0,-13.304257800058384,0,0,0,0,0,0.25370182054186802,0.36091439684123511,3.0444218465024164,8.6619455241896421,5.5143657878700001,272.96463720033188,221.27663700720805,2128.6812480093413,4.0007621773030737E-2,6.4486380332879838,-50189.99827685846,1042.3526545224552,1.9287952521312567E-2,2.0730186964695583,-50741.588897693611,1569.1069201891059,9.2902111811926709,1.7741328608962027E-2,1.2304761597420484,-50782.762491424655,1657.53972584187]
["AKM2G","AKM2G-54M 120 V",20,14.6000003814697,19.273636363636399,13.966403210314001,1100,54.700000762939503,1100,0.51399999856948897,6,93.300003051757798,0.86999998893588804,168,10,1100,1100,1100,19.273636363636399,2.8735632549349721,0.29301417593322854,0.3002743948923311,2.1818181818181817,16.425009629701709,0,-13.304257800058384,0,0,0,0,0,0.35118555158082226,0.49959405595685086,4.2142266189698674,11.990257342964421,7.6332349003067304,272.96463720033182,221.27663700720805,2128.6812480093413,2.0507591876439225E-2,3.3167719120265224,-50489.217604497462,1490.2843589056124,1.0041855766157388E-2,1.1163103457806911,-50769.371244869952,2193.6092602900321,13.439389679505114,9.1361893829095524E-3,0.63403616489974568,-50793.61471246327,2323.4378573651347]
["AKM2G","AKM2G-54M 240 V",20,14.6000003814697,17.148478260869599,12.4264335653068,2300,54.700000762939503,2300,0.51399999856948897,6,93.300003051757798,0.86999998893588804,336,10,1490.2843589056124,2212.2271788108983,2300,17.257298307706787,2.8735632549349721,0.29695809600365702,0.3002743948923311,1.0434782608695652,16.425009629701709,0,-13.304257800058384,0,0,0,0,0,0.35118555158082226,0.49959405595685086,4.2142266189698674,11.990257342964421,7.6332349003067304,272.96463720033182,221.27663700720805,2128.6812480093413,2.0507591876439225E-2,3.3167719120265224,-50489.217604497462,1490.2843589056124,9.8980036084549156E-3,1.0545464030178757,-50773.221973116022,2212.2271788108983,12.695806411581877,9.1361893829095524E-3,0.63403616489974568,-50793.61471246327,2323.4378573651347]
["AKM2G","AKM2G-54M 400 V",20,14.6000003814697,12.9292307692308,9.36900783616354,3900,54.700000762939503,3900,0.51399999856948897,6,93.300003051757798,0.86999998893588804,560,10,1490.2843589056124,2231.6716618550049,2415.8627291251028,15.953939661583608,2.8735632549349721,0.30096544514562967,0.3002743948923311,1.0329520939809811,16.425009629701709,0,-13.304257800058384,0,0,0,0,0,0.35118555158082226,0.49959405595685086,4.2142266189698674,11.990257342964421,7.6332349003067304,272.96463720033188,221.27663700720805,2128.6812480093413,2.0507591876439225E-2,3.3167719120265224,-50489.217604497462,1490.2843589056124,9.7526545395515279E-3,0.98822680293720844,-50777.11277165603,2231.6716618550049,11.897377057019458,9.1361893829095524E-3,0.63403616489974568,-50793.61471246327,2323.4378573651347]
["AKM2G","AKM2G-54M 480 V",20,14.6000003814697,9.7887500000000003,7.0932971259590403,4800,54.700000762939503,4800,0.51399999856948897,6,93.300003051757798,0.86999998893588804,672,10,1490.2843589056124,2242.3252855398518,2415.8627291251028,15.229803318339831,2.8735632549349721,0.30320911484117419,0.3002743948923311,1.0329520939809811,16.425009629701709,0,-13.304257800058384,0,0,0,0,0,0.35118555158082226,0.49959405595685086,4.2142266189698674,11.990257342964421,7.6332349003067304,272.96463720033188,221.27663700720805,2128.6812480093413,2.0507591876439225E-2,3.3167719120265224,-50489.217604497462,1490.2843589056124,9.6751369645723829E-3,0.95096803155856757,-50779.187812589073,2242.3252855398518,11.448814388555647,9.1361893829095524E-3,0.63403616489974568,-50793.61471246327,2323.4378573651347]
["AKM2G","AKM2G-54N 120 V",20,16.299999237060501,19.100000000000001,15.4032256879866,1200,54.700000762939503,1200,0.41600000858306901,4.9000000953674299,83.800003051757798,0.86999998893588804,168,10,1200,1200,1200,19.100000000000001,2.8735632549349721,0.29361761696790006,0.3002743948923311,2,16.425009629701709,0,-13.304257800058384,0,0,0,0,0,0.39207699131976598,0.55776592590176921,4.7049238958371919,13.386382221642462,8.5220356027674615,272.96463720033188,221.27663700720805,2128.6812480093413,1.6834056145949336E-2,2.6918008268656322,-50547.208662438832,1654.7154085680074,8.0772391386748372E-3,0.88258681832648433,-50777.428918098674,2453.2470263524669,14.617040001197685,7.3809803127562468E-3,0.51456630670062264,-50795.733843823997,2588.7261575566608]
["AKM2G","AKM2G-54N 240 V",20,16.299999237060501,16.492115384615399,13.3000929498192,2600,54.700000762939503,2600,0.41600000858306901,4.9000000953674299,83.800003051757798,0.86999998893588804,336,10,1654.7154085680074,2475.9715029028789,2600,16.659452944937041,2.8735632549349721,0.29771459758902286,0.3002743948923311,0.92709690169207093,16.425009629701709,0,-13.304257800058384,0,0,0,0,0,0.39207699131976598,0.55776592590176921,4.7049238958371919,13.386382221642462,8.5220356027674615,272.96463720033188,221.27663700720805,2128.6812480093413,1.6834056145949336E-2,2.6918008268656322,-50547.208662438832,1654.7154085680074,7.9492555239368354E-3,0.82731174300904953,-50780.793659017749,2475.9715029028789,13.70159693066082,7.3809803127562468E-3,0.51456630670062264,-50795.733843823997,2588.7261575566608]
["AKM2G","AKM2G-54N 400 V",20,16.299999237060501,11.0355555555556,8.89964150861449,4500,54.700000762939503,4500,0.41600000858306901,4.9000000953674299,83.800003051757798,0.86999998893588804,560,10,1654.7154085680074,2502.4359739702968,2689.7373722144748,15.014900385680924,2.8735632549349721,0.30223964438045714,0.3002743948923311,0.92709690169207093,16.425009629701709,0,-13.304257800058384,0,0,0,0,0,0.39207699131976598,0.55776592590176921,4.7049238958371919,13.386382221642462,8.5220356027674615,272.96463720033188,221.27663700720805,2128.6812480093413,1.6834056145949336E-2,2.6918008268656322,-50547.208662438832,1654.7154085680074,7.8057808131882667E-3,0.76058524206880818,-50784.565667107199,2502.4359739702968,12.596500057321084,7.3809803127562468E-3,0.51456630670062264,-50795.733843823997,2588.7261575566608]
["AKM2G","AKM2G-62K 240 V",15.300000190734901,9.3199996948242205,14.381176470588199,8.7690101195304493,1700,37.599998474121101,1700,1.1499999761581401,17.399999618530298,111,0.91000000247731805,336,10,1002.548258623289,1665.5880383148572,1700,14.399775603913547,2.7472527397738253,0.38798205270040104,0.44202037166819536,1.411764705882353,16.619965300254588,0,-13.462171893206216,0,0,0,0,0,0.2965259529126742,0.42183570151239363,3.5583114349520901,10.124056836297447,6.4451747585601362,276.20457465439478,223.9030668308726,2153.9475029129944,4.4978396862199219E-2,5.0640003462157628,-50284.826839005087,1002.548258623289,1.7120440050417324E-2,1.9413249241803012,-50728.690101833381,1665.5880383148572,8.7804503783550221,1.4906987258396155E-2,1.4250041695281066,-50763.957238796116,1798.1895524069314]
["AKM2G","AKM2G-62K 400 V",15.300000190734901,9.3199996948242205,12.8925,7.86128055637593,3000,37.599998474121101,3000,1.1499999761581401,17.399999618530298,111,0.91000000247731805,560,10,1002.548258623289,1681.2210344009347,2030.6306306306308,13.950820203738974,2.7472527397738253,0.39105511866065051,0.44202037166819536,1.3346757558387141,16.619965300254588,0,-13.462171893206216,0,0,0,0,0,0.2965259529126742,0.42183570151239363,3.5583114349520901,10.124056836297447,6.4451747585601362,276.20457465439478,223.9030668308726,2153.9475029129944,4.4978396862199219E-2,5.0640003462157628,-50284.826839005087,1002.548258623289,1.6829922431426791E-2,1.8816520881168164,-50733.318944470535,1681.2210344009347,8.5105551282271357,1.4906987258396155E-2,1.4250041695281066,-50763.957238796116,1798.1895524069314]
["AKM2G","AKM2G-62K 480 V",15.300000190734901,9.3199996948242205,11.847162162162199,7.2238794301832803,3700,37.599998474121101,3700,1.1499999761581401,17.399999618530298,111,0.91000000247731805,672,10,1002.548258623289,1688.9497419431104,2030.6306306306308,13.723873191456732,2.7472527397738253,0.39260630546360881,0.44202037166819536,1.3346757558387141,16.619965300254588,0,-13.462171893206216,0,0,0,0,0,0.2965259529126742,0.42183570151239363,3.5583114349520901,10.124056836297447,6.4451747585601362,276.20457465439478,223.9030668308726,2153.9475029129944,4.4978396862199219E-2,5.0640003462157628,-50284.826839005087,1002.548258623289,1.6689427163941603E-2,1.8521045310965116,-50735.557467857558,1688.9497419431104,8.3769139973752527,1.4906987258396155E-2,1.4250041695281066,-50763.957238796116,1798.1895524069314]
["AKM2G","AKM2G-62L 120 V",15.199999809265099,11.6000003814697,14.898,11.372519580718199,1000,37.400001525878899,1000,0.73199999332428001,11,88.300003051757798,0.91000000247731805,168,10,1000,1000,1000,14.898,2.7472527397738253,0.38778399757222581,0.44438408080690633,2.4,16.619965300254588,0,-13.462171893206216,0,0,0,0,0,0.37149474032437096,0.52848576272528158,4.4579368838924518,12.683658305406757,8.074667663176232,276.20457465439478,223.9030668308726,2153.9475029129944,2.8065126897994931E-2,3.1953502118514434,-50477.777470856323,1285.3970761936582,1.0872383010748048E-2,1.244708966339761,-50755.483131921988,2104.1399316152356,11.118223370649707,9.4190486846909335E-3,0.90397637333867131,-50778.958103247918,2274.3817368679124]
["AKM2G","AKM2G-62L 240 V",15.199999809265099,11.6000003814697,13.8475,10.570611148744399,2200,37.400001525878899,2200,0.73199999332428001,11,88.300003051757798,0.91000000247731805,336,10,1285.3970761936582,2133.2779220637062,2200,13.88851890803755,2.7472527397738253,0.39145424345627228,0.44438408080690633,1.0909090909090908,16.619965300254588,0,-13.462171893206216,0,0,0,0,0,0.37149474032437096,0.52848576272528158,4.4579368838924518,12.683658305406757,8.074667663176232,276.20457465439478,223.9030668308726,2153.9475029129944,2.8065126897994931E-2,3.1953502118514434,-50477.777470856323,1285.3970761936582,1.0597133301626083E-2,1.1877042912540821,-50759.929100694113,2133.2779220637062,10.609035497891277,9.4190486846909335E-3,0.90397637333867131,-50778.958103247918,2274.3817368679124]
["AKM2G","AKM2G-62L 400 V",15.199999809265099,11.6000003814697,11.508974358974401,8.7854769936514394,3900,37.400001525878899,3900,0.73199999332428001,11,88.300003051757798,0.91000000247731805,560,10,1285.3970761936582,2163.8713685409516,2552.6612934303057,13.152075631716377,2.7472527397738253,0.3954225943476134,0.44438408080690633,1.0552318289827101,16.619965300254588,0,-13.462171893206216,0,0,0,0,0,0.37149474032437096,0.52848576272528158,4.4579368838924518,12.683658305406757,8.074667663176232,276.20457465439478,223.9030668308726,2153.9475029129944,2.8065126897994931E-2,3.1953502118514434,-50477.777470856323,1285.3970761936582,1.0320600654837876E-2,1.1275354838753449,-50764.39579210685,2163.8713685409516,10.071584367970042,9.4190486846909335E-3,0.90397637333867131,-50778.958103247918,2274.3817368679124]
["AKM2G","AKM2G-62L 480 V",15.199999809265099,11.6000003814697,9.8484374999999993,7.5178915497535899,4800,37.400001525878899,4800,0.73199999332428001,11,88.300003051757798,0.91000000247731805,672,10,1285.3970761936582,2179.3011499009767,2552.6612934303057,12.770277747942567,2.7472527397738253,0.39746969938201571,0.44438408080690633,1.0552318289827101,16.619965300254588,0,-13.462171893206216,0,0,0,0,0,0.37149474032437096,0.52848576272528158,4.4579368838924518,12.683658305406757,8.074667663176232,276.20457465439478,223.9030668308726,2153.9475029129944,2.8065126897994931E-2,3.1953502118514434,-50477.777470856323,1285.3970761936582,1.018577996932832E-2,1.0970047507028933,-50766.573482174259,2179.3011499009767,9.798872014913556,9.4190486846909335E-3,0.90397637333867131,-50778.958103247918,2274.3817368679124]
["AKM2G","AKM2G-62M 120 V",15.1000003814697,14.6000003814697,14.618846153846199,14.056583355829099,1300,37.400001525878899,1300,0.46799999475479098,7,70.300003051757798,0.91000000247731805,168,10,1300,1300,1300,14.618846153846199,2.7472527397738253,0.3911796135873235,0.44438408080690633,1.8461538461538463,16.619965300254588,0,-13.462171893206216,0,0,0,0,0,0.47066744175875325,0.66956813905532886,5.6480093011050387,16.069635337327892,10.230247590479724,276.20457465439478,223.9030668308726,2153.9475029129944,1.8117060751736736E-2,2.0606742689807249,-50590.353203980281,1615.1484526601032,6.7723632188351956E-3,0.76805520565084684,-50775.318943498052,2682.0255147895732,13.478160309756376,5.9965425802321701E-3,0.58297235946045889,-50787.96804566549,2862.0446045286599]
["AKM2G","AKM2G-62M 240 V",15.1000003814697,14.6000003814697,13.13125,12.6262023862033,2800,37.400001525878899,2800,0.46799999475479098,7,70.300003051757798,0.91000000247731805,336,10,1615.1484526601032,2725.677729689547,2800,13.183507856437641,2.7472527397738253,0.39515881431459743,0.44438408080690633,0.8571428571428571,16.619965300254588,0,-13.462171893206216,0,0,0,0,0,0.47066744175875325,0.66956813905532886,5.6480093011050387,16.069635337327892,10.230247590479724,276.20457465439478,223.9030668308726,2153.9475029129944,1.8117060751736736E-2,2.0606742689807249,-50590.353203980281,1615.1484526601032,6.5692103670976602E-3,0.72417630195626992,-50778.631179663695,2725.677729689547,12.70815459420275,5.9965425802321701E-3,0.58297235946045889,-50787.96804566549,2862.0446045286599]
["AKM2G","AKM2G-62M 400 V",15.1000003814697,14.6000003814697,9.6073000000000004,9.2377888003785404,5000,37.400001525878899,5000,0.46799999475479098,7,70.300003051757798,0.91000000247731805,560,10,1615.1484526601032,2780.9027231121195,3206.2587512841374,12.045067291856087,2.7472527397738253,0.39999017343510934,0.44438408080690633,0.83856135442558821,16.619965300254588,0,-13.462171893206216,0,0,0,0,0,0.47066744175875325,0.66956813905532886,5.6480093011050387,16.069635337327892,10.230247590479724,276.20457465439478,223.9030668308726,2153.9475029129944,1.8117060751736736E-2,2.0606742689807249,-50590.353203980281,1615.1484526601032,6.3264412439067346E-3,0.66797099659853609,-50782.58932577318,2780.9027231121195,11.721839925287243,5.9965425802321701E-3,0.58297235946045889,-50787.96804566549,2862.0446045286599]
["AKM2G","AKM2G-63K 240 V",21.5,9.7899999618530291,20.495769230769199,9.3162585393342798,1300,54.700000762939503,1300,1.1799999475479099,19.799999237060501,149,1.30000000353903,336,10,782.55851960781717,1269.3705186389,1300,20.519430052021811,1.9230769178416716,0.30776141442913046,0.33858833988122183,1.8461538461538463,18.520782449825255,0,-15.001833784358457,0,0,0,0,0,0.24700838503833333,0.35139236332805712,2.96410062046,8.4334167198733709,5.3688798324867406,307.79395422337035,249.51074901219886,2400.293405497353,7.2210438715423708E-2,7.5850849025010145,-50157.28926244146,782.55851960781717,2.9233226229166957E-2,2.8443358363176912,-50714.057725893421,1269.3705186389,9.3401099633719333,2.4524572469980684E-2,1.6349804625760866,-50775.058190250384,1405.9322616698989]
["AKM2G","AKM2G-63K 400 V",21.5,9.7899999618530291,18.882954545454499,8.5831609709897894,2200,54.700000762939503,2200,1.1799999475479099,19.799999237060501,149,1.30000000353903,560,10,782.55851960781717,1277.7130000285474,1512.7516778523491,19.980075909573451,1.9230769178416716,0.31052643964731053,0.33858833988122183,1.707052370467262,18.520782449825255,0,-15.001833784358457,0,0,0,0,0,0.24700838503833333,0.35139236332805712,2.96410062046,8.4334167198733709,5.3688798324867406,307.79395422337035,249.51074901219886,2400.293405497353,7.2210438715423708E-2,7.5850849025010145,-50157.28926244146,782.55851960781717,2.8895063824028865E-2,2.775104749017574,-50718.438609431789,1277.7130000285474,9.1127718410551157,2.4524572469980684E-2,1.6349804625760866,-50775.058190250384,1405.9322616698989]
["AKM2G","AKM2G-63K 480 V",21.5,9.7899999618530291,17.791296296296299,8.0869526866728805,2700,54.700000762939503,2700,1.1799999475479099,19.799999237060501,149,1.30000000353903,672,10,782.55851960781717,1281.4271537384093,1512.7516778523491,19.739839395890321,1.9230769178416716,0.31176230674887867,0.33858833988122183,1.707052370467262,18.520782449825255,0,-15.001833784358457,0,0,0,0,0,0.24700838503833333,0.35139236332805712,2.96410062046,8.4334167198733709,5.3688798324867406,307.79395422337035,249.51074901219886,2400.293405497353,7.2210438715423708E-2,7.5850849025010145,-50157.28926244146,782.55851960781717,2.8746812460861616E-2,2.7442030045387553,-50720.359201273372,1281.4271537384093,9.0112979968603177,2.4524572469980684E-2,1.6349804625760866,-50775.058190250384,1405.9322616698989]
["AKM2G","AKM2G-63M 120 V",21.399999618530298,15.199999809265099,20.9145,14.8329790745419,1000,54.5,1000,0.49099999666214,8.1999998092651403,95.5,1.30000000353903,168,10,1000,1000,1000,20.9145,1.9230769178416716,0.30733145598919126,0.33983087063899553,2.4,18.520782449825255,0,-15.001833784358457,0,0,0,0,0,0.3852984686408169,0.54812284798091604,4.6235816236898026,13.154948351541986,8.3747002250659488,307.79395422337041,249.51074901219886,2400.293405497353,2.9837820763421948E-2,3.1439223223304924,-50534.217658264635,1249.7776948642402,1.2018021400845099E-2,1.1758026990499282,-50767.263232173107,2006.9645483124345,14.477346358542668,1.008992172744836E-2,0.68016574892236048,-50792.47872903684,2210.2015411828265]
["AKM2G","AKM2G-63M 240 V",21.399999618530298,15.199999809265099,19.145476190476199,13.5783522295763,2100,54.5,2100,0.49099999666214,8.1999998092651403,95.5,1.30000000353903,336,10,1249.7776948642402,2035.5592082752632,2100,19.214658702221804,1.9230769178416716,0.31123355295030775,0.33983087063899553,1.1428571428571428,18.520782449825255,0,-15.001833784358457,0,0,0,0,0,0.3852984686408169,0.54812284798091604,4.6235816236898026,13.154948351541986,8.3747002250659488,307.79395422337035,249.51074901219886,2400.293405497353,2.9837820763421948E-2,3.1439223223304924,-50534.217658264635,1249.7776948642402,1.170744282257925E-2,1.1110069883203677,-50771.324948107329,2035.5592082752632,13.67953398105981,1.008992172744836E-2,0.68016574892236048,-50792.47872903684,2210.2015411828265]
["AKM2G","AKM2G-63M 400 V",21.399999618530298,15.199999809265099,15.598333333333301,11.062648016020599,3600,54.5,3600,0.49099999666214,8.1999998092651403,95.5,1.30000000353903,560,10,1249.7776948642402,2061.8280511622897,2360.2094240837696,18.077211204557607,1.9230769178416716,0.3148910848964116,0.33983087063899553,1.0858738243009276,18.520782449825255,0,-15.001833784358457,0,0,0,0,0,0.3852984686408169,0.54812284798091604,4.6235816236898026,13.154948351541986,8.3747002250659488,307.79395422337029,249.51074901219886,2400.293405497353,2.9837820763421948E-2,3.1439223223304924,-50534.217658264635,1249.7776948642402,1.1434243450943012E-2,1.0507114248647242,-50774.897822473584,2061.8280511622897,12.937130721791759,1.008992172744836E-2,0.68016574892236048,-50792.47872903684,2210.2015411828265]
["AKM2G","AKM2G-63M 480 V",21.399999618530298,15.199999809265099,12.8394444444444,9.1059891832550495,4500,54.5,4500,0.49099999666214,8.1999998092651403,95.5,1.30000000353903,672,10,1249.7776948642402,2075.936800725121,2360.2094240837696,17.450850391747462,1.9230769178416716,0.31690390990790446,0.33983087063899553,1.0858738243009276,18.520782449825255,0,-15.001833784358457,0,0,0,0,0,0.3852984686408169,0.54812284798091604,4.6235816236898026,13.154948351541986,8.3747002250659488,307.79395422337035,249.51074901219886,2400.293405497353,2.9837820763421948E-2,3.1439223223304924,-50534.217658264635,1249.7776948642402,1.1292129703045216E-2,1.0179355345547318,-50776.756372015319,2075.936800725121,12.533569889170117,1.008992172744836E-2,0.68016574892236048,-50792.47872903684,2210.2015411828265]
["AKM2G","AKM2G-63N 120 V",21.399999618530298,16.799999237060501,20.749545454545501,16.3382250127341,1100,54.5,1100,0.39800000190734902,6.5999999046325701,86,1.30000000353903,168,10,1100,1100,1100,20.749545454545501,1.9230769178416716,0.30802638166271062,0.33983087063899553,2.1818181818181817,18.520782449825255,0,-15.001833784358457,0,0,0,0,0,0.42585618818631188,0.60581996996354148,5.1102742582357426,14.539679279124995,9.2562473129741942,307.79395422337035,249.51074901219886,2400.293405497353,2.3791715126216008E-2,2.536495822739699,-50587.683963670366,1405.8423256445024,9.6541687508056861E-3,0.94134141474761335,-50775.207199191493,2245.1048523311524,15.878336934653564,8.1633902307725534E-3,0.54875324643304846,-50794.981182887008,2461.0676433229928]
["AKM2G","AKM2G-63N 240 V",21.399999618530298,16.799999237060501,18.726304347826101,14.7451217551708,2300,54.5,2300,0.39800000190734902,6.5999999046325701,86,1.30000000353903,336,10,1405.8423256445024,2281.7026460724478,2300,18.747574586375013,1.9230769178416716,0.3118320248303551,0.33983087063899553,1.0434782608695652,18.520782449825255,0,-15.001833784358457,0,0,0,0,0,0.42585618818631188,0.60581996996354148,5.1102742582357426,14.539679279124995,9.2562473129741942,307.79395422337035,249.51074901219886,2400.293405497353,2.3791715126216008E-2,2.536495822739699,-50587.683963670366,1405.8423256445024,9.3680826216844849E-3,0.87969378255815467,-50779.00190268147,2281.7026460724478,14.838478430828715,8.1633902307725534E-3,0.54875324643304846,-50794.981182887008,2461.0676433229928]
["AKM2G","AKM2G-63N 400 V",21.399999618530298,16.799999237060501,14.1386585365854,11.132802164509201,4100,54.5,4100,0.39800000190734902,6.5999999046325701,86,1.30000000353903,560,10,1405.8423256445024,2318.7553467032726,2620.9302325581393,17.293347555604477,1.9230769178416716,0.3159919187069915,0.33983087063899553,0.97518652382892745,18.520782449825255,0,-15.001833784358457,0,0,0,0,0,0.42585618818631188,0.60581996996354148,5.1102742582357426,14.539679279124995,9.2562473129741942,307.79395422337035,249.51074901219886,2400.293405497353,2.3791715126216008E-2,2.536495822739699,-50587.683963670366,1405.8423256445024,9.0931339831395071E-3,0.81606928890490704,-50782.64887627455,2318.7553467032726,13.765274668946152,8.1633902307725534E-3,0.54875324643304846,-50794.981182887008,2461.0676433229928]
["AKM2G","AKM2G-64L 240 V",27,11.3999996185303,25.7054166666667,10.800594718754899,1200,70.699996948242202,1200,0.95499998331069902,16.899999618530298,161,1.6899999463930699,336,10,751.72992289456488,1200,1200,25.7054166666667,1.4792899877515946,0.27072149052496841,0.28884865908337021,2,20.421599315698124,0,-16.541495445715483,0,0,0,0,0,0.25254510728494123,0.35926886482829823,3.0305412874192945,8.6224527558791575,5.4892239106980139,339.38332907761713,275.11842737156735,2646.6392713144778,7.8251252832030826E-2,7.9496925902915798,-50195.638643955324,751.72992289456488,3.2805415939309079E-2,2.8834170973080417,-50724.973142268354,1200.3071756749964,10.827235968972106,2.7690513134044123E-2,1.4618432737973643,-50784.549435620283,1328.1156583352254]
["AKM2G","AKM2G-64L 400 V",27,11.3999996185303,23.420238095238101,9.8404357012981496,2100,70.699996948242202,2100,0.95499998331069902,16.899999618530298,161,1.6899999463930699,560,10,751.72992289456488,1207.68647682236,1400.0000000000002,24.941319027321526,1.4792899877515946,0.27363818396293532,0.28884865908337021,1.8070715339719485,20.421599315698124,0,-16.541495445715483,0,0,0,0,0,0.25254510728494123,0.35926886482829823,3.0305412874192945,8.6224527558791575,5.4892239106980139,339.38332907761713,275.11842737156735,2646.6392713144778,7.8251252832030826E-2,7.9496925902915798,-50195.638643955324,751.72992289456488,3.2455427248160994E-2,2.8091678026596916,-50729.049667224455,1207.68647682236,10.548429744774449,2.7690513134044123E-2,1.4618432737973643,-50784.549435620283,1328.1156583352254]
["AKM2G","AKM2G-64L 480 V",27,11.3999996185303,21.854807692307698,9.1826918661479002,2600,70.699996948242202,2600,0.95499998331069902,16.899999618530298,161,1.6899999463930699,672,10,751.72992289456488,1211.0156561615756,1400.0000000000002,24.603496754393277,1.4792899877515946,0.27493633516163024,0.28884865908337021,1.8070715339719485,20.421599315698124,0,-16.541495445715483,0,0,0,0,0,0.25254510728494123,0.35926886482829823,3.0305412874192945,8.6224527558791575,5.4892239106980139,339.38332907761713,275.11842737156735,2646.6392713144778,7.8251252832030826E-2,7.9496925902915798,-50195.638643955324,751.72992289456488,3.2299864156488625E-2,2.7755278876822955,-50730.86160241405,1211.0156561615756,10.422111808400807,2.7690513134044123E-2,1.4618432737973643,-50784.549435620283,1328.1156583352254]
["AKM2G","AKM2G-64M 240 V",26.899999618530298,15.800000190734901,24.5491176470588,14.4406570343968,1700,70.5,1700,0.49099999666214,8.6999998092651403,115,1.6899999463930699,336,10,1075.2151868347182,1700,1700,24.5491176470588,1.4792899877515946,0.27316641247205836,0.28966807539997341,1.411764705882353,20.421599315698124,0,-16.541495445715483,0,0,0,0,0,0.35131986304444096,0.49978512648514761,4.2158383565332915,11.994843035643543,7.6361542429362599,339.38332907761713,275.11842737156735,2646.6392713144778,3.991108499384298E-2,4.0498029484281712,-50495.124009052983,1075.2151868347182,1.649471094082855E-2,1.4175753085578746,-50767.17285906554,1711.9172604311191,14.494598274263062,1.4132499466687935E-2,0.74681778013445843,-50794.616771328452,1869.5919542851684]
["AKM2G","AKM2G-64M 400 V",26.899999618530298,15.800000190734901,20.532499999999999,12.0779408376935,3000,70.5,3000,0.49099999666214,8.6999998092651403,115,1.6899999463930699,560,10,1075.2151868347182,1730.3734095283312,1960,23.227282276834757,1.4792899877515946,0.27668330652577278,0.28966807539997341,1.2837025718361261,20.421599315698124,0,-16.541495445715483,0,0,0,0,0,0.35131986304444096,0.49978512648514761,4.2158383565332915,11.994843035643543,7.6361542429362599,339.38332907761713,275.11842737156735,2646.6392713144778,3.991108499384298E-2,4.0498029484281712,-50495.124009052983,1075.2151868347182,1.6177911970655559E-2,1.347152340505029,-50770.853394545782,1730.3734095283312,13.774528853580437,1.4132499466687935E-2,0.74681778013445843,-50794.616771328452,1869.5919542851684]
["AKM2G","AKM2G-64M 480 V",26.899999618530298,15.800000190734901,17.654594594594599,10.3850553525862,3700,70.5,3700,0.49099999666214,8.6999998092651403,115,1.6899999463930699,672,10,1075.2151868347182,1739.582836338182,1960,22.553202890251015,1.4792899877515946,0.27850737564871841,0.28966807539997341,1.2837025718361261,20.421599315698124,0,-16.541495445715483,0,0,0,0,0,0.35131986304444096,0.49978512648514761,4.2158383565332915,11.994843035643543,7.6361542429362599,339.38332907761713,275.11842737156735,2646.6392713144778,3.991108499384298E-2,4.0498029484281712,-50495.124009052983,1075.2151868347182,1.6024013541389475E-2,1.3115775053737611,-50772.641369516023,1739.582836338182,13.410778906196379,1.4132499466687935E-2,0.74681778013445843,-50794.616771328452,1869.5919542851684]
["AKM2G","AKM2G-64N 120 V",26.799999237060501,17.799999237060501,26.209444444444401,17.357248086076901,900,70.300003051757798,900,0.38899999856948902,6.8000001907348597,102,1.6899999463930699,168,10,900,900,900,26.209444444444401,1.4792899877515946,0.27081495705389924,0.29049215404248119,2.6666666666666665,20.421599315698124,0,-16.541495445715483,0,0,0,0,0,0.39726754672536085,0.56514997292784142,4.7672105607043305,13.563599350268193,8.6348555308528105,339.38332907761713,275.11842737156735,2646.6392713144778,3.1132002367977214E-2,3.2088612942354038,-50557.736153266967,1223.8598657586424,1.3116447249333385E-2,1.1607878947591226,-50772.782343891311,1923.7148277216661,16.890498663636446,1.1112902502430999E-2,0.59342450290036863,-50796.6980468896,2111.4486413449285]
["AKM2G","AKM2G-64N 240 V",26.799999237060501,17.799999237060501,23.779499999999999,15.7480133444932,2000,70.300003051757798,2000,0.38899999856948902,6.8000001907348597,102,1.6899999463930699,336,10,1223.8598657586424,1948.8345421702561,2000,23.856772613169294,1.4792899877515946,0.27481389151094343,0.29049215404248119,1.2,20.421599315698124,0,-16.541495445715483,0,0,0,0,0,0.39726754672536085,0.56514997292784142,4.7672105607043305,13.563599350268193,8.6348555308528105,339.38332907761708,275.11842737156735,2646.6392713144778,3.1132002367977214E-2,3.2088612942354038,-50557.736153266967,1223.8598657586424,1.2808602536163222E-2,1.0929338333137264,-50776.456992406725,1948.8345421702561,15.903161580487765,1.1112902502430999E-2,0.59342450290036863,-50796.6980468896,2111.4486413449285]
["AKM2G","AKM2G-64N 400 V",26.799999237060501,17.799999237060501,18.875294117647101,12.5001948588465,3400,70.300003051757798,3400,0.38899999856948902,6.8000001907348597,102,1.6899999463930699,560,10,1223.8598657586424,1973.4020664704574,2209.8039215686276,22.200402337407731,1.4792899877515946,0.27876866103213371,0.29049215404248119,1.1366603728856379,20.421599315698124,0,-16.541495445715483,0,0,0,0,0,0.39726754672536085,0.56514997292784142,4.7672105607043305,13.563599350268193,8.6348555308528105,339.38332907761708,275.11842737156735,2646.6392713144778,3.1132002367977214E-2,3.2088612942354038,-50557.736153266967,1223.8598657586424,1.2519962923809738E-2,1.0252416639067046,-50779.902395487072,1973.4020664704574,14.918180170817561,1.1112902502430999E-2,0.59342450290036863,-50796.6980468896,2111.4486413449285]
["AKM2G","AKM2G-64N 480 V",26.799999237060501,17.799999237060501,15.166309523809501,10.043913655361401,4200,70.300003051757798,4200,0.38899999856948902,6.8000001907348597,102,1.6899999463930699,672,10,1223.8598657586424,1986.4380514020977,2209.8039215686276,21.297712588344559,1.4792899877515946,0.28093225000741556,0.29049215404248119,1.1366603728856379,20.421599315698124,0,-16.541495445715483,0,0,0,0,0,0.39726754672536085,0.56514997292784142,4.7672105607043305,13.563599350268193,8.6348555308528105,339.38332907761713,275.11842737156735,2646.6392713144778,3.1132002367977214E-2,3.2088612942354038,-50557.736153266967,1223.8598657586424,1.2371655355989211E-2,0.98865948211556931,-50781.672697722584,1986.4380514020977,14.385876814238967,1.1112902502430999E-2,0.59342450290036863,-50796.6980468896,2111.4486413449285]
["AKM2G","AKM2G-65L 240 V",32.599998474121101,12.3999996185303,31.080909090909099,11.7286445178786,1100,86.800003051757798,1100,0.89600002765655495,16.399999618530298,179,2.0800000056624399,336,10,689.01108817782142,1089.8352129356717,1100,31.094946563738219,1.2019230736510493,0.24535845729894484,0.25717069083115046,2.1818181818181817,22.322416748966521,0,-18.081157566662881,0,0,0,0,0,0.248687204026111,0.35378063922251174,2.984246448313332,8.4907353413402813,5.4053700002374283,370.97271336132036,300.72611337485046,2892.9852106660614,9.2323860076631709E-2,9.1716086222527657,-50148.825891203611,689.01108817782142,3.9703933581906187E-2,3.2699877079515423,-50721.729242453781,1089.8352129356717,11.771300286552858,3.3656835099980457E-2,1.5015752743898916,-50787.567475541815,1206.3017834075395]
["AKM2G","AKM2G-65L 400 V",32.599998474121101,12.3999996185303,28.4992105263158,10.754418679507401,1900,86.800003051757798,1900,0.89600002765655495,16.399999618530298,179,2.0800000056624399,560,10,689.01108817782142,1095.2865776791755,1259.217877094972,30.236031107205481,1.2019230736510493,0.24808165499976526,0.25717069083115046,1.9895518957292124,22.322416748966521,0,-18.081157566662881,0,0,0,0,0,0.248687204026111,0.35378063922251174,2.984246448313332,8.4907353413402813,5.4053700002374283,370.97271336132036,300.72611337485046,2892.9852106660614,9.2323860076631709E-2,9.1716086222527657,-50148.825891203611,689.01108817782142,3.9364738174115635E-2,3.1967965240517815,-50725.422257605962,1095.2865776791755,11.507826695530673,3.3656835099980457E-2,1.5015752743898916,-50787.567475541815,1206.3017834075395]
["AKM2G","AKM2G-65L 480 V",32.599998474121101,12.3999996185303,26.8230434782609,10.121902835079601,2300,86.800003051757798,2300,0.89600002765655495,16.399999618530298,179,2.0800000056624399,672,10,689.01108817782142,1097.9262673038825,1259.217877094972,29.842315589344011,1.2019230736510493,0.24933985442099652,0.25717069083115046,1.9895518957292124,22.322416748966521,0,-18.081157566662881,0,0,0,0,0,0.248687204026111,0.35378063922251174,2.984246448313332,8.4907353413402813,5.4053700002374283,370.97271336132036,300.72611337485046,2892.9852106660614,9.2323860076631709E-2,9.1716086222527657,-50148.825891203611,689.01108817782142,3.9202562882575821E-2,3.1612037923373317,-50727.187953117194,1097.9262673038825,11.379699995845932,3.3656835099980457E-2,1.5015752743898916,-50787.567475541815,1206.3017834075395]
["AKM2G","AKM2G-65M 240 V",32.599998474121101,15.300000190734901,30.2871428571429,14.152869800209199,1400,86.800003051757798,1400,0.58399999141693104,10.699999809265099,144,2.0800000056624399,336,10,869.57432390692099,1370.4864056496842,1400,30.33590048747886,1.2019230736510493,0.24630121513917455,0.25717069083115046,1.7142857142857142,22.322416748966521,0,-18.081157566662881,0,0,0,0,0,0.30684793436177554,0.43651967855659474,3.6821752123413067,10.476472285358273,6.6695294015200597,370.97271336132036,300.72611337485046,2892.9852106660614,5.9803285990138733E-2,5.9337542682461057,-50380.663475647081,869.57432390692099,2.5508542145440287E-2,2.0739478052514322,-50753.302608278995,1370.4864056496842,14.238422056284435,2.178316816494099E-2,0.97147393227027301,-50793.781701375861,1504.8841678752551]
["AKM2G","AKM2G-65M 400 V",32.599998474121101,15.300000190734901,26.7002083333333,12.476732254426199,2400,86.800003051757798,2400,0.58399999141693104,10.699999809265099,144,2.0800000056624399,560,10,869.57432390692099,1379.8594084286522,1565.2777777777778,29.207964751820832,1.2019230736510493,0.24914866035374114,0.25717069083115046,1.594807129500577,22.322416748966521,0,-18.081157566662881,0,0,0,0,0,0.30684793436177554,0.43651967855659474,3.6821752123413067,10.476472285358273,6.6695294015200597,370.97271336132036,300.72611337485046,2892.9852106660614,5.9803285990138733E-2,5.9337542682461057,-50380.663475647081,869.57432390692099,2.5203527315549604E-2,2.0065803016613279,-50756.616832236024,1379.8594084286522,13.775919120306318,2.178316816494099E-2,0.97147393227027301,-50793.781701375861,1504.8841678752551]
["AKM2G","AKM2G-65M 480 V",32.599998474121101,15.300000190734901,24.303103448275898,11.3565898396833,2900,86.800003051757798,2900,0.58399999141693104,10.699999809265099,144,2.0800000056624399,672,10,869.57432390692099,1384.6384687095117,1565.2777777777778,28.638550190110802,1.2019230736510493,0.25059594808681623,0.25717069083115046,1.594807129500577,22.322416748966521,0,-18.081157566662881,0,0,0,0,0,0.30684793436177554,0.43651967855659474,3.6821752123413067,10.476472285358273,6.6695294015200597,370.97271336132036,300.72611337485046,2892.9852106660614,5.9803285990138733E-2,5.9337542682461057,-50380.663475647081,869.57432390692099,2.5050713105557135E-2,1.9719636182380271,-50758.277277781948,1384.6384687095117,13.538262730149482,2.178316816494099E-2,0.97147393227027301,-50793.781701375861,1504.8841678752551]
["AKM2G","AKM2G-65N 240 V",32.700000762939503,19,29.492647058823501,17.047772678417999,1700,87,1700,0.37799999117851302,7,117,2.0800000056624399,336,10,1083.9531915296188,1700,1700,29.492647058823501,1.2019230736510493,0.2463472386778244,0.25657950286168413,1.411764705882353,22.322416748966521,0,-18.081157566662881,0,0,0,0,0,0.37988765933891111,0.54042546933598035,4.5586519120669333,12.970211264063527,8.2570929424875636,370.97271336132036,300.72611337485046,2892.9852106660614,3.943470386746821E-2,3.8722498319074101,-50531.32117392237,1083.9531915296188,1.6652914726203102E-2,1.3138441058017092,-50773.634937279028,1707.1173158280399,17.151636274143346,1.4375924385957299E-2,0.63250716842093346,-50797.853671595738,1857.9002205565109]
["AKM2G","AKM2G-65N 400 V",32.700000762939503,19,23.628548387096799,13.6581203043866,3100,87,3100,0.37799999117851302,7,117,2.0800000056624399,560,10,1083.9531915296188,1725.1009316685102,1926.4957264957266,27.651881103212801,1.2019230736510493,0.25003271319494513,0.25657950286168413,1.291780889762266,22.322416748966521,0,-18.081157566662881,0,0,0,0,0,0.37988765933891111,0.54042546933598035,4.5586519120669333,12.970211264063527,8.2570929424875636,370.97271336132036,300.72611337485046,2892.9852106660614,3.943470386746821E-2,3.8722498319074101,-50531.32117392237,1083.9531915296188,1.6341777379778606E-2,1.2429721203960782,-50776.944284971847,1725.1009316685102,16.226434790697912,1.4375924385957299E-2,0.63250716842093346,-50797.853671595738,1857.9002205565109]
["AKM2G","AKM2G-65N 480 V",32.700000762939503,19,19.577500000000001,11.3164738636736,3800,87,3800,0.37799999117851302,7,117,2.0800000056624399,672,10,{"$f":"IF(AQ594<I594,IF(AQ594<0,0,AQ594),I594)","v":1083.9531915296188},{"$f":"IF(AU594<I594,IF(AU594<0,0,AU594),I594)","v":1734.3002887080152},{"$f":"IF(UAC_V*0.98/L594*1000<I594,IF(UAC_V*0.98/L594*1000<0,0,UAC_V*0.98/L594*1000),I594)","v":1926.4957264957266},{"$f":"C594+(E594-C594)/G594*Q594","v":26.710959483534996},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M594,(inertia/gear^2+gear_inertia)/M594),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M594,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M594))","v":1.2019230736510493},{"$f":"IF((C594+(E594-C594)/G594*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X594^2*time1+Y594^2*time2+Z594^2*time3+AA594^2*time4)/time)/(C594+(E594-C594)/G594*mspeed),SQRT((((X594-Y594)*2/PI()+Y594)^2*time1+Y594^2*time2+((Z594-Y594)*2/PI()+Y594)^2*time3+AA594^2*time4)/time)/(C594+(E594-C594)/G594*mspeed)),IF(AccType=1,SQRT((X594^2*time1+Y594^2*time2+Z594^2*time3+AA594^2*time4+AB594^2*time5+AC594^2*time6+AD594^2*time7+AE594^2*time8)/time)/(C594+(E594-C594)/G594*mspeed),SQRT((((X594-Y594)*2/PI()+Y594)^2*time1+Y594^2*time2+((Z594-Y594)*2/PI()+Y594)^2*time3+AA594^2*time4+((AB594-AC594)*2/PI()+AC594)^2*time5+AC594^2*time6+((AD594-AC594)*2/PI()+AC594)^2*time7+AE594^2*time8)/time)/(C594+(E594-C594)/G594*mspeed))))","v":0.2519434762829984},{"$f":"IF(move1,MAX(ABS(X594),ABS(Z594))/H594,MAX(ABS(X594),ABS(Z594),ABS(AB594),ABS(AD594))/H594)","v":0.25657950286168413},{"$f":"IF(AZ594>0,speed/(MIN(AZ594,I594)),\"NA\")","v":1.291780889762266},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M594+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M594+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":22.322416748966521},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M594+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M594+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-18.081157566662881},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M594+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M594+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M594+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M594+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH594/Irms","v":0.37988765933891111},{"$f":"AI594/Ipeak","v":0.54042546933598035},{"$f":"IF(move1,IF(AccType=1,SQRT((X594^2*time1+Y594^2*time2+Z594^2*time3+AA594^2*time4)/time)/(C594/D594),SQRT((((X594-Y594)*2/PI()+Y594)^2*time1+Y594^2*time2+((Z594-AA594)*2/PI()+AA594)^2*time3+AA594^2*time4)/time)/(C594/D594)),IF(AccType=1,SQRT((X594^2*time1+Y594^2*time2+Z594^2*time3+AA594^2*time4+AB594^2*time5+AC594^2*time6+AD594^2*time7+AE594^2*time8)/time)/(C594/D594),SQRT((((X594-Y594)*2/PI()+Y594)^2*time1+Y594^2*time2+((Z594-AA594)*2/PI()+AA594)^2*time3+AA594^2*time4+((AB594-AC594)*2/PI()+AC594)^2*time5+AC594^2*time6+((AD594-AE594)*2/PI()+AE594)^2*time7+AE594^2*time8)/time)/(C594/D594)))","v":4.5586519120669333},{"$f":"IF(move1,MAX(ABS(X594),ABS(Z594))/(C594/D594),MAX(ABS(X594),ABS(Z594),ABS(AB594),ABS(AD594))/(C594/D594))","v":12.970211264063527},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X594),ABS(Z594))/(C594/D594),MAX(ABS((X594-Y594)*2/PI()+Y594),ABS((Z594-Y594)*2/PI()+Y594))/(C594/D594)),IF(AccType=1,MAX(ABS(X594),ABS(Z594),ABS(AB594),ABS(AD594))/(C594/D594),MAX(ABS((X594-Y594)*2/PI()+Y594),ABS((Z594-Y594)*2/PI()+Y594),ABS((AB594-AC594)*2/PI()+AC594),ABS((AD594-AC594)*2/PI()+AC594))/(C594/D594)))","v":8.2570929424875636},{"$f":"IF((C594+(E594-C594)/G594*mspeed)<0,\"NA\",U594*(C594+(E594-C594)/G594*mspeed)*mspeed/9.55)","v":370.97271336132036},{"$f":"IF(move1,IF(speed1>speed2,AM594/2*time1/time,AM594/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z594*-speed/30*PI(),((Z594-AA594)*2/PI()+AA594)*-speed/30*PI()),IF(AccType=1,X594*-speed/30*PI(),((X594-Y594)*2/PI()+Y594)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z594*-speed/30*PI(),((Z594-AA594)*2/PI()+AA594)*-speed/30*PI()),IF(AccType=1,X594*-speed/30*PI(),((X594-Y594)*2/PI()+Y594)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD594*-speed/30*PI(),((AD594-AE594)*2/PI()+AE594)*-speed/30*PI()),IF(AccType=1,AB594*-speed/30*PI(),((AB594-AC594)*2/PI()+AC594)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD594*-speed/30*PI(),((AD594-AE594)*2/PI()+AE594)*-speed/30*PI()),IF(AccType=1,AB594*-speed/30*PI(),((AB594-AC594)*2/PI()+AC594)*-speed/30*PI()),0)/2*time7/time)))","v":300.72611337485046},{"$f":"IF(move1,MAX(IF(AccType=1,Z594*-speed/30*PI(),((Z594-AA594)*2/PI()+AA594)*-speed/30*PI()),IF(AccType=1,X594*-speed/30*PI(),((X594-Y594)*2/PI()+Y594)*-speed/30*PI()),0),MAX(IF(AccType=1,Z594*-speed/30*PI(),((Z594-AA594)*2/PI()+AA594)*-speed/30*PI()),IF(AccType=1,X594*-speed/30*PI(),((X594-Y594)*2/PI()+Y594)*-speed/30*PI()),IF(AccType=1,AD594*-speed/30*PI(),((AD594-AE594)*2/PI()+AE594)*-speed/30*PI()),IF(AccType=1,AB594*-speed/30*PI(),((AB594-AC594)*2/PI()+AC594)*-speed/30*PI()),0))","v":2892.9852106660614},{"$f":"(L594^2)/1000000+((K594/1000)^2*(D594/C594*H594)^2*PI()*PI()*(O594/2)^2)/1200","v":3.943470386746821E-2},{"$f":"SQRT(3)*L594*J594*D594/C594*H594/1000","v":3.8722498319074101},{"$f":"0.75*J594^2*(D594/C594*H594)^2-(UAC_V*0.98)^2","v":-50531.32117392237},{"$f":"-AO594/2/AN594+SQRT((AO594/2/AN594)^2-AP594/AN594)","v":1083.9531915296188},{"$f":"(L594^2)/1000000+((K594/1000)^2*AV594^2*PI()*PI()*(O594/2)^2)/1200","v":1.6186859747214795E-2},{"$f":"SQRT(3)*L594*J594*AV594/1000","v":1.2061324709783252},{"$f":"0.75*J594^2*AV594^2-(UAC_V*0.98)^2","v":-50778.592034159759},{"$f":"-AS594/2/AR594+SQRT((AS594/2/AR594)^2-AT594/AR594)","v":1734.3002887080152},{"$f":"D594+(F594-D594)*((0.85*UAC_V-D594*J594)/L594*1000)/G594","v":15.74550995000329},{"$f":"(L594^2)/1000000+((K594/1000)^2*AJ594^2*PI()*PI()*(O594/2)^2)/1200","v":1.4375924385957299E-2},{"$f":"SQRT(3)*L594*J594*AJ594/1000","v":0.63250716842093346},{"$f":"0.75*J594^2*AJ594^2-(UAC_V*0.98)^2","v":-50797.853671595738},{"$f":"IF(((AX594/2/AW594)^2-AY594/AW594)>0,-AX594/2/AW594+SQRT((AX594/2/AW594)^2-AY594/AW594),-9999)","v":1857.9002205565109}]
["AKM2G","AKM2G-71L 240 V",22.899999618530298,12.1000003814697,21.264666666666699,11.1919299650016,1500,49.5,1500,0.84500002861022905,17.600000381469702,127,2.5899999309331201,336,8,1016.6946681025908,1496.6656000368027,1500,21.26830190275637,0.96525099099107114,0.38912184632311531,0.50117374429899664,1.6,24.808100342800333,0,-20.094561277668273,0,0,0,0,0,0.38392956282523211,0.54617545235045106,4.6071547539027851,13.108210856410826,8.3449462115545199,412.28189586302858,334.21307738325606,3215.1298044269233,4.4014218518288586E-2,4.8615659300578358,-50438.819506288382,1016.6946681025908,2.1257666038517135E-2,2.0849294498593194,-50737.782437676076,1496.6656000368027,11.216833978113968,1.8967643932617424E-2,1.5511172000860294,-50767.867474604711,1595.6392003948706]
["AKM2G","AKM2G-71L 400 V",22.899999618530298,12.1000003814697,18.9898076923077,9.99463575294652,2600,49.5,2600,0.84500002861022905,17.600000381469702,127,2.5899999309331201,560,8,1016.6946681025908,1507.2545122859619,1774.8031496062993,20.633209455182932,0.96525099099107114,0.39239316099644639,0.50117374429899664,1.5040994226051072,24.808100342800333,0,-20.094561277668273,0,0,0,0,0,0.38392956282523211,0.54617545235045106,4.6071547539027851,13.108210856410826,8.3449462115545199,412.28189586302858,334.21307738325606,3215.1298044269233,4.4014218518288586E-2,4.8615659300578358,-50438.819506288382,1016.6946681025908,2.0988638833175262E-2,2.0295097901957218,-50741.316767491786,1507.2545122859619,10.918678507379887,1.8967643932617424E-2,1.5511172000860294,-50767.867474604711,1595.6392003948706]
["AKM2G","AKM2G-71L 480 V",22.899999618530298,12.1000003814697,17.518281250000001,9.2201481420134002,3200,49.5,3200,0.84500002861022905,17.600000381469702,127,2.5899999309331201,672,8,1016.6946681025908,1511.912864214225,1774.8031496062993,20.357284233230626,0.96525099099107114,0.39381661271236451,0.50117374429899664,1.5040994226051072,24.808100342800333,0,-20.094561277668273,0,0,0,0,0,0.38392956282523211,0.54617545235045106,4.6071547539027851,13.108210856410826,8.3449462115545199,412.28189586302858,334.21307738325606,3215.1298044269233,4.4014218518288586E-2,4.8615659300578358,-50438.819506288382,1016.6946681025908,2.0872212512338846E-2,2.0050510993931603,-50742.846311749374,1511.912864214225,10.787091765165245,1.8967643932617424E-2,1.5511172000860294,-50767.867474604711,1595.6392003948706]
["AKM2G","AKM2G-71N 120 V",22.700000762939499,17.299999237060501,22.010476190476201,16.674602512014001,1050,49.299999237060497,1050,0.40700000524520902,8.5,88.300003051757798,2.5899999309331201,168,8,1050,1050,1050,22.010476190476201,0.96525099099107114,0.38919537751077582,0.50320691129242934,2.2857142857142856,24.808100342800333,0,-20.094561277668273,0,0,0,0,0,0.5537603515335332,0.78777551868348883,6.6451242184023984,18.906612448403731,12.036323313144864,412.28189586302858,334.21307738325606,3215.1298044269233,2.121868497178743E-2,2.338745072596228,-50629.778272910356,1490.5709691637187,1.0239629093879706E-2,0.99773702244443907,-50773.240891959926,2178.5833456848372,16.028774786541497,9.1743030502101034E-3,0.74922042037293624,-50787.16143905124,2312.3510890007469]
["AKM2G","AKM2G-71N 240 V",22.700000762939499,17.299999237060501,19.881363636363599,15.061638519961599,2200,49.299999237060497,2200,0.40700000524520902,8.5,88.300003051757798,2.5899999309331201,336,8,1490.5709691637187,2200,2200,19.881363636363599,0.96525099099107114,0.3941568090209942,0.50320691129242934,1.0909090909090908,24.808100342800333,0,-20.094561277668273,0,0,0,0,0,0.5537603515335332,0.78777551868348883,6.6451242184023984,18.906612448403731,12.036323313144864,412.28189586302858,334.21307738325606,3215.1298044269233,2.121868497178743E-2,2.338745072596228,-50629.778272910356,1490.5709691637187,9.9729312968404645E-3,0.94169682646328567,-50776.725814970021,2209.7063932628416,15.128481763260829,9.1743030502101034E-3,0.74922042037293624,-50787.16143905124,2312.3510890007469]
["AKM2G","AKM2G-71N 400 V",22.700000762939499,17.299999237060501,15.232250000000001,11.539582874791501,4000,49.299999237060497,4000,0.40700000524520902,8.5,88.300003051757798,2.5899999309331201,560,8,1490.5709691637187,2240.4392060410032,2552.6612934303057,18.517240365381433,0.96525099099107114,0.39892658525130353,0.50320691129242934,1.0379046726148879,24.808100342800333,0,-20.094561277668273,0,0,0,0,0,0.5537603515335332,0.78777551868348883,6.6451242184023984,18.906612448403731,12.036323313144864,412.28189586302858,334.21307738325606,3215.1298044269233,2.121868497178743E-2,2.338745072596228,-50629.778272910356,1490.5709691637187,9.7211571771965242E-3,0.88554415173277878,-50780.015731244668,2240.4392060410032,14.226381754270399,9.1743030502101034E-3,0.74922042037293624,-50787.16143905124,2312.3510890007469]
["AKM2G","AKM2G-71N 480 V",22.700000762939499,17.299999237060501,11.9667346938776,9.0657077411835303,4900,49.299999237060497,4900,0.40700000524520902,8.5,88.300003051757798,2.5899999309331201,672,8,1490.5709691637187,2257.6651022015512,2552.6612934303057,17.754670102375197,0.96525099099107114,0.40161092754438976,0.50320691129242934,1.0379046726148879,24.808100342800333,0,-20.094561277668273,0,0,0,0,0,0.5537603515335332,0.78777551868348883,6.6451242184023984,18.906612448403731,12.036323313144864,412.28189586302858,334.21307738325606,3215.1298044269233,2.121868497178743E-2,2.338745072596228,-50629.778272910356,1490.5709691637187,9.58487988629886E-3,0.85361110730269574,-50781.796457865115,2257.6651022015512,13.713373250121272,9.1743030502101034E-3,0.74922042037293624,-50787.16143905124,2312.3510890007469]
["AKM2G","AKM2G-71P 120 V",23,21.100000381469702,21.818076923076902,19.8346149547117,1300,49.799999237060497,1300,0.27399998903274497,5.8000001907348597,73.300003051757798,2.5899999309331201,168,8,1300,1300,1300,21.818076923076902,0.96525099099107114,0.38599096169826747,0.49815463298920043,1.8461538461538463,24.808100342800333,0,-20.094561277668273,0,0,0,0,0,0.66658612963223807,0.94828066430548119,7.9990335555868572,22.758735943331548,14.488661295617623,412.28189586302858,334.21307738325606,3215.1298044269233,1.4612687327506285E-2,1.5892752816181062,-50687.634994349166,1808.8695163251507,6.9012205405062929E-3,0.6463630162967765,-50785.720503097575,2666.3125913409922,18.580668428582907,6.3021799206077244E-3,0.50401495797274742,-50793.339961961457,2799.2458399115044]
["AKM2G","AKM2G-71P 240 V",23,21.100000381469702,18.958518518518499,17.235016461457899,2700,49.799999237060497,2700,0.27399998903274497,5.8000001907348597,73.300003051757798,2.5899999309331201,336,8,1808.8695163251507,2700,2700,18.958518518518499,0.96525099099107114,0.39057928728011787,0.49815463298920043,0.88888888888888884,24.808100342800333,0,-20.094561277668273,0,0,0,0,0,0.66658612963223807,0.94828066430548119,7.9990335555868572,22.758735943331548,14.488661295617623,412.28189586302858,334.21307738325606,3215.1298044269233,1.4612687327506285E-2,1.5892752816181062,-50687.634994349166,1808.8695163251507,6.7123903518752585E-3,0.60511686917224972,-50788.122316608613,2705.9899088895186,17.394986444381171,6.3021799206077244E-3,0.50401495797274742,-50793.339961961457,2799.2458399115044]
["AKM2G","AKM2G-71P 400 V",23,21.100000381469702,12.044693877551,10.949721469535699,4900,49.799999237060497,4900,0.27399998903274497,5.8000001907348597,73.300003051757798,2.5899999309331201,560,8,1808.8695163251507,2759.9636926609542,3075.0339783866448,16.829337318378471,0.96525099099107114,0.39650574074176015,0.49815463298920043,0.85737378467475867,24.808100342800333,0,-20.094561277668273,0,0,0,0,0,0.66658612963223807,0.94828066430548119,7.9990335555868572,22.758735943331548,14.488661295617623,412.28189586302858,334.21307738325606,3215.1298044269233,1.4612687327506285E-2,1.5892752816181062,-50687.634994349166,1808.8695163251507,6.4694195698666423E-3,0.54749228278297846,-50791.212767935525,2759.9636926609542,15.738481808383142,6.3021799206077244E-3,0.50401495797274742,-50793.339961961457,2799.2458399115044]
["AKM2G","AKM2G-72L 240 V",40.5,12.300000190734901,38.6244444444444,11.669016650196699,900,89.699996948242202,900,0.94999998807907104,22.600000381469702,221,4.6799997799098501,336,8,665.40649733584405,898.54781364939379,900,38.627470729086156,0.53418805930972868,0.31091705092446975,0.39012855223215603,2.6666666666666665,34.994529944646544,0,-28.345569255163696,0,0,0,0,0,0.31128514422554204,0.4428320215985912,3.7354217307065043,10.627968518366188,6.7659748988921038,581.56855829557708,471.44397929586188,4535.2910808261913,9.8722605279692247E-2,9.9064721766164396,-50302.82491786575,665.40649733584405,5.8068386888980798E-2,4.260770856289505,-50712.235160777804,898.54781364939379,11.71687178710385,5.1917919537750969E-2,2.4604065989111175,-50774.173735222634,965.51239133663421]
["AKM2G","AKM2G-72L 400 V",40.5,12.300000190734901,36.105161290322599,10.907903901654899,1550,89.699996948242202,1550,0.94999998807907104,22.600000381469702,221,4.6799997799098501,560,8,665.40649733584405,900.97841733712062,1019.9095022624433,37.945383983808348,0.53418805930972868,0.31360699683100957,0.39012855223215603,2.4857267721623879,34.994529944646544,0,-28.345569255163696,0,0,0,0,0,0.31128514422554204,0.4428320215985912,3.7354217307065043,10.627968518366188,6.7659748988921038,581.56855829557708,471.44397929586188,4535.2910808261913,9.8722605279692247E-2,9.9064721766164396,-50302.82491786575,665.40649733584405,5.7812069170159755E-2,4.2011763889122591,-50714.816420575167,900.97841733712062,11.552990471484822,5.1917919537750969E-2,2.4604065989111175,-50774.173735222634,965.51239133663421]
["AKM2G","AKM2G-72L 480 V",40.5,12.300000190734901,34.229210526315804,10.341151395178599,1900,89.699996948242202,1900,0.94999998807907104,22.600000381469702,221,4.6799997799098501,672,8,665.40649733584405,902.61132984669041,1019.9095022624433,37.52100756524699,0.53418805930972868,0.31529516046614231,0.39012855223215603,2.4857267721623879,34.994529944646544,0,-28.345569255163696,0,0,0,0,0,0.31128514422554204,0.4428320215985912,3.7354217307065043,10.627968518366188,6.7659748988921038,581.56855829557708,471.44397929586188,4535.2910808261913,9.8722605279692247E-2,9.9064721766164396,-50302.82491786575,665.40649733584405,5.7641289373979596E-2,4.1609959195610635,-50716.536266647883,902.61132984669041,11.442496520128893,5.1917919537750969E-2,2.4604065989111175,-50774.173735222634,965.51239133663421]
["AKM2G","AKM2G-72N 240 V",41.099998474121101,18.700000762939499,37.3814285714286,16.991558073276298,1400,90.400001525878906,1400,0.40500000119209301,10,147,4.6799997799098501,336,8,1026.6672046079441,1377.4374446763813,1400,37.441357456538775,0.53418805930972868,0.30825497504120158,0.38710762559698214,1.7142857142857142,34.994529944646544,0,-28.345569255163696,0,0,0,0,0,0.46634585226271996,0.66342027672219739,5.5961502271526395,15.922086641332738,10.136315173222155,581.56855829557708,471.44397929586188,4535.2910808261913,4.3871554446880318E-2,4.24132197734943,-50597.042871540252,1026.6672046079441,2.5474954991380472E-2,1.7674296745203266,-50769.019877199607,1377.4374446763813,17.139934414285399,2.2961068496075234E-2,1.045232950979784,-50792.52045256822,1464.7311709578528]
["AKM2G","AKM2G-72N 400 V",41.099998474121101,18.700000762939499,31.952708333333302,14.523958018535,2400,90.400001525878906,2400,0.40500000119209301,10,147,4.6799997799098501,560,8,1026.6672046079441,1386.6203245109293,1533.3333333333335,35.815074131031601,0.53418805930972868,0.31233851334406382,0.38710762559698214,1.6385259272051496,34.994529944646544,0,-28.345569255163696,0,0,0,0,0,0.46634585226271996,0.66342027672219739,5.5961502271526395,15.922086641332738,10.136315173222155,581.56855829557708,471.44397929586188,4535.2910808261913,4.3871554446880318E-2,4.24132197734943,-50597.042871540252,1026.6672046079441,2.5181053021089694E-2,1.698919080496641,-50771.767362186183,1386.6203245109293,16.475541875686432,2.2961068496075234E-2,1.045232950979784,-50792.52045256822,1464.7311709578528]
["AKM2G","AKM2G-72N 480 V",41.099998474121101,18.700000762939499,28.419482758620699,12.917946428475,2900,90.400001525878906,2900,0.40500000119209301,10,147,4.6799997799098501,672,8,1026.6672046079441,1391.0505626437664,1533.3333333333335,35.01750243251422,0.53418805930972868,0.31436159742055197,0.38710762559698214,1.6385259272051496,34.994529944646544,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-28.345569255163696,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.46634585226271996,0.66342027672219739,5.5961502271526395,15.922086641332738,10.136315173222155,581.56855829557708,471.44397929586188,4535.2910808261913,4.3871554446880318E-2,4.24132197734943,-50597.042871540252,1026.6672046079441,2.5041749274301743E-2,1.6654622283378939,-50773.069615969966,1391.0505626437664,16.151088654165751,2.2961068496075234E-2,1.045232950979784,-50792.52045256822,1464.7311709578528]
["AKM2G","AKM2G-72P 240 V",40.5,21.200000762939499,36.110937499999999,18.7103308193761,1600,89.599998474121094,1600,0.31499999761581399,7.6999998092651403,129,4.6799997799098501,336,8,1176.1096425443973,1582.5105039279438,1600,36.158914057096098,0.53418805930972868,0.31327438252206879,0.39056395692633761,1.5,34.994529944646544,0,-28.345569255163696,0,0,0,0,0,0.53652399940970508,0.76325520733046914,6.4382879929164609,18.318124975931259,11.661680552378263,581.56855829557708,471.44397929586188,4535.2910808261913,3.3804174658646935E-2,3.3010320714218944,-50641.455704336346,1176.1096425443973,1.9434641314789804E-2,1.3317915503345337,-50778.513934055314,1582.5105039279438,18.922362886917039,1.7702065495655072E-2,0.82077104826564984,-50795.039437628882,1670.9182714880433]
["AKM2G","AKM2G-72P 400 V",40.5,21.200000762939499,29.025178571428601,15.0389530364005,2800,89.599998474121094,2800,0.31499999761581399,7.6999998092651403,129,4.6799997799098501,560,8,1176.1096425443973,1595.1821652624203,1747.2868217054265,33.962703395561377,0.53418805930972868,0.31823380776267413,0.39056395692633761,1.4363359602637356,34.994529944646544,0,-28.345569255163696,0,0,0,0,0,0.53652399940970508,0.76325520733046914,6.4382879929164609,18.318124975931259,11.661680552378263,581.56855829557708,471.44397929586188,4535.2910808261913,3.3804174658646935E-2,3.3010320714218944,-50641.455704336346,1176.1096425443973,1.9163099564896088E-2,1.2654122848587919,-50781.103929891964,1595.1821652624203,17.979232898456399,1.7702065495655072E-2,0.82077104826564984,-50795.039437628882,1670.9182714880433]
["AKM2G","AKM2G-72P 480 V",40.5,21.200000762939499,24.240147058823499,12.559662029846599,3400,89.599998474121094,3400,0.31499999761581399,7.6999998092651403,129,4.6799997799098501,672,8,1176.1096425443973,1601.7673865590466,1747.2868217054265,32.839852308405085,0.53418805930972868,0.32079805798606592,0.39056395692633761,1.4363359602637356,34.994529944646544,0,-28.345569255163696,0,0,0,0,0,0.53652399940970508,0.76325520733046914,6.4382879929164609,18.318124975931259,11.661680552378263,581.56855829557708,471.44397929586188,4535.2910808261913,3.3804174658646935E-2,3.3010320714218944,-50641.455704336346,1176.1096425443973,1.9025046983353527E-2,1.2302923901516476,-50782.420690985142,1601.7673865590466,17.480242352952509,1.7702065495655072E-2,0.82077104826564984,-50795.039437628882,1670.9182714880433]
["AKM2G","AKM2G-73L 400 V",56.599998474121101,11.6000003814697,52.479523809523798,10.710106691454801,1050,127.300003051758,1050,1.2400000095367401,31.200000762939499,328,6.7699998617172197,560,8,461.77198088179347,609.61970500266193,687.19512195121956,54.207691284118482,0.36927622615429001,0.28962946418205393,0.35491720029978235,3.6648993291406398,45.1809606812837,0,-36.5965781518398,0,0,0,0,0,0.27120967651844757,0.38582094763489655,3.2545161182213711,9.2597027432375167,5.8949098525913373,750.85523958703686,608.67489649629601,5855.4525042943678,0.1947782180791876,18.379181123077753,-50020.205223372213,461.77198088179347,0.12345832610902119,7.8420564260681767,-50662.25341307807,609.61970500266193,11.13201552362605,0.1120354554098517,4.1527264844801905,-50765.086343008945,654.86109834366493]
["AKM2G","AKM2G-73L 480 V",56.599998474121101,11.6000003814697,50.615000000000002,10.3295916356925,1300,127.300003051758,1300,1.2400000095367401,31.200000762939499,328,6.7699998617172197,672,8,461.77198088179347,610.304298773563,687.19512195121956,53.790252091883161,0.36927622615429001,0.29125964476781735,0.35491720029978235,3.6648993291406398,45.1809606812837,0,-36.5965781518398,0,0,0,0,0,0.27120967651844757,0.38582094763489655,3.2545161182213711,9.2597027432375167,5.8949098525913373,750.85523958703698,608.67489649629601,5855.4525042943678,0.1947782180791876,18.379181123077753,-50020.205223372213,461.77198088179347,0.12325469651256887,7.7915966803959131,-50664.086562430391,610.304298773563,11.060386522044956,0.1120354554098517,4.1527264844801905,-50765.086343008945,654.86109834366493]
["AKM2G","AKM2G-73N 240 V",57.799999237060497,17.600000381469702,54.647222222222197,16.559764549046498,900,129.60000610351599,900,0.53700000047683705,14.199999809265099,221,6.7699998617172197,336,8,704.52384449188776,900,900,54.647222222222197,0.36927622615429001,0.28246738154310314,0.34861850735713784,2.6666666666666665,45.1809606812837,0,-36.5965781518398,0,0,0,0,0,0.40294747735122388,0.57323020164498262,4.8353697282146868,13.757524839479583,8.7583123316508384,750.85523958703698,608.67489649629601,5855.4525042943678,9.0164290103150926E-2,8.1117966240711734,-50468.34643931179,704.52384449188776,5.617670196095418E-2,3.4177512177314004,-50745.368925972522,920.49692790060067,16.626975604609388,5.0876429273581533E-2,1.8003113343399182,-50788.569835483751,981.59983113336489]
["AKM2G","AKM2G-73N 400 V",57.799999237060497,17.600000381469702,49.480937500000003,14.994223701509201,1600,129.60000610351599,1600,0.53700000047683705,14.199999809265099,221,6.7699998617172197,560,8,704.52384449188776,923.99752028714954,1019.9095022624433,52.995753976960742,0.36927622615429001,0.28636926637877913,0.34861850735713784,2.4449881956773933,45.1809606812837,0,-36.5965781518398,0,0,0,0,0,0.40294747735122388,0.57323020164498262,4.8353697282146868,13.757524839479583,8.7583123316508384,750.85523958703686,608.67489649629601,5855.4525042943678,9.0164290103150926E-2,8.1117966240711734,-50468.34643931179,704.52384449188776,5.5829698012583848E-2,3.3359362674083726,-50748.197249543366,923.99752028714954,16.228955065239568,5.0876429273581533E-2,1.8003113343399182,-50788.569835483751,981.59983113336489]
["AKM2G","AKM2G-73N 480 V",57.799999237060497,17.600000381469702,46.593947368421098,14.1193781944501,1900,129.60000610351599,1900,0.53700000047683705,14.199999809265099,221,6.7699998617172197,672,8,704.52384449188776,925.49238957900423,1019.9095022624433,52.341517278295584,0.36927622615429001,0.28800748458221848,0.34861850735713784,2.4449881956773933,45.1809606812837,0,-36.5965781518398,0,0,0,0,0,0.40294747735122388,0.57323020164498262,4.8353697282146868,13.757524839479583,8.7583123316508384,750.85523958703698,608.67489649629601,5855.4525042943678,9.0164290103150926E-2,8.1117966240711734,-50468.34643931179,704.52384449188776,5.5683074672840963E-2,3.3007566917333455,-50749.392331760093,925.49238957900423,16.057810382883943,5.0876429273581533E-2,1.8003113343399182,-50788.569835483751,981.59983113336489]
["AKM2G","AKM2G-73Q 240 V",57.099998474121101,27.399999618530298,49.978333333333303,23.913079131966199,1500,128.10000610351599,1500,0.216999992728233,5.6999998092651403,140,6.7699998617172197,336,8,1146.0811130621296,1486.8086245656668,1500,50.04096303905979,0.36927622615429001,0.28895417218404851,0.35270069108953467,1.6,45.1809606812837,0,-36.5965781518398,0,0,0,0,0,0.63500633333109313,0.90335547177019182,7.6200759999731176,21.680531322484605,13.802254915328367,750.85523958703698,608.67489649629601,5855.4525042943678,3.5755313326423621E-2,3.2345360279671183,-50671.713274027847,1146.0811130621296,2.2114801223319935E-2,1.2761629493583153,-50784.387144473025,1486.8086245656668,24.252569026731877,2.0414494681193586E-2,0.72627053740682801,-50798.43208043999,1559.7630319723819]
["AKM2G","AKM2G-73Q 400 V",57.099998474121101,27.399999618530298,38.934615384615398,18.629003341414201,2600,128.10000610351599,2600,0.216999992728233,5.6999998092651403,140,6.7699998617172197,560,8,1146.0811130621296,1498.0422635460859,1610,46.633647858126906,0.36927622615429001,0.29436954294101447,0.35270069108953467,1.5386952702457022,45.1809606812837,0,-36.5965781518398,0,0,0,0,0,0.63500633333109313,0.90335547177019182,7.6200759999731176,21.680531322484605,13.802254915328367,750.85523958703698,608.67489649629601,5855.4525042943678,3.5755313326423621E-2,3.2345360279671183,-50671.713274027847,1146.0811130621296,2.18289181592481E-2,1.2014379928271532,-50786.748606497342,1498.0422635460859,22.832474385054027,2.0414494681193586E-2,0.72627053740682801,-50798.43208043999,1559.7630319723819]
["AKM2G","AKM2G-73Q 480 V",57.099998474121101,27.399999618530298,30.739062499999999,14.7076860107037,3200,128.10000610351599,3200,0.216999992728233,5.6999998092651403,140,6.7699998617172197,672,8,1146.0811130621296,1504.2338069990901,1610,44.708432512742519,0.36927622615429001,0.29748500307229325,0.35270069108953467,1.5386952702457022,45.1809606812837,0,-36.5965781518398,0,0,0,0,0,0.63500633333109313,0.90335547177019182,7.6200759999731176,21.680531322484605,13.802254915328367,750.85523958703698,608.67489649629601,5855.4525042943678,3.5755313326423621E-2,3.2345360279671183,-50671.713274027847,1146.0811130621296,2.1674944396744486E-2,1.1591977561425872,-50788.020466354006,1504.2338069990901,22.029728735360123,2.0414494681193586E-2,0.72627053740682801,-50798.43208043999,1559.7630319723819]
["AKM2G","AKM2G-74P 240 V",72.199996948242202,23.100000381469702,66.468000000000004,21.168152159035799,1000,164.60000610351599,1000,0.34099999070167503,9.1999998092651403,210,8.8600004091858899,336,8,778.73816517098976,989.31166943345033,1000,66.529265478189274,0.28216702985792697,0.27955126859508628,0.33637540482642897,2.4,55.367393687502869,0,-44.847588886877318,0,0,0,0,0,0.5188442688518955,0.73810414898583898,6.226131226222746,17.714499575660135,11.277400687462372,920.14195859632116,745.90584427238775,7175.6142219003696,7.4990392625680247E-2,6.5318912282748824,-50563.291502165455,778.73816517098976,4.9188455072803908E-2,2.6510639378723155,-50765.317936492705,989.31166943345033,21.374005305200459,4.5516550759135334E-2,1.3987603094771273,-50794.068557804036,1041.1303713473562]
["AKM2G","AKM2G-74P 400 V",72.199996948242202,23.100000381469702,57.861764705882401,18.427312984961901,1700,164.60000610351599,1700,0.34099999070167503,9.1999998092651403,210,8.8600004091858899,560,8,778.73816517098976,993.60144992846961,1073.3333333333333,63.819709686230539,0.28216702985792697,0.28453897887964302,0.33637540482642897,2.3051868104607229,55.367393687502869,0,-44.847588886877318,0,0,0,0,0,0.5188442688518955,0.73810414898583898,6.226131226222746,17.714499575660135,11.277400687462372,920.14195859632116,745.90584427238775,7175.6142219003696,7.4990392625680247E-2,6.5318912282748824,-50563.291502165455,778.73816517098976,4.8846924297102787E-2,2.5605507194708603,-50767.992086241597,993.60144992846961,20.644249231547946,4.5516550759135334E-2,1.3987603094771273,-50794.068557804036,1041.1303713473562]
["AKM2G","AKM2G-74P 480 V",72.199996948242202,23.100000381469702,52.297619047619101,16.655292133888299,2100,164.60000610351599,2100,0.34099999070167503,9.1999998092651403,210,8.8600004091858899,672,8,778.73816517098976,995.26416016584619,1073.3333333333333,62.767557221305559,0.28216702985792697,0.28651216919243577,0.33637540482642897,2.3051868104607229,55.367393687502869,0,-44.847588886877318,0,0,0,0,0,0.5188442688518955,0.73810414898583898,6.226131226222746,17.714499575660135,11.277400687462372,920.14195859632116,745.90584427238775,7175.6142219003696,7.4990392625680247E-2,6.5318912282748824,-50563.291502165455,778.73816517098976,4.8716245704059691E-2,2.525059918325427,-50769.015285764552,995.26416016584619,20.358107293916248,4.5516550759135334E-2,1.3987603094771273,-50794.068557804036,1041.1303713473562]
["AKM2G","AKM2G-74Q 240 V",71.699996948242202,28.799999237060501,63.946800000000003,25.578720000000001,1250,163.80000305175801,1250,0.216999992728233,5.9000000953674299,167,8.8600004091858899,336,8,987.9158828172915,1250,1250,63.946800000000003,0.28216702985792697,0.28244210676830639,0.33801827018286268,1.92,55.367393687502869,0,-44.847588886877318,0,0,0,0,0,0.65138170274264151,0.92665095526967312,7.8165804329116986,22.239622926472155,14.158183684991547,920.14195859632116,745.90584427238775,7175.6142219003696,4.7718739477478803E-2,4.1297528578773841,-50652.278409882514,987.9158828172915,3.0957021756743058E-2,1.6244067133570725,-50781.506434343297,1254.8082820346499,25.879623738457745,2.8807242953397177E-2,0.88867785943372501,-50798.080610833596,1312.5877503884312]
["AKM2G","AKM2G-74Q 400 V",71.699996948242202,28.799999237060501,50.7886363636364,20.3154545454546,2200,163.80000305175801,2200,0.216999992728233,5.9000000953674299,167,8.8600004091858899,560,8,987.9158828172915,1262.9848471912028,1349.7005988023952,59.695118969829245,0.28216702985792697,0.28869081875375352,0.33801827018286268,1.8284491831420591,55.367393687502869,0,-44.847588886877318,0,0,0,0,0,0.65138170274264151,0.92665095526967312,7.8165804329116986,22.239622926472155,14.158183684991547,920.14195859632116,745.90584427238775,7175.6142219003696,4.7718739477478803E-2,4.1297528578773841,-50652.278409882514,987.9158828172915,3.0622842005118046E-2,1.533388720149689,-50784.082864148215,1262.9848471912028,24.429548829096788,2.8807242953397177E-2,0.88867785943372501,-50798.080610833596,1312.5877503884312]
["AKM2G","AKM2G-74Q 480 V",71.699996948242202,28.799999237060501,41.737037037036998,16.694814814814801,2700,163.80000305175801,2700,0.216999992728233,5.9000000953674299,167,8.8600004091858899,672,8,987.9158828172915,1266.8977668813304,1349.7005988023952,57.640735096145647,0.28216702985792697,0.29180325035440441,0.33801827018286268,1.8284491831420591,55.367393687502869,0,-44.847588886877318,0,0,0,0,0,0.65138170274264151,0.92665095526967312,7.8165804329116986,22.239622926472155,14.158183684991547,920.14195859632116,745.90584427238775,7175.6142219003696,4.7718739477478803E-2,4.1297528578773841,-50652.278409882514,987.9158828172915,3.0466177491354954E-2,1.4888046719319512,-50785.290702506667,1266.8977668813304,23.719247410662128,2.8807242953397177E-2,0.88867785943372501,-50798.080610833596,1312.5877503884312]
["AKM2G","AKM2G-74R 240 V",71.300003051757798,32.5,61.515172413793103,27.834919163789699,1450,162.89999389648401,1450,0.17000000178813901,4.5999999046325701,148,8.8600004091858899,336,8,1123.763117834113,1424.9444223197374,1450,61.684251437336371,0.28216702985792697,0.2851168798562943,0.33988579350522558,1.6551724137931034,55.367393687502869,0,-44.847588886877318,0,0,0,0,0,0.73918990740070445,1.0515662797012792,8.8702788888084534,25.237590712830702,16.066749254708466,920.14195859632116,745.90584427238775,7175.6142219003696,3.7256669062549895E-2,3.2358333689306256,-50685.654229461688,1123.763117834113,2.414519594444977E-2,1.2363291781373942,-50787.714443974692,1424.9444223197374,28.370229582535217,2.2622803460454321E-2,0.70016320606871318,-50799.564806027069,1483.105306551317]
["AKM2G","AKM2G-74R 400 V",71.300003051757798,32.5,45.076000000000001,20.396379738434302,2500,162.89999389648401,2500,0.17000000178813901,4.5999999046325701,148,8.8600004091858899,560,8,1123.763117834113,1436.14141445823,1522.9729729729731,56.235452317554447,0.28216702985792697,0.29235359856359122,0.33988579350522558,1.618226291416049,55.367393687502869,0,-44.847588886877318,0,0,0,0,0,0.73918990740070445,1.0515662797012792,8.8702788888084534,25.237590712830702,16.066749254708466,920.14195859632116,745.90584427238775,7175.6142219003696,3.7256669062549895E-2,3.2358333689306256,-50685.654229461688,1123.763117834113,2.3827910226626083E-2,1.1454776150142143,-50790.184208289604,1436.14141445823,26.285445247330955,2.2622803460454321E-2,0.70016320606871318,-50799.564806027069,1483.105306551317]
["AKM2G","AKM2G-74R 480 V",71.300003051757798,32.5,34.061666666666703,15.412518587658701,3000,162.89999389648401,3000,0.17000000178813901,4.5999999046325701,148,8.8600004091858899,672,8,1123.763117834113,1441.8342701295564,1522.9729729729731,53.402833197545561,0.28216702985792697,0.29621825536122692,0.33988579350522558,1.618226291416049,55.367393687502869,0,-44.847588886877318,0,0,0,0,0,0.73918990740070445,1.0515662797012792,8.8702788888084534,25.237590712830702,16.066749254708466,920.14195859632116,745.90584427238775,7175.6142219003696,3.7256669062549895E-2,3.2358333689306256,-50685.654229461688,1123.763117834113,2.367071873825833E-2,1.0976854628260015,-50791.407792922531,1441.8342701295564,25.188751620908768,2.2622803460454321E-2,0.70016320606871318,-50799.564806027069,1483.105306551317]
["KBM","KBM-10H01-A (120 V)",0.48699999999999999,1.73,0.44870188775305436,1.5599425940517813,4150,1.17,6565,13,19,17.382100000000001,4.9200000000000008E-3,160,6,6565,6565,6565,0.42641515496356674,508.13008130081295,8.8871438003236172,10.434790447820356,"NA",12.208704823949816,0,-9.8890509073993513,0,0,0,0,0,1.270266577167851,1.8070721548111894,15.243198926014212,43.369731715468546,27.610028732344659,202.89453449872499,164.47485916672517,1582.2481451838962,7.6374634761367834E-4,1.6267065951735979,-48615.614495876362,6984.1633420898688,3.4884847190161828E-4,0.51746625424180959,-50583.595801132462,11322.803746368232,1.3221350221162802,2.067264860325671E-2,10.806202020702981,45818.099776663774,-9999]
["KBM","KBM-10H01-A (240 V)",0.48699999999999999,1.73,0.414767427451606,1.4419671375733765,9900,1.17,13766,13,19,17.382100000000001,4.9200000000000008E-3,325,6,6984.1633420898688,11126.671553299979,12967.3629768555,0.4058173626064755,508.13008130081295,8.8711129170518248,10.434790447820356,"NA",12.208704823949816,0,-9.8890509073993513,0,0,0,0,0,1.270266577167851,1.8070721548111894,15.243198926014212,43.369731715468546,27.610028732344659,202.89453449872499,164.47485916672517,1582.2481451838962,7.6374634761367834E-4,1.6267065951735979,-48615.614495876362,6984.1633420898688,3.5757999980040893E-4,0.56375954799121597,-50542.179624581426,11126.671553299979,1.4404151697654941,2.067264860325671E-2,10.806202020702981,45818.099776663774,-9999]
["KBM","KBM-10H01-A (400 V)",0.48699999999999999,1.73,0.36804580590000802,1.2795362463496316,14400,1.17,16000,13,19,17.382100000000001,4.9200000000000008E-3,565,6,6984.1633420898688,11163.039983039611,12967.3629768555,0.39478538716052325,508.13008130081295,8.8791075814329332,10.434790447820356,"NA",12.208704823949816,0,-9.8890509073993513,0,0,0,0,0,1.270266577167851,1.8070721548111894,15.243198926014212,43.369731715468546,27.610028732344659,202.89453449872499,164.47485916672517,1582.2481451838962,7.6374634761367834E-4,1.6267065951735979,-48615.614495876362,6984.1633420898688,3.5591619643894937E-4,0.55523605013734312,-50550.07152787294,11163.039983039611,1.4186374887454054,2.067264860325671E-2,10.806202020702981,45818.099776663774,-9999]
["KBM","KBM-10H01-B (120 V)",0.50900000000000001,3.37,0.4297183463481174,2.790016532580947,9000,1.19,12319,3.42,5.2,9.3041110000000007,4.9200000000000008E-3,160,6,12319,12319,12319,0.40048103429582871,508.13008130081295,8.4966655092873271,10.259415818445223,1.1913175599291019,12.208704823949816,0,-9.8890509073993513,0,0,0,0,0,2.3674992377461255,3.3679874964563594,28.409990852953506,80.831699914952623,51.459058399941782,202.89453449872499,164.47485916672517,1582.2481451838962,2.1081346565340067E-4,0.43423087158044971,-50260.617682449483,14445.035458791341,9.5357615227737545E-5,0.11550484764039251,-50766.630740183718,22475.700675054195,2.095745755170503,5.3867556039778617E-3,2.8361124843217302,-27575.805276556177,2014.5761975865021]
["KBM","KBM-10H01-B (240 V)",0.50900000000000001,3.37,0.30970691628693148,2.0108227261844664,18500,1.19,20000,3.42,5.2,9.3041110000000007,4.9200000000000008E-3,325,6,14445.035458791341,20000,20000,0.29354801760749349,508.13008130081295,8.5116090228522054,10.259415818445223,1.1913175599291019,12.208704823949816,0,-9.8890509073993513,0,0,0,0,0,2.3674992377461255,3.3679874964563594,28.409990852953506,80.831699914952623,51.459058399941782,202.89453449872499,164.47485916672517,1582.2481451838962,2.1081346565340067E-4,0.43423087158044971,-50260.617682449483,14445.035458791341,9.3923985877269214E-5,0.10566788939462363,-50772.913965924236,22694.544256081987,1.9172617875404709,5.3867556039778617E-3,2.8361124843217302,-27575.805276556177,2014.5761975865021]
["KBM","KBM-10H01-C (120 V)",0.49199999999999999,5.21,0.34500684437985052,3.8004719583592257,15500,1.23,19702,1.44,2.2000000000000002,5.8349039999999999,4.9200000000000008E-3,160,6,19702,19702,19702,0.30515747406269778,508.13008130081295,8.7981322383142846,9.9257762796339968,0.63005877531887922,12.208704823949816,0,-9.8890509073993513,0,0,0,0,0,3.7866080152388193,5.3868015017596997,45.439296182865831,129.2832360422328,82.30426430015055,202.89453449872499,164.47485916672517,1582.2481451838962,9.482626404107243E-5,0.18955470407524055,-50541.319348000005,22108.68721575549,3.5908595233953593E-5,3.3181857024775656E-2,-50797.075113008796,37152.261489945362,2.2800472816340704,2.4609414283385212E-3,1.1977858321340056,-40270.247762922656,3809.1684363658542]
["KBM","KBM-10H01-C (240 V)",0.49199999999999999,5.21,0.29520674928335428,3.2518919286555881,18600,1.23,20000,1.44,2.2000000000000002,5.8349039999999999,4.9200000000000008E-3,325,6,20000,20000,20000,0.28039435406812285,508.13008130081295,8.807076127162377,9.9257762796339968,0.63005877531887922,12.208704823949816,0,-9.8890509073993513,0,0,0,0,0,3.7866080152388193,5.3868015017596997,45.439296182865831,129.2832360422328,82.30426430015055,202.89453449872499,164.47485916672517,1582.2481451838962,9.482626404107243E-5,0.18955470407524055,-50541.319348000005,22108.68721575549,3.5230358122647138E-5,2.6459155315921103E-2,-50800.019273135484,37599.209170185713,1.818105753013004,2.4609414283385212E-3,1.1977858321340056,-40270.247762922656,3809.1684363658542]
["KBM","KBM-10H02-A (120 V)",0.876,1.53,0.85343954991306192,1.4551398975499776,2070,2.33,3359,20,36,35.4,1.03E-2,160,6,3232.9351243946576,3359,3359,0.83939103775747581,242.71844660194174,4.936662263451157,5.2510413531168476,"NA",12.234926352762255,0,-9.9102903457374243,0,0,0,0,0,0.6258882806534366,0.89038419519245871,7.5106593678412388,21.369220684619009,13.604068407914765,203.33030593877226,164.82811385841867,1585.6464553179878,2.8418987989117139E-3,4.9904203768525361,-45836.86075295553,3232.9351243946576,1.4309988553336968E-3,1.6696452530329784,-50249.022860493562,5371.024467160214,1.3615397405222756,1.9007462882929854E-2,16.682559871882919,4716.0431741673674,-9999]
["KBM","KBM-10H02-A (240 V)",0.876,1.53,0.79409940026903569,1.3539631718142127,4750,2.33,6753,20,36,35.4,1.03E-2,325,6,3232.9351243946576,5374.6830528703349,6367.2316384180795,0.78332847044338305,242.71844660194174,4.9529495132399353,5.2510413531168476,"NA",12.234926352762255,0,-9.9102903457374243,0,0,0,0,0,0.6258882806534366,0.89038419519245871,7.5106593678412388,21.369220684619009,13.604068407914765,203.33030593877226,164.82811385841867,1585.6464553179878,2.8418987989117139E-3,4.9904203768525361,-45836.86075295553,3232.9351243946576,1.4299101100079922E-3,1.6645265481743534,-50252.427581638178,5374.6830528703349,1.3573656082792962,1.9007462882929854E-2,16.682559871882919,4716.0431741673674,-9999]
["KBM","KBM-10H02-A (400 V)",0.876,1.53,0.70832694452986378,1.2077185754984889,9100,2.33,11291,20,36,35.4,1.03E-2,565,6,3232.9351243946576,5367.9663950772874,6367.2316384180795,0.7770919420743273,242.71844660194174,4.9559998165980135,5.2510413531168476,"NA",12.234926352762255,0,-9.9102903457374243,0,0,0,0,0,0.6258882806534366,0.89038419519245871,7.5106593678412388,21.369220684619009,13.604068407914765,203.33030593877226,164.82811385841867,1585.6464553179878,2.8418987989117139E-3,4.9904203768525361,-45836.86075295553,3232.9351243946576,1.4319111644315839E-3,1.6739223948584474,-50246.169890195859,5367.9663950772874,1.3650276063193048,1.9007462882929854E-2,16.682559871882919,4716.0431741673674,-9999]
["KBM","KBM-10H02-A (480 V)",0.876,1.53,0.64240722484365043,1.0953234865194381,11000,2.33,13564,20,36,35.4,1.03E-2,679,6,3232.9351243946576,5384.7023918536497,6367.2316384180795,0.76165203862689757,242.71844660194174,4.9632582578875022,5.2510413531168476,"NA",12.234926352762255,0,-9.9102903457374243,0,0,0,0,0,0.6258882806534366,0.89038419519245871,7.5106593678412388,21.369220684619009,13.604068407914765,203.33030593877226,164.82811385841867,1585.6464553179878,2.8418987989117139E-3,4.9904203768525361,-45836.86075295553,3232.9351243946576,1.4269436058521961E-3,1.6504990625304692,-50261.704424611795,5384.7023918536497,1.3459266639112875,1.9007462882929854E-2,16.682559871882919,4716.0431741673674,-9999]
["KBM","KBM-10H02-B (120 V)",0.89900000000000002,2.99,0.82321522288911386,2.6814828107137259,4350,2.48,6174,5.22,9.6999999999999993,18.536100000000001,1.03E-2,160,6,{"$f":"IF(AQ642<I642,IF(AQ642<0,0,AQ642),I642)","v":6174},{"$f":"IF(AU642<I642,IF(AU642<0,0,AU642),I642)","v":6174},{"$f":"IF(UAC_V*0.98/L642*1000<I642,IF(UAC_V*0.98/L642*1000<0,0,UAC_V*0.98/L642*1000),I642)","v":6174},{"$f":"C642+(E642-C642)/G642*Q642","v":0.79143788186606645},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M642,(inertia/gear^2+gear_inertia)/M642),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M642,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M642))","v":242.71844660194174},{"$f":"IF((C642+(E642-C642)/G642*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X642^2*time1+Y642^2*time2+Z642^2*time3+AA642^2*time4)/time)/(C642+(E642-C642)/G642*mspeed),SQRT((((X642-Y642)*2/PI()+Y642)^2*time1+Y642^2*time2+((Z642-Y642)*2/PI()+Y642)^2*time3+AA642^2*time4)/time)/(C642+(E642-C642)/G642*mspeed)),IF(AccType=1,SQRT((X642^2*time1+Y642^2*time2+Z642^2*time3+AA642^2*time4+AB642^2*time5+AC642^2*time6+AD642^2*time7+AE642^2*time8)/time)/(C642+(E642-C642)/G642*mspeed),SQRT((((X642-Y642)*2/PI()+Y642)^2*time1+Y642^2*time2+((Z642-Y642)*2/PI()+Y642)^2*time3+AA642^2*time4+((AB642-AC642)*2/PI()+AC642)^2*time5+AC642^2*time6+((AD642-AC642)*2/PI()+AC642)^2*time7+AE642^2*time8)/time)/(C642+(E642-C642)/G642*mspeed))))","v":4.825565331306108},{"$f":"IF(move1,MAX(ABS(X642),ABS(Z642))/H642,MAX(ABS(X642),ABS(Z642),ABS(AB642),ABS(AD642))/H642)","v":4.9334380454686508},{"$f":"IF(AZ642>0,speed/(MIN(AZ642,I642)),\"NA\")","v":1.0343004418339521},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M642+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M642+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.234926352762255},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M642+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M642+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-9.9102903457374243},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M642+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M642+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M642+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M642+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH642/Irms","v":1.1918483283668178},{"$f":"AI642/Ipeak","v":1.6955149144771571},{"$f":"IF(move1,IF(AccType=1,SQRT((X642^2*time1+Y642^2*time2+Z642^2*time3+AA642^2*time4)/time)/(C642/D642),SQRT((((X642-Y642)*2/PI()+Y642)^2*time1+Y642^2*time2+((Z642-AA642)*2/PI()+AA642)^2*time3+AA642^2*time4)/time)/(C642/D642)),IF(AccType=1,SQRT((X642^2*time1+Y642^2*time2+Z642^2*time3+AA642^2*time4+AB642^2*time5+AC642^2*time6+AD642^2*time7+AE642^2*time8)/time)/(C642/D642),SQRT((((X642-Y642)*2/PI()+Y642)^2*time1+Y642^2*time2+((Z642-AA642)*2/PI()+AA642)^2*time3+AA642^2*time4+((AB642-AC642)*2/PI()+AC642)^2*time5+AC642^2*time6+((AD642-AE642)*2/PI()+AE642)^2*time7+AE642^2*time8)/time)/(C642/D642)))","v":14.302179940401814},{"$f":"IF(move1,MAX(ABS(X642),ABS(Z642))/(C642/D642),MAX(ABS(X642),ABS(Z642),ABS(AB642),ABS(AD642))/(C642/D642))","v":40.692357947451768},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X642),ABS(Z642))/(C642/D642),MAX(ABS((X642-Y642)*2/PI()+Y642),ABS((Z642-Y642)*2/PI()+Y642))/(C642/D642)),IF(AccType=1,MAX(ABS(X642),ABS(Z642),ABS(AB642),ABS(AD642))/(C642/D642),MAX(ABS((X642-Y642)*2/PI()+Y642),ABS((Z642-Y642)*2/PI()+Y642),ABS((AB642-AC642)*2/PI()+AC642),ABS((AD642-AC642)*2/PI()+AC642))/(C642/D642)))","v":25.905559653606886},{"$f":"IF((C642+(E642-C642)/G642*mspeed)<0,\"NA\",U642*(C642+(E642-C642)/G642*mspeed)*mspeed/9.55)","v":203.33030593877226},{"$f":"IF(move1,IF(speed1>speed2,AM642/2*time1/time,AM642/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z642*-speed/30*PI(),((Z642-AA642)*2/PI()+AA642)*-speed/30*PI()),IF(AccType=1,X642*-speed/30*PI(),((X642-Y642)*2/PI()+Y642)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z642*-speed/30*PI(),((Z642-AA642)*2/PI()+AA642)*-speed/30*PI()),IF(AccType=1,X642*-speed/30*PI(),((X642-Y642)*2/PI()+Y642)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD642*-speed/30*PI(),((AD642-AE642)*2/PI()+AE642)*-speed/30*PI()),IF(AccType=1,AB642*-speed/30*PI(),((AB642-AC642)*2/PI()+AC642)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD642*-speed/30*PI(),((AD642-AE642)*2/PI()+AE642)*-speed/30*PI()),IF(AccType=1,AB642*-speed/30*PI(),((AB642-AC642)*2/PI()+AC642)*-speed/30*PI()),0)/2*time7/time)))","v":164.82811385841867},{"$f":"IF(move1,MAX(IF(AccType=1,Z642*-speed/30*PI(),((Z642-AA642)*2/PI()+AA642)*-speed/30*PI()),IF(AccType=1,X642*-speed/30*PI(),((X642-Y642)*2/PI()+Y642)*-speed/30*PI()),0),MAX(IF(AccType=1,Z642*-speed/30*PI(),((Z642-AA642)*2/PI()+AA642)*-speed/30*PI()),IF(AccType=1,X642*-speed/30*PI(),((X642-Y642)*2/PI()+Y642)*-speed/30*PI()),IF(AccType=1,AD642*-speed/30*PI(),((AD642-AE642)*2/PI()+AE642)*-speed/30*PI()),IF(AccType=1,AB642*-speed/30*PI(),((AB642-AC642)*2/PI()+AC642)*-speed/30*PI()),0))","v":1585.6464553179878},{"$f":"(L642^2)/1000000+((K642/1000)^2*(D642/C642*H642)^2*PI()*PI()*(O642/2)^2)/1200","v":8.1742603491368859E-4},{"$f":"SQRT(3)*L642*J642*D642/C642*H642/1000","v":1.3823329860401852},{"$f":"0.75*J642^2*(D642/C642*H642)^2-(UAC_V*0.98)^2","v":-49414.795648000007},{"$f":"-AO642/2/AN642+SQRT((AO642/2/AN642)^2-AP642/AN642)","v":6975.3703801771735},{"$f":"(L642^2)/1000000+((K642/1000)^2*AV642^2*PI()*PI()*(O642/2)^2)/1200","v":3.8048460499725162E-4},{"$f":"SQRT(3)*L642*J642*AV642/1000","v":0.38574146469242288},{"$f":"0.75*J642^2*AV642^2-(UAC_V*0.98)^2","v":-50696.89304272797},{"$f":"-AS642/2/AR642+SQRT((AS642/2/AR642)^2-AT642/AR642)","v":11047.308032028172},{"$f":"D642+(F642-D642)*((0.85*UAC_V-D642*J642)/L642*1000)/G642","v":2.3016900011450252},{"$f":"(L642^2)/1000000+((K642/1000)^2*AJ642^2*PI()*PI()*(O642/2)^2)/1200","v":5.0176055936097591E-3},{"$f":"SQRT(3)*L642*J642*AJ642/1000","v":4.3415266693117216},{"$f":"0.75*J642^2*AJ642^2-(UAC_V*0.98)^2","v":-37090.399514120589},{"$f":"IF(((AX642/2/AW642)^2-AY642/AW642)>0,-AX642/2/AW642+SQRT((AX642/2/AW642)^2-AY642/AW642),-9999)","v":2320.4089478531801}]
["KBM","KBM-10H02-B (240 V)",0.89900000000000002,2.99,0.70664794732801528,2.301784844716662,10000,2.48,12944,5.22,9.6999999999999993,18.536100000000001,1.03E-2,325,6,6975.3703801771735,11033.694352896799,12160.055243551773,0.68676462426650153,242.71844660194174,4.8300036393941896,4.9334380454686508,1.0343004418339521,12.234926352762255,0,-9.9102903457374243,0,0,0,0,0,1.1918483283668178,1.6955149144771571,14.302179940401814,40.692357947451768,25.905559653606886,203.33030593877226,164.82811385841867,1585.6464553179878,8.1742603491368859E-4,1.3823329860401852,-49414.795648000007,6975.3703801771735,3.8114154147706505E-4,0.38916024560424139,-50694.965423849091,11033.694352896799,2.3220896069979053,5.0176055936097591E-3,4.3415266693117216,-37090.399514120589,2320.4089478531801]
["KBM","KBM-10H02-B (400 V)",0.89900000000000002,2.99,0.49317090918607037,1.6064198996288936,15200,2.48,16000,5.22,9.6999999999999993,18.536000000000001,1.03E-2,565,6,6975.3885560271547,11175.287413880231,12160.120845921449,0.60062784666056812,242.71844660194174,4.8483581270206919,4.9334380454686508,1.0342992429232405,12.234926352762255,0,-9.9102903457374243,0,0,0,0,0,1.1918483283668178,1.6955149144771571,14.302179940401814,40.692357947451768,25.905559653606886,203.33030593877226,164.82811385841867,1585.6464553179878,8.1742232770368856E-4,1.382325528522228,-49414.795648000007,6975.3885560271547,3.7449115639235151E-4,0.35304444580790573,-50714.468468887404,11175.287413880231,2.1066007394856836,5.0176018863997592E-3,4.3415032473045612,-37090.399514120589,2320.4116375613685]
["KBM","KBM-10H02-C (120 V)",0.86799999999999999,5.14,0.70215416069953829,4.058694570517563,8500,2.2400000000000002,11008,1.77,3.2,10.46,1.03E-2,160,6,11008,11008,11008,0.65321988246829621,242.71844660194174,5.0049734567383375,5.4620206931974344,0.50568532182520098,12.234926352762255,0,-9.9102903457374243,0,0,0,0,0,2.1220366916669597,3.0187942325843888,25.464440300003517,72.451061582025332,46.123778332138585,203.33030593877226,164.82811385841867,1585.6464553179878,2.4277718973342478E-4,0.42536033604146428,-50391.740820778359,13557.651387176016,1.1566817274879376E-4,9.2130482346528653E-2,-50785.765288247771,20559.392134290039,2.873014161202665,1.7219524228441374E-3,1.4790758788343257,-45806.454526015681,4746.0345325775588]
["KBM","KBM-10H02-C (240 V)",0.86799999999999999,5.14,0.25034642399860291,1.4470891560612886,18500,2.2400000000000002,20000,1.77,3.2,10.46,1.03E-2,325,6,13557.651387176016,20000,20000,0.20026640432281406,242.71844660194174,5.0417399217505938,5.4620206931974344,0.50568532182520098,12.234926352762255,0,-9.9102903457374243,0,0,0,0,0,2.1220366916669597,3.0187942325843888,25.464440300003517,72.451061582025332,46.123778332138585,203.33030593877226,164.82811385841867,1585.6464553179878,2.4277718973342478E-4,0.42536033604146428,-50391.740820778359,13557.651387176016,1.1131038752446128E-4,5.075435118320977E-2,-50799.273960119339,21136.165128395456,1.5827331625547396,1.7219524228441374E-3,1.4790758788343257,-45806.454526015681,4746.0345325775588]
["KBM","KBM-10H03-A (120 V)",1.1579999999999999,1.54,1.0725659208366858,1.3983910310778171,1380,3.46,2455,21.2,41,46.4,1.55E-2,160,6,2310.3946797151139,2455,2455,1.0060140113435243,161.29032258064515,3.8132377113871945,3.5434308038595956,4.3513663158145333,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,0.47755165239399183,0.67936156790750823,5.7306198287279022,16.304677629780198,10.379880161197466,203.75149766521193,165.16954961990689,1588.9310673435045,4.7875027048190433E-3,7.8397593019290408,-43668.261739908907,2310.3946797151139,2.3261729099704116E-3,2.0102044806659736,-50335.93135036304,4239.7082302178624,1.1798472044147406,1.5559397910975496E-2,17.685071025078496,-14487.51624883055,551.5508982264904]
["KBM","KBM-10H03-A (240 V)",1.1579999999999999,1.54,1.0203357995480415,1.3302943931525966,3650,3.46,5155,21.2,41,46.4,1.55E-2,325,6,2310.3946797151139,4141.8289707708991,4857.7586206896558,1.0017858702274154,161.29032258064515,3.7767273463569162,3.5434308038595956,4.3513663158145333,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,0.47755165239399183,0.67936156790750823,5.7306198287279022,16.304677629780198,10.379880161197466,203.75149766521193,165.16954961990689,1588.9310673435045,4.7875027048190433E-3,7.8397593019290408,-43668.261739908907,2310.3946797151139,2.3758393930769293E-3,2.2802636594620598,-50201.38631671475,4141.8289707708991,1.3383527545682963,1.5559397910975496E-2,17.685071025078496,-14487.51624883055,551.5508982264904]
["KBM","KBM-10H03-A (400 V)",1.1579999999999999,1.54,0.98952855922352334,1.290128499639535,6900,3.46,8619,21.2,41,46.4,1.55E-2,565,6,2310.3946797151139,4095.2708645207313,4857.7586206896558,1.0580092488527921,161.29032258064515,3.7569517116890219,3.5434308038595956,4.3513663158145333,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,0.47755165239399183,0.67936156790750823,5.7306198287279022,16.304677629780198,10.379880161197466,203.75149766521193,165.16954961990689,1588.9310673435045,4.7875027048190433E-3,7.8397593019290408,-43668.261739908907,2310.3946797151139,2.4013602773246723E-3,2.4072774404987616,-50132.25099617106,4095.2708645207313,1.4129008196629733,1.5559397910975496E-2,17.685071025078496,-14487.51624883055,551.5508982264904]
["KBM","KBM-10H03-A (480 V)",1.1579999999999999,1.54,0.87628839255302382,1.1424881258839945,8500,3.46,10354,21.2,41,46.4,1.55E-2,679,6,2310.3946797151139,4118.437308722986,4857.7586206896558,1.0215045183047116,161.29032258064515,3.7699033831704836,3.5434308038595956,4.3513663158145333,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,0.47755165239399183,0.67936156790750823,5.7306198287279022,16.304677629780198,10.379880161197466,203.75149766521193,165.16954961990689,1588.9310673435045,4.7875027048190433E-3,7.8397593019290408,-43668.261739908907,2310.3946797151139,2.3885078541233109E-3,2.34417313126011,-50167.067830461106,4118.437308722986,1.3758630737232767,1.5559397910975496E-2,17.685071025078496,-14487.51624883055,551.5508982264904]
["KBM","KBM-10H03-B (120 V)",1.17,2.4,1.0672743242632983,2.1431211330588318,2550,3.57,3799,8.77,17,30,1.55E-2,160,6,3799,3799,3799,1.0169588854416747,161.29032258064515,3.741182736102119,3.4342494625642019,1.2822819196534103,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,0.73660314814817518,1.047886374474718,8.8392377777781022,25.149272987393232,16.010524444444442,203.75149766521193,165.16954961990689,1588.9310673435045,2.0472182408516689E-3,3.3371449556365054,-47711.677651408289,4080.8637159773002,9.7040983989819189E-4,0.82673957654369268,-50615.299353493436,6808.6739522628959,1.8142087307762003,6.3836530286576817E-3,7.2960370958964864,-36018.449637583988,1871.6632927716075]
["KBM","KBM-10H03-B (240 V)",1.17,2.4,0.98185139021865797,1.971589136985257,6030,3.57,7967,8.77,17,30,1.55E-2,325,6,4080.8637159773002,6722.6106544824161,7513.3333333333339,0.96024048942917006,161.29032258064515,3.7279086599960438,3.4342494625642019,1.2822819196534103,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,0.73660314814817518,1.047886374474718,8.8392377777781022,25.149272987393232,16.010524444444442,203.75149766521193,165.16954961990689,1588.9310673435045,2.0472182408516689E-3,3.3371449556365054,-47711.677651408289,4080.8637159773002,9.8444873116532226E-4,0.90541693649887833,-50577.44338086139,6722.6106544824161,1.9868594147338421,6.3836530286576817E-3,7.2960370958964864,-36018.449637583988,1871.6632927716075]
["KBM","KBM-10H03-B (400 V)",1.17,2.4,0.73391973757660023,1.4737344128044181,11450,3.57,13319,8.77,17,30,1.55E-2,565,6,4080.8637159773002,6751.3973396160964,7513.3333333333339,0.91286889750354316,161.29032258064515,3.7379602765024886,3.4342494625642019,1.2822819196534103,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,0.73660314814817518,1.047886374474718,8.8392377777781022,25.149272987393232,16.010524444444442,203.75149766521193,165.16954961990689,1588.9310673435045,2.0472182408516689E-3,3.3371449556365054,-47711.677651408289,4080.8637159773002,9.796498450334837E-4,0.87931507193791969,-50590.383612295227,6751.3973396160964,1.9295811230933226,6.3836530286576817E-3,7.2960370958964864,-36018.449637583988,1871.6632927716075]
["KBM","KBM-10H03-B (480 V)",1.17,2.4,0.49415940372588485,0.99228795928892544,14300,3.57,16000,8.77,17,30,1.55E-2,679,6,4080.8637159773002,6802.0979141689859,7513.3333333333339,0.84852210417993823,161.29032258064515,3.7514440154696143,3.4342494625642019,1.2822819196534103,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,0.73660314814817518,1.047886374474718,8.8392377777781022,25.149272987393232,16.010524444444442,203.75149766521193,165.16954961990689,1588.9310673435045,2.0472182408516689E-3,3.3371449556365054,-47711.677651408289,4080.8637159773002,9.7144972563027461E-4,0.83282227483808491,-50612.495294037093,6802.0979141689859,1.8275566878178826,6.3836530286576817E-3,7.2960370958964864,-36018.449637583988,1871.6632927716075]
["KBM","KBM-10H03-C (120 V)",1.19,3.05,1.0724594626807715,2.6878683275207305,3250,3.58,4762,5.44,11,24,1.55E-2,160,6,4762,4762,4762,1.0177759880879489,161.29032258064515,3.6715030244549616,3.4246565869704471,0.89654994566908719,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,0.92036706378388067,1.309307607602602,11.044404765406568,31.423382582462448,20.004746666666666,203.75149766521193,165.16954961990689,1588.9310673435045,1.3300813298191641E-3,2.074945400814947,-48936.497492897965,5335.589493508648,6.2011743462285301E-4,0.5018832534246217,-50695.834131914897,8646.0638731177423,2.2193813684625496,4.1603671717134099E-3,4.5238044635641623,-41922.865371283406,2676.9283870837799]
["KBM","KBM-10H03-C (240 V)",1.19,3.05,0.94236479462306444,2.3618165278773544,7600,3.58,9983,5.44,11,24,1.55E-2,325,6,5335.589493508648,8575.5407901435319,9391.6666666666679,0.91057818358085774,161.29032258064515,3.6664490843488018,3.4246565869704471,0.89654994566908719,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,0.92036706378388067,1.309307607602602,11.044404765406568,31.423382582462448,20.004746666666666,203.75149766521193,165.16954961990689,1588.9310673435045,1.3300813298191641E-3,2.074945400814947,-48936.497492897965,5335.589493508648,6.2652083757523713E-4,0.53707241923970261,-50679.966083546882,8575.5407901435319,2.3749916193502285,4.1603671717134099E-3,4.5238044635641623,-41922.865371283406,2676.9283870837799]
["KBM","KBM-10H03-C (400 V)",1.19,3.05,0.47746482927568601,1.1966537074578596,14500,3.58,16000,5.44,11,24,1.55E-2,565,6,5335.589493508648,8700.2188262270956,9391.6666666666679,0.76246814436657828,161.29032258064515,3.6899218320244218,3.4246565869704471,0.89654994566908719,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,0.92036706378388067,1.309307607602602,11.044404765406568,31.423382582462448,20.004746666666666,203.75149766521193,165.16954961990689,1588.9310673435045,1.3300813298191641E-3,2.074945400814947,-48936.497492897965,5335.589493508648,6.1539319657362456E-4,0.47425092958098303,-50707.541100603987,8700.2188262270956,2.0971882801548007,4.1603671717134099E-3,4.5238044635641623,-41922.865371283406,2676.9283870837799]
["KBM","KBM-10H03-D (120 V)",1.18,4.66,1.0070167308359925,3.888095485853253,5500,15.5,7333,2.34,4.7,15.7,1.55E-2,160,6,2071.5353563665481,7333,7333,0.94936612494915151,161.29032258064515,3.69629148458292,0.79098519879704521,0.52301579167414047,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,1.4181171201742517,2.0174032806889328,17.017405442091022,48.417678736534391,30.823651615819212,203.75149766521193,165.16954961990689,1588.9310673435045,6.3732086860845052E-3,3.895038410101912,-35417.797210262863,2071.5353563665481,2.613031476111213E-4,0.19152322678747899,-50767.956516695318,13577.047825727392,3.0098531912955728,1.8000387987530408E-3,1.9613731446794203,-46903.394601130232,4588.7715786128592]
["KBM","KBM-10H03-D (240 V)",1.18,4.66,0.62437708443743556,2.4107223337352726,13000,15.5,15373,2.34,4.7,15.7,1.55E-2,325,6,2071.5353563665481,13714.981354146323,14356.687898089174,0.59381862100946248,161.29032258064515,3.7125247394587664,0.79098519879704521,0.52301579167414047,12.260270581354201,0,-9.9308191708969034,0,0,0,0,0,1.4181171201742517,2.0174032806889328,17.017405442091022,48.417678736534391,30.823651615819212,203.75149766521193,165.16954961990689,1588.9310673435045,6.3732086860845052E-3,3.895038410101912,-35417.797210262863,2071.5353563665481,2.577629348452118E-4,0.16707684793957414,-50776.847823930562,13714.981354146323,2.6256699638866383,1.8000387987530408E-3,1.9613731446794203,-46903.394601130232,4588.7715786128592]
["KBM","KBM-10H04-A (120 V)",1.44,1.6,1.3285977858106046,1.4285997696888222,1150,4.66,2022,20.399999999999999,44,56.2,2.01E-2,160,6,1834.9533314677865,2022,2022,1.244125846007863,124.37810945273633,3.0918441452411591,2.6357704883858037,2.6393207366923992,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,0.39972299604828088,0.56864307758693744,4.7966759525793705,13.647433862086498,8.6882262386831286,204.12409034629323,165.47158894737723,1591.8366856737687,7.0004029838826405E-3,10.281832335505445,-42437.415466666673,1834.9533314677865,3.3539730365869094E-3,2.3195514064153517,-50379.291634050089,3545.2689220434349,1.1680915749887293,1.3975982355243064E-2,17.252746122568912,-27244.695912521958,909.32487538732551]
["KBM","KBM-10H04-A (240 V)",1.44,1.6,1.2891550390443522,1.3861882140261852,3000,4.66,4251,20.399999999999999,44,56.2,2.01E-2,325,6,1834.9533314677865,3440.4427105164555,4010.6761565836296,1.2670088512206674,124.37810945273633,3.0459493624796621,2.6357704883858037,2.6393207366923992,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,0.39972299604828088,0.56864307758693744,4.7966759525793705,13.647433862086498,8.6882262386831286,204.12409034629323,165.47158894737723,1591.8366856737687,7.0004029838826405E-3,10.281832335505445,-42437.415466666673,1834.9533314677865,3.436705920068272E-3,2.7670941722938012,-50199.10050873673,3440.4427105164555,1.3934674527657445,1.3975982355243064E-2,17.252746122568912,-27244.695912521958,909.32487538732551]
["KBM","KBM-10H04-A (400 V)",1.44,1.6,1.1791305349069114,1.2678822955988294,5750,4.66,7109,20.399999999999999,44,56.2,2.01E-2,565,6,1834.9533314677865,3421.9891298227558,4010.6761565836296,1.2847491349823954,124.37810945273633,3.0411888993528078,2.6357704883858037,2.6393207366923992,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,0.39972299604828088,0.56864307758693744,4.7966759525793705,13.647433862086498,8.6882262386831286,204.12409034629323,165.47158894737723,1591.8366856737687,7.0004029838826405E-3,10.281832335505445,-42437.415466666673,1834.9533314677865,3.452562790136953E-3,2.8448427663504776,-50164.564455581189,3421.9891298227558,1.432620487888675,1.3975982355243064E-2,17.252746122568912,-27244.695912521958,909.32487538732551]
["KBM","KBM-10H04-A (480 V)",1.44,1.6,1.1106983262583334,1.1942992755465951,7050,4.66,8541,20.399999999999999,44,56.2,2.01E-2,679,6,1834.9533314677865,3421.6971908631672,4010.6761565836296,1.2801743812782411,124.37810945273633,3.0424866331969618,2.6357704883858037,2.6393207366923992,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,0.39972299604828088,0.56864307758693744,4.7966759525793705,13.647433862086498,8.6882262386831286,204.12409034629323,165.47158894737723,1591.8366856737687,7.0004029838826405E-3,10.281832335505445,-42437.415466666673,1834.9533314677865,3.4528167652448892E-3,2.8460707625586643,-50164.011301157276,3421.6971908631672,1.4332388885074039,1.3975982355243064E-2,17.252746122568912,-27244.695912521958,909.32487538732551]
["KBM","KBM-10H04-B (120 V)",1.41,2.4,1.2732395447351628,2.1115083660616301,2100,4.75,3131,9.02,19,36.4,2.01E-2,160,6,3131,3131,3131,1.2060966736027594,124.37810945273633,3.1269240625777526,2.5858295738690202,1.1883995451005482,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,0.61234161096757911,0.87111279970764866,7.3480993316109497,20.906707192983568,13.309623174152875,204.12409034629323,165.47158894737723,1591.8366856737687,3.0717459418121767E-3,4.5978445844263867,-46816.327351742875,3226.6465221488488,1.4062233388594545E-3,0.9917033363025024,-50619.59298151765,5657.4769446632499,1.7438664633247845,6.0586490932236234E-3,7.5689268555411386,-39995.653723483752,2019.5228194882393]
["KBM","KBM-10H04-B (240 V)",1.41,2.4,1.1888682496021099,1.971589136985257,4980,4.75,6571,9.02,19,36.4,2.01E-2,325,6,3226.6465221488488,5562.7366862333374,6192.3076923076924,1.1629924296326632,124.37810945273633,3.1058754130505477,2.5858295738690202,1.1883995451005482,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,0.61234161096757911,0.87111279970764866,7.3480993316109497,20.906707192983568,13.309623174152875,204.12409034629323,165.47158894737723,1591.8366856737687,3.0717459418121767E-3,4.5978445844263867,-46816.327351742875,3226.6465221488488,1.430688598897276E-3,1.1311773011037352,-50563.725902643797,5562.7366862333374,1.9891252628269169,6.0586490932236234E-3,7.5689268555411386,-39995.653723483752,2019.5228194882393]
["KBM","KBM-10H04-B (400 V)",1.41,2.4,0.90467020283814192,1.5002822600964212,9500,4.75,10987,9.02,19,36.4,2.01E-2,565,6,3226.6465221488488,5578.9776828059712,6192.3076923076924,1.1132396146502237,124.37810945273633,3.1147687260668735,2.5858295738690202,1.1883995451005482,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,0.61234161096757911,0.87111279970764866,7.3480993316109497,20.906707192983568,13.309623174152875,204.12409034629323,165.47158894737723,1591.8366856737687,3.0717459418121767E-3,4.5978445844263867,-46816.327351742875,3226.6465221488488,1.4263269460412004E-3,1.1075991770576481,-50573.685854173193,5578.9776828059712,1.9476641743270184,6.0586490932236234E-3,7.5689268555411386,-39995.653723483752,2019.5228194882393]
["KBM","KBM-10H04-B (480 V)",1.41,2.4,0.71412130987319988,1.1842807792258705,11500,4.75,13200,9.02,19,36.4,2.01E-2,679,6,3226.6465221488488,5599.4451829487807,6192.3076923076924,1.07117090614372,124.37810945273633,3.1222134240633364,2.5858295738690202,1.1883995451005482,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,0.61234161096757911,0.87111279970764866,7.3480993316109497,20.906707192983568,13.309623174152875,204.12409034629323,165.47158894737723,1591.8366856737687,3.0717459418121767E-3,4.5978445844263867,-46816.327351742875,3226.6465221488488,1.4209283457739974E-3,1.077701401484437,-50586.01370298698,5599.4451829487807,1.8950902580744768,6.0586490932236234E-3,7.5689268555411386,-39995.653723483752,2019.5228194882393]
["KBM","KBM-10H04-C (120 V)",1.44,3.1,1.308607309866695,2.726265228888948,2700,4.8,3944,5.44,11.8,29,2.01E-2,160,6,3944,3944,3944,1.2480693444867574,124.37810945273633,3.0443802650929235,2.5588938491412181,0.83257941761125176,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,0.7744633048435442,1.1017459628246911,9.2935596581225308,26.441903107792587,16.833438337448559,204.12409034629323,165.47158894737723,1591.8366856737687,1.9415401765434858E-3,2.8235661324880161,-48435.205866666671,4320.183724416177,8.9305548574941738E-4,0.61408468295639085,-50693.06130860831,7198.1929972703783,2.2473501331776005,3.7615906351688129E-3,4.5997090048011415,-44515.825003314894,2882.6078920925338]
["KBM","KBM-10H04-C (240 V)",1.44,3.1,1.1519786357127662,2.3999554910682628,6300,4.8,8273,5.44,11.8,29,2.01E-2,325,6,4320.183724416177,7141.7239125014903,7772.4137931034484,1.113496973866438,124.37810945273633,3.0415266410530291,2.5588938491412181,0.83257941761125176,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,0.7744633048435442,1.1017459628246911,9.2935596581225308,26.441903107792587,16.833438337448559,204.12409034629323,165.47158894737723,1591.8366856737687,1.9415401765434858E-3,2.8235661324880161,-48435.205866666671,4320.183724416177,9.0113799521743341E-4,0.66003883088196369,-50675.65605877764,7141.7239125014903,2.4155273623561588,3.7615906351688129E-3,4.5997090048011415,-44515.825003314894,2882.6078920925338]
["KBM","KBM-10H04-C (400 V)",1.44,3.1,0.66845076098596046,1.3926057520540844,12000,4.8,13833,5.44,11.8,29,2.01E-2,565,6,4320.183724416177,7206.0683699574392,7772.4137931034484,0.97668028607301649,124.37810945273633,3.0596104851476524,2.5588938491412181,0.83257941761125176,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,0.7744633048435442,1.1017459628246911,9.2935596581225308,26.441903107792587,16.833438337448559,204.12409034629323,165.47158894737723,1591.8366856737687,1.9415401765434858E-3,2.8235661324880161,-48435.205866666671,4320.183724416177,8.9195908867791831E-4,0.60758331576061508,-50695.422340787562,7206.0683699574392,2.2235572446090042,3.7615906351688129E-3,4.5997090048011415,-44515.825003314894,2882.6078920925338]
["KBM","KBM-10H04-D (120 V)",1.41,4.21,1.2277667038517641,3.5484586816524977,4200,4.91,5489,2.94,6.2,20.9,2.01E-2,160,6,5489,5489,5489,1.1718384374862698,124.37810945273633,3.104851508391441,2.5015662883661602,0.55925745307483232,12.282690475877846,0,-9.9489792854610535,0,0,0,0,0,1.0741492425722952,1.5280770361538336,12.889790910867541,36.673848867692008,23.347297317993171,204.12409034629323,165.47158894737723,1591.8366856737687,1.048361926170838E-3,1.5602662671762528,-49411.859237375451,6161.3743180905749,4.5959733832992984E-4,0.301181887189235,-50753.243532216031,10186.007105492925,2.8299229183957353,1.9878307771963267E-3,2.4847966781327107,-47271.464267496536,4291.4045880026279]
["KBM","KBM-10H04-D (240 V)",1.41,4.21,0.909696148409465,2.629179619680535,9500,4.91,11509,2.94,6.2,20.9,2.01E-2,325,6,{"$f":"IF(AQ672<I672,IF(AQ672<0,0,AQ672),I672)","v":6161.3743180905749},{"$f":"IF(AU672<I672,IF(AU672<0,0,AU672),I672)","v":10208.37829178884},{"$f":"IF(UAC_V*0.98/L672*1000<I672,IF(UAC_V*0.98/L672*1000<0,0,UAC_V*0.98/L672*1000),I672)","v":10784.688995215312},{"$f":"C672+(E672-C672)/G672*Q672","v":0.87239042338156181},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M672,(inertia/gear^2+gear_inertia)/M672),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M672,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M672))","v":124.37810945273633},{"$f":"IF((C672+(E672-C672)/G672*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X672^2*time1+Y672^2*time2+Z672^2*time3+AA672^2*time4)/time)/(C672+(E672-C672)/G672*mspeed),SQRT((((X672-Y672)*2/PI()+Y672)^2*time1+Y672^2*time2+((Z672-Y672)*2/PI()+Y672)^2*time3+AA672^2*time4)/time)/(C672+(E672-C672)/G672*mspeed)),IF(AccType=1,SQRT((X672^2*time1+Y672^2*time2+Z672^2*time3+AA672^2*time4+AB672^2*time5+AC672^2*time6+AD672^2*time7+AE672^2*time8)/time)/(C672+(E672-C672)/G672*mspeed),SQRT((((X672-Y672)*2/PI()+Y672)^2*time1+Y672^2*time2+((Z672-Y672)*2/PI()+Y672)^2*time3+AA672^2*time4+((AB672-AC672)*2/PI()+AC672)^2*time5+AC672^2*time6+((AD672-AC672)*2/PI()+AC672)^2*time7+AE672^2*time8)/time)/(C672+(E672-C672)/G672*mspeed))))","v":3.1142319380765269},{"$f":"IF(move1,MAX(ABS(X672),ABS(Z672))/H672,MAX(ABS(X672),ABS(Z672),ABS(AB672),ABS(AD672))/H672)","v":2.5015662883661602},{"$f":"IF(AZ672>0,speed/(MIN(AZ672,I672)),\"NA\")","v":0.55925745307483232},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M672+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M672+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.282690475877846},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M672+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M672+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-9.9489792854610535},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M672+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M672+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M672+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M672+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH672/Irms","v":1.0741492425722952},{"$f":"AI672/Ipeak","v":1.5280770361538336},{"$f":"IF(move1,IF(AccType=1,SQRT((X672^2*time1+Y672^2*time2+Z672^2*time3+AA672^2*time4)/time)/(C672/D672),SQRT((((X672-Y672)*2/PI()+Y672)^2*time1+Y672^2*time2+((Z672-AA672)*2/PI()+AA672)^2*time3+AA672^2*time4)/time)/(C672/D672)),IF(AccType=1,SQRT((X672^2*time1+Y672^2*time2+Z672^2*time3+AA672^2*time4+AB672^2*time5+AC672^2*time6+AD672^2*time7+AE672^2*time8)/time)/(C672/D672),SQRT((((X672-Y672)*2/PI()+Y672)^2*time1+Y672^2*time2+((Z672-AA672)*2/PI()+AA672)^2*time3+AA672^2*time4+((AB672-AC672)*2/PI()+AC672)^2*time5+AC672^2*time6+((AD672-AE672)*2/PI()+AE672)^2*time7+AE672^2*time8)/time)/(C672/D672)))","v":12.889790910867541},{"$f":"IF(move1,MAX(ABS(X672),ABS(Z672))/(C672/D672),MAX(ABS(X672),ABS(Z672),ABS(AB672),ABS(AD672))/(C672/D672))","v":36.673848867692008},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X672),ABS(Z672))/(C672/D672),MAX(ABS((X672-Y672)*2/PI()+Y672),ABS((Z672-Y672)*2/PI()+Y672))/(C672/D672)),IF(AccType=1,MAX(ABS(X672),ABS(Z672),ABS(AB672),ABS(AD672))/(C672/D672),MAX(ABS((X672-Y672)*2/PI()+Y672),ABS((Z672-Y672)*2/PI()+Y672),ABS((AB672-AC672)*2/PI()+AC672),ABS((AD672-AC672)*2/PI()+AC672))/(C672/D672)))","v":23.347297317993171},{"$f":"IF((C672+(E672-C672)/G672*mspeed)<0,\"NA\",U672*(C672+(E672-C672)/G672*mspeed)*mspeed/9.55)","v":204.12409034629323},{"$f":"IF(move1,IF(speed1>speed2,AM672/2*time1/time,AM672/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z672*-speed/30*PI(),((Z672-AA672)*2/PI()+AA672)*-speed/30*PI()),IF(AccType=1,X672*-speed/30*PI(),((X672-Y672)*2/PI()+Y672)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z672*-speed/30*PI(),((Z672-AA672)*2/PI()+AA672)*-speed/30*PI()),IF(AccType=1,X672*-speed/30*PI(),((X672-Y672)*2/PI()+Y672)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD672*-speed/30*PI(),((AD672-AE672)*2/PI()+AE672)*-speed/30*PI()),IF(AccType=1,AB672*-speed/30*PI(),((AB672-AC672)*2/PI()+AC672)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD672*-speed/30*PI(),((AD672-AE672)*2/PI()+AE672)*-speed/30*PI()),IF(AccType=1,AB672*-speed/30*PI(),((AB672-AC672)*2/PI()+AC672)*-speed/30*PI()),0)/2*time7/time)))","v":165.47158894737723},{"$f":"IF(move1,MAX(IF(AccType=1,Z672*-speed/30*PI(),((Z672-AA672)*2/PI()+AA672)*-speed/30*PI()),IF(AccType=1,X672*-speed/30*PI(),((X672-Y672)*2/PI()+Y672)*-speed/30*PI()),0),MAX(IF(AccType=1,Z672*-speed/30*PI(),((Z672-AA672)*2/PI()+AA672)*-speed/30*PI()),IF(AccType=1,X672*-speed/30*PI(),((X672-Y672)*2/PI()+Y672)*-speed/30*PI()),IF(AccType=1,AD672*-speed/30*PI(),((AD672-AE672)*2/PI()+AE672)*-speed/30*PI()),IF(AccType=1,AB672*-speed/30*PI(),((AB672-AC672)*2/PI()+AC672)*-speed/30*PI()),0))","v":1591.8366856737687},{"$f":"(L672^2)/1000000+((K672/1000)^2*(D672/C672*H672)^2*PI()*PI()*(O672/2)^2)/1200","v":1.048361926170838E-3},{"$f":"SQRT(3)*L672*J672*D672/C672*H672/1000","v":1.5602662671762528},{"$f":"0.75*J672^2*(D672/C672*H672)^2-(UAC_V*0.98)^2","v":-49411.859237375451},{"$f":"-AO672/2/AN672+SQRT((AO672/2/AN672)^2-AP672/AN672)","v":6161.3743180905749},{"$f":"(L672^2)/1000000+((K672/1000)^2*AV672^2*PI()*PI()*(O672/2)^2)/1200","v":4.5835985565251009E-4},{"$f":"SQRT(3)*L672*J672*AV672/1000","v":0.2928897900574538},{"$f":"0.75*J672^2*AV672^2-(UAC_V*0.98)^2","v":-50756.062893065697},{"$f":"-AS672/2/AR672+SQRT((AS672/2/AR672)^2-AT672/AR672)","v":10208.37829178884},{"$f":"D672+(F672-D672)*((0.85*UAC_V-D672*J672)/L672*1000)/G672","v":2.7520098807499913},{"$f":"(L672^2)/1000000+((K672/1000)^2*AJ672^2*PI()*PI()*(O672/2)^2)/1200","v":1.9878307771963267E-3},{"$f":"SQRT(3)*L672*J672*AJ672/1000","v":2.4847966781327107},{"$f":"0.75*J672^2*AJ672^2-(UAC_V*0.98)^2","v":-47271.464267496536},{"$f":"IF(((AX672/2/AW672)^2-AY672/AW672)>0,-AX672/2/AW672+SQRT((AX672/2/AW672)^2-AY672/AW672),-9999)","v":4291.4045880026279}]
["KBM","KBM-14H01-A (120 V)",1.2,1.53,1.1018419137131217,1.3519532683596587,1300,3.28,2308,21.4,38,49.3,2.41E-2,160,8,2204.16391106437,2308,2308,1.0257316437306807,103.7344398340249,3.7085889962544316,3.7506664744918266,4.3533102312926468,12.30218603633319,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-9.9647706894298818,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.45941017596066502,0.65355363318020065,5.5129221115279803,15.685287196324817,9.9855639644444434,204.44808398201607,165.73423184082964,1594.3633103087811,5.7538220217480916E-3,7.6419703522315059,-44798.170579720005,2204.16391106437,2.6512494758745607E-3,1.9696005620522552,-50406.132810622905,4004.6455395508847,1.0778463106831224,2.1377944427660809E-2,18.247102765804815,-16557.255323798723,551.3046101672744]
["KBM","KBM-14H01-A (240 V)",1.2,1.53,1.083203791789616,1.3290844071038235,3350,3.28,4849,21.4,38,49.3,2.41E-2,325,8,2204.16391106437,3841.6326883896022,4572.0081135902637,1.06606324437583,103.7344398340249,3.6511179246498884,3.7506664744918266,4.3533102312926468,12.30218603633319,0,-9.9647706894298818,0,0,0,0,0,0.45941017596066502,0.65355363318020065,5.5129221115279803,15.685287196324817,9.9855639644444434,204.44808398201607,165.73423184082964,1594.3633103087811,5.7538220217480916E-3,7.6419703522315059,-44798.170579720005,2204.16391106437,2.7676331972076936E-3,2.4340286334298558,-50195.766895280751,3841.6326883896022,1.3320004234289249,2.1377944427660809E-2,18.247102765804815,-16557.255323798723,551.3046101672744]
["KBM","KBM-14H01-A (400 V)",1.2,1.53,0.9698504344662372,1.1900005330874077,6400,3.28,8109,21.4,38,49.3,2.41E-2,565,8,2204.16391106437,3826.9191702537282,4572.0081135902637,1.0623806586926994,103.7344398340249,3.6526448493453585,3.7506664744918266,4.3533102312926468,12.30218603633319,0,-9.9647706894298818,0,0,0,0,0,0.45941017596066502,0.65355363318020065,5.5129221115279803,15.685287196324817,9.9855639644444434,204.44808398201607,165.73423184082964,1594.3633103087811,5.7538220217480916E-3,7.6419703522315059,-44798.170579720005,2204.16391106437,2.7791780909336792E-3,2.4753524249220322,-50174.899267846471,3826.9191702537282,1.3546144991260152,2.1377944427660809E-2,18.247102765804815,-16557.255323798723,551.3046101672744]
["KBM","KBM-14H01-A (480 V)",1.2,1.53,0.89449107256710791,1.0975350583645496,7900,3.28,9741,21.4,38,49.3,2.41E-2,679,8,2204.16391106437,3830.3957279058741,4572.0081135902637,1.0518708746232841,103.7344398340249,3.6564263165167277,3.7506664744918266,4.3533102312926468,12.30218603633319,0,-9.9647706894298818,0,0,0,0,0,0.45941017596066502,0.65355363318020065,5.5129221115279803,15.685287196324817,9.9855639644444434,204.44808398201607,165.73423184082964,1594.3633103087811,5.7538220217480916E-3,7.6419703522315059,-44798.170579720005,2204.16391106437,2.7764344381324777E-3,2.4655945347629222,-50179.858475425455,3830.3957279058741,1.3492745809158533,2.1377944427660809E-2,18.247102765804815,-16557.255323798723,551.3046101672744]
["KBM","KBM-14H01-B (120 V)",1.25,3.25,1.1186318857316073,2.8391672226690541,3500,3.43,5022,4.74,9,23.7,2.41E-2,160,8,5022,5022,5022,1.0615055228983235,103.7344398340249,3.5066347337360502,3.586643159280813,0.92495556862941386,12.30218603633319,0,-9.9647706894298818,0,0,0,0,0,0.93683643725312071,1.3327368206027621,11.242037247037448,31.985683694466292,20.362718672592589,204.44808398201607,165.73423184082964,1594.3633103087811,1.4094217263012007E-3,1.7352209524491575,-49465.011629093206,5340.5018636709192,6.2095824605575933E-4,0.45881393762326506,-50711.464977230607,8675.0581494713388,2.3580297886266823,4.9814127132585696E-3,3.9620785029726799,-43818.18049897709,2594.7192291152819]
["KBM","KBM-14H01-B (240 V)",1.25,3.25,0.93691211782398764,2.377949537624334,7950,3.43,10088,4.74,9,23.7,2.41E-2,325,8,5340.5018636709192,8646.053216925884,9510.5485232067513,0.90950006404170769,103.7344398340249,3.5090099801471131,3.586643159280813,0.92495556862941386,12.30218603633319,0,-9.9647706894298818,0,0,0,0,0,0.93683643725312071,1.3327368206027621,11.242037247037448,31.985683694466292,20.362718672592589,204.44808398201607,165.73423184082964,1594.3633103087811,1.4094217263012007E-3,1.7352209524491575,-49465.011629093206,5340.5018636709192,6.2393174920894368E-4,0.47018249831784686,-50706.764273832363,8646.053216925884,2.4164574050816254,4.9814127132585696E-3,3.9620785029726799,-43818.18049897709,2594.7192291152819]
["KBM","KBM-14H01-B (400 V)",1.25,3.25,0.56102117439893107,1.4239116101495712,12000,3.43,12000,4.74,9,23.7,2.41E-2,565,8,5340.5018636709192,8802.786211421253,9510.5485232067513,0.74458889116980853,103.7344398340249,3.5323528584902362,3.586643159280813,0.92495556862941386,12.30218603633319,0,-9.9647706894298818,0,0,0,0,0,0.93683643725312071,1.3327368206027621,11.242037247037448,31.985683694466292,20.362718672592589,204.44808398201607,165.73423184082964,1594.3633103087811,1.4094217263012007E-3,1.7352209524491575,-49465.011629093206,5340.5018636709192,6.0841256029870448E-4,0.40736984819445471,-50731.297997285888,8802.786211421253,2.0936378742260446,4.9814127132585696E-3,3.9620785029726799,-43818.18049897709,2594.7192291152819]
["KBM","KBM-14H01-C (120 V)",1.21,6.25,0.91036627448564134,4.5747048969127704,7500,3.59,9539,1.29,2.4,12.1,2.41E-2,160,8,9539,9539,9539,0.82890585230913771,103.7344398340249,3.6275224262286656,3.426792767780833,0.43255370748039018,12.30218603633319,0,-9.9647706894298818,0,0,0,0,0,1.8611658400610314,2.6476812233843812,22.333990080732377,63.544349361225152,40.453589225589219,204.44808398201607,165.73423184082964,1594.3633103087811,4.070488535243762E-4,0.50133128093326429,-50376.000357144003,10525.925842395798,1.5230939109131663E-4,7.5423871212386542E-2,-50795.446250343797,18016.107464304288,2.7898002657309906,1.3868480679397686E-3,1.0936862904879516,-48762.69414725549,5548.4439469491863]
["KBM","KBM-14H01-C (240 V)",1.21,6.25,0.64723010190704111,3.2524125723971915,13500,3.59,12000,1.29,2.4,12.1,2.41E-2,325,8,10525.925842395798,12000,12000,0.70976009058403655,103.7344398340249,3.6299089867967624,3.426792767780833,0.43255370748039018,12.30218603633319,0,-9.9647706894298818,0,0,0,0,0,1.8611658400610314,2.6476812233843812,22.333990080732377,63.544349361225152,40.453589225589219,204.44808398201607,165.73423184082964,1594.3633103087811,4.070488535243762E-4,0.50133128093326429,-50376.000357144003,10525.925842395798,1.523967917074952E-4,7.5980526648529209E-2,-50795.302339270223,18009.183218393944,2.810390000236906,1.3868480679397686E-3,1.0936862904879516,-48762.69414725549,5548.4439469491863]
["KBM","KBM-14H02-A (120 V)",2.08,1.59,1.9757165349338732,1.4634937295806467,725,6.67,1461,23.8,47,80.8,4.8800000000000003E-2,160,8,1182.1558441081677,1461,1461,1.8698508379839844,51.229508196721305,2.1667832357363617,1.8624544411011901,2.4931295200184338,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.27813357421736268,0.39567083502024142,3.3376028906083524,9.4961000404857945,6.0454050461538467,206.44874468260474,167.3560517078985,1609.9652174299836,1.4085709989137867E-2,16.982771584944864,-39760.95589675603,1182.1558441081677,6.9825060064772322E-3,4.1619386528807425,-50141.862079210114,2398.2470726276174,1.2495301198058313,1.7152565247862489E-2,20.136053173186237,-35278.931053642737,962.64553475033847]
["KBM","KBM-14H02-A (240 V)",2.08,1.59,1.8621128341751756,1.3793428401297596,2000,6.67,2944,23.8,47,80.8,4.8800000000000003E-2,325,8,1182.1558441081677,2350.5919118184538,2789.6039603960398,1.8239180951615608,51.229508196721305,2.1499706878984366,1.8624544411011901,2.4931295200184338,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.27813357421736268,0.39567083502024142,3.3376028906083524,9.4961000404857945,6.0454050461538467,206.44874468260474,167.3560517078985,1609.9652174299836,1.4085709989137867E-2,16.982771584944864,-39760.95589675603,1182.1558441081677,7.0858366846263243E-3,4.6114351765319208,-49990.85049651398,2350.5919118184538,1.3844815191161983,1.7152565247862489E-2,20.136053173186237,-35278.931053642737,962.64553475033847]
["KBM","KBM-14H02-A (400 V)",2.08,1.59,1.7384616860807027,1.2877493970968168,3900,6.67,4924,23.8,47,80.8,4.8800000000000003E-2,565,8,1182.1558441081677,2331.3002366634992,2789.6039603960398,1.8758388840846898,51.229508196721305,2.1398031041178611,1.8624544411011901,2.4931295200184338,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.27813357421736268,0.39567083502024142,3.3376028906083524,9.4961000404857945,6.0454050461538467,206.44874468260474,167.3560517078985,1609.9652174299836,1.4085709989137867E-2,16.982771584944864,-39760.95589675603,1182.1558441081677,7.1304001237275693E-3,4.792295053087126,-49925.723705616969,2331.3002366634992,1.4387807008361575,1.7152565247862489E-2,20.136053173186237,-35278.931053642737,962.64553475033847]
["KBM","KBM-14H02-A (480 V)",2.08,1.59,1.6370222718023522,1.2126090902239646,4900,6.67,5915,23.8,47,80.8,4.8800000000000003E-2,679,8,1182.1558441081677,2330.9658873341036,2789.6039603960398,1.8692722503515355,51.229508196721305,2.1411439307086551,1.8624544411011901,2.4931295200184338,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.27813357421736268,0.39567083502024142,3.3376028906083524,9.4961000404857945,6.0454050461538467,206.44874468260474,167.3560517078985,1609.9652174299836,1.4085709989137867E-2,16.982771584944864,-39760.95589675603,1182.1558441081677,7.1311864325521723E-3,4.7954250326074366,-49924.574562475573,2330.9658873341036,1.4397204080282124,1.7152565247862489E-2,20.136053173186237,-35278.931053642737,962.64553475033847]
["KBM","KBM-14H02-B (120 V)",2.08,2.42,1.909859317102744,2.1702946785258455,1350,6.83,2139,10.3,20,53.4,4.8800000000000003E-2,160,8,2139,2139,2139,1.8104215402094588,51.229508196721305,2.158170172278691,1.8188244688352764,1.2447499746032122,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.42332279849435078,0.60221598789244279,5.0798735819322092,14.453183709418628,9.2011825230769233,206.44874468260474,167.3560517078985,1609.9652174299836,6.1754293340383886E-3,7.5702782718222004,-45780.794993405078,2177.9548476944101,3.0276783596547524E-3,1.7425778458203354,-50538.939269176888,3807.9697879843393,1.8291658273667299,7.3079764125483539E-3,8.7656223291386066,-44068.835425285346,1928.0980509881479]
["KBM","KBM-14H02-B (240 V)",2.08,2.42,1.7941102675813656,2.0387616677060971,3300,6.83,4489,10.3,20,53.4,4.8800000000000003E-2,325,8,2177.9548476944101,3747.1821685325922,4220.9737827715353,1.7553694219740421,51.229508196721305,2.1393577449241961,1.8188244688352764,1.2447499746032122,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.42332279849435078,0.60221598789244279,5.0798735819322092,14.453183709418628,9.2011825230769233,206.44874468260474,167.3560517078985,1609.9652174299836,6.1754293340383886E-3,7.5702782718222004,-45780.794993405078,2177.9548476944101,3.072981495184065E-3,1.9538884334095701,-50470.458993339467,3747.1821685325922,2.0509763517608661,7.3079764125483539E-3,8.7656223291386066,-44068.835425285346,1928.0980509881479]
["KBM","KBM-14H02-B (400 V)",2.08,2.42,1.382510102678852,1.5710342075896044,6700,6.83,7505,10.3,20,53.4,4.8800000000000003E-2,565,8,2177.9548476944101,3757.0713396510178,4220.9737827715353,1.6888777159818782,51.229508196721305,2.1476590908459259,1.8188244688352764,1.2447499746032122,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.42332279849435078,0.60221598789244279,5.0798735819322092,14.453183709418628,9.2011825230769233,206.44874468260474,167.3560517078985,1609.9652174299836,6.1754293340383886E-3,7.5702782718222004,-45780.794993405078,2177.9548476944101,3.0653346920628002E-3,1.9198531787260023,-50482.017910418836,3757.0713396510178,2.0152498991709686,7.3079764125483539E-3,8.7656223291386066,-44068.835425285346,1928.0980509881479]
["KBM","KBM-14H02-B (480 V)",2.08,2.42,1.2401683877290546,1.4092822587830165,7700,6.83,9016,10.3,20,53.4,4.8800000000000003E-2,679,8,2177.9548476944101,3761.0847462496031,4220.9737827715353,1.6697820952817579,51.229508196721305,2.1500306653744392,1.8188244688352764,1.2447499746032122,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.42332279849435078,0.60221598789244279,5.0798735819322092,14.453183709418628,9.2011825230769233,206.44874468260474,167.3560517078985,1609.9652174299836,6.1754293340383886E-3,7.5702782718222004,-45780.794993405078,2177.9548476944101,3.0622618441065617E-3,1.9060050227265961,-50486.662831199501,3761.0847462496031,2.0007136339550908,7.3079764125483539E-3,8.7656223291386066,-44068.835425285346,1928.0980509881479]
["KBM","KBM-14H02-C (120 V)",2.11,3.1,1.9098593171027443,2.7322737011484182,1800,6.98,2704,6.3,12.8,42.3,4.8800000000000003E-2,160,8,2704,2704,2704,1.8093442185810114,51.229508196721305,2.1197157214853668,1.7797379831153204,0.91056817560847747,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.53456296359162858,0.7604654517900733,6.4147555630995434,18.251170842961759,11.619056227488153,206.44874468260474,167.3560517078985,1609.9652174299836,4.0566879184936264E-3,4.7334326853383857,-47674.674585865097,2894.0142377704819,1.8984529308983371E-3,1.0386038479040856,-50654.444080154535,4899.1564107765107,2.2501340056617698,4.7000079761520038E-3,5.3630568119581907,-46786.474045195144,2635.7169779146143]
["KBM","KBM-14H02-C (240 V)",2.11,3.1,1.7301078519636623,2.4751185292756257,4250,6.98,5671,6.3,12.8,42.3,4.8800000000000003E-2,325,8,2894.0142377704819,4840.9785364575282,5328.6052009456271,1.6772824153381984,51.229508196721305,2.1096322026793226,1.7797379831153204,0.91056817560847747,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.53456296359162858,0.7604654517900733,6.4147555630995434,18.251170842961759,11.619056227488153,206.44874468260474,167.3560517078985,1609.9652174299836,4.0566879184936264E-3,4.7334326853383857,-47674.674585865097,2894.0142377704819,1.9227894220441859E-3,1.1485556070471885,-50620.84387705745,4840.9785364575282,2.4883443615443297,4.7000079761520038E-3,5.3630568119581907,-46786.474045195144,2635.7169779146143]
["KBM","KBM-14H02-C (400 V)",2.11,3.1,1.2055986939211072,1.7247477738499388,8000,6.98,9481,6.3,12.8,42.3,4.8800000000000003E-2,565,8,2894.0142377704819,4866.463491414549,5328.6052009456271,1.5598455077974291,51.229508196721305,2.1205808252206397,1.7797379831153204,0.91056817560847747,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.53456296359162858,0.7604654517900733,6.4147555630995434,18.251170842961759,11.619056227488153,206.44874468260474,167.3560517078985,1609.9652174299836,4.0566879184936264E-3,4.7334326853383857,-47674.674585865097,2894.0142377704819,1.9119165360207331E-3,1.100790223379468,-50635.855539028358,4866.463491414549,2.3848607144337284,4.7000079761520038E-3,5.3630568119581907,-46786.474045195144,2635.7169779146143]
["KBM","KBM-14H02-C (480 V)",2.11,3.1,0.5496668278490825,0.78636169935491063,10250,6.98,11390,6.3,12.8,42.3,4.8800000000000003E-2,679,8,2894.0142377704819,4920.4679581146029,5328.6052009456271,1.3609688412144481,51.229508196721305,2.1389592175221233,1.7797379831153204,0.91056817560847747,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.53456296359162858,0.7604654517900733,6.4147555630995434,18.251170842961759,11.619056227488153,206.44874468260474,167.3560517078985,1609.9652174299836,4.0566879184936264E-3,4.7334326853383857,-47674.674585865097,2894.0142377704819,1.8899748762565426E-3,0.99745762327958332,-50666.149315561124,4920.4679581146029,2.1609907587741075,4.7000079761520038E-3,5.3630568119581907,-46786.474045195144,2635.7169779146143]
["KBM","KBM-14H02-D (120 V)",2.1749999999999998,5.97,1.8608885653821607,4.975637875353371,3900,7.31,5084,1.69,3.6,22.6,4.8800000000000003E-2,160,8,5084,5084,5084,1.7655275554879244,51.229508196721305,2.0415736826037039,1.6993941343563526,0.47206923682140045,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.99869918924355472,1.4207423294866912,11.984390270922656,34.097815907680591,21.707343801379313,206.44874468260474,167.3560517078985,1609.9652174299836,1.1973672377044277E-3,1.3273584470053374,-49942.778232224322,5927.8257402751988,5.36411857256739E-4,0.25656265231864134,-50772.941152319698,9492.7642190142215,3.8782666486927768,1.314391317534721E-3,1.4360265048695662,-49795.795463481918,5633.007143608862]
["KBM","KBM-14H02-D (240 V)",2.1749999999999998,5.97,1.1051433127055206,2.9549286435976487,8900,7.31,10660,1.69,3.6,22.6,4.8800000000000003E-2,325,8,5927.8257402751988,9608.2288060152696,9973.4513274336277,1.0200081077336083,51.229508196721305,2.0588173063614459,1.6993941343563526,0.42606017333441681,12.422571122144937,0,-10.062282608937398,0,0,0,0,0,0.99869918924355472,1.4207423294866912,11.984390270922656,34.097815907680591,21.707343801379313,206.44874468260474,167.3560517078985,1609.9652174299836,1.1973672377044277E-3,1.3273584470053374,-49942.778232224322,5927.8257402751988,5.2812273012520694E-4,0.21107803222402088,-50783.352333146897,9608.2288060152696,3.1907095021352823,1.314391317534721E-3,1.4360265048695662,-49795.795463481918,5633.007143608862]
["KBM","KBM-14H03-A (120 V)",2.82,1.64,2.5783100780887045,1.4403966916696673,500,10.4,1051,26.6,54,108,7.3099999999999998E-2,160,8,665.21458201707162,1051,1051,2.3119677841424568,34.19972640218878,1.6941830396527189,1.2058660242222259,2.5517669748740941,12.54100665191115,0,-10.158215388048031,0,0,0,0,0,0.21361673533592518,0.30388964109240968,2.5634008240311021,7.2933513862178323,4.64309169929078,208.41700601962111,168.95160728562217,1625.3144620876851,2.5701254041447769E-2,30.094982734427266,-31392.694598219408,665.21458201707162,1.2110433212094705E-2,5.3669959398672606,-50187.776481941197,1826.1636228991952,1.0786119989633778,1.9936571385351341E-2,23.103260785596998,-39364.816658794065,940.52475152768125]
["KBM","KBM-14H03-A (240 V)",2.82,1.64,2.5464790894703255,1.422614016463869,1500,10.4,2217,26.6,54,108,7.3099999999999998E-2,325,8,665.21458201707162,1731.3806107374344,2087.037037037037,2.5042874659184489,34.19972640218878,1.6100611257115831,1.2058660242222259,2.5517669748740941,12.54100665191115,0,-10.158215388048031,0,0,0,0,0,0.21361673533592518,0.30388964109240968,2.5634008240311021,7.2933513862178323,4.64309169929078,208.41700601962111,168.95160728562217,1625.3144620876851,2.5701254041447769E-2,30.094982734427266,-31392.694598219408,665.21458201707162,1.2455508206740875E-2,7.1462915409295249,-49710.563746828688,1731.3806107374344,1.4361992985460899,1.9936571385351341E-2,23.103260785596998,-39364.816658794065,940.52475152768125]
["KBM","KBM-14H03-A (400 V)",2.82,1.64,2.4124538742350454,1.3477395945447181,2850,10.4,3710,26.6,54,108,7.3099999999999998E-2,565,8,665.21458201707162,1715.4318640811196,2087.037037037037,2.5746955753613983,34.19972640218878,1.5996787259195351,1.2058660242222259,2.5517669748740941,12.54100665191115,0,-10.158215388048031,0,0,0,0,0,0.21361673533592518,0.30388964109240968,2.5634008240311021,7.2933513862178323,4.64309169929078,208.41700601962111,168.95160728562217,1625.3144620876851,2.5701254041447769E-2,30.094982734427266,-31392.694598219408,665.21458201707162,1.2522555133942678E-2,7.4428131011956005,-49617.842894818918,1715.4318640811196,1.4957916135837348,1.9936571385351341E-2,23.103260785596998,-39364.816658794065,940.52475152768125]
["KBM","KBM-14H03-A (480 V)",2.82,1.64,2.3210095867568072,1.2966534004227974,3600,10.4,4458,26.6,54,108,7.3099999999999998E-2,679,8,665.21458201707162,1712.7295013561793,2087.037037037037,2.5826012217623533,34.19972640218878,1.598528641502434,1.2058660242222259,2.5517669748740941,12.54100665191115,0,-10.158215388048031,0,0,0,0,0,0.21361673533592518,0.30388964109240968,2.5634008240311021,7.2933513862178323,4.64309169929078,208.41700601962111,168.95160728562217,1625.3144620876851,2.5701254041447769E-2,30.094982734427266,-31392.694598219408,665.21458201707162,1.2534174511779923E-2,7.4930080259756764,-49601.774170153127,1712.7295013561793,1.5058793514470492,1.9936571385351341E-2,23.103260785596998,-39364.816658794065,940.52475152768125]
["KBM","KBM-14H03-B (120 V)",2.87,2.81,2.6571955716212092,2.5306624491630565,1150,10.4,1789,9.01,19,63.7,7.3099999999999998E-2,160,8,1732.2903851171056,1789,1789,2.5389503283742116,34.19972640218878,1.5818746193576767,1.2058660242222259,1.3415315818893236,12.54100665191115,0,-10.158215388048031,0,0,0,0,0,0.35963748919625615,0.51161772200740907,4.3156498703550739,12.278825328177817,7.8169429853658547,208.41700601962111,168.95160728562217,1625.3144620876851,8.9833134574440338E-3,10.122379445261004,-44492.29691571791,1732.2903851171056,4.2795498985052699E-3,2.1482826139277607,-50520.816063591337,3194.0268290703102,2.1610586971158607,6.9605064303895625E-3,7.7707295650682235,-47084.801990059284,2101.9027595685475]
["KBM","KBM-14H03-B (240 V)",2.87,2.81,2.4794664818526857,2.3613966493835101,2850,10.4,3757,9.01,19,63.7,7.3099999999999998E-2,325,8,1732.2903851171056,3150.7215035306153,3538.4615384615381,2.4382588233416818,34.19972640218878,1.5696601405363981,1.2058660242222259,1.1418225648519735,12.54100665191115,0,-10.158215388048031,0,0,0,0,0,0.35963748919625615,0.51161772200740907,4.3156498703550739,12.278825328177817,7.8169429853658547,208.41700601962111,168.95160728562217,1625.3144620876851,8.9833134574440338E-3,10.122379445261004,-44492.29691571791,1732.2903851171056,4.328928133552977E-3,2.3753487519116199,-50457.531072383055,3150.7215035306153,2.3894752234747285,6.9605064303895625E-3,7.7707295650682235,-47084.801990059284,2101.9027595685475]
["KBM","KBM-14H03-B (400 V)",2.87,2.81,1.961016263096568,1.8676345362824456,5600,10.4,6283,9.01,19,63.7,7.3099999999999998E-2,565,8,1732.2903851171056,3156.2768345027162,3538.4615384615381,2.3576778014771405,34.19972640218878,1.5760694223789065,1.2058660242222259,1.1418225648519735,12.54100665191115,0,-10.158215388048031,0,0,0,0,0,0.35963748919625615,0.51161772200740907,4.3156498703550739,12.278825328177817,7.8169429853658547,208.41700601962111,168.95160728562217,1625.3144620876851,8.9833134574440338E-3,10.122379445261004,-44492.29691571791,1732.2903851171056,4.3223723049220959E-3,2.3464670642191177,-50465.933267335291,3156.2768345027162,2.3604217730717805,6.9605064303895625E-3,7.7707295650682235,-47084.801990059284,2101.9027595685475]
["KBM","KBM-14H03-B (480 V)",2.87,2.81,1.7923295129733443,1.7069804885460422,6500,10.4,7549,9.01,19,63.7,7.3099999999999998E-2,679,8,1732.2903851171056,3156.9990998849653,3538.4615384615381,2.3465838834591164,34.19972640218878,1.5769547094304242,1.2058660242222259,1.1418225648519735,12.54100665191115,0,-10.158215388048031,0,0,0,0,0,0.35963748919625615,0.51161772200740907,4.3156498703550739,12.278825328177817,7.8169429853658547,208.41700601962111,168.95160728562217,1625.3144620876851,8.9833134574440338E-3,10.122379445261004,-44492.29691571791,1732.2903851171056,4.3215247233798475E-3,2.3427070529302858,-50467.019559512351,3156.9990998849653,2.3566394005644096,6.9605064303895625E-3,7.7707295650682235,-47084.801990059284,2101.9027595685475]
["KBM","KBM-14H03-C (120 V)",2.92,6.04,2.4828171122335672,4.9855765305894924,3000,10.4,3806,1.96,4.0999999999999996,30,7.3099999999999998E-2,160,8,3806,3806,3806,2.365360643053652,34.19972640218878,1.5443228131220894,1.2058660242222259,0.63058328954282716,12.54100665191115,0,-10.158215388048031,0,0,0,0,0,0.7597918329497465,1.0808744317571826,9.1175019953969585,25.940986362172382,16.514544832876712,208.41700601962111,168.95160728562217,1625.3144620876851,1.9237196708762545E-3,2.190914249130445,-49471.797431376996,4533.5918825709668,9.3344379448291679E-4,0.39599766826847793,-50761.600512979428,7165.2804948316289,3.8882544281168347,1.5033084555502382E-3,1.6819170060076922,-50019.369773583923,5235.9199238974052]
["KBM","KBM-14H03-C (240 V)",2.92,6.04,1.7796416363911933,3.573577583114846,6600,10.4,7980,1.96,4.0999999999999996,30,7.3099999999999998E-2,325,8,4533.5918825709668,7181.317471913816,7513.3333333333339,1.6792006907837922,34.19972640218878,1.5509611994529307,1.2058660242222259,0.45837217430428878,12.54100665191115,0,-10.158215388048031,0,0,0,0,0,0.7597918329497465,1.0808744317571826,9.1175019953969585,25.940986362172382,16.514544832876712,208.41700601962111,168.95160728562217,1625.3144620876851,1.9237196708762545E-3,2.190914249130445,-49471.797431376996,4533.5918825709668,9.3114404453837837E-4,0.38213987887265755,-50764.595864715331,7181.317471913816,3.7521864274697254,1.5033084555502382E-3,1.6819170060076922,-50019.369773583923,5235.9199238974052]
["KBM","KBM-17H01-A (120 V)",2.08,1.65,1.909859317102744,1.4805110985292589,750,5.95,1460,21.3,66,77.900000000000006,5.1199999999999996E-2,160,10,1054.2785081182196,1460,1460,1.7487928039600082,48.828125000000007,2.2099352137854726,2.0897930182215365,3.1698654460710101,12.434268458418142,0,-10.071757451318696,0,0,0,0,0,0.28890095968123702,0.41098844063281109,3.4668115161748441,9.8637225751874666,6.2794408205128187,206.64314086403843,167.51363744397,1611.4811922109914,2.6022022275276519E-2,13.564858363011515,-43224.698956309665,1054.2785081182196,7.3257362393894538E-3,3.4050891625489688,-50327.496484972653,2398.9378280662827,1.1848156988388414,4.1385777363615428E-2,18.046735796758032,-37387.943920417885,757.12992896110336]
["KBM","KBM-17H01-A (240 V)",2.08,1.65,1.8853739412424524,1.4615301870096529,1950,5.95,3068,21.3,66,77.900000000000006,5.1199999999999996E-2,325,10,1054.2785081182196,2260.91705308476,2893.4531450577665,1.8543418588617353,48.828125000000007,2.1476326820477523,2.0897930182215365,3.1698654460710101,12.434268458418142,0,-10.071757451318696,0,0,0,0,0,0.28890095968123702,0.41098844063281109,3.4668115161748441,9.8637225751874666,6.2794408205128187,206.64314086403843,167.51363744397,1611.4811922109914,2.6022022275276519E-2,13.564858363011515,-43224.698956309665,1054.2785081182196,7.9542674422952864E-3,4.1702196364088238,-50088.714843200702,2260.91705308476,1.4510462008356071,4.1385777363615428E-2,18.046735796758032,-37387.943920417885,757.12992896110336]
["KBM","KBM-17H01-A (400 V)",2.08,1.65,1.7590809499630535,1.363628643382212,3800,5.95,5132,21.3,66,77.900000000000006,5.1199999999999996E-2,565,10,1054.2785081182196,2238.2641757100369,2893.4531450577665,1.8909732597366857,48.828125000000007,2.1403394212602187,2.0897930182215365,3.1698654460710101,12.434268458418142,0,-10.071757451318696,0,0,0,0,0,0.28890095968123702,0.41098844063281109,3.4668115161748441,9.8637225751874666,6.2794408205128187,206.64314086403843,167.51363744397,1611.4811922109914,2.6022022275276519E-2,13.564858363011515,-43224.698956309665,1054.2785081182196,8.0699036674329368E-3,4.2961714936170639,-50044.784155974638,2238.2641757100369,1.4948717016064947,4.1385777363615428E-2,18.046735796758032,-37387.943920417885,757.12992896110336]
["KBM","KBM-17H01-A (480 V)",2.08,1.65,1.6634258568314222,1.2894774083964513,4650,5.95,6166,21.3,66,77.900000000000006,5.1199999999999996E-2,679,10,1054.2785081182196,2240.5712146752421,2893.4531450577665,1.8792765518362327,48.828125000000007,2.1427720372580796,2.0897930182215365,3.1698654460710101,12.434268458418142,0,-10.071757451318696,0,0,0,0,0,0.28890095968123702,0.41098844063281109,3.4668115161748441,9.8637225751874666,6.2794408205128187,206.64314086403843,167.51363744397,1611.4811922109914,2.6022022275276519E-2,13.564858363011515,-43224.698956309665,1054.2785081182196,8.0579553455455127E-3,4.2833288652584596,-50049.323373603787,2240.5712146752421,1.4904030527790328,4.1385777363615428E-2,18.046735796758032,-37387.943920417885,757.12992896110336]
["KBM","KBM-17H01-B (120 V)",2.0699999999999998,3.11,1.8568076694054458,2.7265898229154857,1800,6.14,2782,6.02,18,41.2,5.1199999999999996E-2,160,10,2310.7595572199057,2782,2782,1.7404994090477501,48.828125000000007,2.1672433654788046,2.0251251560941599,1.3057213206401006,12.434268458418142,0,-10.071757451318696,0,0,0,0,0,0.54716513775025211,0.77839321468760903,6.5659816530030248,18.681437152502617,11.892972267525494,206.64314086403843,167.51363744397,1611.4811922109914,7.3666213224903567E-3,3.9628966775858756,-48492.18427225393,2310.7595572199057,2.0187236533937406E-3,0.943402212325398,-50674.079117285379,4781.9762051734015,2.1960516774189478,1.1120334540238435E-2,5.1091039722230125,-46960.702552463568,1838.0644951278377]
["KBM","KBM-17H01-B (240 V)",2.0699999999999998,3.11,1.7052315331274501,2.50401106186116,4200,6.14,5838,6.02,18,41.2,5.1199999999999996E-2,325,10,2310.7595572199057,4650.9657496086074,5470.8737864077666,1.6660653223901258,48.828125000000007,2.1520198049477206,2.0251251560941599,1.3057213206401006,12.434268458418142,0,-10.071757451318696,0,0,0,0,0,0.54716513775025211,0.77839321468760903,6.5659816530030248,18.681437152502617,11.892972267525494,206.64314086403843,167.51363744397,1611.4811922109914,7.3666213224903567E-3,3.9628966775858756,-48492.18427225393,2310.7595572199057,2.1107952943736309E-3,1.0700752710452226,-50636.514703891968,4650.9657496086074,2.4909212245231149,1.1120334540238435E-2,5.1091039722230125,-46960.702552463568,1838.0644951278377]
["KBM","KBM-17H01-B (400 V)",2.0699999999999998,3.11,1.0653261508694498,1.5643555813060936,8650,6.14,9600,6.02,18,41.2,5.1199999999999996E-2,565,10,2310.7595572199057,4716.9957489582321,5470.8737864077666,1.5221338409897909,48.828125000000007,2.166131157379668,2.0251251560941599,1.3057213206401006,12.434268458418142,0,-10.071757451318696,0,0,0,0,0,0.54716513775025211,0.77839321468760903,6.5659816530030248,18.681437152502617,11.892972267525494,206.64314086403843,167.51363744397,1611.4811922109914,7.3666213224903567E-3,3.9628966775858756,-48492.18427225393,2310.7595572199057,2.0632539530150971E-3,1.0066597605043661,-50655.911149758067,4716.9957489582321,2.3433025985773961,1.1120334540238435E-2,5.1091039722230125,-46960.702552463568,1838.0644951278377]
["KBM","KBM-17H01-B (480 V)",2.0699999999999998,3.11,0.71619724391352901,1.0516846459816871,9600,6.14,9600,6.02,18,41.2,5.1199999999999996E-2,679,10,2310.7595572199057,4784.6089771887164,5470.8737864077666,1.3952690812381088,48.828125000000007,2.1782578467057023,2.0251251560941599,1.3057213206401006,12.434268458418142,0,-10.071757451318696,0,0,0,0,0,0.54716513775025211,0.77839321468760903,6.5659816530030248,18.681437152502617,11.892972267525494,206.64314086403843,167.51363744397,1611.4811922109914,7.3666213224903567E-3,3.9628966775858756,-48492.18427225393,2310.7595572199057,2.0169656495839677E-3,0.94081761200287661,-50674.796367256757,4784.6089771887164,2.1900352447674489,1.1120334540238435E-2,5.1091039722230125,-46960.702552463568,1838.0644951278377]
["KBM","KBM-17H01-C (120 V)",2.0699999999999998,6.1,1.7384616860807027,4.8970751720583179,3900,6.35,5468,1.56,5,21.5,5.1199999999999996E-2,160,10,4474.9565906551752,5468,5468,1.605166281920329,48.828125000000007,2.1511397836071233,1.9581525131367155,0.64743694995186407,12.434268458418142,0,-10.071757451318696,0,0,0,0,0,1.0732177943011376,1.5267519644998122,12.878613531613651,36.642047147995491,23.327051714439072,206.64314086403843,167.51363744397,1611.4811922109914,2.2622186719710811E-3,1.0870684727370978,-50166.048120919979,4474.9565906551752,5.2279160399924286E-4,0.19936613467176323,-50783.663593480829,9667.1019701920704,3.4318453047119171,3.259415873324842E-3,1.3551380440169456,-49811.974971150856,3706.9246668396613]
["KBM","KBM-17H01-C (240 V)",2.0699999999999998,6.1,0.90187801085407349,2.5405014390255594,9000,6.35,9600,1.56,5,21.5,5.1199999999999996E-2,325,10,4474.9565906551752,9600,9600,0.82400321157767853,48.828125000000007,2.1727662455808918,1.9581525131367155,0.64743694995186407,12.434268458418142,0,-10.071757451318696,0,0,0,0,0,1.0732177943011376,1.5267519644998122,12.878613531613651,36.642047147995491,23.327051714439072,206.64314086403843,167.51363744397,1611.4811922109914,2.2622186719710811E-3,1.0870684727370978,-50166.048120919979,4474.9565906551752,4.9913641047391502E-4,0.15561720997601908,-50792.062803655645,9932.9283295350051,2.6787608249908508,3.259415873324842E-3,1.3551380440169456,-49811.974971150856,3706.9246668396613]
["KBM","KBM-17H02-A (120 V)",3.58,1.59,3.3104228163114229,1.4330834702646853,375,12.2,812,27.5,97,140,9.5399999999999999E-2,160,10,472.71716234697635,812,812,2.9962755382530011,26.20545073375262,1.3657363240400404,1.0368601968401385,3.1666936563768981,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.16455165968445504,0.23409001511062624,1.9746199162134603,5.61816036265503,3.5766319711980139,210.22327053877603,170.41584141661951,1639.4003944278797,7.6400195858433745E-2,36.132273191648366,-34152.849209235828,472.71716234697635,2.2098246093325863E-2,7.5777099358276416,-50072.740511842596,1343.5735435026049,1.1363617847509069,4.4348591385126729E-2,23.850396932247211,-43549.529466508327,757.88827731000242]
["KBM","KBM-17H02-A (240 V)",3.58,1.59,3.2293984816464585,1.3980080007127527,1100,12.2,1710,27.5,97,140,9.5399999999999999E-2,325,10,472.71716234697635,1271.359838524784,1610,3.174781191126816,26.20545073375262,1.2939180297816766,1.0368601968401385,3.1666936563768981,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.16455165968445504,0.23409001511062624,1.9746199162134603,5.61816036265503,3.5766319711980139,210.22327053877603,170.41584141661951,1639.4003944278797,7.6400195858433745E-2,36.132273191648366,-34152.849209235828,472.71716234697635,2.3396147042202605E-2,9.3409679452893126,-49692.230380677014,1271.359838524784,1.4007819110920652,4.4348591385126729E-2,23.850396932247211,-43549.529466508327,757.88827731000242]
["KBM","KBM-17H02-A (400 V)",3.58,1.59,3.1376260209545084,1.3582796627508693,2100,12.2,2861,27.5,97,140,9.5399999999999999E-2,565,10,472.71716234697635,1252.3382263474198,1610,3.3161895979523419,26.20545073375262,1.2757980886340277,1.0368601968401385,3.1666936563768981,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.16455165968445504,0.23409001511062624,1.9746199162134603,5.61816036265503,3.5766319711980139,210.22327053877603,170.41584141661951,1639.4003944278797,7.6400195858433745E-2,36.132273191648366,-34152.849209235828,472.71716234697635,2.3782721915847252E-2,9.8050511714916233,-49578.896881689172,1252.3382263474198,1.4703763463061674,4.4348591385126729E-2,23.850396932247211,-43549.529466508327,757.88827731000242]
["KBM","KBM-17H02-A (480 V)",3.58,1.59,3.0667933265015219,1.3276161586586674,2600,12.2,3438,27.5,97,140,9.5399999999999999E-2,679,10,472.71716234697635,1249.5485211281468,1610,3.3333551384988005,26.20545073375262,1.2736086183291067,1.0368601968401385,3.1666936563768981,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.16455165968445504,0.23409001511062624,1.9746199162134603,5.61816036265503,3.5766319711980139,210.22327053877603,170.41584141661951,1639.4003944278797,7.6400195858433745E-2,36.132273191648366,-34152.849209235828,472.71716234697635,2.3841062910454968E-2,9.873195257530103,-49561.792849575068,1249.5485211281468,1.4805953090121409,4.4348591385126729E-2,23.850396932247211,-43549.529466508327,757.88827731000242]
["KBM","KBM-17H02-B (120 V)",3.52,2.99,3.246760839074665,2.7056340325622208,1000,12.3,1565,7.78,27,72.8,9.5399999999999999E-2,160,10,1237.3711695743309,1565,1565,3.0923807131518508,26.20545073375262,1.3089495925171402,1.0284304391422512,1.5335463258785942,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.31471445747468979,0.44771053811949074,3.7765734896962773,10.745052914867777,6.8405131407407413,210.22327053877603,170.41584141661951,1639.4003944278797,2.1662477493410739E-2,10.249560421072978,-45849.657153441156,1237.3711695743309,6.1046986617374682E-3,2.2732039216489941,-50561.404713547941,2697.7430923289362,2.3172174639236984,1.2313801850205992E-2,6.7105835078996119,-48680.94818339355,1734.4087177931133]
["KBM","KBM-17H02-B (240 V)",3.52,2.99,3.0516230392837325,2.5430191994031106,2300,12.3,3285,7.78,27,72.8,9.5399999999999999E-2,325,10,1237.3711695743309,2649.4325070821142,3096.1538461538462,2.9804638498739124,26.20545073375262,1.2969495747879474,1.0284304391422512,1.3837568823188313,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.31471445747468979,0.44771053811949074,3.7765734896962773,10.745052914867777,6.8405131407407413,210.22327053877603,170.41584141661951,1639.4003944278797,2.1662477493410739E-2,10.249560421072978,-45849.657153441156,1237.3711695743309,6.2594608604300099E-3,2.4821523008465078,-50514.534243156515,2649.4325070821142,2.5302114803090845,1.2313801850205992E-2,6.7105835078996119,-48680.94818339355,1734.4087177931133]
["KBM","KBM-17H02-B (400 V)",3.52,2.99,2.6043536142310146,2.1702946785258455,4400,12.3,5495,7.78,27,72.8,9.5399999999999999E-2,565,10,1237.3711695743309,2645.077785707902,3096.1538461538462,2.9695554739633474,26.20545073375262,1.2977118518370021,1.0284304391422512,1.3837568823188313,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.31471445747468979,0.44771053811949074,3.7765734896962773,10.745052914867777,6.8405131407407413,210.22327053877603,170.41584141661951,1639.4003944278797,2.1662477493410739E-2,10.249560421072978,-45849.657153441156,1237.3711695743309,6.2739488457827577E-3,2.5008193963248093,-50510.146487656501,2645.077785707902,2.5492400061844371,1.2313801850205992E-2,6.7105835078996119,-48680.94818339355,1734.4087177931133]
["KBM","KBM-17H02-B (480 V)",3.52,2.99,2.2252489291013626,1.8543741075844689,5450,12.3,6602,7.78,27,72.8,9.5399999999999999E-2,679,10,1237.3711695743309,2657.0163648264056,3096.1538461538462,2.8887752690359276,26.20545073375262,1.3027716824289832,1.0284304391422512,1.3837568823188313,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.31471445747468979,0.44771053811949074,3.7765734896962773,10.745052914867777,6.8405131407407413,210.22327053877603,170.41584141661951,1639.4003944278797,2.1662477493410739E-2,10.249560421072978,-45849.657153441156,1237.3711695743309,6.2344436708700237E-3,2.449583943966573,-50522.110818395522,2657.0163648264056,2.4970125382279269,1.2313801850205992E-2,6.7105835078996119,-48680.94818339355,1734.4087177931133]
["KBM","KBM-17H02-C (120 V)",3.64,5.27,3.2166051656467265,4.5304298107700376,1900,12.7,2797,2.5099999999999998,9.1999999999999993,43,9.5399999999999999E-2,160,10,2310.112350897934,2797,2797,3.0167182359546807,26.20545073375262,1.2561539238305519,0.99603892924800708,0.85806220951018952,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.53641066117263436,0.76309397316437566,6.4369279340716128,18.314255355945015,11.659217075783474,210.22327053877603,170.41584141661951,1639.4003944278797,7.7328293424558442E-3,3.437286694500266,-49207.683009709501,2310.112350897934,2.0770639854113806E-3,0.67672789357963203,-50743.239956469886,4782.4778634053628,3.6200225287346335,4.2147722819922719E-3,2.1795768810423923,-50162.845859873654,3200.9922276487105]
["KBM","KBM-17H02-C (240 V)",3.64,5.27,2.6891697281044387,3.7875629973301956,4350,12.7,5622,2.5099999999999998,9.1999999999999993,43,9.5399999999999999E-2,325,10,2310.112350897934,4743.9524159487992,5241.8604651162786,2.6030589504560453,26.20545073375262,1.2554719436278259,0.99603892924800708,0.7497675187305658,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.53641066117263436,0.76309397316437566,6.4369279340716128,18.314255355945015,11.659217075783474,210.22327053877603,170.41584141661951,1639.4003944278797,7.7328293424558442E-3,3.437286694500266,-49207.683009709501,2310.112350897934,2.1036796332959597E-3,0.71512643295109568,-50736.013729704522,4743.9524159487992,3.8254279493091081,4.2147722819922719E-3,2.1795768810423923,-50162.845859873654,3200.9922276487105]
["KBM","KBM-17H02-C (400 V)",3.64,5.27,0.99787623049680418,1.4054594795729638,7560,12.7,9375,2.5099999999999998,9.1999999999999993,43,9.5399999999999999E-2,565,10,2310.112350897934,4875.3062910377648,5241.8604651162786,1.9361425085768065,26.20545073375262,1.2767841317564195,0.99603892924800708,0.7497675187305658,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.53641066117263436,0.76309397316437566,6.4369279340716128,18.314255355945015,11.659217075783474,210.22327053877603,170.41584141661951,1639.4003944278797,7.7328293424558442E-3,3.437286694500266,-49207.683009709501,2310.112350897934,2.0165870604503893E-3,0.5801041397868294,-50759.659619659571,4875.3062910377648,3.1031527959227487,4.2147722819922719E-3,2.1795768810423923,-50162.845859873654,3200.9922276487105]
["KBM","KBM-17H02-D (120 V)",3.58,6.5,3.083627022405472,5.4577469423105702,2400,12.8,3365,1.65,3.1,34.200000000000003,9.5399999999999999E-2,160,10,3365,3365,3365,2.8840437209976724,26.20545073375262,1.2751648870605938,0.98825737511325695,0.71322436849925708,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.67269546411884129,0.95697175988620786,8.0723455694260959,22.967322237268988,14.621451454583074,210.22327053877603,170.41584141661951,1639.4003944278797,2.236880984939061E-3,2.2714907743900832,-49702.327004775136,4233.2841459140927,1.2037323730476029E-3,0.40598346489728943,-50769.930661534745,6327.9430257069707,4.1537243087894211,1.592077894176066E-3,1.4290952124093139,-50368.633990687049,5193.7448430034337]
["KBM","KBM-17H02-D (240 V)",3.58,6.5,2.1997486777344109,3.8933604915653293,5600,12.8,7054,1.65,3.1,34.200000000000003,9.5399999999999999E-2,325,10,4233.2841459140927,6341.7585557425273,6590.6432748538009,2.01692488713344,26.20545073375262,1.2817471054492864,0.98825737511325695,0.46209432164020792,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.67269546411884129,0.95697175988620786,8.0723455694260959,22.967322237268988,14.621451454583074,210.22327053877603,170.41584141661951,1639.4003944278797,2.236880984939061E-3,2.2714907743900832,-49702.327004775136,4233.2841459140927,1.2010215080234523E-3,0.38950822656441692,-50772.731932696952,6341.7585557425273,3.9851617837770665,1.592077894176066E-3,1.4290952124093139,-50368.633990687049,5193.7448430034337]
["KBM","KBM-17H02-E (120 V)",3.75,9.33,3.0012074983043124,7.2844842191852246,3500,12.9,4633,0.8,3.1,24.8,9.5399999999999999E-2,160,10,4153.695712245395,4633,4633,2.7588126684696799,26.20545073375262,1.2169507767387708,0.98059646522865807,0.51802287934383773,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.92180390872693607,1.3113516529502844,11.061646904723233,31.472439670806828,20.035977379081483,210.22327053877603,170.41584141661951,1639.4003944278797,2.650497638264534E-3,1.1029158588490393,-50310.711105740804,4153.695712245395,6.6245942886233053E-4,0.16834084653099118,-50793.64097659877,8630.2529471139023,4.898771827634941,1.4082769957817543E-3,0.68851408306941764,-50612.468613023171,5755.467543595636]
["KBM","KBM-17H02-E (240 V)",3.75,9.33,1.1013522061959158,2.6731849664949414,7500,12.9,9600,0.8,3.1,24.8,9.5399999999999999E-2,325,10,4153.695712245395,8920.4649935066918,9088.7096774193542,0.59971067669892486,26.20545073375262,1.238257017197393,0.98059646522865807,0.41699479352821411,12.64969440144969,0,-10.246252465174248,0,0,0,0,0,0.92180390872693607,1.3113516529502844,11.061646904723233,31.472439670806828,20.035977379081483,210.22327053877603,170.41584141661951,1639.4003944278797,2.650497638264534E-3,1.1029158588490393,-50310.711105740804,4153.695712245395,6.2840087143350119E-4,8.9357032945464043E-2,-50801.914406487056,8920.4649935066918,2.6003178944077581,1.4082769957817543E-3,0.68851408306941764,-50612.468613023171,5755.467543595636]
["KBM","KBM-17H03-A (120 V)",4.88,3,4.5018112474564687,2.7283704530039206,700,18.5,1136,8.61,33,100,0.14200000000000002,160,10,862.51303695395904,1136,1136,4.2662536815864982,17.6056338028169,0.97622765389436206,0.6960441989596996,2.112676056338028,12.876817680754442,0,-10.430222321411096,0,0,0,0,0,0.2318558803621186,0.32983651846194778,2.7822705643454233,7.9160764430867472,5.0395307832422578,213.9977963949473,173.47563112534047,1668.8355714257755,3.8962277474955669E-2,16.9604331690743,-43613.75266793411,862.51303695395904,1.1227764478565451E-2,3.4920312142441832,-50500.302949968609,1970.9880557666497,2.3416087823025027,1.568678216244096E-2,7.5154308154422358,-49393.117491457531,1551.0097094869186]
["KBM","KBM-17H03-A (240 V)",4.88,3,4.2971834634811747,2.6043536142310151,1700,18.5,2389,8.61,33,100,0.14200000000000002,325,10,862.51303695395904,1930.4184815709446,2254,4.2181883450228783,17.6056338028169,0.95780832800097038,0.6960441989596996,1.5473790946118136,12.876817680754442,0,-10.430222321411096,0,0,0,0,0,0.2318558803621186,0.32983651846194778,2.7822705643454233,7.9160764430867472,5.0395307832422578,213.9977963949473,173.47563112534047,1668.8355714257755,3.8962277474955669E-2,16.9604331690743,-43613.75266793411,862.51303695395904,1.1519645885665864E-2,3.8850068083483085,-50427.828052477184,1930.4184815709446,2.605121633685743,1.568678216244096E-2,7.5154308154422358,-49393.117491457531,1551.0097094869186]
["KBM","KBM-17H03-A (400 V)",4.88,3,3.5950293027816365,2.1788056380494769,3400,18.5,3997,8.61,33,100,0.14200000000000002,565,10,862.51303695395904,1932.7364961594571,2254,4.1495559520560601,17.6056338028169,0.96103185773152855,0.6960441989596996,1.5473790946118136,12.876817680754442,0,-10.430222321411096,0,0,0,0,0,0.2318558803621186,0.32983651846194778,2.7822705643454233,7.9160764430867472,5.0395307832422578,213.9977963949473,173.47563112534047,1668.8355714257755,3.8962277474955669E-2,16.9604331690743,-43613.75266793411,862.51303695395904,1.150228710377503E-2,3.8627540316498643,-50432.138282274318,1932.7364961594571,2.5901998606113374,1.568678216244096E-2,7.5154308154422358,-49393.117491457531,1551.0097094869186]
["KBM","KBM-17H03-A (480 V)",4.88,3,3.4812625526936092,2.1098560925415812,3950,18.5,4803,8.61,33,100,0.14200000000000002,679,10,862.51303695395904,1928.4715572122971,2254,4.1971074979397196,17.6056338028169,0.95884169541601638,0.6960441989596996,1.5473790946118136,12.876817680754442,0,-10.430222321411096,0,0,0,0,0,0.2318558803621186,0.32983651846194778,2.7822705643454233,7.9160764430867472,5.0395307832422578,213.9977963949473,173.47563112534047,1668.8355714257755,3.8962277474955669E-2,16.9604331690743,-43613.75266793411,862.51303695395904,1.153429005734889E-2,3.9036809945735005,-50424.191867315145,1928.4715572122971,2.6176437549912155,1.568678216244096E-2,7.5154308154422358,-49393.117491457531,1551.0097094869186]
["KBM","KBM-17H03-B (120 V)",4.8899999999999997,5.32,4.3653927248062727,4.5951502366381822,1400,18.8,1998,2.81,11,57,0.14200000000000002,160,10,1684.8382566120974,1998,1998,4.1413104744020952,17.6056338028169,0.95870075013048239,0.68493711067842777,1.2012012012012012,12.876817680754442,0,-10.430222321411096,0,0,0,0,0,0.41031694775795358,0.58371395758021161,4.9238033730954429,14.009134981925079,8.9184923232598639,213.9977963949473,173.47563112534047,1668.8355714257755,1.3656948226580453E-2,5.6741710728172361,-48327.765619914135,1684.8382566120974,3.5859294013781589E-3,1.0209143750048457,-50724.961003301672,3621.4005345593055,3.6799974354036724,5.2279132846631184E-3,2.4741911308390887,-50334.121084031794,2875.2720312309775]
["KBM","KBM-17H03-B (240 V)",4.8899999999999997,5.32,3.8500338614610872,4.0526672225906184,3150,18.8,4194,2.81,11,57,0.14200000000000002,325,10,{"$f":"IF(AQ736<I736,IF(AQ736<0,0,AQ736),I736)","v":1684.8382566120974},{"$f":"IF(AU736<I736,IF(AU736<0,0,AU736),I736)","v":3573.8007733040213},{"$f":"IF(UAC_V*0.98/L736*1000<I736,IF(UAC_V*0.98/L736*1000<0,0,UAC_V*0.98/L736*1000),I736)","v":3954.385964912281},{"$f":"C736+(E736-C736)/G736*Q736","v":3.7101168920252814},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M736,(inertia/gear^2+gear_inertia)/M736),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M736,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M736))","v":17.6056338028169},{"$f":"IF((C736+(E736-C736)/G736*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X736^2*time1+Y736^2*time2+Z736^2*time3+AA736^2*time4)/time)/(C736+(E736-C736)/G736*mspeed),SQRT((((X736-Y736)*2/PI()+Y736)^2*time1+Y736^2*time2+((Z736-Y736)*2/PI()+Y736)^2*time3+AA736^2*time4)/time)/(C736+(E736-C736)/G736*mspeed)),IF(AccType=1,SQRT((X736^2*time1+Y736^2*time2+Z736^2*time3+AA736^2*time4+AB736^2*time5+AC736^2*time6+AD736^2*time7+AE736^2*time8)/time)/(C736+(E736-C736)/G736*mspeed),SQRT((((X736-Y736)*2/PI()+Y736)^2*time1+Y736^2*time2+((Z736-Y736)*2/PI()+Y736)^2*time3+AA736^2*time4+((AB736-AC736)*2/PI()+AC736)^2*time5+AC736^2*time6+((AD736-AC736)*2/PI()+AC736)^2*time7+AE736^2*time8)/time)/(C736+(E736-C736)/G736*mspeed))))","v":0.95463076728995244},{"$f":"IF(move1,MAX(ABS(X736),ABS(Z736))/H736,MAX(ABS(X736),ABS(Z736),ABS(AB736),ABS(AD736))/H736)","v":0.68493711067842777},{"$f":"IF(AZ736>0,speed/(MIN(AZ736,I736)),\"NA\")","v":0.8347036294066752},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M736+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M736+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.876817680754442},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M736+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M736+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.430222321411096},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M736+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M736+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M736+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M736+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH736/Irms","v":0.41031694775795358},{"$f":"AI736/Ipeak","v":0.58371395758021161},{"$f":"IF(move1,IF(AccType=1,SQRT((X736^2*time1+Y736^2*time2+Z736^2*time3+AA736^2*time4)/time)/(C736/D736),SQRT((((X736-Y736)*2/PI()+Y736)^2*time1+Y736^2*time2+((Z736-AA736)*2/PI()+AA736)^2*time3+AA736^2*time4)/time)/(C736/D736)),IF(AccType=1,SQRT((X736^2*time1+Y736^2*time2+Z736^2*time3+AA736^2*time4+AB736^2*time5+AC736^2*time6+AD736^2*time7+AE736^2*time8)/time)/(C736/D736),SQRT((((X736-Y736)*2/PI()+Y736)^2*time1+Y736^2*time2+((Z736-AA736)*2/PI()+AA736)^2*time3+AA736^2*time4+((AB736-AC736)*2/PI()+AC736)^2*time5+AC736^2*time6+((AD736-AE736)*2/PI()+AE736)^2*time7+AE736^2*time8)/time)/(C736/D736)))","v":4.9238033730954429},{"$f":"IF(move1,MAX(ABS(X736),ABS(Z736))/(C736/D736),MAX(ABS(X736),ABS(Z736),ABS(AB736),ABS(AD736))/(C736/D736))","v":14.009134981925079},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X736),ABS(Z736))/(C736/D736),MAX(ABS((X736-Y736)*2/PI()+Y736),ABS((Z736-Y736)*2/PI()+Y736))/(C736/D736)),IF(AccType=1,MAX(ABS(X736),ABS(Z736),ABS(AB736),ABS(AD736))/(C736/D736),MAX(ABS((X736-Y736)*2/PI()+Y736),ABS((Z736-Y736)*2/PI()+Y736),ABS((AB736-AC736)*2/PI()+AC736),ABS((AD736-AC736)*2/PI()+AC736))/(C736/D736)))","v":8.9184923232598639},{"$f":"IF((C736+(E736-C736)/G736*mspeed)<0,\"NA\",U736*(C736+(E736-C736)/G736*mspeed)*mspeed/9.55)","v":213.9977963949473},{"$f":"IF(move1,IF(speed1>speed2,AM736/2*time1/time,AM736/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z736*-speed/30*PI(),((Z736-AA736)*2/PI()+AA736)*-speed/30*PI()),IF(AccType=1,X736*-speed/30*PI(),((X736-Y736)*2/PI()+Y736)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z736*-speed/30*PI(),((Z736-AA736)*2/PI()+AA736)*-speed/30*PI()),IF(AccType=1,X736*-speed/30*PI(),((X736-Y736)*2/PI()+Y736)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD736*-speed/30*PI(),((AD736-AE736)*2/PI()+AE736)*-speed/30*PI()),IF(AccType=1,AB736*-speed/30*PI(),((AB736-AC736)*2/PI()+AC736)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD736*-speed/30*PI(),((AD736-AE736)*2/PI()+AE736)*-speed/30*PI()),IF(AccType=1,AB736*-speed/30*PI(),((AB736-AC736)*2/PI()+AC736)*-speed/30*PI()),0)/2*time7/time)))","v":173.47563112534047},{"$f":"IF(move1,MAX(IF(AccType=1,Z736*-speed/30*PI(),((Z736-AA736)*2/PI()+AA736)*-speed/30*PI()),IF(AccType=1,X736*-speed/30*PI(),((X736-Y736)*2/PI()+Y736)*-speed/30*PI()),0),MAX(IF(AccType=1,Z736*-speed/30*PI(),((Z736-AA736)*2/PI()+AA736)*-speed/30*PI()),IF(AccType=1,X736*-speed/30*PI(),((X736-Y736)*2/PI()+Y736)*-speed/30*PI()),IF(AccType=1,AD736*-speed/30*PI(),((AD736-AE736)*2/PI()+AE736)*-speed/30*PI()),IF(AccType=1,AB736*-speed/30*PI(),((AB736-AC736)*2/PI()+AC736)*-speed/30*PI()),0))","v":1668.8355714257755},{"$f":"(L736^2)/1000000+((K736/1000)^2*(D736/C736*H736)^2*PI()*PI()*(O736/2)^2)/1200","v":1.3656948226580453E-2},{"$f":"SQRT(3)*L736*J736*D736/C736*H736/1000","v":5.6741710728172361},{"$f":"0.75*J736^2*(D736/C736*H736)^2-(UAC_V*0.98)^2","v":-48327.765619914135},{"$f":"-AO736/2/AN736+SQRT((AO736/2/AN736)^2-AP736/AN736)","v":1684.8382566120974},{"$f":"(L736^2)/1000000+((K736/1000)^2*AV736^2*PI()*PI()*(O736/2)^2)/1200","v":3.6562025087112818E-3},{"$f":"SQRT(3)*L736*J736*AV736/1000","v":1.1223416665515569},{"$f":"0.75*J736^2*AV736^2-(UAC_V*0.98)^2","v":-50708.233959950936},{"$f":"-AS736/2/AR736+SQRT((AS736/2/AR736)^2-AT736/AR736)","v":3573.8007733040213},{"$f":"D736+(F736-D736)*((0.85*UAC_V-D736*J736)/L736*1000)/G736","v":4.0456031922724272},{"$f":"(L736^2)/1000000+((K736/1000)^2*AJ736^2*PI()*PI()*(O736/2)^2)/1200","v":5.2279132846631184E-3},{"$f":"SQRT(3)*L736*J736*AJ736/1000","v":2.4741911308390887},{"$f":"0.75*J736^2*AJ736^2-(UAC_V*0.98)^2","v":-50334.121084031794},{"$f":"IF(((AX736/2/AW736)^2-AY736/AW736)>0,-AX736/2/AW736+SQRT((AX736/2/AW736)^2-AY736/AW736),-9999)","v":2875.2720312309775}]
["KBM","KBM-17H03-B (400 V)",4.8899999999999997,5.32,1.8011681364546206,1.8959664594259165,6150,18.8,7006,2.81,11,57,0.14200000000000002,565,10,1684.8382566120974,3637.0828436735619,3954.385964912281,3.0632784751393274,17.6056338028169,0.97054000380066319,0.68493711067842777,0.8347036294066752,12.876817680754442,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-10.430222321411096,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.41031694775795358,0.58371395758021161,4.9238033730954429,14.009134981925079,8.9184923232598639,213.9977963949473,173.47563112534047,1668.8355714257755,1.3656948226580453E-2,5.6741710728172361,-48327.765619914135,1684.8382566120974,3.5636861374357533E-3,0.98663988906841782,-50730.255547037479,3637.0828436735619,3.556451305156231,5.2279132846631184E-3,2.4741911308390887,-50334.121084031794,2875.2720312309775]
["KBM","KBM-17H03-C (120 V)",5.05,6.14,4.4762327744595565,5.2723589805177342,1600,18.8,2239,2.1,8.8000000000000007,51.34,0.14200000000000002,160,10,1930.6834454921473,2239,2239,4.2470844887593415,17.6056338028169,0.92589260864703427,0.68493711067842777,1.0719071013845467,12.876817680754442,0,-10.430222321411096,0,0,0,0,0,0.45855736729150048,0.65234043366198247,5.502688407498006,15.656170407887579,9.9670276412174523,213.9977963949473,173.47563112534047,1668.8355714257755,1.0955224928801929E-2,4.2684542281114854,-49077.0573450101,1930.6834454921473,2.9181813954221631E-3,0.78640322127602713,-50746.503135025981,4037.5385896962139,4.2112351966841333,4.2176087356127247E-3,1.8612360216243009,-50476.587525697381,3245.867088232224]
["KBM","KBM-17H03-C (240 V)",5.05,6.14,3.8063629746453294,4.4833486156010949,3575,18.8,4700,2.1,8.8000000000000007,51.34,0.14200000000000002,325,10,1930.6834454921473,4002.8693683733295,4390.3389170237624,3.6575198449882134,17.6056338028169,0.92497539609695678,0.68493711067842777,0.73940180998202754,12.876817680754442,0,-10.430222321411096,0,0,0,0,0,0.45855736729150048,0.65234043366198247,5.502688407498006,15.656170407887579,9.9670276412174523,213.9977963949473,173.47563112534047,1668.8355714257755,1.0955224928801929E-2,4.2684542281114854,-49077.0573450101,1930.6834454921473,2.9570591699183682E-3,0.83879262006305977,-50738.427486724671,4002.8693683733295,4.4917834881154493,4.2176087356127247E-3,1.8612360216243009,-50476.587525697381,3245.867088232224]
["KBM","KBM-17H03-C (400 V)",5.05,6.14,1.429447174066097,1.6836833616797373,6480,18.8,7200,2.1,8.8000000000000007,51.34,0.14200000000000002,565,10,1930.6834454921473,4098.8232070553631,4390.3389170237624,2.7598756257241117,17.6056338028169,0.94333229401698948,0.68493711067842777,0.73940180998202754,12.876817680754442,0,-10.430222321411096,0,0,0,0,0,0.45855736729150048,0.65234043366198247,5.502688407498006,15.656170407887579,9.9670276412174523,213.9977963949473,173.47563112534047,1668.8355714257755,1.0955224928801929E-2,4.2684542281114854,-49077.0573450101,1930.6834454921473,2.8530720478032231E-3,0.68981111277069973,-50760.027576671928,4098.8232070553631,3.6939788121037975,4.2176087356127247E-3,1.8612360216243009,-50476.587525697381,3245.867088232224]
["KBM","KBM-17H03-D (120 V)",5,10.38,4.0139416156057672,8.0278832312115345,2950,19,3838,0.74,2.9,30,0.14200000000000002,160,10,3532.7056279518783,3838,3838,3.7171213290491307,17.6056338028169,0.93334045557253065,0.67772724635549697,0.62532569046378317,12.876817680754442,0,-10.430222321411096,0,0,0,0,0,0.78296803374766011,1.1138447293852594,9.3956164049719213,26.732273505246226,17.018293873777775,213.9977963949473,173.47563112534047,1668.8355714257755,3.5903972108365162E-3,1.5166820675931789,-50166.180973844806,3532.7056279518783,9.5020495308583688E-4,0.20718563115308283,-50793.236142845475,7203.0860589198619,5.3882288251556254,1.4008256247704683E-3,0.65437940217497226,-50686.212110558095,5786.2026912774973]
["KBM","KBM-17H03-D (240 V)",5,10.38,1.4103576495527956,2.8207152991055913,6500,19,8030,0.74,2.9,30,0.14200000000000002,325,10,3532.7056279518783,7379.9454814559213,7513.3333333333339,0.92440540858066811,17.6056338028169,0.95268024650596683,0.67772724635549697,0.41477980085590815,12.876817680754442,0,-10.430222321411096,0,0,0,0,0,0.78296803374766011,1.1138447293852594,9.3956164049719213,26.732273505246226,17.018293873777775,213.9977963949473,173.47563112534047,1668.8355714257755,3.5903972108365162E-3,1.5166820675931789,-50166.180973844806,3532.7056279518783,9.1660830376453888E-4,0.11916507471711768,-50801.215468046576,7379.9454814559213,3.0990985570238632,1.4008256247704683E-3,0.65437940217497226,-50686.212110558095,5786.2026912774973]
["KBM","KBM-17H04-A (120 V)",5.98,3.15,5.4908455366703892,2.8014518044236678,600,23.7,960,8.64,34,118,0.20300000000000001,160,10,717.73838207742233,960,960,5.1973528586726223,12.315270935960591,0.82509528154766287,0.55587025222356257,2.5,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.20325408580119231,0.28914780992022054,2.4390490296143077,6.9395474380852935,4.4178531103678926,218.9386993397209,177.48093525049032,1707.3665971097168,5.0969185492360604E-2,22.045202524812183,-42079.381589342403,717.73838207742233,1.5205055861972792E-2,4.0995127375332263,-50503.414727714793,1692.6664823754891,2.3215383538931147,1.856315502951035E-2,7.8013120343812368,-49712.433961186056,1439.7712393526485]
["KBM","KBM-17H04-A (240 V)",5.98,3.15,5.2862177526950962,2.6970498738240285,1400,23.7,2018,8.64,34,118,0.20300000000000001,325,10,717.73838207742233,1649.6622528645541,1910.1694915254236,5.1624954392239708,12.315270935960591,0.80440235674959093,0.55587025222356257,1.6669314780027766,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.20325408580119231,0.28914780992022054,2.4390490296143077,6.9395474380852935,4.4178531103678926,218.9386993397209,177.48093525049032,1707.3665971097168,5.0969185492360604E-2,22.045202524812183,-42079.381589342403,717.73838207742233,1.5642172707273309E-2,4.7476819120786402,-50400.454392087791,1649.6622528645541,2.688594073647717,1.856315502951035E-2,7.8013120343812368,-49712.433961186056,1439.7712393526485]
["KBM","KBM-17H04-A (400 V)",5.98,3.15,4.703912762493796,2.3999554910682632,2700,23.7,3377,8.64,34,118,0.20300000000000001,565,10,717.73838207742233,1641.9000012068673,1910.1694915254236,5.2039971715549989,12.315270935960591,0.80295776045514622,0.55587025222356257,1.6669314780027766,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.20325408580119231,0.28914780992022054,2.4390490296143077,6.9395474380852935,4.4178531103678926,218.9386993397209,177.48093525049032,1707.3665971097168,5.0969185492360604E-2,22.045202524812183,-42079.381589342403,717.73838207742233,1.5726560602960411E-2,4.8628754178799118,-50380.577313095724,1641.9000012068673,2.7538277145603627,1.856315502951035E-2,7.8013120343812368,-49712.433961186056,1439.7712393526485]
["KBM","KBM-17H04-A (480 V)",5.98,3.15,4.332815167158464,2.2106199832441145,3350,23.7,4058,8.64,34,118,0.20300000000000001,679,10,717.73838207742233,1642.3450415721663,1910.1694915254236,5.1724639275312914,12.315270935960591,0.80415874031858137,0.55587025222356257,1.6669314780027766,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.20325408580119231,0.28914780992022054,2.4390490296143077,6.9395474380852935,4.4178531103678926,218.9386993397209,177.48093525049032,1707.3665971097168,5.0969185492360604E-2,22.045202524812183,-42079.381589342403,717.73838207742233,1.572167670636326E-2,4.8562831597502631,-50381.727686590173,1642.3450415721663,2.7500945440431384,1.856315502951035E-2,7.8013120343812368,-49712.433961186056,1439.7712393526485]
["KBM","KBM-17H04-B (120 V)",6.12,5.53,5.4510568008974154,4.7816287727170312,1200,23.7,1660,2.8,12,69.3,0.20300000000000001,160,10,1433.8127756122724,1660,1660,5.1946285745747582,12.315270935960591,0.78904277656866739,0.55587025222356257,1.4457831325301205,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.34866120266593786,0.49600293523061229,4.1839344319912541,11.904070445534694,7.5783666172839501,218.9386993397209,177.48093525049032,1707.3665971097168,1.838140627174089E-2,7.1973719747136995,-48108.529536303351,1433.8127756122724,5.2551536251839847E-3,1.3141023497115232,-50715.265747980877,2984.0229867777198,3.9100048719267564,6.5029727180670304E-3,2.5469915524275994,-50467.461953354534,2596.8407914857089]
["KBM","KBM-17H04-B (240 V)",6.12,5.53,4.8647359963937822,4.267312277538406,2650,23.7,3485,2.8,12,69.3,0.20300000000000001,325,10,1433.8127756122724,2946.9787485794532,3252.5252525252527,4.7240617575531001,12.315270935960591,0.78398926688539727,0.55587025222356257,0.92419990007431607,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.34866120266593786,0.49600293523061229,4.1839344319912541,11.904070445534694,7.5783666172839501,218.9386993397209,177.48093525049032,1707.3665971097168,1.838140627174089E-2,7.1973719747136995,-48108.529536303351,1433.8127756122724,5.3479889135799501E-3,1.4425747897632775,-50696.829632624926,2946.9787485794532,4.2922641888064126,6.5029727180670304E-3,2.5469915524275994,-50467.461953354534,2596.8407914857089]
["KBM","KBM-17H04-B (400 V)",6.12,5.53,2.902986161996171,2.5464790894703255,5000,23.7,5822,2.8,12,69.3,0.20300000000000001,565,10,1433.8127756122724,2977.3389479187158,3252.5252525252527,4.2043718808235457,12.315270935960591,0.79429608559837361,0.55587025222356257,0.92419990007431607,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.34866120266593786,0.49600293523061229,4.1839344319912541,11.904070445534694,7.5783666172839501,218.9386993397209,177.48093525049032,1707.3665971097168,1.838140627174089E-2,7.1973719747136995,-48108.529536303351,1433.8127756122724,5.2715010232781178E-3,1.3376205071407059,-50712.019326041111,2977.3389479187158,3.9799812403177204,6.5029727180670304E-3,2.5469915524275994,-50467.461953354534,2596.8407914857089]
["KBM","KBM-17H04-B (480 V)",6.12,5.53,1.8009638297240791,1.5797928330912976,5700,23.7,6987,2.8,12,69.3,0.20300000000000001,679,10,1433.8127756122724,3001.0220194584813,3252.5252525252527,3.8460486579235669,12.315270935960591,0.80139291964467119,0.55587025222356257,0.92419990007431607,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.34866120266593786,0.49600293523061229,4.1839344319912541,11.904070445534694,7.5783666172839501,218.9386993397209,177.48093525049032,1707.3665971097168,1.838140627174089E-2,7.1973719747136995,-48108.529536303351,1433.8127756122724,5.2143883298596131E-3,1.2535348393665133,-50723.361308409512,3001.0220194584813,3.7297911613421508,6.5029727180670304E-3,2.5469915524275994,-50467.461953354534,2596.8407914857089]
["KBM","KBM-17H04-C (120 V)",6.1,6.2,5.4052622182153129,5.3517447705102104,1325,23.7,1868,2.23,9.1,61.4,0.20300000000000001,160,10,1690.0098129364267,1868,1868,5.1205508102839286,12.315270935960591,0.78972148173664758,0.55587025222356257,1.2847965738758029,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.39218571351366155,0.55792059331782984,4.7062285621639388,13.390094239627915,8.5243987468123859,218.9386993397209,177.48093525049032,1707.3665971097168,1.3650068039579633E-2,5.7127347815458362,-48640.989910378128,1690.0098129364267,4.0856354931225643E-3,1.0211361447223808,-50736.013442340343,3401.1873050413137,4.3057596882511451,5.0072423160346605E-3,2.0216111215281964,-50534.141771246483,2981.362528668983]
["KBM","KBM-17H04-C (240 V)",6.1,6.2,4.6473243382833438,4.601311226023113,3000,23.7,3922,2.23,9.1,61.4,0.20300000000000001,325,10,1690.0098129364267,3372.8359814927621,3671.0097719869709,4.4667877529077513,12.315270935960591,0.78728976703526976,0.55587025222356257,0.80500106140110039,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.39218571351366155,0.55792059331782984,4.7062285621639388,13.390094239627915,8.5243987468123859,218.9386993397209,177.48093525049032,1707.3665971097168,1.3650068039579633E-2,5.7127347815458362,-48640.989910378128,1690.0098129364267,4.1339028221691722E-3,1.0964271836945678,-50725.440814044159,3372.8359814927621,4.6232346127932846,5.0072423160346605E-3,2.0216111215281964,-50534.141771246483,2981.362528668983]
["KBM","KBM-17H04-C (400 V)",6.1,6.2,1.6122189040477708,1.5962563406413572,5775,23.7,6548,2.23,9.1,61.4,0.20300000000000001,565,10,1690.0098129364267,3441.0894962713696,3671.0097719869709,3.4259123132733449,12.315270935960591,0.80540064399498856,0.55587025222356257,0.80500106140110039,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.39218571351366155,0.55792059331782984,4.7062285621639388,13.390094239627915,8.5243987468123859,218.9386993397209,177.48093525049032,1707.3665971097168,1.3650068039579633E-2,5.7127347815458362,-48640.989910378128,1690.0098129364267,4.0211974785110266E-3,0.91097283844856314,-50750.128148707743,3441.0894962713696,3.8412410971408208,5.0072423160346605E-3,2.0216111215281964,-50534.141771246483,2981.362528668983]
["KBM","KBM-17H04-D (120 V)",6.07,9.56,5.5993602705966818,8.48387919787376,2200,24,2881,0.94,3.8,40,0.20300000000000001,160,10,2718.2468695416965,2881,2881,5.4536758816313817,12.315270935960591,0.77515690516275781,0.54892187407076798,0.83304408191600143,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.60771382444764532,0.86452934367653078,7.2925658933717443,20.748704248236738,13.209035375434741,218.9386993397209,177.48093525049032,1707.3665971097168,5.8421555307359733E-3,2.4616647977020558,-49858.317253711641,2718.2468695416965,1.7573229090016387E-3,0.47405813734031083,-50770.045762878355,5241.805423005444,7.2791913086425826,2.1180455026702264E-3,0.86023988663495798,-50689.533021475356,4693.196025353418]
["KBM","KBM-17H04-D (240 V)",6.07,9.56,3.9629580829881941,6.0044819439215056,5000,24,6037,0.94,3.8,40,0.20300000000000001,325,10,2718.2468695416965,5322.9776493863155,5635,3.8268525938852123,12.315270935960591,0.78750862246074782,0.54892187407076798,0.51137859723625534,13.174124977698431,0,-10.67104123193573,0,0,0,0,0,0.60771382444764532,0.86452934367653078,7.2925658933717443,20.748704248236738,13.209035375434741,218.9386993397209,177.48093525049032,1707.3665971097168,5.8421555307359733E-3,2.4616647977020558,-49858.317253711641,2718.2468695416965,1.715766938035314E-3,0.40665666528354455,-50779.320993215704,5322.9776493863155,6.2442376374789905,2.1180455026702264E-3,0.86023988663495798,-50689.533021475356,4693.196025353418]
["KBM","KBM-25H01-A (120 V)",4.9000000000000004,3.1,4.4336019861313707,2.6870315067462855,700,14.37,1132,8.98,37,100.3,0.26600000000000001,160,10,978.76347406597222,1132,1132,4.1457677832867308,9.3984962406015029,1.0302467332846137,0.93814753339388279,2.1201413427561837,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.24980530588954844,0.35537124294300421,2.9976636706745814,8.5289098306321005,5.4296726349206335,224.04159910235589,181.61756082236636,1747.1609351111642,3.3325286234856297E-2,14.182744492534097,-45806.441267351831,978.76347406597222,1.1317860262697134E-2,3.2976729377763885,-50534.917715772361,1972.4003512879824,2.1138281795199503,1.8358774389066947E-2,8.4705486863312967,-49022.119414689412,1419.5925480503179]
["KBM","KBM-25H01-A (240 V)",4.9000000000000004,3.1,4.1090912580089336,2.4903583381872325,1650,14.37,2379,8.98,37,100.3,0.26600000000000001,325,10,978.76347406597222,1910.1549559147838,2247.258225324028,3.984388937460265,9.3984962406015029,1.0116775453462266,0.93814753339388279,1.6906259498869469,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.24980530588954844,0.35537124294300421,2.9976636706745814,8.5289098306321005,5.4296726349206335,224.04159910235589,181.61756082236636,1747.1609351111642,3.3325286234856297E-2,14.182744492534097,-45806.441267351831,978.76347406597222,1.1794680503489498E-2,3.8726246114082117,-50432.468965901782,1910.1549559147838,2.4823756590661215,1.8358774389066947E-2,8.4705486863312967,-49022.119414689412,1419.5925480503179]
["KBM","KBM-25H01-A (400 V)",4.9000000000000004,3.1,3.304359770860303,2.0026422853698809,3150,14.37,3979,8.98,37,100.3,0.26600000000000001,565,10,978.76347406597222,1904.1052217300105,2247.258225324028,3.9354708278389312,9.3984962406015029,1.0143389579735067,0.93814753339388279,1.6906259498869469,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.24980530588954844,0.35537124294300421,2.9976636706745814,8.5289098306321005,5.4296726349206335,224.04159910235586,181.61756082236636,1747.1609351111642,3.3325286234856297E-2,14.182744492534097,-45806.441267351831,978.76347406597222,1.1844351656253492E-2,3.9276808411522941,-50421.796710259187,1904.1052217300105,2.5176670333434141,1.8358774389066947E-2,8.4705486863312967,-49022.119414689412,1419.5925480503179]
["KBM","KBM-25H01-A (480 V)",4.9000000000000004,3.1,2.7893997920842706,1.6905453285359218,3800,14.37,4779,8.98,37,100.3,0.26600000000000001,679,10,978.76347406597222,1910.5640769793999,2247.258225324028,3.8388323847081463,9.3984962406015029,1.019153450456471,0.93814753339388279,1.6906259498869469,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.24980530588954844,0.35537124294300421,2.9976636706745814,8.5289098306321005,5.4296726349206335,224.04159910235589,181.61756082236636,1747.1609351111642,3.3325286234856297E-2,14.182744492534097,-45806.441267351831,978.76347406597222,1.1791343041510674E-2,3.8688972301143871,-50433.18604705359,1910.5640769793999,2.479986385246864,1.8358774389066947E-2,8.4705486863312967,-49022.119414689412,1419.5925480503179]
["KBM","KBM-25H01-B (120 V)",4.96,5.34,4.2630788328186258,4.4874514029669745,1400,14.64,1989,2.87,12,57.5,0.26600000000000001,160,10,1948.7718710921272,1989,1989,3.9698741417687478,9.3984962406015029,1.0006397067767148,0.92084563216325777,1.2066365007541477,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.42510442468170689,0.60475051657431367,5.1012530961804829,14.514012397783528,9.2399072688172019,224.04159910235589,181.61756082236636,1747.1609351111642,1.0661921313160422E-2,4.5051683668662887,-49270.449828823243,1948.7718710921272,3.6549675980442104E-3,0.98092725384928858,-50732.402474302893,3593.8654381626652,3.4318352617199039,5.8341286705961663E-3,2.641058259445872,-50277.735521377152,2717.9875885002157]
["KBM","KBM-25H01-B (240 V)",4.96,5.34,3.3346749981159021,3.510184208543055,3150,14.64,4173,2.87,12,57.5,0.26600000000000001,325,10,1948.7718710921272,3581.8802706229944,3920,3.1118350610797041,9.3984962406015029,1.0023770645668606,0.92084563216325777,0.88300623967319836,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.42510442468170689,0.60475051657431367,5.1012530961804829,14.514012397783528,9.2399072688172019,224.04159910235589,181.61756082236636,1747.1609351111642,1.0661921313160422E-2,4.5051683668662887,-49270.449828823243,1948.7718710921272,3.6730711975620695E-3,1.0060674099735791,-50728.625282917892,3581.8802706229944,3.5197896680572978,5.8341286705961663E-3,2.641058259445872,-50277.735521377152,2717.9875885002157]
["KBM","KBM-25H01-B (400 V)",4.96,5.34,1.4226503076377583,1.497526639618693,4900,14.64,6970,2.87,12,57.5,0.26600000000000001,565,10,1948.7718710921272,3665.6835037666979,3920,2.3137133848272504,9.3984962406015029,1.0224916927581422,0.92084563216325777,0.88300623967319836,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.42510442468170689,0.60475051657431367,5.1012530961804829,14.514012397783528,9.2399072688172019,224.04159910235589,181.61756082236636,1747.1609351111642,1.0661921313160422E-2,4.5051683668662887,-49270.449828823243,1948.7718710921272,3.5523160341350561E-3,0.82399713865933621,-50753.820016293481,3665.6835037666979,2.8828054526068727,5.8341286705961663E-3,2.641058259445872,-50277.735521377152,2717.9875885002157]
["KBM","KBM-25H01-C (120 V)",4.8499999999999996,6.45,3.9834208613857238,5.2002883307907624,1750,15.1,2470,1.97,7.9,46.3,0.26600000000000001,160,10,2396.401103400091,2470,2470,3.6268854443558505,9.3984962406015029,1.0241763570054556,0.89279338111722484,0.97165991902834004,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.52511451231387973,0.74702415252501819,6.3013741477665564,17.928579660600438,11.413688302405498,224.04159910235589,181.61756082236636,1747.1609351111642,7.3185968558146762E-3,3.1725083064621877,-49631.388494491795,2396.401103400091,2.3128421466775771E-3,0.5735750558717041,-50766.79293844747,4562.7211854455936,3.6306335081073891,3.8154144986023157E-3,1.8031582893551616,-50425.979729476952,3406.8067365109096]
["KBM","KBM-25H01-C (240 V)",4.8499999999999996,6.45,2.3166932544737429,3.0244037264670274,4225,15.1,5178,1.97,7.9,46.3,0.26600000000000001,325,10,2396.401103400091,4608.6773773196401,4868.2505399568036,2.0866405945755968,9.3984962406015029,1.0347212566760324,0.89279338111722484,0.70447201312568919,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.52511451231387973,0.74702415252501819,6.3013741477665564,17.928579660600438,11.413688302405498,224.04159910235586,181.61756082236636,1747.1609351111642,7.3185968558146762E-3,3.1725083064621877,-49631.388494491795,2396.401103400091,2.2791481446824491E-3,0.51327966724287,-50774.435406331497,4608.6773773196401,3.2489738524107024,3.8154144986023157E-3,1.8031582893551616,-50425.979729476952,3406.8067365109096]
["KBM","KBM-25H01-D (120 V)",4.75,7.95,3.6744032513824534,5.9941325471165632,2300,15.2,3097,1.3,5.2,37.1,0.26600000000000001,160,10,2963.410697101574,3097,3097,3.3016855954484603,9.3984962406015029,1.0439352636241923,0.88691974045197997,0.77494349370358406,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.66086014878963406,0.94013492487909867,7.9303217854756092,22.563238197098368,14.36420356491228,224.04159910235589,181.61756082236636,1747.1609351111642,4.9747269056431677E-3,2.1251764578237542,-49984.842112000006,2963.410697101574,1.4527632400673303E-3,0.30957011408711066,-50787.753548518267,5807.0633765688508,3.7057928405817222,2.5235813644225438E-3,1.1999397504536018,-50543.636288911257,4243.8901580069878]
["KBM","KBM-25H01-D (240 V)",4.75,7.95,1.3252085057447611,2.1618409555379463,4900,15.2,6489,1.3,5.2,37.1,0.26600000000000001,325,10,2963.410697101574,5963.0341684775804,6075.4716981132078,0.58221455098869779,9.3984962406015029,1.0685222013839693,0.88691974045197997,0.56551887787950805,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.66086014878963406,0.94013492487909867,7.9303217854756092,22.563238197098368,14.36420356491228,224.04159910235589,181.61756082236636,1747.1609351111642,4.9747269056431677E-3,2.1251764578237542,-49984.842112000006,2963.410697101574,1.3998753711264424E-3,0.17161648606482774,-50799.810536851444,5963.0341684775804,2.054381597074558,2.5235813644225438E-3,1.1999397504536018,-50543.636288911257,4243.8901580069878]
["KBM","KBM-25H01-E (120 V)",5.09,10.44,3.6221469807121007,7.2733875114700819,2900,15.32,3815,0.75,3.4,30,0.26600000000000001,160,10,3755.3361358414709,3815,3815,3.1590140453160913,9.3984962406015029,0.97465814847635313,0.87997258843799575,0.62909567496723462,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.80987643247897478,1.152124425121511,9.718517189747697,27.650986202916265,17.603164542239682,224.04159910235589,181.61756082236636,1747.1609351111642,3.2469255087942362E-3,1.2245728517823724,-50388.610369632668,3755.3361358414709,9.309629411255588E-4,0.14065529240653682,-50799.664469088348,7311.7774655863432,3.6092164859493145,1.636542546600757E-3,0.68601544562596639,-50674.433002322949,5358.9125211939381]
["KBM","KBM-25H01-E (240 V)",5.09,10.44,1.4421386680163577,2.8958607791493125,4900,15.32,6918,0.75,3.4,30,0.26600000000000001,325,10,3755.3361358414709,6918,6918,-6.0184631563844349E-2,9.3984962406015029,0.99672076143219179,0.87997258843799575,0.44785205776512516,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,0.80987643247897478,1.152124425121511,9.718517189747697,27.650986202916265,17.603164542239682,224.04159910235589,181.61756082236636,1747.1609351111642,3.2469255087942362E-3,1.2245728517823724,-50388.610369632668,3755.3361358414709,9.0155430545945487E-4,3.1513973149440364E-2,-50804.884130415652,7489.3763243575331,0.80864892804729038,1.636542546600757E-3,0.68601544562596639,-50674.433002322949,5358.9125211939381]
["KBM","KBM-25H01-F (120 V)",4.63,12,2.4658943081579734,6.2905467044846262,3950,15.73,4765,0.56000000000000005,2.1,23.7,0.26600000000000001,160,10,4715.1301877093192,4765,4765,2.0193762983222134,9.3984962406015029,1.0811482617436459,0.857036239979027,0.50367261280167885,13.481180054870094,0,-10.919755844444776,0,0,0,0,0,1.0233785261830595,1.4558509778477424,12.280542314196714,34.94042346834582,22.243764434845211,224.04159910235589,181.61756082236636,1747.1609351111642,2.0688350544394588E-3,0.93718640071617698,-50414.233354658558,4715.1301877093192,5.6190467015331403E-4,1.1184956125688809E-2,-50805.104318376892,9498.7789250804944,0.48656098779690993,1.0103461981141441E-3,0.51133472578723849,-50688.786554774029,6834.5282206340762]
["KBM","KBM-25H02-A (120 V)",8.6999999999999993,3.33,8.0801740338962258,3.0262824096989611,390,29.4,707,8.9600000000000009,45,162,0.51500000000000001,160,10,581.71421286150496,707,707,7.576366774268287,4.8543689320388346,0.64702686594758818,0.49982240453113036,3.3946251768033946,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.1647389017475335,0.23435638433144987,1.9768668209704019,5.6245532239547966,3.5807017931034486,244.21020292610376,197.96708093978114,1904.4433186406945,7.8970404630503171E-2,28.291499266412547,-43180.475017323763,581.71421286150496,2.8916815563840716E-2,6.3698085516207019,-50418.648216503774,1214.8904510479595,2.5336272886109676,3.1582507326035673E-2,9.0022652522890869,-50033.166595102011,1124.1754718609359]
["KBM","KBM-25H02-A (240 V)",8.6999999999999993,3.33,8.0691556147590937,3.0221556609584623,1000,29.4,1484,8.9600000000000009,45,162,0.51500000000000001,325,10,581.71421286150496,1173.6080179004432,1391.3580246913582,7.9596359714337961,4.8543689320388346,0.61374967151408177,0.49982240453113036,2.1348980297774078,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.1647389017475335,0.23435638433144987,1.9768668209704019,5.6245532239547966,3.5807017931034486,244.21020292610376,197.96708093978114,1904.4433186406945,7.8970404630503171E-2,28.291499266412547,-43180.475017323763,581.71421286150496,3.0029421309786475E-2,7.5805199510997108,-50257.755995951258,1173.6080179004432,3.0151945783487282,3.1582507326035673E-2,9.0022652522890869,-50033.166595102011,1124.1754718609359]
["KBM","KBM-25H02-A (400 V)",8.6999999999999993,3.33,7.5170103891095179,2.8153596962956997,1950,29.4,2482,8.9600000000000009,45,162,0.51500000000000001,565,10,581.71421286150496,1169.708056229324,1391.3580246913582,7.9903833444645178,4.8543689320388346,0.61295425855901975,0.49982240453113036,2.1348980297774078,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.1647389017475335,0.23435638433144987,1.9768668209704019,5.6245532239547966,3.5807017931034486,244.21020292610376,197.96708093978114,1904.4433186406945,7.8970404630503171E-2,28.291499266412547,-43180.475017323763,581.71421286150496,3.0143049709801986E-2,7.6934523775886161,-50241.324366272063,1169.708056229324,3.0601140881271722,3.1582507326035673E-2,9.0022652522890869,-50033.166595102011,1124.1754718609359]
["KBM","KBM-25H02-A (480 V)",8.6999999999999993,3.33,7.4404935895461071,2.7867017189311265,2400,29.4,2982,8.9600000000000009,45,162,0.51500000000000001,679,10,581.71421286150496,1166.3697843933189,1391.3580246913582,8.0878957414987038,4.8543689320388346,0.61027677934546865,0.49982240453113036,2.1348980297774078,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.1647389017475335,0.23435638433144987,1.9768668209704019,5.6245532239547966,3.5807017931034486,244.21020292610376,197.96708093978114,1904.4433186406945,7.8970404630503171E-2,28.291499266412547,-43180.475017323763,581.71421286150496,3.0241499888577342E-2,7.7899758973116144,-50227.087636024466,1166.3697843933189,3.09850686266366,3.1582507326035673E-2,9.0022652522890869,-50033.166595102011,1124.1754718609359]
["KBM","KBM-25H02-B (120 V)",8.75,5.18,8.0214091318315255,4.6636099603671664,750,29.7,1098,3.7,19,104,0.51500000000000001,160,10,1026.8212303512842,1098,1098,7.6833429690013535,4.8543689320388346,0.62141519249440202,0.49477369337425026,2.1857923497267762,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.2547961680361851,0.36247120776597574,3.0575540164342212,8.6993089863834179,5.5381521066666659,244.21020292610376,197.96708093978114,1904.4433186406945,3.3762794270852589E-2,11.718549173790825,-47631.056941139206,1026.8212303512842,1.2011136929172746E-2,2.6743710896230617,-50639.843322739194,1944.9951469729433,4.0126010096331273,1.3092645803287185E-2,3.6911404469188835,-50490.244185491858,1827.8577025609848]
["KBM","KBM-25H02-B (240 V)",8.75,5.18,7.6956096012669404,4.4741916286435703,1700,29.7,2303,3.7,19,104,0.51500000000000001,325,10,1026.8212303512842,1910.3659300948009,2167.3076923076924,7.5651344148478179,4.8543689320388346,0.60977923726713612,0.49477369337425026,1.3130124936078968,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.2547961680361851,0.36247120776597574,3.0575540164342212,8.6993089863834179,5.5381521066666659,244.21020292610376,197.96708093978114,1904.4433186406945,3.3762794270852589E-2,11.718549173790825,-47631.056941139206,1026.8212303512842,1.2303154017878317E-2,2.9832579741942697,-50599.450214945602,1910.3659300948009,4.4760519606630957,1.3092645803287185E-2,3.6911404469188835,-50490.244185491858,1827.8577025609848]
["KBM","KBM-25H02-B (400 V)",8.75,5.18,6.7906109052542005,3.9480295960780238,3150,29.7,3845,3.7,19,104,0.51500000000000001,565,10,1026.8212303512842,1907.2668117974642,2167.3076923076924,7.5636260978391938,4.8543689320388346,0.60983771532295561,0.49477369337425026,1.3130124936078968,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.2547961680361851,0.36247120776597574,3.0575540164342212,8.6993089863834179,5.5381521066666659,244.21020292610376,197.96708093978114,1904.4433186406945,3.3762794270852589E-2,11.718549173790825,-47631.056941139206,1026.8212303512842,1.2330407400556912E-2,3.0104692629413785,-50595.680405345905,1907.2668117974642,4.5168795201307148,1.3092645803287185E-2,3.6911404469188835,-50490.244185491858,1827.8577025609848]
["KBM","KBM-25H02-B (480 V)",8.75,5.18,6.0876765732649973,3.5393468449215102,4000,29.7,4614,3.7,19,104,0.51500000000000001,679,10,1026.8212303512842,1909.7206798095008,2167.3076923076924,7.4789264739057177,4.8543689320388346,0.61125714655291274,0.49477369337425026,1.3130124936078968,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.2547961680361851,0.36247120776597574,3.0575540164342212,8.6993089863834179,5.5381521066666659,244.21020292610376,197.96708093978114,1904.4433186406945,3.3762794270852589E-2,11.718549173790825,-47631.056941139206,1026.8212303512842,1.230881309948121E-2,2.9889286948512406,-50598.667425506079,1909.7206798095008,4.484560256135552,1.3092645803287185E-2,3.6911404469188835,-50490.244185491858,1827.8577025609848]
["KBM","KBM-25H02-C (120 V)",8.75,6.5,7.9912534584035866,5.7907633756547732,950,29.7,1380,2.35,12,83.4,0.51500000000000001,160,10,1345.9216352439469,1380,1380,7.6478208132599468,4.8543689320388346,0.61563627399381649,0.49477369337425026,1.7391304347826086,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.31972492128092722,0.45483838812332861,3.8366990553711267,10.916121314959886,6.9494186666666646,244.21020292610376,197.96708093978114,1904.4433186406945,2.1368232093066306E-2,7.4895598082909327,-48789.020892510205,1345.9216352439469,7.6626121263954254E-3,1.6588600818008201,-50706.252910887401,2466.4553170981203,4.8866948047126284,8.3855004547550589E-3,2.3590818904297715,-50605.130549971764,2319.9501523188601]
["KBM","KBM-25H02-C (240 V)",8.75,6.5,7.4617759365874656,5.4070840120199026,2150,29.7,2895,2.35,12,83.4,0.51500000000000001,325,10,1345.9216352439469,2431.3962399760298,2702.6378896882493,7.2931706306847079,4.8543689320388346,0.60909549997996559,0.49477369337425026,1.0345049860666737,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.31972492128092722,0.45483838812332861,3.8366990553711267,10.916121314959886,6.9494186666666646,244.21020292610376,197.96708093978114,1904.4433186406945,2.1368232093066306E-2,7.4895598082909327,-48789.020892510205,1345.9216352439469,7.8194349541300737E-3,1.833620609427385,-50684.315505116887,2431.3962399760298,5.401506977113864,8.3855004547550589E-3,2.3590818904297715,-50605.130549971764,2319.9501523188601]
["KBM","KBM-25H02-C (400 V)",8.75,6.5,6.0399300903374282,4.3767609350271224,4000,29.7,4826,2.35,12,83.4,0.51500000000000001,565,10,1345.9216352439469,2434.7558292964336,2702.6378896882493,7.1004103724120489,4.8543689320388346,0.61164732991086468,0.49477369337425026,1.0345049860666737,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.31972492128092722,0.45483838812332861,3.8366990553711267,10.916121314959886,6.9494186666666646,244.21020292610376,197.96708093978114,1904.4433186406945,2.1368232093066306E-2,7.4895598082909327,-48789.020892510205,1345.9216352439469,7.8039684783064826E-3,1.8171322664970337,-50686.479057202276,2434.7558292964336,5.3529353702495897,8.3855004547550589E-3,2.3590818904297715,-50605.130549971764,2319.9501523188601]
["KBM","KBM-25H02-C (480 V)",8.75,6.5,4.8414933688554562,3.5083285281561278,5000,29.7,5791,2.35,12,83.4,0.51500000000000001,679,10,1345.9216352439469,2444.7860879886798,2702.6378896882493,6.838907472673263,4.8543689320388346,0.61507414972572561,0.49477369337425026,1.0345049860666737,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.31972492128092722,0.45483838812332861,3.8366990553711267,10.916121314959886,6.9494186666666646,244.21020292610376,197.96708093978114,1904.4433186406945,2.1368232093066306E-2,7.4895598082909327,-48789.020892510205,1345.9216352439469,7.7583444641780505E-3,1.7675980746597328,-50692.861243554049,2444.7860879886798,5.2070168081221535,8.3855004547550589E-3,2.3590818904297715,-50605.130549971764,2319.9501523188601]
["KBM","KBM-25H02-D (120 V)",8.6199999999999992,8,7.7953441514397719,7.0228325688646587,1225,29.8,1717,1.57,7.8,67,0.51500000000000001,160,10,1703.7578404445048,1717,1717,7.4641354351200722,4.8543689320388346,0.6210651209482172,0.49311337896695406,1.3977868375072802,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.39944216472719812,0.56824356895650552,4.7933059767263773,13.637845654956132,8.682122196442382,244.21020292610376,197.96708093978114,1904.4433186406945,1.4057540157768531E-2,5.0388806019076311,-49391.130276215139,1703.7578404445048,4.9130191420154309E-3,1.0607278148044978,-50742.498856254184,3107.6089221654997,5.8219554084447234,5.4319735289296176E-3,1.5818342565695029,-50665.808272707909,2911.9326247549416]
["KBM","KBM-25H02-D (240 V)",8.6199999999999992,8,6.9736147541916713,6.2825358145870904,2725,29.8,3597,1.57,7.8,67,0.51500000000000001,325,10,1703.7578404445048,3078.2826401525831,3364.1791044776119,6.7601691298439919,4.8543689320388346,0.61874651677427228,0.49311337896695406,0.82419489365828846,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.39944216472719812,0.56824356895650552,4.7933059767263773,13.637845654956132,8.682122196442382,244.21020292610376,197.96708093978114,1904.4433186406945,1.4057540157768531E-2,5.0388806019076311,-49391.130276215139,1703.7578404445048,4.982222443488428E-3,1.1440174290987903,-50732.272058471724,3078.2826401525831,6.2791022972507866,5.4319735289296176E-3,1.5818342565695029,-50665.808272707909,2911.9326247549416]
["KBM","KBM-25H02-D (400 V)",8.6199999999999992,8,4.4612543893712751,4.0191480985326802,5180,29.8,5995,1.57,7.8,67,0.51500000000000001,565,10,1703.7578404445048,3102.5644320937645,3364.1791044776119,6.129116561068968,4.8543689320388346,0.62546869192517229,0.49311337896695406,0.82419489365828846,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.39944216472719812,0.56824356895650552,4.7933059767263773,13.637845654956132,8.682122196442382,244.21020292610376,197.96708093978114,1904.4433186406945,1.4057540157768531E-2,5.0388806019076311,-49391.130276215139,1703.7578404445048,4.9247055037463716E-3,1.07524578484956,-50740.771856881453,3102.5644320937645,5.9016393509640075,5.4319735289296176E-3,1.5818342565695029,-50665.808272707909,2911.9326247549416]
["KBM","KBM-25H02-D (480 V)",8.6199999999999992,8,2.8488734813449264,2.5665526858963297,6000,29.8,7193,1.57,7.8,67,0.51500000000000001,679,10,1703.7578404445048,3125.9967982662224,3364.1791044776119,5.6132461633824908,4.8543689320388346,0.63095505670175822,0.49311337896695406,0.82419489365828846,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.39944216472719812,0.56824356895650552,4.7933059767263773,13.637845654956132,8.682122196442382,244.21020292610376,197.96708093978114,1904.4433186406945,1.4057540157768531E-2,5.0388806019076311,-49391.130276215139,1703.7578404445048,4.8711956404670813E-3,1.0070570873779454,-50748.679493359428,3125.9967982662224,5.5273759909399871,5.4319735289296176E-3,1.5818342565695029,-50665.808272707909,2911.9326247549416]
["KBM","KBM-25H02-E (120 V)",8.85,10.199999999999999,7.8184865793893579,8.7848163813363573,1600,29.8,2143,0.96,5,54,0.51500000000000001,160,10,2143,2143,2143,7.4684167122696214,4.8543689320388346,0.60344183116943151,0.49311337896695406,1.1199253383107792,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.49605300694172544,0.70568146266852805,5.952636083300705,16.936355104044672,10.782018531073444,244.21020292610376,197.96708093978114,1904.4433186406945,8.9797996966562328E-3,3.0838893371993312,-49989.798765081301,2193.9590100931805,3.1793946909175301E-3,0.64273192224882958,-50769.742962630517,3896.2444152571793,7.1582069507547725,3.5135835921047921E-3,0.96811220238171958,-50724.806670404636,3664.3050242767113]
["KBM","KBM-25H02-E (240 V)",8.85,10.199999999999999,6.5120897548433847,7.3169547807229041,3600,29.8,4480,0.96,5,54,0.51500000000000001,325,10,2193.9590100931805,3879.3669635672777,4174.0740740740739,6.3306633975427644,4.8543689320388346,0.60359225504212466,0.49311337896695406,0.65496730869825182,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.49605300694172544,0.70568146266852805,5.952636083300705,16.936355104044672,10.782018531073444,244.21020292610382,197.96708093978114,1904.4433186406945,8.9797996966562328E-3,3.0838893371993312,-49989.798765081301,2193.9590100931805,3.2009891996706264E-3,0.66856026721302897,-50766.839284045273,3879.3669635672777,7.4458613087370837,3.5135835921047921E-3,0.96811220238171958,-50724.806670404636,3664.3050242767113]
["KBM","KBM-25H02-E (400 V)",8.85,10.199999999999999,2.9443664472000637,3.3082769069663636,6000,29.8,7430,0.96,5,54,0.51500000000000001,565,10,2193.9590100931805,3947.2929641423702,4174.0740740740739,4.9647890380382833,4.8543689320388346,0.61445017176933114,0.49311337896695406,0.65496730869825182,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.49605300694172544,0.70568146266852805,5.952636083300705,16.936355104044672,10.782018531073444,244.21020292610376,197.96708093978114,1904.4433186406945,8.9797996966562328E-3,3.0838893371993312,-49989.798765081301,2193.9590100931805,3.1167880741574056E-3,0.56117112841912087,-50778.161282975721,3947.2929641423702,6.2498515056756467,3.5135835921047921E-3,0.96811220238171958,-50724.806670404636,3664.3050242767113]
["KBM","KBM-25H02-F (120 V)",8.93,12.74,7.639437268410977,10.669605123479018,2100,30.1,2666,0.61,3.2,43.3,0.51500000000000001,160,10,2666,2666,2666,7.2915998845636496,4.8543689320388346,0.5969132166902138,0.48819862768156913,0.90022505626406601,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.61402938409494989,0.87351381369709813,7.3683526091393983,20.964331528730355,13.346307965658827,244.21020292610376,197.96708093978114,1904.4433186406945,5.7575324103834452E-3,1.9645488096689794,-50290.536205327808,2789.7722807815071,2.0257842417751499E-3,0.38728926563488436,-50785.159763282645,4912.2558665801844,8.4655874671015408,2.2499327276343612E-3,0.61057567842090266,-50755.450062473115,4615.8452003046141]
["KBM","KBM-25H02-F (240 V)",8.93,12.74,5.6022539968347154,7.8243770905512786,4500,30.1,5564,0.61,3.2,43.3,0.51500000000000001,325,10,2789.7722807815071,4936.6631312290956,5205.5427251732108,5.2793419991286576,4.8543689320388346,0.60083105270877957,0.48819862768156913,0.51994811261036578,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.61402938409494989,0.87351381369709813,7.3683526091393983,20.964331528730355,13.346307965658827,244.21020292610376,197.96708093978114,1904.4433186406945,5.7575324103834452E-3,1.9645488096689794,-50290.536205327808,2789.7722807815071,2.0097789259148173E-3,0.36617380645813402,-50787.2811835713,4936.6631312290956,8.0040338367013835,2.2499327276343612E-3,0.61057567842090266,-50755.450062473115,4615.8452003046141]
["KBM","KBM-25H02-G (120 V)",8.74,14.37,7.341021750113673,11.615540743850747,2400,30,3027,0.49,2.5,38.200000000000003,0.51500000000000001,160,10,3027,3027,3027,6.9755386823308703,4.8543689320388346,0.60928625703574935,0.48982595644050775,0.79286422200198214,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.70764675742933614,1.0066932199728396,8.4917610891520336,24.160637279348151,15.38113940503432,244.21020292610376,197.96708093978114,1904.4433186406945,4.5858355526250377E-3,1.5991406403466366,-50367.046532097491,3144.3145775381881,1.5566861906332354E-3,0.28231453653690303,-50791.505375411165,5622.1311825367593,8.7078947358545484,1.7632693717417856E-3,0.49866464561891921,-50762.55795564982,5225.9869347995018]
["KBM","KBM-25H02-G (240 V)",8.74,14.37,4.3692536263907114,6.9133759911245436,5300,30,6316,0.49,2.5,38.200000000000003,0.51500000000000001,325,10,3144.3145775381881,5683.4234107970797,5900.5235602094235,4.0530561769004771,4.8543689320388346,0.61723542589274738,0.48982595644050775,0.45924339841314155,14.694778693215232,0,-11.902770741504339,0,0,0,0,0,0.70764675742933614,1.0066932199728396,8.4917610891520336,24.160637279348151,15.38113940503432,244.21020292610376,197.96708093978114,1904.4433186406945,4.5858355526250377E-3,1.5991406403466366,-50367.046532097491,3144.3145775381881,1.5301658502634352E-3,0.24085356728883048,-50795.221531880343,5683.4234107970797,7.429045405998929,1.7632693717417856E-3,0.49866464561891921,-50762.55795564982,5225.9869347995018]
["KBM","KBM-25H03-A (120 V)",11.86,5.3,11.285532328334398,4.9281800560412217,550,42.2,827,3.97,21,139,0.76600000000000001,160,10,791.78158730213499,827,827,10.996209519150085,3.2637075718015667,0.4912701748997147,0.37720675620350808,2.9020556227327692,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.20834890867967507,0.29639566853736865,2.5001869041561009,7.1134960448968476,4.5285922328399213,264.54080356771311,214.44792250392209,2062.9890144877304,5.1569116979886337E-2,18.024763117748442,-46601.287459099629,791.78158730213499,2.1117847012875276E-2,4.2547391222380551,-50570.92257701073,1450.0195048170485,4.4515064015290449,2.1180617104793045E-2,4.3284175745785864,-50562.73985223435,1446.2585348468199]
["KBM","KBM-25H03-A (240 V)",11.86,5.3,11.018419137131216,4.8115367411053347,1300,42.2,1735,3.97,21,139,0.76600000000000001,325,10,791.78158730213499,1431.4818089158748,1621.5827338129495,10.933301772362778,3.2637075718015667,0.48365451857497566,0.37720675620350808,1.6594543383311444,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.20834890867967507,0.29639566853736865,2.5001869041561009,7.1134960448968476,4.5285922328399213,264.54080356771311,214.44792250392209,2062.9890144877304,5.1569116979886337E-2,18.024763117748442,-46601.287459099629,791.78158730213499,2.1434999510670783E-2,4.6149800382654345,-50529.578498607887,1431.4818089158748,4.8284072402683762,2.1180617104793045E-2,4.3284175745785864,-50562.73985223435,1446.2585348468199]
["KBM","KBM-25H03-A (400 V)",11.86,5.3,9.9869726790164322,4.3611234406185293,2400,42.2,2899,3.97,21,139,0.76600000000000001,565,10,791.78158730213499,1432.4448031198535,1621.5827338129495,10.742079894981494,3.2637075718015667,0.48617978436526765,0.37720675620350808,1.6594543383311444,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.20834890867967507,0.29639566853736865,2.5001869041561009,7.1134960448968476,4.5285922328399213,264.54080356771311,214.44792250392209,2062.9890144877304,5.1569116979886337E-2,18.024763117748442,-46601.287459099629,791.78158730213499,2.1418045276212057E-2,4.5964367597112137,-50531.788656823868,1432.4448031198535,4.8090063978623139,2.1180617104793045E-2,4.3284175745785864,-50562.73985223435,1446.2585348468199]
["KBM","KBM-25H03-A (480 V)",11.86,5.3,9.3846535409358971,4.09810198294144,2900,42.2,3479,3.97,21,139,0.76600000000000001,679,10,791.78158730213499,1433.8914909344182,1621.5827338129495,10.636076474218394,3.2637075718015667,0.48757914162038063,0.37720675620350808,1.6594543383311444,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.20834890867967507,0.29639566853736865,2.5001869041561009,7.1134960448968476,4.5285922328399213,264.54080356771311,214.44792250392209,2062.9890144877304,5.1569116979886337E-2,18.024763117748442,-46601.287459099629,791.78158730213499,2.1392673773830726E-2,4.568546711172667,-50535.096092177344,1433.8914909344182,4.7798265290051614,2.1180617104793045E-2,4.3284175745785864,-50562.73985223435,1446.2585348468199]
["KBM","KBM-25H03-B (120 V)",11.84,7.27,10.742958658702936,6.4716618425921304,800,42.3,1144,2.1,11.4,100,0.76600000000000001,160,10,1144,1144,1144,10.271230881945197,3.2637075718015667,0.49860703432703252,0.3763150144630743,2.0979020979020979,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.28627456135199963,0.40725214513900293,3.4352947362239958,9.7740514833360699,6.2223544304304292,264.54080356771311,214.44792250392209,2062.9890144877304,2.8026622426156465E-2,9.4471975711842582,-48573.921451275259,1158.6907443358164,1.0799958326423387E-2,1.9901210727103322,-50706.145452898862,2076.6245511472016,5.4714139859488435,1.1034612452380131E-2,2.2632611434034291,-50677.10122491901,2042.925080227478]
["KBM","KBM-25H03-B (240 V)",11.84,7.27,10.02022080068974,6.0362775907769519,1825,42.3,2399,2.1,11.4,100,0.76600000000000001,325,10,1158.6907443358164,2050.7214018415239,2254,9.7951451229306414,3.2637075718015667,0.49121064521651409,0.3763150144630743,1.1747861060733378,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.28627456135199963,0.40725214513900293,3.4352947362239958,9.7740514833360699,6.2223544304304292,264.54080356771311,214.44792250392209,2062.9890144877304,2.8026622426156465E-2,9.4471975711842582,-48573.921451275259,1158.6907443358164,1.0978608625712438E-2,2.2011535345842632,-50684.033077929686,2050.7214018415239,6.0516027891424784,1.1034612452380131E-2,2.2632611434034291,-50677.10122491901,2042.925080227478]
["KBM","KBM-25H03-B (400 V)",11.84,7.27,5.2661562052465376,3.1723832561726133,3400,42.3,4000,2.1,11.4,100,0.76600000000000001,565,10,1158.6907443358164,2092.7768978472609,2254,7.7936504636127593,3.2637075718015667,0.51014861626554031,0.3763150144630743,1.1747861060733378,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.28627456135199963,0.40725214513900293,3.4352947362239958,9.7740514833360699,6.2223544304304292,264.54080356771317,214.44792250392209,2062.9890144877304,2.8026622426156465E-2,9.4471975711842582,-48573.921451275259,1158.6907443358164,1.0694456332482996E-2,1.8542500012063008,-50719.203923325666,2092.7768978472609,5.0978654159110555,1.1034612452380131E-2,2.2632611434034291,-50677.10122491901,2042.925080227478]
["KBM","KBM-25H03-B (480 V)",11.84,7.27,6.6499920800324466,4.006019325320751,4150,42.3,4800,2.1,11.4,100,0.76600000000000001,679,10,{"$f":"IF(AQ800<I800,IF(AQ800<0,0,AQ800),I800)","v":1158.6907443358164},{"$f":"IF(AU800<I800,IF(AU800<0,0,AU800),I800)","v":2059.7175745004361},{"$f":"IF(UAC_V*0.98/L800*1000<I800,IF(UAC_V*0.98/L800*1000<0,0,UAC_V*0.98/L800*1000),I800)","v":2254},{"$f":"C800+(E800-C800)/G800*Q800","v":9.2641083073364765},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M800,(inertia/gear^2+gear_inertia)/M800),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M800,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M800))","v":3.2637075718015667},{"$f":"IF((C800+(E800-C800)/G800*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X800^2*time1+Y800^2*time2+Z800^2*time3+AA800^2*time4)/time)/(C800+(E800-C800)/G800*mspeed),SQRT((((X800-Y800)*2/PI()+Y800)^2*time1+Y800^2*time2+((Z800-Y800)*2/PI()+Y800)^2*time3+AA800^2*time4)/time)/(C800+(E800-C800)/G800*mspeed)),IF(AccType=1,SQRT((X800^2*time1+Y800^2*time2+Z800^2*time3+AA800^2*time4+AB800^2*time5+AC800^2*time6+AD800^2*time7+AE800^2*time8)/time)/(C800+(E800-C800)/G800*mspeed),SQRT((((X800-Y800)*2/PI()+Y800)^2*time1+Y800^2*time2+((Z800-Y800)*2/PI()+Y800)^2*time3+AA800^2*time4+((AB800-AC800)*2/PI()+AC800)^2*time5+AC800^2*time6+((AD800-AC800)*2/PI()+AC800)^2*time7+AE800^2*time8)/time)/(C800+(E800-C800)/G800*mspeed))))","v":0.49619688666599759},{"$f":"IF(move1,MAX(ABS(X800),ABS(Z800))/H800,MAX(ABS(X800),ABS(Z800),ABS(AB800),ABS(AD800))/H800)","v":0.3763150144630743},{"$f":"IF(AZ800>0,speed/(MIN(AZ800,I800)),\"NA\")","v":1.1747861060733378},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M800+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M800+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":15.918125111788042},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M800+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M800+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-12.893681340548314},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M800+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M800+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M800+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M800+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH800/Irms","v":0.28627456135199963},{"$f":"AI800/Ipeak","v":0.40725214513900293},{"$f":"IF(move1,IF(AccType=1,SQRT((X800^2*time1+Y800^2*time2+Z800^2*time3+AA800^2*time4)/time)/(C800/D800),SQRT((((X800-Y800)*2/PI()+Y800)^2*time1+Y800^2*time2+((Z800-AA800)*2/PI()+AA800)^2*time3+AA800^2*time4)/time)/(C800/D800)),IF(AccType=1,SQRT((X800^2*time1+Y800^2*time2+Z800^2*time3+AA800^2*time4+AB800^2*time5+AC800^2*time6+AD800^2*time7+AE800^2*time8)/time)/(C800/D800),SQRT((((X800-Y800)*2/PI()+Y800)^2*time1+Y800^2*time2+((Z800-AA800)*2/PI()+AA800)^2*time3+AA800^2*time4+((AB800-AC800)*2/PI()+AC800)^2*time5+AC800^2*time6+((AD800-AE800)*2/PI()+AE800)^2*time7+AE800^2*time8)/time)/(C800/D800)))","v":3.4352947362239958},{"$f":"IF(move1,MAX(ABS(X800),ABS(Z800))/(C800/D800),MAX(ABS(X800),ABS(Z800),ABS(AB800),ABS(AD800))/(C800/D800))","v":9.7740514833360699},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X800),ABS(Z800))/(C800/D800),MAX(ABS((X800-Y800)*2/PI()+Y800),ABS((Z800-Y800)*2/PI()+Y800))/(C800/D800)),IF(AccType=1,MAX(ABS(X800),ABS(Z800),ABS(AB800),ABS(AD800))/(C800/D800),MAX(ABS((X800-Y800)*2/PI()+Y800),ABS((Z800-Y800)*2/PI()+Y800),ABS((AB800-AC800)*2/PI()+AC800),ABS((AD800-AC800)*2/PI()+AC800))/(C800/D800)))","v":6.2223544304304292},{"$f":"IF((C800+(E800-C800)/G800*mspeed)<0,\"NA\",U800*(C800+(E800-C800)/G800*mspeed)*mspeed/9.55)","v":264.54080356771311},{"$f":"IF(move1,IF(speed1>speed2,AM800/2*time1/time,AM800/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z800*-speed/30*PI(),((Z800-AA800)*2/PI()+AA800)*-speed/30*PI()),IF(AccType=1,X800*-speed/30*PI(),((X800-Y800)*2/PI()+Y800)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z800*-speed/30*PI(),((Z800-AA800)*2/PI()+AA800)*-speed/30*PI()),IF(AccType=1,X800*-speed/30*PI(),((X800-Y800)*2/PI()+Y800)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD800*-speed/30*PI(),((AD800-AE800)*2/PI()+AE800)*-speed/30*PI()),IF(AccType=1,AB800*-speed/30*PI(),((AB800-AC800)*2/PI()+AC800)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD800*-speed/30*PI(),((AD800-AE800)*2/PI()+AE800)*-speed/30*PI()),IF(AccType=1,AB800*-speed/30*PI(),((AB800-AC800)*2/PI()+AC800)*-speed/30*PI()),0)/2*time7/time)))","v":214.44792250392209},{"$f":"IF(move1,MAX(IF(AccType=1,Z800*-speed/30*PI(),((Z800-AA800)*2/PI()+AA800)*-speed/30*PI()),IF(AccType=1,X800*-speed/30*PI(),((X800-Y800)*2/PI()+Y800)*-speed/30*PI()),0),MAX(IF(AccType=1,Z800*-speed/30*PI(),((Z800-AA800)*2/PI()+AA800)*-speed/30*PI()),IF(AccType=1,X800*-speed/30*PI(),((X800-Y800)*2/PI()+Y800)*-speed/30*PI()),IF(AccType=1,AD800*-speed/30*PI(),((AD800-AE800)*2/PI()+AE800)*-speed/30*PI()),IF(AccType=1,AB800*-speed/30*PI(),((AB800-AC800)*2/PI()+AC800)*-speed/30*PI()),0))","v":2062.9890144877304},{"$f":"(L800^2)/1000000+((K800/1000)^2*(D800/C800*H800)^2*PI()*PI()*(O800/2)^2)/1200","v":2.8026622426156465E-2},{"$f":"SQRT(3)*L800*J800*D800/C800*H800/1000","v":9.4471975711842582},{"$f":"0.75*J800^2*(D800/C800*H800)^2-(UAC_V*0.98)^2","v":-48573.921451275259},{"$f":"-AO800/2/AN800+SQRT((AO800/2/AN800)^2-AP800/AN800)","v":1158.6907443358164},{"$f":"(L800^2)/1000000+((K800/1000)^2*AV800^2*PI()*PI()*(O800/2)^2)/1200","v":1.0915262901799987E-2},{"$f":"SQRT(3)*L800*J800*AV800/1000","v":2.1287210097461227},{"$f":"0.75*J800^2*AV800^2-(UAC_V*0.98)^2","v":-50691.873671566638},{"$f":"-AS800/2/AR800+SQRT((AS800/2/AR800)^2-AT800/AR800)","v":2059.7175745004361},{"$f":"D800+(F800-D800)*((0.85*UAC_V-D800*J800)/L800*1000)/G800","v":5.8524649905073129},{"$f":"(L800^2)/1000000+((K800/1000)^2*AJ800^2*PI()*PI()*(O800/2)^2)/1200","v":1.1034612452380131E-2},{"$f":"SQRT(3)*L800*J800*AJ800/1000","v":2.2632611434034291},{"$f":"0.75*J800^2*AJ800^2-(UAC_V*0.98)^2","v":-50677.10122491901},{"$f":"IF(((AX800/2/AW800)^2-AY800/AW800)>0,-AX800/2/AW800+SQRT((AX800/2/AW800)^2-AY800/AW800),-9999)","v":2042.925080227478}]
["KBM","KBM-25H03-C (120 V)",11.9,8.1999999999999993,10.769484482551585,7.2278419345983789,900,42.4,1276,1.66,9.1,90,0.76600000000000001,160,10,1276,1276,1276,10.297180221928691,3.2637075718015667,0.49367905113040861,0.37542747905160478,1.8808777429467085,15.918125111788042,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-12.893681340548314,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.3212676084813027,0.45703300390988066,3.8552113017756322,10.968792093837136,6.982949925925924,264.54080356771311,214.44792250392209,2062.9890144877304,2.26347239484481E-2,7.5603860555854405,-49040.979836126833,1314.381917230548,8.7164526676229773E-3,1.5570065754286657,-50730.336868026912,2324.8199472118049,6.0169890592620989,8.9302696219849837E-3,1.8069667143269064,-50704.384422633171,2283.7917264292219]
["KBM","KBM-25H03-C (240 V)",11.9,8.1999999999999993,9.8753701274580923,6.6277651862134848,2050,42.4,2676,1.66,9.1,90,0.76600000000000001,325,10,1314.381917230548,2298.1989790974385,2504.4444444444448,9.6302427774995181,3.2637075718015667,0.48845326104038911,0.37542747905160478,1.0508839191533781,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.3212676084813027,0.45703300390988066,3.8552113017756322,10.968792093837136,6.982949925925924,264.54080356771311,214.44792250392209,2062.9890144877304,2.26347239484481E-2,7.5603860555854405,-49040.979836126833,1314.381917230548,8.8529873249236519E-3,1.7208159047477467,-50713.764710554547,2298.1989790974385,6.65002359994579,8.9302696219849837E-3,1.8069667143269064,-50704.384422633171,2283.7917264292219]
["KBM","KBM-25H03-C (400 V)",11.9,8.1999999999999993,7.4635291734146705,5.0090799821574974,3800,42.4,4459,1.66,9.1,90,0.76600000000000001,565,10,1314.381917230548,2304.4770429283676,2504.4444444444448,9.2095407443454391,3.2637075718015667,0.4919416422784606,0.37542747905160478,1.0508839191533781,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.3212676084813027,0.45703300390988066,3.8552113017756322,10.968792093837136,6.982949925925924,264.54080356771311,214.44792250392209,2062.9890144877304,2.26347239484481E-2,7.5603860555854405,-49040.979836126833,1314.381917230548,8.8200497905037527E-3,1.6827586927252216,-50717.762567347461,2304.4770429283676,6.5029530403352709,8.9302696219849837E-3,1.8069667143269064,-50704.384422633171,2283.7917264292219]
["KBM","KBM-25H03-C (480 V)",11.9,8.1999999999999993,5.2243241637149138,3.5062578279965866,4725,42.4,5351,1.66,9.1,90,0.76600000000000001,679,10,1314.381917230548,2317.5506761641268,2504.4444444444448,8.6256683495798896,3.2637075718015667,0.49678109901144768,0.37542747905160478,1.0508839191533781,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.3212676084813027,0.45703300390988066,3.8552113017756322,10.968792093837136,6.982949925925924,264.54080356771311,214.44792250392209,2062.9890144877304,2.26347239484481E-2,7.5603860555854405,-49040.979836126833,1314.381917230548,8.7529172608524358E-3,1.6023952669788157,-50725.910907665559,2317.5506761641268,6.1923918255582429,8.9302696219849837E-3,1.8069667143269064,-50704.384422633171,2283.7917264292219]
["KBM","KBM-25H03-D (120 V)",11.9,10.24,10.663381187156988,8.9608245270226785,1200,42.6,1595,1.06,5.7,72.099999999999994,0.76600000000000001,160,10,1595,1595,1595,10.256327494596164,3.2637075718015667,0.48928060131988643,0.37366490872741881,1.5047021943573669,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.40119272083518781,0.57073389756550963,4.8143126500222539,13.697613541572231,8.720171614814813,264.54080356771311,214.44792250392209,2062.9890144877304,1.4175455120792279E-2,4.8524866773580868,-49672.764375475497,1708.5850188516158,5.5751965705338191E-3,0.99413497992413591,-50757.63083443261,2929.4744884367778,7.5100633065975337,5.7064036498080152E-3,1.1543215122585277,-50741.079918125797,2882.5101565417508]
["KBM","KBM-25H03-D (240 V)",11.9,10.24,9.1956189341983965,7.7274108690742835,2700,42.6,3338,1.06,5.7,72.099999999999994,0.76600000000000001,325,10,1708.5850188516158,2916.3415100805651,3126.2135922330099,8.9789263847136525,3.2637075718015667,0.48872296924954867,0.37366490872741881,0.83260764738444659,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.40119272083518781,0.57073389756550963,4.8143126500222539,13.697613541572231,8.720171614814813,264.54080356771311,214.44792250392209,2062.9890144877304,1.4175455120792279E-2,4.8524866773580868,-49672.764375475497,1708.5850188516158,5.6107913887345736E-3,1.0400331353022236,-50753.140780540278,2916.3415100805651,7.8567949471759517,5.7064036498080152E-3,1.1543215122585277,-50741.079918125797,2882.5101565417508]
["KBM","KBM-25H03-D (400 V)",11.9,10.199999999999999,5.0010749128257421,4.2025839603577664,4850,42.6,5560,1.06,5.7,72.099999999999994,0.76600000000000001,565,10,1713.2094133886899,2947.1065760160368,3126.2135922330099,7.7078623728137599,3.2637075718015667,0.49697273884261062,0.37366490872741881,0.83221394635396673,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.39962556176942532,0.56850446827814427,4.7955067412331038,13.644107238675463,8.686108444444443,264.54080356771311,214.44792250392209,2062.9890144877304,1.4105458934623991E-2,4.833531651274658,-49681.593937306126,1713.2094133886899,5.5287942898455747E-3,0.93090924127814811,-50763.484179148189,2947.1065760160368,7.0324326936258483,5.7024427007868386E-3,1.149812443851268,-50741.579565980988,2883.8738049448702]
["KBM","KBM-25H03-E (120 V)",11.8,12.7,10.269407475568853,10.80990260586195,1525,42.6,2006,0.69,3.6,57.4,0.76600000000000001,160,10,2006,2006,2006,9.7866435383548325,3.2637075718015667,0.49306988496118676,0.37366490872741881,1.1964107676969093,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.5017897237472021,0.71384247499896925,6.0214766849664256,17.132219399975263,10.906709614563713,264.54080356771311,214.44792250392209,2062.9890144877304,8.8965411141455411E-3,3.1452337211898,-50054.536649520043,2201.7908468163914,3.4949718923644015E-3,0.59461353539980621,-50778.332153929223,3727.5703621189446,8.6678857932351985,3.6117539768943997E-3,0.74819596360581775,-50762.683673958345,3646.8333640348692]
["KBM","KBM-25H03-E (240 V)",11.8,12.7,8.0747728480446916,8.4997608926786228,3400,42.6,4193,0.69,3.6,57.4,0.76600000000000001,325,10,2201.7908468163914,3727.124053205117,3926.8292682926831,7.7163577289101699,3.2637075718015667,0.49488153154602693,0.37366490872741881,0.65810519988898852,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.5017897237472021,0.71384247499896925,6.0214766849664256,17.132219399975263,10.906709614563713,264.54080356771311,214.44792250392209,2062.9890144877304,8.8965411141455411E-3,3.1452337211898,-50054.536649520043,2201.7908468163914,3.495580071916359E-3,0.59551597325013028,-50778.250659532408,3727.124053205117,8.6810409398243902,3.6117539768943997E-3,0.74819596360581775,-50762.683673958345,3646.8333640348692]
["KBM","KBM-25H03-F (120 V)",11.75,14.79,9.936430230872384,12.20691674554347,1850,42,2347,0.51,2.7,49.4,0.76600000000000001,160,10,2347,2347,2347,9.4492171631662085,3.2637075718015667,0.4947902333527765,0.37900297885209622,1.0225820195994888,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.58685438879416463,0.83485485958633021,7.0422526655299755,20.036516630071926,12.755642656075647,264.54080356771311,214.44792250392209,2062.9890144877304,6.6296963679867288E-3,2.3069455819869047,-50259.953768311963,2584.8736149074102,2.5750000181385267E-3,0.41357265407110899,-50787.637755311167,4361.5189499111866,9.4775058806629673,2.6842481641902922E-3,0.55662165279361808,-50773.420045202482,4246.7276743167849]
["KBM","KBM-25H03-F (240 V)",11.75,14.79,6.7427350280639562,8.2834582654348363,4100,42,4902,0.51,2.7,49.4,0.76600000000000001,325,10,2584.8736149074102,4384.3016697625744,4562.7530364372469,6.395521907950525,3.2637075718015667,0.49959806652067767,0.37900297885209622,0.56514101775695158,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.58685438879416463,0.83485485958633021,7.0422526655299755,20.036516630071926,12.755642656075647,264.54080356771311,214.44792250392209,2062.9890144877304,6.6296963679867288E-3,2.3069455819869047,-50259.953768311963,2584.8736149074102,2.5551736962221463E-3,0.38191048656308346,-50790.217981225433,4384.3016697625744,8.7519299128180208,2.6842481641902922E-3,0.55662165279361808,-50773.420045202482,4246.7276743167849]
["KBM","KBM-25H03-G (120 V)",11.2,20,8.5422798546777301,14.856138877700401,2750,42,3324,0.28000000000000003,1.3,34.6,0.76600000000000001,160,10,3324,3324,3324,7.9875411770722824,3.2637075718015667,0.51978532179042236,0.37900297885209622,0.72202166064981954,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.83255325368630295,1.184384308912801,9.9906390442356354,28.425223413907222,18.09605925925926,264.54080356771306,214.44792250392209,2062.9890144877304,3.1518043091219939E-3,1.2585081167795462,-50474.41,3807.1340214223151,1.2300844970407074E-3,0.16333592857155038,-50799.588767758214,6360.2749079463929,9.733901974517142,1.3109523934300509E-3,0.30365383279335262,-50785.904919189983,6109.3857723281053]
["KBM","KBM-25H03-G (240 V)",11.2,20,3.5388569699256727,6.1545338607403011,5100,42,6937,0.28000000000000003,1.3,34.6,0.76600000000000001,325,10,3807.1340214223151,6454.5227315317043,6514.4508670520236,1.5041133652685446,3.2637075718015667,0.53173645134983627,0.37900297885209622,0.39283818201014198,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.83255325368630295,1.184384308912801,9.9906390442356354,28.425223413907222,18.09605925925926,264.54080356771311,214.44792250392209,2062.9890144877304,3.1518043091219939E-3,1.2585081167795462,-50474.41,3807.1340214223151,1.20619827488676E-3,8.5578550053849192E-2,-50803.630612067456,6454.5227315317043,5.0999998875358887,1.3109523934300509E-3,0.30365383279335262,-50785.904919189983,6109.3857723281053]
["KBM","KBM-25H03-H (120 V)",11,21.1,7.9793274858614645,15.198719020688504,2950,42.6,3642,0.25,1.1000000000000001,31.8,0.76600000000000001,160,10,3642,3642,3642,7.2707493910194758,3.2637075718015667,0.53093168633052046,0.37366490872741881,0.65897858319604607,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.89431356777794135,1.2722440903739687,10.731762813335296,30.533858168975247,19.438457837037035,264.54080356771311,214.44792250392209,2062.9890144877304,2.6725191589977554E-3,1.1251932683351202,-50492.163112241738,4141.2019506846173,1.0319950899700691E-3,0.12576741280193604,-50801.249592450142,6955.472674499948,9.1335659920101335,1.1052485798805456E-3,0.26766375292654188,-50787.448110480524,6658.721898423405]
["KBM","KBM-25H03-H (240 V)",11,21.1,3.0300652627110845,5.7715528813544461,5200,42.6,7600,0.25,1.1000000000000001,31.8,0.76600000000000001,325,10,4141.2019506846173,7054.0622647121563,7088.0503144654094,0.18838156105224435,3.2637075718015667,0.54276385528856286,0.37366490872741881,0.36042952936182115,15.918125111788042,0,-12.893681340548314,0,0,0,0,0,0.89431356777794135,1.2722440903739687,10.731762813335296,30.533858168975247,19.438457837037035,264.54080356771311,214.44792250392209,2062.9890144877304,2.6725191589977554E-3,1.1251932683351202,-50492.163112241738,4141.2019506846173,1.0142299173182736E-3,4.7734832855473287E-2,-50804.596678170434,7054.0622647121563,3.4666312702929929,1.1052485798805456E-3,0.26766375292654188,-50787.448110480524,6658.721898423405]
["KBM","KBM-25H04-A (120 V)",14.82,5.5,13.687325105903,4.9772091294192728,450,54.4,685,4.08,23,167,1.02,160,10,647.57675380541991,685,685,13.095817105652344,2.4509803921568629,0.44067026195014236,0.31536936030702872,3.5036496350364965,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.18648376052878302,0.26529046503560216,2.2378051263453962,6.3669711608544519,4.053339731094117,285.11439943611452,231.12574623815235,2223.4296788110255,7.222341182475106E-2,23.825973101413155,-45716.44227769674,647.57675380541991,2.9896520441232553E-2,5.070025686498421,-50574.736172848134,1218.6062843318057,4.2960853218536172,2.9676064351058965E-2,4.7835494440052004,-50600.04019216141,1227.6756465550629]
["KBM","KBM-25H04-A (240 V)",14.82,5.5,13.187123856185615,4.7953177658856783,1050,54.4,1437,4.08,23,167,1.02,325,10,647.57675380541991,1199.2007043675303,1349.7005988023952,12.955098836374145,2.4509803921568629,0.42711187072601603,0.31536936030702872,1.9549137483785353,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.18648376052878302,0.26529046503560216,2.2378051263453962,6.3669711608544519,4.053339731094117,285.11439943611452,231.12574623815235,2223.4296788110255,7.222341182475106E-2,23.825973101413155,-45716.44227769674,647.57675380541991,3.0399812633529828E-2,5.6700556863265401,-50516.96813684568,1199.2007043675303,4.8045206305342205,2.9676064351058965E-2,4.7835494440052004,-50600.04019216141,1227.6756465550629]
["KBM","KBM-25H04-A (400 V)",14.82,5.5,12.032113697747288,4.3753140719081047,2000,54.4,2400,4.08,23,167,1.02,565,10,647.57675380541991,1194.8306415356294,1349.7005988023952,13.1544740104755,2.4509803921568629,0.42492128565011422,0.31536936030702872,1.9549137483785353,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.18648376052878302,0.26529046503560216,2.2378051263453962,6.3669711608544519,4.053339731094117,285.11439943611452,231.12574623815235,2223.4296788110255,7.222341182475106E-2,23.825973101413155,-45716.44227769674,647.57675380541991,3.051901935684034E-2,5.8030945155752462,-50503.285551680776,1194.8306415356294,4.9172510577377739,2.9676064351058965E-2,4.7835494440052004,-50600.04019216141,1227.6756465550629]
["KBM","KBM-25H04-A (480 V)",14.82,5.5,11.399472798957003,4.1452628359843651,2400,54.4,2888,4.08,23,167,1.02,679,10,647.57675380541991,1194.9164591233737,1349.7005988023952,13.116981561914383,2.4509803921568629,0.42534461146908642,0.31536936030702872,1.9549137483785353,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.18648376052878302,0.26529046503560216,2.2378051263453962,6.3669711608544519,4.053339731094117,285.11439943611452,231.12574623815235,2223.4296788110255,7.222341182475106E-2,23.825973101413155,-45716.44227769674,647.57675380541991,3.0516657774918007E-2,5.8004885345820281,-50503.556614796005,1194.9164591233737,4.9150428802281789,2.9676064351058965E-2,4.7835494440052004,-50600.04019216141,1227.6756465550629]
["KBM","KBM-25H04-B (120 V)",14.9,6.2,13.641852265019601,5.5681029653141225,525,53.8,772,3.2,18,148,1.02,160,10,770.32950541441437,772,772,13.049923711609775,2.4509803921568629,0.43638244845496049,0.31888649071937475,3.1088082901554404,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.20908936976725687,0.29744904318891119,2.5090724372070823,7.1387770365338685,4.5446866119811089,285.11439943611452,231.12574623815235,2223.4296788110255,5.5291116436579142E-2,18.363692750852262,-46956.260125003384,770.32950541441437,2.3420710303521747E-2,3.9140095457257518,-50630.312132897736,1389.1114050823323,4.7714410152777189,2.3279977714588267E-2,3.7280030759409373,-50646.535925239397,1397.0741792170347]
["KBM","KBM-25H04-B (240 V)",14.9,6.2,13.130282805081366,5.359299104114843,1200,53.8,1618,3.2,18,148,1.02,325,10,770.32950541441437,1367.6352468903926,1522.9729729729731,12.883060322667735,2.4509803921568629,0.42362257178557311,0.31888649071937475,1.7178758549134714,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.20908936976725687,0.29744904318891119,2.5090724372070823,7.1387770365338685,4.5446866119811089,285.11439943611452,231.12574623815235,2223.4296788110255,5.5291116436579142E-2,18.363692750852262,-46956.260125003384,770.32950541441437,2.382402370824881E-2,4.4037621827829589,-50583.817763850107,1367.6352468903926,5.3684824359730481,2.3279977714588267E-2,3.7280030759409373,-50646.535925239397,1397.0741792170347]
["KBM","KBM-25H04-B (400 V)",14.9,6.2,11.735024470642415,4.7898059063846592,2250,53.8,2704,3.2,18,148,1.02,565,10,770.32950541441437,1364.4261758448074,1522.9729729729731,12.980722018593882,2.4509803921568629,0.42270923834809965,0.31888649071937475,1.7178758549134714,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.20908936976725687,0.29744904318891119,2.5090724372070823,7.1387770365338685,4.5446866119811089,285.11439943611452,231.12574623815235,2223.4296788110255,5.5291116436579142E-2,18.363692750852262,-46956.260125003384,770.32950541441437,2.3887216267693523E-2,4.4756446729645498,-50576.53286296298,1364.4261758448074,5.4561120285751628,2.3279977714588267E-2,3.7280030759409373,-50646.535925239397,1397.0741792170347]
["KBM","KBM-25H04-B (480 V)",14.9,6.2,10.92863942564348,4.4606691533238694,2700,53.8,3245,3.2,18,148,1.02,679,10,770.32950541441437,1365.1855923931507,1522.9729729729731,12.891983615440848,2.4509803921568629,0.42357030017482916,0.31888649071937475,1.7178758549134714,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.20908936976725687,0.29744904318891119,2.5090724372070823,7.1387770365338685,4.5446866119811089,285.11439943611452,231.12574623815235,2223.4296788110255,5.5291116436579142E-2,18.363692750852262,-46956.260125003384,770.32950541441437,2.3872193799884693E-2,4.458661392572469,-50578.264667941745,1365.1855923931507,5.4354082669491266,2.3279977714588267E-2,3.7280030759409373,-50646.535925239397,1397.0741792170347]
["KBM","KBM-25H04-C (120 V)",15.1,8.6300000000000008,13.687325105903,7.646550338493296,750,54.4,1060,1.66,9.6,108,1.02,160,10,1060,1060,1060,13.103419483009572,2.4509803921568629,0.42316469756365205,0.31536936030702872,2.2641509433962264,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.28718409303847747,0.40854603841628423,3.4462091164617297,9.8051049219908215,6.2421236634780479,285.11439943611452,231.12574623815235,2223.4296788110255,2.9981511393068736E-2,9.6543984552800897,-48807.401736683074,1125.0110631954858,1.2447544081822864E-2,1.9967500371695546,-50719.704523513879,1939.9688334331927,6.4302999300771857,1.240235583383999E-2,1.938317153569715,-50724.632878347424,1945.7209023739163]
["KBM","KBM-25H04-C (240 V)",15.1,8.6300000000000008,12.638774892591691,7.0607680964199391,1700,54.4,2223,1.66,9.6,108,1.02,325,10,1125.0110631954858,1919.5700264649813,2087.037037037037,12.320885914962327,2.4509803921568629,0.41740043684475514,0.31536936030702872,1.2334759816126923,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.28718409303847747,0.40854603841628423,3.4462091164617297,9.8051049219908215,6.2421236634780479,285.11439943611452,231.12574623815235,2223.4296788110255,2.9981511393068736E-2,9.6543984552800897,-48807.401736683074,1125.0110631954858,1.2614280177802318E-2,2.1989624786961777,-50701.519825473391,1919.5700264649813,7.0815014447407698,1.240235583383999E-2,1.938317153569715,-50724.632878347424,1945.7209023739163]
["KBM","KBM-25H04-C (400 V)",15.1,8.6300000000000008,10.064655448858906,5.6227125412619587,3150,54.4,3707,1.66,9.6,108,1.02,565,10,1125.0110631954858,1921.258846956657,2087.037037037037,12.02882531226831,2.4509803921568629,0.41937649611876626,0.31536936030702872,1.2334759816126923,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.28718409303847747,0.40854603841628423,3.4462091164617297,9.8051049219908215,6.2421236634780479,285.11439943611452,231.12574623815235,2223.4296788110255,2.9981511393068736E-2,9.6543984552800897,-48807.401736683074,1125.0110631954858,1.2600098815107329E-2,2.1824928600596185,-50703.066483963237,1921.258846956657,7.0284629644124124,1.240235583383999E-2,1.938317153569715,-50724.632878347424,1945.7209023739163]
["KBM","KBM-25H04-C (480 V)",15.1,8.6300000000000008,8.0858978879934362,4.517261389940467,3850,54.4,4450,1.66,9.6,108,1.02,679,10,1125.0110631954858,1927.2849865605897,2087.037037037037,11.588786053331642,2.4509803921568629,0.42233862930909039,0.31536936030702872,1.2334759816126923,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.28718409303847747,0.40854603841628423,3.4462091164617297,9.8051049219908215,6.2421236634780479,285.11439943611452,231.12574623815235,2223.4296788110255,2.9981511393068736E-2,9.6543984552800897,-48807.401736683074,1125.0110631954858,1.2550046596966877E-2,2.1233435379431831,-50708.52531678402,1927.2849865605897,6.8379794913741039,1.240235583383999E-2,1.938317153569715,-50724.632878347424,1945.7209023739163]
["KBM","KBM-25H04-D (120 V)",15,10.7,13.369015219719209,9.284038347027229,1000,54.8,1325,1.08,6.2,87,1.02,160,10,1325,1325,1325,12.838945166127953,2.4509803921568629,0.42274770046808213,0.31306739417340079,1.8113207547169812,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.35844213141928777,0.50991721457643124,4.301305577031453,12.23801314983435,7.7909611456790113,285.11439943611452,231.12574623815235,2223.4296788110255,1.9646805771190295E-2,6.361751671399408,-49468.395423155205,1433.1197625691348,8.0383818158506898E-3,1.2541394302947932,-50753.209091339013,2435.9405210396212,7.7062339046618007,8.0487599206238436E-3,1.267928237524677,-50752.060448688324,2433.5600029741117]
["KBM","KBM-25H04-D (240 V)",15,10.7,11.777465788800255,8.1787956866668434,2250,54.8,2776,1.08,6.2,87,1.02,325,10,1433.1197625691348,2418.1238912614599,2590.8045977011493,11.536672459329107,2.4509803921568629,0.42010439836281666,0.31306739417340079,0.98620950256698114,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.35844213141928777,0.50991721457643124,4.301305577031453,12.23801314983435,7.7909611456790113,285.11439943611452,231.12574623815235,2223.4296788110255,1.9646805771190295E-2,6.361751671399408,-49468.395423155205,1433.1197625691348,8.1175559032050041E-3,1.3557922231803186,-50744.446149014526,2418.1238912614599,8.3308536081136442,8.0487599206238436E-3,1.267928237524677,-50752.060448688324,2433.5600029741117]
["KBM","KBM-25H04-D (400 V)",15,10.7,6.9376214952587638,4.8177927050408087,4150,54.8,4626,1.08,6.2,87,1.02,565,10,1433.1197625691348,2436.0257092389556,2590.8045977011493,10.267431008393933,2.4509803921568629,0.4269616893052286,0.31306739417340079,0.98620950256698114,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.35844213141928777,0.50991721457643124,4.301305577031453,12.23801314983435,7.7909611456790113,285.11439943611452,231.12574623815235,2223.4296788110255,1.9646805771190295E-2,6.361751671399408,-49468.395423155205,1433.1197625691348,8.0380115943754077E-3,1.2536447360760499,-50753.250067238369,2436.0257092389556,7.7031941873314675,8.0487599206238436E-3,1.267928237524677,-50752.060448688324,2433.5600029741117]
["KBM","KBM-25H04-D (480 V)",15,10.7,4.0432128096111288,2.8077866733410617,4700,54.8,5551,1.08,6.2,87,1.02,679,10,1433.1197625691348,2451.2819590031968,2590.8045977011493,9.2854947301196678,2.4509803921568629,0.43233191409304161,0.31306739417340079,0.98620950256698114,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.35844213141928777,0.50991721457643124,4.301305577031453,12.23801314983435,7.7909611456790113,285.11439943611452,231.12574623815235,2223.4296788110255,1.9646805771190295E-2,6.361751671399408,-49468.395423155205,1433.1197625691348,7.9730315337716625E-3,1.1635641261365453,-50760.442022868549,2451.2819590031968,7.1496813691392713,8.0487599206238436E-3,1.267928237524677,-50752.060448688324,2433.5600029741117]
["KBM","KBM-25H04-E (120 V)",14.6,13.8,12.584608714480584,11.65241547637091,1400,53.8,1837,0.65,3.5,65.5,1.02,160,10,1837,1837,1837,11.955518720357738,2.4509803921568629,0.43225009359016608,0.31888649071937475,1.3064779531845401,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.47495532712708094,0.67566805413725062,5.6994639255249711,16.216033299294015,10.323447427701677,285.11439943611452,231.12574623815235,2223.4296788110255,1.0803707883045573E-2,3.7499354350619143,-49985.742963281104,1984.4227703684824,4.5143070710715301E-3,0.69550028593055269,-50776.972793675814,3277.6570230599114,9.4315273588600412,4.5586880637963918E-3,0.76127231195598877,-50771.389501022626,3254.8039954117648]
["KBM","KBM-25H04-E (240 V)",14.6,13.8,9.9719703688069501,9.233305897043472,3050,53.8,3681,0.65,3.5,65.5,1.02,325,10,1984.4227703684824,3275.0328010383901,3441.2213740458014,9.6305085749721826,2.4509803921568629,0.43334171613244021,0.31888649071937475,0.7373715908494749,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.47495532712708094,0.67566805413725062,5.6994639255249711,16.216033299294015,10.323447427701677,285.11439943611452,231.12574623815235,2223.4296788110255,1.0803707883045573E-2,3.7499354350619143,-49985.742963281104,1984.4227703684824,4.5193019473945221E-3,0.70320990590349208,-50776.344419802997,3275.0328010383901,9.5360758301865545,4.5586880637963918E-3,0.76127231195598877,-50771.389501022626,3254.8039954117648]
["KBM","KBM-25H04-E (400 V)",14.6,13.8,4.5670548887239537,4.2287545265962532,4600,53.8,6135,0.65,3.5,65.5,1.02,565,10,1984.4227703684824,3314.9203571141989,3441.2213740458014,7.3699100019177513,2.4509803921568629,0.44288039114206296,0.31888649071937475,0.7373715908494749,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.47495532712708094,0.67566805413725062,5.6994639255249711,16.216033299294015,10.323447427701677,285.11439943611452,231.12574623815235,2223.4296788110255,1.0803707883045573E-2,3.7499354350619143,-49985.742963281104,1984.4227703684824,4.4464392321527909E-3,0.58068890814814378,-50785.510818247989,3314.9203571141989,7.8745953595950837,4.5586880637963918E-3,0.76127231195598877,-50771.389501022626,3254.8039954117648]
["KBM","KBM-25H04-F (120 V)",14.5,19.399999999999999,11.793381283109445,15.316079588453825,2000,54.1,2495,0.33,1.8,46.3,1.02,160,10,2495,2495,2495,11.123493150679034,2.4509803921568629,0.43415010216378597,0.31711817376529317,0.96192384769539074,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.67229558648412979,0.95640289682076374,8.0675470378095575,22.953669523698331,14.612759867177521,285.11439943611452,231.12574623815235,2223.4296788110255,5.6340120734180987E-3,1.9155193835389135,-50377.251287836247,2825.0880469878553,2.2251854052974408E-3,0.29269840855893781,-50795.168774779362,4712.4847143967081,11.060246414875177,2.2859451550428524E-3,0.38671213979684615,-50787.719712567319,4629.7060768088859]
["KBM","KBM-25H04-F (240 V)",14.5,19.399999999999999,4.8481044203377346,6.2962395069321229,4550,54.1,5206,0.33,1.8,46.3,1.02,325,10,2825.0880469878553,4778.4046915046265,4868.2505399568036,4.3635905231272663,2.4509803921568629,0.4452679788320843,0.31711817376529317,0.51839144001431858,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.67229558648412979,0.95640289682076374,8.0675470378095575,22.953669523698331,14.612759867177521,285.11439943611452,231.12574623815235,2223.4296788110255,5.6340120734180987E-3,1.9155193835389135,-50377.251287836247,2825.0880469878553,2.1825528031785891E-3,0.20212538525957535,-50800.395473486569,4778.4046915046265,7.6377476006068896,2.2859451550428524E-3,0.38671213979684615,-50787.719712567319,4629.7060768088859]
["KBM","KBM-25H04-G (120 V)",14,20.3,11.77006323330761,16.577553849729028,2150,54.5,2701,0.3,1.5,42.8,1.02,160,10,2701,2701,2701,11.198577113099468,2.4509803921568629,0.44561208857361456,0.31479070093031858,0.88855979266938168,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.72860900545509433,1.036513964209101,8.7433080654611324,24.876335141018426,15.836766814814816,285.11439943611452,231.12574623815235,2223.4296788110255,4.7209896331133934E-3,1.7574790454747957,-50383.625832812504,3086.0062051339046,1.9057306180701196E-3,0.28106048262791328,-50794.37917376859,5089.4879119619345,12.637877360108403,1.9478710093840501E-3,0.35220228820129912,-50788.230785137595,5016.6358977261025]
["KBM","KBM-25H04-G (240 V)",14,20.3,4.8473059841683774,6.8271915269977148,4600,54.5,5637,0.3,1.5,42.8,1.02,325,10,3086.0062051339046,5186.9532161828001,5266.3551401869163,3.6794357256184984,2.4509803921568629,0.46024165104719211,0.31479070093031858,0.47840824985681168,17.156093200702362,0,-13.89643549256891,0,0,0,0,0,0.72860900545509433,1.036513964209101,8.7433080654611324,24.876335141018426,15.836766814814816,285.11439943611452,231.12574623815235,2223.4296788110255,4.7209896331133934E-3,1.7574790454747957,-50383.625832812504,3086.0062051339046,1.8567538516687829E-3,0.16320203706215161,-50801.525006646159,5186.9532161828001,7.3383753917545587,1.9478710093840501E-3,0.35220228820129912,-50788.230785137595,5016.6358977261025]
["KBM","KBM-35H01-A (120 V)",12.6,5.41,11.650141834326739,4.9156716600534764,500,40.799999999999997,798,4.13,32,144,1.52,160,10,642.90657620786806,798,798,11.084026367585476,1.6447368421052631,0.58646617704015613,0.48022152592206641,3.007518796992481,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.24639769574498813,0.35052360110359082,2.9567723489398574,8.4125664264861797,5.3556061234567895,325.61360390147161,263.95610791970807,2539.2577581875917,8.5350833684642746E-2,18.045131622824574,-46879.297064946673,642.90657620786806,2.4487653409443935E-2,4.348157769761964,-50577.217340003604,1351.112976328604,4.221162999144191,2.677514870443029E-2,5.516730906201599,-50438.233882481676,1273.3464318964598]
["KBM","KBM-35H01-A (240 V)",12.6,5.41,11.459155902616464,4.8350868787411239,1200,40.799999999999997,1675,4.13,32,144,1.52,325,10,642.90657620786806,1309.3803900508406,1565.2777777777778,11.355167592317288,1.6447368421052631,0.56581645345926235,0.48022152592206641,1.8847973653372223,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.24639769574498813,0.35052360110359082,2.9567723489398574,8.4125664264861797,5.3556061234567895,325.61360390147172,263.95610791970807,2539.2577581875917,8.5350833684642746E-2,18.045131622824574,-46879.297064946673,642.90657620786806,2.565587207203163E-2,4.9793292463145047,-50506.238803250351,1309.3803900508406,4.8339001223154696,2.677514870443029E-2,5.516730906201599,-50438.233882481676,1273.3464318964598]
["KBM","KBM-35H01-A (400 V)",12.6,5.41,10.926171907145932,4.6101991169392118,2150,40.799999999999997,2795,4.13,32,144,1.52,565,10,642.90657620786806,1300.5127929625137,1565.2777777777778,11.587518675359645,1.6447368421052631,0.56222484769980285,0.48022152592206641,1.8847973653372223,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.24639769574498813,0.35052360110359082,2.9567723489398574,8.4125664264861797,5.3556061234567895,325.61360390147166,263.95610791970807,2539.2577581875917,8.5350833684642746E-2,18.045131622824574,-46879.297064946673,642.90657620786806,2.5921500309439922E-2,5.1119814714994858,-50490.099783890895,1300.5127929625137,4.9626780311114604,2.677514870443029E-2,5.516730906201599,-50438.233882481676,1273.3464318964598]
["KBM","KBM-35H01-A (480 V)",12.6,5.41,10.504226244065093,4.4321629721793636,2700,40.799999999999997,3353,4.13,32,144,1.52,679,10,642.90657620786806,1299.6969975432003,1565.2777777777778,11.591158941437616,1.6447368421052631,0.56217692618349158,0.48022152592206641,1.8847973653372223,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.24639769574498813,0.35052360110359082,2.9567723489398574,8.4125664264861797,5.3556061234567895,325.61360390147172,263.95610791970807,2539.2577581875917,8.5350833684642746E-2,18.045131622824574,-46879.297064946673,642.90657620786806,2.5946253418542519E-2,5.1241680281994304,-50488.595836453256,1299.6969975432003,4.9745086603003354,2.677514870443029E-2,5.516730906201599,-50438.233882481676,1273.3464318964598]
["KBM","KBM-35H01-B (120 V)",12.45,6.1,11.632779476898532,5.5394187985231103,550,41.4,901,3.3,25,127,1.52,160,10,729.33195535190441,901,901,11.111244197610141,1.6447368421052631,0.58462982752096049,0.47326179366232629,2.6637069922308547,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.28117092243220249,0.39999174488448425,3.3740510691864301,9.5998018772276215,6.1114236858545281,325.61360390147166,263.95610791970807,2539.2577581875917,6.9005192470452642E-2,14.724451059951607,-47444.606664131228,729.33195535190441,1.8958825621982006E-2,3.4063468108231816,-50625.310062068245,1546.7302512791196,4.692567998525381,2.0928801879272031E-2,4.4362976921041266,-50500.107963094917,1450.992628781381]
["KBM","KBM-35H01-B (240 V)",12.45,6.1,11.275515583664278,5.3692931350782276,1300,41.4,1892,3.3,25,127,1.52,325,10,729.33195535190441,1504.6012149846356,1774.8031496062993,11.090668707846733,1.6447368421052631,0.57186186838127961,0.47326179366232629,1.6540401049560429,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.28117092243220249,0.39999174488448425,3.3740510691864301,9.5998018772276215,6.1114236858545281,325.61360390147161,263.95610791970807,2539.2577581875917,6.9005192470452642E-2,14.724451059951607,-47444.606664131228,729.33195535190441,1.9771406974349939E-2,3.864588524526952,-50573.666347822167,1504.6012149846356,5.3238397159216762,2.0928801879272031E-2,4.4362976921041266,-50500.107963094917,1450.992628781381]
["KBM","KBM-35H01-B (400 V)",12.45,6.1,10.646449810232319,5.0697380048725327,2350,41.4,3153,3.3,25,127,1.52,565,10,729.33195535190441,1493.0469623910094,1774.8031496062993,11.304133986233037,1.6447368421052631,0.56896067667339056,0.47326179366232629,1.6540401049560429,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.28117092243220249,0.39999174488448425,3.3740510691864301,9.5998018772276215,6.1114236858545281,325.61360390147166,263.95610791970807,2539.2577581875917,6.9005192470452642E-2,14.724451059951607,-47444.606664131228,729.33195535190441,2.0008833753408655E-2,3.9885549897093417,-50558.576657791324,1493.0469623910094,5.4946153590701829,2.0928801879272031E-2,4.4362976921041266,-50500.107963094917,1450.992628781381]
["KBM","KBM-35H01-B (480 V)",12.45,6.1,10.207868763825012,4.8608898875357198,2900,41.4,3783,3.3,25,127,1.52,679,10,729.33195535190441,1492.0046699373825,1774.8031496062993,11.296458525867049,1.6447368421052631,0.56908128282694193,0.47326179366232629,1.6540401049560429,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.28117092243220249,0.39999174488448425,3.3740510691864301,9.5998018772276215,6.1114236858545281,325.61360390147166,263.95610791970807,2539.2577581875917,6.9005192470452642E-2,14.724451059951607,-47444.606664131228,729.33195535190441,2.0030568767837341E-2,3.9997114248096541,-50557.195286103408,1492.0046699373825,5.5099844137310319,2.0928801879272031E-2,4.4362976921041266,-50500.107963094917,1450.992628781381]
["KBM","KBM-35H01-C (120 V)",12.45,8.32,11.482589759268032,7.5049606269725704,815,40.799999999999997,1242,1.75,13.4,93,1.52,160,10,1064.657569359247,1242,1242,10.975738013510302,1.6447368421052631,0.57800781256670108,0.48022152592206641,1.932367149758454,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.38349870075998771,0.54556251105555875,4.6019844091198525,13.093500265333411,8.3355811584114221,325.61360390147166,263.95610791970807,2539.2577581875917,3.6096094692917982E-2,7.6859182800421619,-49097.640639163888,1064.657569359247,1.0149151408258327E-2,1.7968636339072683,-50711.833635135321,2148.549746971165,6.3743146097290966,1.1214310113837021E-2,2.3497275500288892,-50645.568730507439,2022.9409192950934]
["KBM","KBM-35H01-C (240 V)",12.45,8.32,10.976501238239955,7.1741838158431079,1840,40.799999999999997,2600,1.75,13.4,93,1.52,325,10,1064.657569359247,2102.4200657333849,2423.6559139784949,10.766351432849122,1.6447368421052631,0.56966940109281294,0.48022152592206641,1.1863915436721184,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.38349870075998771,0.54556251105555875,4.6019844091198525,13.093500265333411,8.3355811584114221,325.61360390147172,263.95610791970807,2539.2577581875917,3.6096094692917982E-2,7.6859182800421619,-49097.640639163888,1064.657569359247,1.0514586540449376E-2,2.0038041519024214,-50689.0994415776,2102.4200657333849,7.1084292872759001,1.1214310113837021E-2,2.3497275500288892,-50645.568730507439,2022.9409192950934]
["KBM","KBM-35H01-C (400 V)",12.45,8.32,9.6876921882023268,6.3318249596093636,3450,40.799999999999997,4334,1.75,13.4,93,1.52,565,10,1064.657569359247,2096.6526258989184,2423.6559139784949,10.771275383435743,1.6447368421052631,0.56966630247097405,0.48022152592206641,1.1863915436721184,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.38349870075998771,0.54556251105555875,4.6019844091198525,13.093500265333411,8.3355811584114221,325.61360390147166,263.95610791970807,2539.2577581875917,3.6096094692917982E-2,7.6859182800421619,-49097.640639163888,1064.657569359247,1.0562317539477289E-2,2.0292759043949853,-50686.130034219044,2096.6526258989184,7.1987894910136152,1.1214310113837021E-2,2.3497275500288892,-50645.568730507439,2022.9409192950934]
["KBM","KBM-35H01-C (480 V)",12.45,8.32,8.8330993416001924,5.7732675435295375,4200,40.799999999999997,5201,1.75,13.4,93,1.52,679,10,1064.657569359247,2100.3902442735571,2423.6559139784949,10.641213605378676,1.6447368421052631,0.57095659280697675,0.48022152592206641,1.1863915436721184,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.38349870075998771,0.54556251105555875,4.6019844091198525,13.093500265333411,8.3355811584114221,325.61360390147166,263.95610791970807,2539.2577581875917,3.6096094692917982E-2,7.6859182800421619,-49097.640639163888,1064.657569359247,1.0531332612503719E-2,2.0127774378345764,-50688.057646714769,2100.3902442735571,7.1402617238254855,1.1214310113837021E-2,2.3497275500288892,-50645.568730507439,2022.9409192950934]
["KBM","KBM-35H01-D (120 V)",12.65,10.57,11.589373583328015,9.4222549457951352,1100,41.2,1556,1.08,8.5,74,1.52,160,10,1368.7836357187323,1556,1556,11.149695723325811,1.6447368421052631,0.56378274369217329,0.47555918101020161,1.5424164524421593,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.47950637327608808,0.68214233986510753,5.7540764793130572,16.371416156762582,10.422367227053138,325.61360390147166,263.95610791970807,2539.2577581875917,2.3081960173350388E-2,4.7653826622573376,-49768.414569131543,1368.7836357187323,6.4206963381568559E-3,1.1038601080308463,-50749.530565280234,2726.7677111963117,7.9743985300212525,7.089723419929481E-3,1.4427214002259514,-50710.134203859117,2574.6266152758035]
["KBM","KBM-35H01-D (240 V)",12.65,10.57,10.757574928986886,8.745995877225111,2450,41.2,3252,1.08,8.5,74,1.52,325,10,1368.7836357187323,2681.7497044948741,3045.9459459459463,10.578567193890567,1.6447368421052631,0.55981358063507658,0.47555918101020161,0.9321740037022429,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.47950637327608808,0.68214233986510753,5.7540764793130572,16.371416156762582,10.422367227053138,325.61360390147166,263.95610791970807,2539.2577581875917,2.3081960173350388E-2,4.7653826622573376,-49768.414569131543,1368.7836357187323,6.6050895365156806E-3,1.2067911433499059,-50738.672378393552,2681.7497044948741,8.7179828762352916,7.089723419929481E-3,1.4427214002259514,-50710.134203859117,2574.6266152758035]
["KBM","KBM-35H01-D (400 V)",12.65,10.57,8.4999233343583658,6.9105067759011103,4550,41.2,5420,1.08,8.5,74,1.52,565,10,1368.7836357187323,2690.8588159161659,3045.9459459459463,10.195654860995658,1.6447368421052631,0.56269892136303423,0.47555918101020161,0.9321740037022429,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.47950637327608808,0.68214233986510753,5.7540764793130572,16.371416156762582,10.422367227053138,325.61360390147161,263.95610791970807,2539.2577581875917,2.3081960173350388E-2,4.7653826622573376,-49768.414569131543,1368.7836357187323,6.5668902386959577E-3,1.1862014503575886,-50740.921784111102,2690.8588159161659,8.5692408242877658,7.089723419929481E-3,1.4427214002259514,-50710.134203859117,2574.6266152758035]
["KBM","KBM-35H01-D (480 V)",12.65,10.57,6.1741141716683536,5.0196050176165476,5800,41.2,6505,1.08,8.5,74,1.52,679,10,1368.7836357187323,2713.888617210092,3045.9459459459463,9.6198564076101043,1.6447368421052631,0.5669755628548554,0.47555918101020161,0.9321740037022429,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.47950637327608808,0.68214233986510753,5.7540764793130572,16.371416156762582,10.422367227053138,325.61360390147172,263.95610791970807,2539.2577581875917,2.3081960173350388E-2,4.7653826622573376,-49768.414569131543,1368.7836357187323,6.4723308767007061E-3,1.133625790119414,-50746.490011321046,2713.888617210092,8.189428867439263,7.089723419929481E-3,1.4427214002259514,-50710.134203859117,2574.6266152758035]
["KBM","KBM-35H01-E (120 V)",12.2,12.8,10.777063289365486,11.226107593089049,1400,41.1,1996,0.74,5.4,57.8,1.52,160,10,1751.4152842767196,1996,1996,10.171298803981079,1.6447368421052631,0.58652226233956717,0.47671625930949652,1.2024048096192386,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.60208812414399082,0.8565262626282103,7.2250574897278899,20.556630303077046,13.086757304189435,325.61360390147166,263.95610791970807,2539.2577581875917,1.4489686842120434E-2,3.1945680687306601,-50041.484910370331,1751.4152842767196,3.8463128250565879E-3,0.68021480126270328,-50770.53605992379,3545.8036570541672,9.1817590623723362,4.3676973700842465E-3,0.96950986824766927,-50734.822196885398,3299.0338131317781]
["KBM","KBM-35H01-E (240 V)",12.2,12.8,9.5955028593145926,9.9953154784527012,3100,41.1,4166,0.74,5.4,57.8,1.52,325,10,1751.4152842767196,3503.3431085163479,3899.6539792387548,9.2566299648481429,1.6447368421052631,0.58257385771263459,0.47671625930949652,0.7274857233796207,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.60208812414399082,0.8565262626282103,7.2250574897278899,20.556630303077046,13.086757304189435,325.61360390147166,263.95610791970807,2539.2577581875917,1.4489686842120434E-2,3.1945680687306601,-50041.484910370331,1751.4152842767196,3.9270778831505997E-3,0.7325446677066384,-50765.003804987267,3503.3431085163479,9.8881244995289599,4.3676973700842465E-3,0.96950986824766927,-50734.822196885398,3299.0338131317781]
["KBM","KBM-35H01-E (400 V)",12.2,12.8,5.1268764455012183,5.3404962973971024,6100,41.1,6943,0.74,5.4,57.8,1.52,565,10,1751.4152842767196,3564.4534952770891,3899.6539792387548,8.0669147579737874,1.6447368421052631,0.58976914483206866,0.47671625930949652,0.7274857233796207,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.60208812414399082,0.8565262626282103,7.2250574897278899,20.556630303077046,13.086757304189435,325.61360390147166,263.95610791970807,2539.2577581875917,1.4489686842120434E-2,3.1945680687306601,-50041.484910370331,1751.4152842767196,3.8119553889336979E-3,0.65669062608945772,-50772.889479831887,3564.4534952770891,8.8642221487667712,4.3676973700842465E-3,0.96950986824766927,-50734.822196885398,3299.0338131317781]
["KBM","KBM-35H01-F (120 V)",12.4,14.58,11.071215728829969,12.725535320494217,1600,41.1,2288,0.56999999999999995,4.4000000000000004,52.6,1.52,160,10,1939.3158402428969,2288,2288,10.499838492226855,1.6447368421052631,0.57267291537738407,0.47671625930949652,1.048951048951049,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.67475445545763924,0.95990086625034976,8.0970534654916708,23.037620790008393,14.666204903225802,325.61360390147166,263.95610791970807,2539.2577581875917,1.2063253765421899E-2,2.5095675373278952,-50236.08920741138,1939.3158402428969,3.2019065029300934E-3,0.54294650955302259,-50778.523165558654,3898.4334871490255,10.455283618371201,3.6230075809516194E-3,0.76162111438124747,-50752.746100540768,3639.1539781417782]
["KBM","KBM-35H01-F (240 V)",12.4,14.58,9.4962449378164226,10.915224066455659,3600,41.1,4576,0.56999999999999995,4.4000000000000004,52.6,1.52,325,10,1939.3158402428969,3869.1590579566814,4285.1711026615967,9.2791416108513456,1.6447368421052631,0.57215959138073869,0.47671625930949652,0.65949394128837768,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.67475445545763924,0.95990086625034976,8.0970534654916708,23.037620790008393,14.666204903225802,325.61360390147166,263.95610791970807,2539.2577581875917,1.2063253765421899E-2,2.5095675373278952,-50236.08920741138,1939.3158402428969,3.2446914765307758E-3,0.5690129018324831,-50775.904148168636,3869.1590579566814,10.957232741156501,3.6230075809516194E-3,0.76162111438124747,-50752.746100540768,3639.1539781417782]
["KBM","KBM-35H01-F (400 V)",12.4,14.58,3.7039695846841094,4.2574363042346084,6600,41.1,7200,0.56999999999999995,4.4000000000000004,52.6,1.52,565,10,1939.3158402428969,3978.8902353419853,4285.1711026615967,7.1574923476155599,1.6447368421052631,0.58334289328153066,0.47671625930949652,0.65949394128837768,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.67475445545763924,0.95990086625034976,8.0970534654916708,23.037620790008393,14.666204903225802,325.61360390147166,263.95610791970807,2539.2577581875917,1.2063253765421899E-2,2.5095675373278952,-50236.08920741138,1939.3158402428969,3.0902076350016123E-3,0.46810285150314573,-50785.36064266639,3978.8902353419853,9.0140520086642866,3.6230075809516194E-3,0.76162111438124747,-50752.746100540768,3639.1539781417782]
["KBM","KBM-35H01-G (120 V)",12.4,20.100000000000001,10.605814505613111,16.834626199385891,2350,41.2,3026,0.3,2.2000000000000002,38.1,1.52,160,10,2818.0965506758484,3026,3026,10.089699869780969,1.6447368421052631,0.57123555556294847,0.47555918101020161,0.79312623925974879,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.93021704764736279,1.3233201242545973,11.162604571768354,31.759682982110338,20.218842150537633,325.61360390147161,263.95610791970807,2539.2577581875917,5.8902206027177956E-3,1.3221430488509529,-50504.104234053077,2818.0965506758484,1.6247473910050228E-3,0.26112614503318543,-50793.416683334392,5511.4926221505912,13.18996064106377,1.8584432434600737E-3,0.40027930723063687,-50777.565893491192,5120.5229225395415]
["KBM","KBM-35H01-G (240 V)",12.4,20.100000000000001,7.1259373576805212,11.31101167885797,5300,41.2,6316,0.3,2.2000000000000002,38.1,1.52,325,10,2818.0965506758484,5576.3696291190081,5916.010498687664,6.8509202376034928,1.6447368421052631,0.57623498050284605,0.47555918101020161,0.46870212990077026,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.93021704764736279,1.3233201242545973,11.162604571768354,31.759682982110338,20.218842150537633,325.61360390147166,263.95610791970807,2539.2577581875917,5.8902206027177956E-3,1.3221430488509529,-50504.104234053077,2818.0965506758484,1.591434986475159E-3,0.23466445749725309,-50795.676149721265,5576.3696291190081,11.853332257679492,1.8584432434600737E-3,0.40027930723063687,-50777.565893491192,5120.5229225395415]
["KBM","KBM-35H01-H (120 V)",12.2,21.2,10.313240312354818,17.450491222258577,2500,41.4,3237,0.27,1.6,35.700000000000003,1.52,160,10,3237,3237,3237,9.7570235564370194,1.6447368421052631,0.58067822073517783,0.47326179366232629,0.74142724745134381,19.593038257620307,0,-15.870360988672449,0,0,0,0,0,0.9972084556134847,1.4186216224779731,11.966501467361816,34.046918939471354,21.674941785063748,325.61360390147166,263.95610791970807,2539.2577581875917,3.9987667004109289E-3,1.2010718241405245,-50522.189257439401,3407.4870636700498,1.3665855085690654E-3,0.22083230025345613,-50795.594035411181,6016.4353255486894,13.227262993785367,1.5217844403777993E-3,0.36186830597563979,-50779.473515431731,5658.8639898452248]
["KBM","KBM-35H01-H (240 V)",12.2,21.2,6.3605136185653901,10.762290386743469,5600,41.4,6756,0.27,1.6,35.700000000000003,1.52,325,10,{"$f":"IF(AQ864<I864,IF(AQ864<0,0,AQ864),I864)","v":3407.4870636700498},{"$f":"IF(AU864<I864,IF(AU864<0,0,AU864),I864)","v":6083.4893184976308},{"$f":"IF(UAC_V*0.98/L864*1000<I864,IF(UAC_V*0.98/L864*1000<0,0,UAC_V*0.98/L864*1000),I864)","v":6313.7254901960778},{"$f":"C864+(E864-C864)/G864*Q864","v":5.856347673755387},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M864,(inertia/gear^2+gear_inertia)/M864),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M864,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M864))","v":1.6447368421052631},{"$f":"IF((C864+(E864-C864)/G864*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X864^2*time1+Y864^2*time2+Z864^2*time3+AA864^2*time4)/time)/(C864+(E864-C864)/G864*mspeed),SQRT((((X864-Y864)*2/PI()+Y864)^2*time1+Y864^2*time2+((Z864-Y864)*2/PI()+Y864)^2*time3+AA864^2*time4)/time)/(C864+(E864-C864)/G864*mspeed)),IF(AccType=1,SQRT((X864^2*time1+Y864^2*time2+Z864^2*time3+AA864^2*time4+AB864^2*time5+AC864^2*time6+AD864^2*time7+AE864^2*time8)/time)/(C864+(E864-C864)/G864*mspeed),SQRT((((X864-Y864)*2/PI()+Y864)^2*time1+Y864^2*time2+((Z864-Y864)*2/PI()+Y864)^2*time3+AA864^2*time4+((AB864-AC864)*2/PI()+AC864)^2*time5+AC864^2*time6+((AD864-AC864)*2/PI()+AC864)^2*time7+AE864^2*time8)/time)/(C864+(E864-C864)/G864*mspeed))))","v":0.5871179823273095},{"$f":"IF(move1,MAX(ABS(X864),ABS(Z864))/H864,MAX(ABS(X864),ABS(Z864),ABS(AB864),ABS(AD864))/H864)","v":0.47326179366232629},{"$f":"IF(AZ864>0,speed/(MIN(AZ864,I864)),\"NA\")","v":0.4241133917172733},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M864+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M864+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":19.593038257620307},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M864+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M864+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-15.870360988672449},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M864+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M864+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M864+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M864+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH864/Irms","v":0.9972084556134847},{"$f":"AI864/Ipeak","v":1.4186216224779731},{"$f":"IF(move1,IF(AccType=1,SQRT((X864^2*time1+Y864^2*time2+Z864^2*time3+AA864^2*time4)/time)/(C864/D864),SQRT((((X864-Y864)*2/PI()+Y864)^2*time1+Y864^2*time2+((Z864-AA864)*2/PI()+AA864)^2*time3+AA864^2*time4)/time)/(C864/D864)),IF(AccType=1,SQRT((X864^2*time1+Y864^2*time2+Z864^2*time3+AA864^2*time4+AB864^2*time5+AC864^2*time6+AD864^2*time7+AE864^2*time8)/time)/(C864/D864),SQRT((((X864-Y864)*2/PI()+Y864)^2*time1+Y864^2*time2+((Z864-AA864)*2/PI()+AA864)^2*time3+AA864^2*time4+((AB864-AC864)*2/PI()+AC864)^2*time5+AC864^2*time6+((AD864-AE864)*2/PI()+AE864)^2*time7+AE864^2*time8)/time)/(C864/D864)))","v":11.966501467361816},{"$f":"IF(move1,MAX(ABS(X864),ABS(Z864))/(C864/D864),MAX(ABS(X864),ABS(Z864),ABS(AB864),ABS(AD864))/(C864/D864))","v":34.046918939471354},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X864),ABS(Z864))/(C864/D864),MAX(ABS((X864-Y864)*2/PI()+Y864),ABS((Z864-Y864)*2/PI()+Y864))/(C864/D864)),IF(AccType=1,MAX(ABS(X864),ABS(Z864),ABS(AB864),ABS(AD864))/(C864/D864),MAX(ABS((X864-Y864)*2/PI()+Y864),ABS((Z864-Y864)*2/PI()+Y864),ABS((AB864-AC864)*2/PI()+AC864),ABS((AD864-AC864)*2/PI()+AC864))/(C864/D864)))","v":21.674941785063748},{"$f":"IF((C864+(E864-C864)/G864*mspeed)<0,\"NA\",U864*(C864+(E864-C864)/G864*mspeed)*mspeed/9.55)","v":325.61360390147166},{"$f":"IF(move1,IF(speed1>speed2,AM864/2*time1/time,AM864/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z864*-speed/30*PI(),((Z864-AA864)*2/PI()+AA864)*-speed/30*PI()),IF(AccType=1,X864*-speed/30*PI(),((X864-Y864)*2/PI()+Y864)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z864*-speed/30*PI(),((Z864-AA864)*2/PI()+AA864)*-speed/30*PI()),IF(AccType=1,X864*-speed/30*PI(),((X864-Y864)*2/PI()+Y864)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD864*-speed/30*PI(),((AD864-AE864)*2/PI()+AE864)*-speed/30*PI()),IF(AccType=1,AB864*-speed/30*PI(),((AB864-AC864)*2/PI()+AC864)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD864*-speed/30*PI(),((AD864-AE864)*2/PI()+AE864)*-speed/30*PI()),IF(AccType=1,AB864*-speed/30*PI(),((AB864-AC864)*2/PI()+AC864)*-speed/30*PI()),0)/2*time7/time)))","v":263.95610791970807},{"$f":"IF(move1,MAX(IF(AccType=1,Z864*-speed/30*PI(),((Z864-AA864)*2/PI()+AA864)*-speed/30*PI()),IF(AccType=1,X864*-speed/30*PI(),((X864-Y864)*2/PI()+Y864)*-speed/30*PI()),0),MAX(IF(AccType=1,Z864*-speed/30*PI(),((Z864-AA864)*2/PI()+AA864)*-speed/30*PI()),IF(AccType=1,X864*-speed/30*PI(),((X864-Y864)*2/PI()+Y864)*-speed/30*PI()),IF(AccType=1,AD864*-speed/30*PI(),((AD864-AE864)*2/PI()+AE864)*-speed/30*PI()),IF(AccType=1,AB864*-speed/30*PI(),((AB864-AC864)*2/PI()+AC864)*-speed/30*PI()),0))","v":2539.2577581875917},{"$f":"(L864^2)/1000000+((K864/1000)^2*(D864/C864*H864)^2*PI()*PI()*(O864/2)^2)/1200","v":3.9987667004109289E-3},{"$f":"SQRT(3)*L864*J864*D864/C864*H864/1000","v":1.2010718241405245},{"$f":"0.75*J864^2*(D864/C864*H864)^2-(UAC_V*0.98)^2","v":-50522.189257439401},{"$f":"-AO864/2/AN864+SQRT((AO864/2/AN864)^2-AP864/AN864)","v":3407.4870636700498},{"$f":"(L864^2)/1000000+((K864/1000)^2*AV864^2*PI()*PI()*(O864/2)^2)/1200","v":1.3416070315707949E-3},{"$f":"SQRT(3)*L864*J864*AV864/1000","v":0.18852100277410336},{"$f":"0.75*J864^2*AV864^2-(UAC_V*0.98)^2","v":-50798.18855093274},{"$f":"-AS864/2/AR864+SQRT((AS864/2/AR864)^2-AT864/AR864)","v":6083.4893184976308},{"$f":"D864+(F864-D864)*((0.85*UAC_V-D864*J864)/L864*1000)/G864","v":11.291902863318471},{"$f":"(L864^2)/1000000+((K864/1000)^2*AJ864^2*PI()*PI()*(O864/2)^2)/1200","v":1.5217844403777993E-3},{"$f":"SQRT(3)*L864*J864*AJ864/1000","v":0.36186830597563979},{"$f":"0.75*J864^2*AJ864^2-(UAC_V*0.98)^2","v":-50779.473515431731},{"$f":"IF(((AX864/2/AW864)^2-AY864/AW864)>0,-AX864/2/AW864+SQRT((AX864/2/AW864)^2-AY864/AW864),-9999)","v":5658.8639898452248}]
["KBM","KBM-35H02-A (120 V)",17.3,4.97,16.160348067792452,4.5522107233218172,325,58.8,531,5.5,44,215,2.2799999999999998,160,10,429.44455895517831,531,531,15.43798407383936,1.0964912280701755,0.52099759511261579,0.39621079496829231,4.5197740112994351,23.297194744135588,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-18.870727742749828,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.1960297794203627,0.27887056329083298,2.3523573530443525,6.6928935189799921,4.2608283485335026,387.17239468881462,313.85825767567286,3019.3164388399728,0.15981473447468164,34.597872067302063,-44331.321430041098,429.44455895517831,5.2481713701107664E-2,8.1199431311193813,-50448.570078677054,906.12615018174461,3.964525456707169,5.3451898216566575E-2,8.7268159227029614,-50393.276191732068,892.7606697992461]
["KBM","KBM-35H02-A (240 V)",17.3,4.97,15.875705573416559,4.4720297389905799,800,58.8,1114,5.5,44,215,2.2799999999999998,325,10,429.44455895517831,882.63962569647083,1048.372093023256,15.728576625548527,1.0964912280701755,0.49637834614915988,0.39621079496829231,2.6882904693143401,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.1960297794203627,0.27887056329083298,2.3523573530443525,6.6928935189799921,4.2608283485335026,387.17239468881462,313.85825767567286,3019.3164388399728,0.15981473447468164,34.597872067302063,-44331.321430041098,429.44455895517831,5.4225682878188894E-2,9.1821286772070749,-50349.175754219643,882.63962569647083,4.4831327387055282,5.3451898216566575E-2,8.7268159227029614,-50393.276191732068,892.7606697992461]
["KBM","KBM-35H02-A (400 V)",17.3,4.97,15.311803145737517,4.3131839847147937,1450,58.8,1863,5.5,44,215,2.2799999999999998,565,10,429.44455895517831,876.57411929158366,1048.372093023256,16.098067650687288,1.0964912280701755,0.49087986103155107,0.39621079496829231,2.6882904693143401,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.1960297794203627,0.27887056329083298,2.3523573530443525,6.6928935189799921,4.2608283485335026,387.17239468881462,313.85825767567286,3019.3164388399728,0.15981473447468164,34.597872067302063,-44331.321430041098,429.44455895517831,5.4705837521984449E-2,9.4536434319105158,-50321.810220996733,876.57411929158366,4.6156985879376524,5.3451898216566575E-2,8.7268159227029614,-50393.276191732068,892.7606697992461]
["KBM","KBM-35H02-A (480 V)",17.3,4.97,15.006037491521562,4.2270528145131161,1750,58.8,2235,5.5,44,215,2.2799999999999998,679,10,429.44455895517831,875.55461693567872,1048.372093023256,16.15229173407106,1.0964912280701755,0.49007942005577243,0.39621079496829231,2.6882904693143401,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.1960297794203627,0.27887056329083298,2.3523573530443525,6.6928935189799921,4.2608283485335026,387.17239468881462,313.85825767567286,3019.3164388399728,0.15981473447468164,34.597872067302063,-44331.321430041098,429.44455895517831,5.4787765370186703E-2,9.4991964281535672,-50317.140893560601,875.55461693567872,4.6379396320334836,5.3451898216566575E-2,8.7268159227029614,-50393.276191732068,892.7606697992461]
["KBM","KBM-35H02-B (120 V)",17.600000000000001,6.3,16.472536610011169,5.7395597944289785,400,58.8,661,3.43,28,174,2.2799999999999998,160,10,580.48830701823795,661,661,15.736866748043456,1.0964912280701755,0.50151169833342701,0.39621079496829231,3.6308623298033282,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.24425285415933476,0.34747236479179494,2.9310342499120172,8.3393367550030781,5.3089866666666641,387.17239468881462,313.85825767567286,3019.3164388399728,0.10169026752584735,21.757510581125761,-46896.211768002715,580.48830701823795,3.4146144969775236E-2,5.0650102317115984,-50593.3228299037,1145.3294835865233,4.8997771869691018,3.4819576450871893E-2,5.4880193038575156,-50556.461725132845,1128.7387465265822]
["KBM","KBM-35H02-B (240 V)",17.600000000000001,6.3,16.083025828233634,5.6038417519977815,950,58.8,1386,3.43,28,174,2.2799999999999998,325,10,580.48830701823795,1118.0987382847256,1295.4022988505747,15.814603255302641,1.0964912280701755,0.48511840698441039,0.39621079496829231,2.1262670457494384,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.24425285415933476,0.34747236479179494,2.9310342499120172,8.3393367550030781,5.3089866666666641,387.17239468881462,313.85825767567286,3019.3164388399728,0.10169026752584735,21.757510581125761,-46896.211768002715,580.48830701823795,3.5273123964755022E-2,5.7554166911030977,-50531.636241179251,1118.0987382847256,5.5676608959264744,3.4819576450871893E-2,5.4880193038575156,-50556.461725132845,1128.7387465265822]
["KBM","KBM-35H02-B (400 V)",17.600000000000001,6.3,15.305400360670603,5.3328921117319172,1800,58.8,2313,3.43,28,174,2.2799999999999998,565,10,580.48830701823795,1109.9957651242817,1295.4022988505747,16.185002287604814,1.0964912280701755,0.48097461568936983,0.39621079496829231,2.1262670457494384,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.24425285415933476,0.34747236479179494,2.9310342499120172,8.3393367550030781,5.3089866666666641,387.17239468881462,313.85825767567286,3019.3164388399728,0.10169026752584735,21.757510581125761,-46896.211768002715,580.48830701823795,3.5630020267623824E-2,5.9573993785243244,-50512.101080763299,1109.9957651242817,5.7630544131582848,3.4819576450871893E-2,5.4880193038575156,-50556.461725132845,1128.7387465265822]
["KBM","KBM-35H02-B (480 V)",17.600000000000001,6.3,14.823112654331526,5.16484761474966,2200,58.8,2776,3.43,28,174,2.2799999999999998,679,10,580.48830701823795,1109.1097688897876,1295.4022988505747,16.20005778082394,1.0964912280701755,0.48081448495394641,0.39621079496829231,2.1262670457494384,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.24425285415933476,0.34747236479179494,2.9310342499120172,8.3393367550030781,5.3089866666666641,387.17239468881462,313.85825767567286,3019.3164388399728,0.10169026752584735,21.757510581125761,-46896.211768002715,580.48830701823795,3.5669652063491861E-2,5.9794078050569288,-50509.931785414396,1109.1097688897876,5.7843448708893241,3.4819576450871893E-2,5.4880193038575156,-50556.461725132845,1128.7387465265822]
["KBM","KBM-35H02-C (120 V)",17.5,8.6999999999999993,16.119212636347161,7.8630305543156886,625,59.2,923,1.8,14.6,124,2.2799999999999998,160,10,854.80109861304436,923,923,15.460853221357487,1.0964912280701755,0.49618794603831018,0.3935336950022903,2.6002166847237271,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.33922899799435235,0.48258474827138004,4.0707479759322283,11.58203395851312,7.3733518222222196,387.17239468881462,313.85825767567286,3019.3164388399728,5.3339831827869243E-2,11.37778514160213,-48700.353894243271,854.80109861304436,1.7377588270825941E-2,2.6125227532931534,-50694.187134227461,1634.4700989794405,6.7577989017823681,1.7758835893578233E-2,2.850491659127421,-50673.049849460935,1610.8506339224848]
["KBM","KBM-35H02-C (240 V)",17.5,8.6999999999999993,15.48350232079725,7.5529279613645128,1400,59.2,1935,1.8,14.6,124,2.2799999999999998,325,10,854.80109861304436,1605.4560562711852,1817.741935483871,15.187572563190825,1.0964912280701755,0.4859634055923101,0.3935336950022903,1.4898960520975837,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.33922899799435235,0.48258474827138004,4.0707479759322283,11.58203395851312,7.3733518222222196,387.17239468881462,313.85825767567286,3019.3164388399728,5.3339831827869243E-2,11.37778514160213,-48700.353894243271,854.80109861304436,1.7849092266499767E-2,2.9039749617356674,-50668.045819159932,1605.4560562711852,7.5116968005287674,1.7758835893578233E-2,2.850491659127421,-50673.049849460935,1610.8506339224848]
["KBM","KBM-35H02-C (400 V)",17.5,8.6999999999999993,14.155427879702691,6.9050867705866787,2550,59.2,3224,1.8,14.6,124,2.2799999999999998,565,10,854.80109861304436,1598.8889356222885,1817.741935483871,15.402902212731707,1.0964912280701755,0.48429228031440413,0.3935336950022903,1.4898960520975837,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.33922899799435235,0.48258474827138004,4.0707479759322283,11.58203395851312,7.3733518222222196,387.17239468881462,313.85825767567286,3019.3164388399728,5.3339831827869243E-2,11.37778514160213,-48700.353894243271,854.80109861304436,1.7960573805538994E-2,2.9687059101070856,-50661.865014621741,1598.8889356222885,7.6791360051306397,1.7758835893578233E-2,2.850491659127421,-50673.049849460935,1610.8506339224848]
["KBM","KBM-35H02-C (480 V)",17.5,8.6999999999999993,13.100441253251635,6.3904591479276274,3200,59.2,3869,1.8,14.6,124,2.2799999999999998,679,10,854.80109861304436,1599.9065868427708,1817.741935483871,15.300349056836113,1.0964912280701755,0.48511194480708048,0.3935336950022903,1.4898960520975837,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.33922899799435235,0.48258474827138004,4.0707479759322283,11.58203395851312,7.3733518222222196,387.17239468881462,313.85825767567286,3019.3164388399728,5.3339831827869243E-2,11.37778514160213,-48700.353894243271,854.80109861304436,1.7943182572664768E-2,2.9587010495414052,-50662.829226382717,1599.9065868427708,7.653256484786553,1.7758835893578233E-2,2.850491659127421,-50673.049849460935,1610.8506339224848]
["KBM","KBM-35H02-D (120 V)",17.45,10.92,15.952942531093511,9.7274039823740921,850,59.4,1165,1.1399999999999999,9.3000000000000007,99,2.2799999999999998,160,10,1098.4708248491929,1165,1165,15.398150645557577,1.0964912280701755,0.49165035319898437,0.39220866572618834,2.0600858369098711,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.42701091141666331,0.60746267097889362,5.1241309369999595,14.579104103493446,9.2813459356892682,387.17239468881462,313.85825767567286,3019.3164388399728,3.4373633840441876E-2,7.2663167473263588,-49458.375001722394,1098.4708248491929,1.1033739022531889E-2,1.6275114126220025,-50737.595634164507,2071.905389275259,8.3257500636762494,1.1332956117589051E-2,1.8143105809444953,-50721.19604519623,2037.0172678890194]
["KBM","KBM-35H02-D (240 V)",17.45,10.92,15.020785439916175,9.1590155121440091,1850,59.4,2437,1.1399999999999999,9.3000000000000007,99,2.2799999999999998,325,10,1098.4708248491929,2041.5249569344362,2276.7676767676771,14.769296135048844,1.0964912280701755,0.48574810356533804,0.39220866572618834,1.1781932523758833,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.42701091141666331,0.60746267097889362,5.1241309369999595,14.579104103493446,9.2813459356892682,387.17239468881462,313.85825767567286,3019.3164388399728,3.4373633840441876E-2,7.2663167473263588,-49458.375001722394,1098.4708248491929,1.1293148609081162E-2,1.7905832185629182,-50723.377828216537,2041.5249569344362,9.1599654726539743,1.1332956117589051E-2,1.8143105809444953,-50721.19604519623,2037.0172678890194]
["KBM","KBM-35H02-D (400 V)",17.45,10.92,12.441369265697876,7.5862007717669977,3500,59.4,4061,1.1399999999999999,9.3000000000000007,99,2.2799999999999998,565,10,1098.4708248491929,2041.5681542910456,2276.7676767676771,14.528439713212974,1.0964912280701755,0.48728771229642004,0.39220866572618834,1.1781932523758833,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.42701091141666331,0.60746267097889362,5.1241309369999595,14.579104103493446,9.2813459356892682,387.17239468881462,313.85825767567286,3019.3164388399728,3.4373633840441876E-2,7.2663167473263588,-49458.375001722394,1098.4708248491929,1.1292768784382073E-2,1.7903553086169133,-50723.398645773581,2041.5681542910456,9.1587995691569262,1.1332956117589051E-2,1.8143105809444953,-50721.19604519623,2037.0172678890194]
["KBM","KBM-35H02-D (480 V)",17.45,10.92,10.548641577020971,6.4320985225737637,4300,59.4,4873,1.1399999999999999,9.3000000000000007,99,2.2799999999999998,679,10,1098.4708248491929,2047.7942142288907,2276.7676767676771,14.163357709559005,1.0964912280701755,0.48957594965588419,0.39220866572618834,1.1781932523758833,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.42701091141666331,0.60746267097889362,5.1241309369999595,14.579104103493446,9.2813459356892682,387.17239468881462,313.85825767567286,3019.3164388399728,3.4373633840441876E-2,7.2663167473263588,-49458.375001722394,1098.4708248491929,1.1238351996572391E-2,1.7573976406762601,-50726.381138979326,2047.7942142288907,8.990200256225874,1.1332956117589051E-2,1.8143105809444953,-50721.19604519623,2037.0172678890194]
["KBM","KBM-35H02-E (120 V)",17.100000000000001,12,15.580431271101332,10.671528267877624,950,59.4,1305,0.94,7.4,88.4,2.2799999999999998,160,10,1241.5761845834363,1305,1305,15.012592430302355,1.0964912280701755,0.49996526148383746,0.39220866572618834,1.8390804597701149,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.47884714377101556,0.68120452468232706,5.7461657252521867,16.348908592375849,10.408038466536709,387.17239468881462,313.85825767567286,3019.3164388399728,2.7378895815966042E-2,5.9994622722815141,-49653.670103047094,1241.5761845834363,8.7440660571906914E-3,1.3076932570160862,-50750.452452343918,2335.5308342952744,9.0858411229866167,9.0342788194986267E-3,1.4979924849247386,-50733.371521669455,2288.2805935206902]
["KBM","KBM-35H02-E (240 V)",17.100000000000001,12,14.533563583806249,9.9544956053467466,2050,59.4,2728,0.94,7.4,88.4,2.2799999999999998,325,10,1241.5761845834363,2305.990145921799,2549.7737556561083,14.213084348352368,1.0964912280701755,0.49521879176595285,0.39220866572618834,1.0488224244857232,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.47884714377101556,0.68120452468232706,5.7461657252521867,16.348908592375849,10.408038466536709,387.17239468881462,313.85825767567286,3019.3164388399728,2.7378895815966042E-2,5.9994622722815141,-49653.670103047094,1241.5761845834363,8.9227156064964272E-3,1.4278419791464791,-50739.937750845449,2305.990145921799,9.9206333761007492,9.0342788194986267E-3,1.4979924849247386,-50733.371521669455,2288.2805935206902]
["KBM","KBM-35H02-E (400 V)",17.100000000000001,12,11.496360954248335,7.8742198316769416,3850,59.4,4547,0.94,7.4,88.4,2.2799999999999998,565,10,1241.5761845834363,2311.5124020204676,2549.7737556561083,13.735615285532178,1.0964912280701755,0.4979873387894016,0.39220866572618834,1.0488224244857232,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.47884714377101556,0.68120452468232706,5.7461657252521867,16.348908592375849,10.408038466536709,387.17239468881462,313.85825767567286,3019.3164388399728,2.7378895815966042E-2,5.9994622722815141,-49653.670103047094,1241.5761845834363,8.8886124952326367E-3,1.4056996167707505,-50741.944943343282,2311.5124020204676,9.7667884391829531,9.0342788194986267E-3,1.4979924849247386,-50733.371521669455,2288.2805935206902]
["KBM","KBM-35H02-E (480 V)",17.100000000000001,12,9.1226258870120436,6.2483738952137289,4700,59.4,5457,0.94,7.4,88.4,2.2799999999999998,679,10,1241.5761845834363,2322.7824832632041,2549.7737556561083,13.1575096059392,1.0964912280701755,0.50131661402265582,0.39220866572618834,1.0488224244857232,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.47884714377101556,0.68120452468232706,5.7461657252521867,16.348908592375849,10.408038466536709,387.17239468881462,313.85825767567286,3019.3164388399728,2.7378895815966042E-2,5.9994622722815141,-49653.670103047094,1241.5761845834363,8.8200216950483582E-3,1.3600739961504191,-50745.981963264581,2322.7824832632041,9.4497820327723918,9.0342788194986267E-3,1.4979924849247386,-50733.371521669455,2288.2805935206902]
["KBM","KBM-35H02-F (120 V)",17.3,14.92,15.597184423005743,13.106877666391382,1200,59.4,1607,0.61,4.9000000000000004,72.099999999999994,2.2799999999999998,160,10,1556.7687458613204,1607,1607,15.019646139808524,1.0964912280701755,0.49151643812530482,0.39220866572618834,1.4934660858742999,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.58848376437662209,0.83717279764572006,7.061805172519465,20.092147143497282,12.79105814086919,387.17239468881462,313.85825767567286,3019.3164388399728,1.8154352086988401E-2,3.9024279373386861,-50072.775299383786,1556.7687458613204,5.7972703829910315E-3,0.83900236477589374,-50771.307102282262,2887.8799523471121,11.013806897389667,6.0061351656525873E-3,0.97438861314326075,-50759.500213189072,2827.1230267991464]
["KBM","KBM-35H02-F (240 V)",17.3,14.92,13.873506360085971,11.658408705954598,2650,59.4,3356,0.61,4.9000000000000004,72.099999999999994,2.2799999999999998,325,10,1556.7687458613204,2863.6073731893789,3126.2135922330099,13.597308508888933,1.0964912280701755,0.48984351621408195,0.39220866572618834,0.84891954727462537,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.58848376437662209,0.83717279764572006,7.061805172519465,20.092147143497282,12.79105814086919,387.17239468881462,313.85825767567286,3019.3164388399728,1.8154352086988401E-2,3.9024279373386861,-50072.775299383786,1556.7687458613204,5.8786208812246533E-3,0.89417429414825578,-50766.708450953491,2863.6073731893789,11.738063468973856,6.0061351656525873E-3,0.97438861314326075,-50759.500213189072,2827.1230267991464]
["KBM","KBM-35H02-F (400 V)",17.3,14.92,7.6956096012669395,6.4668988245940673,5100,59.4,5593,0.61,4.9000000000000004,72.099999999999994,2.2799999999999998,565,10,1556.7687458613204,2900.2820401309468,3126.2135922330099,11.838148827480079,1.0964912280701755,0.49777973354601124,0.39220866572618834,0.84891954727462537,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.58848376437662209,0.83717279764572006,7.061805172519465,20.092147143497282,12.79105814086919,387.17239468881462,313.85825767567286,3019.3164388399728,1.8154352086988401E-2,3.9024279373386861,-50072.775299383786,1556.7687458613204,5.7567815856527475E-3,0.81014367925192587,-50773.595888039235,2900.2820401309468,10.634971267101097,6.0061351656525873E-3,0.97438861314326075,-50759.500213189072,2827.1230267991464]
["KBM","KBM-35H02-F (480 V)",17.3,14.92,6.2689363695640994,5.2680137559362183,5400,59.4,6711,0.61,4.9000000000000004,72.099999999999994,2.2799999999999998,679,10,1556.7687458613204,2911.0994632577899,3126.2135922330099,11.353236404865838,1.0964912280701755,0.49996986249117403,0.39220866572618834,0.84891954727462537,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.58848376437662209,0.83717279764572006,7.061805172519465,20.092147143497282,12.79105814086919,387.17239468881462,313.85825767567286,3019.3164388399728,1.8154352086988401E-2,3.9024279373386861,-50072.775299383786,1556.7687458613204,5.7220652218733011E-3,0.78455449031548419,-50775.558364679098,2911.0994632577899,10.299055186957425,6.0061351656525873E-3,0.97438861314326075,-50759.500213189072,2827.1230267991464]
["KBM","KBM-35H02-G (120 V)",17.100000000000001,18.64,15.094049441618461,16.057499405977087,1550,59.4,2032,0.39,3.1,57,2.2799999999999998,160,10,1983.6417982216799,2032,2032,14.470263526044331,1.0964912280701755,0.49579073911550176,0.39220866572618834,1.1811023622047243,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.74380922999097754,1.058137695006548,8.9257107598917305,25.395304680157153,16.167153084687019,387.17239468881462,313.85825767567286,3019.3164388399728,1.1533272593584727E-2,2.4930806770391358,-50326.901207892748,1983.6417982216799,3.5900655475092362E-3,0.50585735404750631,-50785.469967478923,3691.3391728377082,13.137961292437231,3.7654746344215747E-3,0.62249180826925687,-50775.343437106625,3590.3898836986527]
["KBM","KBM-35H02-G (240 V)",17.100000000000001,18.64,12.44217172759582,13.236352901697682,3400,59.4,4241,0.39,3.1,57,2.2799999999999998,325,10,1983.6417982216799,3683.2904620695199,3954.385964912281,12.054078103028216,1.0964912280701755,0.49682022155848432,0.39220866572618834,0.66845108128692465,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.74380922999097754,1.058137695006548,8.9257107598917305,25.395304680157153,16.167153084687019,387.17239468881462,313.85825767567286,3019.3164388399728,1.1533272593584727E-2,2.4930806770391358,-50326.901207892748,1983.6417982216799,3.6033642763321039E-3,0.51562517013107068,-50784.702219446546,3683.2904620695199,13.391647808192545,3.7654746344215747E-3,0.62249180826925687,-50775.343437106625,3590.3898836986527]
["KBM","KBM-35H02-G (400 V)",17.100000000000001,18.64,3.6056826762543186,3.8358326343131051,5800,59.4,7068,0.39,3.1,57,2.2799999999999998,565,10,1983.6417982216799,3777.7469815710447,3954.385964912281,8.3106695623892914,1.0964912280701755,0.51019268604911283,0.39220866572618834,0.66845108128692465,23.297194744135588,0,-18.870727742749828,0,0,0,0,0,0.74380922999097754,1.058137695006548,8.9257107598917305,25.395304680157153,16.167153084687019,387.17239468881462,313.85825767567286,3019.3164388399728,1.1533272593584727E-2,2.4930806770391358,-50326.901207892748,1983.6417982216799,3.455028335156748E-3,0.39316298057406496,-50793.26579183642,3777.7469815710447,10.211099985147639,3.7654746344215747E-3,0.62249180826925687,-50775.343437106625,3590.3898836986527]
["KBM","KBM-35H03-A (120 V)",21.8,10.199999999999999,20.567715722644937,9.3489616921113345,650,76.099999999999994,867,1.41,12,132,3.04,160,10,844.72056596793539,867,867,20.156322356204864,0.82236842105263153,0.45312374955922724,0.35481407661827696,2.7681660899653977,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.37003032052803037,0.5264024895883771,4.4403638463363642,12.633659750121049,8.0428375942915373,448.73118547615752,363.76040743163765,3499.3751194923539,5.4962565284357029E-2,11.478417209983911,-48914.749335880762,844.72056596793539,1.9514947014241491E-2,2.7090354302651107,-50699.861662040414,1543.9162489328428,8.4035156614431319,1.9339312304181941E-2,2.5927638955649051,-50708.706478734151,1553.6289277074748]
["KBM","KBM-35H03-A (240 V)",21.8,10.199999999999999,19.644267261628229,8.9292123916491946,1400,76.099999999999994,1818,1.41,12,132,3.04,325,10,844.72056596793539,1528.7946957043682,1707.5757575757575,19.445948017300704,0.82236842105263153,0.44967216601214716,0.35481407661827696,1.5447704128047006,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.37003032052803037,0.5264024895883771,4.4403638463363642,12.633659750121049,8.0428375942915373,448.73118547615752,363.76040743163765,3499.3751194923539,5.4962565284357029E-2,11.478417209983911,-48914.749335880762,844.72056596793539,1.9798142449723253E-2,2.8866661383237511,-50685.600177425607,1528.7946957043682,8.9545318720276992,1.9339312304181941E-2,2.5927638955649051,-50708.706478734151,1553.6289277074748]
["KBM","KBM-35H03-A (400 V)",21.8,10.199999999999999,17.188733853924695,7.8130608426930426,2550,76.099999999999994,3029,1.41,12,132,3.04,565,10,844.72056596793539,1529.8727028452781,1707.5757575757575,19.033470508848961,0.82236842105263153,0.45227069789586838,0.35481407661827696,1.5447704128047006,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.37003032052803037,0.5264024895883771,4.4403638463363642,12.633659750121049,8.0428375942915373,448.73118547615752,363.76040743163765,3499.3751194923539,5.4962565284357029E-2,11.478417209983911,-48914.749335880762,844.72056596793539,1.9777560945865934E-2,2.8741266101405021,-50686.636644698156,1529.8727028452781,8.9156338493965492,1.9339312304181941E-2,2.5927638955649051,-50708.706478734151,1553.6289277074748]
["KBM","KBM-35H03-A (480 V)",21.8,10.199999999999999,15.586916362161105,7.0849619828005022,3100,76.099999999999994,3635,1.41,12,132,3.04,679,10,844.72056596793539,1532.4823235531294,1707.5757575757575,18.728567467824103,0.82236842105263153,0.45418523300524427,0.35481407661827696,1.5447704128047006,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.37003032052803037,0.5264024895883771,4.4403638463363642,12.633659750121049,8.0428375942915373,448.73118547615752,363.76040743163765,3499.3751194923539,5.4962565284357029E-2,11.478417209983911,-48914.749335880762,844.72056596793539,1.9727987234651332E-2,2.8436962509883994,-50689.133135217438,1532.4823235531294,8.8212378895426724,1.9339312304181941E-2,2.5927638955649051,-50708.706478734151,1553.6289277074748]
["KBM","KBM-35H03-B (120 V)",21.7,14,19.629109648000426,12.345351979874481,900,76.599999999999994,1197,0.75,6.2,96.2,3.04,160,10,1197,1197,1197,18.945715831840566,0.82236842105263153,0.45932939129858225,0.35249805784139526,2.0050125313283207,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.5102252364017118,0.72584277501749661,6.1227028368205412,17.42022660041992,11.090060692951015,448.73118547615752,363.76040743163765,3499.3751194923539,2.8557938666551951E-2,6.1758115339889281,-49774.826233090535,1216.4980246718101,1.0119951450595022E-2,1.3077129613023062,-50758.962899225728,2175.9041265250921,10.464427307424105,1.0226537291041296E-2,1.3858967799902664,-50753.273827395627,2161.0269743539075]
["KBM","KBM-35H03-B (240 V)",21.7,14,17.910753839658661,11.264625056389095,2050,76.599999999999994,2504,0.75,6.2,96.2,3.04,325,10,1216.4980246718101,2152.6859033033911,2343.0353430353434,17.720947905603268,0.82236842105263153,0.45483049796925829,0.35249805784139526,1.1105830831739338,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.5102252364017118,0.72584277501749661,6.1227028368205412,17.42022660041992,11.090060692951015,448.73118547615752,363.76040743163765,3499.3751194923539,2.8557938666551951E-2,6.1758115339889281,-49774.826233090535,1216.4980246718101,1.0287764943078589E-2,1.4288757828049399,-50750.005771254495,2152.6859033033911,11.433982229258064,1.0226537291041296E-2,1.3858967799902664,-50753.273827395627,2161.0269743539075]
["KBM","KBM-35H03-B (400 V)",21.7,14,13.105153077224749,8.2422346397639927,3800,76.599999999999994,4173,0.75,6.2,96.2,3.04,565,10,1216.4980246718101,2161.1211450204332,2343.0353430353434,16.811972257099107,0.82236842105263153,0.45893632697127573,0.35249805784139526,1.1105830831739338,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.5102252364017118,0.72584277501749661,6.1227028368205412,17.42022660041992,11.090060692951015,448.73118547615752,363.76040743163765,3499.3751194923539,2.8557938666551951E-2,6.1758115339889281,-49774.826233090535,1216.4980246718101,1.0225852028374918E-2,1.3854082122513869,-50753.310403628595,2161.1211450204332,11.086151133483803,1.0226537291041296E-2,1.3858967799902664,-50753.273827395627,2161.0269743539075]
["KBM","KBM-35H03-B (480 V)",21.7,14,10.26549382942725,6.4562854273127357,4800,76.599999999999994,5007,0.75,6.2,96.2,3.04,679,10,1216.4980246718101,2163.7280442737206,2343.0353430353434,16.545591317981422,0.82236842105263153,0.46014599836668485,0.35249805784139526,1.1105830831739338,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.5102252364017118,0.72584277501749661,6.1227028368205412,17.42022660041992,11.090060692951015,448.73118547615752,363.76040743163765,3499.3751194923539,2.8557938666551951E-2,6.1758115339889281,-49774.826233090535,1216.4980246718101,1.0206935425789503E-2,1.3718526566982863,-50754.320086626256,2163.7280442737206,10.977678456455422,1.0226537291041296E-2,1.3858967799902664,-50753.273827395627,2161.0269743539075]
["KBM","KBM-35H03-C (120 V)",20.7,20.2,18.044877685729375,17.185597795932736,1450,75.2,1813,0.36,2.8,63.6,3.04,160,10,1813,1813,1813,17.380181547743007,0.82236842105263153,0.47753846413944839,0.35906052168418717,1.3237727523441809,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.77174648076027041,1.0978810282994116,9.2609577691232445,26.34914467918588,16.774386487743779,448.73118547615752,363.76040743163765,3499.3751194923539,1.2726010844285641E-2,2.9101750186989843,-50281.723511168246,1876.683248046279,4.3630610066566142E-3,0.55707732326908055,-50785.979640731886,3348.4997656806599,14.047376945704046,4.4985545845454503E-3,0.66522243691418159,-50777.809859913694,3286.5760139034924]
["KBM","KBM-35H03-C (240 V)",20.7,20.2,14.724399251211478,14.023237382106169,3100,75.2,3783,0.36,2.8,63.6,3.04,325,10,1876.683248046279,3342.9475902452427,3544.0251572327047,14.256090282764433,0.82236842105263153,0.47858779279528535,0.35906052168418717,0.73024326528492522,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.77174648076027041,1.0978810282994116,9.2609577691232445,26.34914467918588,16.774386487743779,448.73118547615752,363.76040743163765,3499.3751194923539,1.2726010844285641E-2,2.9101750186989843,-50281.723511168246,1876.683248046279,4.3747464476843962E-3,0.56721715960824703,-50785.275050201119,3342.9475902452427,14.303065154996347,4.4985545845454503E-3,0.66522243691418159,-50777.809859913694,3286.5760139034924]
["KBM","KBM-35H03-C (400 V)",20.7,20.2,5.7009300615516914,5.4294572014778009,5000,75.2,6305,0.36,2.8,63.6,3.04,565,10,1876.683248046279,3401.4178785799973,3544.0251572327047,10.49637906985803,0.82236842105263153,0.49056552645592871,0.35906052168418717,0.73024326528492522,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.77174648076027041,1.0978810282994116,9.2609577691232445,26.34914467918588,16.774386487743779,448.73118547615752,363.76040743163765,3499.3751194923539,1.2726010844285641E-2,2.9101750186989843,-50281.723511168246,1876.683248046279,4.2565654997417622E-3,0.45435617414160295,-50792.400941011743,3401.4178785799973,11.457139214213091,4.4985545845454503E-3,0.66522243691418159,-50777.809859913694,3286.5760139034924]
["KBM","KBM-35H03-D (120 V)",20,21.5,17.188733853924695,17.904931097838226,1550,75.7,1996,0.32,2.2999999999999998,57.8,3.04,160,10,1996,1996,1996,16.379814691892705,0.82236842105263153,0.49477036808809799,0.35668891982365752,1.2024048096192386,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.8501628001543523,1.2094355238729038,10.201953601852228,29.02645257294969,18.478813629629627,448.73118547615752,363.76040743163765,3499.3751194923539,1.0543996780891933E-2,2.60701054511095,-50296.567551520006,2063.9405895319669,3.5519370258283631E-3,0.44629540080145519,-50790.255096983354,3719.1406985877197,13.931053730039581,3.7122574900041415E-3,0.59198749032084275,-50778.935368717423,3619.6007464009072]
["KBM","KBM-35H03-D (240 V)",20,21.5,13.298799803649256,13.852916462134642,3400,75.7,4166,0.32,2.2999999999999998,57.8,3.04,325,10,2063.9405895319669,3714.5062416948799,3899.6539792387548,12.678926483473003,0.82236842105263153,0.49660846585008417,0.35668891982365752,0.66305655461763346,27.001351230650876,0,-21.871094496827208,0,0,0,0,0,0.8501628001543523,1.2094355238729038,10.201953601852228,29.02645257294969,18.478813629629627,448.73118547615752,363.76040743163765,3499.3751194923539,1.0543996780891933E-2,2.60701054511095,-50296.567551520006,2063.9405895319669,3.5589424946228213E-3,0.45364034345369808,-50789.760462667415,3714.5062416948799,14.160325173457338,3.7122574900041415E-3,0.59198749032084275,-50778.935368717423,3619.6007464009072]
["KBM","KBM-35H04-A (120 V)",25.6,10.86,23.786429676643269,9.7485367527226519,550,92.3,778,1.35,11,147,3.81,160,10,778,778,778,23.034622342597206,0.65616797900262469,0.44831032611196064,0.33319877159593192,3.0848329048843186,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.38212292039040352,0.54360533573370284,4.5854750446848422,13.046528057608869,8.3056777222222227,511.0999603528075,414.31916442123344,3985.7503617322654,5.9753067325012302E-2,13.458705545314521,-48709.542954376884,797.25081375830359,2.3353641490252715E-2,2.8783452794923421,-50709.310220417705,1413.2185180100992,8.3739653410712638,2.3325303268109585E-2,2.8548730847367847,-50710.867108959763,1414.5456583431255]
["KBM","KBM-35H04-A (240 V)",25.6,10.86,22.612734314496489,9.2675140633182327,1250,92.3,1633,1.35,11,147,3.81,325,10,797.25081375830359,1394.9802415319041,1533.3333333333335,22.266258714013073,0.65616797900262469,0.44081748388741526,0.33319877159593192,1.6966578532439518,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.38212292039040352,0.54360533573370284,4.5854750446848422,13.046528057608869,8.3056777222222227,511.0999603528075,414.31916442123344,3985.7503617322654,5.9753067325012302E-2,13.458705545314521,-48709.542954376884,797.25081375830359,2.3757481830311865E-2,3.1941524044677023,-50687.123422845034,1394.9802415319041,9.2927425071913241,2.3325303268109585E-2,2.8548730847367847,-50710.867108959763,1414.5456583431255]
["KBM","KBM-35H04-A (400 V)",25.6,10.86,20.136560191191975,8.252688602947531,2300,92.3,2721,1.35,11,147,3.81,565,10,797.25081375830359,1391.477483174896,1533.3333333333335,22.294672402331425,0.65616797900262469,0.44070058674639312,0.33319877159593192,1.6966578532439518,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.38212292039040352,0.54360533573370284,4.5854750446848422,13.046528057608869,8.3056777222222227,511.0999603528075,414.31916442123344,3985.7503617322654,5.9753067325012302E-2,13.458705545314521,-48709.542954376884,797.25081375830359,2.3838075192890107E-2,3.2535100364082781,-50682.695661564518,1391.477483174896,9.4654315713351913,2.3325303268109585E-2,2.8548730847367847,-50710.867108959763,1414.5456583431255]
["KBM","KBM-35H04-A (480 V)",25.6,10.86,18.416500557776462,7.5477461302362556,2800,92.3,3266,1.35,11,147,3.81,679,10,797.25081375830359,1392.7110587860036,1533.3333333333335,22.026950316440068,0.65616797900262469,0.4422485973674905,0.33319877159593192,1.6966578532439518,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.38212292039040352,0.54360533573370284,4.5854750446848422,13.046528057608869,8.3056777222222227,511.0999603528075,414.31916442123344,3985.7503617322654,5.9753067325012302E-2,13.458705545314521,-48709.542954376884,797.25081375830359,2.3809581926142995E-2,3.2326490793862059,-50684.2610681839,1392.7110587860036,9.4047408222686926,2.3325303268109585E-2,2.8548730847367847,-50710.867108959763,1414.5456583431255]
["KBM","KBM-35H04-B (120 V)",25.9,13.3,23.708598419206478,11.795322596620139,725,93,948,0.9,7.6,122,3.81,160,10,948,948,948,23.034553519183092,0.65616797900262469,0.44056148126146294,0.33069082385273674,2.5316455696202533,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.46255683758372479,0.65803005151777694,5.5506820510046975,15.792721236426646,10.0539585985986,511.0999603528075,414.31916442123344,3985.7503617322654,4.1970652956830092E-2,9.0823407759937265,-49419.630001826154,982.30006368449688,1.6114264472895878E-2,1.9356167095968675,-50742.229805723087,1715.4713721687658,10.177858181545439,1.6084493678701128E-2,1.9120535886743504,-50743.752634272336,1717.7389634123183]
["KBM","KBM-35H04-B (240 V)",25.9,13.3,22.117403059351133,11.003683114105042,1550,93,1984,0.9,7.6,122,3.81,325,10,982.30006368449688,1698.77569460319,1847.5409836065576,21.754333067577626,0.65616797900262469,0.43589053798357513,0.33069082385273674,1.3971855160299551,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.46255683758372479,0.65803005151777694,5.5506820510046975,15.792721236426646,10.0539585985986,511.0999603528075,414.31916442123344,3985.7503617322654,4.1970652956830092E-2,9.0823407759937265,-49419.630001826154,982.30006368449688,1.6339742780307309E-2,2.105534896333241,-50730.696193233052,1698.77569460319,11.07132185051136,1.6084493678701128E-2,1.9120535886743504,-50743.752634272336,1717.7389634123183]
["KBM","KBM-35H04-B (400 V)",25.9,13.3,18.327948183424581,9.1183821808082506,2850,93,3307,0.9,7.6,122,3.81,565,10,982.30006368449688,1698.3676971462471,1847.5409836065576,21.387674313547631,0.65616797900262469,0.43761557555831854,0.33069082385273674,1.3971855160299551,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.46255683758372479,0.65803005151777694,5.5506820510046975,15.792721236426646,10.0539585985986,511.0999603528075,414.31916442123344,3985.7503617322654,4.1970652956830092E-2,9.0823407759937265,-49419.630001826154,982.30006368449688,1.6345389756531888E-2,2.1096147370263223,-50730.407340454876,1698.3676971462471,11.09277446546948,1.6084493678701128E-2,1.9120535886743504,-50743.752634272336,1717.7389634123183]
["KBM","KBM-35H04-B (480 V)",25.9,13.3,16.149545696089383,8.0345998488006884,3400,93,3968,0.9,7.6,122,3.81,679,10,982.30006368449688,1700.6926037962082,1847.5409836065576,21.022786612260678,0.65616797900262469,0.43930953198822442,0.33069082385273674,1.3971855160299551,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.46255683758372479,0.65803005151777694,5.5506820510046975,15.792721236426646,10.0539585985986,511.0999603528075,414.31916442123344,3985.7503617322654,4.1970652956830092E-2,9.0823407759937265,-49419.630001826154,982.30006368449688,1.6313298141186483E-2,2.0863229510742642,-50732.048883092932,1700.6926037962082,10.970301615839901,1.6084493678701128E-2,1.9120535886743504,-50743.752634272336,1717.7389634123183]
["KBM","KBM-35H04-C (120 V)",25.3,14.7,22.977994908892388,13.055678925507038,800,93,1080,0.73,6.1,107,3.81,160,10,1080,1080,1080,22.165293127004723,0.65616797900262469,0.45058430362345003,0.33069082385273674,2.2222222222222223,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.52337146653169941,0.74454450805183858,6.2804575983803925,17.869068193244125,11.375802125603864,511.0999603528075,414.31916442123344,3985.7503617322654,3.3788718806741905E-2,7.3104990884043923,-49638.171683955778,1108.6926798853096,1.2400311866245146E-2,1.5085844718894212,-50755.465111607438,1963.2218640588205,11.150706067605258,1.2439107240425653E-2,1.5390378275533054,-50753.438508283696,1959.0226329941277]
["KBM","KBM-35H04-C (240 V)",25.3,14.7,21.088029959676135,11.98183520436144,1800,93,2260,0.73,6.1,107,3.81,325,10,1108.6926798853096,1945.4068157994236,2106.5420560747662,20.747780430894988,0.65616797900262469,0.44586325684615707,0.33069082385273674,1.225100700512016,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.52337146653169941,0.74454450805183858,6.2804575983803925,17.869068193244125,11.375802125603864,511.0999603528075,414.31916442123344,3985.7503617322654,3.3788718806741905E-2,7.3104990884043923,-49638.171683955778,1108.6926798853096,1.2567767633986471E-2,1.6359805007345241,-50746.717511599629,1945.4068157994236,12.092354147843505,1.2439107240425653E-2,1.5390378275533054,-50753.438508283696,1959.0226329941277]
["KBM","KBM-35H04-C (400 V)",25.3,14.7,16.14699240823229,9.1744275046774373,3300,93,3766,0.73,6.1,107,3.81,565,10,1108.6926798853096,1950.8429174938979,2106.5420560747662,19.889066656312753,0.65616797900262469,0.44949395780181517,0.33069082385273674,1.225100700512016,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.52337146653169941,0.74454450805183858,6.2804575983803925,17.869068193244125,11.375802125603864,511.0999603528075,414.31916442123344,3985.7503617322654,3.3788718806741905E-2,7.3104990884043923,-49638.171683955778,1108.6926798853096,1.2515877998179374E-2,1.5975908173003031,-50749.428136528906,1950.8429174938979,11.808596702383872,1.2439107240425653E-2,1.5390378275533054,-50753.438508283696,1959.0226329941277]
["KBM","KBM-35H04-C (480 V)",25.3,14.7,11.206042017217307,6.3670693279643791,4150,93,4520,0.73,6.1,107,3.81,679,10,1108.6926798853096,1961.6972221313283,2106.5420560747662,18.637812476226394,0.65616797900262469,0.45481027412213415,0.33069082385273674,1.225100700512016,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.52337146653169941,0.74454450805183858,6.2804575983803925,17.869068193244125,11.375802125603864,511.0999603528075,414.31916442123344,3985.7503617322654,3.3788718806741905E-2,7.3104990884043923,-49638.171683955778,1108.6926798853096,1.2414348855613594E-2,1.5196736009905196,-50754.731843533336,1961.6972221313283,11.232671394344443,1.2439107240425653E-2,1.5390378275533054,-50753.438508283696,1959.0226329941277]
["KBM","KBM-35H04-D (120 V)",24.7,19.2,21.838826104261813,16.544565230501373,1150,91.5,1443,0.43,3.4,80,3.81,160,10,1443,1443,1443,21.109848755173736,0.65616797900262469,0.4584738534413868,0.33611198489950295,1.6632016632016633,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.70019257920195621,0.99608895929731245,8.402310950423475,23.906135023135498,15.219118236617186,511.0999603528075,414.31916442123344,3985.7503617322654,1.842450150702819E-2,4.2378388639899969,-50103.625693861562,1538.0607915377375,6.8523671680789603E-3,0.82197089025594117,-50778.767963108279,2662.8881176600112,13.795497521956513,6.9505481710470923E-3,0.90679383950833437,-50773.039880180855,2638.3125909202363]
["KBM","KBM-35H04-D (240 V)",24.7,19.2,18.65932552809381,14.13585267279834,2500,91.5,3015,0.43,3.4,80,3.81,325,10,1538.0607915377375,2651.5927657377051,2817.5,18.293036508046846,0.65616797900262469,0.45784504550308153,0.33611198489950295,0.90967234445971634,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.70019257920195621,0.99608895929731245,8.402310950423475,23.906135023135498,15.219118236617186,511.0999603528075,414.31916442123344,3985.7503617322654,1.842450150702819E-2,4.2378388639899969,-50103.625693861562,1538.0607915377375,6.8969165776905442E-3,0.86149476284299809,-50776.168858343524,2651.5927657377051,14.458843989327262,6.9505481710470923E-3,0.90679383950833437,-50773.039880180855,2638.3125909202363]
["KBM","KBM-35H04-D (400 V)",24.7,19.2,10.111019914073351,7.6598635712676897,4250,91.5,5025,0.43,3.4,80,3.81,565,10,1538.0607915377375,2678.5802802892445,2817.5,15.505234266424562,0.65616797900262469,0.46692244856647641,0.33611198489950295,0.90967234445971634,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.70019257920195621,0.99608895929731245,8.402310950423475,23.906135023135498,15.219118236617186,511.0999603528075,414.31916442123344,3985.7503617322654,1.842450150702819E-2,4.2378388639899969,-50103.625693861562,1538.0607915377375,6.7921574168157851E-3,0.76531656833161232,-50782.280724618642,2678.5802802892445,12.844643219230727,6.9505481710470923E-3,0.90679383950833437,-50773.039880180855,2638.3125909202363]
["KBM","KBM-35H04-E (120 V)",24.7,20.7,22.042959618227506,17.776580337280247,1200,92.1,1536,0.37,2.8,75,3.81,160,10,1536,1536,1536,21.298988311331208,0.65616797900262469,0.45608232791621067,0.33392233027475049,1.5625,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.75489512445210905,1.0739084092424147,9.058741493425309,25.773801821817955,16.408111848852904,511.0999603528075,414.31916442123344,3985.7503617322654,1.5228744898188632E-2,3.7098524518699181,-50193.470879349101,1697.7575592320368,5.9685492522624731E-3,0.70166664701121984,-50783.278396287649,2858.7416502983324,14.598465857056212,6.0590020554288932E-3,0.78864621375299027,-50777.51720664592,2830.5616730155771]
["KBM","KBM-35H04-E (240 V)",24.7,20.7,18.657856405542191,15.046658391566282,2600,92.1,3208,0.37,2.8,75,3.81,325,10,1697.7575592320368,2848.7353950153893,3005.333333333333,18.07981987719328,0.65616797900262469,0.45703759823713308,0.33392233027475049,0.84788825584680783,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.75489512445210905,1.0739084092424147,9.058741493425309,25.773801821817955,16.408111848852904,511.0999603528075,414.31916442123344,3985.7503617322654,1.5228744898188632E-2,3.7098524518699181,-50193.470879349101,1697.7575592320368,6.0001059279082489E-3,0.7331845305496828,-50781.268464185006,2848.7353950153893,15.254208507334369,6.0590020554288932E-3,0.78864621375299027,-50777.51720664592,2830.5616730155771]
["KBM","KBM-35H04-E (400 V)",24.7,20.7,6.8402026628842849,5.5162924700679721,4600,92.1,5347,0.37,2.8,75,3.81,565,10,1697.7575592320368,2890.0138037304619,3005.333333333333,13.479334600849356,0.65616797900262469,0.47105595122356198,0.33392233027475049,0.84788825584680783,30.754246618304517,0,-24.910939760826658,0,0,0,0,0,0.75489512445210905,1.0739084092424147,9.058741493425309,25.773801821817955,16.408111848852904,511.0999603528075,414.31916442123344,3985.7503617322654,1.5228744898188632E-2,3.7098524518699181,-50193.470879349101,1697.7575592320368,5.8741866991641771E-3,0.59758372088385781,-50789.288608734874,2890.0138037304619,12.432977373536342,6.0590020554288932E-3,0.78864621375299027,-50777.51720664592,2830.5616730155771]
["KBM","KBM-45H01-A (120 V)",30.7,10.24,28.329579870357374,9.1979155423238232,450,118,617,1.36,21,187,6.1,160,10,479.53169465658493,617,617,27.449890622245555,0.4098360655737705,0.5201748664798147,0.35521572016092134,3.8897893030794166,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.40949056661440358,0.5825383536710701,4.9138867993728432,13.980920488105683,8.9005304186270937,696.58631680414328,564.68222092275857,5432.2429652769379,0.1754392238223442,17.337430403901937,-48656.210265877329,479.53169465658493,4.0759937258039378E-2,3.5201974444966071,-50716.568747403129,1073.1241711247278,7.9914554190812712,4.2152380560281449E-2,3.9206405831289008,-50695.266790428119,1051.141702023848]
["KBM","KBM-45H01-A (240 V)",30.7,10.24,27.341143907997175,8.876994775323757,950,118,1293,1.36,21,187,6.1,325,10,479.53169465658493,1052.4571686788902,1205.3475935828876,26.978892449906173,0.4098360655737705,0.5061964470148923,0.35521572016092134,2.2832316474354375,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.40949056661440358,0.5825383536710701,4.9138867993728432,13.980920488105683,8.9005304186270937,696.58631680414339,564.68222092275857,5432.2429652769379,0.1754392238223442,17.337430403901937,-48656.210265877329,479.53169465658493,4.2066060005506556E-2,3.8970127987425323,-50696.587344551153,1052.4571686788902,8.8468912723710993,4.2152380560281449E-2,3.9206405831289008,-50695.266790428119,1051.141702023848]
["KBM","KBM-45H01-A (400 V)",30.7,10.24,24.99187334951591,8.1142445939986718,1750,118,2155,1.36,21,187,6.1,565,10,479.53169465658493,1047.2058019565332,1205.3475935828876,27.284238087605914,0.4098360655737705,0.50405472636920123,0.35521572016092134,2.2832316474354375,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.40949056661440358,0.5825383536710701,4.9138867993728432,13.980920488105683,8.9005304186270937,696.58631680414339,564.68222092275857,5432.2429652769379,0.1754392238223442,17.337430403901937,-48656.210265877329,479.53169465658493,4.2412967152124142E-2,3.9911202918014097,-50691.280269498493,1047.2058019565332,9.0605315147834293,4.2152380560281449E-2,3.9206405831289008,-50695.266790428119,1051.141702023848]
["KBM","KBM-45H01-A (480 V)",30.7,10.24,23.64587725936731,7.6772328764179578,2100,118,2586,1.36,21,187,6.1,679,10,479.53169465658493,1047.3409933308415,1205.3475935828876,27.181870515118135,0.4098360655737705,0.50481375737507006,0.35521572016092134,2.2832316474354375,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.40949056661440358,0.5825383536710701,4.9138867993728432,13.980920488105683,8.9005304186270937,696.58631680414339,564.68222092275857,5432.2429652769379,0.1754392238223442,17.337430403901937,-48656.210265877329,479.53169465658493,4.2403958722057919E-2,3.9887046032730966,-50691.418082786389,1047.3409933308415,9.0550474851274849,4.2152380560281449E-2,3.9206405831289008,-50695.266790428119,1051.141702023848]
["KBM","KBM-45H01-B (120 V)",30.2,12.5,27.738432938873189,11.184851991481125,525,118,763,0.92,14,150,6.1,160,10,597.25158995064908,763,763,26.622522537829035,0.4098360655737705,0.52459428306326339,0.35521572016092134,3.145478374836173,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.50814234833621363,0.72287967334072711,6.0977081800345632,17.349112160177452,11.044787834191807,696.58631680414339,564.68222092275857,5432.2429652769379,0.11863570911371593,11.674137148365727,-49290.876909346087,597.25158995064908,2.6081583394117362E-2,2.253304883711269,-50748.744634456038,1352.3798138490158,9.4271462404130411,2.7416197648191479E-2,2.6399584488941588,-50727.722437645694,1312.9568847770499]
["KBM","KBM-45H01-B (240 V)",30.2,12.5,26.101410667070837,10.52476236575437,1200,118,1596,0.92,14,150,6.1,325,10,{"$f":"IF(AQ928<I928,IF(AQ928<0,0,AQ928),I928)","v":597.25158995064908},{"$f":"IF(AU928<I928,IF(AU928<0,0,AU928),I928)","v":1326.9262066387062},{"$f":"IF(UAC_V*0.98/L928*1000<I928,IF(UAC_V*0.98/L928*1000<0,0,UAC_V*0.98/L928*1000),I928)","v":1502.6666666666665},{"$f":"C928+(E928-C928)/G928*Q928","v":25.667895336572034},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M928,(inertia/gear^2+gear_inertia)/M928),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M928,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M928))","v":0.4098360655737705},{"$f":"IF((C928+(E928-C928)/G928*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X928^2*time1+Y928^2*time2+Z928^2*time3+AA928^2*time4)/time)/(C928+(E928-C928)/G928*mspeed),SQRT((((X928-Y928)*2/PI()+Y928)^2*time1+Y928^2*time2+((Z928-Y928)*2/PI()+Y928)^2*time3+AA928^2*time4)/time)/(C928+(E928-C928)/G928*mspeed)),IF(AccType=1,SQRT((X928^2*time1+Y928^2*time2+Z928^2*time3+AA928^2*time4+AB928^2*time5+AC928^2*time6+AD928^2*time7+AE928^2*time8)/time)/(C928+(E928-C928)/G928*mspeed),SQRT((((X928-Y928)*2/PI()+Y928)^2*time1+Y928^2*time2+((Z928-Y928)*2/PI()+Y928)^2*time3+AA928^2*time4+((AB928-AC928)*2/PI()+AC928)^2*time5+AC928^2*time6+((AD928-AC928)*2/PI()+AC928)^2*time7+AE928^2*time8)/time)/(C928+(E928-C928)/G928*mspeed))))","v":0.51406990861466173},{"$f":"IF(move1,MAX(ABS(X928),ABS(Z928))/H928,MAX(ABS(X928),ABS(Z928),ABS(AB928),ABS(AD928))/H928)","v":0.35521572016092134},{"$f":"IF(AZ928>0,speed/(MIN(AZ928,I928)),\"NA\")","v":1.8279351194441835},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M928+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M928+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":41.91545497898872},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M928+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M928+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-33.951518532980856},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M928+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M928+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M928+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M928+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH928/Irms","v":0.50814234833621363},{"$f":"AI928/Ipeak","v":0.72287967334072711},{"$f":"IF(move1,IF(AccType=1,SQRT((X928^2*time1+Y928^2*time2+Z928^2*time3+AA928^2*time4)/time)/(C928/D928),SQRT((((X928-Y928)*2/PI()+Y928)^2*time1+Y928^2*time2+((Z928-AA928)*2/PI()+AA928)^2*time3+AA928^2*time4)/time)/(C928/D928)),IF(AccType=1,SQRT((X928^2*time1+Y928^2*time2+Z928^2*time3+AA928^2*time4+AB928^2*time5+AC928^2*time6+AD928^2*time7+AE928^2*time8)/time)/(C928/D928),SQRT((((X928-Y928)*2/PI()+Y928)^2*time1+Y928^2*time2+((Z928-AA928)*2/PI()+AA928)^2*time3+AA928^2*time4+((AB928-AC928)*2/PI()+AC928)^2*time5+AC928^2*time6+((AD928-AE928)*2/PI()+AE928)^2*time7+AE928^2*time8)/time)/(C928/D928)))","v":6.0977081800345632},{"$f":"IF(move1,MAX(ABS(X928),ABS(Z928))/(C928/D928),MAX(ABS(X928),ABS(Z928),ABS(AB928),ABS(AD928))/(C928/D928))","v":17.349112160177452},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X928),ABS(Z928))/(C928/D928),MAX(ABS((X928-Y928)*2/PI()+Y928),ABS((Z928-Y928)*2/PI()+Y928))/(C928/D928)),IF(AccType=1,MAX(ABS(X928),ABS(Z928),ABS(AB928),ABS(AD928))/(C928/D928),MAX(ABS((X928-Y928)*2/PI()+Y928),ABS((Z928-Y928)*2/PI()+Y928),ABS((AB928-AC928)*2/PI()+AC928),ABS((AD928-AC928)*2/PI()+AC928))/(C928/D928)))","v":11.044787834191807},{"$f":"IF((C928+(E928-C928)/G928*mspeed)<0,\"NA\",U928*(C928+(E928-C928)/G928*mspeed)*mspeed/9.55)","v":696.58631680414339},{"$f":"IF(move1,IF(speed1>speed2,AM928/2*time1/time,AM928/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z928*-speed/30*PI(),((Z928-AA928)*2/PI()+AA928)*-speed/30*PI()),IF(AccType=1,X928*-speed/30*PI(),((X928-Y928)*2/PI()+Y928)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z928*-speed/30*PI(),((Z928-AA928)*2/PI()+AA928)*-speed/30*PI()),IF(AccType=1,X928*-speed/30*PI(),((X928-Y928)*2/PI()+Y928)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD928*-speed/30*PI(),((AD928-AE928)*2/PI()+AE928)*-speed/30*PI()),IF(AccType=1,AB928*-speed/30*PI(),((AB928-AC928)*2/PI()+AC928)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD928*-speed/30*PI(),((AD928-AE928)*2/PI()+AE928)*-speed/30*PI()),IF(AccType=1,AB928*-speed/30*PI(),((AB928-AC928)*2/PI()+AC928)*-speed/30*PI()),0)/2*time7/time)))","v":564.68222092275857},{"$f":"IF(move1,MAX(IF(AccType=1,Z928*-speed/30*PI(),((Z928-AA928)*2/PI()+AA928)*-speed/30*PI()),IF(AccType=1,X928*-speed/30*PI(),((X928-Y928)*2/PI()+Y928)*-speed/30*PI()),0),MAX(IF(AccType=1,Z928*-speed/30*PI(),((Z928-AA928)*2/PI()+AA928)*-speed/30*PI()),IF(AccType=1,X928*-speed/30*PI(),((X928-Y928)*2/PI()+Y928)*-speed/30*PI()),IF(AccType=1,AD928*-speed/30*PI(),((AD928-AE928)*2/PI()+AE928)*-speed/30*PI()),IF(AccType=1,AB928*-speed/30*PI(),((AB928-AC928)*2/PI()+AC928)*-speed/30*PI()),0))","v":5432.2429652769379},{"$f":"(L928^2)/1000000+((K928/1000)^2*(D928/C928*H928)^2*PI()*PI()*(O928/2)^2)/1200","v":0.11863570911371593},{"$f":"SQRT(3)*L928*J928*D928/C928*H928/1000","v":11.674137148365727},{"$f":"0.75*J928^2*(D928/C928*H928)^2-(UAC_V*0.98)^2","v":-49290.876909346087},{"$f":"-AO928/2/AN928+SQRT((AO928/2/AN928)^2-AP928/AN928)","v":597.25158995064908},{"$f":"(L928^2)/1000000+((K928/1000)^2*AV928^2*PI()*PI()*(O928/2)^2)/1200","v":2.6926995681427965E-2},{"$f":"SQRT(3)*L928*J928*AV928/1000","v":2.5051686787858269},{"$f":"0.75*J928^2*AV928^2-(UAC_V*0.98)^2","v":-50735.428109898123},{"$f":"-AS928/2/AR928+SQRT((AS928/2/AR928)^2-AT928/AR928)","v":1326.9262066387062},{"$f":"D928+(F928-D928)*((0.85*UAC_V-D928*J928)/L928*1000)/G928","v":10.480868196104467},{"$f":"(L928^2)/1000000+((K928/1000)^2*AJ928^2*PI()*PI()*(O928/2)^2)/1200","v":2.7416197648191479E-2},{"$f":"SQRT(3)*L928*J928*AJ928/1000","v":2.6399584488941588},{"$f":"0.75*J928^2*AJ928^2-(UAC_V*0.98)^2","v":-50727.722437645694},{"$f":"IF(((AX928/2/AW928)^2-AY928/AW928)>0,-AX928/2/AW928+SQRT((AX928/2/AW928)^2-AY928/AW928),-9999)","v":1312.9568847770499}]
["KBM","KBM-45H01-B (400 V)",30.2,12.5,23.09597313705644,9.3128923939743711,2150,118,2660,0.92,14,150,6.1,565,10,597.25158995064908,1321.9778421769961,1502.6666666666665,25.831922742771376,0.4098360655737705,0.51316999507222194,0.35521572016092134,1.8279351194441835,41.91545497898872,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-33.951518532980856,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.50814234833621363,0.72287967334072711,6.0977081800345632,17.349112160177452,11.044787834191807,696.58631680414328,564.68222092275857,5432.2429652769379,0.11863570911371593,11.674137148365727,-49290.876909346087,597.25158995064908,2.7098209603148116E-2,2.553152794580817,-50732.731231194717,1321.9778421769961,10.681619226329564,2.7416197648191479E-2,2.6399584488941588,-50727.722437645694,1312.9568847770499]
["KBM","KBM-45H01-B (480 V)",30.2,12.5,20.720171836492035,8.3549079985854977,2650,118,3192,0.92,14,150,6.1,679,10,597.25158995064908,1324.4550434025214,1502.6666666666665,25.462035388019853,0.4098360655737705,0.51538389094420123,0.35521572016092134,1.8279351194441835,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.50814234833621363,0.72287967334072711,6.0977081800345632,17.349112160177452,11.044787834191807,696.58631680414339,564.68222092275857,5432.2429652769379,0.11863570911371593,11.674137148365727,-49290.876909346087,597.25158995064908,2.7012215260138975E-2,2.5291659660443817,-50734.085772402257,1324.4550434025214,10.581265589282344,2.7416197648191479E-2,2.6399584488941588,-50727.722437645694,1312.9568847770499]
["KBM","KBM-45H01-C (120 V)",31.3,14.3,28.427521373798537,12.69085775616006,650,119,854,0.69,11,135,6.1,160,10,690.06011825454971,854,854,27.526005004959924,0.4098360655737705,0.5027240829529156,0.35223071410914891,2.810304449648712,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.5608852512523379,0.79791135010588221,6.7306230150280548,19.149872402541174,12.19118740977399,696.58631680414328,564.68222092275857,5432.2429652769379,9.1764589441662964E-2,8.7716672376422391,-49749.712179315145,690.06011825454971,2.1178724465777999E-2,1.7579500767345217,-50762.767839886277,1507.2380653410978,10.895898550988722,2.1922735931422216E-2,1.9669326712437472,-50752.089710106913,1477.3273594134248]
["KBM","KBM-45H01-C (240 V)",31.3,14.3,26.601611916788226,11.875719605709028,1400,119,1783,0.69,11,135,6.1,325,10,690.06011825454971,1483.712906364894,1669.6296296296296,26.320672115591197,0.4098360655737705,0.49462061969000992,0.35223071410914891,1.6245553057061934,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.5608852512523379,0.79791135010588221,6.7306230150280548,19.149872402541174,12.19118740977399,696.58631680414339,564.68222092275857,5432.2429652769379,9.1764589441662964E-2,8.7716672376422391,-49749.712179315145,690.06011825454971,2.1759408902453769E-2,1.9230029197534693,-50754.433796579149,1483.712906364894,11.918907711992507,2.1922735931422216E-2,1.9669326712437472,-50752.089710106913,1477.3273594134248]
["KBM","KBM-45H01-C (400 V)",31.3,14.3,22.23076245107594,9.9244475228017581,2500,119,2972,0.69,11,135,6.1,565,10,690.06011825454971,1484.3099827312062,1669.6296296296296,25.915376068148529,0.4098360655737705,0.49666651572427589,0.35223071410914891,1.6245553057061934,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.5608852512523379,0.79791135010588221,6.7306230150280548,19.149872402541174,12.19118740977399,696.58631680414339,564.68222092275857,5432.2429652769379,9.1764589441662964E-2,8.7716672376422391,-49749.712179315145,690.06011825454971,2.1744263003364156E-2,1.9188782020437625,-50754.651172094949,1484.3099827312062,11.893342420741508,2.1922735931422216E-2,1.9669326712437472,-50752.089710106913,1477.3273594134248]
["KBM","KBM-45H01-C (480 V)",31.3,14.3,18.621128341751753,8.3130037239963173,3100,119,3567,0.69,11,135,6.1,679,10,690.06011825454971,1490.1016224630982,1669.6296296296296,25.205546055175127,0.4098360655737705,0.50018647535526717,0.35223071410914891,1.6245553057061934,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.5608852512523379,0.79791135010588221,6.7306230150280548,19.149872402541174,12.19118740977399,696.58631680414328,564.68222092275857,5432.2429652769379,9.1764589441662964E-2,8.7716672376422391,-49749.712179315145,690.06011825454971,2.1598458333455972E-2,1.8787077315129486,-50756.743775851217,1490.1016224630982,11.644363011461429,2.1922735931422216E-2,1.9669326712437472,-50752.089710106913,1477.3273594134248]
["KBM","KBM-45H01-D (120 V)",29.7,20.2,26.335954793732576,17.326286048508273,950,118,1263,0.35,5,91.2,6.1,160,10,1048.7004131235039,1263,1263,25.227590425772888,0.4098360655737705,0.52425435559505629,0.35521572016092134,1.9002375296912113,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.83498224425326262,1.1878397735347532,10.019786931039151,28.508154564834079,18.148854869684495,696.58631680414328,564.68222092275857,5432.2429652769379,4.1426920880529877E-2,4.4371124731678089,-50213.3923677856,1048.7004131235039,9.3177884450733398E-3,0.7712583916681478,-50787.28071542691,2293.6265575984912,13.950070176828415,1.0010595993109312E-2,1.0033968603729171,-50774.898126773202,2202.576557623117]
["KBM","KBM-45H01-D (240 V)",29.7,20.2,22.804629703024432,15.003045857252916,2100,118,2635,0.35,5,91.2,6.1,325,10,1048.7004131235039,2270.0641660044325,2471.4912280701756,22.246222370240201,0.4098360655737705,0.52209327355971669,0.35521572016092134,1.089632953594099,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.83498224425326262,1.1878397735347532,10.019786931039151,28.508154564834079,18.148854869684495,696.58631680414351,564.68222092275857,5432.2429652769379,4.1426920880529877E-2,4.4371124731678089,-50213.3923677856,1048.7004131235039,9.487473219304883E-3,0.83411003830130548,-50784.247929819903,2270.0641660044325,15.08689395824022,1.0010595993109312E-2,1.0033968603729171,-50774.898126773202,2202.576557623117]
["KBM","KBM-45H01-D (400 V)",29.7,20.2,12.723792477454767,8.3709161035886623,3700,118,4392,0.35,5,91.2,6.1,565,10,1048.7004131235039,2300.8000233390912,2471.4912280701756,19.143551712410453,0.4098360655737705,0.53322611997852598,0.35521572016092134,1.089632953594099,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.83498224425326262,1.1878397735347532,10.019786931039151,28.508154564834079,18.148854869684495,696.58631680414328,564.68222092275857,5432.2429652769379,4.1426920880529877E-2,4.4371124731678089,-50213.3923677856,1048.7004131235039,9.2674453760484918E-3,0.75160088563732597,-50788.180499958798,2300.8000233390912,13.594516718229052,1.0010595993109312E-2,1.0033968603729171,-50774.898126773202,2202.576557623117]
["KBM","KBM-45H01-E (120 V)",31.2,23.4,27.345712949425653,19.960374415639162,1100,118,1394,0.26,3.2,82.7,6.1,160,10,1394,1394,1394,26.315567137726692,0.4098360655737705,0.49740600394365125,0.35521572016092134,1.7216642754662841,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.92075393518521886,1.3098579680933973,11.049047222222626,31.436591234241536,20.013155555555549,696.58631680414339,564.68222092275857,5432.2429652769379,2.3330214601692188E-2,3.2959662470946212,-50408.064925000006,1400.9686551999566,7.3944621436201289E-3,0.60474750594073823,-50791.791669883081,2580.2849494917887,16.238077171734723,7.6826045757259027E-3,0.74534107580751741,-50784.853311758758,2523.0130481108249]
["KBM","KBM-45H01-E (240 V)",31.2,23.4,23.167423890072417,16.910528386914173,2300,118,2909,0.26,3.2,82.7,6.1,325,10,1400.9686551999566,2570.180814292889,2725.5139056831922,22.223837823007269,0.4098360655737705,0.4973190135398331,0.35521572016092134,0.9512435941609837,41.91545497898872,0,-33.951518532980856,0,0,0,0,0,0.92075393518521886,1.3098579680933973,11.049047222222626,31.436591234241536,20.013155555555549,696.58631680414339,564.68222092275857,5432.2429652769379,2.3330214601692188E-2,3.2959662470946212,-50408.064925000006,1400.9686551999566,7.4433264022535153E-3,0.63080018008223715,-50790.615037467644,2570.180814292889,16.937617606517719,7.6826045757259027E-3,0.74534107580751741,-50784.853311758758,2523.0130481108249]
["KBM","KBM-45H02-A (120 V)",43.7,13.3,40.226411866476546,12.00788413924673,400,171,568,0.95,16,202,9.2200000000000006,160,10,471.75861347407425,568,568,38.767504850396691,0.27114967462039041,0.50471061305664611,0.33404673762664755,4.225352112676056,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.50919213240711414,0.7243730886577846,6.1103055888853692,17.38495412778683,11.067605539452495,949.3013526679722,769.54367781566657,7403.0101805867125,0.18337496924834726,17.298239926827986,-48971.828068289229,471.75861347407425,4.6470749084153162E-2,3.4486836413234689,-50732.290802997675,1008.3989870857157,10.37570833073457,4.725171477387205E-2,3.6786568160815487,-50722.248300347375,997.87806459039666]
["KBM","KBM-45H02-A (240 V)",43.7,13.3,38.46847317687061,11.483126321453913,880,171,1188,0.95,16,202,9.2200000000000006,325,10,471.75861347407425,992.25944653367333,1115.841584158416,37.801100102222236,0.27114967462039041,0.48949079374796334,0.33404673762664755,2.4051034742257196,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.50919213240711414,0.7243730886577846,6.1103055888853692,17.38495412778683,11.067605539452495,949.3013526679722,769.54367781566657,7403.0101805867125,0.18337496924834726,17.298239926827986,-48971.828068289229,471.75861347407425,4.7682013201227801E-2,3.7994249293404705,-50716.715057140886,992.25944653367333,11.430948440440311,4.725171477387205E-2,3.6786568160815487,-50722.248300347375,997.87806459039666]
["KBM","KBM-45H02-A (400 V)",43.7,13.3,34.85493253712508,10.40445747376868,1600,171,1980,0.95,16,202,9.2200000000000006,565,10,471.75861347407425,988.66035844987675,1115.841584158416,38.234520269775466,0.27114967462039041,0.48725517224084425,0.33404673762664755,2.4051034742257196,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.50919213240711414,0.7243730886577846,6.1103055888853692,17.38495412778683,11.067605539452495,949.3013526679722,769.54367781566657,7403.0101805867125,0.18337496924834726,17.298239926827986,-48971.828068289229,471.75861347407425,4.7962522526375923E-2,3.8761275825780945,-50713.107964437171,988.66035844987675,11.661716014668038,4.725171477387205E-2,3.6786568160815487,-50722.248300347375,997.87806459039666]
["KBM","KBM-45H02-A (480 V)",43.7,13.3,32.565549894187811,9.7210596699068095,1950,171,2376,0.95,16,202,9.2200000000000006,679,10,471.75861347407425,989.02339229579593,1115.841584158416,38.052701735898125,0.27114967462039041,0.48822794702947803,0.33404673762664755,2.4051034742257196,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.50919213240711414,0.7243730886577846,6.1103055888853692,17.38495412778683,11.067605539452495,949.3013526679722,769.54367781566657,7403.0101805867125,0.18337496924834726,17.298239926827986,-48971.828068289229,471.75861347407425,4.7934054675732467E-2,3.8684126565047201,-50713.474034892381,989.02339229579593,11.638504890930461,4.725171477387205E-2,3.6786568160815487,-50722.248300347375,997.87806459039666]
["KBM","KBM-45H02-B (120 V)",43.5,14.9,39.894839068368434,13.387529888714239,450,171,638,0.76,12,180,9.2200000000000006,160,10,557.13240006989486,638,638,38.388682945820136,0.27114967462039041,0.50339861584042378,0.33404673762664755,3.761755485893417,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.57307107972386861,0.815246822604344,6.8768529566864238,19.565923742504257,12.456053919114515,949.3013526679722,769.54367781566657,7403.0101805867125,0.13397977436369921,13.878414256467329,-49318.968778749113,557.13240006989486,3.6289237271611513E-2,2.7156165340823661,-50748.257429319594,1145.7313129837742,11.460979071405355,3.69939044627699E-2,2.951394096562213,-50737.947599435014,1131.9087964507733]
["KBM","KBM-45H02-B (240 V)",43.5,14.9,37.515093728803905,12.588957627115404,1050,171,1334,0.76,12,180,9.2200000000000006,325,10,557.13240006989486,1129.1917172487395,1252.2222222222224,37.063708009576509,0.27114967462039041,0.49055963242068706,0.33404673762664755,2.1203121731410417,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.57307107972386861,0.815246822604344,6.8768529566864238,19.565923742504257,12.456053919114515,949.3013526679722,769.54367781566657,7403.0101805867125,0.13397977436369921,13.878414256467329,-49318.968778749113,557.13240006989486,3.7136536454360783E-2,2.9968614605942676,-50735.860782299424,1129.1917172487395,12.647944232442363,3.69939044627699E-2,2.951394096562213,-50737.947599435014,1131.9087964507733]
["KBM","KBM-45H02-B (400 V)",43.5,14.9,32.769165125026028,10.996364135914774,1900,171,2223,0.76,12,180,9.2200000000000006,565,10,557.13240006989486,1127.0591717112945,1252.2222222222224,37.134586386337453,0.27114967462039041,0.49027778245827935,0.33404673762664755,2.1203121731410417,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.57307107972386861,0.815246822604344,6.8768529566864238,19.565923742504257,12.456053919114515,949.3013526679722,769.54367781566657,7403.0101805867125,0.13397977436369921,13.878414256467329,-49318.968778749113,557.13240006989486,3.7249432466540382E-2,3.0323664469678828,-50734.209025704506,1127.0591717112945,12.797789359930526,3.69939044627699E-2,2.951394096562213,-50737.947599435014,1131.9087964507733]
["KBM","KBM-45H02-B (480 V)",43.5,14.9,29.257419325829272,9.8179259482648558,2350,171,2667,0.76,12,180,9.2200000000000006,679,10,557.13240006989486,1128.6333311467222,1252.2222222222224,36.659722863653087,0.27114967462039041,0.49252009445606787,0.33404673762664755,2.1203121731410417,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.57307107972386861,0.815246822604344,6.8768529566864238,19.565923742504257,12.456053919114515,949.3013526679722,769.54367781566657,7403.0101805867125,0.13397977436369921,13.878414256467329,-49318.968778749113,557.13240006989486,3.7166016470976615E-2,3.0061731680795543,-50735.429466693822,1128.6333311467222,12.68724333202749,3.69939044627699E-2,2.951394096562213,-50737.947599435014,1131.9087964507733]
["KBM","KBM-45H02-C (120 V)",41.8,21.1,37.242256683503506,18.345939252957393,750,168,941,0.38,5.9,123,9.2200000000000006,160,10,816.6548455372232,941,941,36.081551385569064,0.27114967462039041,0.5140511277454779,0.34001185794140909,2.5504782146652496,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.84453500292950279,1.2014294597594768,10.134420035154033,28.834307034227443,18.356489980506822,949.3013526679722,769.54367781566657,7403.0101805867125,6.6603654677383994E-2,6.8653833220766289,-50026.300059504138,816.6548455372232,1.6849227101612949E-2,1.2550498107189336,-50779.13134596825,1699.167589429333,15.502852932498188,1.7540802907936338E-2,1.4860690078020764,-50768.667153547001,1659.4365606765571]
["KBM","KBM-45H02-C (240 V)",41.8,21.1,33.243488738319641,16.376102826758444,1600,168,1964,0.38,5.9,123,9.2200000000000006,325,10,816.6548455372232,1684.2634607386785,1832.520325203252,32.792862956595478,0.27114967462039041,0.50975360331733932,0.34001185794140909,1.4462740287109941,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.84453500292950279,1.2014294597594768,10.134420035154033,28.834307034227443,18.356489980506822,949.3013526679722,769.54367781566657,7403.0101805867125,6.6603654677383994E-2,6.8653833220766289,-50026.300059504138,816.6548455372232,1.7101270865780924E-2,1.3438517137153592,-50775.317686752998,1684.2634607386785,16.599767836211008,1.7540802907936338E-2,1.4860690078020764,-50768.667153547001,1659.4365606765571]
["KBM","KBM-45H02-C (400 V)",41.8,21.1,22.654882933908411,11.160040854142075,2900,168,3274,0.38,5.9,123,9.2200000000000006,565,10,816.6548455372232,1694.1594566655176,1832.520325203252,30.615558232245704,0.27114967462039041,0.5171891030913679,0.34001185794140909,1.4462740287109941,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.84453500292950279,1.2014294597594768,10.134420035154033,28.834307034227443,18.356489980506822,949.3013526679722,769.54367781566657,7403.0101805867125,6.6603654677383994E-2,6.8653833220766289,-50026.300059504138,816.6548455372232,1.6932930363397134E-2,1.285221417039321,-50777.864836889144,1694.1594566655176,15.875544097045879,1.7540802907936338E-2,1.4860690078020764,-50768.667153547001,1659.4365606765571]
["KBM","KBM-45H02-C (480 V)",41.8,21.1,12.34587629984274,6.0817124629767196,3500,168,3929,0.38,5.9,123,9.2200000000000006,679,10,816.6548455372232,1711.5710246249303,1832.520325203252,27.396335805454967,0.27114967462039041,0.52833581421866271,0.34001185794140909,1.4462740287109941,57.121992134156727,0,-46.268813628666948,0,0,0,0,0,0.84453500292950279,1.2014294597594768,10.134420035154033,28.834307034227443,18.356489980506822,949.3013526679722,769.54367781566657,7403.0101805867125,6.6603654677383994E-2,6.8653833220766289,-50026.300059504138,816.6548455372232,1.6646256994103024E-2,1.1786846936420958,-50782.202474601327,1711.5710246249303,14.559561941890365,1.7540802907936338E-2,1.4860690078020764,-50768.667153547001,1659.4365606765571]
["KBM","KBM-45H03-A (120 V)",54.6,14.1,50.202016335272141,12.67727685234145,350,218,480,0.93,16,240,12.2,160,10,420.09343880998574,480,480,48.568479545516077,0.20491803278688525,0.51468796390123794,0.32865222327242061,5,71.646184673387694,0,-58.033409585444033,0,0,0,0,0,0.54191063448289278,0.77091819589038957,6.5029276137947134,18.502036701369349,11.77876239316239,1190.676611281501,965.21263343773853,9285.3455336710449,0.22442625491965246,21.763953091181758,-48749.302126062677,420.09343880998574,6.3981788594328931E-2,4.2567366993775222,-50726.515002917418,857.76450527617283,11.010878491285714,6.4902941058108121E-2,4.5535958090813091,-50715.163321213186,849.5841253362654]
["KBM","KBM-45H03-A (240 V)",54.6,14.1,47.7464829275686,12.05719265847692,800,218,1005,0.93,16,240,12.2,325,10,420.09343880998574,845.45340929537463,939.16666666666674,47.357088281811023,0.20491803278688525,0.49636873093829259,0.32865222327242061,2.8249115401609934,71.646184673387694,0,-58.033409585444033,0,0,0,0,0,0.54191063448289278,0.77091819589038957,6.5029276137947134,18.502036701369349,11.77876239316239,1190.676611281501,965.21263343773853,9285.3455336710449,0.22442625491965246,21.763953091181758,-48749.302126062677,420.09343880998574,6.5382656457737678E-2,4.7007755050305633,-50709.25162175046,845.45340929537463,12.159471340633489,6.4902941058108121E-2,4.5535958090813091,-50715.163321213186,849.5841253362654]
["KBM","KBM-45H03-A (400 V)",54.6,14.1,43.688031878725276,11.032331282506384,1400,218,1676,0.93,16,240,12.2,565,10,420.09343880998574,842.43721267173737,939.16666666666674,48.033822850821764,0.20491803278688525,0.49297843113408163,0.32865222327242061,2.8249115401609934,71.646184673387694,0,-58.033409585444033,0,0,0,0,0,0.54191063448289278,0.77091819589038957,6.5029276137947134,18.502036701369349,11.77876239316239,1190.676611281501,965.21263343773853,9285.3455336710449,0.22442625491965246,21.763953091181758,-48749.302126062677,420.09343880998574,6.5739111114154175E-2,4.8072207952014292,-50704.858907231697,842.43721267173737,12.434812814352654,6.4902941058108121E-2,4.5535958090813091,-50715.163321213186,849.5841253362654]
["KBM","KBM-45H03-A (480 V)",54.6,14.1,40.837285986285153,10.312445956132615,1700,218,2011,0.93,16,240,12.2,679,10,420.09343880998574,842.74446721172285,939.16666666666674,47.777381712426219,0.20491803278688525,0.49429566839991601,0.32865222327242061,2.8249115401609934,71.646184673387694,0,-58.033409585444033,0,0,0,0,0,0.54191063448289278,0.77091819589038957,6.5029276137947134,18.502036701369349,11.77876239316239,1190.676611281501,965.21263343773853,9285.3455336710449,0.22442625491965246,21.763953091181758,-48749.302126062677,420.09343880998574,6.5702561246474944E-2,4.7964148864867981,-50705.309323943962,842.74446721172285,12.406861226963626,6.4902941058108121E-2,4.5535958090813091,-50715.163321213186,849.5841253362654]
["KBM","KBM-45H03-B (120 V)",53,19.899999999999999,49.482718670389282,18.125537974501569,550,216,699,0.47,7.7,165,12.2,160,10,631.50799271040523,699,699,48.529855182912925,0.20491803278688525,0.50250284199903161,0.33169529941383191,3.4334763948497855,71.646184673387694,0,-58.033409585444033,0,0,0,0,0,0.78791326213173063,1.1208797759437223,9.4549591455807676,26.901114622649338,17.125781467505238,1190.676611281501,965.21263343773853,9285.3455336710449,0.10741161384298485,10.893649239278348,-49715.430029858318,631.50799271040523,3.0448237839317795E-2,2.1840804263589897,-50761.356443445322,1255.8088089125165,16.260211761317287,3.0800532699934755E-2,2.3003442168116952,-50756.56878314216,1246.9106858769353]
["KBM","KBM-45H03-B (240 V)",53,19.899999999999999,45.50447416401321,16.668305554583593,1150,216,1459,0.47,7.7,165,12.2,325,10,631.50799271040523,1251.007800616648,1366.0606060606062,44.846120616919045,0.20491803278688525,0.50305946194186801,0.33169529941383191,1.9247569430460953,71.646184673387694,0,-58.033409585444033,0,0,0,0,0,0.78791326213173063,1.1208797759437223,9.4549591455807676,26.901114622649338,17.125781467505238,1190.6766112815008,965.21263343773853,9285.3455336710449,0.10741161384298485,10.893649239278348,-49715.430029858318,631.50799271040523,3.0637044428291536E-2,2.2471382337896437,-50758.790576292391,1251.007800616648,16.72966942855901,3.0800532699934755E-2,2.3003442168116952,-50756.56878314216,1246.9106858769353]
["KBM","KBM-45H03-B (400 V)",53,19.899999999999999,33.533576381687716,12.283361311973522,2150,216,2432,0.47,7.7,165,12.2,565,10,631.50799271040523,1259.4171223184646,1366.0606060606062,41.59704780688044,0.20491803278688525,0.51483888212851137,0.33169529941383191,1.9247569430460953,71.646184673387694,0,-58.033409585444033,0,0,0,0,0,0.78791326213173063,1.1208797759437223,9.4549591455807676,26.901114622649338,17.125781467505238,1190.6766112815008,965.21263343773853,9285.3455336710449,0.10741161384298485,10.893649239278348,-49715.430029858318,631.50799271040523,3.0308306886185656E-2,2.1361454810693878,-50763.258094432575,1259.4171223184646,15.903341953882833,3.0800532699934755E-2,2.3003442168116952,-50756.56878314216,1246.9106858769353]
["KBM","KBM-45H03-B (480 V)",53,19.899999999999999,24.699622899069141,9.0474809154099418,2600,216,2918,0.47,7.7,165,12.2,679,10,631.50799271040523,1266.5079289798316,1366.0606060606062,39.21436461867377,0.20491803278688525,0.52368949413148602,0.33169529941383191,1.9247569430460953,71.646184673387694,0,-58.033409585444033,0,0,0,0,0,0.78791326213173063,1.1208797759437223,9.4549591455807676,26.901114622649338,17.125781467505238,1190.676611281501,965.21263343773853,9285.3455336710449,0.10741161384298485,10.893649239278348,-49715.430029858318,631.50799271040523,3.0038275754119954E-2,2.0404624264551954,-50766.92779693503,1266.5079289798316,15.190993309931969,3.0800532699934755E-2,2.3003442168116952,-50756.56878314216,1246.9106858769353]
["KBM","KBM-43H01-A (400 V)",6.12,5.12,4.82490774847009,3.9875270648513141,4750,18,5478,2.9,6.8,72.8,1.94,565,16,1896.8785658498336,2816.8139686512054,3096.1538461538462,5.3519928537260233,1.2886597938144331,1.2683017384402895,1.2022262280795213,1.0981561190806715,21.640072105431383,0,-17.528458405399419,0,0,0,0,0,0.53025573941780768,0.7543380254616604,6.3630688730136926,18.104112611079849,11.525436049382712,359.63293565237166,291.53361173221487,2804.5533448639071,1.0819322829054226E-2,5.5065685307322925,-49374.819792387549,1896.8785658498336,5.7989557818424724E-3,1.6558939002490234,-50675.817198666286,2816.8139686512054,4.5283762270662802,8.5330285295826536E-3,4.2145127292674687,-49967.298972820055,2185.4816071226519]
["KBM","KBM-43H02-A (400 V)",11.6,5.12,9.9780405138429078,4.3194980579406526,2450,34.5,2866,3.55,12,139,2.85,565,16,984.94694917748541,1459.5207812695735,1621.5827338129495,10.63376180554139,0.8771929824561403,0.81096075705361348,0.75580614808759561,1.7928489719280585,26.07531210902205,0,-21.12100280830786,0,0,0,0,0,0.33709291356045862,0.47954596982109515,4.0451149627255036,11.509103275706284,7.3269227075351191,433.34148777932177,351.28486999264641,3379.3604493292582,3.6897123643143917E-2,13.014720551425221,-48613.465069203332,984.94694917748541,2.0997656441988408E-2,4.019715707631188,-50596.085490784943,1459.5207812695735,4.7031795437564767,2.3390154556238024E-2,6.2621777506190694,-50297.747467259091,1338.6515192180418]
["KBM","KBM-43H02-A (480 V)",11.6,5.12,6.8754935415698784,2.9764041305497306,3000,34.5,3439,3.55,12,139,2.85,679,16,984.94694917748541,1480.8192652450364,1621.5827338129495,9.2679532725273592,0.8771929824561403,0.84165894882282954,0.75580614808759561,1.7928489719280585,26.07531210902205,0,-21.12100280830786,0,0,0,0,0,0.33709291356045862,0.47954596982109515,4.0451149627255036,11.509103275706284,7.3269227075351191,433.34148777932177,351.28486999264641,3379.3604493292582,3.6897123643143917E-2,13.014720551425221,-48613.465069203332,984.94694917748541,2.0663480418773313E-2,3.59689100587434,-50637.75633419415,1480.8192652450364,4.2084628442340541,2.3390154556238024E-2,6.2621777506190694,-50297.747467259091,1338.6515192180418]
["KBM","KBM-43H03-A (400 V)",21,4.78,18.636530433018713,4.2068917456024186,1240,64.5,1491,4.83,19,268,4.75,565,16,516.13441815621945,752.96615612258472,841.04477611940297,19.564828552449509,0.52631578947368418,0.61667788928804523,0.5478403616327171,3.2505455961300673,35.335703325310256,0,-28.621919693501308,0,0,0,0,0,0.23557569305163359,0.33512829741068062,2.826908316619603,8.0430791378563349,5.1203832098765432,587.23846474767902,476.04024438255817,4579.5071509602094,0.11278233636413708,32.916289147443393,-47033.850649232503,516.13441815621945,7.5642368385846689E-2,10.050290784184755,-50453.577155662912,752.96615612258472,4.4826628423743733,7.6806078943665701E-2,11.480082708709491,-50346.426502148272,738.33758949799585]
["KBM","KBM-43H03-A (480 V)",21,4.78,16.182532804310163,3.652941942282204,1490,64.5,1790,4.83,19,268,4.75,679,16,516.13441815621945,757.24208613911549,841.04477611940297,18.551685295858437,0.52631578947368418,0.63559159105707541,0.5478403616327171,3.2505455961300673,35.335703325310256,0,-28.621919693501308,0,0,0,0,0,0.23557569305163359,0.33512829741068062,2.826908316619603,8.0430791378563349,5.1203832098765432,587.2384647476789,476.04024438255817,4579.5071509602094,0.11278233636413708,32.916289147443393,-47033.850649232503,516.13441815621945,7.5326703404229728E-2,9.625901132897086,-50482.642552418729,757.24208613911549,4.2933752126563274,7.6806078943665701E-2,11.480082708709491,-50346.426502148272,738.33758949799585]
["KBM","KBM-43S01-A (240 V)",6.12,5.12,4.9618894022767375,4.1007350432039154,2550,18,3284,2.9,6.8,72.8,1.94,325,16,1896.8785658498336,2849.3683876121727,3096.1538461538462,4.825927950387725,1.2886597938144331,1.2858764862873771,1.2022262280795213,1.0981561190806715,21.640072105431383,0,-17.528458405399419,0,0,0,0,0,0.53025573941780768,0.7543380254616604,6.3630688730136926,18.104112611079849,11.525436049382712,359.63293565237166,291.53361173221487,2804.5533448639071,1.0819322829054226E-2,5.5065685307322925,-49374.819792387549,1896.8785658498336,5.7146233570454646E-3,1.5095326688220665,-50697.671430616727,2849.3683876121727,4.1281218865808755,8.5330285295826536E-3,4.2145127292674687,-49967.298972820055,2185.4816071226519]
["KBM","KBM-43S02-A (240 V)",11.6,5.12,10.136945606160719,4.3882881411951162,1300,34.5,1717,3.55,12,139,2.85,325,16,984.94694917748541,1472.5696565426545,1621.5827338129495,9.9427311490468213,0.8771929824561403,0.82626001950356509,0.75580614808759561,1.7928489719280585,26.07531210902205,0,-21.12100280830786,0,0,0,0,0,0.33709291356045862,0.47954596982109515,4.0451149627255036,11.509103275706284,7.3269227075351191,433.34148777932177,351.28486999264641,3379.3604493292582,3.6897123643143917E-2,13.014720551425221,-48613.465069203332,984.94694917748541,2.078976691404967E-2,3.7622680842141545,-50622.00875087345,1472.5696565426545,4.401958640560502,2.3390154556238024E-2,6.2621777506190694,-50297.747467259091,1338.6515192180418]
["KBM","KBM-43S03-A (240 V)",21,4.78,18.813539541609121,4.2468486549907727,670,64.5,893,4.83,19,268,4.75,325,16,516.13441815621945,757.81117804089718,841.04477611940297,18.526978842219354,0.52631578947368418,0.63603510665326668,0.5478403616327171,3.2505455961300673,35.335703325310256,0,-28.621919693501308,0,0,0,0,0,0.23557569305163359,0.33512829741068062,2.826908316619603,8.0430791378563349,5.1203832098765432,587.2384647476789,476.04024438255817,4579.5071509602094,0.11278233636413708,32.916289147443393,-47033.850649232503,516.13441815621945,7.52855363974477E-2,9.5691677022271637,-50486.433075457557,757.81117804089718,4.2680707864416467,7.6806078943665701E-2,11.480082708709491,-50346.426502148272,738.33758949799585]
["KBM","KBM-57H01-A (400 V)",18.8,5.67,13.222102964557459,3.9468964073305846,1625,46.1,1975,3.39,13,203,6.56,565,24,687.34108812770512,992.00408804281051,1110.344827586207,15.394894361944079,0.38109756097560976,0.89971348336014623,0.95786213517035201,2.7792411180420324,44.157444431353227,0,-35.76752998939611,0,0,0,0,0,0.3900652630814096,0.5549040556865531,4.6807831569769149,13.317697336477275,8.4783094468085078,733.84558491227187,594.88615366978979,5722.8047983033775,7.9900891930766382E-2,16.572289009537378,-49139.014479509133,687.34108812770512,4.5723503212507274E-2,5.6607959257214659,-50610.757014531628,992.00408804281051,4.7492073928576151,5.5596529377508655E-2,10.105681980887608,-50185.60596872749,863.54508229598775]
["KBM","KBM-57H01-A (480 V)",18.8,5.67,10.713844949600761,3.1981626715226152,2050,46.1,2370,3.39,13,203,6.56,679,24,687.34108812770512,996.0959010546236,1110.344827586207,14.870933706831792,0.38109756097560976,0.91193389696009519,0.95786213517035201,2.7792411180420324,44.157444431353227,0,-35.76752998939611,0,0,0,0,0,0.3900652630814096,0.5549040556865531,4.6807831569769149,13.317697336477275,8.4783094468085078,733.84558491227187,594.88615366978979,5722.8047983033775,7.9900891930766382E-2,16.572289009537378,-49139.014479509133,687.34108812770512,4.548664755345045E-2,5.5102970941131817,-50620.956463967872,996.0959010546236,4.6229442007077584,5.5596529377508655E-2,10.105681980887608,-50185.60596872749,863.54508229598775]
["KBM","KBM-57H02-A (400 V)",33.5,5.22,26.795904964199107,4.1479729046747842,825,115,1023,4.4000000000000004,22,390,11.8,565,24,299.64593763009827,513.69061511031191,577.9487179487179,29.325659754304787,0.21186440677966101,0.82118288598909128,0.60605764024220299,5.0609816227609254,69.696628627853343,0,-56.454269188561206,0,0,0,0,0,0.31808676730688817,0.45250796198680904,3.8170412076826579,10.860191087683416,6.9138123781094514,1158.2772477092153,938.94834409249427,9032.6830701697945,0.33616593689141883,53.260034962049318,-46142.715351481398,299.64593763009827,0.16446873435830678,13.806301890528491,-50491.856298664679,513.69061511031191,4.6451469190034178,0.17950069210709912,20.549227520909241,-50111.092360772367,474.2163040478942]
["KBM","KBM-57H02-A (480 V)",33.5,5.22,24.931661036070302,3.8593902532616569,1015,115,1228,4.4000000000000004,22,390,11.8,679,24,299.64593763009827,513.99539609941246,577.9487179487179,29.160998246621602,0.21186440677966101,0.82512404224886715,0.60605764024220299,5.0609816227609254,69.696628627853343,0,-56.454269188561206,0,0,0,0,0,0.31808676730688817,0.45250796198680904,3.8170412076826579,10.860191087683416,6.9138123781094514,1158.2772477092153,938.94834409249427,9032.6830701697945,0.33616593689141883,53.260034962049318,-46142.715351481398,299.64593763009827,0.16437215313642334,13.752293020248407,-50494.30272959439,513.99539609941246,4.6269755694726289,0.17950069210709912,20.549227520909241,-50111.092360772367,474.2163040478942]
["KBM","KBM-57H03-A (400 V)",59.9,5.47,51.264644827494706,4.635139676988671,475,218,597,5.92,35,669,22.1,565,24,142.88386847746318,287.98760693244202,336.9207772795217,54.66447311338635,0.11312217194570134,0.81524294365222194,0.54998943486405083,9.0064134456264302,119.89769680036309,0,-97.117134408294106,0,0,0,0,0,0.32068561562913239,0.45620506503755293,3.8482273875495885,10.948921560901271,6.9702999517714703,1992.5608596955731,1615.253794732542,15538.741505327054,1.0225387978968383,136.56061042339675,-40388.255757220395,142.88386847746318,0.4844357536686843,34.583144212086097,-50137.098069004038,287.98760693244202,5.0414564952408689,0.51804978340789998,47.814533093990825,-49528.110851952952,266.47677396660652]
["KBM","KBM-57H03-A (480 V)",59.9,5.47,49.392913373346836,4.465905368295374,580,218,717,5.92,35,669,22.1,679,24,142.88386847746318,287.91670281223924,336.9207772795217,54.684197003950771,0.11312217194570134,0.81478720159020379,0.54998943486405083,9.0064134456264302,119.89769680036309,0,-97.117134408294106,0,0,0,0,0,0.32068561562913239,0.45620506503755293,3.8482273875495885,10.948921560901271,6.9702999517714703,1992.5608596955731,1615.253794732542,15538.741505327054,1.0225387978968383,136.56061042339675,-40388.255757220395,142.88386847746318,0.48452998794970797,34.627305026771914,-50135.390821375688,287.91670281223924,5.0478941639695307,0.51804978340789998,47.814533093990825,-49528.110851952952,266.47677396660652]
["KBM","KBM-57S01-A (240 V)",18.8,5.67,16.00592325412811,4.7778875385457047,880,46.1,1183,3.39,13,203,6.56,325,24,687.34108812770512,990.68594895974593,1110.344827586207,15.654485713124487,0.38109756097560976,0.89369023800485281,0.95786213517035201,2.7792411180420324,44.157444431353227,0,-35.76752998939611,0,0,0,0,0,0.3900652630814096,0.5549040556865531,4.6807831569769149,13.317697336477275,8.4783094468085078,733.84558491227187,594.88615366978979,5722.8047983033775,7.9900891930766382E-2,16.572289009537378,-49139.014479509133,687.34108812770512,4.5800775357941317E-2,5.7090366624020508,-50607.429530850968,990.68594895974593,4.7896796632391219,5.5596529377508655E-2,10.105681980887608,-50185.60596872749,863.54508229598775]
["KBM","KBM-57S02-A (240 V)",33.5,5.22,29.506253494564866,4.5675315007066359,445,115,612,4.4000000000000004,22,390,11.8,325,24,299.64593763009827,514.92663543445417,577.9487179487179,28.878682132984668,0.21186440677966101,0.83186796832643162,0.60605764024220299,5.0609816227609254,69.696628627853343,0,-56.454269188561206,0,0,0,0,0,0.31808676730688817,0.45250796198680904,3.8170412076826579,10.860191087683416,6.9138123781094514,1158.2772477092153,938.94834409249427,9032.6830701697945,0.33616593689141883,53.260034962049318,-46142.715351481398,299.64593763009827,0.16407890047024132,13.586988648813465,-50501.730906405355,514.92663543445417,4.5713587143757834,0.17950069210709912,20.549227520909241,-50111.092360772367,474.2163040478942]
["KBM","KBM-57S03-A (240 V)",59.9,5.47,53.858032742297389,4.8696232135892759,250,218,357,5.92,35,669,22.1,325,24,142.88386847746318,289.71365913646429,336.9207772795217,52.898238229553073,0.11312217194570134,0.86024344465410707,0.54998943486405083,9.0064134456264302,119.89769680036309,0,-97.117134408294106,0,0,0,0,0,0.32068561562913239,0.45620506503755293,3.8482273875495885,10.948921560901271,6.9702999517714703,1992.5608596955731,1615.253794732542,15538.741505327054,1.0225387978968383,136.56061042339675,-40388.255757220395,142.88386847746318,0.4821748343261375,33.506168416324158,-50178.059268511402,289.71365913646429,4.8844572765618537,0.51804978340789998,47.814533093990825,-49528.110851952952,266.47677396660652]
["KBM","KBM-79H01-A (400 V)",43.4,4.95,35.571129781038607,4.0102739324733498,600,152,744,6.26,23,534,32.5,565,32,191.54687770136559,364.30310807945347,422.09737827715355,38.646530410802825,7.6923076923076927E-2,1.5984874410490537,1.1222773288437924,9.6173640062517229,170.58615398425644,0,-138.1747847272477,0,0,0,0,0,0.56985896213638843,0.81067728707955977,6.8383075456366615,19.456254889909435,12.386236559139787,2834.9443125750022,2298.1253177089011,22107.965556359628,0.61991499195707211,100.37724576294784,-41971.756996946213,191.54687770136559,0.30738606527786633,25.866610186547256,-50218.567465963555,364.30310807945347,4.4674870332490269,0.4560366459276417,71.715922255430101,-46296.072426051978,249.54862875522764]
["KBM","KBM-79H01-A (480 V)",43.4,4.95,33.814974895278034,3.8122857830076704,730,152,894,6.26,23,534,32.5,679,32,191.54687770136559,364.26805538908837,422.09737827715355,38.617098005818271,7.6923076923076927E-2,1.6000680733580888,1.1222773288437924,9.6173640062517229,170.58615398425644,0,-138.1747847272477,0,0,0,0,0,0.56985896213638843,0.81067728707955977,6.8383075456366615,19.456254889909435,12.386236559139787,2834.9443125750022,2298.1253177089011,22107.965556359628,0.61991499195707211,100.37724576294784,-41971.756996946213,191.54687770136559,0.30740967172264577,25.880340615969299,-50217.944554420574,364.26805538908837,4.4698584501050256,0.4560366459276417,71.715922255430101,-46296.072426051978,249.54862875522764]
["KBM","KBM-79H02-A (400 V)",79.31,5.39,67.254331666546648,4.5137135346675601,350,319,443,6.4,32,901,59.7,565,32,93.79572222971683,213.7642201999553,250.16648168701445,71.946941313457287,4.1876046901172526E-2,1.6712192784954762,0.95033217893602784,16.164954251977473,303.15596508059286,0,-245.55633171528021,0,0,0,0,0,0.60344135377383057,0.85845135742886314,7.2412962452859668,20.602832578292716,13.116170586120099,5038.101035490432,4084.0969931855343,39289.01307444484,1.8251555411105096,216.52940908268576,-36366.589156376664,93.79572222971683,0.86447186435544343,49.36525723278848,-50054.690173755836,213.7642201999553,4.9426062277964666,1.1827144091051858,131.00034780266449,-45520.277644466114,148.46933449913141]
["KBM","KBM-79H02-A (480 V)",79.31,5.39,64.846386115581552,4.3521064507101714,430,319,532,6.4,32,901,59.7,679,32,93.79572222971683,213.6332443666272,250.16648168701445,72.124165675826731,4.1876046901172526E-2,1.6617044169598423,0.95033217893602784,16.164954251977473,303.15596508059286,0,-245.55633171528021,0,0,0,0,0,0.60344135377383057,0.85845135742886314,7.2412962452859668,20.602832578292716,13.116170586120099,5038.101035490432,4084.0969931855343,39289.01307444484,1.8251555411105096,216.52940908268576,-36366.589156376664,93.79572222971683,0.86481507303783378,49.525830585396328,-50049.800036421067,213.6332443666272,4.9586833414814038,1.1827144091051858,131.00034780266449,-45520.277644466114,148.46933449913141]
["KBM","KBM-79H03-A (400 V)",143,6.76,122.74824985962429,5.7358995261506687,240,637,307,5.75,34,1300,114,565,32,48.817590135076571,145.97233775161973,173.38461538461539,130.68251953519859,2.1929824561403508E-2,1.9025254559483735,0.89137864719290738,24.923851112874541,567.80819826188201,0,-459.92464059212449,0,0,0,0,0,0.78617721484877467,1.1184100874855252,9.4341265781852961,26.841842099652606,17.088047407407405,9436.3146404282197,7649.4742718024854,73587.942494739909,3.8970718944828411,389.87188259144398,-28319.940349793389,48.817590135076571,1.7849519374055203,80.865930881079564,-49837.808109872261,145.97233775161973,6.2458818678877535,2.4007243241146896,221.24031318052002,-43564.438672157608,96.293305120903568]
["KBM","KBM-79H03-A (480 V)",143,6.76,119.2070523758296,5.5704230082163368,300,637,369,5.75,34,1300,114,679,32,48.817590135076571,145.80028675714135,173.38461538461539,131.43660471199436,2.1929824561403508E-2,1.8618696413201672,0.89137864719290738,24.923851112874541,567.80819826188201,0,-459.92464059212449,0,0,0,0,0,0.78617721484877467,1.1184100874855252,9.4341265781852961,26.841842099652606,17.088047407407405,9436.3146404282197,7649.4742718024854,73587.942494739909,3.8970718944828411,389.87188259144398,-28319.940349793389,48.817590135076571,1.7860608431013156,81.33676064324743,-49826.510794092173,145.80028675714135,6.2822475789151921,2.4007243241146896,221.24031318052002,-43564.438672157608,96.293305120903568]
["KBM","KBM-79S01-A (240 V)",43.4,4.95,38.505228167394037,4.3410629275528798,310,152,445,6.26,23,534,32.5,325,32,191.54687770136559,366.1127368340741,422.09737827715355,37.619231252213851,7.6923076923076927E-2,1.6530455172866811,1.1222773288437924,9.6173640062517229,170.58615398425644,0,-138.1747847272477,0,0,0,0,0,0.56985896213638843,0.81067728707955977,6.8383075456366615,19.456254889909435,12.386236559139787,2834.9443125750017,2298.1253177089011,22107.965556359628,0.61991499195707211,100.37724576294784,-41971.756996946213,191.54687770136559,0.30618225174627411,25.1564919603668,-50250.332916095052,366.1127368340741,4.3448407357768932,0.4560366459276417,71.715922255430101,-46296.072426051978,249.54862875522764]
["KBM","KBM-79S02-A (240 V)",79.31,5.39,71.354466152866408,4.7888903458299605,180,319,265,6.4,32,901,59.7,325,32,93.79572222971683,214.97911098746613,250.16648168701445,69.80848003395846,4.1876046901172526E-2,1.7952226073144049,0.95033217893602784,16.164954251977473,303.15596508059286,0,-245.55633171528021,0,0,0,0,0,0.60344135377383057,0.85845135742886314,7.2412962452859668,20.602832578292716,13.116170586120099,5038.101035490432,4084.0969931855343,39289.01307444484,1.8251555411105096,216.52940908268576,-36366.589156376664,93.79572222971683,0.86133671346589058,47.873523515160137,-50099.360717368982,214.97911098746613,4.7932491135775495,1.1827144091051858,131.00034780266449,-45520.277644466114,148.46933449913141]
["KBM","KBM-79S03-A (240 V)",143,6.76,128.72451797272495,6.0151643912488302,125,637,184,5.75,34,1300,114,325,32,48.817590135076571,146.93547280583758,173.38461538461539,126.21940239032884,2.1929824561403508E-2,2.1827369877947644,0.89137864719290738,24.923851112874541,567.80819826188201,0,-459.92464059212449,0,0,0,0,0,0.78617721484877467,1.1184100874855252,9.4341265781852961,26.841842099652606,17.088047407407405,9436.3146404282197,7649.4742718024854,73587.942494739909,3.8970718944828411,389.87188259144398,-28319.940349793389,48.817590135076571,1.7788562180345515,78.227164246503733,-49899.910114489729,146.93547280583758,6.0420701452387959,2.4007243241146896,221.24031318052002,-43564.438672157608,96.293305120903568]
["KBM","KBM-118H01-A (400 V)",325,43.7,109.48238123518914,14.443585914932603,785,994,872,0.27600000000000002,2.5,648,267,565,38,231.32211547105618,328.01792284710729,347.83950617283955,234.94440554880509,9.3632958801498131E-3,2.2965185610402288,1.3214420379062117,9.5506638998928892,1313.5133856787745,0,-1063.9458423998071,0,0,0,0,0,5.1729789899900318,7.3590429428413406,62.075747879880382,176.61703062819217,112.43789383475784,21829.071206827517,17695.56494635854,170231.33478396916,0.75139721169624418,41.402748804354658,-49784.576956877951,231.32211547105618,0.44029615513584347,10.268888048746637,-50742.377755869384,328.01792284710729,33.149631414508413,0.65450568246581331,34.830316204380338,-50082.881260754177,251.29143116709571]
["KBM","KBM-118H02-A (400 V)",445,46.5,239.54167706034417,24.797275058006644,590,1451,685,0.29199999999999998,2.7,585,396,565,38,217.13250714153182,357.05822193806449,385.29914529914532,320.66002801489805,6.313131313131313E-3,2.3723339441354137,1.3385563131382532,9.9957818292760354,1942.2452103636053,0,-1573.2186203945203,0,0,0,0,0,5.9443604590073713,8.4564047080437863,71.332325508088459,202.95371299305089,129.20434656679151,32277.865958889677,26165.798260199925,251714.97926312327,0.83981762885279965,44.860044415419679,-49335.057300786459,217.13250714153182,0.3688322205999065,10.373432498918758,-50726.550823427846,357.05822193806449,35.060906484434838,0.70355787582904861,38.227550342217633,-49737.627232692837,240.10127881850988]
["KBM","KBM-118H02-A (480 V)",445,46.5,139.13728616498514,14.403445772772789,710,1451,822,0.29199999999999998,2.7,585,396,679,38,217.13250714153182,359.91803363160557,385.29914529914532,289.94999081024645,6.313131313131313E-3,2.7254290933576932,1.3385563131382532,9.9957818292760354,1942.2452103636053,0,-1573.2186203945203,0,0,0,0,0,5.9443604590073713,8.4564047080437863,71.332325508088459,202.95371299305089,129.20434656679151,32277.865958889677,26165.798260199925,251714.97926312327,0.83981762885279965,44.860044415419679,-49335.057300786459,217.13250714153182,0.36500550643311303,9.5985231668077571,-50737.856583399996,359.91803363160557,32.441809707173157,0.70355787582904861,38.227550342217633,-49737.627232692837,240.10127881850988]
["KBM","KBM-118H03-A (400 V)",560,44,374.83733148884318,29.284166522565872,435,1932,516,0.373,4.3,775,542,565,38,141.981121710824,261.34914300757691,290.83870967741939,448.75378222439798,4.6125461254612546E-3,2.5360897498915098,1.37361965164785,15.307287620149264,2653.8331669836462,0,-2149.6048652567533,0,0,0,0,0,6.1072599056388368,8.6881442966726521,73.287118867666038,208.51546312014364,132.74506666666665,44103.633662773958,35752.263871214192,343936.77844108053,1.8656705274531626,76.005134736652323,-48400.672796530002,141.981121710824,0.67249754012753904,18.116377114668204,-50668.55100114012,261.34914300757691,36.182634969798372,1.5680100963252288,66.464470867100758,-48966.439547286711,156.78806458440332]
["KBM","KBM-118H03-A (480 V)",560,44,302.72162633703306,23.650127057580708,535,1932,619,0.373,4.3,775,542,679,38,141.981121710824,262.42226839189476,290.83870967741939,433.80266462651718,4.6125461254612546E-3,2.720580863392204,1.37361965164785,15.307287620149264,2653.8331669836462,0,-2149.6048652567533,0,0,0,0,0,6.1072599056388368,8.6881442966726521,73.287118867666038,208.51546312014364,132.74506666666665,44103.633662773958,35752.263871214192,343936.77844108053,1.8656705274531626,76.005134736652323,-48400.672796530002,141.981121710824,0.66868669123339874,17.629549869177804,-50675.794327329939,262.42226839189476,35.210327294514357,1.5680100963252288,66.464470867100758,-48966.439547286711,156.78806458440332]
["KBM","KBM-118H04-A (400 V)",672,42.8,502.32108656444967,31.395067910278105,340,2400,413,0.45500000000000002,4.5,970,648,565,38,119.08036546919112,209.20004277275663,232.37113402061857,567.59754132837645,3.8580246913580245E-3,2.4948714618669512,1.3210272996042716,17.838169936628795,3170.4655190502517,0,-2568.0770704307033,0,0,0,0,0,5.9143315363293079,8.4136857772414899,70.971978435951698,201.92845865379576,128.55164938271602,52689.465009429681,42712.300547704006,410892.33126891253,2.3457249252312979,116.85020965642296,-47177.258125000008,119.08036546919112,1.0219373655408774,28.064741793375173,-50595.884377742375,209.20004277275663,36.712781758564624,1.934487308080399,98.270103060135881,-48239.262148089671,134.54294967063038]
["KBM","KBM-118H04-A (480 V)",672,42.8,450.74953525668928,28.17184595354308,420,2400,495,0.45500000000000002,4.5,970,648,679,38,{"$f":"IF(AQ992<I992,IF(AQ992<0,0,AQ992),I992)","v":119.08036546919112},{"$f":"IF(AU992<I992,IF(AU992<0,0,AU992),I992)","v":209.38644199519712},{"$f":"IF(UAC_V*0.98/L992*1000<I992,IF(UAC_V*0.98/L992*1000<0,0,UAC_V*0.98/L992*1000),I992)","v":232.37113402061857},{"$f":"C992+(E992-C992)/G992*Q992","v":561.69798189908181},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M992,(inertia/gear^2+gear_inertia)/M992),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M992,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M992))","v":3.8580246913580245E-3},{"$f":"IF((C992+(E992-C992)/G992*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X992^2*time1+Y992^2*time2+Z992^2*time3+AA992^2*time4)/time)/(C992+(E992-C992)/G992*mspeed),SQRT((((X992-Y992)*2/PI()+Y992)^2*time1+Y992^2*time2+((Z992-Y992)*2/PI()+Y992)^2*time3+AA992^2*time4)/time)/(C992+(E992-C992)/G992*mspeed)),IF(AccType=1,SQRT((X992^2*time1+Y992^2*time2+Z992^2*time3+AA992^2*time4+AB992^2*time5+AC992^2*time6+AD992^2*time7+AE992^2*time8)/time)/(C992+(E992-C992)/G992*mspeed),SQRT((((X992-Y992)*2/PI()+Y992)^2*time1+Y992^2*time2+((Z992-Y992)*2/PI()+Y992)^2*time3+AA992^2*time4+((AB992-AC992)*2/PI()+AC992)^2*time5+AC992^2*time6+((AD992-AC992)*2/PI()+AC992)^2*time7+AE992^2*time8)/time)/(C992+(E992-C992)/G992*mspeed))))","v":2.5668357677152973},{"$f":"IF(move1,MAX(ABS(X992),ABS(Z992))/H992,MAX(ABS(X992),ABS(Z992),ABS(AB992),ABS(AD992))/H992)","v":1.3210272996042716},{"$f":"IF(AZ992>0,speed/(MIN(AZ992,I992)),\"NA\")","v":17.838169936628795},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M992+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M992+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":3170.4655190502517},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M992+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M992+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-2568.0770704307033},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M992+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M992+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M992+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M992+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH992/Irms","v":5.9143315363293079},{"$f":"AI992/Ipeak","v":8.4136857772414899},{"$f":"IF(move1,IF(AccType=1,SQRT((X992^2*time1+Y992^2*time2+Z992^2*time3+AA992^2*time4)/time)/(C992/D992),SQRT((((X992-Y992)*2/PI()+Y992)^2*time1+Y992^2*time2+((Z992-AA992)*2/PI()+AA992)^2*time3+AA992^2*time4)/time)/(C992/D992)),IF(AccType=1,SQRT((X992^2*time1+Y992^2*time2+Z992^2*time3+AA992^2*time4+AB992^2*time5+AC992^2*time6+AD992^2*time7+AE992^2*time8)/time)/(C992/D992),SQRT((((X992-Y992)*2/PI()+Y992)^2*time1+Y992^2*time2+((Z992-AA992)*2/PI()+AA992)^2*time3+AA992^2*time4+((AB992-AC992)*2/PI()+AC992)^2*time5+AC992^2*time6+((AD992-AE992)*2/PI()+AE992)^2*time7+AE992^2*time8)/time)/(C992/D992)))","v":70.971978435951698},{"$f":"IF(move1,MAX(ABS(X992),ABS(Z992))/(C992/D992),MAX(ABS(X992),ABS(Z992),ABS(AB992),ABS(AD992))/(C992/D992))","v":201.92845865379576},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X992),ABS(Z992))/(C992/D992),MAX(ABS((X992-Y992)*2/PI()+Y992),ABS((Z992-Y992)*2/PI()+Y992))/(C992/D992)),IF(AccType=1,MAX(ABS(X992),ABS(Z992),ABS(AB992),ABS(AD992))/(C992/D992),MAX(ABS((X992-Y992)*2/PI()+Y992),ABS((Z992-Y992)*2/PI()+Y992),ABS((AB992-AC992)*2/PI()+AC992),ABS((AD992-AC992)*2/PI()+AC992))/(C992/D992)))","v":128.55164938271602},{"$f":"IF((C992+(E992-C992)/G992*mspeed)<0,\"NA\",U992*(C992+(E992-C992)/G992*mspeed)*mspeed/9.55)","v":52689.465009429681},{"$f":"IF(move1,IF(speed1>speed2,AM992/2*time1/time,AM992/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z992*-speed/30*PI(),((Z992-AA992)*2/PI()+AA992)*-speed/30*PI()),IF(AccType=1,X992*-speed/30*PI(),((X992-Y992)*2/PI()+Y992)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z992*-speed/30*PI(),((Z992-AA992)*2/PI()+AA992)*-speed/30*PI()),IF(AccType=1,X992*-speed/30*PI(),((X992-Y992)*2/PI()+Y992)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD992*-speed/30*PI(),((AD992-AE992)*2/PI()+AE992)*-speed/30*PI()),IF(AccType=1,AB992*-speed/30*PI(),((AB992-AC992)*2/PI()+AC992)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD992*-speed/30*PI(),((AD992-AE992)*2/PI()+AE992)*-speed/30*PI()),IF(AccType=1,AB992*-speed/30*PI(),((AB992-AC992)*2/PI()+AC992)*-speed/30*PI()),0)/2*time7/time)))","v":42712.300547704006},{"$f":"IF(move1,MAX(IF(AccType=1,Z992*-speed/30*PI(),((Z992-AA992)*2/PI()+AA992)*-speed/30*PI()),IF(AccType=1,X992*-speed/30*PI(),((X992-Y992)*2/PI()+Y992)*-speed/30*PI()),0),MAX(IF(AccType=1,Z992*-speed/30*PI(),((Z992-AA992)*2/PI()+AA992)*-speed/30*PI()),IF(AccType=1,X992*-speed/30*PI(),((X992-Y992)*2/PI()+Y992)*-speed/30*PI()),IF(AccType=1,AD992*-speed/30*PI(),((AD992-AE992)*2/PI()+AE992)*-speed/30*PI()),IF(AccType=1,AB992*-speed/30*PI(),((AB992-AC992)*2/PI()+AC992)*-speed/30*PI()),0))","v":410892.33126891253},{"$f":"(L992^2)/1000000+((K992/1000)^2*(D992/C992*H992)^2*PI()*PI()*(O992/2)^2)/1200","v":2.3457249252312979},{"$f":"SQRT(3)*L992*J992*D992/C992*H992/1000","v":116.85020965642296},{"$f":"0.75*J992^2*(D992/C992*H992)^2-(UAC_V*0.98)^2","v":-47177.258125000008},{"$f":"-AO992/2/AN992+SQRT((AO992/2/AN992)^2-AP992/AN992)","v":119.08036546919112},{"$f":"(L992^2)/1000000+((K992/1000)^2*AV992^2*PI()*PI()*(O992/2)^2)/1200","v":1.0209111664727109},{"$f":"SQRT(3)*L992*J992*AV992/1000","v":27.886479770304874},{"$f":"0.75*J992^2*AV992^2-(UAC_V*0.98)^2","v":-50598.534494106811},{"$f":"-AS992/2/AR992+SQRT((AS992/2/AR992)^2-AT992/AR992)","v":209.38644199519712},{"$f":"D992+(F992-D992)*((0.85*UAC_V-D992*J992)/L992*1000)/G992","v":36.47958899317225},{"$f":"(L992^2)/1000000+((K992/1000)^2*AJ992^2*PI()*PI()*(O992/2)^2)/1200","v":1.934487308080399},{"$f":"SQRT(3)*L992*J992*AJ992/1000","v":98.270103060135881},{"$f":"0.75*J992^2*AJ992^2-(UAC_V*0.98)^2","v":-48239.262148089671},{"$f":"IF(((AX992/2/AW992)^2-AY992/AW992)>0,-AX992/2/AW992+SQRT((AX992/2/AW992)^2-AY992/AW992),-9999)","v":134.54294967063038}]
["KBM","KBM-118S01-A (240 V)",325,43.7,252.45952847951898,33.306006395714903,400,994,523,0.27600000000000002,2.5,648,267,325,38,231.32211547105618,325.43054421012215,347.83950617283955,265.98278718957749,9.3632958801498131E-3,1.8989892007528375,1.3214420379062117,9.5506638998928892,1313.5133856787745,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-1063.9458423998071,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},5.1729789899900318,7.3590429428413406,62.075747879880382,176.61703062819217,112.43789383475784,21829.071206827517,17695.56494635854,170231.33478396916,0.75139721169624418,41.402748804354658,-49784.576956877951,231.32211547105618,0.44441564226318797,11.25843593435734,-50729.69490578321,325.43054421012215,36.344052029406896,0.65450568246581331,34.830316204380338,-50082.881260754177,251.29143116709571]
["KBM","KBM-118S02-A (240 V)",445,46.5,356.90495988357532,36.946683217761418,320,1451,411,0.29199999999999998,2.7,585,396,325,38,217.13250714153182,354.6390376474169,385.29914529914532,347.36893672375174,6.313131313131313E-3,2.1286877483036011,1.3385563131382532,9.9957818292760354,1942.2452103636053,0,-1573.2186203945203,0,0,0,0,0,5.9443604590073713,8.4564047080437863,71.332325508088459,202.95371299305089,129.20434656679151,32277.865958889677,26165.798260199925,251714.97926312327,0.83981762885279965,44.860044415419679,-49335.057300786459,217.13250714153182,0.37220374179896987,11.011067651591793,-50716.589899314829,354.6390376474169,37.216033677038425,0.70355787582904861,38.227550342217633,-49737.627232692837,240.10127881850988]
["KBM","KBM-118S03-A (240 V)",560,44,467.30600312088416,36.508281493819069,235,1932,309,0.373,4.3,775,542,325,38,141.981121710824,260.84865766098193,290.83870967741939,457.11019293979314,4.6125461254612546E-3,2.4424712721654234,1.37361965164785,15.307287620149264,2653.8331669836462,0,-2149.6048652567533,0,0,0,0,0,6.1072599056388368,8.6881442966726521,73.287118867666038,208.51546312014364,132.74506666666665,44103.633662773958,35752.263871214192,343936.77844108053,1.8656705274531626,76.005134736652323,-48400.672796530002,141.981121710824,0.67429870831617333,18.341975990994822,-50665.127499165777,260.84865766098193,36.633208599396397,1.5680100963252288,66.464470867100758,-48966.439547286711,156.78806458440332]
["KBM","KBM-118S04-A (240 V)",672,42.8,577.08722068131567,36.067951292582229,185,2400,247,0.45500000000000002,4.5,970,648,325,38,119.08036546919112,209.61236455897944,232.37113402061857,564.46004270349181,3.8580246913580245E-3,2.5306555694672777,1.3210272996042716,17.838169936628795,3170.4655190502517,0,-2568.0770704307033,0,0,0,0,0,5.9143315363293079,8.4136857772414899,70.971978435951698,201.92845865379576,128.55164938271602,52689.465009429681,42712.300547704006,410892.33126891253,2.3457249252312979,116.85020965642296,-47177.258125000008,119.08036546919112,1.0196737539053293,27.670000364250672,-50601.730060538415,209.61236455897944,36.196402308320309,1.934487308080399,98.270103060135881,-48239.262148089671,134.54294967063038]
["KBM","KBM-60H01-A (400 V)",54,13.7,34.759439571269944,8.6038216760569171,1250,127,1639,0.91600000000000004,7.8,245,16.3,565,38,425.51109640473891,768.39983697363937,920,42.172445202625894,0.15337423312883436,0.68449282092054353,0.72148924519775504,3.5037449878471878,91.629134140114886,0,-74.219598653493051,0,0,0,0,0,0.68087678307868227,0.9686104457712762,8.1705213969441868,23.246650698510628,14.799277475994513,1522.7700878974299,1234.4215992264958,11875.135784558888,0.24755724953138974,12.524278422296174,-50151.859083718482,425.51109640473891,8.0535208997474628E-2,4.141901580262453,-50733.709151601084,768.39983697363937,10.655592158994134,9.9588611861836873E-2,5.7525804150475786,-50667.33333847735,684.98135803959758]
["KBM","KBM-60H01-A (480 V)",54,13.7,24.858012674165401,6.1529734341993567,1600,127,1895,0.91600000000000004,7.8,245,16.3,679,38,425.51109640473891,778.03131885337325,920,39.829138229295388,0.15337423312883436,0.70354302552140013,0.72148924519775504,3.5037449878471878,91.629134140114886,0,-74.219598653493051,0,0,0,0,0,0.68087678307868227,0.9686104457712762,8.1705213969441868,23.246650698510628,14.799277475994513,1522.7700878974299,1234.4215992264958,11875.135784558888,0.24755724953138974,12.524278422296174,-50151.859083718482,425.51109640473891,7.8736807143685139E-2,3.9561486211320567,-50739.974194450297,778.03131885337325,10.177717990218161,9.9588611861836873E-2,5.7525804150475786,-50667.33333847735,684.98135803959758]
["KBM","KBM-60H02-A (400 V)",108,16.399999999999999,88.643815200699777,13.055053785080968,725,255,974,0.92100000000000004,11,411,31.7,565,38,248.09239201627736,437.5373982077337,548.41849148418498,96.318545191291165,7.8864353312302835E-2,0.61062214898809708,0.65367467409093216,5.7172671407970466,166.68704189318771,0,-135.01650393348206,0,0,0,0,0,0.74136156641786632,1.0546556662994899,8.8963387970143959,25.31173599118776,16.113951604938269,2770.1455854304313,2245.5967390184128,21602.640629357131,0.70760195024155381,25.38764123306548,-49851.263907479173,248.09239201627736,0.24315859565985604,9.4247207819635346,-50673.700084095566,437.5373982077337,14.374952330202039,0.26220672293929603,10.564869439708385,-50639.969665053366,419.78097942532293]
["KBM","KBM-60H02-A (480 V)",108,16.399999999999999,84.001439455620698,12.371346017028085,885,255,1169,0.92100000000000004,11,411,31.7,679,38,248.09239201627736,437.2598349232365,548.41849148418498,96.142817376236621,7.8864353312302835E-2,0.61182819823604306,0.65367467409093216,5.7172671407970466,166.68704189318771,0,-135.01650393348206,0,0,0,0,0,0.74136156641786632,1.0546556662994899,8.8963387970143959,25.31173599118776,16.113951604938269,2770.1455854304313,2245.5967390184128,21602.640629357131,0.70760195024155381,25.38764123306548,-49851.263907479173,248.09239201627736,0.2434379730817362,9.4424380961217125,-50673.205362626482,437.2598349232365,14.401975469914612,0.26220672293929603,10.564869439708385,-50639.969665053366,419.78097942532293]
["KBM","KBM-60H03-A (400 V)",154,18.7,119.77083853017209,14.090686885902599,590,393,778,0.86699999999999999,11,515,47.5,565,38,197.44302257055318,359.8100791333855,437.66990291262135,133.12542830995218,5.2631578947368418E-2,0.67018637545243021,0.6200878007424806,7.0402620919614058,243.69450569179489,0,-197.39254961035385,0,0,0,0,0,0.86671189912229918,1.2329781537977718,10.40054278946759,29.59147569114652,18.838518518518512,4049.9204465357175,3283.0361681555737,31582.807937656617,1.0833844362918668,36.906289996527782,-49521.274392206804,197.44302257055318,0.3569693275733089,12.358649885316362,-50661.191457264751,359.8100791333855,15.980268615374387,0.39272334998065173,14.569132743139718,-50605.084942136658,340.89639968664346]
["KBM","KBM-60H03-A (480 V)",154,18.7,110.74531456811052,13.028860537424766,720,393,930,0.86699999999999999,11,515,47.5,679,38,197.44302257055318,359.95803753497887,437.66990291262135,132.37517821908921,5.2631578947368418E-2,0.6751011167418085,0.6200878007424806,7.0402620919614058,243.69450569179489,0,-197.39254961035385,0,0,0,0,0,0.86671189912229918,1.2329781537977718,10.40054278946759,29.59147569114652,18.838518518518512,4049.9204465357175,3283.0361681555737,31582.807937656617,1.0833844362918668,36.906289996527782,-49521.274392206804,197.44302257055318,0.35671293022980582,12.341368479004204,-50661.593805321376,359.95803753497887,15.957923009868736,0.39272334998065173,14.569132743139718,-50605.084942136658,340.89639968664346]
["KBM","KBM-60S01-A (240 V)",54,13.7,44.708070377632424,11.066354053869413,660,127,983,0.91600000000000004,7.8,245,16.3,325,38,425.51109640473891,767.09292517104143,920,43.200343220446371,0.15337423312883436,0.67596955196828723,0.72148924519775504,3.5037449878471878,91.629134140114886,0,-74.219598653493051,0,0,0,0,0,0.68087678307868227,0.9686104457712762,8.1705213969441868,23.246650698510628,14.799277475994513,1522.7700878974299,1234.4215992264958,11875.135784558888,0.24755724953138974,12.524278422296174,-50151.859083718482,425.51109640473891,8.0784825673562197E-2,4.1670295788612481,-50732.83956888337,767.09292517104143,10.720237274203166,9.9588611861836873E-2,5.7525804150475786,-50667.33333847735,684.98135803959758]
["KBM","KBM-60S02-A (240 V)",108,16.399999999999999,95.989033210228826,14.136823742301742,385,255,584,0.92100000000000004,11,411,31.7,325,38,248.09239201627736,443.24378540842082,548.41849148418498,94.171983412174015,7.8864353312302835E-2,0.62383182558377404,0.65367467409093216,5.7172671407970466,166.68704189318771,0,-135.01650393348206,0,0,0,0,0,0.74136156641786632,1.0546556662994899,8.8963387970143959,25.31173599118776,16.113951604938269,2770.1455854304313,2245.5967390184128,21602.640629357131,0.70760195024155381,25.38764123306548,-49851.263907479173,248.09239201627736,0.2375359767012892,9.0607887228541415,-50683.656616346991,443.24378540842082,13.819868935992467,0.26220672293929603,10.564869439708385,-50639.969665053366,419.78097942532293]
["KBM","KBM-60S03-A (240 V)",154,18.7,133.38699992463609,15.692588226427775,315,393,467,0.86699999999999999,11,515,47.5,325,38,197.44302257055318,363.80447742725966,437.66990291262135,130.19332787102911,5.2631578947368418E-2,0.68823593992287235,0.6200878007424806,7.0402620919614058,243.69450569179489,0,-197.39254961035385,0,0,0,0,0,0.86671189912229918,1.2329781537977718,10.40054278946759,29.59147569114652,18.838518518518512,4049.9204465357175,3283.0361681555737,31582.807937656617,1.0833844362918668,36.906289996527782,-49521.274392206804,197.44302257055318,0.35016529171883709,11.891545233500112,-50671.868598321824,363.80447742725966,15.376282105781348,0.39272334998065173,14.569132743139718,-50605.084942136658,340.89639968664346]
["KBM","KBM-88H01-A (400 V)",205,17,162.33804195373327,13.306396881453548,425,414,542,0.93,13,738,98.4,565,46,174.39504159521326,255.3751999513465,305.42005420054204,179.36516219674982,2.540650406504065E-2,1.0824990601273754,1.1878635567295703,11.667059673228312,491.77551248604209,0,-398.33816511369412,0,0,0,0,0,1.1944558328782049,1.6992243317607147,14.333469994538458,40.781383962257152,25.962235374887083,8172.7394611090776,6625.1669873379487,63734.106418191062,1.4113098397515564,40.812701158126359,-50040.588749870316,174.39504159521326,0.70753476039577767,17.693661931973377,-50661.45802560803,255.3751999513465,14.883935774361193,1.0402596845449523,30.863275862347493,-50367.928617227328,205.70735619936298]
["KBM","KBM-88H01-A (480 V)",205,17,151.31962281660205,12.403247771852628,520,414,651,0.93,13,738,98.4,679,46,174.39504159521326,255.54278313989471,305.42005420054204,178.61993656645228,2.540650406504065E-2,1.0912961083143435,1.1878635567295703,11.667059673228312,491.77551248604209,0,-398.33816511369412,0,0,0,0,0,1.1944558328782049,1.6992243317607147,14.333469994538458,40.781383962257152,25.962235374887083,8172.7394611090804,6625.1669873379487,63734.106418191062,1.4113098397515564,40.812701158126359,-50040.588749870316,174.39504159521326,0.7067412406546113,17.650512120968596,-50662.158067484241,255.54278313989471,14.847638086627576,1.0402596845449523,30.863275862347493,-50367.928617227328,205.70735619936298]
["KBM","KBM-88H01-B (400 V)",205,32,66.998273370021394,10.197606296806908,935,414,1006,0.26100000000000001,3.7,397,98.4,565,46,338.86187048871511,515.34771262532388,567.7581863979849,128.93703298705378,2.540650406504065E-2,1.2493125310728126,1.1878635567295703,6.0490388393437327,491.77551248604209,0,-398.33816511369412,0,0,0,0,0,2.2483874501236798,3.1985399186084038,26.980649401484158,76.764958046601691,48.870090117434508,8172.7394611090785,6625.1669873379487,63734.106418191062,0.4063632653612248,11.59813340574218,-50591.789097168643,338.86187048871511,0.18389569685902707,3.7702560031934267,-50782.612381638086,515.34771262532388,21.007733464176027,0.29986280747188809,8.7707106031244582,-50683.140691959597,396.75724751345433]
["KBM","KBM-88H01-B (480 V)",205,32,67.048252621692072,10.20521348884202,940,414,1068,0.26100000000000001,3.7,397,98.4,679,46,338.86187048871511,515.10291667734577,567.7581863979849,129.40494953691191,2.540650406504065E-2,1.2459038339420374,1.1878635567295703,6.0490388393437327,491.77551248604209,0,-398.33816511369412,0,0,0,0,0,2.2483874501236798,3.1985399186084038,26.980649401484158,76.764958046601691,48.870090117434508,8172.7394611090785,6625.1669873379487,63734.106418191062,0.4063632653612248,11.59813340574218,-50591.789097168643,338.86187048871511,0.18405179938876298,3.7814341919685788,-50782.478483480976,515.10291667734577,21.070017937750698,0.29986280747188809,8.7707106031244582,-50683.140691959597,396.75724751345433]
["KBM","KBM-88H02-A (400 V)",385,15,331.71240770731868,12.907097576160259,190,789,257,1.66,29,1560,198,565,46,80.108775950359927,117.40997571628054,144.48717948717947,352.07107938388015,1.2626262626262626E-2,1.3294200533928335,1.2385487551636216,25.852851012173662,977.21496782409747,0,-791.54412393751886,0,0,0,0,0,1.1151384113840919,1.5863879347793788,13.381660936609101,38.073310434705093,24.238222222222216,16240.180990608225,13164.975034303847,126647.05983000301,5.8912834617309935,137.87986404702104,-48852.203792157197,80.108775950359927,3.1299659836377582,61.876680116793246,-50411.841095673495,117.40997571628054,13.795380723660392,4.5832694915838861,108.71615311579815,-49590.991489532214,92.833088268287369]
["KBM","KBM-88H02-A (480 V)",385,15,323.05067172269821,12.570065047575806,235,789,309,1.66,29,1560,198,679,46,80.108775950359927,117.22694238326886,144.48717948717947,354.09731771640224,1.2626262626262626E-2,1.2913945378183058,1.2385487551636216,25.852851012173662,977.21496782409747,0,-791.54412393751886,0,0,0,0,0,1.1151384113840919,1.5863879347793788,13.381660936609101,38.073310434705093,24.238222222222216,16240.180990608225,13164.975034303847,126647.05983000301,5.8912834617309935,137.87986404702104,-48852.203792157197,80.108775950359927,3.137439663126937,62.20783665627637,-50407.619839183317,117.22694238326886,13.869211939761136,4.5832694915838861,108.71615311579815,-49590.991489532214,92.833088268287369]
["KBM","KBM-88H02-B (400 V)",385,31.7,273.02307055855135,22.563890128805898,440,789,545,0.36899999999999999,6.4,733,198,565,46,186.20588181206469,267.54445449260834,307.50341064120056,316.91180340188714,1.2626262626262626E-2,1.2717007919689756,1.2385487551636216,11.286944451665084,977.21496782409747,0,-791.54412393751886,0,0,0,0,0,2.3566591760583804,3.3525665021670874,28.279910112700566,80.461596052010094,51.223442962962949,16240.180990608225,13164.975034303847,126647.05983000301,1.2894056295513745,30.434523324444495,-50374.172109876556,186.20588181206469,0.6623749682239376,12.411612432641379,-50733.48157219946,267.54445449260834,26.493372002287835,1.0048859303014457,23.997153758566711,-50537.21137807014,212.63505019252085]
["KBM","KBM-88H02-B (480 V)",385,31.7,233.08964847367582,19.263607311874036,550,789,654,0.36899999999999999,6.4,733,198,679,46,186.20588181206469,268.56094434037345,307.50341064120056,310.82329552547685,1.2626262626262626E-2,1.3195938583574511,1.2385487551636216,11.286944451665084,977.21496782409747,0,-791.54412393751886,0,0,0,0,0,2.3566591760583804,3.3525665021670874,28.279910112700566,80.461596052010094,51.223442962962949,16240.180990608225,13164.975034303847,126647.05983000301,1.2894056295513745,30.434523324444495,-50374.172109876556,186.20588181206469,0.65803811070186513,12.194552814169564,-50735.966736068687,268.56094434037345,26.03004451361079,1.0048859303014457,23.997153758566711,-50537.21137807014,212.63505019252085]
["KBM","KBM-88H03-A (400 V)",538,18.100000000000001,462.41745283790686,15.413915094596895,165,1200,221,1.41,26,1812,298,565,46,67.116403590875478,102.38538330471637,124.39293598233995,491.0997087131048,8.389261744966443E-3,1.5544717449493071,1.2205033160064063,30.442658142903998,1464.6039792076874,0,-1186.3292231582266,0,0,0,0,0,1.4431937670871635,2.0530771393788063,17.318325205045962,49.273851345091352,31.368708026986099,24340.021883679659,19731.047370614997,189812.67570531624,8.0771003636998877,178.65512478481151,-48374.889701496664,67.116403590875478,4.0911682636679778,73.339162534102158,-50395.620764908934,102.38538330471637,16.572881041756926,6.1774479844084524,138.81441438452765,-49337.948397977845,78.836742466243066]
["KBM","KBM-88H03-A (480 V)",538,18.100000000000001,443.08736156783664,14.769578718927887,225,1200,265,1.41,26,1812,298,679,46,67.116403590875478,102.15342685483375,124.39293598233995,494.90821658809205,8.389261744966443E-3,1.481267739882324,1.2205033160064063,30.442658142903998,1464.6039792076874,0,-1186.3292231582266,0,0,0,0,0,1.4431937670871635,2.0530771393788063,17.318325205045962,49.273851345091352,31.368708026986099,24340.021883679659,19731.047370614997,189812.67570531624,8.0771003636998877,178.65512478481151,-48374.889701496664,67.116403590875478,4.1047359265325607,73.952475225483042,-50388.742424505654,102.15342685483375,16.711474910631946,6.1774479844084524,138.81441438452765,-49337.948397977845,78.836742466243066]
["KBM","KBM-88H03-B (400 V)",545,35.5,400.51687418082179,25.839798334246566,345,1200,426,0.37,7,940,298,565,46,141.11383251681428,208.80998431758886,239.78723404255319,457.55211815519181,8.389261744966443E-3,1.4464149243028734,1.2205033160064063,14.709486893985156,1464.6039792076874,0,-1186.3292231582266,0,0,0,0,0,2.7942174218255089,3.9750337356171941,33.530609061906105,95.400809654812662,60.734041726129796,24340.021883679659,19731.047370614997,189812.67570531624,2.1861561239418492,47.087247227828627,-50177.837441292824,141.11383251681428,1.0763399563016063,18.113023785230926,-50712.334731030918,208.80998431758886,30.067737660267884,1.6699839090283268,36.586628325291684,-50426.430548830627,163.16000804768942]
["KBM","KBM-88H03-B (480 V)",545,35.5,359.5029302781636,23.193737437300879,425,1200,511,0.37,7,940,298,679,46,141.11383251681428,209.0836248078962,239.78723404255319,453.7425888736833,8.389261744966443E-3,1.4795910795581966,1.2205033160064063,14.709486893985156,1464.6039792076874,0,-1186.3292231582266,0,0,0,0,0,2.7942174218255089,3.9750337356171941,33.530609061906105,95.400809654812662,60.734041726129796,24340.021883679659,19731.047370614997,189812.67570531624,2.1861561239418492,47.087247227828627,-50177.837441292824,141.11383251681428,1.0739711677858816,18.001374469807242,-50713.475560547129,209.0836248078962,29.88239906821871,1.6699839090283268,36.586628325291684,-50426.430548830627,163.16000804768942]
["KBM","KBM-88S01-A (240 V)",205,17,179.31456921686876,14.697915509579408,225,414,325,0.93,13,738,98.4,325,46,174.39504159521326,257.10471132168476,305.42005420054204,175.64957659257746,2.540650406504065E-2,1.1263832072720863,1.1878635567295703,11.667059673228312,491.77551248604209,0,-398.33816511369412,0,0,0,0,0,1.1944558328782049,1.6992243317607147,14.333469994538458,40.781383962257152,25.962235374887083,8172.7394611090785,6625.1669873379487,63734.106418191062,1.4113098397515564,40.812701158126359,-50040.588749870316,174.39504159521326,0.69942749780035363,17.247725355178094,-50668.610240006477,257.10471132168476,14.508813236472893,1.0402596845449523,30.863275862347493,-50367.928617227328,205.70735619936298]
["KBM","KBM-88S01-B (240 V)",205,32,156.03550620729419,23.74969653079059,500,414,604,0.26100000000000001,3.7,397,98.4,325,46,338.86187048871511,502.34737292363548,567.7581863979849,155.80563035339716,2.540650406504065E-2,1.0750440423335594,1.1878635567295703,6.0490388393437327,491.77551248604209,0,-398.33816511369412,0,0,0,0,0,2.2483874501236798,3.1985399186084038,26.980649401484158,76.764958046601691,48.870090117434508,8172.7394611090785,6625.1669873379487,63734.106418191062,0.4063632653612248,11.59813340574218,-50591.789097168643,338.86187048871511,0.19255363384441737,4.3470344185246503,-50775.185968955077,502.34737292363548,24.221522450097719,0.29986280747188809,8.7707106031244582,-50683.140691959597,396.75724751345433]
["KBM","KBM-88S02-A (240 V)",385,15,346.63946605414804,13.487916967087473,100,789,154,1.66,29,1560,198,325,46,80.108775950359927,118.52231108942212,144.48717948717947,339.53420862113398,1.2626262626262626E-2,1.6217938730880681,1.2385487551636216,25.852851012173662,977.21496782409747,0,-791.54412393751886,0,0,0,0,0,1.1151384113840919,1.5863879347793788,13.381660936609101,38.073310434705093,24.238222222222216,16240.180990608225,13164.975034303847,126647.05983000301,5.8912834617309935,137.87986404702104,-48852.203792157197,80.108775950359927,3.0853762611129021,59.862865193817889,-50437.026100713636,118.52231108942212,13.346401503750789,4.5832694915838861,108.71615311579815,-49590.991489532214,92.833088268287369]
["KBM","KBM-88S02-B (240 V)",385,31.7,323.45702476889028,26.731985518090106,235,789,327,0.36899999999999999,6.4,733,198,325,46,186.20588181206469,267.75201538263673,307.50341064120056,314.87976318819864,1.2626262626262626E-2,1.2876143301691128,1.2385487551636216,11.286944451665084,977.21496782409747,0,-791.54412393751886,0,0,0,0,0,2.3566591760583804,3.3525665021670874,28.279910112700566,80.461596052010094,51.223442962962949,16240.180990608224,13164.975034303847,126647.05983000301,1.2894056295513745,30.434523324444495,-50374.172109876556,186.20588181206469,0.66148483270201097,12.367371889669439,-50733.991649513868,267.75201538263673,26.398937764278891,1.0048859303014457,23.997153758566711,-50537.21137807014,212.63505019252085]
["KBM","KBM-88S03-A (240 V)",538,18.100000000000001,482.76999404541584,16.092333134847195,90,1200,132,1.41,26,1812,298,325,46,67.116403590875478,103.33035226019251,124.39293598233995,474.58960032644768,8.389261744966443E-3,1.9730903953936574,1.2205033160064063,30.442658142903998,1464.6039792076874,0,-1186.3292231582266,0,0,0,0,0,1.4431937670871635,2.0530771393788063,17.318325205045962,49.273851345091352,31.368708026986099,24340.021883679659,19731.047370614997,189812.67570531624,8.0771003636998877,178.65512478481151,-48374.889701496664,67.116403590875478,4.0369814350272097,70.836766899948998,-50423.091631224321,103.33035226019251,16.007400011823592,6.1774479844084524,138.81441438452765,-49337.948397977845,78.836742466243066]
["KBM","KBM-88S03-B (240 V)",545,35.5,463.67140087438844,29.914283927379898,180,1200,255,0.37,7,940,298,325,46,141.11383251681428,209.67668190417362,239.78723404255319,450.26271773015048,8.389261744966443E-3,1.5096919405897404,1.2205033160064063,14.709486893985156,1464.6039792076874,0,-1186.3292231582266,0,0,0,0,0,2.7942174218255089,3.9750337356171941,33.530609061906105,95.400809654812662,60.734041726129796,24340.021883679659,19731.047370614997,189812.67570531624,2.1861561239418492,47.087247227828627,-50177.837441292824,141.11383251681428,1.0688744841942666,17.758770130080457,-50715.930168477527,209.67668190417362,29.479674281422195,1.6699839090283268,36.586628325291684,-50426.430548830627,163.16000804768942]
["KBM","KBM-163H01-A (400 V)",776,43.2,534.60145384567647,29.535991925175495,300,1966,365,0.37,4.2,1100,1060,565,56,124.63196098866862,184.27134222388634,204.90909090909091,627.72388629749344,2.3584905660377358E-3,4.4107741874942423,2.6340326785099903,28.260199776304717,5178.5082459506411,0,-4194.5916792200196,0,0,0,0,0,8.4437396357791012,12.012003663287571,101.32487562934921,288.28808791890168,183.52989690721648,86060.809488883999,69764.518573305948,671134.66867520311,2.5725241885138996,77.154378213855807,-49575.243041825066,124.63196098866862,1.3555113407012922,25.213717713699701,-50673.810503936751,184.27134222388634,35.766945231635773,5.0413055093993595,129.37842420352908,-47346.735072440431,84.925089666645746]
["KBM","KBM-163H01-A (480 V)",776,43.2,440.54088247836631,24.339275275047861,375,1966,438,0.37,4.2,1100,1060,679,56,124.63196098866862,184.87982411135221,204.90909090909091,610.61433961613579,2.3584905660377358E-3,4.8920154572081778,2.6340326785099903,28.260199776304717,5178.5082459506411,0,-4194.5916792200196,0,0,0,0,0,8.4437396357791012,12.012003663287571,101.32487562934921,288.28808791890168,183.52989690721648,86060.809488883984,69764.518573305948,671134.66867520311,2.5725241885138996,77.154378213855807,-49575.243041825066,124.63196098866862,1.3492741646517348,24.667421018200372,-50679.440648824559,184.87982411135221,34.991995491576951,5.0413055093993595,129.37842420352908,-47346.735072440431,84.925089666645746]
["KBM","KBM-163H02-A (400 V)",1090,40.6,843.68035333013711,31.017660048902101,200,2915,243,0.50900000000000001,6.3,1645,1570,565,56,79.335292413997593,120.98221244592699,137.02127659574467,940.99852088490491,1.5923566878980893E-3,5.0457768805471881,2.6292254559200514,45.840248384041111,7664.1922040069494,0,-6207.9956852456289,0,0,0,0,0,8.3613048660831417,11.894732549032192,100.3356583929977,285.4735811767726,181.73812626571524,127369.9980435483,103251.48748849278,993279.30963930057,5.7231399054328129,157.46440871065298,-48514.434673127973,79.335292413997593,3.0286989288705195,51.495398114105576,-50560.171869168778,120.98221244592699,35.507828047373188,11.158964355364494,263.5665902200102,-44387.319488529967,52.355737252844804]
["KBM","KBM-163H02-A (480 V)",1090,40.6,781.87301838940914,28.74533155843416,245,2915,291,0.50900000000000001,6.3,1645,1570,679,56,79.335292413997593,121.01149297110726,137.02127659574467,937.80854665559787,1.5923566878980893E-3,5.159518443790601,2.6292254559200514,45.840248384041111,7664.1922040069494,0,-6207.9956852456289,0,0,0,0,0,8.3613048660831417,11.894732549032192,100.3356583929977,285.4735811767726,181.73812626571524,127369.9980435483,103251.48748849278,993279.30963930057,5.7231399054328129,157.46440871065298,-48514.434673127973,79.335292413997593,3.0277826161821659,51.422229151390709,-50560.867573756885,121.01149297110726,35.457375559546463,11.158964355364494,263.5665902200102,-44387.319488529967,52.355737252844804]
["KBM","KBM-163H03-A (400 V)",1375,38.6,1115.3578411880026,30.810990088066365,150,3930,183,0.64,8.4,2190,1680,565,56,55.760958441430503,89.656740027561341,102.92237442922375,1219.8088697813196,1.488095238095238E-3,4.8572591990888192,2.0865954494984478,54.283046175611304,8200.3201165288992,0,-6642.2592943884065,0,0,0,0,0,6.7425402614389229,9.5918895908489539,80.910483137267079,230.20535018037489,146.55327762962963,136279.82302592689,110474.16705843504,1062761.4871021451,10.334029821388199,267.83163534448545,-47065.987292419813,55.760958441430503,5.3392207244409331,83.875734552702824,-50438.44856535751,89.656740027561341,34.550283905879404,14.568116817197367,355.77895237496466,-44207.160429879106,44.212699343285749]
["KBM","KBM-163H03-A (480 V)",1375,38.6,1063.9507945693204,29.390905927329289,180,3930,220,0.64,8.4,2190,1680,679,56,55.760958441430503,89.628564432611356,102.92237442922375,1220.1172569407986,1.488095238095238E-3,4.8465758603698132,2.0865954494984478,54.283046175611304,8200.3201165288992,0,-6642.2592943884065,0,0,0,0,0,6.7425402614389229,9.5918895908489539,80.910483137267079,230.20535018037489,146.55327762962963,136279.82302592686,110474.16705843504,1062761.4871021451,10.334029821388199,267.83163534448545,-47065.987292419813,55.760958441430503,5.3410983147197353,84.020590368486438,-50437.180829117984,89.628564432611356,34.609953243947572,14.568116817197367,355.77895237496466,-44207.160429879106,44.212699343285749]
["KBM","KBM-163S01-A (240 V)",776,43.2,580.77085597351629,32.086787622846202,165,1966,219,0.37,4.2,1100,1060,325,56,124.63196098866862,187.02715822431577,204.90909090909091,554.70816963734001,2.3584905660377358E-3,7.5300161731264765,2.6340326785099903,28.260199776304717,5178.5082459506411,0,-4194.5916792200196,0,0,0,0,0,8.4437396357791012,12.012003663287571,101.32487562934921,288.28808791890168,183.52989690721648,86060.809488883984,69764.518573305948,671134.66867520311,2.5725241885138996,77.154378213855807,-49575.243041825066,124.63196098866862,1.3279961600197558,22.705046844439746,-50698.647778469385,187.02715822431577,32.208267586241647,5.0413055093993595,129.37842420352908,-47346.735072440431,84.925089666645746]
["KBM","KBM-163S02-A (240 V)",1090,40.6,945.38036196585824,34.756630954627141,110,2915,146,0.50900000000000001,6.3,1645,1570,325,56,79.335292413997593,121.30300122833435,137.02127659574467,930.52003518093852,1.5923566878980893E-3,5.4273808524515168,2.6292254559200514,45.840248384041111,7664.1922040069494,0,-6207.9956852456289,0,0,0,0,0,8.3613048660831417,11.894732549032192,100.3356583929977,285.4735811767726,181.73812626571524,127369.9980435483,103251.48748849278,993279.30963930057,5.7231399054328129,157.46440871065298,-48514.434673127973,79.335292413997593,3.0187137490896392,50.692371514017324,-50567.753053490349,121.30300122833435,34.954113900524206,11.158964355364494,263.5665902200102,-44387.319488529967,52.355737252844804]
["KBM","KBM-163S03-A (240 V)",1375,38.6,1209.1796801406749,33.402753595046264,80,3930,110,0.64,8.4,2190,1680,325,56,55.760958441430503,90.135457801201198,102.92237442922375,1188.1713694592265,1.488095238095238E-3,6.5648864847700521,2.0865954494984478,54.283046175611304,8200.3201165288992,0,-6642.2592943884065,0,0,0,0,0,6.7425402614389229,9.5918895908489539,80.910483137267079,230.20535018037489,146.55327762962963,136279.82302592689,110474.16705843504,1062761.4871021451,10.334029821388199,267.83163534448545,-47065.987292419813,55.760958441430503,5.3077208414746826,81.407096059947079,-50459.717072990898,90.135457801201198,33.533396706732432,14.568116817197367,355.77895237496466,-44207.160429879106,44.212699343285749]
["KBM","KBM-260H01-A (400 V)",1932,33.1,1710.4475354640751,28.84397193025422,85,6494,111,1.06,16,3584,4880,565,58,25.138950014405914,52.088134936346584,62.890625000000007,1796.2322980208542,5.1229508196721314E-4,11.077814497221041,3.6644238498311941,"NA",23796.768480803774,0,-19275.382469451055,0,0,0,0,0,11.941173064883133,16.987427465377092,143.2940767785976,407.69825916905017,259.54877294685991,395474.7316042129,320588.48182039178,3084061.1951121688,34.764057805170467,732.0953520520244,-40373.839099254656,25.138950014405914,14.531281091710188,203.05563080551812,-50002.680252114376,52.088134936346584,30.858907278163738,132.13186484504541,1707.8647451919408,5963.8020790585433,-9999]
["KBM","KBM-260H01-A (480 V)",1932,33.1,1680.6761990504149,28.341925784998566,105,6494,134,1.06,16,3584,4880,679,58,25.138950014405914,52.002407495918554,62.890625000000007,1807.5291170437768,5.1229508196721314E-4,9.8263716199073965,3.6644238498311941,"NA",23796.768480803774,0,-19275.382469451055,0,0,0,0,0,11.941173064883133,16.987427465377092,143.2940767785976,407.69825916905017,259.54877294685991,395474.7316042129,320588.48182039178,3084061.1951121688,34.764057805170467,732.0953520520244,-40373.839099254656,25.138950014405914,14.55462479068402,204.45632666340759,-49991.57091341498,52.002407495918554,31.0717747737956,132.13186484504541,1707.8647451919408,5963.8020790585433,-9999]
["KBM","KBM-260H02-A (400 V)",2706,31,2428.9938042061262,27.322764951699956,55,9741,74,1.48,24,5380,7190,565,58,12.164848459155289,33.370192609634884,41.895910780669148,2537.9318162235672,3.4770514603616132E-4,28.538438412635998,3.598753171518807,"NA",35055.4546437647,0,-28394.918261449402,0,0,0,0,0,11.76244595950488,16.733171562526262,141.14935151405857,401.59611750063033,255.66402890695574,582581.056234163,472264.75278917921,4543186.921831904,78.559271215097397,1539.012202733609,-30347.329122844534,12.164848459155289,32.327655676717619,401.88661190753004,-49410.133251902669,33.370192609634884,29.140628901903842,289.36553992675624,3525.9345537780227,56574.976378071588,-9999]
["KBM","KBM-260H02-A (480 V)",2706,31,2406.2823087173174,27.067292561499631,68,9741,89,1.48,24,5380,7190,679,58,12.164848459155289,33.290316813320771,41.895910780669148,2559.2691632741535,3.4770514603616132E-4,17.21523848863233,3.598753171518807,"NA",35055.4546437647,0,-28394.918261449402,0,0,0,0,0,11.76244595950488,16.733171562526262,141.14935151405857,401.59611750063033,255.66402890695574,582581.056234163,472264.75278917921,4543186.921831904,78.559271215097397,1539.012202733609,-30347.329122844534,12.164848459155289,32.38618604489789,405.34802733237132,-49385.999270616732,33.290316813320771,29.391614675955541,289.36553992675624,3525.9345537780227,56574.976378071588,-9999]
["KBM","KBM-260H03-A (400 V)",3444,29.5,3366.1270463935866,28.286781902467116,40,12812,55,1.9,32,7180,9560,565,58,5.4500661577046099,23.720607575128202,31.392757660167131,3397.8201556696526,2.6150627615062759E-4,6.3865629194493678,3.6377282402088489,"NA",46606.574213555774,0,-37751.325112980172,0,0,0,0,0,11.69268339517126,16.633927837058355,140.31220074205513,399.21426808940055,254.14769647696477,774547.28539995605,627880.66715975327,6040212.0180768268,136.85574434483163,2593.07140327052,-18197.467135752424,5.4500661577046099,57.472626591589183,683.12567954249289,-48542.11941386632,23.720607575128202,28.910921783771027,509.04787957799931,6005.1636941387123,124075.11227346209,-9999]
["KBM","KBM-260H03-A (480 V)",3444,29.5,3288.7777440509253,27.636787765133825,50,12812,67,1.9,32,7180,9560,679,58,5.4500661577046099,23.758033230651726,31.392757660167131,3370.244489700503,2.6150627615062759E-4,8.0213412408425633,3.6377282402088489,"NA",46606.574213555774,0,-37751.325112980172,0,0,0,0,0,11.69268339517126,16.633927837058355,140.31220074205513,399.21426808940055,254.14769647696477,774547.28539995593,627880.66715975327,6040212.0180768268,136.85574434483163,2593.07140327052,-18197.467135752424,5.4500661577046099,57.417601772080118,679.94365465045928,-48563.152966867579,23.758033230651726,28.776253631888334,509.04787957799931,6005.1636941387123,124075.11227346209,-9999]
["KBM","KBM-260S01-A (240 V)",1932,33.1,1761.3147035503084,29.701765658521222,45,6494,67,1.06,16,3584,4880,325,58,25.138950014405914,52.546058664218023,62.890625000000007,1732.6924533252236,5.1229508196721314E-4,38.150643519107781,3.6644238498311941,"NA",23796.768480803774,0,-19275.382469451055,0,0,0,0,0,11.941173064883133,16.987427465377092,143.2940767785976,407.69825916905017,259.54877294685991,395474.7316042129,320588.48182039178,3084061.1951121688,34.764057805170467,732.0953520520244,-40373.839099254656,25.138950014405914,14.409112507809995,195.5615555973325,-50060.820659874735,52.546058664218023,29.720012626153419,132.13186484504541,1707.8647451919408,5963.8020790585433,-9999]
["KBM","KBM-260S02-A (240 V)",2706,31,2482.8171122335671,27.928201487441697,28,9741,44,1.48,24,5380,7190,325,58,12.164848459155289,33.749365090397923,41.895910780669148,2436.9899728157625,3.4770514603616132E-4,"NA",3.598753171518807,"NA",35055.4546437647,0,-28394.918261449402,0,0,0,0,0,11.76244595950488,16.733171562526262,141.14935151405857,401.59611750063033,255.66402890695574,"NA",472264.75278917921,4543186.921831904,78.559271215097397,1539.012202733609,-30347.329122844534,12.164848459155289,32.056614746298315,385.45253587329114,-49521.89227454058,33.749365090397923,27.949000972855991,289.36553992675624,3525.9345537780227,56574.976378071588,-9999]
["KBM","KBM-260S03-A (240 V)",3444,29.5,3317.1240770731874,27.874992244312498,19,12812,33,1.9,32,7180,9560,325,58,5.4500661577046099,24.018758094503625,31.392757660167131,3283.6104157475793,2.6150627615062759E-4,38.216615986559646,3.6377282402088489,"NA",46606.574213555774,0,-37751.325112980172,0,0,0,0,0,11.69268339517126,16.633927837058355,140.31220074205513,399.21426808940055,254.14769647696477,774547.28539995581,627880.66715975327,6040212.0180768268,136.85574434483163,2593.07140327052,-18197.467135752424,5.4500661577046099,57.04172036785944,657.79525378934704,-48706.835790517071,24.018758094503625,27.838899490319438,509.04787957799931,6005.1636941387123,124075.11227346209,-9999]
["KBM","KBMS-10H01-A (120 V)",0.48699999999999999,1.73,0.44870188775305436,1.5599425940517813,4150,1.17,6565,13,19,17.382100000000001,1.0200000000000001E-2,160,6,6565,6565,6565,0.42641515496356674,245.09803921568627,8.9058765819157273,10.45678543910331,"NA",12.234438963750872,0,-9.9098955606382066,0,0,0,0,0,1.272944110792656,1.8108811950110377,15.275329329511871,43.461148680264905,27.668226579663852,203.32220609787919,164.82154778608245,1585.5832897021132,7.6374634761367834E-4,1.6267065951735979,-48615.614495876362,6984.1633420898688,3.4884847190161828E-4,0.51746625424180959,-50583.595801132462,11322.803746368232,1.3221350221162802,2.0758615145515632E-2,10.828979892518975,46225.864091563475,-9999]
["KBM","KBMS-10H01-A (240 V)",0.48699999999999999,1.73,0.414767427451606,1.4419671375733765,9900,1.17,13766,13,19,17.382100000000001,1.0200000000000001E-2,325,6,6984.1633420898688,11126.671553299979,12967.3629768555,0.4058173626064755,245.09803921568627,8.8898119079186131,10.45678543910331,"NA",12.234438963750872,0,-9.9098955606382066,0,0,0,0,0,1.272944110792656,1.8108811950110377,15.275329329511871,43.461148680264905,27.668226579663852,203.32220609787919,164.82154778608245,1585.5832897021132,7.6374634761367834E-4,1.6267065951735979,-48615.614495876362,6984.1633420898688,3.5757999980040893E-4,0.56375954799121597,-50542.179624581426,11126.671553299979,1.4404151697654941,2.0758615145515632E-2,10.828979892518975,46225.864091563475,-9999]
["KBM","KBMS-10H01-A (400 V)",0.48699999999999999,1.73,0.36804580590000802,1.2795362463496316,14400,1.17,16000,13,19,17.382100000000001,1.0200000000000001E-2,565,6,6984.1633420898688,11163.039983039611,12967.3629768555,0.39478538716052325,245.09803921568627,8.8978234238670098,10.45678543910331,"NA",12.234438963750872,0,-9.9098955606382066,0,0,0,0,0,1.272944110792656,1.8108811950110377,15.275329329511871,43.461148680264905,27.668226579663852,203.32220609787919,164.82154778608245,1585.5832897021132,7.6374634761367834E-4,1.6267065951735979,-48615.614495876362,6984.1633420898688,3.5591619643894937E-4,0.55523605013734312,-50550.07152787294,11163.039983039611,1.4186374887454054,2.0758615145515632E-2,10.828979892518975,46225.864091563475,-9999]
["KBM","KBMS-10H01-B (120 V)",0.50900000000000001,3.37,0.4297183463481174,2.790016532580947,9000,1.19,12319,3.42,5.2,9.3041110000000007,1.0200000000000001E-2,160,6,12319,12319,12319,0.40048103429582871,245.09803921568627,8.5145752205312153,10.281041146009137,1.1961670123962582,12.234438963750872,0,-9.9098955606382066,0,0,0,0,0,2.3724895751522301,3.375086714787201,28.46987490182676,81.002081154892821,51.567526466128214,203.32220609787919,164.82154778608245,1585.5832897021132,2.1081346565340067E-4,0.43423087158044971,-50260.617682449483,14445.035458791341,9.5357615227737545E-5,0.11550484764039251,-50766.630740183718,22475.700675054195,2.095745755170503,5.4091231787353408E-3,2.8420905889786536,-27477.773995721091,2006.4087833287815]
["KBM","KBMS-10H01-B (240 V)",0.50900000000000001,3.37,0.30970691628693148,2.0108227261844664,18500,1.19,20000,3.42,5.2,9.3041110000000007,1.0200000000000001E-2,325,6,14445.035458791341,20000,20000,0.29354801760749349,245.09803921568627,8.5295502328072779,10.281041146009137,1.1961670123962582,12.234438963750872,0,-9.9098955606382066,0,0,0,0,0,2.3724895751522301,3.375086714787201,28.46987490182676,81.002081154892821,51.567526466128214,203.32220609787919,164.82154778608245,1585.5832897021132,2.1081346565340067E-4,0.43423087158044971,-50260.617682449483,14445.035458791341,9.3923985877269214E-5,0.10566788939462363,-50772.913965924236,22694.544256081987,1.9172617875404709,5.4091231787353408E-3,2.8420905889786536,-27477.773995721091,2006.4087833287815]
["KBM","KBMS-10H01-C (120 V)",0.49199999999999999,5.21,0.34500684437985052,3.8004719583592257,15500,1.23,19702,1.44,2.2000000000000002,5.8349039999999999,1.0200000000000001E-2,160,6,19702,19702,19702,0.30515747406269778,245.09803921568627,8.816677396729844,9.9466983445129049,0.63173936160358357,12.234438963750872,0,-9.9098955606382066,0,0,0,0,0,3.7945896235618246,5.3981560807200246,45.535075482741895,129.55574593728059,82.477749487503772,203.32220609787919,164.82154778608245,1585.5832897021132,9.482626404107243E-5,0.18955470407524055,-50541.319348000005,22108.68721575549,3.5908595233953593E-5,3.3181857024775656E-2,-50797.075113008796,37152.261489945362,2.2800472816340704,2.4711832822282421E-3,1.2003105870937121,-40225.788889553965,3799.0350860961548]
["KBM","KBMS-10H01-C (240 V)",0.49199999999999999,5.21,0.29520674928335428,3.2518919286555881,18600,1.23,20000,1.44,2.2000000000000002,5.8349039999999999,1.0200000000000001E-2,325,6,20000,20000,20000,0.28039435406812285,245.09803921568627,8.8256401379696765,9.9466983445129049,0.63173936160358357,12.234438963750872,0,-9.9098955606382066,0,0,0,0,0,3.7945896235618246,5.3981560807200246,45.535075482741895,129.55574593728059,82.477749487503772,203.32220609787919,164.82154778608245,1585.5832897021132,9.482626404107243E-5,0.18955470407524055,-50541.319348000005,22108.68721575549,3.5230358122647138E-5,2.6459155315921103E-2,-50800.019273135484,37599.209170185713,1.818105753013004,2.4711832822282421E-3,1.2003105870937121,-40225.788889553965,3799.0350860961548]
["KBM","KBMS-10H02-A (120 V)",0.876,1.53,0.85343954991306192,1.4551398975499776,2070,2.33,3359,20,36,35.4,1.49E-2,160,6,3232.9351243946576,3359,3359,0.83939103775747581,167.78523489932886,4.945708451720237,5.2606636254445913,"NA",12.257346247285898,0,-9.928450460301578,0,0,0,0,0,0.62703518982405582,0.89201577998227866,7.5244222778886698,21.408378719574689,13.62899718721461,203.7028986198535,165.13015318588904,1588.5520736482526,2.8418987989117139E-3,4.9904203768525361,-45836.86075295553,3232.9351243946576,1.4309988553336968E-3,1.6696452530329784,-50249.022860493562,5371.024467160214,1.3615397405222756,1.9072590255100701E-2,16.713129833804064,4919.7092987311189,-9999]
["KBM","KBMS-10H02-A (240 V)",0.876,1.53,0.79409940026903569,1.3539631718142127,4750,2.33,6753,20,36,35.4,1.49E-2,325,6,3232.9351243946576,5374.6830528703349,6367.2316384180795,0.78332847044338305,167.78523489932886,4.9620255470848544,5.2606636254445913,"NA",12.257346247285898,0,-9.928450460301578,0,0,0,0,0,0.62703518982405582,0.89201577998227866,7.5244222778886698,21.408378719574689,13.62899718721461,203.7028986198535,165.13015318588904,1588.5520736482526,2.8418987989117139E-3,4.9904203768525361,-45836.86075295553,3232.9351243946576,1.4299101100079922E-3,1.6645265481743534,-50252.427581638178,5374.6830528703349,1.3573656082792962,1.9072590255100701E-2,16.713129833804064,4919.7092987311189,-9999]
["KBM","KBMS-10H02-A (400 V)",0.876,1.53,0.70832694452986378,1.2077185754984889,9100,2.33,11291,20,36,35.4,1.49E-2,565,6,3232.9351243946576,5367.9663950772874,6367.2316384180795,0.7770919420743273,167.78523489932886,4.9650814399722512,5.2606636254445913,"NA",12.257346247285898,0,-9.928450460301578,0,0,0,0,0,0.62703518982405582,0.89201577998227866,7.5244222778886698,21.408378719574689,13.62899718721461,203.7028986198535,165.13015318588904,1588.5520736482526,2.8418987989117139E-3,4.9904203768525361,-45836.86075295553,3232.9351243946576,1.4319111644315839E-3,1.6739223948584474,-50246.169890195859,5367.9663950772874,1.3650276063193048,1.9072590255100701E-2,16.713129833804064,4919.7092987311189,-9999]
["KBM","KBMS-10H02-A (480 V)",0.876,1.53,0.64240722484365043,1.0953234865194381,11000,2.33,13564,20,36,35.4,1.49E-2,679,6,3232.9351243946576,5384.7023918536497,6367.2316384180795,0.76165203862689757,167.78523489932886,4.9723531819946922,5.2606636254445913,"NA",12.257346247285898,0,-9.928450460301578,0,0,0,0,0,0.62703518982405582,0.89201577998227866,7.5244222778886698,21.408378719574689,13.62899718721461,203.7028986198535,165.13015318588904,1588.5520736482526,2.8418987989117139E-3,4.9904203768525361,-45836.86075295553,3232.9351243946576,1.4269436058521961E-3,1.6504990625304692,-50261.704424611795,5384.7023918536497,1.3459266639112875,1.9072590255100701E-2,16.713129833804064,4919.7092987311189,-9999]
["KBM","KBMS-10H02-B (120 V)",0.89900000000000002,2.99,0.82321522288911386,2.6814828107137259,4350,2.48,6174,5.22,9.6999999999999993,18.536100000000001,1.49E-2,160,6,6174,6174,6174,0.79143788186606645,167.78523489932886,4.8344079399680231,4.9424783255185076,1.036900466727291,12.257346247285898,0,-9.928450460301578,0,0,0,0,0,1.1940323311993426,1.6986218612988893,14.328387974392111,40.766924671173342,25.95303030428871,203.7028986198535,165.13015318588904,1588.5520736482526,8.1742603491368859E-4,1.3823329860401852,-49414.795648000007,6975.3703801771735,3.8048460499725162E-4,0.38574146469242288,-50696.89304272797,11047.308032028172,2.3016900011450252,5.034751101956534E-3,4.3494823011799584,-37040.090227617606,2314.59052919031]
["KBM","KBMS-10H02-B (240 V)",0.89900000000000002,2.99,0.70664794732801528,2.301784844716662,10000,2.48,12944,5.22,9.6999999999999993,18.536100000000001,1.49E-2,325,6,6975.3703801771735,11033.694352896799,12160.055243551773,0.68676462426650153,167.78523489932886,4.8388543810351141,4.9424783255185076,1.036900466727291,12.257346247285898,0,-9.928450460301578,0,0,0,0,0,1.1940323311993426,1.6986218612988893,14.328387974392111,40.766924671173342,25.95303030428871,203.7028986198535,165.13015318588904,1588.5520736482526,8.1742603491368859E-4,1.3823329860401852,-49414.795648000007,6975.3703801771735,3.8114154147706505E-4,0.38916024560424139,-50694.965423849091,11033.694352896799,2.3220896069979053,5.034751101956534E-3,4.3494823011799584,-37040.090227617606,2314.59052919031]
["KBM","KBMS-10H02-B (400 V)",0.89900000000000002,2.99,0.49317090918607037,1.6064198996288936,15200,2.48,16000,5.22,9.6999999999999993,18.536000000000001,1.49E-2,565,6,6975.3885560271547,11175.287413880231,12160.120845921449,0.60062784666056812,167.78523489932886,4.8572425023480603,4.9424783255185076,1.0368992652598625,12.257346247285898,0,-9.928450460301578,0,0,0,0,0,1.1940323311993426,1.6986218612988893,14.328387974392111,40.766924671173342,25.95303030428871,203.7028986198535,165.13015318588904,1588.5520736482526,8.1742232770368856E-4,1.382325528522228,-49414.795648000007,6975.3885560271547,3.7449115639235151E-4,0.35304444580790573,-50714.468468887404,11175.287413880231,2.1066007394856836,5.0347473947465341E-3,4.3494588362531328,-37040.090227617606,2314.5932111337006]
["KBM","KBMS-10H02-C (120 V)",0.86799999999999999,5.14,0.70215416069953829,4.058694570517563,8500,2.2400000000000002,11008,1.77,3.2,10.46,1.49E-2,160,6,{"$f":"IF(AQ1056<I1056,IF(AQ1056<0,0,AQ1056),I1056)","v":11008},{"$f":"IF(AU1056<I1056,IF(AU1056<0,0,AU1056),I1056)","v":11008},{"$f":"IF(UAC_V*0.98/L1056*1000<I1056,IF(UAC_V*0.98/L1056*1000<0,0,UAC_V*0.98/L1056*1000),I1056)","v":11008},{"$f":"C1056+(E1056-C1056)/G1056*Q1056","v":0.65321988246829621},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M1056,(inertia/gear^2+gear_inertia)/M1056),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M1056,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M1056))","v":167.78523489932886},{"$f":"IF((C1056+(E1056-C1056)/G1056*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X1056^2*time1+Y1056^2*time2+Z1056^2*time3+AA1056^2*time4)/time)/(C1056+(E1056-C1056)/G1056*mspeed),SQRT((((X1056-Y1056)*2/PI()+Y1056)^2*time1+Y1056^2*time2+((Z1056-Y1056)*2/PI()+Y1056)^2*time3+AA1056^2*time4)/time)/(C1056+(E1056-C1056)/G1056*mspeed)),IF(AccType=1,SQRT((X1056^2*time1+Y1056^2*time2+Z1056^2*time3+AA1056^2*time4+AB1056^2*time5+AC1056^2*time6+AD1056^2*time7+AE1056^2*time8)/time)/(C1056+(E1056-C1056)/G1056*mspeed),SQRT((((X1056-Y1056)*2/PI()+Y1056)^2*time1+Y1056^2*time2+((Z1056-Y1056)*2/PI()+Y1056)^2*time3+AA1056^2*time4+((AB1056-AC1056)*2/PI()+AC1056)^2*time5+AC1056^2*time6+((AD1056-AC1056)*2/PI()+AC1056)^2*time7+AE1056^2*time8)/time)/(C1056+(E1056-C1056)/G1056*mspeed))))","v":5.0141448218743747},{"$f":"IF(move1,MAX(ABS(X1056),ABS(Z1056))/H1056,MAX(ABS(X1056),ABS(Z1056),ABS(AB1056),ABS(AD1056))/H1056)","v":5.472029574681204},{"$f":"IF(AZ1056>0,speed/(MIN(AZ1056,I1056)),\"NA\")","v":0.50666785692846983},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M1056+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M1056+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.257346247285898},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M1056+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M1056+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-9.928450460301578},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M1056+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M1056+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M1056+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M1056+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH1056/Irms","v":2.1259252184492836},{"$f":"AI1056/Ipeak","v":3.0243260229958486},{"$f":"IF(move1,IF(AccType=1,SQRT((X1056^2*time1+Y1056^2*time2+Z1056^2*time3+AA1056^2*time4)/time)/(C1056/D1056),SQRT((((X1056-Y1056)*2/PI()+Y1056)^2*time1+Y1056^2*time2+((Z1056-AA1056)*2/PI()+AA1056)^2*time3+AA1056^2*time4)/time)/(C1056/D1056)),IF(AccType=1,SQRT((X1056^2*time1+Y1056^2*time2+Z1056^2*time3+AA1056^2*time4+AB1056^2*time5+AC1056^2*time6+AD1056^2*time7+AE1056^2*time8)/time)/(C1056/D1056),SQRT((((X1056-Y1056)*2/PI()+Y1056)^2*time1+Y1056^2*time2+((Z1056-AA1056)*2/PI()+AA1056)^2*time3+AA1056^2*time4+((AB1056-AC1056)*2/PI()+AC1056)^2*time5+AC1056^2*time6+((AD1056-AE1056)*2/PI()+AE1056)^2*time7+AE1056^2*time8)/time)/(C1056/D1056)))","v":25.511102621391402},{"$f":"IF(move1,MAX(ABS(X1056),ABS(Z1056))/(C1056/D1056),MAX(ABS(X1056),ABS(Z1056),ABS(AB1056),ABS(AD1056))/(C1056/D1056))","v":72.583824551900364},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X1056),ABS(Z1056))/(C1056/D1056),MAX(ABS((X1056-Y1056)*2/PI()+Y1056),ABS((Z1056-Y1056)*2/PI()+Y1056))/(C1056/D1056)),IF(AccType=1,MAX(ABS(X1056),ABS(Z1056),ABS(AB1056),ABS(AD1056))/(C1056/D1056),MAX(ABS((X1056-Y1056)*2/PI()+Y1056),ABS((Z1056-Y1056)*2/PI()+Y1056),ABS((AB1056-AC1056)*2/PI()+AC1056),ABS((AD1056-AC1056)*2/PI()+AC1056))/(C1056/D1056)))","v":46.208297863799274},{"$f":"IF((C1056+(E1056-C1056)/G1056*mspeed)<0,\"NA\",U1056*(C1056+(E1056-C1056)/G1056*mspeed)*mspeed/9.55)","v":203.7028986198535},{"$f":"IF(move1,IF(speed1>speed2,AM1056/2*time1/time,AM1056/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z1056*-speed/30*PI(),((Z1056-AA1056)*2/PI()+AA1056)*-speed/30*PI()),IF(AccType=1,X1056*-speed/30*PI(),((X1056-Y1056)*2/PI()+Y1056)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z1056*-speed/30*PI(),((Z1056-AA1056)*2/PI()+AA1056)*-speed/30*PI()),IF(AccType=1,X1056*-speed/30*PI(),((X1056-Y1056)*2/PI()+Y1056)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD1056*-speed/30*PI(),((AD1056-AE1056)*2/PI()+AE1056)*-speed/30*PI()),IF(AccType=1,AB1056*-speed/30*PI(),((AB1056-AC1056)*2/PI()+AC1056)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD1056*-speed/30*PI(),((AD1056-AE1056)*2/PI()+AE1056)*-speed/30*PI()),IF(AccType=1,AB1056*-speed/30*PI(),((AB1056-AC1056)*2/PI()+AC1056)*-speed/30*PI()),0)/2*time7/time)))","v":165.13015318588904},{"$f":"IF(move1,MAX(IF(AccType=1,Z1056*-speed/30*PI(),((Z1056-AA1056)*2/PI()+AA1056)*-speed/30*PI()),IF(AccType=1,X1056*-speed/30*PI(),((X1056-Y1056)*2/PI()+Y1056)*-speed/30*PI()),0),MAX(IF(AccType=1,Z1056*-speed/30*PI(),((Z1056-AA1056)*2/PI()+AA1056)*-speed/30*PI()),IF(AccType=1,X1056*-speed/30*PI(),((X1056-Y1056)*2/PI()+Y1056)*-speed/30*PI()),IF(AccType=1,AD1056*-speed/30*PI(),((AD1056-AE1056)*2/PI()+AE1056)*-speed/30*PI()),IF(AccType=1,AB1056*-speed/30*PI(),((AB1056-AC1056)*2/PI()+AC1056)*-speed/30*PI()),0))","v":1588.5520736482526},{"$f":"(L1056^2)/1000000+((K1056/1000)^2*(D1056/C1056*H1056)^2*PI()*PI()*(O1056/2)^2)/1200","v":2.4277718973342478E-4},{"$f":"SQRT(3)*L1056*J1056*D1056/C1056*H1056/1000","v":0.42536033604146428},{"$f":"0.75*J1056^2*(D1056/C1056*H1056)^2-(UAC_V*0.98)^2","v":-50391.740820778359},{"$f":"-AO1056/2/AN1056+SQRT((AO1056/2/AN1056)^2-AP1056/AN1056)","v":13557.651387176016},{"$f":"(L1056^2)/1000000+((K1056/1000)^2*AV1056^2*PI()*PI()*(O1056/2)^2)/1200","v":1.1566817274879376E-4},{"$f":"SQRT(3)*L1056*J1056*AV1056/1000","v":9.2130482346528653E-2},{"$f":"0.75*J1056^2*AV1056^2-(UAC_V*0.98)^2","v":-50785.765288247771},{"$f":"-AS1056/2/AR1056+SQRT((AS1056/2/AR1056)^2-AT1056/AR1056)","v":20559.392134290039},{"$f":"D1056+(F1056-D1056)*((0.85*UAC_V-D1056*J1056)/L1056*1000)/G1056","v":2.873014161202665},{"$f":"(L1056^2)/1000000+((K1056/1000)^2*AJ1056^2*PI()*PI()*(O1056/2)^2)/1200","v":1.7278676393976998E-3},{"$f":"SQRT(3)*L1056*J1056*AJ1056/1000","v":1.4817862118792358},{"$f":"0.75*J1056^2*AJ1056^2-(UAC_V*0.98)^2","v":-45788.11798225368},{"$f":"IF(((AX1056/2/AW1056)^2-AY1056/AW1056)>0,-AX1056/2/AW1056+SQRT((AX1056/2/AW1056)^2-AY1056/AW1056),-9999)","v":4736.8309774954332}]
["KBM","KBMS-10H02-C (240 V)",0.86799999999999999,5.14,0.25034642399860291,1.4470891560612886,18500,2.2400000000000002,20000,1.77,3.2,10.46,1.49E-2,325,6,13557.651387176016,20000,20000,0.20026640432281406,167.78523489932886,5.0509786596066473,5.472029574681204,0.50666785692846983,12.257346247285898,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-9.928450460301578,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},2.1259252184492836,3.0243260229958486,25.511102621391402,72.583824551900364,46.208297863799274,203.7028986198535,165.13015318588904,1588.5520736482526,2.4277718973342478E-4,0.42536033604146428,-50391.740820778359,13557.651387176016,1.1131038752446128E-4,5.075435118320977E-2,-50799.273960119339,21136.165128395456,1.5827331625547396,1.7278676393976998E-3,1.4817862118792358,-45788.11798225368,4736.8309774954332]
["KBM","KBMS-10H03-A (120 V)",1.1579999999999999,1.54,1.0725659208366858,1.3983910310778171,1380,3.46,2455,21.2,41,46.4,2.0199999999999999E-2,160,6,2310.3946797151139,2455,2455,1.0060140113435243,123.76237623762377,3.8203624250598329,3.5500514060373498,4.3900247742349059,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,0.47844391745710135,0.68063089780978048,5.7413270094852162,16.335141547434731,10.399274093520118,204.13219018718632,165.47815501971357,1591.8998512896444,4.7875027048190433E-3,7.8397593019290408,-43668.261739908907,2310.3946797151139,2.3261729099704116E-3,2.0102044806659736,-50335.93135036304,4239.7082302178624,1.1798472044147406,1.5609542313967549E-2,17.718114091593257,-14351.67654434876,546.69395354796654]
["KBM","KBMS-10H03-A (240 V)",1.1579999999999999,1.54,1.0203357995480415,1.3302943931525966,3650,3.46,5155,21.2,41,46.4,2.0199999999999999E-2,325,6,2310.3946797151139,4141.8289707708991,4857.7586206896558,1.0017858702274154,123.76237623762377,3.7837838434858684,3.5500514060373498,4.3900247742349059,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,0.47844391745710135,0.68063089780978048,5.7413270094852162,16.335141547434731,10.399274093520118,204.13219018718632,165.47815501971357,1591.8998512896444,4.7875027048190433E-3,7.8397593019290408,-43668.261739908907,2310.3946797151139,2.3758393930769293E-3,2.2802636594620598,-50201.38631671475,4141.8289707708991,1.3383527545682963,1.5609542313967549E-2,17.718114091593257,-14351.67654434876,546.69395354796654]
["KBM","KBMS-10H03-A (400 V)",1.1579999999999999,1.54,0.98952855922352334,1.290128499639535,6900,3.46,8619,21.2,41,46.4,2.0199999999999999E-2,565,6,2310.3946797151139,4095.2708645207313,4857.7586206896558,1.0580092488527921,123.76237623762377,3.7639712597092725,3.5500514060373498,4.3900247742349059,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,0.47844391745710135,0.68063089780978048,5.7413270094852162,16.335141547434731,10.399274093520118,204.13219018718632,165.47815501971357,1591.8998512896444,4.7875027048190433E-3,7.8397593019290408,-43668.261739908907,2310.3946797151139,2.4013602773246723E-3,2.4072774404987616,-50132.25099617106,4095.2708645207313,1.4129008196629733,1.5609542313967549E-2,17.718114091593257,-14351.67654434876,546.69395354796654]
["KBM","KBMS-10H03-A (480 V)",1.1579999999999999,1.54,0.87628839255302382,1.1424881258839945,8500,3.46,10354,21.2,41,46.4,2.0199999999999999E-2,679,6,2310.3946797151139,4118.437308722986,4857.7586206896558,1.0215045183047116,123.76237623762377,3.7769471302986499,3.5500514060373498,4.3900247742349059,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,0.47844391745710135,0.68063089780978048,5.7413270094852162,16.335141547434731,10.399274093520118,204.13219018718632,165.47815501971357,1591.8998512896444,4.7875027048190433E-3,7.8397593019290408,-43668.261739908907,2310.3946797151139,2.3885078541233109E-3,2.34417313126011,-50167.067830461106,4118.437308722986,1.3758630737232767,1.5609542313967549E-2,17.718114091593257,-14351.67654434876,546.69395354796654]
["KBM","KBMS-10H03-B (120 V)",1.17,2.4,1.0672743242632983,2.1431211330588318,2550,3.57,3799,8.77,17,30,2.0199999999999999E-2,160,6,3799,3799,3799,1.0169588854416747,123.76237623762377,3.7481728211188874,3.4406660685964234,1.2856376367164881,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,0.73797942912463987,1.0498442619563446,8.855753149495678,25.196262286952269,16.040438761633428,204.13219018718632,165.47815501971357,1591.8998512896444,2.0472182408516689E-3,3.3371449556365054,-47711.677651408289,4080.8637159773002,9.7040983989819189E-4,0.82673957654369268,-50615.299353493436,6808.6739522628959,1.8142087307762003,6.404163660129184E-3,7.3096691270436605,-35963.142570317985,1866.7779562906912]
["KBM","KBMS-10H03-B (240 V)",1.17,2.4,0.98185139021865797,1.971589136985257,6030,3.57,7967,8.77,17,30,2.0199999999999999E-2,325,6,4080.8637159773002,6722.6106544824161,7513.3333333333339,0.96024048942917006,123.76237623762377,3.7348739435189944,3.4406660685964234,1.2856376367164881,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,0.73797942912463987,1.0498442619563446,8.855753149495678,25.196262286952269,16.040438761633428,204.13219018718632,165.47815501971357,1591.8998512896444,2.0472182408516689E-3,3.3371449556365054,-47711.677651408289,4080.8637159773002,9.8444873116532226E-4,0.90541693649887833,-50577.44338086139,6722.6106544824161,1.9868594147338421,6.404163660129184E-3,7.3096691270436605,-35963.142570317985,1866.7779562906912]
["KBM","KBMS-10H03-B (400 V)",1.17,2.4,0.73391973757660023,1.4737344128044181,11450,3.57,13319,8.77,17,30,2.0199999999999999E-2,565,6,4080.8637159773002,6751.3973396160964,7513.3333333333339,0.91286889750354316,123.76237623762377,3.7449443406247558,3.4406660685964234,1.2856376367164881,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,0.73797942912463987,1.0498442619563446,8.855753149495678,25.196262286952269,16.040438761633428,204.13219018718632,165.47815501971357,1591.8998512896444,2.0472182408516689E-3,3.3371449556365054,-47711.677651408289,4080.8637159773002,9.796498450334837E-4,0.87931507193791969,-50590.383612295227,6751.3973396160964,1.9295811230933226,6.404163660129184E-3,7.3096691270436605,-35963.142570317985,1866.7779562906912]
["KBM","KBMS-10H03-B (480 V)",1.17,2.4,0.49415940372588485,0.99228795928892544,14300,3.57,16000,8.77,17,30,2.0199999999999999E-2,679,6,4080.8637159773002,6802.0979141689859,7513.3333333333339,0.84852210417993823,123.76237623762377,3.7584532728231062,3.4406660685964234,1.2856376367164881,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,0.73797942912463987,1.0498442619563446,8.855753149495678,25.196262286952269,16.040438761633428,204.13219018718632,165.47815501971357,1591.8998512896444,2.0472182408516689E-3,3.3371449556365054,-47711.677651408289,4080.8637159773002,9.7144972563027461E-4,0.83282227483808491,-50612.495294037093,6802.0979141689859,1.8275566878178826,6.404163660129184E-3,7.3096691270436605,-35963.142570317985,1866.7779562906912]
["KBM","KBMS-10H03-C (120 V)",1.19,3.05,1.0724594626807715,2.6878683275207305,3250,3.58,4762,5.44,11,24,2.0199999999999999E-2,160,6,4762,4762,4762,1.0177759880879489,123.76237623762377,3.6783629187960227,3.4310552695221315,0.8984486491857876,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,0.92208669216781425,1.3117539386523864,11.065040306013771,31.482094527657274,20.042123851851851,204.13219018718632,165.47815501971357,1591.8998512896444,1.3300813298191641E-3,2.074945400814947,-48936.497492897965,5335.589493508648,6.2011743462285301E-4,0.5018832534246217,-50695.834131914897,8646.0638731177423,2.2193813684625496,4.1737738613295029E-3,4.5322568113990878,-41889.642723752855,2671.2711986099398]
["KBM","KBMS-10H03-C (240 V)",1.19,3.05,0.94236479462306444,2.3618165278773544,7600,3.58,9983,5.44,11,24,2.0199999999999999E-2,325,6,5335.589493508648,8575.5407901435319,9391.6666666666679,0.91057818358085774,123.76237623762377,3.6732995358282055,3.4310552695221315,0.8984486491857876,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,0.92208669216781425,1.3117539386523864,11.065040306013771,31.482094527657274,20.042123851851851,204.13219018718632,165.47815501971357,1591.8998512896444,1.3300813298191641E-3,2.074945400814947,-48936.497492897965,5335.589493508648,6.2652083757523713E-4,0.53707241923970261,-50679.966083546882,8575.5407901435319,2.3749916193502285,4.1737738613295029E-3,4.5322568113990878,-41889.642723752855,2671.2711986099398]
["KBM","KBMS-10H03-C (400 V)",1.19,3.05,0.47746482927568601,1.1966537074578596,14500,3.58,16000,5.44,11,24,2.0199999999999999E-2,565,6,5335.589493508648,8700.2188262270956,9391.6666666666679,0.76246814436657828,123.76237623762377,3.6968161403569666,3.4310552695221315,0.8984486491857876,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,0.92208669216781425,1.3117539386523864,11.065040306013771,31.482094527657274,20.042123851851851,204.13219018718632,165.47815501971357,1591.8998512896444,1.3300813298191641E-3,2.074945400814947,-48936.497492897965,5335.589493508648,6.1539319657362456E-4,0.47425092958098303,-50707.541100603987,8700.2188262270956,2.0971882801548007,4.1737738613295029E-3,4.5322568113990878,-41889.642723752855,2671.2711986099398]
["KBM","KBMS-10H03-D (120 V)",1.18,4.66,1.0070167308359925,3.888095485853253,5500,15.5,7333,2.34,4.7,15.7,2.0199999999999999E-2,160,6,2071.5353563665481,7333,7333,0.94936612494915151,123.76237623762377,3.7031976940750853,0.79246308805736976,0.52396366028987185,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,1.420766752638899,2.0211726288977339,17.049201031666787,48.508143093545613,30.881243014187074,204.13219018718632,165.47815501971357,1591.8998512896444,6.3732086860845052E-3,3.895038410101912,-35417.797210262863,2071.5353563665481,2.613031476111213E-4,0.19152322678747899,-50767.956516695318,13577.047825727392,3.0098531912955728,1.8058495724686088E-3,1.9650378052955975,-46888.800739745086,4580.4703300840565]
["KBM","KBMS-10H03-D (240 V)",1.18,4.66,0.62437708443743556,2.4107223337352726,13000,15.5,15373,2.34,4.7,15.7,2.0199999999999999E-2,325,6,2071.5353563665481,13714.981354146323,14356.687898089174,0.59381862100946248,123.76237623762377,3.7194612794211825,0.79246308805736976,0.52396366028987185,12.283177864889231,0,-9.9493740705602765,0,0,0,0,0,1.420766752638899,2.0211726288977339,17.049201031666787,48.508143093545613,30.881243014187074,204.13219018718632,165.47815501971357,1591.8998512896444,6.3732086860845052E-3,3.895038410101912,-35417.797210262863,2071.5353563665481,2.577629348452118E-4,0.16707684793957414,-50776.847823930562,13714.981354146323,2.6256699638866383,1.8058495724686088E-3,1.9650378052955975,-46888.800739745086,4580.4703300840565]
["KBM","KBMS-10H04-A (120 V)",1.44,1.6,1.3285977858106046,1.4285997696888222,1150,4.66,2022,20.399999999999999,44,56.2,2.5499999999999998E-2,160,6,1834.9533314677865,2022,2022,1.244125846007863,98.039215686274517,3.0984692626509056,2.6414183438825232,2.6511279609418246,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,0.40057951133682529,0.5698615501153963,4.8069541360419032,13.676677202769511,8.7068431275720162,204.56148175451906,165.82615685353804,1595.2476289310359,7.0004029838826405E-3,10.281832335505445,-42437.415466666673,1834.9533314677865,3.3539730365869094E-3,2.3195514064153517,-50379.291634050089,3545.2689220434349,1.1680915749887293,1.4022391079852502E-2,17.289714825819523,-27143.618324508036,905.27505098146594]
["KBM","KBMS-10H04-A (240 V)",1.44,1.6,1.2891550390443522,1.3861882140261852,3000,4.66,4251,20.399999999999999,44,56.2,2.5499999999999998E-2,325,6,1834.9533314677865,3440.4427105164555,4010.6761565836296,1.2670088512206674,98.039215686274517,3.0524761378288106,2.6414183438825232,2.6511279609418246,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,0.40057951133682529,0.5698615501153963,4.8069541360419032,13.676677202769511,8.7068431275720162,204.56148175451906,165.82615685353804,1595.2476289310359,7.0004029838826405E-3,10.281832335505445,-42437.415466666673,1834.9533314677865,3.436705920068272E-3,2.7670941722938012,-50199.10050873673,3440.4427105164555,1.3934674527657445,1.4022391079852502E-2,17.289714825819523,-27143.618324508036,905.27505098146594]
["KBM","KBMS-10H04-A (400 V)",1.44,1.6,1.1791305349069114,1.2678822955988294,5750,4.66,7109,20.399999999999999,44,56.2,2.5499999999999998E-2,565,6,1834.9533314677865,3421.9891298227558,4010.6761565836296,1.2847491349823954,98.039215686274517,3.0477054741143275,2.6414183438825232,2.6511279609418246,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,0.40057951133682529,0.5698615501153963,4.8069541360419032,13.676677202769511,8.7068431275720162,204.56148175451906,165.82615685353804,1595.2476289310359,7.0004029838826405E-3,10.281832335505445,-42437.415466666673,1834.9533314677865,3.452562790136953E-3,2.8448427663504776,-50164.564455581189,3421.9891298227558,1.432620487888675,1.4022391079852502E-2,17.289714825819523,-27143.618324508036,905.27505098146594]
["KBM","KBMS-10H04-A (480 V)",1.44,1.6,1.1106983262583334,1.1942992755465951,7050,4.66,8541,20.399999999999999,44,56.2,2.5499999999999998E-2,679,6,1834.9533314677865,3421.6971908631672,4010.6761565836296,1.2801743812782411,98.039215686274517,3.0490059887063712,2.6414183438825232,2.6511279609418246,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,0.40057951133682529,0.5698615501153963,4.8069541360419032,13.676677202769511,8.7068431275720162,204.56148175451906,165.82615685353804,1595.2476289310359,7.0004029838826405E-3,10.281832335505445,-42437.415466666673,1834.9533314677865,3.4528167652448892E-3,2.8460707625586643,-50164.011301157276,3421.6971908631672,1.4332388885074039,1.4022391079852502E-2,17.289714825819523,-27143.618324508036,905.27505098146594]
["KBM","KBMS-10H04-B (120 V)",1.41,2.4,1.2732395447351628,2.1115083660616301,2100,4.75,3131,9.02,19,36.4,2.5499999999999998E-2,160,6,3131,3131,3131,1.2060966736027594,98.039215686274517,3.1336243482560668,2.5913704173668548,1.1913752038167502,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,0.61365371949471104,0.87297939592145812,7.363844633936532,20.951505502114994,13.338142663514576,204.56148175451906,165.82615685353804,1595.2476289310359,3.0717459418121767E-3,4.5978445844263867,-46816.327351742875,3226.6465221488488,1.4062233388594545E-3,0.9917033363025024,-50619.59298151765,5657.4769446632499,1.7438664633247845,6.0789572617798273E-3,7.5851453409266076,-39949.279474742514,2014.4787236726415]
["KBM","KBMS-10H04-B (240 V)",1.41,2.4,1.1888682496021099,1.971589136985257,4980,4.75,6571,9.02,19,36.4,2.5499999999999998E-2,325,6,3226.6465221488488,5562.7366862333374,6192.3076923076924,1.1629924296326632,98.039215686274517,3.112530596269655,2.5913704173668548,1.1913752038167502,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,0.61365371949471104,0.87297939592145812,7.363844633936532,20.951505502114994,13.338142663514576,204.56148175451906,165.82615685353804,1595.2476289310359,3.0717459418121767E-3,4.5978445844263867,-46816.327351742875,3226.6465221488488,1.430688598897276E-3,1.1311773011037352,-50563.725902643797,5562.7366862333374,1.9891252628269169,6.0789572617798273E-3,7.5851453409266076,-39949.279474742514,2014.4787236726415]
["KBM","KBMS-10H04-B (400 V)",1.41,2.4,0.90467020283814192,1.5002822600964212,9500,4.75,10987,9.02,19,36.4,2.5499999999999998E-2,565,6,3226.6465221488488,5578.9776828059712,6192.3076923076924,1.1132396146502237,98.039215686274517,3.1214429656290976,2.5913704173668548,1.1913752038167502,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,0.61365371949471104,0.87297939592145812,7.363844633936532,20.951505502114994,13.338142663514576,204.56148175451906,165.82615685353804,1595.2476289310359,3.0717459418121767E-3,4.5978445844263867,-46816.327351742875,3226.6465221488488,1.4263269460412004E-3,1.1075991770576481,-50573.685854173193,5578.9776828059712,1.9476641743270184,6.0789572617798273E-3,7.5851453409266076,-39949.279474742514,2014.4787236726415]
["KBM","KBMS-10H04-B (480 V)",1.41,2.4,0.71412130987319988,1.1842807792258705,11500,4.75,13200,9.02,19,36.4,2.5499999999999998E-2,679,6,3226.6465221488488,5599.4451829487807,6192.3076923076924,1.07117090614372,98.039215686274517,3.1289036159168111,2.5913704173668548,1.1913752038167502,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,0.61365371949471104,0.87297939592145812,7.363844633936532,20.951505502114994,13.338142663514576,204.56148175451906,165.82615685353804,1595.2476289310359,3.0717459418121767E-3,4.5978445844263867,-46816.327351742875,3226.6465221488488,1.4209283457739974E-3,1.077701401484437,-50586.01370298698,5599.4451829487807,1.8950902580744768,6.0789572617798273E-3,7.5851453409266076,-39949.279474742514,2014.4787236726415]
["KBM","KBMS-10H04-C (120 V)",1.44,3.1,1.308607309866695,2.726265228888948,2700,4.8,3944,5.44,11.8,29,2.5499999999999998E-2,160,6,3944,3944,3944,1.2480693444867574,98.039215686274517,3.0509036782239507,2.5643769755192833,0.83433181645267285,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,0.77612280321509897,1.1041067533485804,9.313473638581188,26.498562080365929,16.869508559670781,204.56148175451906,165.82615685353804,1595.2476289310359,1.9415401765434858E-3,2.8235661324880161,-48435.205866666671,4320.183724416177,8.9305548574941738E-4,0.61408468295639085,-50693.06130860831,7198.1929972703783,2.2473501331776005,3.7741203653083744E-3,4.6095651329809462,-44488.842902736731,2876.5533720193912]
["KBM","KBMS-10H04-C (240 V)",1.44,3.1,1.1519786357127662,2.3999554910682628,6300,4.8,8273,5.44,11.8,29,2.5499999999999998E-2,325,6,4320.183724416177,7141.7239125014903,7772.4137931034484,1.113496973866438,98.039215686274517,3.0480439395180445,2.5643769755192833,0.83433181645267285,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,0.77612280321509897,1.1041067533485804,9.313473638581188,26.498562080365929,16.869508559670781,204.56148175451906,165.82615685353804,1595.2476289310359,1.9415401765434858E-3,2.8235661324880161,-48435.205866666671,4320.183724416177,9.0113799521743341E-4,0.66003883088196369,-50675.65605877764,7141.7239125014903,2.4155273623561588,3.7741203653083744E-3,4.6095651329809462,-44488.842902736731,2876.5533720193912]
["KBM","KBMS-10H04-C (400 V)",1.44,3.1,0.66845076098596046,1.3926057520540844,12000,4.8,13833,5.44,11.8,29,2.5499999999999998E-2,565,6,4320.183724416177,7206.0683699574392,7772.4137931034484,0.97668028607301649,98.039215686274517,3.0661665331694756,2.5643769755192833,0.83433181645267285,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,0.77612280321509897,1.1041067533485804,9.313473638581188,26.498562080365929,16.869508559670781,204.56148175451906,165.82615685353804,1595.2476289310359,1.9415401765434858E-3,2.8235661324880161,-48435.205866666671,4320.183724416177,8.9195908867791831E-4,0.60758331576061508,-50695.422340787562,7206.0683699574392,2.2235572446090042,3.7741203653083744E-3,4.6095651329809462,-44488.842902736731,2876.5533720193912]
["KBM","KBMS-10H04-D (120 V)",1.41,4.21,1.2277667038517641,3.5484586816524977,4200,4.91,5489,2.94,6.2,20.9,2.5499999999999998E-2,160,6,5489,5489,5489,1.1718384374862698,98.039215686274517,3.1115044976161994,2.506926574845735,0.5603274371092235,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,1.0764508996136388,1.5313513570122244,12.917410795363667,36.752432568293386,23.397325255581819,204.56148175451906,165.82615685353804,1595.2476289310359,1.048361926170838E-3,1.5602662671762528,-49411.859237375451,6161.3743180905749,4.5959733832992984E-4,0.301181887189235,-50753.243532216031,10186.007105492925,2.8299229183957353,1.9944848667989936E-3,2.490121031159144,-47256.304233293034,4283.209853834398]
["KBM","KBMS-10H04-D (240 V)",1.41,4.21,0.909696148409465,2.629179619680535,9500,4.91,11509,2.94,6.2,20.9,2.5499999999999998E-2,325,6,6161.3743180905749,10208.37829178884,10784.688995215312,0.87239042338156181,98.039215686274517,3.1209050274244148,2.506926574845735,0.5603274371092235,12.309009482492559,0,-9.9702976808189749,0,0,0,0,0,1.0764508996136388,1.5313513570122244,12.917410795363667,36.752432568293386,23.397325255581819,204.56148175451906,165.82615685353804,1595.2476289310359,1.048361926170838E-3,1.5602662671762528,-49411.859237375451,6161.3743180905749,4.5835985565251009E-4,0.2928897900574538,-50756.062893065697,10208.37829178884,2.7520098807499913,1.9944848667989936E-3,2.490121031159144,-47256.304233293034,4283.209853834398]
["KBM","KBMS-14H01-A (120 V)",1.2,1.53,1.1018419137131217,1.3519532683596587,1300,3.28,2308,21.4,38,49.3,3.3599999999999998E-2,160,8,2204.16391106437,2308,2308,1.0257316437306807,74.404761904761912,3.7225470785270902,3.7647829245166555,4.4183076357966193,12.348487992414629,0,-10.002275273855851,0,0,0,0,0,0.46113926619941403,0.65601342459702716,5.5336711943929684,15.744322190328653,10.023146808888887,205.21756886685785,166.35800871277922,1600.3640438169361,5.7538220217480916E-3,7.6419703522315059,-44798.170579720005,2204.16391106437,2.6512494758745607E-3,1.9696005620522552,-50406.132810622905,4004.6455395508847,1.0778463106831224,2.1520838570681166E-2,18.315779710567359,-16298.971288461275,543.19440786682139]
["KBM","KBMS-14H01-A (240 V)",1.2,1.53,1.083203791789616,1.3290844071038235,3350,3.28,4849,21.4,38,49.3,3.3599999999999998E-2,325,8,2204.16391106437,3841.6326883896022,4572.0081135902637,1.06606324437583,74.404761904761912,3.6648597020296179,3.7647829245166555,4.4183076357966193,12.348487992414629,0,-10.002275273855851,0,0,0,0,0,0.46113926619941403,0.65601342459702716,5.5336711943929684,15.744322190328653,10.023146808888887,205.21756886685785,166.35800871277922,1600.3640438169361,5.7538220217480916E-3,7.6419703522315059,-44798.170579720005,2204.16391106437,2.7676331972076936E-3,2.4340286334298558,-50195.766895280751,3841.6326883896022,1.3320004234289249,2.1520838570681166E-2,18.315779710567359,-16298.971288461275,543.19440786682139]
["KBM","KBMS-14H01-A (400 V)",1.2,1.53,0.9698504344662372,1.1900005330874077,6400,3.28,8109,21.4,38,49.3,3.3599999999999998E-2,565,8,2204.16391106437,3826.9191702537282,4572.0081135902637,1.0623806586926994,74.404761904761912,3.6663923736386832,3.7647829245166555,4.4183076357966193,12.348487992414629,0,-10.002275273855851,0,0,0,0,0,0.46113926619941403,0.65601342459702716,5.5336711943929684,15.744322190328653,10.023146808888887,205.21756886685785,166.35800871277922,1600.3640438169361,5.7538220217480916E-3,7.6419703522315059,-44798.170579720005,2204.16391106437,2.7791780909336792E-3,2.4753524249220322,-50174.899267846471,3826.9191702537282,1.3546144991260152,2.1520838570681166E-2,18.315779710567359,-16298.971288461275,543.19440786682139]
["KBM","KBMS-14H01-A (480 V)",1.2,1.53,0.89449107256710791,1.0975350583645496,7900,3.28,9741,21.4,38,49.3,3.3599999999999998E-2,679,8,2204.16391106437,3830.3957279058741,4572.0081135902637,1.0518708746232841,74.404761904761912,3.6701880731852072,3.7647829245166555,4.4183076357966193,12.348487992414629,0,-10.002275273855851,0,0,0,0,0,0.46113926619941403,0.65601342459702716,5.5336711943929684,15.744322190328653,10.023146808888887,205.21756886685785,166.35800871277922,1600.3640438169361,5.7538220217480916E-3,7.6419703522315059,-44798.170579720005,2204.16391106437,2.7764344381324777E-3,2.4655945347629222,-50179.858475425455,3830.3957279058741,1.3492745809158533,2.1520838570681166E-2,18.315779710567359,-16298.971288461275,543.19440786682139]
["KBM","KBMS-14H01-B (120 V)",1.25,3.25,1.1186318857316073,2.8391672226690541,3500,3.43,5022,4.74,9,23.7,3.3599999999999998E-2,160,8,5022,5022,5022,1.0615055228983235,74.404761904761912,3.519832717164002,3.6001422718409994,0.92872988419010583,12.348487992414629,0,-10.002275273855851,0,0,0,0,0,0.9403624251909618,1.3377528658449183,11.284349102291541,32.106068780278036,20.439358198518512,205.21756886685785,166.35800871277922,1600.3640438169361,1.4094217263012007E-3,1.7352209524491575,-49465.011629093206,5340.5018636709192,6.2095824605575933E-4,0.45881393762326506,-50711.464977230607,8675.0581494713388,2.3580297886266823,5.0147444989034366E-3,3.9769906482039463,-43765.487486735728,2584.1744094332744]
["KBM","KBMS-14H01-B (240 V)",1.25,3.25,0.93691211782398764,2.377949537624334,7950,3.43,10088,4.74,9,23.7,3.3599999999999998E-2,325,8,5340.5018636709192,8646.053216925884,9510.5485232067513,0.90950006404170769,74.404761904761912,3.5222169033321684,3.6001422718409994,0.92872988419010583,12.348487992414629,0,-10.002275273855851,0,0,0,0,0,0.9403624251909618,1.3377528658449183,11.284349102291541,32.106068780278036,20.439358198518512,205.21756886685785,166.35800871277922,1600.3640438169361,1.4094217263012007E-3,1.7352209524491575,-49465.011629093206,5340.5018636709192,6.2393174920894368E-4,0.47018249831784686,-50706.764273832363,8646.053216925884,2.4164574050816254,5.0147444989034366E-3,3.9769906482039463,-43765.487486735728,2584.1744094332744]
["KBM","KBMS-14H01-B (400 V)",1.25,3.25,0.56102117439893107,1.4239116101495712,12000,3.43,12000,4.74,9,23.7,3.3599999999999998E-2,565,8,5340.5018636709192,8802.786211421253,9510.5485232067513,0.74458889116980853,74.404761904761912,3.5456476376810993,3.6001422718409994,0.92872988419010583,12.348487992414629,0,-10.002275273855851,0,0,0,0,0,0.9403624251909618,1.3377528658449183,11.284349102291541,32.106068780278036,20.439358198518512,205.21756886685785,166.35800871277922,1600.3640438169361,1.4094217263012007E-3,1.7352209524491575,-49465.011629093206,5340.5018636709192,6.0841256029870448E-4,0.40736984819445471,-50731.297997285888,8802.786211421253,2.0936378742260446,5.0147444989034366E-3,3.9769906482039463,-43765.487486735728,2584.1744094332744]
["KBM","KBMS-14H01-C (120 V)",1.21,6.25,0.91036627448564134,4.5747048969127704,7500,3.59,9539,1.29,2.4,12.1,3.3599999999999998E-2,160,8,9539,9539,9539,0.82890585230913771,74.404761904761912,3.6411753968119118,3.4396902485834624,0.43409463997531972,12.348487992414629,0,-10.002275273855851,0,0,0,0,0,1.8681707429890375,2.6576463482297323,22.41804891586845,63.78351235751358,40.605845117845107,205.21756886685785,166.35800871277922,1600.3640438169361,4.070488535243762E-4,0.50133128093326429,-50376.000357144003,10525.925842395798,1.5230939109131663E-4,7.5423871212386542E-2,-50795.446250343797,18016.107464304288,2.7898002657309906,1.3962029570286857E-3,1.0978026170041892,-48747.290684548112,5528.7482935436637]
["KBM","KBMS-14H01-C (240 V)",1.21,6.25,0.64723010190704111,3.2524125723971915,13500,3.59,12000,1.29,2.4,12.1,3.3599999999999998E-2,325,8,10525.925842395798,12000,12000,0.70976009058403655,74.404761904761912,3.6435709397204064,3.4396902485834624,0.43409463997531972,12.348487992414629,0,-10.002275273855851,0,0,0,0,0,1.8681707429890375,2.6576463482297323,22.41804891586845,63.78351235751358,40.605845117845107,205.21756886685785,166.35800871277922,1600.3640438169361,4.070488535243762E-4,0.50133128093326429,-50376.000357144003,10525.925842395798,1.523967917074952E-4,7.5980526648529209E-2,-50795.302339270223,18009.183218393944,2.810390000236906,1.3962029570286857E-3,1.0978026170041892,-48747.290684548112,5528.7482935436637]
["KBM","KBMS-14H02-A (120 V)",2.08,1.59,1.9757165349338732,1.4634937295806467,725,6.67,1461,23.8,47,80.8,5.5600000000000004E-2,160,8,1182.1558441081677,1461,1461,1.8698508379839844,44.964028776978417,2.1725640447457022,1.8674233245755654,2.5022690137361319,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.27887561294330354,0.39672645400883905,3.3465073553196425,9.5214348962121367,6.0615337162393157,206.99953386333365,167.80254462676766,1614.2604793095047,1.4085709989137867E-2,16.982771584944864,-39760.95589675603,1182.1558441081677,6.9825060064772322E-3,4.1619386528807425,-50141.862079210114,2398.2470726276174,1.2495301198058313,1.7209328478107674E-2,20.189774595650789,-35195.975000398779,959.12948880606803]
["KBM","KBMS-14H02-A (240 V)",2.08,1.59,1.8621128341751756,1.3793428401297596,2000,6.67,2944,23.8,47,80.8,5.5600000000000004E-2,325,8,1182.1558441081677,2350.5919118184538,2789.6039603960398,1.8239180951615608,44.964028776978417,2.1557066423388433,1.8674233245755654,2.5022690137361319,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.27887561294330354,0.39672645400883905,3.3465073553196425,9.5214348962121367,6.0615337162393157,206.99953386333362,167.80254462676766,1614.2604793095047,1.4085709989137867E-2,16.982771584944864,-39760.95589675603,1182.1558441081677,7.0858366846263243E-3,4.6114351765319208,-49990.85049651398,2350.5919118184538,1.3844815191161983,1.7209328478107674E-2,20.189774595650789,-35195.975000398779,959.12948880606803]
["KBM","KBMS-14H02-A (400 V)",2.08,1.59,1.7384616860807027,1.2877493970968168,3900,6.67,4924,23.8,47,80.8,5.5600000000000004E-2,565,8,1182.1558441081677,2331.3002366634992,2789.6039603960398,1.8758388840846898,44.964028776978417,2.1455119322361917,1.8674233245755654,2.5022690137361319,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.27887561294330354,0.39672645400883905,3.3465073553196425,9.5214348962121367,6.0615337162393157,206.99953386333362,167.80254462676766,1614.2604793095047,1.4085709989137867E-2,16.982771584944864,-39760.95589675603,1182.1558441081677,7.1304001237275693E-3,4.792295053087126,-49925.723705616969,2331.3002366634992,1.4387807008361575,1.7209328478107674E-2,20.189774595650789,-35195.975000398779,959.12948880606803]
["KBM","KBMS-14H02-A (480 V)",2.08,1.59,1.6370222718023522,1.2126090902239646,4900,6.67,5915,23.8,47,80.8,5.5600000000000004E-2,679,8,1182.1558441081677,2330.9658873341036,2789.6039603960398,1.8692722503515355,44.964028776978417,2.1468563360479593,1.8674233245755654,2.5022690137361319,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.27887561294330354,0.39672645400883905,3.3465073553196425,9.5214348962121367,6.0615337162393157,206.99953386333362,167.80254462676766,1614.2604793095047,1.4085709989137867E-2,16.982771584944864,-39760.95589675603,1182.1558441081677,7.1311864325521723E-3,4.7954250326074366,-49924.574562475573,2330.9658873341036,1.4397204080282124,1.7209328478107674E-2,20.189774595650789,-35195.975000398779,959.12948880606803]
["KBM","KBMS-14H02-B (120 V)",2.08,2.42,1.909859317102744,2.1702946785258455,1350,6.83,2139,10.3,20,53.4,5.5600000000000004E-2,160,8,2139,2139,2139,1.8104215402094588,44.964028776978417,2.1639280023051719,1.8236769509398272,1.2477139662549441,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.42445219076905322,0.60382265327131468,5.0934262892286384,14.491743678511552,9.2257305618233598,206.99953386333362,167.80254462676766,1614.2604793095047,6.1754293340383886E-3,7.5702782718222004,-45780.794993405078,2177.9548476944101,3.0276783596547524E-3,1.7425778458203354,-50538.939269176888,3807.9697879843393,1.8291658273667299,7.3317868766651639E-3,8.7890083271918638,-44032.843498203802,1923.5177812457141]
["KBM","KBMS-14H02-B (240 V)",2.08,2.42,1.7941102675813656,2.0387616677060971,3300,6.83,4489,10.3,20,53.4,5.5600000000000004E-2,325,8,2177.9548476944101,3747.1821685325922,4220.9737827715353,1.7553694219740421,44.964028776978417,2.145065384858865,1.8236769509398272,1.2477139662549441,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.42445219076905322,0.60382265327131468,5.0934262892286384,14.491743678511552,9.2257305618233598,206.99953386333362,167.80254462676766,1614.2604793095047,6.1754293340383886E-3,7.5702782718222004,-45780.794993405078,2177.9548476944101,3.072981495184065E-3,1.9538884334095701,-50470.458993339467,3747.1821685325922,2.0509763517608661,7.3317868766651639E-3,8.7890083271918638,-44032.843498203802,1923.5177812457141]
["KBM","KBMS-14H02-B (400 V)",2.08,2.42,1.382510102678852,1.5710342075896044,6700,6.83,7505,10.3,20,53.4,5.5600000000000004E-2,565,8,2177.9548476944101,3757.0713396510178,4220.9737827715353,1.6888777159818782,44.964028776978417,2.1533888781253325,1.8236769509398272,1.2477139662549441,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.42445219076905322,0.60382265327131468,5.0934262892286384,14.491743678511552,9.2257305618233598,206.99953386333362,167.80254462676766,1614.2604793095047,6.1754293340383886E-3,7.5702782718222004,-45780.794993405078,2177.9548476944101,3.0653346920628002E-3,1.9198531787260023,-50482.017910418836,3757.0713396510178,2.0152498991709686,7.3317868766651639E-3,8.7890083271918638,-44032.843498203802,1923.5177812457141]
["KBM","KBMS-14H02-B (480 V)",2.08,2.42,1.2401683877290546,1.4092822587830165,7700,6.83,9016,10.3,20,53.4,5.5600000000000004E-2,679,8,2177.9548476944101,3761.0847462496031,4220.9737827715353,1.6697820952817579,44.964028776978417,2.155766779830083,1.8236769509398272,1.2477139662549441,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.42445219076905322,0.60382265327131468,5.0934262892286384,14.491743678511552,9.2257305618233598,206.99953386333362,167.80254462676766,1614.2604793095047,6.1754293340383886E-3,7.5702782718222004,-45780.794993405078,2177.9548476944101,3.0622618441065617E-3,1.9060050227265961,-50486.662831199501,3761.0847462496031,2.0007136339550908,7.3317868766651639E-3,8.7890083271918638,-44032.843498203802,1923.5177812457141]
["KBM","KBMS-14H02-C (120 V)",2.11,3.1,1.9098593171027443,2.7322737011484182,1800,6.98,2704,6.3,12.8,42.3,5.5600000000000004E-2,160,8,2704,2704,2704,1.8093442185810114,44.964028776978417,2.1253709580304472,1.7844861855184841,0.91248457412288608,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.53598913596781472,0.76249431442039828,6.4318696316137762,18.299863546089558,11.650054965069335,206.99953386333362,167.80254462676766,1614.2604793095047,4.0566879184936264E-3,4.7334326853383857,-47674.674585865097,2894.0142377704819,1.8984529308983371E-3,1.0386038479040856,-50654.444080154535,4899.1564107765107,2.2501340056617698,4.715559832062545E-3,5.3773650300691891,-46765.002358336125,2630.1814497050195]
["KBM","KBMS-14H02-C (240 V)",2.11,3.1,1.7301078519636623,2.4751185292756257,4250,6.98,5671,6.3,12.8,42.3,5.5600000000000004E-2,325,8,2894.0142377704819,4840.9785364575282,5328.6052009456271,1.6772824153381984,44.964028776978417,2.1152605371811353,1.7844861855184841,0.91248457412288608,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.53598913596781472,0.76249431442039828,6.4318696316137762,18.299863546089558,11.650054965069335,206.99953386333362,167.80254462676766,1614.2604793095047,4.0566879184936264E-3,4.7334326853383857,-47674.674585865097,2894.0142377704819,1.9227894220441859E-3,1.1485556070471885,-50620.84387705745,4840.9785364575282,2.4883443615443297,4.715559832062545E-3,5.3773650300691891,-46765.002358336125,2630.1814497050195]
["KBM","KBMS-14H02-C (400 V)",2.11,3.1,1.2055986939211072,1.7247477738499388,8000,6.98,9481,6.3,12.8,42.3,5.5600000000000004E-2,565,8,2894.0142377704819,4866.463491414549,5328.6052009456271,1.5598455077974291,44.964028776978417,2.1262383697951455,1.7844861855184841,0.91248457412288608,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.53598913596781472,0.76249431442039828,6.4318696316137762,18.299863546089558,11.650054965069335,206.99953386333362,167.80254462676766,1614.2604793095047,4.0566879184936264E-3,4.7334326853383857,-47674.674585865097,2894.0142377704819,1.9119165360207331E-3,1.100790223379468,-50635.855539028358,4866.463491414549,2.3848607144337284,4.715559832062545E-3,5.3773650300691891,-46765.002358336125,2630.1814497050195]
["KBM","KBMS-14H02-C (480 V)",2.11,3.1,0.5496668278490825,0.78636169935491063,10250,6.98,11390,6.3,12.8,42.3,5.5600000000000004E-2,679,8,2894.0142377704819,4920.4679581146029,5328.6052009456271,1.3609688412144481,44.964028776978417,2.1446657942167051,1.7844861855184841,0.91248457412288608,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,0.53598913596781472,0.76249431442039828,6.4318696316137762,18.299863546089558,11.650054965069335,206.99953386333362,167.80254462676766,1614.2604793095047,4.0566879184936264E-3,4.7334326853383857,-47674.674585865097,2894.0142377704819,1.8899748762565426E-3,0.99745762327958332,-50666.149315561124,4920.4679581146029,2.1609907587741075,4.715559832062545E-3,5.3773650300691891,-46765.002358336125,2630.1814497050195]
["KBM","KBMS-14H02-D (120 V)",2.1749999999999998,5.97,1.8608885653821607,4.975637875353371,3900,7.31,5084,1.69,3.6,22.6,5.5600000000000004E-2,160,8,5084,5084,5084,1.7655275554879244,44.964028776978417,2.0470204422716671,1.7039279856250371,0.47206923682140045,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,1.0013636409411599,1.424532759430394,12.016363691293918,34.188786226329455,21.765257304929754,206.99953386333362,167.80254462676766,1614.2604793095047,1.1973672377044277E-3,1.3273584470053374,-49942.778232224322,5927.8257402751988,5.36411857256739E-4,0.25656265231864134,-50772.941152319698,9492.7642190142215,3.8782666486927768,1.318685089228817E-3,1.4398577118034614,-49790.402466990417,5622.9832383540042]
["KBM","KBMS-14H02-D (240 V)",2.1749999999999998,5.97,1.1051433127055206,2.9549286435976487,8900,7.31,10660,1.69,3.6,22.6,5.5600000000000004E-2,325,8,5927.8257402751988,9608.2288060152696,9973.4513274336277,1.0200081077336083,44.964028776978417,2.0643100706753419,1.7039279856250371,0.42681969663892211,12.45571357491902,0,-10.089127995684406,0,0,0,0,0,1.0013636409411599,1.424532759430394,12.016363691293918,34.188786226329455,21.765257304929754,206.99953386333362,167.80254462676766,1614.2604793095047,1.1973672377044277E-3,1.3273584470053374,-49942.778232224322,5927.8257402751988,5.2812273012520694E-4,0.21107803222402088,-50783.352333146897,9608.2288060152696,3.1907095021352823,1.318685089228817E-3,1.4398577118034614,-49790.402466990417,5622.9832383540042]
["KBM","KBMS-14H03-A (120 V)",2.82,1.64,2.5783100780887045,1.4403966916696673,500,10.4,1051,26.6,54,108,8.8099999999999998E-2,160,8,665.21458201707162,1051,1051,2.3119677841424568,28.376844494892168,1.7040593544460769,1.2128956734248737,2.5672994011237957,12.614115003618686,0,-10.217433152931134,0,0,0,0,0,0.21486202352139747,0.30566117916570101,2.5783442822567695,7.3358682999768243,4.6701588072498019,209.63198215358176,169.93651813606874,1634.7893044689813,2.5701254041447769E-2,30.094982734427266,-31392.694598219408,665.21458201707162,1.2110433212094705E-2,5.3669959398672606,-50187.776481941197,1826.1636228991952,1.0786119989633778,2.0033303156895346E-2,23.237942263885422,-39231.043902184661,934.83447974530623]
["KBM","KBMS-14H03-A (240 V)",2.82,1.64,2.5464790894703255,1.422614016463869,1500,10.4,2217,26.6,54,108,8.8099999999999998E-2,325,8,665.21458201707162,1731.3806107374344,2087.037037037037,2.5042874659184489,28.376844494892168,1.6194470480953509,1.2128956734248737,2.5672994011237957,12.614115003618686,0,-10.217433152931134,0,0,0,0,0,0.21486202352139747,0.30566117916570101,2.5783442822567695,7.3358682999768243,4.6701588072498019,209.63198215358176,169.93651813606874,1634.7893044689813,2.5701254041447769E-2,30.094982734427266,-31392.694598219408,665.21458201707162,1.2455508206740875E-2,7.1462915409295249,-49710.563746828688,1731.3806107374344,1.4361992985460899,2.0033303156895346E-2,23.237942263885422,-39231.043902184661,934.83447974530623]
["KBM","KBMS-14H03-A (400 V)",2.82,1.64,2.4124538742350454,1.3477395945447181,2850,10.4,3710,26.6,54,108,8.8099999999999998E-2,565,8,665.21458201707162,1715.4318640811196,2087.037037037037,2.5746955753613983,28.376844494892168,1.6090041236455435,1.2128956734248737,2.5672994011237957,12.614115003618686,0,-10.217433152931134,0,0,0,0,0,0.21486202352139747,0.30566117916570101,2.5783442822567695,7.3358682999768243,4.6701588072498019,209.63198215358176,169.93651813606874,1634.7893044689813,2.5701254041447769E-2,30.094982734427266,-31392.694598219408,665.21458201707162,1.2522555133942678E-2,7.4428131011956005,-49617.842894818918,1715.4318640811196,1.4957916135837348,2.0033303156895346E-2,23.237942263885422,-39231.043902184661,934.83447974530623]
["KBM","KBMS-14H03-A (480 V)",2.82,1.64,2.3210095867568072,1.2966534004227974,3600,10.4,4458,26.6,54,108,8.8099999999999998E-2,679,8,665.21458201707162,1712.7295013561793,2087.037037037037,2.5826012217623533,28.376844494892168,1.6078473347605799,1.2128956734248737,2.5672994011237957,12.614115003618686,0,-10.217433152931134,0,0,0,0,0,0.21486202352139747,0.30566117916570101,2.5783442822567695,7.3358682999768243,4.6701588072498019,209.63198215358176,169.93651813606874,1634.7893044689813,2.5701254041447769E-2,30.094982734427266,-31392.694598219408,665.21458201707162,1.2534174511779923E-2,7.4930080259756764,-49601.774170153127,1712.7295013561793,1.5058793514470492,2.0033303156895346E-2,23.237942263885422,-39231.043902184661,934.83447974530623]
["KBM","KBMS-14H03-B (120 V)",2.87,2.81,2.6571955716212092,2.5306624491630565,1150,10.4,1789,9.01,19,63.7,8.8099999999999998E-2,160,8,1732.2903851171056,1789,1789,2.5389503283742116,28.376844494892168,1.5910962272587936,1.2128956734248737,1.3415315818893236,12.614115003618686,0,-10.217433152931134,0,0,0,0,0,0.36173401181020176,0.51460022009536166,4.3408081417224214,12.35040528228868,7.8625121994579938,209.63198215358176,169.93651813606874,1634.7893044689813,8.9833134574440338E-3,10.122379445261004,-44492.29691571791,1732.2903851171056,4.2795498985052699E-3,2.1482826139277607,-50520.816063591337,3194.0268290703102,2.1610586971158607,6.994449271460217E-3,7.8160293759873554,-47041.299576563433,2094.1353040743702]
["KBM","KBMS-14H03-B (240 V)",2.87,2.81,2.4794664818526857,2.3613966493835101,2850,10.4,3757,9.01,19,63.7,8.8099999999999998E-2,325,8,1732.2903851171056,3150.7215035306153,3538.4615384615381,2.4382588233416818,28.376844494892168,1.5788105435942059,1.2128956734248737,1.1460577524912245,12.614115003618686,0,-10.217433152931134,0,0,0,0,0,0.36173401181020176,0.51460022009536166,4.3408081417224214,12.35040528228868,7.8625121994579938,209.63198215358176,169.93651813606874,1634.7893044689813,8.9833134574440338E-3,10.122379445261004,-44492.29691571791,1732.2903851171056,4.328928133552977E-3,2.3753487519116199,-50457.531072383055,3150.7215035306153,2.3894752234747285,6.994449271460217E-3,7.8160293759873554,-47041.299576563433,2094.1353040743702]
["KBM","KBMS-14H03-B (400 V)",2.87,2.81,1.961016263096568,1.8676345362824456,5600,10.4,6283,9.01,19,63.7,8.8099999999999998E-2,565,8,1732.2903851171056,3156.2768345027162,3538.4615384615381,2.3576778014771405,28.376844494892168,1.5852571886280544,1.2128956734248737,1.1460577524912245,12.614115003618686,0,-10.217433152931134,0,0,0,0,0,0.36173401181020176,0.51460022009536166,4.3408081417224214,12.35040528228868,7.8625121994579938,209.63198215358176,169.93651813606874,1634.7893044689813,8.9833134574440338E-3,10.122379445261004,-44492.29691571791,1732.2903851171056,4.3223723049220959E-3,2.3464670642191177,-50465.933267335291,3156.2768345027162,2.3604217730717805,6.994449271460217E-3,7.8160293759873554,-47041.299576563433,2094.1353040743702]
["KBM","KBMS-14H03-B (480 V)",2.87,2.81,1.7923295129733443,1.7069804885460422,6500,10.4,7549,9.01,19,63.7,8.8099999999999998E-2,679,8,1732.2903851171056,3156.9990998849653,3538.4615384615381,2.3465838834591164,28.376844494892168,1.5861476364995062,1.2128956734248737,1.1460577524912245,12.614115003618686,0,-10.217433152931134,0,0,0,0,0,0.36173401181020176,0.51460022009536166,4.3408081417224214,12.35040528228868,7.8625121994579938,209.63198215358176,169.93651813606874,1634.7893044689813,8.9833134574440338E-3,10.122379445261004,-44492.29691571791,1732.2903851171056,4.3215247233798475E-3,2.3427070529302858,-50467.019559512351,3156.9990998849653,2.3566394005644096,6.994449271460217E-3,7.8160293759873554,-47041.299576563433,2094.1353040743702]
["KBM","KBMS-14H03-C (120 V)",2.92,6.04,2.4828171122335672,4.9855765305894924,3000,10.4,3806,1.96,4.0999999999999996,30,8.8099999999999998E-2,160,8,3806,3806,3806,2.365360643053652,28.376844494892168,1.553325511111608,1.2128956734248737,0.63058328954282716,12.614115003618686,0,-10.217433152931134,0,0,0,0,0,0.76422107296927388,1.0871754369557201,9.1706528756312871,26.092210486937283,16.610817100761032,209.63198215358176,169.93651813606874,1634.7893044689813,1.9237196708762545E-3,2.190914249130445,-49471.797431376996,4533.5918825709668,9.3344379448291679E-4,0.39599766826847793,-50761.600512979428,7165.2804948316289,3.8882544281168347,1.5103629846651145E-3,1.6917218154166209,-50010.181472012082,5221.398397169758]
["KBM","KBMS-14H03-C (240 V)",2.92,6.04,1.7796416363911933,3.573577583114846,6600,10.4,7980,1.96,4.0999999999999996,30,8.8099999999999998E-2,325,8,4533.5918825709668,7181.317471913816,7513.3333333333339,1.6792006907837922,28.376844494892168,1.5600025962085144,1.2128956734248737,0.45964697911213059,12.614115003618686,0,-10.217433152931134,0,0,0,0,0,0.76422107296927388,1.0871754369557201,9.1706528756312871,26.092210486937283,16.610817100761032,209.63198215358176,169.93651813606874,1634.7893044689813,1.9237196708762545E-3,2.190914249130445,-49471.797431376996,4533.5918825709668,9.3114404453837837E-4,0.38213987887265755,-50764.595864715331,7181.317471913816,3.7521864274697254,1.5103629846651145E-3,1.6917218154166209,-50010.181472012082,5221.398397169758]
["KBM","KBMS-17H01-A (120 V)",2.08,1.65,1.909859317102744,1.4805110985292589,750,5.95,1460,21.3,66,77.900000000000006,8.6199999999999999E-2,160,10,1054.2785081182196,1460,1460,1.7487928039600082,29.002320185614849,2.2402533905189674,2.1184629600676299,3.2280633845248907,12.604854612402399,0,-10.209932236045942,0,0,0,0,0,0.2928644018217369,0.41662680509743505,3.5143728218608428,9.9990433223384407,6.3655886837606825,209.47808517661346,169.81176276167889,1633.5891577673508,2.6022022275276519E-2,13.564858363011515,-43224.698956309665,1054.2785081182196,7.3257362393894538E-3,3.4050891625489688,-50327.496484972653,2398.9378280662827,1.1848156988388414,4.2361464852406355E-2,18.294319581991072,-37017.276148710211,743.47982493324992]
["KBM","KBMS-17H01-A (240 V)",2.08,1.65,1.8853739412424524,1.4615301870096529,1950,5.95,3068,21.3,66,77.900000000000006,8.6199999999999999E-2,325,10,1054.2785081182196,2260.91705308476,2893.4531450577665,1.8543418588617353,29.002320185614849,2.177096128218837,2.1184629600676299,3.2280633845248907,12.604854612402399,0,-10.209932236045942,0,0,0,0,0,0.2928644018217369,0.41662680509743505,3.5143728218608428,9.9990433223384407,6.3655886837606825,209.47808517661346,169.81176276167889,1633.5891577673508,2.6022022275276519E-2,13.564858363011515,-43224.698956309665,1054.2785081182196,7.9542674422952864E-3,4.1702196364088238,-50088.714843200702,2260.91705308476,1.4510462008356071,4.2361464852406355E-2,18.294319581991072,-37017.276148710211,743.47982493324992]
["KBM","KBMS-17H01-A (400 V)",2.08,1.65,1.7590809499630535,1.363628643382212,3800,5.95,5132,21.3,66,77.900000000000006,8.6199999999999999E-2,565,10,1054.2785081182196,2238.2641757100369,2893.4531450577665,1.8909732597366857,29.002320185614849,2.1697028109372756,2.1184629600676299,3.2280633845248907,12.604854612402399,0,-10.209932236045942,0,0,0,0,0,0.2928644018217369,0.41662680509743505,3.5143728218608428,9.9990433223384407,6.3655886837606825,209.47808517661346,169.81176276167889,1633.5891577673508,2.6022022275276519E-2,13.564858363011515,-43224.698956309665,1054.2785081182196,8.0699036674329368E-3,4.2961714936170639,-50044.784155974638,2238.2641757100369,1.4948717016064947,4.2361464852406355E-2,18.294319581991072,-37017.276148710211,743.47982493324992]
["KBM","KBMS-17H01-A (480 V)",2.08,1.65,1.6634258568314222,1.2894774083964513,4650,5.95,6166,21.3,66,77.900000000000006,8.6199999999999999E-2,679,10,{"$f":"IF(AQ1120<I1120,IF(AQ1120<0,0,AQ1120),I1120)","v":1054.2785081182196},{"$f":"IF(AU1120<I1120,IF(AU1120<0,0,AU1120),I1120)","v":2240.5712146752421},{"$f":"IF(UAC_V*0.98/L1120*1000<I1120,IF(UAC_V*0.98/L1120*1000<0,0,UAC_V*0.98/L1120*1000),I1120)","v":2893.4531450577665},{"$f":"C1120+(E1120-C1120)/G1120*Q1120","v":1.8792765518362327},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M1120,(inertia/gear^2+gear_inertia)/M1120),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M1120,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M1120))","v":29.002320185614849},{"$f":"IF((C1120+(E1120-C1120)/G1120*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X1120^2*time1+Y1120^2*time2+Z1120^2*time3+AA1120^2*time4)/time)/(C1120+(E1120-C1120)/G1120*mspeed),SQRT((((X1120-Y1120)*2/PI()+Y1120)^2*time1+Y1120^2*time2+((Z1120-Y1120)*2/PI()+Y1120)^2*time3+AA1120^2*time4)/time)/(C1120+(E1120-C1120)/G1120*mspeed)),IF(AccType=1,SQRT((X1120^2*time1+Y1120^2*time2+Z1120^2*time3+AA1120^2*time4+AB1120^2*time5+AC1120^2*time6+AD1120^2*time7+AE1120^2*time8)/time)/(C1120+(E1120-C1120)/G1120*mspeed),SQRT((((X1120-Y1120)*2/PI()+Y1120)^2*time1+Y1120^2*time2+((Z1120-Y1120)*2/PI()+Y1120)^2*time3+AA1120^2*time4+((AB1120-AC1120)*2/PI()+AC1120)^2*time5+AC1120^2*time6+((AD1120-AC1120)*2/PI()+AC1120)^2*time7+AE1120^2*time8)/time)/(C1120+(E1120-C1120)/G1120*mspeed))))","v":2.172168800077158},{"$f":"IF(move1,MAX(ABS(X1120),ABS(Z1120))/H1120,MAX(ABS(X1120),ABS(Z1120),ABS(AB1120),ABS(AD1120))/H1120)","v":2.1184629600676299},{"$f":"IF(AZ1120>0,speed/(MIN(AZ1120,I1120)),\"NA\")","v":3.2280633845248907},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M1120+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M1120+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":12.604854612402399},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M1120+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M1120+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-10.209932236045942},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M1120+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M1120+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M1120+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M1120+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH1120/Irms","v":0.2928644018217369},{"$f":"AI1120/Ipeak","v":0.41662680509743505},{"$f":"IF(move1,IF(AccType=1,SQRT((X1120^2*time1+Y1120^2*time2+Z1120^2*time3+AA1120^2*time4)/time)/(C1120/D1120),SQRT((((X1120-Y1120)*2/PI()+Y1120)^2*time1+Y1120^2*time2+((Z1120-AA1120)*2/PI()+AA1120)^2*time3+AA1120^2*time4)/time)/(C1120/D1120)),IF(AccType=1,SQRT((X1120^2*time1+Y1120^2*time2+Z1120^2*time3+AA1120^2*time4+AB1120^2*time5+AC1120^2*time6+AD1120^2*time7+AE1120^2*time8)/time)/(C1120/D1120),SQRT((((X1120-Y1120)*2/PI()+Y1120)^2*time1+Y1120^2*time2+((Z1120-AA1120)*2/PI()+AA1120)^2*time3+AA1120^2*time4+((AB1120-AC1120)*2/PI()+AC1120)^2*time5+AC1120^2*time6+((AD1120-AE1120)*2/PI()+AE1120)^2*time7+AE1120^2*time8)/time)/(C1120/D1120)))","v":3.5143728218608428},{"$f":"IF(move1,MAX(ABS(X1120),ABS(Z1120))/(C1120/D1120),MAX(ABS(X1120),ABS(Z1120),ABS(AB1120),ABS(AD1120))/(C1120/D1120))","v":9.9990433223384407},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X1120),ABS(Z1120))/(C1120/D1120),MAX(ABS((X1120-Y1120)*2/PI()+Y1120),ABS((Z1120-Y1120)*2/PI()+Y1120))/(C1120/D1120)),IF(AccType=1,MAX(ABS(X1120),ABS(Z1120),ABS(AB1120),ABS(AD1120))/(C1120/D1120),MAX(ABS((X1120-Y1120)*2/PI()+Y1120),ABS((Z1120-Y1120)*2/PI()+Y1120),ABS((AB1120-AC1120)*2/PI()+AC1120),ABS((AD1120-AC1120)*2/PI()+AC1120))/(C1120/D1120)))","v":6.3655886837606825},{"$f":"IF((C1120+(E1120-C1120)/G1120*mspeed)<0,\"NA\",U1120*(C1120+(E1120-C1120)/G1120*mspeed)*mspeed/9.55)","v":209.47808517661346},{"$f":"IF(move1,IF(speed1>speed2,AM1120/2*time1/time,AM1120/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z1120*-speed/30*PI(),((Z1120-AA1120)*2/PI()+AA1120)*-speed/30*PI()),IF(AccType=1,X1120*-speed/30*PI(),((X1120-Y1120)*2/PI()+Y1120)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z1120*-speed/30*PI(),((Z1120-AA1120)*2/PI()+AA1120)*-speed/30*PI()),IF(AccType=1,X1120*-speed/30*PI(),((X1120-Y1120)*2/PI()+Y1120)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD1120*-speed/30*PI(),((AD1120-AE1120)*2/PI()+AE1120)*-speed/30*PI()),IF(AccType=1,AB1120*-speed/30*PI(),((AB1120-AC1120)*2/PI()+AC1120)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD1120*-speed/30*PI(),((AD1120-AE1120)*2/PI()+AE1120)*-speed/30*PI()),IF(AccType=1,AB1120*-speed/30*PI(),((AB1120-AC1120)*2/PI()+AC1120)*-speed/30*PI()),0)/2*time7/time)))","v":169.81176276167889},{"$f":"IF(move1,MAX(IF(AccType=1,Z1120*-speed/30*PI(),((Z1120-AA1120)*2/PI()+AA1120)*-speed/30*PI()),IF(AccType=1,X1120*-speed/30*PI(),((X1120-Y1120)*2/PI()+Y1120)*-speed/30*PI()),0),MAX(IF(AccType=1,Z1120*-speed/30*PI(),((Z1120-AA1120)*2/PI()+AA1120)*-speed/30*PI()),IF(AccType=1,X1120*-speed/30*PI(),((X1120-Y1120)*2/PI()+Y1120)*-speed/30*PI()),IF(AccType=1,AD1120*-speed/30*PI(),((AD1120-AE1120)*2/PI()+AE1120)*-speed/30*PI()),IF(AccType=1,AB1120*-speed/30*PI(),((AB1120-AC1120)*2/PI()+AC1120)*-speed/30*PI()),0))","v":1633.5891577673508},{"$f":"(L1120^2)/1000000+((K1120/1000)^2*(D1120/C1120*H1120)^2*PI()*PI()*(O1120/2)^2)/1200","v":2.6022022275276519E-2},{"$f":"SQRT(3)*L1120*J1120*D1120/C1120*H1120/1000","v":13.564858363011515},{"$f":"0.75*J1120^2*(D1120/C1120*H1120)^2-(UAC_V*0.98)^2","v":-43224.698956309665},{"$f":"-AO1120/2/AN1120+SQRT((AO1120/2/AN1120)^2-AP1120/AN1120)","v":1054.2785081182196},{"$f":"(L1120^2)/1000000+((K1120/1000)^2*AV1120^2*PI()*PI()*(O1120/2)^2)/1200","v":8.0579553455455127E-3},{"$f":"SQRT(3)*L1120*J1120*AV1120/1000","v":4.2833288652584596},{"$f":"0.75*J1120^2*AV1120^2-(UAC_V*0.98)^2","v":-50049.323373603787},{"$f":"-AS1120/2/AR1120+SQRT((AS1120/2/AR1120)^2-AT1120/AR1120)","v":2240.5712146752421},{"$f":"D1120+(F1120-D1120)*((0.85*UAC_V-D1120*J1120)/L1120*1000)/G1120","v":1.4904030527790328},{"$f":"(L1120^2)/1000000+((K1120/1000)^2*AJ1120^2*PI()*PI()*(O1120/2)^2)/1200","v":4.2361464852406355E-2},{"$f":"SQRT(3)*L1120*J1120*AJ1120/1000","v":18.294319581991072},{"$f":"0.75*J1120^2*AJ1120^2-(UAC_V*0.98)^2","v":-37017.276148710211},{"$f":"IF(((AX1120/2/AW1120)^2-AY1120/AW1120)>0,-AX1120/2/AW1120+SQRT((AX1120/2/AW1120)^2-AY1120/AW1120),-9999)","v":743.47982493324992}]
["KBM","KBMS-17H01-B (120 V)",2.0699999999999998,3.11,1.8568076694054458,2.7265898229154857,1800,6.14,2782,6.02,18,41.2,8.6199999999999999E-2,160,10,2310.7595572199057,2782,2782,1.7404994090477501,29.002320185614849,2.1969758512861728,2.0529079173293812,1.3228813882891859,12.604854612402399,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-10.209932236045942,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.55467171497714884,0.78907201780538372,6.6560605797257857,18.937728427329208,12.056132360565396,209.47808517661346,169.81176276167889,1633.5891577673508,7.3666213224903567E-3,3.9628966775858756,-48492.18427225393,2310.7595572199057,2.0187236533937406E-3,0.943402212325398,-50674.079117285379,4781.9762051734015,2.1960516774189478,1.1380654065656366E-2,5.1791959442470823,-46854.494493574821,1814.2216084117686]
["KBM","KBMS-17H01-B (240 V)",2.0699999999999998,3.11,1.7052315331274501,2.50401106186116,4200,6.14,5838,6.02,18,41.2,8.6199999999999999E-2,325,10,2310.7595572199057,4650.9657496086074,5470.8737864077666,1.6660653223901258,29.002320185614849,2.181543438207822,2.0529079173293812,1.3228813882891859,12.604854612402399,0,-10.209932236045942,0,0,0,0,0,0.55467171497714884,0.78907201780538372,6.6560605797257857,18.937728427329208,12.056132360565396,209.47808517661346,169.81176276167889,1633.5891577673508,7.3666213224903567E-3,3.9628966775858756,-48492.18427225393,2310.7595572199057,2.1107952943736309E-3,1.0700752710452226,-50636.514703891968,4650.9657496086074,2.4909212245231149,1.1380654065656366E-2,5.1791959442470823,-46854.494493574821,1814.2216084117686]
["KBM","KBMS-17H01-B (400 V)",2.0699999999999998,3.11,1.0653261508694498,1.5643555813060936,8650,6.14,9600,6.02,18,41.2,8.6199999999999999E-2,565,10,2310.7595572199057,4716.9957489582321,5470.8737864077666,1.5221338409897909,29.002320185614849,2.1958483847661094,2.0529079173293812,1.3228813882891859,12.604854612402399,0,-10.209932236045942,0,0,0,0,0,0.55467171497714884,0.78907201780538372,6.6560605797257857,18.937728427329208,12.056132360565396,209.47808517661346,169.81176276167889,1633.5891577673508,7.3666213224903567E-3,3.9628966775858756,-48492.18427225393,2310.7595572199057,2.0632539530150971E-3,1.0066597605043661,-50655.911149758067,4716.9957489582321,2.3433025985773961,1.1380654065656366E-2,5.1791959442470823,-46854.494493574821,1814.2216084117686]
["KBM","KBMS-17H01-B (480 V)",2.0699999999999998,3.11,0.71619724391352901,1.0516846459816871,9600,6.14,9600,6.02,18,41.2,8.6199999999999999E-2,679,10,2310.7595572199057,4784.6089771887164,5470.8737864077666,1.3952690812381088,29.002320185614849,2.2081414405574975,2.0529079173293812,1.3228813882891859,12.604854612402399,0,-10.209932236045942,0,0,0,0,0,0.55467171497714884,0.78907201780538372,6.6560605797257857,18.937728427329208,12.056132360565396,209.47808517661346,169.81176276167889,1633.5891577673508,7.3666213224903567E-3,3.9628966775858756,-48492.18427225393,2310.7595572199057,2.0169656495839677E-3,0.94081761200287661,-50674.796367256757,4784.6089771887164,2.1900352447674489,1.1380654065656366E-2,5.1791959442470823,-46854.494493574821,1814.2216084117686]
["KBM","KBMS-17H01-C (120 V)",2.0699999999999998,6.1,1.7384616860807027,4.8970751720583179,3900,6.35,5468,1.56,5,21.5,8.6199999999999999E-2,160,10,4474.9565906551752,5468,5468,1.605166281920329,29.002320185614849,2.180651343824374,1.9850164743940786,0.65532343353266065,12.604854612402399,0,-10.209932236045942,0,0,0,0,0,1.0879413059037324,1.5476975268851578,13.055295670844789,37.144740645243786,23.647076334227947,209.47808517661346,169.81176276167889,1633.5891577673508,2.2622186719710811E-3,1.0870684727370978,-50166.048120919979,4474.9565906551752,5.2279160399924286E-4,0.19936613467176323,-50783.663593480829,9667.1019701920704,3.4318453047119171,3.3366911616717204E-3,1.373729229161424,-49784.536963195009,3662.3137174605345]
["KBM","KBMS-17H01-C (240 V)",2.0699999999999998,6.1,0.90187801085407349,2.5405014390255594,9000,6.35,9600,1.56,5,21.5,8.6199999999999999E-2,325,10,4474.9565906551752,9600,9600,0.82400321157767853,29.002320185614849,2.202574499969153,1.9850164743940786,0.65532343353266065,12.604854612402399,0,-10.209932236045942,0,0,0,0,0,1.0879413059037324,1.5476975268851578,13.055295670844789,37.144740645243786,23.647076334227947,209.47808517661346,169.81176276167889,1633.5891577673508,2.2622186719710811E-3,1.0870684727370978,-50166.048120919979,4474.9565906551752,4.9913641047391502E-4,0.15561720997601908,-50792.062803655645,9932.9283295350051,2.6787608249908508,3.3366911616717204E-3,1.373729229161424,-49784.536963195009,3662.3137174605345]
["KBM","KBMS-17H02-A (120 V)",3.58,1.59,3.3104228163114229,1.4330834702646853,375,12.2,812,27.5,97,140,0.128,160,10,472.71716234697635,812,812,2.9962755382530011,19.53125,1.3828909068263953,1.0498838704230116,3.2020679686874494,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.16661854113074973,0.237030345885307,1.9994224935689966,5.6887283012473677,3.6215569162011172,212.86381866991732,172.55638099825697,1659.9923852032321,7.6400195858433745E-2,36.132273191648366,-34152.849209235828,472.71716234697635,2.2098246093325863E-2,7.5777099358276416,-50072.740511842596,1343.5735435026049,1.1363617847509069,4.4974214475837396E-2,24.14997423824677,-43366.113371071653,749.515632856406]
["KBM","KBMS-17H02-A (240 V)",3.58,1.59,3.2293984816464585,1.3980080007127527,1100,12.2,1710,27.5,97,140,0.128,325,10,472.71716234697635,1271.359838524784,1610,3.174781191126816,19.53125,1.3101705256477791,1.0498838704230116,3.2020679686874494,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.16661854113074973,0.237030345885307,1.9994224935689966,5.6887283012473677,3.6215569162011172,212.86381866991732,172.55638099825697,1659.9923852032321,7.6400195858433745E-2,36.132273191648366,-34152.849209235828,472.71716234697635,2.3396147042202605E-2,9.3409679452893126,-49692.230380677014,1271.359838524784,1.4007819110920652,4.4974214475837396E-2,24.14997423824677,-43366.113371071653,749.515632856406]
["KBM","KBMS-17H02-A (400 V)",3.58,1.59,3.1376260209545084,1.3582796627508693,2100,12.2,2861,27.5,97,140,0.128,565,10,472.71716234697635,1252.3382263474198,1610,3.3161895979523419,19.53125,1.2918229856400649,1.0498838704230116,3.2020679686874494,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.16661854113074973,0.237030345885307,1.9994224935689966,5.6887283012473677,3.6215569162011172,212.86381866991732,172.55638099825697,1659.9923852032321,7.6400195858433745E-2,36.132273191648366,-34152.849209235828,472.71716234697635,2.3782721915847252E-2,9.8050511714916233,-49578.896881689172,1252.3382263474198,1.4703763463061674,4.4974214475837396E-2,24.14997423824677,-43366.113371071653,749.515632856406]
["KBM","KBMS-17H02-A (480 V)",3.58,1.59,3.0667933265015219,1.3276161586586674,2600,12.2,3438,27.5,97,140,0.128,679,10,472.71716234697635,1249.5485211281468,1610,3.3333551384988005,19.53125,1.2896060140898866,1.0498838704230116,3.2020679686874494,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.16661854113074973,0.237030345885307,1.9994224935689966,5.6887283012473677,3.6215569162011172,212.86381866991732,172.55638099825697,1659.9923852032321,7.6400195858433745E-2,36.132273191648366,-34152.849209235828,472.71716234697635,2.3841062910454968E-2,9.873195257530103,-49561.792849575068,1249.5485211281468,1.4805953090121409,4.4974214475837396E-2,24.14997423824677,-43366.113371071653,749.515632856406]
["KBM","KBMS-17H02-B (120 V)",3.52,2.99,3.246760839074665,2.7056340325622208,1000,12.3,1565,7.78,27,72.8,0.128,160,10,1237.3711695743309,1565,1565,3.0923807131518508,19.53125,1.3253908950971118,1.04134822920006,1.5335463258785942,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.31866748641576814,0.45333408884103471,3.8240098369892177,10.880018132184833,6.9264346666666663,212.86381866991732,172.55638099825697,1659.9923852032321,2.1662477493410739E-2,10.249560421072978,-45849.657153441156,1237.3711695743309,6.1046986617374682E-3,2.2732039216489941,-50561.404713547941,2697.7430923289362,2.3172174639236984,1.2491108769317746E-2,6.7948730287278165,-48627.24993684089,1719.7261330693043]
["KBM","KBMS-17H02-B (240 V)",3.52,2.99,3.0516230392837325,2.5430191994031106,2300,12.3,3285,7.78,27,72.8,0.128,325,10,1237.3711695743309,2649.4325070821142,3096.1538461538462,2.9804638498739124,19.53125,1.3132401489337775,1.04134822920006,1.3955710469530214,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.31866748641576814,0.45333408884103471,3.8240098369892177,10.880018132184833,6.9264346666666663,212.86381866991732,172.55638099825697,1659.9923852032321,2.1662477493410739E-2,10.249560421072978,-45849.657153441156,1237.3711695743309,6.2594608604300099E-3,2.4821523008465078,-50514.534243156515,2649.4325070821142,2.5302114803090845,1.2491108769317746E-2,6.7948730287278165,-48627.24993684089,1719.7261330693043]
["KBM","KBMS-17H02-B (400 V)",3.52,2.99,2.6043536142310146,2.1702946785258455,4400,12.3,5495,7.78,27,72.8,0.128,565,10,1237.3711695743309,2645.077785707902,3096.1538461538462,2.9695554739633474,19.53125,1.3140120007041849,1.04134822920006,1.3955710469530214,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.31866748641576814,0.45333408884103471,3.8240098369892177,10.880018132184833,6.9264346666666663,212.86381866991732,172.55638099825697,1659.9923852032321,2.1662477493410739E-2,10.249560421072978,-45849.657153441156,1237.3711695743309,6.2739488457827577E-3,2.5008193963248093,-50510.146487656501,2645.077785707902,2.5492400061844371,1.2491108769317746E-2,6.7948730287278165,-48627.24993684089,1719.7261330693043]
["KBM","KBMS-17H02-B (480 V)",3.52,2.99,2.2252489291013626,1.8543741075844689,5450,12.3,6602,7.78,27,72.8,0.128,679,10,1237.3711695743309,2657.0163648264056,3096.1538461538462,2.8887752690359276,19.53125,1.3191353862307806,1.04134822920006,1.3955710469530214,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.31866748641576814,0.45333408884103471,3.8240098369892177,10.880018132184833,6.9264346666666663,212.86381866991732,172.55638099825697,1659.9923852032321,2.1662477493410739E-2,10.249560421072978,-45849.657153441156,1237.3711695743309,6.2344436708700237E-3,2.449583943966573,-50522.110818395522,2657.0163648264056,2.4970125382279269,1.2491108769317746E-2,6.7948730287278165,-48627.24993684089,1719.7261330693043]
["KBM","KBMS-17H02-C (120 V)",3.64,5.27,3.2166051656467265,4.5304298107700376,1900,12.7,2797,2.5099999999999998,9.1999999999999993,43,0.128,160,10,2310.112350897934,2797,2797,3.0167182359546807,19.53125,1.2719320766843993,1.0085498597764362,0.85806220951018952,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.54314834613611895,0.77267895564305278,6.5177801536334279,18.544294935433268,11.805664820512817,212.86381866991732,172.55638099825697,1659.9923852032321,7.7328293424558442E-3,3.437286694500266,-49207.683009709501,2310.112350897934,2.0770639854113806E-3,0.67672789357963203,-50743.239956469886,4782.4778634053628,3.6200225287346335,4.2745769692144756E-3,2.206953858125686,-50146.608711209323,3176.6732510203997]
["KBM","KBMS-17H02-C (240 V)",3.64,5.27,2.6891697281044387,3.7875629973301956,4350,12.7,5622,2.5099999999999998,9.1999999999999993,43,0.128,325,10,2310.112350897934,4743.9524159487992,5241.8604651162786,2.6030589504560453,19.53125,1.2712415303436566,1.0085498597764362,0.75550735324417784,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.54314834613611895,0.77267895564305278,6.5177801536334279,18.544294935433268,11.805664820512817,212.86381866991732,172.55638099825697,1659.9923852032321,7.7328293424558442E-3,3.437286694500266,-49207.683009709501,2310.112350897934,2.1036796332959597E-3,0.71512643295109568,-50736.013729704522,4743.9524159487992,3.8254279493091081,4.2745769692144756E-3,2.206953858125686,-50146.608711209323,3176.6732510203997]
["KBM","KBMS-17H02-C (400 V)",3.64,5.27,0.99787623049680418,1.4054594795729638,7560,12.7,9375,2.5099999999999998,9.1999999999999993,43,0.128,565,10,2310.112350897934,4875.3062910377648,5241.8604651162786,1.9361425085768065,19.53125,1.292821414138811,1.0085498597764362,0.75550735324417784,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.54314834613611895,0.77267895564305278,6.5177801536334279,18.544294935433268,11.805664820512817,212.86381866991732,172.55638099825697,1659.9923852032321,7.7328293424558442E-3,3.437286694500266,-49207.683009709501,2310.112350897934,2.0165870604503893E-3,0.5801041397868294,-50759.659619659571,4875.3062910377648,3.1031527959227487,4.2745769692144756E-3,2.206953858125686,-50146.608711209323,3176.6732510203997]
["KBM","KBMS-17H02-D (120 V)",3.58,6.5,3.083627022405472,5.4577469423105702,2400,12.8,3365,1.65,3.1,34.200000000000003,0.128,160,10,3365,3365,3365,2.8840437209976724,19.53125,1.291181830621577,1.0006705639969327,0.71322436849925708,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.68114497946532904,0.96899198003427378,8.1737397535839484,23.255807520822572,14.805106890130352,212.86381866991732,172.55638099825697,1659.9923852032321,2.236880984939061E-3,2.2714907743900832,-49702.327004775136,4233.2841459140927,1.2037323730476029E-3,0.40598346489728943,-50769.930661534745,6327.9430257069707,4.1537243087894211,1.602756760575976E-3,1.4470456261892874,-50357.598988861202,5172.022323958432]
["KBM","KBMS-17H02-D (240 V)",3.58,6.5,2.1997486777344109,3.8933604915653293,5600,12.8,7054,1.65,3.1,34.200000000000003,0.128,325,10,4233.2841459140927,6341.7585557425273,6590.6432748538009,2.01692488713344,19.53125,1.2978467261773616,1.0006705639969327,0.46403512005012937,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.68114497946532904,0.96899198003427378,8.1737397535839484,23.255807520822572,14.805106890130352,212.86381866991732,172.55638099825697,1659.9923852032321,2.236880984939061E-3,2.2714907743900832,-49702.327004775136,4233.2841459140927,1.2010215080234523E-3,0.38950822656441692,-50772.731932696952,6341.7585557425273,3.9851617837770665,1.602756760575976E-3,1.4470456261892874,-50357.598988861202,5172.022323958432]
["KBM","KBMS-17H02-E (120 V)",3.75,9.33,3.0012074983043124,7.2844842191852246,3500,12.9,4633,0.8,3.1,24.8,0.128,160,10,4153.695712245395,4633,4633,2.7588126684696799,19.53125,1.2322365112389189,0.99291342784191783,0.51802287934383773,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.93338239659951761,1.3278231270529968,11.200588759194211,31.867755049271921,20.287642965333333,212.86381866991732,172.55638099825697,1659.9923852032321,2.650497638264534E-3,1.1029158588490393,-50310.711105740804,4153.695712245395,6.6245942886233053E-4,0.16834084653099118,-50793.64097659877,8630.2529471139023,4.898771827634941,1.4283293443475506E-3,0.69716229109440919,-50607.597540597359,5713.3742658710162]
["KBM","KBMS-17H02-E (240 V)",3.75,9.33,1.1013522061959158,2.6731849664949414,7500,12.9,9600,0.8,3.1,24.8,0.128,325,10,4153.695712245395,8920.4649935066918,9088.7096774193542,0.59971067669892486,19.53125,1.2538103726572971,0.99291342784191783,0.4200670021455552,12.80858321916074,0,-10.374952407520199,0,0,0,0,0,0.93338239659951761,1.3278231270529968,11.200588759194211,31.867755049271921,20.287642965333333,212.86381866991732,172.55638099825697,1659.9923852032321,2.650497638264534E-3,1.1029158588490393,-50310.711105740804,4153.695712245395,6.2840087143350119E-4,8.9357032945464043E-2,-50801.914406487056,8920.4649935066918,2.6003178944077581,1.4283293443475506E-3,0.69716229109440919,-50607.597540597359,5713.3742658710162]
["KBM","KBMS-17H03-A (120 V)",4.88,3,4.5018112474564687,2.7283704530039206,700,18.5,1136,8.61,33,100,0.17499999999999999,160,10,862.51303695395904,1136,1136,4.2662536815864982,14.285714285714286,0.98842126198615377,0.70473816510870402,2.112676056338028,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.23475188492379531,0.33395635385530292,2.8170226190855439,8.0149524925272697,5.1024772313296882,216.67074388966088,175.6424349963232,1689.6802246646291,3.8962277474955669E-2,16.9604331690743,-43613.75266793411,862.51303695395904,1.1227764478565451E-2,3.4920312142441832,-50500.302949968609,1970.9880557666497,2.3416087823025027,1.5829731308765319E-2,7.6093025856578258,-49357.622853997535,1541.7290692891122]
["KBM","KBMS-17H03-A (240 V)",4.88,3,4.2971834634811747,2.6043536142310151,1700,18.5,2389,8.61,33,100,0.17499999999999999,325,10,862.51303695395904,1930.4184815709446,2254,4.2181883450228783,14.285714285714286,0.96977186881248889,0.70473816510870402,1.5566937458775649,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.23475188492379531,0.33395635385530292,2.8170226190855439,8.0149524925272697,5.1024772313296882,216.67074388966088,175.6424349963232,1689.6802246646291,3.8962277474955669E-2,16.9604331690743,-43613.75266793411,862.51303695395904,1.1519645885665864E-2,3.8850068083483085,-50427.828052477184,1930.4184815709446,2.605121633685743,1.5829731308765319E-2,7.6093025856578258,-49357.622853997535,1541.7290692891122]
["KBM","KBMS-17H03-A (400 V)",4.88,3,3.5950293027816365,2.1788056380494769,3400,18.5,3997,8.61,33,100,0.17499999999999999,565,10,862.51303695395904,1932.7364961594571,2254,4.1495559520560601,14.285714285714286,0.97303566216193749,0.70473816510870402,1.5566937458775649,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.23475188492379531,0.33395635385530292,2.8170226190855439,8.0149524925272697,5.1024772313296882,216.67074388966088,175.6424349963232,1689.6802246646291,3.8962277474955669E-2,16.9604331690743,-43613.75266793411,862.51303695395904,1.150228710377503E-2,3.8627540316498643,-50432.138282274318,1932.7364961594571,2.5901998606113374,1.5829731308765319E-2,7.6093025856578258,-49357.622853997535,1541.7290692891122]
["KBM","KBMS-17H03-A (480 V)",4.88,3,3.4812625526936092,2.1098560925415812,3950,18.5,4803,8.61,33,100,0.17499999999999999,679,10,862.51303695395904,1928.4715572122971,2254,4.1971074979397196,14.285714285714286,0.9708181435419545,0.70473816510870402,1.5566937458775649,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.23475188492379531,0.33395635385530292,2.8170226190855439,8.0149524925272697,5.1024772313296882,216.67074388966088,175.6424349963232,1689.6802246646291,3.8962277474955669E-2,16.9604331690743,-43613.75266793411,862.51303695395904,1.153429005734889E-2,3.9036809945735005,-50424.191867315145,1928.4715572122971,2.6176437549912155,1.5829731308765319E-2,7.6093025856578258,-49357.622853997535,1541.7290692891122]
["KBM","KBMS-17H03-B (120 V)",4.8899999999999997,5.32,4.3653927248062727,4.5951502366381822,1400,18.8,1998,2.81,11,57,0.17499999999999999,160,10,1684.8382566120974,1998,1998,4.1413104744020952,14.285714285714286,0.97067543777405008,0.69349234332505449,1.2012012012012012,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.41544202696916194,0.59100485864007035,4.9853043236299435,14.184116607361689,9.0298890858138279,216.67074388966088,175.6424349963232,1689.6802246646291,1.3656948226580453E-2,5.6741710728172361,-48327.765619914135,1684.8382566120974,3.5859294013781589E-3,1.0209143750048457,-50724.961003301672,3621.4005345593055,3.6799974354036724,5.2776574029732726E-3,2.5050951078707651,-50322.280537128499,2859.6507354678479]
["KBM","KBMS-17H03-B (240 V)",4.8899999999999997,5.32,3.8500338614610872,4.0526672225906184,3150,18.8,4194,2.81,11,57,0.17499999999999999,325,10,1684.8382566120974,3573.8007733040213,3954.385964912281,3.7101168920252814,14.285714285714286,0.96655461866034176,0.69349234332505449,0.83926333038966472,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.41544202696916194,0.59100485864007035,4.9853043236299435,14.184116607361689,9.0298890858138279,216.67074388966088,175.6424349963232,1689.6802246646291,1.3656948226580453E-2,5.6741710728172361,-48327.765619914135,1684.8382566120974,3.6562025087112818E-3,1.1223416665515569,-50708.233959950936,3573.8007733040213,4.0456031922724272,5.2776574029732726E-3,2.5050951078707651,-50322.280537128499,2859.6507354678479]
["KBM","KBMS-17H03-B (400 V)",4.8899999999999997,5.32,1.8011681364546206,1.8959664594259165,6150,18.8,7006,2.81,11,57,0.17499999999999999,565,10,1684.8382566120974,3637.0828436735619,3954.385964912281,3.0632784751393274,14.285714285714286,0.98266257008583424,0.69349234332505449,0.83926333038966472,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.41544202696916194,0.59100485864007035,4.9853043236299435,14.184116607361689,9.0298890858138279,216.67074388966088,175.6424349963232,1689.6802246646291,1.3656948226580453E-2,5.6741710728172361,-48327.765619914135,1684.8382566120974,3.5636861374357533E-3,0.98663988906841782,-50730.255547037479,3637.0828436735619,3.556451305156231,5.2776574029732726E-3,2.5050951078707651,-50322.280537128499,2859.6507354678479]
["KBM","KBMS-17H03-C (120 V)",5.05,6.14,4.4762327744595565,5.2723589805177342,1600,18.8,2239,2.1,8.8000000000000007,51.34,0.17499999999999999,160,10,1930.6834454921473,2239,2239,4.2470844887593415,14.285714285714286,0.937457504970029,0.69349234332505449,1.0719071013845467,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.46428499527053885,0.66048851629288519,5.5714199432464664,15.851724391029245,10.091521173450674,216.67074388966088,175.6424349963232,1689.6802246646291,1.0955224928801929E-2,4.2684542281114854,-49077.0573450101,1930.6834454921473,2.9181813954221631E-3,0.78640322127602713,-50746.503135025981,4037.5385896962139,4.2112351966841333,4.2573709123449243E-3,1.8844838598959142,-50468.328170342174,3228.7992749674122]
["KBM","KBMS-17H03-C (240 V)",5.05,6.14,3.8063629746453294,4.4833486156010949,3575,18.8,4700,2.1,8.8000000000000007,51.34,0.17499999999999999,325,10,1930.6834454921473,4002.8693683733295,4390.3389170237624,3.6575198449882134,14.285714285714286,0.93652883594222525,0.69349234332505449,0.74331037503848019,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.46428499527053885,0.66048851629288519,5.5714199432464664,15.851724391029245,10.091521173450674,216.67074388966088,175.6424349963232,1689.6802246646291,1.0955224928801929E-2,4.2684542281114854,-49077.0573450101,1930.6834454921473,2.9570591699183682E-3,0.83879262006305977,-50738.427486724671,4002.8693683733295,4.4917834881154493,4.2573709123449243E-3,1.8844838598959142,-50468.328170342174,3228.7992749674122]
["KBM","KBMS-17H03-C (400 V)",5.05,6.14,1.429447174066097,1.6836833616797373,6480,18.8,7200,2.1,8.8000000000000007,51.34,0.17499999999999999,565,10,1930.6834454921473,4098.8232070553631,4390.3389170237624,2.7598756257241117,14.285714285714286,0.95511502138359083,0.69349234332505449,0.74331037503848019,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.46428499527053885,0.66048851629288519,5.5714199432464664,15.851724391029245,10.091521173450674,216.67074388966088,175.6424349963232,1689.6802246646291,1.0955224928801929E-2,4.2684542281114854,-49077.0573450101,1930.6834454921473,2.8530720478032231E-3,0.68981111277069973,-50760.027576671928,4098.8232070553631,3.6939788121037975,4.2573709123449243E-3,1.8844838598959142,-50468.328170342174,3228.7992749674122]
["KBM","KBMS-17H03-D (120 V)",5,10.38,4.0139416156057672,8.0278832312115345,2950,19,3838,0.74,2.9,30,0.17499999999999999,160,10,3532.7056279518783,3838,3838,3.7171213290491307,14.285714285714286,0.94499837950663113,0.68619242392163293,0.62532569046378317,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.79274772531226001,1.1277572487152037,9.5129727037471206,27.06617396916489,17.230861511111108,216.67074388966088,175.6424349963232,1689.6802246646291,3.5903972108365162E-3,1.5166820675931789,-50166.180973844806,3532.7056279518783,9.5020495308583688E-4,0.20718563115308283,-50793.236142845475,7203.0860589198619,5.3882288251556254,1.4134149228081435E-3,0.66255295261849001,-50683.222106937923,5758.4183397997194]
["KBM","KBMS-17H03-D (240 V)",5,10.38,1.4103576495527956,2.8207152991055913,6500,19,8030,0.74,2.9,30,0.17499999999999999,325,10,3532.7056279518783,7379.9454814559213,7513.3333333333339,0.92440540858066811,14.285714285714286,0.96457973482341453,0.68619242392163293,0.41678111216967839,13.037656054511025,0,-10.56050140415393,0,0,0,0,0,0.79274772531226001,1.1277572487152037,9.5129727037471206,27.06617396916489,17.230861511111108,216.67074388966088,175.6424349963232,1689.6802246646291,3.5903972108365162E-3,1.5166820675931789,-50166.180973844806,3532.7056279518783,9.1660830376453888E-4,0.11916507471711768,-50801.215468046576,7379.9454814559213,3.0990985570238632,1.4134149228081435E-3,0.66255295261849001,-50683.222106937923,5758.4183397997194]
["KBM","KBMS-17H04-A (120 V)",5.98,3.15,5.4908455366703892,2.8014518044236678,600,23.7,960,8.64,34,118,0.24,160,10,717.73838207742233,960,960,5.1973528586726223,10.416666666666668,0.83638959357772702,0.56347927898355954,2.5,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.20603632818914794,0.29310580805823322,2.4724359382697751,7.0345393933975977,4.4783268673355634,221.9356404701573,179.91038201492543,1730.7378749835825,5.0969185492360604E-2,22.045202524812183,-42079.381589342403,717.73838207742233,1.5205055861972792E-2,4.0995127375332263,-50503.414727714793,1692.6664823754891,2.3215383538931147,1.8691030384642971E-2,7.9081002494282622,-49682.313663548419,1432.4823347479139]
["KBM","KBMS-17H04-A (240 V)",5.98,3.15,5.2862177526950962,2.6970498738240285,1400,23.7,2018,8.64,34,118,0.24,325,10,717.73838207742233,1649.6622528645541,1910.1694915254236,5.1624954392239708,10.416666666666668,0.81541341379721755,0.56347927898355954,1.6754133309590504,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.20603632818914794,0.29310580805823322,2.4724359382697751,7.0345393933975977,4.4783268673355634,221.9356404701573,179.91038201492543,1730.7378749835825,5.0969185492360604E-2,22.045202524812183,-42079.381589342403,717.73838207742233,1.5642172707273309E-2,4.7476819120786402,-50400.454392087791,1649.6622528645541,2.688594073647717,1.8691030384642971E-2,7.9081002494282622,-49682.313663548419,1432.4823347479139]
["KBM","KBMS-17H04-A (400 V)",5.98,3.15,4.703912762493796,2.3999554910682632,2700,23.7,3377,8.64,34,118,0.24,565,10,717.73838207742233,1641.9000012068673,1910.1694915254236,5.2039971715549989,10.416666666666668,0.81394904315468009,0.56347927898355954,1.6754133309590504,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.20603632818914794,0.29310580805823322,2.4724359382697751,7.0345393933975977,4.4783268673355634,221.9356404701573,179.91038201492543,1730.7378749835825,5.0969185492360604E-2,22.045202524812183,-42079.381589342403,717.73838207742233,1.5726560602960411E-2,4.8628754178799118,-50380.577313095724,1641.9000012068673,2.7538277145603627,1.8691030384642971E-2,7.9081002494282622,-49682.313663548419,1432.4823347479139]
["KBM","KBMS-17H04-A (480 V)",5.98,3.15,4.332815167158464,2.2106199832441145,3350,23.7,4058,8.64,34,118,0.24,679,10,717.73838207742233,1642.3450415721663,1910.1694915254236,5.1724639275312914,10.416666666666668,0.81516646262408909,0.56347927898355954,1.6754133309590504,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.20603632818914794,0.29310580805823322,2.4724359382697751,7.0345393933975977,4.4783268673355634,221.9356404701573,179.91038201492543,1730.7378749835825,5.0969185492360604E-2,22.045202524812183,-42079.381589342403,717.73838207742233,1.572167670636326E-2,4.8562831597502631,-50381.727686590173,1642.3450415721663,2.7500945440431384,1.8691030384642971E-2,7.9081002494282622,-49682.313663548419,1432.4823347479139]
["KBM","KBMS-17H04-B (120 V)",6.12,5.53,5.4510568008974154,4.7816287727170312,1200,23.7,1660,2.8,12,69.3,0.24,160,10,1433.8127756122724,1660,1660,5.1946285745747582,10.416666666666668,0.79984358409106482,0.56347927898355954,1.4457831325301205,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.35343384953927842,0.50279246856525261,4.2412061944713413,12.067019245566062,7.6821030452674899,221.9356404701573,179.91038201492543,1730.7378749835825,1.838140627174089E-2,7.1973719747136995,-48108.529536303351,1433.8127756122724,5.2551536251839847E-3,1.3141023497115232,-50715.265747980877,2984.0229867777198,3.9100048719267564,6.5498454416743407E-3,2.5818560316876145,-50458.153521675129,2585.4531095973653]
["KBM","KBMS-17H04-B (240 V)",6.12,5.53,4.8647359963937822,4.267312277538406,2650,23.7,3485,2.8,12,69.3,0.24,325,10,1433.8127756122724,2946.9787485794532,3252.5252525252527,4.7240617575531001,10.416666666666668,0.79472089946947411,0.56347927898355954,0.92827055771812239,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.35343384953927842,0.50279246856525261,4.2412061944713413,12.067019245566062,7.6821030452674899,221.9356404701573,179.91038201492543,1730.7378749835825,1.838140627174089E-2,7.1973719747136995,-48108.529536303351,1433.8127756122724,5.3479889135799501E-3,1.4425747897632775,-50696.829632624926,2946.9787485794532,4.2922641888064126,6.5498454416743407E-3,2.5818560316876145,-50458.153521675129,2585.4531095973653]
["KBM","KBMS-17H04-B (400 V)",6.12,5.53,2.902986161996171,2.5464790894703255,5000,23.7,5822,2.8,12,69.3,0.24,565,10,1433.8127756122724,2977.3389479187158,3252.5252525252527,4.2043718808235457,10.416666666666668,0.80516880301129978,0.56347927898355954,0.92827055771812239,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.35343384953927842,0.50279246856525261,4.2412061944713413,12.067019245566062,7.6821030452674899,221.9356404701573,179.91038201492543,1730.7378749835825,1.838140627174089E-2,7.1973719747136995,-48108.529536303351,1433.8127756122724,5.2715010232781178E-3,1.3376205071407059,-50712.019326041111,2977.3389479187158,3.9799812403177204,6.5498454416743407E-3,2.5818560316876145,-50458.153521675129,2585.4531095973653]
["KBM","KBMS-17H04-B (480 V)",6.12,5.53,1.8009638297240791,1.5797928330912976,5700,23.7,6987,2.8,12,69.3,0.24,679,10,1433.8127756122724,3001.0220194584813,3252.5252525252527,3.8460486579235669,10.416666666666668,0.81236278202974432,0.56347927898355954,0.92827055771812239,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.35343384953927842,0.50279246856525261,4.2412061944713413,12.067019245566062,7.6821030452674899,221.9356404701573,179.91038201492543,1730.7378749835825,1.838140627174089E-2,7.1973719747136995,-48108.529536303351,1433.8127756122724,5.2143883298596131E-3,1.2535348393665133,-50723.361308409512,3001.0220194584813,3.7297911613421508,6.5498454416743407E-3,2.5818560316876145,-50458.153521675129,2585.4531095973653]
["KBM","KBMS-17H04-C (120 V)",6.1,6.2,5.4052622182153129,5.3517447705102104,1325,23.7,1868,2.23,9.1,61.4,0.24,160,10,1690.0098129364267,1868,1868,5.1205508102839286,10.416666666666668,0.8005315797108451,0.56347927898355954,1.2847965738758029,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.39755414540415562,0.56555768616013835,4.7706497448498677,13.57338446784332,8.6410849301760795,221.9356404701573,179.91038201492543,1730.7378749835825,1.3650068039579633E-2,5.7127347815458362,-48640.989910378128,1690.0098129364267,4.0856354931225643E-3,1.0211361447223808,-50736.013442340343,3401.1873050413137,4.3057596882511451,5.0413472154303036E-3,2.0492839337725708,-50526.671326299329,2969.095926462167]
["KBM","KBMS-17H04-C (240 V)",6.1,6.2,4.6473243382833438,4.601311226023113,3000,23.7,3922,2.23,9.1,61.4,0.24,325,10,1690.0098129364267,3372.8359814927621,3671.0097719869709,4.4667877529077513,10.416666666666668,0.7980665784967218,0.56347927898355954,0.80832686428549494,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.39755414540415562,0.56555768616013835,4.7706497448498677,13.57338446784332,8.6410849301760795,221.9356404701573,179.91038201492543,1730.7378749835825,1.3650068039579633E-2,5.7127347815458362,-48640.989910378128,1690.0098129364267,4.1339028221691722E-3,1.0964271836945678,-50725.440814044159,3372.8359814927621,4.6232346127932846,5.0413472154303036E-3,2.0492839337725708,-50526.671326299329,2969.095926462167]
["KBM","KBMS-17H04-C (400 V)",6.1,6.2,1.6122189040477708,1.5962563406413572,5775,23.7,6548,2.23,9.1,61.4,0.24,565,10,1690.0098129364267,3441.0894962713696,3671.0097719869709,3.4259123132733449,10.416666666666668,0.81642536609184924,0.56347927898355954,0.80832686428549494,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.39755414540415562,0.56555768616013835,4.7706497448498677,13.57338446784332,8.6410849301760795,221.9356404701573,179.91038201492543,1730.7378749835825,1.3650068039579633E-2,5.7127347815458362,-48640.989910378128,1690.0098129364267,4.0211974785110266E-3,0.91097283844856314,-50750.128148707743,3441.0894962713696,3.8412410971408208,5.0413472154303036E-3,2.0492839337725708,-50526.671326299329,2969.095926462167]
["KBM","KBMS-17H04-D (120 V)",6.07,9.56,5.5993602705966818,8.48387919787376,2200,24,2881,0.94,3.8,40,0.24,160,10,2718.2468695416965,2881,2881,5.4536758816313817,10.416666666666668,0.78576763601404231,0.55643578799626503,0.83304408191600143,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.6160325116487414,0.87636344863991666,7.3923901397848972,21.032722767357999,13.389847180425896,221.9356404701573,179.91038201492543,1730.7378749835825,5.8421555307359733E-3,2.4616647977020558,-49858.317253711641,2718.2468695416965,1.7573229090016387E-3,0.47405813734031083,-50770.045762878355,5241.805423005444,7.2791913086425826,2.1323250971669429E-3,0.87201527539022761,-50686.345837419707,4675.3064272604197]
["KBM","KBMS-17H04-D (240 V)",6.07,9.56,3.9629580829881941,6.0044819439215056,5000,24,6037,0.94,3.8,40,0.24,325,10,2718.2468695416965,5322.9776493863155,5635,3.8268525938852123,10.416666666666668,0.7982884297234365,0.55643578799626503,0.51333533691102329,13.354458911910362,0,-10.817111718647391,0,0,0,0,0,0.6160325116487414,0.87636344863991666,7.3923901397848972,21.032722767357999,13.389847180425896,221.9356404701573,179.91038201492543,1730.7378749835825,5.8421555307359733E-3,2.4616647977020558,-49858.317253711641,2718.2468695416965,1.715766938035314E-3,0.40665666528354455,-50779.320993215704,5322.9776493863155,6.2442376374789905,2.1323250971669429E-3,0.87201527539022761,-50686.345837419707,4675.3064272604197]
["KBM","KBMS-25H01-A (120 V)",4.9000000000000004,3.1,4.4336019861313707,2.6870315067462855,700,14.37,1132,8.98,37,100.3,0.434,160,10,978.76347406597222,1132,1132,4.1457677832867308,5.7603686635944698,1.0928213721825946,0.99512829464123354,2.1201413427561837,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.26497786242947763,0.37695561344713457,3.1797343491537315,9.0469347227312298,5.7594575238095231,237.64933180271592,192.64856234736905,1853.2791697816904,3.3325286234856297E-2,14.182744492534097,-45806.441267351831,978.76347406597222,1.1317860262697134E-2,3.2976729377763885,-50534.917715772361,1972.4003512879824,2.1138281795199503,1.9397471763675483E-2,8.9850288668459957,-48798.946742015833,1371.3246896707587]
["KBM","KBMS-25H01-A (240 V)",4.9000000000000004,3.1,4.1090912580089336,2.4903583381872325,1650,14.37,2379,8.98,37,100.3,0.434,325,10,978.76347406597222,1910.1549559147838,2247.258225324028,3.984388937460265,5.7603686635944698,1.0731243376882966,0.99512829464123354,1.7501325674929806,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.26497786242947763,0.37695561344713457,3.1797343491537315,9.0469347227312298,5.7594575238095231,237.64933180271592,192.64856234736905,1853.2791697816904,3.3325286234856297E-2,14.182744492534097,-45806.441267351831,978.76347406597222,1.1794680503489498E-2,3.8726246114082117,-50432.468965901782,1910.1549559147838,2.4823756590661215,1.9397471763675483E-2,8.9850288668459957,-48798.946742015833,1371.3246896707587]
["KBM","KBMS-25H01-A (400 V)",4.9000000000000004,3.1,3.304359770860303,2.0026422853698809,3150,14.37,3979,8.98,37,100.3,0.434,565,10,978.76347406597222,1904.1052217300105,2247.258225324028,3.9354708278389312,5.7603686635944698,1.0759473979371905,0.99512829464123354,1.7501325674929806,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.26497786242947763,0.37695561344713457,3.1797343491537315,9.0469347227312298,5.7594575238095231,237.64933180271592,192.64856234736905,1853.2791697816904,3.3325286234856297E-2,14.182744492534097,-45806.441267351831,978.76347406597222,1.1844351656253492E-2,3.9276808411522941,-50421.796710259187,1904.1052217300105,2.5176670333434141,1.9397471763675483E-2,8.9850288668459957,-48798.946742015833,1371.3246896707587]
["KBM","KBMS-25H01-A (480 V)",4.9000000000000004,3.1,2.7893997920842706,1.6905453285359218,3800,14.37,4779,8.98,37,100.3,0.434,679,10,978.76347406597222,1910.5640769793999,2247.258225324028,3.8388323847081463,5.7603686635944698,1.0810543107878836,0.99512829464123354,1.7501325674929806,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.26497786242947763,0.37695561344713457,3.1797343491537315,9.0469347227312298,5.7594575238095231,237.64933180271592,192.64856234736905,1853.2791697816904,3.3325286234856297E-2,14.182744492534097,-45806.441267351831,978.76347406597222,1.1791343041510674E-2,3.8688972301143871,-50433.18604705359,1910.5640769793999,2.479986385246864,1.9397471763675483E-2,8.9850288668459957,-48798.946742015833,1371.3246896707587]
["KBM","KBMS-25H01-B (120 V)",4.96,5.34,4.2630788328186258,4.4874514029669745,1400,14.64,1989,2.87,12,57.5,0.434,160,10,1948.7718710921272,1989,1989,3.9698741417687478,5.7603686635944698,1.0614160880993784,0.97677551871547297,1.2066365007541477,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.45092421620250467,0.6414815674725366,5.411090594430056,15.395557619340879,9.8011163870967728,237.64933180271592,192.64856234736905,1853.2791697816904,1.0661921313160422E-2,4.5051683668662887,-49270.449828823243,1948.7718710921272,3.6549675980442104E-3,0.98092725384928858,-50732.402474302893,3593.8654381626652,3.4318352617199039,6.1505283329253407E-3,2.8014696070911747,-50211.720910438147,2638.5572754983723]
["KBM","KBMS-25H01-B (240 V)",4.96,5.34,3.3346749981159021,3.510184208543055,3150,14.64,4173,2.87,12,57.5,0.434,325,10,1948.7718710921272,3581.8802706229944,3920,3.1118350610797041,5.7603686635944698,1.0632589687054117,0.97677551871547297,0.90958798669499663,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.45092421620250467,0.6414815674725366,5.411090594430056,15.395557619340879,9.8011163870967728,237.64933180271592,192.64856234736905,1853.2791697816904,1.0661921313160422E-2,4.5051683668662887,-49270.449828823243,1948.7718710921272,3.6730711975620695E-3,1.0060674099735791,-50728.625282917892,3581.8802706229944,3.5197896680572978,6.1505283329253407E-3,2.8014696070911747,-50211.720910438147,2638.5572754983723]
["KBM","KBMS-25H01-B (400 V)",4.96,5.34,1.4226503076377583,1.497526639618693,4900,14.64,6970,2.87,12,57.5,0.434,565,10,1948.7718710921272,3665.6835037666979,3920,2.3137133848272504,5.7603686635944698,1.0845953096718688,0.97677551871547297,0.90958798669499663,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.45092421620250467,0.6414815674725366,5.411090594430056,15.395557619340879,9.8011163870967728,237.64933180271592,192.64856234736905,1853.2791697816904,1.0661921313160422E-2,4.5051683668662887,-49270.449828823243,1948.7718710921272,3.5523160341350561E-3,0.82399713865933621,-50753.820016293481,3665.6835037666979,2.8828054526068727,6.1505283329253407E-3,2.8014696070911747,-50211.720910438147,2638.5572754983723]
["KBM","KBMS-25H01-C (120 V)",4.8499999999999996,6.45,3.9834208613857238,5.2002883307907624,1750,15.1,2470,1.97,7.9,46.3,0.434,160,10,2396.401103400091,2470,2470,3.6268854443558505,5.7603686635944698,1.086382296259583,0.94701944331089571,0.97165991902834004,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.55700866924400683,0.79239655224454209,6.6841040309280819,19.017517253869009,12.106927505154641,237.64933180271592,192.64856234736905,1853.2791697816904,7.3185968558146762E-3,3.1725083064621877,-49631.388494491795,2396.401103400091,2.3128421466775771E-3,0.5735750558717041,-50766.79293844747,4562.7211854455936,3.6306335081073891,4.0246543933083528E-3,1.9126776648474493,-50378.519971636961,3308.3551559171042]
["KBM","KBMS-25H01-C (240 V)",4.8499999999999996,6.45,2.3166932544737429,3.0244037264670274,4225,15.1,5178,1.97,7.9,46.3,0.434,325,10,2396.401103400091,4608.6773773196401,4868.2505399568036,2.0866405945755968,5.7603686635944698,1.0975676670598262,0.94701944331089571,0.72543602089017545,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.55700866924400683,0.79239655224454209,6.6841040309280819,19.017517253869009,12.106927505154641,237.64933180271592,192.64856234736905,1853.2791697816904,7.3185968558146762E-3,3.1725083064621877,-49631.388494491795,2396.401103400091,2.2791481446824491E-3,0.51327966724287,-50774.435406331497,4608.6773773196401,3.2489738524107024,4.0246543933083528E-3,1.9126776648474493,-50378.519971636961,3308.3551559171042]
["KBM","KBMS-25H01-D (120 V)",4.75,7.95,3.6744032513824534,5.9941325471165632,2300,15.2,3097,1.3,5.2,37.1,0.434,160,10,2963.410697101574,3097,3097,3.3016855954484603,5.7603686635944698,1.1073413100048375,0.94078905223648202,0.77494349370358406,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.70099915999594586,0.99723639537067088,8.4119899199513508,23.933673488896101,15.236649768421053,237.64933180271592,192.64856234736905,1853.2791697816904,4.9747269056431677E-3,2.1251764578237542,-49984.842112000006,2963.410697101574,1.4527632400673303E-3,0.30957011408711066,-50787.753548518267,5807.0633765688508,3.7057928405817222,2.6671660374366917E-3,1.2728211235831051,-50510.902908610202,4119.713400072088]
["KBM","KBMS-25H01-D (240 V)",4.75,7.95,1.3252085057447611,2.1618409555379463,4900,15.2,6489,1.3,5.2,37.1,0.434,325,10,2963.410697101574,5963.0341684775804,6075.4716981132078,0.58221455098869779,5.7603686635944698,1.1334215975634729,0.94078905223648202,0.58256479685164608,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.70099915999594586,0.99723639537067088,8.4119899199513508,23.933673488896101,15.236649768421053,237.64933180271592,192.64856234736905,1853.2791697816904,4.9747269056431677E-3,2.1251764578237542,-49984.842112000006,2963.410697101574,1.3998753711264424E-3,0.17161648606482774,-50799.810536851444,5963.0341684775804,2.054381597074558,2.6671660374366917E-3,1.2728211235831051,-50510.902908610202,4119.713400072088]
["KBM","KBMS-25H01-E (120 V)",5.09,10.44,3.6221469807121007,7.2733875114700819,2900,15.32,3815,0.75,3.4,30,0.434,160,10,3755.3361358414709,3815,3815,3.1590140453160913,5.7603686635944698,1.0338564741972596,0.93341994738867662,0.62909567496723462,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.85906632425643947,1.2221016136321452,10.308795891077274,29.330438727171483,18.672337225933202,237.64933180271592,192.64856234736905,1853.2791697816904,3.2469255087942362E-3,1.2245728517823724,-50388.610369632668,3755.3361358414709,9.309629411255588E-4,0.14065529240653682,-50799.664469088348,7311.7774655863432,3.6092164859493145,1.7287312326109872E-3,0.72768232735596017,-50658.070675126066,5206.9038961828064]
["KBM","KBMS-25H01-E (240 V)",5.09,10.44,1.4421386680163577,2.8958607791493125,4900,15.32,6918,0.75,3.4,30,0.434,325,10,3755.3361358414709,6918,6918,-6.0184631563844349E-2,5.7603686635944698,1.0572591157057305,0.93341994738867662,0.46092650216944575,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,0.85906632425643947,1.2221016136321452,10.308795891077274,29.330438727171483,18.672337225933202,237.64933180271592,192.64856234736905,1853.2791697816904,3.2469255087942362E-3,1.2245728517823724,-50388.610369632668,3755.3361358414709,9.0155430545945487E-4,3.1513973149440364E-2,-50804.884130415652,7489.3763243575331,0.80864892804729038,1.7287312326109872E-3,0.72768232735596017,-50658.070675126066,5206.9038961828064]
["KBM","KBMS-25H01-F (120 V)",4.63,12,2.4658943081579734,6.2905467044846262,3950,15.73,4765,0.56000000000000005,2.1,23.7,0.434,160,10,4715.1301877093192,4765,4765,2.0193762983222134,5.7603686635944698,1.1468145336066005,0.9090905018432629,0.50367261280167885,14.299993593994525,0,-11.582994811135565,0,0,0,0,0,1.0855360071659783,1.5442757660901216,13.02643208599174,37.062618386162917,23.594795680345573,237.64933180271592,192.64856234736905,1853.2791697816904,2.0688350544394588E-3,0.93718640071617698,-50414.233354658558,4715.1301877093192,5.6190467015331403E-4,1.1184956125688809E-2,-50805.104318376892,9498.7789250804944,0.48656098779690993,1.0665018480020905E-3,0.54239193255956553,-50674.220777072012,6643.4739022784115]
["KBM","KBMS-25H02-A (120 V)",8.6999999999999993,3.33,8.0801740338962258,3.0262824096989611,390,29.4,707,8.9600000000000009,45,162,0.67800000000000005,160,10,581.71421286150496,707,707,7.576366774268287,3.6873156342182889,0.68200709120445613,0.52684431230511852,3.3946251768033946,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.17364518399789766,0.24702639781271896,2.0837422079747721,5.928633547505255,3.7742853394636016,257.41294358181017,208.66977884796827,2007.4032725174548,7.8970404630503171E-2,28.291499266412547,-43180.475017323763,581.71421286150496,2.8916815563840716E-2,6.3698085516207019,-50418.648216503774,1214.8904510479595,2.5336272886109676,3.2175342406227048E-2,9.488954882844018,-49947.437618039847,1107.1724670325721]
["KBM","KBMS-25H02-A (240 V)",8.6999999999999993,3.33,8.0691556147590937,3.0221556609584623,1000,29.4,1484,8.9600000000000009,45,162,0.67800000000000005,325,10,581.71421286150496,1173.6080179004432,1391.3580246913582,7.9596359714337961,3.6873156342182889,0.64693083120124439,0.52684431230511852,2.1676839620411137,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.17364518399789766,0.24702639781271896,2.0837422079747721,5.928633547505255,3.7742853394636016,257.41294358181017,208.66977884796827,2007.4032725174548,7.8970404630503171E-2,28.291499266412547,-43180.475017323763,581.71421286150496,3.0029421309786475E-2,7.5805199510997108,-50257.755995951258,1173.6080179004432,3.0151945783487282,3.2175342406227048E-2,9.488954882844018,-49947.437618039847,1107.1724670325721]
["KBM","KBMS-25H02-A (400 V)",8.6999999999999993,3.33,7.5170103891095179,2.8153596962956997,1950,29.4,2482,8.9600000000000009,45,162,0.67800000000000005,565,10,581.71421286150496,1169.708056229324,1391.3580246913582,7.9903833444645178,3.6873156342182889,0.64609241582108279,0.52684431230511852,2.1676839620411137,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.17364518399789766,0.24702639781271896,2.0837422079747721,5.928633547505255,3.7742853394636016,257.41294358181017,208.66977884796827,2007.4032725174548,7.8970404630503171E-2,28.291499266412547,-43180.475017323763,581.71421286150496,3.0143049709801986E-2,7.6934523775886161,-50241.324366272063,1169.708056229324,3.0601140881271722,3.2175342406227048E-2,9.488954882844018,-49947.437618039847,1107.1724670325721]
["KBM","KBMS-25H02-A (480 V)",8.6999999999999993,3.33,7.4404935895461071,2.7867017189311265,2400,29.4,2982,8.9600000000000009,45,162,0.67800000000000005,679,10,{"$f":"IF(AQ1184<I1184,IF(AQ1184<0,0,AQ1184),I1184)","v":581.71421286150496},{"$f":"IF(AU1184<I1184,IF(AU1184<0,0,AU1184),I1184)","v":1166.3697843933189},{"$f":"IF(UAC_V*0.98/L1184*1000<I1184,IF(UAC_V*0.98/L1184*1000<0,0,UAC_V*0.98/L1184*1000),I1184)","v":1391.3580246913582},{"$f":"C1184+(E1184-C1184)/G1184*Q1184","v":8.0878957414987038},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M1184,(inertia/gear^2+gear_inertia)/M1184),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M1184,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M1184))","v":3.6873156342182889},{"$f":"IF((C1184+(E1184-C1184)/G1184*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X1184^2*time1+Y1184^2*time2+Z1184^2*time3+AA1184^2*time4)/time)/(C1184+(E1184-C1184)/G1184*mspeed),SQRT((((X1184-Y1184)*2/PI()+Y1184)^2*time1+Y1184^2*time2+((Z1184-Y1184)*2/PI()+Y1184)^2*time3+AA1184^2*time4)/time)/(C1184+(E1184-C1184)/G1184*mspeed)),IF(AccType=1,SQRT((X1184^2*time1+Y1184^2*time2+Z1184^2*time3+AA1184^2*time4+AB1184^2*time5+AC1184^2*time6+AD1184^2*time7+AE1184^2*time8)/time)/(C1184+(E1184-C1184)/G1184*mspeed),SQRT((((X1184-Y1184)*2/PI()+Y1184)^2*time1+Y1184^2*time2+((Z1184-Y1184)*2/PI()+Y1184)^2*time3+AA1184^2*time4+((AB1184-AC1184)*2/PI()+AC1184)^2*time5+AC1184^2*time6+((AD1184-AC1184)*2/PI()+AC1184)^2*time7+AE1184^2*time8)/time)/(C1184+(E1184-C1184)/G1184*mspeed))))","v":0.6432701839999666},{"$f":"IF(move1,MAX(ABS(X1184),ABS(Z1184))/H1184,MAX(ABS(X1184),ABS(Z1184),ABS(AB1184),ABS(AD1184))/H1184)","v":0.52684431230511852},{"$f":"IF(AZ1184>0,speed/(MIN(AZ1184,I1184)),\"NA\")","v":2.1676839620411137},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M1184+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M1184+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":15.489222781770483},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M1184+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M1184+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-12.54627045323409},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M1184+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M1184+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M1184+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M1184+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH1184/Irms","v":0.17364518399789766},{"$f":"AI1184/Ipeak","v":0.24702639781271896},{"$f":"IF(move1,IF(AccType=1,SQRT((X1184^2*time1+Y1184^2*time2+Z1184^2*time3+AA1184^2*time4)/time)/(C1184/D1184),SQRT((((X1184-Y1184)*2/PI()+Y1184)^2*time1+Y1184^2*time2+((Z1184-AA1184)*2/PI()+AA1184)^2*time3+AA1184^2*time4)/time)/(C1184/D1184)),IF(AccType=1,SQRT((X1184^2*time1+Y1184^2*time2+Z1184^2*time3+AA1184^2*time4+AB1184^2*time5+AC1184^2*time6+AD1184^2*time7+AE1184^2*time8)/time)/(C1184/D1184),SQRT((((X1184-Y1184)*2/PI()+Y1184)^2*time1+Y1184^2*time2+((Z1184-AA1184)*2/PI()+AA1184)^2*time3+AA1184^2*time4+((AB1184-AC1184)*2/PI()+AC1184)^2*time5+AC1184^2*time6+((AD1184-AE1184)*2/PI()+AE1184)^2*time7+AE1184^2*time8)/time)/(C1184/D1184)))","v":2.0837422079747721},{"$f":"IF(move1,MAX(ABS(X1184),ABS(Z1184))/(C1184/D1184),MAX(ABS(X1184),ABS(Z1184),ABS(AB1184),ABS(AD1184))/(C1184/D1184))","v":5.928633547505255},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X1184),ABS(Z1184))/(C1184/D1184),MAX(ABS((X1184-Y1184)*2/PI()+Y1184),ABS((Z1184-Y1184)*2/PI()+Y1184))/(C1184/D1184)),IF(AccType=1,MAX(ABS(X1184),ABS(Z1184),ABS(AB1184),ABS(AD1184))/(C1184/D1184),MAX(ABS((X1184-Y1184)*2/PI()+Y1184),ABS((Z1184-Y1184)*2/PI()+Y1184),ABS((AB1184-AC1184)*2/PI()+AC1184),ABS((AD1184-AC1184)*2/PI()+AC1184))/(C1184/D1184)))","v":3.7742853394636016},{"$f":"IF((C1184+(E1184-C1184)/G1184*mspeed)<0,\"NA\",U1184*(C1184+(E1184-C1184)/G1184*mspeed)*mspeed/9.55)","v":257.41294358181017},{"$f":"IF(move1,IF(speed1>speed2,AM1184/2*time1/time,AM1184/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z1184*-speed/30*PI(),((Z1184-AA1184)*2/PI()+AA1184)*-speed/30*PI()),IF(AccType=1,X1184*-speed/30*PI(),((X1184-Y1184)*2/PI()+Y1184)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z1184*-speed/30*PI(),((Z1184-AA1184)*2/PI()+AA1184)*-speed/30*PI()),IF(AccType=1,X1184*-speed/30*PI(),((X1184-Y1184)*2/PI()+Y1184)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD1184*-speed/30*PI(),((AD1184-AE1184)*2/PI()+AE1184)*-speed/30*PI()),IF(AccType=1,AB1184*-speed/30*PI(),((AB1184-AC1184)*2/PI()+AC1184)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD1184*-speed/30*PI(),((AD1184-AE1184)*2/PI()+AE1184)*-speed/30*PI()),IF(AccType=1,AB1184*-speed/30*PI(),((AB1184-AC1184)*2/PI()+AC1184)*-speed/30*PI()),0)/2*time7/time)))","v":208.66977884796827},{"$f":"IF(move1,MAX(IF(AccType=1,Z1184*-speed/30*PI(),((Z1184-AA1184)*2/PI()+AA1184)*-speed/30*PI()),IF(AccType=1,X1184*-speed/30*PI(),((X1184-Y1184)*2/PI()+Y1184)*-speed/30*PI()),0),MAX(IF(AccType=1,Z1184*-speed/30*PI(),((Z1184-AA1184)*2/PI()+AA1184)*-speed/30*PI()),IF(AccType=1,X1184*-speed/30*PI(),((X1184-Y1184)*2/PI()+Y1184)*-speed/30*PI()),IF(AccType=1,AD1184*-speed/30*PI(),((AD1184-AE1184)*2/PI()+AE1184)*-speed/30*PI()),IF(AccType=1,AB1184*-speed/30*PI(),((AB1184-AC1184)*2/PI()+AC1184)*-speed/30*PI()),0))","v":2007.4032725174548},{"$f":"(L1184^2)/1000000+((K1184/1000)^2*(D1184/C1184*H1184)^2*PI()*PI()*(O1184/2)^2)/1200","v":7.8970404630503171E-2},{"$f":"SQRT(3)*L1184*J1184*D1184/C1184*H1184/1000","v":28.291499266412547},{"$f":"0.75*J1184^2*(D1184/C1184*H1184)^2-(UAC_V*0.98)^2","v":-43180.475017323763},{"$f":"-AO1184/2/AN1184+SQRT((AO1184/2/AN1184)^2-AP1184/AN1184)","v":581.71421286150496},{"$f":"(L1184^2)/1000000+((K1184/1000)^2*AV1184^2*PI()*PI()*(O1184/2)^2)/1200","v":3.0241499888577342E-2},{"$f":"SQRT(3)*L1184*J1184*AV1184/1000","v":7.7899758973116144},{"$f":"0.75*J1184^2*AV1184^2-(UAC_V*0.98)^2","v":-50227.087636024466},{"$f":"-AS1184/2/AR1184+SQRT((AS1184/2/AR1184)^2-AT1184/AR1184)","v":1166.3697843933189},{"$f":"D1184+(F1184-D1184)*((0.85*UAC_V-D1184*J1184)/L1184*1000)/G1184","v":3.09850686266366},{"$f":"(L1184^2)/1000000+((K1184/1000)^2*AJ1184^2*PI()*PI()*(O1184/2)^2)/1200","v":3.2175342406227048E-2},{"$f":"SQRT(3)*L1184*J1184*AJ1184/1000","v":9.488954882844018},{"$f":"0.75*J1184^2*AJ1184^2-(UAC_V*0.98)^2","v":-49947.437618039847},{"$f":"IF(((AX1184/2/AW1184)^2-AY1184/AW1184)>0,-AX1184/2/AW1184+SQRT((AX1184/2/AW1184)^2-AY1184/AW1184),-9999)","v":1107.1724670325721}]
["KBM","KBMS-25H02-B (120 V)",8.75,5.18,8.0214091318315255,4.6636099603671664,750,29.7,1098,3.7,19,104,0.67800000000000005,160,10,1026.8212303512842,1098,1098,7.6833429690013535,3.6873156342182889,0.65501077338215907,0.52152265258486474,2.1857923497267762,15.489222781770483,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-12.54627045323409,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.26857121791674832,0.38206749528367184,3.2228546150009798,9.1696198868081247,5.8375613250370364,257.41294358181017,208.66977884796827,2007.4032725174548,3.3762794270852589E-2,11.718549173790825,-47631.056941139206,1026.8212303512842,1.2011136929172746E-2,2.6743710896230617,-50639.843322739194,1944.9951469729433,4.0126010096331273,1.3345464693462122E-2,3.8906946402348961,-50455.273147569518,1804.0915829210185]
["KBM","KBMS-25H02-B (240 V)",8.75,5.18,7.6956096012669404,4.4741916286435703,1700,29.7,2303,3.7,19,104,0.67800000000000005,325,10,1026.8212303512842,1910.3659300948009,2167.3076923076924,7.5651344148478179,3.6873156342182889,0.64274574329517697,0.52152265258486474,1.3303094048663215,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.26857121791674832,0.38206749528367184,3.2228546150009798,9.1696198868081247,5.8375613250370364,257.41294358181017,208.66977884796827,2007.4032725174548,3.3762794270852589E-2,11.718549173790825,-47631.056941139206,1026.8212303512842,1.2303154017878317E-2,2.9832579741942697,-50599.450214945602,1910.3659300948009,4.4760519606630957,1.3345464693462122E-2,3.8906946402348961,-50455.273147569518,1804.0915829210185]
["KBM","KBMS-25H02-B (400 V)",8.75,5.18,6.7906109052542005,3.9480295960780238,3150,29.7,3845,3.7,19,104,0.67800000000000005,565,10,1026.8212303512842,1907.2668117974642,2167.3076923076924,7.5636260978391938,3.6873156342182889,0.64280738285119499,0.52152265258486474,1.3303094048663215,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.26857121791674832,0.38206749528367184,3.2228546150009798,9.1696198868081247,5.8375613250370364,257.41294358181017,208.66977884796827,2007.4032725174548,3.3762794270852589E-2,11.718549173790825,-47631.056941139206,1026.8212303512842,1.2330407400556912E-2,3.0104692629413785,-50595.680405345905,1907.2668117974642,4.5168795201307148,1.3345464693462122E-2,3.8906946402348961,-50455.273147569518,1804.0915829210185]
["KBM","KBMS-25H02-B (480 V)",8.75,5.18,6.0876765732649973,3.5393468449215102,4000,29.7,4614,3.7,19,104,0.67800000000000005,679,10,1026.8212303512842,1909.7206798095008,2167.3076923076924,7.4789264739057177,3.6873156342182889,0.64430355281763074,0.52152265258486474,1.3303094048663215,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.26857121791674832,0.38206749528367184,3.2228546150009798,9.1696198868081247,5.8375613250370364,257.41294358181017,208.66977884796827,2007.4032725174548,3.3762794270852589E-2,11.718549173790825,-47631.056941139206,1026.8212303512842,1.230881309948121E-2,2.9889286948512406,-50598.667425506079,1909.7206798095008,4.484560256135552,1.3345464693462122E-2,3.8906946402348961,-50455.273147569518,1804.0915829210185]
["KBM","KBMS-25H02-C (120 V)",8.75,6.5,7.9912534584035866,5.7907633756547732,950,29.7,1380,2.35,12,83.4,0.67800000000000005,160,10,1345.9216352439469,1380,1380,7.6478208132599468,3.6873156342182889,0.64891942910525657,0.52152265258486474,1.7391304347826086,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.33701021553259919,0.4794283241976578,4.0441225863911905,11.506279780743787,7.3251252148148129,257.41294358181017,208.66977884796827,2007.4032725174548,2.1368232093066306E-2,7.4895598082909327,-48789.020892510205,1345.9216352439469,7.6626121263954254E-3,1.6588600818008201,-50706.252910887401,2466.4553170981203,4.8866948047126284,8.5442936927130411E-3,2.4866209777067376,-50582.917510294959,2291.9556281814612]
["KBM","KBMS-25H02-C (240 V)",8.75,6.5,7.4617759365874656,5.4070840120199026,2150,29.7,2895,2.35,12,83.4,0.67800000000000005,325,10,1345.9216352439469,2431.3962399760298,2702.6378896882493,7.2931706306847079,3.6873156342182889,0.64202504110657721,0.52152265258486474,1.0471406908973477,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.33701021553259919,0.4794283241976578,4.0441225863911905,11.506279780743787,7.3251252148148129,257.41294358181017,208.66977884796827,2007.4032725174548,2.1368232093066306E-2,7.4895598082909327,-48789.020892510205,1345.9216352439469,7.8194349541300737E-3,1.833620609427385,-50684.315505116887,2431.3962399760298,5.401506977113864,8.5442936927130411E-3,2.4866209777067376,-50582.917510294959,2291.9556281814612]
["KBM","KBMS-25H02-C (400 V)",8.75,6.5,6.0399300903374282,4.3767609350271224,4000,29.7,4826,2.35,12,83.4,0.67800000000000005,565,10,1345.9216352439469,2434.7558292964336,2702.6378896882493,7.1004103724120489,3.6873156342182889,0.64471483066558144,0.52152265258486474,1.0471406908973477,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.33701021553259919,0.4794283241976578,4.0441225863911905,11.506279780743787,7.3251252148148129,257.41294358181017,208.66977884796827,2007.4032725174548,2.1368232093066306E-2,7.4895598082909327,-48789.020892510205,1345.9216352439469,7.8039684783064826E-3,1.8171322664970337,-50686.479057202276,2434.7558292964336,5.3529353702495897,8.5442936927130411E-3,2.4866209777067376,-50582.917510294959,2291.9556281814612]
["KBM","KBMS-25H02-C (480 V)",8.75,6.5,4.8414933688554562,3.5083285281561278,5000,29.7,5791,2.35,12,83.4,0.67800000000000005,679,10,1345.9216352439469,2444.7860879886798,2702.6378896882493,6.838907472673263,3.6873156342182889,0.64832691470260562,0.52152265258486474,1.0471406908973477,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.33701021553259919,0.4794283241976578,4.0441225863911905,11.506279780743787,7.3251252148148129,257.41294358181017,208.66977884796827,2007.4032725174548,2.1368232093066306E-2,7.4895598082909327,-48789.020892510205,1345.9216352439469,7.7583444641780505E-3,1.7675980746597328,-50692.861243554049,2444.7860879886798,5.2070168081221535,8.5442936927130411E-3,2.4866209777067376,-50582.917510294959,2291.9556281814612]
["KBM","KBMS-25H02-D (120 V)",8.6199999999999992,8,7.7953441514397719,7.0228325688646587,1225,29.8,1717,1.57,7.8,67,0.67800000000000005,160,10,1703.7578404445048,1717,1717,7.4641354351200722,3.6873156342182889,0.65464177591158679,0.51977257656947928,1.3977868375072802,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.42103721376551762,0.59896453139097006,5.0524465651862114,14.37514875338328,9.1515039271289851,257.41294358181017,208.66977884796827,2007.4032725174548,1.4057540157768531E-2,5.0388806019076311,-49391.130276215139,1703.7578404445048,4.9130191420154309E-3,1.0607278148044978,-50742.498856254184,3107.6089221654997,5.8219554084447234,5.5366896515272167E-3,1.6673529908384346,-50650.333424144701,2877.7594584362723]
["KBM","KBMS-25H02-D (240 V)",8.6199999999999992,8,6.9736147541916713,6.2825358145870904,2725,29.8,3597,1.57,7.8,67,0.67800000000000005,325,10,1703.7578404445048,3078.2826401525831,3364.1791044776119,6.7601691298439919,3.6873156342182889,0.6521978209978897,0.51977257656947928,0.83398214293564377,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.42103721376551762,0.59896453139097006,5.0524465651862114,14.37514875338328,9.1515039271289851,257.41294358181017,208.66977884796827,2007.4032725174548,1.4057540157768531E-2,5.0388806019076311,-49391.130276215139,1703.7578404445048,4.982222443488428E-3,1.1440174290987903,-50732.272058471724,3078.2826401525831,6.2791022972507866,5.5366896515272167E-3,1.6673529908384346,-50650.333424144701,2877.7594584362723]
["KBM","KBMS-25H02-D (400 V)",8.6199999999999992,8,4.4612543893712751,4.0191480985326802,5180,29.8,5995,1.57,7.8,67,0.67800000000000005,565,10,1703.7578404445048,3102.5644320937645,3364.1791044776119,6.129116561068968,3.6873156342182889,0.65928341722659944,0.51977257656947928,0.83398214293564377,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.42103721376551762,0.59896453139097006,5.0524465651862114,14.37514875338328,9.1515039271289851,257.41294358181017,208.66977884796827,2007.4032725174548,1.4057540157768531E-2,5.0388806019076311,-49391.130276215139,1703.7578404445048,4.9247055037463716E-3,1.07524578484956,-50740.771856881453,3102.5644320937645,5.9016393509640075,5.5366896515272167E-3,1.6673529908384346,-50650.333424144701,2877.7594584362723]
["KBM","KBMS-25H02-D (480 V)",8.6199999999999992,8,2.8488734813449264,2.5665526858963297,6000,29.8,7193,1.57,7.8,67,0.67800000000000005,679,10,1703.7578404445048,3125.9967982662224,3364.1791044776119,5.6132461633824908,3.6873156342182889,0.66506639144218493,0.51977257656947928,0.83398214293564377,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.42103721376551762,0.59896453139097006,5.0524465651862114,14.37514875338328,9.1515039271289851,257.41294358181017,208.66977884796827,2007.4032725174548,1.4057540157768531E-2,5.0388806019076311,-49391.130276215139,1703.7578404445048,4.8711956404670813E-3,1.0070570873779454,-50748.679493359428,3125.9967982662224,5.5273759909399871,5.5366896515272167E-3,1.6673529908384346,-50650.333424144701,2877.7594584362723]
["KBM","KBMS-25H02-E (120 V)",8.85,10.199999999999999,7.8184865793893579,8.7848163813363573,1600,29.8,2143,0.96,5,54,0.67800000000000005,160,10,2143,2143,2143,7.4684167122696214,3.6873156342182889,0.63606571789600441,0.51977257656947928,1.1199253383107792,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.52287112970507577,0.74383273245790449,6.2744535564609087,17.851985578989709,11.364926995605773,257.41294358181023,208.66977884796827,2007.4032725174548,8.9797996966562328E-3,3.0838893371993312,-49989.798765081301,2193.9590100931805,3.1793946909175301E-3,0.64273192224882958,-50769.742962630517,3896.2444152571793,7.1582069507547725,3.5799445606509513E-3,1.0204512700395041,-50715.883525846606,3624.0374572885617]
["KBM","KBMS-25H02-E (240 V)",8.85,10.199999999999999,6.5120897548433847,7.3169547807229041,3600,29.8,4480,0.96,5,54,0.67800000000000005,325,10,2193.9590100931805,3879.3669635672777,4174.0740740740739,6.3306633975427644,3.6873156342182889,0.63622427413727101,0.51977257656947928,0.66224481073538244,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.52287112970507577,0.74383273245790449,6.2744535564609087,17.851985578989709,11.364926995605773,257.41294358181023,208.66977884796827,2007.4032725174548,8.9797996966562328E-3,3.0838893371993312,-49989.798765081301,2193.9590100931805,3.2009891996706264E-3,0.66856026721302897,-50766.839284045273,3879.3669635672777,7.4458613087370837,3.5799445606509513E-3,1.0204512700395041,-50715.883525846606,3624.0374572885617]
["KBM","KBMS-25H02-E (400 V)",8.85,10.199999999999999,2.9443664472000637,3.3082769069663636,6000,29.8,"",0.96,5,54,0.67800000000000005,565,10,2193.9590100931805,3947.2929641423702,4174.0740740740739,4.9647890380382833,3.6873156342182889,0.64766920261457184,0.51977257656947928,0.66224481073538244,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.52287112970507577,0.74383273245790449,6.2744535564609087,17.851985578989709,11.364926995605773,257.41294358181017,208.66977884796827,2007.4032725174548,8.9797996966562328E-3,3.0838893371993312,-49989.798765081301,2193.9590100931805,3.1167880741574056E-3,0.56117112841912087,-50778.161282975721,3947.2929641423702,6.2498515056756467,3.5799445606509513E-3,1.0204512700395041,-50715.883525846606,3624.0374572885617]
["KBM","KBMS-25H02-F (120 V)",8.93,12.74,7.639437268410977,10.669605123479018,2100,30.1,2666,0.61,3.2,43.3,0.67800000000000005,160,10,2666,2666,2666,7.2915998845636496,3.6873156342182889,0.62918414681310098,0.51459211899569712,0.90022505626406601,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.64722566588847452,0.92073860694175036,7.7667079906616943,22.09772656660201,14.067849656671227,257.41294358181017,208.66977884796827,2007.4032725174548,5.7575324103834452E-3,1.9645488096689794,-50290.536205327808,2789.7722807815071,2.0257842417751499E-3,0.38728926563488436,-50785.159763282645,4912.2558665801844,8.4655874671015408,2.2915807898985026E-3,0.64358524246156834,-50749.929831254864,4567.651402738562]
["KBM","KBMS-25H02-F (240 V)",8.93,12.74,5.6022539968347154,7.8243770905512786,4500,30.1,5564,0.61,3.2,43.3,0.67800000000000005,325,10,2789.7722807815071,4936.6631312290956,5205.5427251732108,5.2793419991286576,3.6873156342182889,0.63331379287180811,0.51459211899569712,0.52543414292979229,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.64722566588847452,0.92073860694175036,7.7667079906616943,22.09772656660201,14.067849656671227,257.41294358181017,208.66977884796827,2007.4032725174548,5.7575324103834452E-3,1.9645488096689794,-50290.536205327808,2789.7722807815071,2.0097789259148173E-3,0.36617380645813402,-50787.2811835713,4936.6631312290956,8.0040338367013835,2.2915807898985026E-3,0.64358524246156834,-50749.929831254864,4567.651402738562]
["KBM","KBMS-25H02-G (120 V)",8.74,14.37,7.341021750113673,11.615540743850747,2400,30,3027,0.49,2.5,38.200000000000003,0.67800000000000005,160,10,3027,3027,3027,6.9755386823308703,3.6873156342182889,0.64222611106454774,0.51630742605901614,0.79286422200198214,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.74590427698521722,1.0611180938884526,8.9508513238226062,25.466834253322862,16.212690225273324,257.41294358181017,208.66977884796827,2007.4032725174548,4.5858355526250377E-3,1.5991406403466366,-50367.046532097491,3144.3145775381881,1.5566861906332354E-3,0.28231453653690303,-50791.505375411165,5622.1311825367593,8.7078947358545484,1.7970314827532392E-3,0.52562396145171664,-50757.827047769359,5170.4017431302718]
["KBM","KBMS-25H02-G (240 V)",8.74,14.37,4.3692536263907114,6.9133759911245436,5300,30,6316,0.49,2.5,38.200000000000003,0.67800000000000005,325,10,3144.3145775381881,5683.4234107970797,5900.5235602094235,4.0530561769004771,3.6873156342182889,0.65060503598247132,0.51630742605901614,0.46418056453520162,15.489222781770483,0,-12.54627045323409,0,0,0,0,0,0.74590427698521722,1.0611180938884526,8.9508513238226062,25.466834253322862,16.212690225273324,257.41294358181017,208.66977884796827,2007.4032725174548,4.5858355526250377E-3,1.5991406403466366,-50367.046532097491,3144.3145775381881,1.5301658502634352E-3,0.24085356728883048,-50795.221531880343,5683.4234107970797,7.429045405998929,1.7970314827532392E-3,0.52562396145171664,-50757.827047769359,5170.4017431302718]
["KBM","KBMS-25H03-A (120 V)",11.86,5.3,11.285532328334398,4.9281800560412217,550,42.2,827,3.97,21,139,0.93099999999999994,160,10,791.78158730213499,827,827,10.996209519150085,2.6852846401718584,0.51608939684045341,0.39626343555855364,2.9020556227327692,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.21887480271891155,0.3113697301750496,2.6264976326269385,7.4728735242011899,4.7573790419086865,277.90554104128091,225.28194185883552,2167.2122806819975,5.1569116979886337E-2,18.024763117748442,-46601.287459099629,791.78158730213499,2.1117847012875276E-2,4.2547391222380551,-50570.92257701073,1450.0195048170485,4.4515064015290449,2.1373261072544988E-2,4.547091456944008,-50537.62673673965,1435.0029893557867]
["KBM","KBMS-25H03-A (240 V)",11.86,5.3,11.018419137131216,4.8115367411053347,1300,42.2,1735,3.97,21,139,0.93099999999999994,325,10,791.78158730213499,1431.4818089158748,1621.5827338129495,10.933301772362778,2.6852846401718584,0.50808899364076587,0.39626343555855364,1.6724703835477219,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.21887480271891155,0.3113697301750496,2.6264976326269385,7.4728735242011899,4.7573790419086865,277.90554104128091,225.28194185883552,2167.2122806819975,5.1569116979886337E-2,18.024763117748442,-46601.287459099629,791.78158730213499,2.1434999510670783E-2,4.6149800382654345,-50529.578498607887,1431.4818089158748,4.8284072402683762,2.1373261072544988E-2,4.547091456944008,-50537.62673673965,1435.0029893557867]
["KBM","KBMS-25H03-A (400 V)",11.86,5.3,9.9869726790164322,4.3611234406185293,2400,42.2,2899,3.97,21,139,0.93099999999999994,565,10,791.78158730213499,1432.4448031198535,1621.5827338129495,10.742079894981494,2.6852846401718584,0.51074183715775656,0.39626343555855364,1.6724703835477219,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.21887480271891155,0.3113697301750496,2.6264976326269385,7.4728735242011899,4.7573790419086865,277.90554104128091,225.28194185883552,2167.2122806819975,5.1569116979886337E-2,18.024763117748442,-46601.287459099629,791.78158730213499,2.1418045276212057E-2,4.5964367597112137,-50531.788656823868,1432.4448031198535,4.8090063978623139,2.1373261072544988E-2,4.547091456944008,-50537.62673673965,1435.0029893557867]
["KBM","KBMS-25H03-A (480 V)",11.86,5.3,9.3846535409358971,4.09810198294144,2900,42.2,3479,3.97,21,139,0.93099999999999994,679,10,791.78158730213499,1433.8914909344182,1621.5827338129495,10.636076474218394,2.6852846401718584,0.5122118906612142,0.39626343555855364,1.6724703835477219,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.21887480271891155,0.3113697301750496,2.6264976326269385,7.4728735242011899,4.7573790419086865,277.90554104128091,225.28194185883552,2167.2122806819975,5.1569116979886337E-2,18.024763117748442,-46601.287459099629,791.78158730213499,2.1392673773830726E-2,4.568546711172667,-50535.096092177344,1433.8914909344182,4.7798265290051614,2.1373261072544988E-2,4.547091456944008,-50537.62673673965,1435.0029893557867]
["KBM","KBMS-25H03-B (120 V)",11.84,7.27,10.742958658702936,6.4716618425921304,800,42.3,1144,2.1,11.4,100,0.93099999999999994,160,10,1144,1144,1144,10.271230881945197,2.6852846401718584,0.52379691818005158,0.39532664256668953,2.0979020979020979,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.30073729944847233,0.42782673299813806,3.6088475933816682,10.267841591955314,6.536710976976976,277.90554104128097,225.28194185883552,2167.2122806819975,2.8026622426156465E-2,9.4471975711842582,-48573.921451275259,1158.6907443358164,1.0799958326423387E-2,1.9901210727103322,-50706.145452898862,2076.6245511472016,5.4714139859488435,1.1141791423469589E-2,2.3776022605686369,-50663.835187263474,2028.3841739937272]
["KBM","KBMS-25H03-B (240 V)",11.84,7.27,10.02022080068974,6.0362775907769519,1825,42.3,2399,2.1,11.4,100,0.93099999999999994,325,10,1158.6907443358164,2050.7214018415239,2254,9.7951451229306414,2.6852846401718584,0.51602685968703599,0.39532664256668953,1.1832078117995719,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.30073729944847233,0.42782673299813806,3.6088475933816682,10.267841591955314,6.536710976976976,277.90554104128091,225.28194185883552,2167.2122806819975,2.8026622426156465E-2,9.4471975711842582,-48573.921451275259,1158.6907443358164,1.0978608625712438E-2,2.2011535345842632,-50684.033077929686,2050.7214018415239,6.0516027891424784,1.1141791423469589E-2,2.3776022605686369,-50663.835187263474,2028.3841739937272]
["KBM","KBMS-25H03-B (400 V)",11.84,7.27,5.2661562052465376,3.1723832561726133,3400,42.3,4000,2.1,11.4,100,0.93099999999999994,565,10,1158.6907443358164,2092.7768978472609,2254,7.7936504636127593,2.6852846401718584,0.53592158677497503,0.39532664256668953,1.1832078117995719,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.30073729944847233,0.42782673299813806,3.6088475933816682,10.267841591955314,6.536710976976976,277.90554104128091,225.28194185883552,2167.2122806819975,2.8026622426156465E-2,9.4471975711842582,-48573.921451275259,1158.6907443358164,1.0694456332482996E-2,1.8542500012063008,-50719.203923325666,2092.7768978472609,5.0978654159110555,1.1141791423469589E-2,2.3776022605686369,-50663.835187263474,2028.3841739937272]
["KBM","KBMS-25H03-B (480 V)",11.84,7.27,6.6499920800324466,4.006019325320751,4150,42.3,4800,2.1,11.4,100,0.93099999999999994,679,10,1158.6907443358164,2059.7175745004361,2254,9.2641083073364765,2.6852846401718584,0.5212650086194236,0.39532664256668953,1.1832078117995719,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.30073729944847233,0.42782673299813806,3.6088475933816682,10.267841591955314,6.536710976976976,277.90554104128091,225.28194185883552,2167.2122806819975,2.8026622426156465E-2,9.4471975711842582,-48573.921451275259,1158.6907443358164,1.0915262901799987E-2,2.1287210097461227,-50691.873671566638,2059.7175745004361,5.8524649905073129,1.1141791423469589E-2,2.3776022605686369,-50663.835187263474,2028.3841739937272]
["KBM","KBMS-25H03-C (120 V)",11.9,8.1999999999999993,10.769484482551585,7.2278419345983789,900,42.4,1276,1.66,9.1,90,0.93099999999999994,160,10,1276,1276,1276,10.297180221928691,2.6852846401718584,0.5186199707374255,0.39439426840969261,1.8808777429467085,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.3374982133188455,0.48012254636093105,4.0499785598261457,11.522941112662345,7.3357321481481463,277.90554104128091,225.28194185883552,2167.2122806819975,2.26347239484481E-2,7.5603860555854405,-49040.979836126833,1314.381917230548,8.7164526676229773E-3,1.5570065754286657,-50730.336868026912,2324.8199472118049,6.0169890592620989,9.0162800344891717E-3,1.8982556022215604,-50693.944742859094,2268.246350888388]
["KBM","KBMS-25H03-C (240 V)",11.9,8.1999999999999993,9.8753701274580923,6.6277651862134848,2050,42.4,2676,1.66,9.1,90,0.93099999999999994,325,10,1314.381917230548,2298.1989790974385,2504.4444444444448,9.6302427774995181,2.6852846401718584,0.51313017104396041,0.39439426840969261,1.058086128545962,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.3374982133188455,0.48012254636093105,4.0499785598261457,11.522941112662345,7.3357321481481463,277.90554104128091,225.28194185883552,2167.2122806819975,2.26347239484481E-2,7.5603860555854405,-49040.979836126833,1314.381917230548,8.8529873249236519E-3,1.7208159047477467,-50713.764710554547,2298.1989790974385,6.65002359994579,9.0162800344891717E-3,1.8982556022215604,-50693.944742859094,2268.246350888388]
["KBM","KBMS-25H03-C (400 V)",11.9,8.1999999999999993,7.4635291734146705,5.0090799821574974,3800,42.4,4459,1.66,9.1,90,0.93099999999999994,565,10,1314.381917230548,2304.4770429283676,2504.4444444444448,9.2095407443454391,2.6852846401718584,0.51679478709657012,0.39439426840969261,1.058086128545962,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.3374982133188455,0.48012254636093105,4.0499785598261457,11.522941112662345,7.3357321481481463,277.90554104128091,225.28194185883552,2167.2122806819975,2.26347239484481E-2,7.5603860555854405,-49040.979836126833,1314.381917230548,8.8200497905037527E-3,1.6827586927252216,-50717.762567347461,2304.4770429283676,6.5029530403352709,9.0162800344891717E-3,1.8982556022215604,-50693.944742859094,2268.246350888388]
["KBM","KBMS-25H03-C (480 V)",11.9,8.1999999999999993,5.2243241637149138,3.5062578279965866,4725,42.4,5351,1.66,9.1,90,0.93099999999999994,679,10,1314.381917230548,2317.5506761641268,2504.4444444444448,8.6256683495798896,2.6852846401718584,0.52187873567307919,0.39439426840969261,1.058086128545962,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.3374982133188455,0.48012254636093105,4.0499785598261457,11.522941112662345,7.3357321481481463,277.90554104128091,225.28194185883552,2167.2122806819975,2.26347239484481E-2,7.5603860555854405,-49040.979836126833,1314.381917230548,8.7529172608524358E-3,1.6023952669788157,-50725.910907665559,2317.5506761641268,6.1923918255582429,9.0162800344891717E-3,1.8982556022215604,-50693.944742859094,2268.246350888388]
["KBM","KBMS-25H03-D (120 V)",11.9,10.24,10.663381187156988,8.9608245270226785,1200,42.6,1595,1.06,5.7,72.099999999999994,0.93099999999999994,160,10,1595,1595,1595,10.256327494596164,2.6852846401718584,0.51399930897995416,0.39254265212607897,1.5047021943573669,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.42146118346158273,0.59956766765072367,5.057534201538993,14.389624023617369,9.1607191703703688,277.90554104128091,225.28194185883552,2167.2122806819975,1.4175455120792279E-2,4.8524866773580868,-49672.764375475497,1708.5850188516158,5.5751965705338191E-3,0.99413497992413591,-50757.63083443261,2929.4744884367778,7.5100633065975337,5.7590284143574349E-3,1.21263842883007,-50734.441647702115,2864.6735322935224]
["KBM","KBMS-25H03-D (240 V)",11.9,10.24,9.1956189341983965,7.7274108690742835,2700,42.6,3338,1.06,5.7,72.099999999999994,0.93099999999999994,325,10,1708.5850188516158,2916.3415100805651,3126.2135922330099,8.9789263847136525,2.6852846401718584,0.51341350505058214,0.39254265212607897,0.83779180173403767,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.42146118346158273,0.59956766765072367,5.057534201538993,14.389624023617369,9.1607191703703688,277.90554104128091,225.28194185883552,2167.2122806819975,1.4175455120792279E-2,4.8524866773580868,-49672.764375475497,1708.5850188516158,5.6107913887345736E-3,1.0400331353022236,-50753.140780540278,2916.3415100805651,7.8567949471759517,5.7590284143574349E-3,1.21263842883007,-50734.441647702115,2864.6735322935224]
["KBM","KBMS-25H03-D (400 V)",11.9,10.199999999999999,5.0010749128257421,4.2025839603577664,4850,42.6,5560,1.06,5.7,72.099999999999994,0.93099999999999994,565,10,1713.2094133886899,2947.1065760160368,3126.2135922330099,7.7078623728137599,2.6852846401718584,0.52208005724709028,0.39254265212607897,0.83736434431820506,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.41981485071368585,0.59722560644896305,5.0377782085642302,14.333414554775112,9.1249351111111086,277.90554104128097,225.28194185883552,2167.2122806819975,1.4105458934623991E-2,4.833531651274658,-49681.593937306126,1713.2094133886899,5.5287942898455747E-3,0.93090924127814811,-50763.484179148189,2947.1065760160368,7.0324326936258483,5.7546571373533967E-3,1.2079015599674523,-50734.993055753024,2866.135889693413]
["KBM","KBMS-25H03-E (120 V)",11.8,12.7,10.269407475568853,10.80990260586195,1525,42.6,2006,0.69,3.6,57.4,0.93099999999999994,160,10,2006,2006,2006,9.7866435383548325,2.6852846401718584,0.5179800291799852,0.39254265212607897,1.1964107676969093,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.5271403987068739,0.74990616402984189,6.3256847844824868,17.997747936716205,11.457722194601377,277.90554104128091,225.28194185883552,2167.2122806819975,8.8965411141455411E-3,3.1452337211898,-50054.536649520043,2201.7908468163914,3.4949718923644015E-3,0.59461353539980621,-50778.332153929223,3727.5703621189446,8.6678857932351985,3.6445924452570581E-3,0.78599520855222305,-50758.283408998912,3625.6184205070695]
["KBM","KBMS-25H03-E (240 V)",11.8,12.7,8.0747728480446916,8.4997608926786228,3400,42.6,4193,0.69,3.6,57.4,0.93099999999999994,325,10,2201.7908468163914,3727.124053205117,3926.8292682926831,7.7163577289101699,2.6852846401718584,0.51988320108218555,0.39254265212607897,0.66195603663783853,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.5271403987068739,0.74990616402984189,6.3256847844824868,17.997747936716205,11.457722194601377,277.90554104128091,225.28194185883552,2167.2122806819975,8.8965411141455411E-3,3.1452337211898,-50054.536649520043,2201.7908468163914,3.495580071916359E-3,0.59551597325013028,-50778.250659532408,3727.124053205117,8.6810409398243902,3.6445924452570581E-3,0.78599520855222305,-50758.283408998912,3625.6184205070695]
["KBM","KBMS-25H03-F (120 V)",11.75,14.79,9.936430230872384,12.20691674554347,1850,42,2347,0.51,2.7,49.4,0.93099999999999994,160,10,2347,2347,2347,9.4492171631662085,2.6852846401718584,0.51978729045724925,0.3981504042993087,1.0225820195994888,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.61650257438848088,0.87703215653420064,7.3980308926617706,21.048771756820816,13.400064284444442,277.90554104128091,225.28194185883552,2167.2122806819975,6.6296963679867288E-3,2.3069455819869047,-50259.953768311963,2584.8736149074102,2.5750000181385267E-3,0.41357265407110899,-50787.637755311167,4361.5189499111866,9.4775058806629673,2.7095133564259727E-3,0.58474246501374882,-50770.131996919481,4222.1493431658582]
["KBM","KBMS-25H03-F (240 V)",11.75,14.79,6.7427350280639562,8.2834582654348363,4100,42,4902,0.51,2.7,49.4,0.93099999999999994,325,10,2584.8736149074102,4384.3016697625744,4562.7530364372469,6.395521907950525,2.6852846401718584,0.52483801782989736,0.3981504042993087,0.56843086421960354,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.61650257438848088,0.87703215653420064,7.3980308926617706,21.048771756820816,13.400064284444442,277.90554104128091,225.28194185883552,2167.2122806819975,6.6296963679867288E-3,2.3069455819869047,-50259.953768311963,2584.8736149074102,2.5551736962221463E-3,0.38191048656308346,-50790.217981225433,4384.3016697625744,8.7519299128180208,2.7095133564259727E-3,0.58474246501374882,-50770.131996919481,4222.1493431658582]
["KBM","KBMS-25H03-G (120 V)",11.2,20,8.5422798546777301,14.856138877700401,2750,42,3324,0.28000000000000003,1.3,34.6,0.93099999999999994,160,10,3324,3324,3324,7.9875411770722824,2.6852846401718584,0.54604514362000578,0.3981504042993087,0.72202166064981954,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.87461427232017908,1.2442200134353398,10.495371267842149,29.861280322448156,19.010281481481481,277.90554104128091,225.28194185883552,2167.2122806819975,3.1518043091219939E-3,1.2585081167795462,-50474.41,3807.1340214223151,1.2300844970407074E-3,0.16333592857155038,-50799.588767758214,6360.2749079463929,9.733901974517142,1.3227405288014961E-3,0.31899458062277797,-50783.910220842103,6076.7966699716017]
["KBM","KBMS-25H03-G (240 V)",11.2,20,3.5388569699256727,6.1545338607403011,5100,42,6937,0.28000000000000003,1.3,34.6,0.93099999999999994,325,10,3807.1340214223151,6454.5227315317043,6514.4508670520236,1.5041133652685446,2.6852846401718584,0.55860005039231109,0.3981504042993087,0.39494492416696508,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.87461427232017908,1.2442200134353398,10.495371267842149,29.861280322448156,19.010281481481481,277.90554104128091,225.28194185883552,2167.2122806819975,3.1518043091219939E-3,1.2585081167795462,-50474.41,3807.1340214223151,1.20619827488676E-3,8.5578550053849192E-2,-50803.630612067456,6454.5227315317043,5.0999998875358887,1.3227405288014961E-3,0.31899458062277797,-50783.910220842103,6076.7966699716017]
["KBM","KBMS-25H03-H (120 V)",11,21.1,7.9793274858614645,15.198719020688504,2950,42.6,3642,0.25,1.1000000000000001,31.8,0.93099999999999994,160,10,3642,3642,3642,7.2707493910194758,2.6852846401718584,0.55775462823025579,0.39254265212607897,0.65897858319604607,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.93949474924865772,1.3365185162501796,11.273936990983893,32.076444390004312,20.420498725925924,277.90554104128091,225.28194185883552,2167.2122806819975,2.6725191589977554E-3,1.1251932683351202,-50492.163112241738,4141.2019506846173,1.0319950899700691E-3,0.12576741280193604,-50801.249592450142,6955.472674499948,9.1335659920101335,1.1149872437077582E-3,0.28118626340813385,-50785.613276489901,6624.0213213090192]
["KBM","KBMS-25H03-H (240 V)",11,21.1,3.0300652627110845,5.7715528813544461,5200,42.6,7600,0.25,1.1000000000000001,31.8,0.93099999999999994,325,10,4141.2019506846173,7054.0622647121563,7088.0503144654094,0.18838156105224435,2.6852846401718584,0.57018456445041599,0.39254265212607897,0.36231767435279316,16.722316980570966,0,-13.545076754262482,0,0,0,0,0,0.93949474924865772,1.3365185162501796,11.273936990983893,32.076444390004312,20.420498725925924,277.90554104128091,225.28194185883552,2167.2122806819975,2.6725191589977554E-3,1.1251932683351202,-50492.163112241738,4141.2019506846173,1.0142299173182736E-3,4.7734832855473287E-2,-50804.596678170434,7054.0622647121563,3.4666312702929929,1.1149872437077582E-3,0.28118626340813385,-50785.613276489901,6624.0213213090192]
["KBM","KBMS-25H04-A (120 V)",14.82,5.5,13.687325105903,4.9772091294192728,450,54.4,685,4.08,23,167,1.18,160,10,647.57675380541991,685,685,13.095817105652344,2.1186440677966103,0.46070072840242149,0.32970433123007548,3.5036496350364965,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.19496029509827315,0.27734912253722044,2.3395235411792776,6.6563789408932905,4.2375824461438496,298.07414486502881,241.63146197625014,2324.4946642115265,7.222341182475106E-2,23.825973101413155,-45716.44227769674,647.57675380541991,2.9896520441232553E-2,5.070025686498421,-50574.736172848134,1218.6062843318057,4.2960853218536172,2.9842217028326842E-2,5.0009835096418014,-50580.969135647487,1220.8043863148637]
["KBM","KBMS-25H04-A (240 V)",14.82,5.5,13.187123856185615,4.7953177658856783,1050,54.4,1437,4.08,23,167,1.18,325,10,647.57675380541991,1199.2007043675303,1349.7005988023952,12.955098836374145,2.1186440677966103,0.44652604666810763,0.32970433123007548,1.9659169207645721,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.19496029509827315,0.27734912253722044,2.3395235411792776,6.6563789408932905,4.2375824461438496,298.07414486502881,241.63146197625014,2324.4946642115265,7.222341182475106E-2,23.825973101413155,-45716.44227769674,647.57675380541991,3.0399812633529828E-2,5.6700556863265401,-50516.96813684568,1199.2007043675303,4.8045206305342205,2.9842217028326842E-2,5.0009835096418014,-50580.969135647487,1220.8043863148637]
["KBM","KBMS-25H04-A (400 V)",14.82,5.5,12.032113697747288,4.3753140719081047,2000,54.4,2400,4.08,23,167,1.18,565,10,647.57675380541991,1194.8306415356294,1349.7005988023952,13.1544740104755,2.1186440677966103,0.44423588954330123,0.32970433123007548,1.9659169207645721,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.19496029509827315,0.27734912253722044,2.3395235411792776,6.6563789408932905,4.2375824461438496,298.07414486502881,241.63146197625014,2324.4946642115265,7.222341182475106E-2,23.825973101413155,-45716.44227769674,647.57675380541991,3.051901935684034E-2,5.8030945155752462,-50503.285551680776,1194.8306415356294,4.9172510577377739,2.9842217028326842E-2,5.0009835096418014,-50580.969135647487,1220.8043863148637]
["KBM","KBMS-25H04-A (480 V)",14.82,5.5,11.399472798957003,4.1452628359843651,2400,54.4,2888,4.08,23,167,1.18,679,10,647.57675380541991,1194.9164591233737,1349.7005988023952,13.116981561914383,2.1186440677966103,0.44467845744495393,0.32970433123007548,1.9659169207645721,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.19496029509827315,0.27734912253722044,2.3395235411792776,6.6563789408932905,4.2375824461438496,298.07414486502881,241.63146197625014,2324.4946642115265,7.222341182475106E-2,23.825973101413155,-45716.44227769674,647.57675380541991,3.0516657774918007E-2,5.8004885345820281,-50503.556614796005,1194.9164591233737,4.9150428802281789,2.9842217028326842E-2,5.0009835096418014,-50580.969135647487,1220.8043863148637]
["KBM","KBMS-25H04-B (120 V)",14.9,6.2,13.641852265019601,5.5681029653141225,525,53.8,772,3.2,18,148,1.18,160,10,770.32950541441437,772,772,13.049923711609775,2.1186440677966103,0.4562180142938223,0.33338133120661906,3.1088082901554404,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.21859343202940487,0.31096945424295258,2.6231211843528586,7.4632669018308624,4.7512632761620681,298.07414486502881,241.63146197625014,2324.4946642115265,5.5291116436579142E-2,18.363692750852262,-46956.260125003384,770.32950541441437,2.3420710303521747E-2,3.9140095457257518,-50630.312132897736,1389.1114050823323,4.7714410152777189,2.3407909526895029E-2,3.8974577612109798,-50631.787819114965,1389.8245478800727]
["KBM","KBMS-25H04-B (240 V)",14.9,6.2,13.130282805081366,5.359299104114843,1200,53.8,1618,3.2,18,148,1.18,325,10,770.32950541441437,1367.6352468903926,1522.9729729729731,12.883060322667735,2.1186440677966103,0.44287814323037189,0.33338133120661906,1.7268366742124164,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.21859343202940487,0.31096945424295258,2.6231211843528586,7.4632669018308624,4.7512632761620681,298.07414486502881,241.63146197625014,2324.4946642115265,5.5291116436579142E-2,18.363692750852262,-46956.260125003384,770.32950541441437,2.382402370824881E-2,4.4037621827829589,-50583.817763850107,1367.6352468903926,5.3684824359730481,2.3407909526895029E-2,3.8974577612109798,-50631.787819114965,1389.8245478800727]
["KBM","KBMS-25H04-B (400 V)",14.9,6.2,11.735024470642415,4.7898059063846592,2250,53.8,2704,3.2,18,148,1.18,565,10,770.32950541441437,1364.4261758448074,1522.9729729729731,12.980722018593882,2.1186440677966103,0.44192329463664959,0.33338133120661906,1.7268366742124164,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.21859343202940487,0.31096945424295258,2.6231211843528586,7.4632669018308624,4.7512632761620681,298.07414486502881,241.63146197625014,2324.4946642115265,5.5291116436579142E-2,18.363692750852262,-46956.260125003384,770.32950541441437,2.3887216267693523E-2,4.4756446729645498,-50576.53286296298,1364.4261758448074,5.4561120285751628,2.3407909526895029E-2,3.8974577612109798,-50631.787819114965,1389.8245478800727]
["KBM","KBMS-25H04-B (480 V)",14.9,6.2,10.92863942564348,4.4606691533238694,2700,53.8,3245,3.2,18,148,1.18,679,10,770.32950541441437,1365.1855923931507,1522.9729729729731,12.891983615440848,2.1186440677966103,0.44282349563732137,0.33338133120661906,1.7268366742124164,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.21859343202940487,0.31096945424295258,2.6231211843528586,7.4632669018308624,4.7512632761620681,298.07414486502881,241.63146197625014,2324.4946642115265,5.5291116436579142E-2,18.363692750852262,-46956.260125003384,770.32950541441437,2.3872193799884693E-2,4.458661392572469,-50578.264667941745,1365.1855923931507,5.4354082669491266,2.3407909526895029E-2,3.8974577612109798,-50631.787819114965,1389.8245478800727]
["KBM","KBMS-25H04-C (120 V)",15.1,8.6300000000000008,13.687325105903,7.646550338493296,750,54.4,1060,1.66,9.6,108,1.18,160,10,1060,1060,1060,13.103419483009572,2.1186440677966103,0.44239945654381801,0.32970433123007548,2.2641509433962264,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.30023791544931733,0.42711631288975166,3.6028549853918079,10.250791509354039,6.5258565572725047,298.07414486502881,241.63146197625014,2324.4946642115265,2.9981511393068736E-2,9.6543984552800897,-48807.401736683074,1125.0110631954858,1.2447544081822864E-2,1.9967500371695546,-50719.704523513879,1939.9688334331927,6.4302999300771857,1.2471004620044121E-2,2.0264224787319751,-50717.145852573944,1937.02270147278]
["KBM","KBMS-25H04-C (240 V)",15.1,8.6300000000000008,12.638774892591691,7.0607680964199391,1700,54.4,2223,1.66,9.6,108,1.18,325,10,1125.0110631954858,1919.5700264649813,2087.037037037037,12.320885914962327,2.1186440677966103,0.43637318397406211,0.32970433123007548,1.2390149058011575,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.30023791544931733,0.42711631288975166,3.6028549853918079,10.250791509354039,6.5258565572725047,298.07414486502881,241.63146197625014,2324.4946642115265,2.9981511393068736E-2,9.6543984552800897,-48807.401736683074,1125.0110631954858,1.2614280177802318E-2,2.1989624786961777,-50701.519825473391,1919.5700264649813,7.0815014447407698,1.2471004620044121E-2,2.0264224787319751,-50717.145852573944,1937.02270147278]
["KBM","KBMS-25H04-C (400 V)",15.1,8.6300000000000008,10.064655448858906,5.6227125412619587,3150,54.4,3707,1.66,9.6,108,1.18,565,10,1125.0110631954858,1921.258846956657,2087.037037037037,12.02882531226831,2.1186440677966103,0.43843906412416467,0.32970433123007548,1.2390149058011575,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.30023791544931733,0.42711631288975166,3.6028549853918079,10.250791509354039,6.5258565572725047,298.07414486502881,241.63146197625014,2324.4946642115265,2.9981511393068736E-2,9.6543984552800897,-48807.401736683074,1125.0110631954858,1.2600098815107329E-2,2.1824928600596185,-50703.066483963237,1921.258846956657,7.0284629644124124,1.2471004620044121E-2,2.0264224787319751,-50717.145852573944,1937.02270147278]
["KBM","KBMS-25H04-C (480 V)",15.1,8.6300000000000008,8.0858978879934362,4.517261389940467,3850,54.4,4450,1.66,9.6,108,1.18,679,10,1125.0110631954858,1927.2849865605897,2087.037037037037,11.588786053331642,2.1186440677966103,0.44153583973223082,0.32970433123007548,1.2390149058011575,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.30023791544931733,0.42711631288975166,3.6028549853918079,10.250791509354039,6.5258565572725047,298.07414486502881,241.63146197625014,2324.4946642115265,2.9981511393068736E-2,9.6543984552800897,-48807.401736683074,1125.0110631954858,1.2550046596966877E-2,2.1233435379431831,-50708.52531678402,1927.2849865605897,6.8379794913741039,1.2471004620044121E-2,2.0264224787319751,-50717.145852573944,1937.02270147278]
["KBM","KBMS-25H04-D (120 V)",15,10.7,13.369015219719209,9.284038347027229,1000,54.8,1325,1.08,6.2,87,1.18,160,10,1325,1325,1325,12.838945166127953,2.1186440677966103,0.44196350503481313,0.32729773027219172,1.8113207547169812,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.37473495557470987,0.53309526978445088,4.4968194668965182,12.794286474826821,8.1450957432098754,298.07414486502881,241.63146197625014,2324.4946642115265,1.9646805771190295E-2,6.361751671399408,-49468.395423155205,1433.1197625691348,8.0383818158506898E-3,1.2541394302947932,-50753.209091339013,2435.9405210396212,7.7062339046618007,8.0933656983677958E-3,1.325561339230344,-50747.123506934135,2423.4861411112861]
["KBM","KBMS-25H04-D (240 V)",15,10.7,11.777465788800255,8.1787956866668434,2250,54.8,2776,1.08,6.2,87,1.18,325,10,1433.1197625691348,2418.1238912614599,2590.8045977011493,11.536672459329107,2.1186440677966103,0.43920005283385372,0.32729773027219172,0.99030894350379217,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.37473495557470987,0.53309526978445088,4.4968194668965182,12.794286474826821,8.1450957432098754,298.07414486502881,241.63146197625014,2324.4946642115265,1.9646805771190295E-2,6.361751671399408,-49468.395423155205,1433.1197625691348,8.1175559032050041E-3,1.3557922231803186,-50744.446149014526,2418.1238912614599,8.3308536081136442,8.0933656983677958E-3,1.325561339230344,-50747.123506934135,2423.4861411112861]
["KBM","KBMS-25H04-D (400 V)",15,10.7,6.9376214952587638,4.8177927050408087,4150,54.8,4626,1.08,6.2,87,1.18,565,10,1433.1197625691348,2436.0257092389556,2590.8045977011493,10.267431008393933,2.1186440677966103,0.44636903881910261,0.32729773027219172,0.99030894350379217,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.37473495557470987,0.53309526978445088,4.4968194668965182,12.794286474826821,8.1450957432098754,298.07414486502881,241.63146197625014,2324.4946642115265,1.9646805771190295E-2,6.361751671399408,-49468.395423155205,1433.1197625691348,8.0380115943754077E-3,1.2536447360760499,-50753.250067238369,2436.0257092389556,7.7031941873314675,8.0933656983677958E-3,1.325561339230344,-50747.123506934135,2423.4861411112861]
["KBM","KBMS-25H04-D (480 V)",15,10.7,4.0432128096111288,2.8077866733410617,4700,54.8,5551,1.08,6.2,87,1.18,679,10,1433.1197625691348,2451.2819590031968,2590.8045977011493,9.2854947301196678,2.1186440677966103,0.45198336473363437,0.32729773027219172,0.99030894350379217,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.37473495557470987,0.53309526978445088,4.4968194668965182,12.794286474826821,8.1450957432098754,298.07414486502881,241.63146197625014,2324.4946642115265,1.9646805771190295E-2,6.361751671399408,-49468.395423155205,1433.1197625691348,7.9730315337716625E-3,1.1635641261365453,-50760.442022868549,2451.2819590031968,7.1496813691392713,8.0933656983677958E-3,1.325561339230344,-50747.123506934135,2423.4861411112861]
["KBM","KBMS-25H04-E (120 V)",14.6,13.8,12.584608714480584,11.65241547637091,1400,53.8,1837,0.65,3.5,65.5,1.18,160,10,1837,1837,1837,11.955518720357738,2.1186440677966103,0.45189782511699178,0.33338133120661906,1.3064779531845401,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.49654420563285728,0.70638023841621667,5.9585304675942874,16.953125721989199,10.792695038051752,298.07414486502881,241.63146197625014,2324.4946642115265,1.0803707883045573E-2,3.7499354350619143,-49985.742963281104,1984.4227703684824,4.5143070710715301E-3,0.69550028593055269,-50776.972793675814,3277.6570230599114,9.4315273588600412,4.583646148240271E-3,0.79587559886307913,-50768.249681902824,3242.3707588781335]
["KBM","KBMS-25H04-E (240 V)",14.6,13.8,9.9719703688069501,9.233305897043472,3050,53.8,3681,0.65,3.5,65.5,1.18,325,10,1984.4227703684824,3275.0328010383901,3441.2213740458014,9.6305085749721826,2.1186440677966103,0.45303906686573292,0.33338133120661906,0.74019912541723165,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.49654420563285728,0.70638023841621667,5.9585304675942874,16.953125721989199,10.792695038051752,298.07414486502881,241.63146197625014,2324.4946642115265,1.0803707883045573E-2,3.7499354350619143,-49985.742963281104,1984.4227703684824,4.5193019473945221E-3,0.70320990590349208,-50776.344419802997,3275.0328010383901,9.5360758301865545,4.583646148240271E-3,0.79587559886307913,-50768.249681902824,3242.3707588781335]
["KBM","KBMS-25H04-E (400 V)",14.6,13.8,4.5670548887239537,4.2287545265962532,4600,53.8,6135,0.65,3.5,65.5,1.18,565,10,1984.4227703684824,3314.9203571141989,3441.2213740458014,7.3699100019177513,2.1186440677966103,0.46301131801215667,0.33338133120661906,0.74019912541723165,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.49654420563285728,0.70638023841621667,5.9585304675942874,16.953125721989199,10.792695038051752,298.07414486502881,241.63146197625014,2324.4946642115265,1.0803707883045573E-2,3.7499354350619143,-49985.742963281104,1984.4227703684824,4.4464392321527909E-3,0.58068890814814378,-50785.510818247989,3314.9203571141989,7.8745953595950837,4.583646148240271E-3,0.79587559886307913,-50768.249681902824,3242.3707588781335]
["KBM","KBMS-25H04-F (120 V)",14.5,19.399999999999999,11.793381283109445,15.316079588453825,2000,54.1,2495,0.33,1.8,46.3,1.18,160,10,2495,2495,2495,11.123493150679034,2.1186440677966103,0.45388419771668526,0.33153263620917017,0.96192384769539074,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.70285447677886292,0.99987575576716214,8.4342537213463551,23.997018138411892,15.276976224776501,298.07414486502881,241.63146197625014,2324.4946642115265,5.6340120734180987E-3,1.9155193835389135,-50377.251287836247,2825.0880469878553,2.2251854052974408E-3,0.29269840855893781,-50795.168774779362,4712.4847143967081,11.060246414875177,2.2991713574745227E-3,0.40428996433306646,-50786.098198239903,4612.7813287216004]
["KBM","KBMS-25H04-F (240 V)",14.5,19.399999999999999,4.8481044203377346,6.2962395069321229,4550,54.1,5206,0.33,1.8,46.3,1.18,325,10,2825.0880469878553,4778.4046915046265,4868.2505399568036,4.3635905231272663,2.1186440677966103,0.4655074324153608,0.33153263620917017,0.52029346916064256,17.935915618916106,0,-14.528091651322041,0,0,0,0,0,0.70285447677886292,0.99987575576716214,8.4342537213463551,23.997018138411892,15.276976224776501,298.07414486502881,241.63146197625014,2324.4946642115265,5.6340120734180987E-3,1.9155193835389135,-50377.251287836247,2825.0880469878553,2.1825528031785891E-3,0.20212538525957535,-50800.395473486569,4778.4046915046265,7.6377476006068896,2.2991713574745227E-3,0.40428996433306646,-50786.098198239903,4612.7813287216004]
["KBM","KBMS-25H04-G (120 V)",14,20.3,11.77006323330761,16.577553849729028,2150,54.5,2701,0.3,1.5,42.8,1.18,160,10,{"$f":"IF(AQ1248<I1248,IF(AQ1248<0,0,AQ1248),I1248)","v":2701},{"$f":"IF(AU1248<I1248,IF(AU1248<0,0,AU1248),I1248)","v":2701},{"$f":"IF(UAC_V*0.98/L1248*1000<I1248,IF(UAC_V*0.98/L1248*1000<0,0,UAC_V*0.98/L1248*1000),I1248)","v":2701},{"$f":"C1248+(E1248-C1248)/G1248*Q1248","v":11.198577113099468},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M1248,(inertia/gear^2+gear_inertia)/M1248),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M1248,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M1248))","v":2.1186440677966103},{"$f":"IF((C1248+(E1248-C1248)/G1248*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X1248^2*time1+Y1248^2*time2+Z1248^2*time3+AA1248^2*time4)/time)/(C1248+(E1248-C1248)/G1248*mspeed),SQRT((((X1248-Y1248)*2/PI()+Y1248)^2*time1+Y1248^2*time2+((Z1248-Y1248)*2/PI()+Y1248)^2*time3+AA1248^2*time4)/time)/(C1248+(E1248-C1248)/G1248*mspeed)),IF(AccType=1,SQRT((X1248^2*time1+Y1248^2*time2+Z1248^2*time3+AA1248^2*time4+AB1248^2*time5+AC1248^2*time6+AD1248^2*time7+AE1248^2*time8)/time)/(C1248+(E1248-C1248)/G1248*mspeed),SQRT((((X1248-Y1248)*2/PI()+Y1248)^2*time1+Y1248^2*time2+((Z1248-Y1248)*2/PI()+Y1248)^2*time3+AA1248^2*time4+((AB1248-AC1248)*2/PI()+AC1248)^2*time5+AC1248^2*time6+((AD1248-AC1248)*2/PI()+AC1248)^2*time7+AE1248^2*time8)/time)/(C1248+(E1248-C1248)/G1248*mspeed))))","v":0.46586718350877876},{"$f":"IF(move1,MAX(ABS(X1248),ABS(Z1248))/H1248,MAX(ABS(X1248),ABS(Z1248),ABS(AB1248),ABS(AD1248))/H1248)","v":0.32909936915442395},{"$f":"IF(AZ1248>0,speed/(MIN(AZ1248,I1248)),\"NA\")","v":0.88855979266938168},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M1248+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M1248+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":17.935915618916106},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M1248+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M1248+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-14.528091651322041},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M1248+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M1248+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M1248+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M1248+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH1248/Irms","v":0.76172759661214406},{"$f":"AI1248/Ipeak","v":1.0836282353095148},{"$f":"IF(move1,IF(AccType=1,SQRT((X1248^2*time1+Y1248^2*time2+Z1248^2*time3+AA1248^2*time4)/time)/(C1248/D1248),SQRT((((X1248-Y1248)*2/PI()+Y1248)^2*time1+Y1248^2*time2+((Z1248-AA1248)*2/PI()+AA1248)^2*time3+AA1248^2*time4)/time)/(C1248/D1248)),IF(AccType=1,SQRT((X1248^2*time1+Y1248^2*time2+Z1248^2*time3+AA1248^2*time4+AB1248^2*time5+AC1248^2*time6+AD1248^2*time7+AE1248^2*time8)/time)/(C1248/D1248),SQRT((((X1248-Y1248)*2/PI()+Y1248)^2*time1+Y1248^2*time2+((Z1248-AA1248)*2/PI()+AA1248)^2*time3+AA1248^2*time4+((AB1248-AC1248)*2/PI()+AC1248)^2*time5+AC1248^2*time6+((AD1248-AE1248)*2/PI()+AE1248)^2*time7+AE1248^2*time8)/time)/(C1248/D1248)))","v":9.1407311593457283},{"$f":"IF(move1,MAX(ABS(X1248),ABS(Z1248))/(C1248/D1248),MAX(ABS(X1248),ABS(Z1248),ABS(AB1248),ABS(AD1248))/(C1248/D1248))","v":26.007077647428357},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X1248),ABS(Z1248))/(C1248/D1248),MAX(ABS((X1248-Y1248)*2/PI()+Y1248),ABS((Z1248-Y1248)*2/PI()+Y1248))/(C1248/D1248)),IF(AccType=1,MAX(ABS(X1248),ABS(Z1248),ABS(AB1248),ABS(AD1248))/(C1248/D1248),MAX(ABS((X1248-Y1248)*2/PI()+Y1248),ABS((Z1248-Y1248)*2/PI()+Y1248),ABS((AB1248-AC1248)*2/PI()+AC1248),ABS((AD1248-AC1248)*2/PI()+AC1248))/(C1248/D1248)))","v":16.556619851851853},{"$f":"IF((C1248+(E1248-C1248)/G1248*mspeed)<0,\"NA\",U1248*(C1248+(E1248-C1248)/G1248*mspeed)*mspeed/9.55)","v":298.07414486502881},{"$f":"IF(move1,IF(speed1>speed2,AM1248/2*time1/time,AM1248/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z1248*-speed/30*PI(),((Z1248-AA1248)*2/PI()+AA1248)*-speed/30*PI()),IF(AccType=1,X1248*-speed/30*PI(),((X1248-Y1248)*2/PI()+Y1248)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z1248*-speed/30*PI(),((Z1248-AA1248)*2/PI()+AA1248)*-speed/30*PI()),IF(AccType=1,X1248*-speed/30*PI(),((X1248-Y1248)*2/PI()+Y1248)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD1248*-speed/30*PI(),((AD1248-AE1248)*2/PI()+AE1248)*-speed/30*PI()),IF(AccType=1,AB1248*-speed/30*PI(),((AB1248-AC1248)*2/PI()+AC1248)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD1248*-speed/30*PI(),((AD1248-AE1248)*2/PI()+AE1248)*-speed/30*PI()),IF(AccType=1,AB1248*-speed/30*PI(),((AB1248-AC1248)*2/PI()+AC1248)*-speed/30*PI()),0)/2*time7/time)))","v":241.63146197625014},{"$f":"IF(move1,MAX(IF(AccType=1,Z1248*-speed/30*PI(),((Z1248-AA1248)*2/PI()+AA1248)*-speed/30*PI()),IF(AccType=1,X1248*-speed/30*PI(),((X1248-Y1248)*2/PI()+Y1248)*-speed/30*PI()),0),MAX(IF(AccType=1,Z1248*-speed/30*PI(),((Z1248-AA1248)*2/PI()+AA1248)*-speed/30*PI()),IF(AccType=1,X1248*-speed/30*PI(),((X1248-Y1248)*2/PI()+Y1248)*-speed/30*PI()),IF(AccType=1,AD1248*-speed/30*PI(),((AD1248-AE1248)*2/PI()+AE1248)*-speed/30*PI()),IF(AccType=1,AB1248*-speed/30*PI(),((AB1248-AC1248)*2/PI()+AC1248)*-speed/30*PI()),0))","v":2324.4946642115265},{"$f":"(L1248^2)/1000000+((K1248/1000)^2*(D1248/C1248*H1248)^2*PI()*PI()*(O1248/2)^2)/1200","v":4.7209896331133934E-3},{"$f":"SQRT(3)*L1248*J1248*D1248/C1248*H1248/1000","v":1.7574790454747957},{"$f":"0.75*J1248^2*(D1248/C1248*H1248)^2-(UAC_V*0.98)^2","v":-50383.625832812504},{"$f":"-AO1248/2/AN1248+SQRT((AO1248/2/AN1248)^2-AP1248/AN1248)","v":3086.0062051339046},{"$f":"(L1248^2)/1000000+((K1248/1000)^2*AV1248^2*PI()*PI()*(O1248/2)^2)/1200","v":1.9057306180701196E-3},{"$f":"SQRT(3)*L1248*J1248*AV1248/1000","v":0.28106048262791328},{"$f":"0.75*J1248^2*AV1248^2-(UAC_V*0.98)^2","v":-50794.37917376859},{"$f":"-AS1248/2/AR1248+SQRT((AS1248/2/AR1248)^2-AT1248/AR1248)","v":5089.4879119619345},{"$f":"D1248+(F1248-D1248)*((0.85*UAC_V-D1248*J1248)/L1248*1000)/G1248","v":12.637877360108403},{"$f":"(L1248^2)/1000000+((K1248/1000)^2*AJ1248^2*PI()*PI()*(O1248/2)^2)/1200","v":1.958659016454881E-3},{"$f":"SQRT(3)*L1248*J1248*AJ1248/1000","v":0.36821148311954},{"$f":"0.75*J1248^2*AJ1248^2-(UAC_V*0.98)^2","v":-50786.656787887987},{"$f":"IF(((AX1248/2/AW1248)^2-AY1248/AW1248)>0,-AX1248/2/AW1248+SQRT((AX1248/2/AW1248)^2-AY1248/AW1248),-9999)","v":4998.953726347574}]
["KBM","KBMS-25H04-G (240 V)",14,20.3,4.8473059841683774,6.8271915269977148,4600,54.5,5637,0.3,1.5,42.8,1.18,325,10,3086.0062051339046,5186.9532161828001,5266.3551401869163,3.6794357256184984,2.1186440677966103,0.48116172609479169,0.32909936915442395,0.48010046329305223,17.935915618916106,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-14.528091651322041,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.76172759661214406,1.0836282353095148,9.1407311593457283,26.007077647428357,16.556619851851853,298.07414486502881,241.63146197625014,2324.4946642115265,4.7209896331133934E-3,1.7574790454747957,-50383.625832812504,3086.0062051339046,1.8567538516687829E-3,0.16320203706215161,-50801.525006646159,5186.9532161828001,7.3383753917545587,1.958659016454881E-3,0.36821148311954,-50786.656787887987,4998.953726347574]
["KBM","KBMS-35H01-A (120 V)",12.6,5.41,11.650141834326739,4.9156716600534764,500,40.799999999999997,798,4.13,32,144,2.17,160,10,642.90657620786806,798,798,11.084026367585476,1.1520737327188941,0.68129279770585305,0.5578692850885697,3.007518796992481,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.2862381191863419,0.40720030277456948,3.4348574302361028,9.7728072665896679,6.2215623374485602,378.26256970643601,306.63557810573053,2949.8342613771279,8.5350833684642746E-2,18.045131622824574,-46879.297064946673,642.90657620786806,2.4487653409443935E-2,4.348157769761964,-50577.217340003604,1351.112976328604,4.221162999144191,2.8885995679565471E-2,6.4087396348162864,-50309.983209552651,1213.4473707649579]
["KBM","KBMS-35H01-A (240 V)",12.6,5.41,11.459155902616464,4.8350868787411239,1200,40.799999999999997,1675,4.13,32,144,2.17,325,10,642.90657620786806,1309.3803900508406,1565.2777777777778,11.355167592317288,1.1520737327188941,0.6573041884713321,0.5578692850885697,1.9778360873508991,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.2862381191863419,0.40720030277456948,3.4348574302361028,9.7728072665896679,6.2215623374485602,378.26256970643601,306.63557810573053,2949.8342613771279,8.5350833684642746E-2,18.045131622824574,-46879.297064946673,642.90657620786806,2.565587207203163E-2,4.9793292463145047,-50506.238803250351,1309.3803900508406,4.8339001223154696,2.8885995679565471E-2,6.4087396348162864,-50309.983209552651,1213.4473707649579]
["KBM","KBMS-35H01-A (400 V)",12.6,5.41,10.926171907145932,4.6101991169392118,2150,40.799999999999997,2795,4.13,32,144,2.17,565,10,642.90657620786806,1300.5127929625137,1565.2777777777778,11.587518675359645,1.1520737327188941,0.65313185043733313,0.5578692850885697,1.9778360873508991,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.2862381191863419,0.40720030277456948,3.4348574302361028,9.7728072665896679,6.2215623374485602,378.26256970643595,306.63557810573053,2949.8342613771279,8.5350833684642746E-2,18.045131622824574,-46879.297064946673,642.90657620786806,2.5921500309439922E-2,5.1119814714994858,-50490.099783890895,1300.5127929625137,4.9626780311114604,2.8885995679565471E-2,6.4087396348162864,-50309.983209552651,1213.4473707649579]
["KBM","KBMS-35H01-A (480 V)",12.6,5.41,10.504226244065093,4.4321629721793636,2700,40.799999999999997,3353,4.13,32,144,2.17,679,10,642.90657620786806,1299.6969975432003,1565.2777777777778,11.591158941437616,1.1520737327188941,0.65307618041714066,0.5578692850885697,1.9778360873508991,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.2862381191863419,0.40720030277456948,3.4348574302361028,9.7728072665896679,6.2215623374485602,378.26256970643601,306.63557810573053,2949.8342613771279,8.5350833684642746E-2,18.045131622824574,-46879.297064946673,642.90657620786806,2.5946253418542519E-2,5.1241680281994304,-50488.595836453256,1299.6969975432003,4.9745086603003354,2.8885995679565471E-2,6.4087396348162864,-50309.983209552651,1213.4473707649579]
["KBM","KBMS-35H01-B (120 V)",12.45,6.1,11.632779476898532,5.5394187985231103,550,41.4,901,3.3,25,127,2.17,160,10,729.33195535190441,901,901,11.111244197610141,1.1520737327188941,0.67915952600071772,0.54978422298583685,2.6637069922308547,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.32663388252696163,0.46466702701754764,3.9196065903235393,11.152008648421143,7.0995892071991671,378.26256970643601,306.63557810573053,2949.8342613771279,6.9005192470452642E-2,14.724451059951607,-47444.606664131228,729.33195535190441,1.8958825621982006E-2,3.4063468108231816,-50625.310062068245,1546.7302512791196,4.692567998525381,2.2606463379919794E-2,5.15360950799161,-50393.483966754582,1383.3975086024589]
["KBM","KBMS-35H01-B (240 V)",12.45,6.1,11.275515583664278,5.3692931350782276,1300,41.4,1892,3.3,25,127,2.17,325,10,729.33195535190441,1504.6012149846356,1774.8031496062993,11.090668707846733,1.1520737327188941,0.66432709585586469,0.54978422298583685,1.7348592758595736,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.32663388252696163,0.46466702701754764,3.9196065903235393,11.152008648421143,7.0995892071991671,378.26256970643601,306.63557810573053,2949.8342613771279,6.9005192470452642E-2,14.724451059951607,-47444.606664131228,729.33195535190441,1.9771406974349939E-2,3.864588524526952,-50573.666347822167,1504.6012149846356,5.3238397159216762,2.2606463379919794E-2,5.15360950799161,-50393.483966754582,1383.3975086024589]
["KBM","KBMS-35H01-B (400 V)",12.45,6.1,10.646449810232319,5.0697380048725327,2350,41.4,3153,3.3,25,127,2.17,565,10,729.33195535190441,1493.0469623910094,1774.8031496062993,11.304133986233037,1.1520737327188941,0.66095680598625217,0.54978422298583685,1.7348592758595736,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.32663388252696163,0.46466702701754764,3.9196065903235393,11.152008648421143,7.0995892071991671,378.26256970643601,306.63557810573053,2949.8342613771279,6.9005192470452642E-2,14.724451059951607,-47444.606664131228,729.33195535190441,2.0008833753408655E-2,3.9885549897093417,-50558.576657791324,1493.0469623910094,5.4946153590701829,2.2606463379919794E-2,5.15360950799161,-50393.483966754582,1383.3975086024589]
["KBM","KBMS-35H01-B (480 V)",12.45,6.1,10.207868763825012,4.8608898875357198,2900,41.4,3783,3.3,25,127,2.17,679,10,729.33195535190441,1492.0046699373825,1774.8031496062993,11.296458525867049,1.1520737327188941,0.66109691313478081,0.54978422298583685,1.7348592758595736,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.32663388252696163,0.46466702701754764,3.9196065903235393,11.152008648421143,7.0995892071991671,378.26256970643601,306.63557810573053,2949.8342613771279,6.9005192470452642E-2,14.724451059951607,-47444.606664131228,729.33195535190441,2.0030568767837341E-2,3.9997114248096541,-50557.195286103408,1492.0046699373825,5.5099844137310319,2.2606463379919794E-2,5.15360950799161,-50393.483966754582,1383.3975086024589]
["KBM","KBMS-35H01-C (120 V)",12.45,8.32,11.482589759268032,7.5049606269725704,815,40.799999999999997,1242,1.75,13.4,93,2.17,160,10,1064.657569359247,1242,1242,10.975738013510302,1.1520737327188941,0.67146678723544628,0.5578692850885697,1.932367149758454,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.44550719715152803,0.63377535488295023,5.3460863658183362,15.210608517190806,9.6833741317864046,378.26256970643601,306.63557810573053,2949.8342613771279,3.6096094692917982E-2,7.6859182800421619,-49097.640639163888,1064.657569359247,1.0149151408258327E-2,1.7968636339072683,-50711.833635135321,2148.549746971165,6.3743146097290966,1.2110955876194911E-2,2.7296586215509739,-50589.78723464541,1934.2287521350488]
["KBM","KBMS-35H01-C (240 V)",12.45,8.32,10.976501238239955,7.1741838158431079,1840,40.799999999999997,2600,1.75,13.4,93,2.17,325,10,1064.657569359247,2102.4200657333849,2423.6559139784949,10.766351432849122,1.1520737327188941,0.66178012515010853,0.5578692850885697,1.2408046345866908,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.44550719715152803,0.63377535488295023,5.3460863658183362,15.210608517190806,9.6833741317864046,378.26256970643601,306.63557810573053,2949.8342613771279,3.6096094692917982E-2,7.6859182800421619,-49097.640639163888,1064.657569359247,1.0514586540449376E-2,2.0038041519024214,-50689.0994415776,2102.4200657333849,7.1084292872759001,1.2110955876194911E-2,2.7296586215509739,-50589.78723464541,1934.2287521350488]
["KBM","KBMS-35H01-C (400 V)",12.45,8.32,9.6876921882023268,6.3318249596093636,3450,40.799999999999997,4334,1.75,13.4,93,2.17,565,10,1064.657569359247,2096.6526258989184,2423.6559139784949,10.771275383435743,1.1520737327188941,0.66177652550732557,0.5578692850885697,1.2408046345866908,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.44550719715152803,0.63377535488295023,5.3460863658183362,15.210608517190806,9.6833741317864046,378.26256970643601,306.63557810573053,2949.8342613771279,3.6096094692917982E-2,7.6859182800421619,-49097.640639163888,1064.657569359247,1.0562317539477289E-2,2.0292759043949853,-50686.130034219044,2096.6526258989184,7.1987894910136152,1.2110955876194911E-2,2.7296586215509739,-50589.78723464541,1934.2287521350488]
["KBM","KBMS-35H01-C (480 V)",12.45,8.32,8.8330993416001924,5.7732675435295375,4200,40.799999999999997,5201,1.75,13.4,93,2.17,679,10,1064.657569359247,2100.3902442735571,2423.6559139784949,10.641213605378676,1.1520737327188941,0.66327544487775658,0.5578692850885697,1.2408046345866908,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.44550719715152803,0.63377535488295023,5.3460863658183362,15.210608517190806,9.6833741317864046,378.26256970643601,306.63557810573053,2949.8342613771279,3.6096094692917982E-2,7.6859182800421619,-49097.640639163888,1064.657569359247,1.0531332612503719E-2,2.0127774378345764,-50688.057646714769,2100.3902442735571,7.1402617238254855,1.2110955876194911E-2,2.7296586215509739,-50589.78723464541,1934.2287521350488]
["KBM","KBMS-35H01-D (120 V)",12.65,10.57,11.589373583328015,9.4222549457951352,1100,41.2,1556,1.08,8.5,74,2.17,160,10,1368.7836357187323,1556,1556,11.149695723325811,1.1520737327188941,0.65494164503543517,0.55245307843722435,1.5424164524421593,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.55703849830829133,0.79243898685822201,6.6844619796994964,19.018535684597328,12.107575858293076,378.26256970643601,306.63557810573053,2949.8342613771279,2.3081960173350388E-2,4.7653826622573376,-49768.414569131543,1368.7836357187323,6.4206963381568559E-3,1.1038601080308463,-50749.530565280234,2726.7677111963117,7.9743985300212525,7.6537637120925274E-3,1.6759972485211925,-50676.920099659852,2466.0045597258718]
["KBM","KBMS-35H01-D (240 V)",12.65,10.57,10.757574928986886,8.745995877225111,2450,41.2,3252,1.08,8.5,74,2.17,325,10,1368.7836357187323,2681.7497044948741,3045.9459459459463,10.578567193890567,1.1520737327188941,0.65033070188204167,0.55245307843722435,0.97323421018604728,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.55703849830829133,0.79243898685822201,6.6844619796994964,19.018535684597328,12.107575858293076,378.26256970643595,306.63557810573053,2949.8342613771279,2.3081960173350388E-2,4.7653826622573376,-49768.414569131543,1368.7836357187323,6.6050895365156806E-3,1.2067911433499059,-50738.672378393552,2681.7497044948741,8.7179828762352916,7.6537637120925274E-3,1.6759972485211925,-50676.920099659852,2466.0045597258718]
["KBM","KBMS-35H01-D (400 V)",12.65,10.57,8.4999233343583658,6.9105067759011103,4550,41.2,5420,1.08,8.5,74,2.17,565,10,1368.7836357187323,2690.8588159161659,3045.9459459459463,10.195654860995658,1.1520737327188941,0.65368257780233086,0.55245307843722435,0.97323421018604728,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.55703849830829133,0.79243898685822201,6.6844619796994964,19.018535684597328,12.107575858293076,378.26256970643601,306.63557810573053,2949.8342613771279,2.3081960173350388E-2,4.7653826622573376,-49768.414569131543,1368.7836357187323,6.5668902386959577E-3,1.1862014503575886,-50740.921784111102,2690.8588159161659,8.5692408242877658,7.6537637120925274E-3,1.6759972485211925,-50676.920099659852,2466.0045597258718]
["KBM","KBMS-35H01-D (480 V)",12.65,10.57,6.1741141716683536,5.0196050176165476,5800,41.2,6505,1.08,8.5,74,2.17,679,10,1368.7836357187323,2713.888617210092,3045.9459459459463,9.6198564076101043,1.1520737327188941,0.65865071605277969,0.55245307843722435,0.97323421018604728,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.55703849830829133,0.79243898685822201,6.6844619796994964,19.018535684597328,12.107575858293076,378.26256970643601,306.63557810573053,2949.8342613771279,2.3081960173350388E-2,4.7653826622573376,-49768.414569131543,1368.7836357187323,6.4723308767007061E-3,1.133625790119414,-50746.490011321046,2713.888617210092,8.189428867439263,7.6537637120925274E-3,1.6759972485211925,-50676.920099659852,2466.0045597258718]
["KBM","KBMS-35H01-E (120 V)",12.2,12.8,10.777063289365486,11.226107593089049,1400,41.1,1996,0.74,5.4,57.8,2.17,160,10,1751.4152842767196,1996,1996,10.171298803981079,1.1520737327188941,0.6813579515238255,0.55379724651128082,1.2024048096192386,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.69944068153045702,0.9950193150432195,8.3932881783654842,23.880463561037267,15.202775276259867,378.26256970643601,306.63557810573053,2949.8342613771279,1.4489686842120434E-2,3.1945680687306601,-50041.484910370331,1751.4152842767196,3.8463128250565879E-3,0.68021480126270328,-50770.53605992379,3545.8036570541672,9.1817590623723362,4.7266119919327698E-3,1.126271414108611,-50710.237218735543,3158.4887006193317]
["KBM","KBMS-35H01-E (240 V)",12.2,12.8,9.5955028593145926,9.9953154784527012,3100,41.1,4166,0.74,5.4,57.8,2.17,325,10,1751.4152842767196,3503.3431085163479,3899.6539792387548,9.2566299648481429,1.1520737327188941,0.67677112326318489,0.55379724651128082,0.75985707959930215,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.69944068153045702,0.9950193150432195,8.3932881783654842,23.880463561037267,15.202775276259867,378.26256970643601,306.63557810573053,2949.8342613771279,1.4489686842120434E-2,3.1945680687306601,-50041.484910370331,1751.4152842767196,3.9270778831505997E-3,0.7325446677066384,-50765.003804987267,3503.3431085163479,9.8881244995289599,4.7266119919327698E-3,1.126271414108611,-50710.237218735543,3158.4887006193317]
["KBM","KBMS-35H01-E (400 V)",12.2,12.8,5.1268764455012183,5.3404962973971024,6100,41.1,6943,0.74,5.4,57.8,2.17,565,10,1751.4152842767196,3564.4534952770891,3899.6539792387548,8.0669147579737874,1.1520737327188941,0.68512982745416928,0.55379724651128082,0.75985707959930215,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.69944068153045702,0.9950193150432195,8.3932881783654842,23.880463561037267,15.202775276259867,378.26256970643601,306.63557810573053,2949.8342613771279,1.4489686842120434E-2,3.1945680687306601,-50041.484910370331,1751.4152842767196,3.8119553889336979E-3,0.65669062608945772,-50772.889479831887,3564.4534952770891,8.8642221487667712,4.7266119919327698E-3,1.126271414108611,-50710.237218735543,3158.4887006193317]
["KBM","KBMS-35H01-F (120 V)",12.4,14.58,11.071215728829969,12.725535320494217,1600,41.1,2288,0.56999999999999995,4.4000000000000004,52.6,2.17,160,10,1939.3158402428969,2288,2288,10.499838492226855,1.1520737327188941,0.66526928229163773,0.55379724651128082,1.048951048951049,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.78385654402666038,1.1151087177584909,9.4062785283199251,26.762609226203782,17.037606193548385,378.26256970643601,306.63557810573053,2949.8342613771279,1.2063253765421899E-2,2.5095675373278952,-50236.08920741138,1939.3158402428969,3.2019065029300934E-3,0.54294650955302259,-50778.523165558654,3898.4334871490255,10.455283618371201,3.922289434185774E-3,0.8847688070050812,-50734.426014955294,3485.4931443556698]
["KBM","KBMS-35H01-F (240 V)",12.4,14.58,9.4962449378164226,10.915224066455659,3600,41.1,4576,0.56999999999999995,4.4000000000000004,52.6,2.17,325,10,1939.3158402428969,3869.1590579566814,4285.1711026615967,9.2791416108513456,1.1520737327188941,0.66467295814628102,0.55379724651128082,0.68856827444532687,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.78385654402666038,1.1151087177584909,9.4062785283199251,26.762609226203782,17.037606193548385,378.26256970643601,306.63557810573053,2949.8342613771279,1.2063253765421899E-2,2.5095675373278952,-50236.08920741138,1939.3158402428969,3.2446914765307758E-3,0.5690129018324831,-50775.904148168636,3869.1590579566814,10.957232741156501,3.922289434185774E-3,0.8847688070050812,-50734.426014955294,3485.4931443556698]
["KBM","KBMS-35H01-F (400 V)",12.4,14.58,3.7039695846841094,4.2574363042346084,6600,41.1,7200,0.56999999999999995,4.4000000000000004,52.6,2.17,565,10,1939.3158402428969,3978.8902353419853,4285.1711026615967,7.1574923476155599,1.1520737327188941,0.67766450537929057,0.55379724651128082,0.68856827444532687,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,0.78385654402666038,1.1151087177584909,9.4062785283199251,26.762609226203782,17.037606193548385,378.26256970643601,306.63557810573053,2949.8342613771279,1.2063253765421899E-2,2.5095675373278952,-50236.08920741138,1939.3158402428969,3.0902076350016123E-3,0.46810285150314573,-50785.36064266639,3978.8902353419853,9.0140520086642866,3.922289434185774E-3,0.8847688070050812,-50734.426014955294,3485.4931443556698]
["KBM","KBMS-35H01-G (120 V)",12.4,20.100000000000001,10.605814505613111,16.834626199385891,2350,41.2,3026,0.3,2.2000000000000002,38.1,2.17,160,10,2818.0965506758484,3026,3026,10.089699869780969,1.1520737327188941,0.66359951355198243,0.55245307843722435,0.79312623925974879,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,1.0806252767445732,1.5372897960868086,12.967503320934878,36.894955106083408,23.488057921146954,378.26256970643601,306.63557810573053,2949.8342613771279,5.8902206027177956E-3,1.3221430488509529,-50504.104234053077,2818.0965506758484,1.6247473910050228E-3,0.26112614503318543,-50793.416683334392,5511.4926221505912,13.18996064106377,2.0006425439528974E-3,0.46500108576295385,-50767.921001618772,4922.5680094699719]
["KBM","KBMS-35H01-G (240 V)",12.4,20.100000000000001,7.1259373576805212,11.31101167885797,5300,41.2,6316,0.3,2.2000000000000002,38.1,2.17,325,10,2818.0965506758484,5576.3696291190081,5916.010498687664,6.8509202376034928,1.1520737327188941,0.66940730322096786,0.55245307843722435,0.48755039958471097,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,1.0806252767445732,1.5372897960868086,12.967503320934878,36.894955106083408,23.488057921146954,378.26256970643601,306.63557810573053,2949.8342613771279,5.8902206027177956E-3,1.3221430488509529,-50504.104234053077,2818.0965506758484,1.591434986475159E-3,0.23466445749725309,-50795.676149721265,5576.3696291190081,11.853332257679492,2.0006425439528974E-3,0.46500108576295385,-50767.921001618772,4922.5680094699719]
["KBM","KBMS-35H01-H (120 V)",12.2,21.2,10.313240312354818,17.450491222258577,2500,41.4,3237,0.27,1.6,35.700000000000003,2.17,160,10,3237,3237,3237,9.7570235564370194,1.1520737327188941,0.67456897781922398,0.54978422298583685,0.74142724745134381,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,1.1584486287848192,1.6480007405403321,13.901383545417831,39.552017772967972,25.179596551305405,378.26256970643601,306.63557810573053,2949.8342613771279,3.9987667004109289E-3,1.2010718241405245,-50522.189257439401,3407.4870636700498,1.3665855085690654E-3,0.22083230025345613,-50795.594035411181,6016.4353255486894,13.227262993785367,1.6082205834481442E-3,0.42037935047418862,-50770.495389390053,5489.4846471679048]
["KBM","KBMS-35H01-H (240 V)",12.2,21.2,6.3605136185653901,10.762290386743469,5600,41.4,6756,0.27,1.6,35.700000000000003,2.17,325,10,3407.4870636700498,6083.4893184976308,6313.7254901960778,5.856347673755387,1.1520737327188941,0.68204999439515801,0.54978422298583685,0.43719951038358229,22.761066831613643,0,-18.43646413360705,0,0,0,0,0,1.1584486287848192,1.6480007405403321,13.901383545417831,39.552017772967972,25.179596551305405,378.26256970643595,306.63557810573053,2949.8342613771279,3.9987667004109289E-3,1.2010718241405245,-50522.189257439401,3407.4870636700498,1.3416070315707949E-3,0.18852100277410336,-50798.18855093274,6083.4893184976308,11.291902863318471,1.6082205834481442E-3,0.42037935047418862,-50770.495389390053,5489.4846471679048]
["KBM","KBMS-35H02-A (120 V)",17.3,4.97,16.160348067792452,4.5522107233218172,325,58.8,531,5.5,44,215,2.94,160,10,429.44455895517831,531,531,15.43798407383936,0.85034013605442182,0.59293450155075933,0.45091772481747083,4.5197740112994351,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.22309665272945042,0.31737570382889785,2.677159832753405,7.6170168918935488,4.8491435598372927,440.63134458308593,357.19433509532632,3436.2095036170394,0.15981473447468164,34.597872067302063,-44331.321430041098,429.44455895517831,5.2481713701107664E-2,8.1199431311193813,-50448.570078677054,906.12615018174461,3.964525456707169,5.5585390008131189E-2,9.9317737697707358,-50271.68174032501,865.85092765203444]
["KBM","KBMS-35H02-A (240 V)",17.3,4.97,15.875705573416559,4.4720297389905799,800,58.8,1114,5.5,44,215,2.94,325,10,429.44455895517831,882.63962569647083,1048.372093023256,15.728576625548527,0.85034013605442182,0.56491594206096851,0.45091772481747083,2.7718397282407312,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.22309665272945042,0.31737570382889785,2.677159832753405,7.6170168918935488,4.8491435598372927,440.63134458308593,357.19433509532632,3436.2095036170394,0.15981473447468164,34.597872067302063,-44331.321430041098,429.44455895517831,5.4225682878188894E-2,9.1821286772070749,-50349.175754219643,882.63962569647083,4.4831327387055282,5.5585390008131189E-2,9.9317737697707358,-50271.68174032501,865.85092765203444]
["KBM","KBMS-35H02-A (400 V)",17.3,4.97,15.311803145737517,4.3131839847147937,1450,58.8,1863,5.5,44,215,2.94,565,10,429.44455895517831,876.57411929158366,1048.372093023256,16.098067650687288,0.85034013605442182,0.55865825188527984,0.45091772481747083,2.7718397282407312,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.22309665272945042,0.31737570382889785,2.677159832753405,7.6170168918935488,4.8491435598372927,440.63134458308593,357.19433509532632,3436.2095036170394,0.15981473447468164,34.597872067302063,-44331.321430041098,429.44455895517831,5.4705837521984449E-2,9.4536434319105158,-50321.810220996733,876.57411929158366,4.6156985879376524,5.5585390008131189E-2,9.9317737697707358,-50271.68174032501,865.85092765203444]
["KBM","KBMS-35H02-A (480 V)",17.3,4.97,15.006037491521562,4.2270528145131161,1750,58.8,2235,5.5,44,215,2.94,679,10,429.44455895517831,875.55461693567872,1048.372093023256,16.15229173407106,0.85034013605442182,0.55774728977058607,0.45091772481747083,2.7718397282407312,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.22309665272945042,0.31737570382889785,2.677159832753405,7.6170168918935488,4.8491435598372927,440.63134458308593,357.19433509532632,3436.2095036170394,0.15981473447468164,34.597872067302063,-44331.321430041098,429.44455895517831,5.4787765370186703E-2,9.4991964281535672,-50317.140893560601,875.55461693567872,4.6379396320334836,5.5585390008131189E-2,9.9317737697707358,-50271.68174032501,865.85092765203444]
["KBM","KBMS-35H02-B (120 V)",17.600000000000001,6.3,16.472536610011169,5.7395597944289785,400,58.8,661,3.43,28,174,2.94,160,10,580.48830701823795,661,661,15.736866748043456,0.85034013605442182,0.57075808345896284,0.45091772481747083,3.6308623298033282,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.27797814364577006,0.3954497205998671,3.3357377237492409,9.490793294396811,6.0420266666666658,440.63134458308593,357.19433509532632,3436.2095036170394,0.10169026752584735,21.757510581125761,-46896.211768002715,580.48830701823795,3.4146144969775236E-2,5.0650102317115984,-50593.3228299037,1145.3294835865233,4.8997771869691018,3.6160910280655212E-2,6.2457792914194332,-50483.042159489996,1098.3436355370241]
["KBM","KBMS-35H02-B (240 V)",17.600000000000001,6.3,16.083025828233634,5.6038417519977815,950,58.8,1386,3.43,28,174,2.94,325,10,580.48830701823795,1118.0987382847256,1295.4022988505747,15.814603255302641,0.85034013605442182,0.55210128326259245,0.45091772481747083,2.1851084873146682,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.27797814364577006,0.3954497205998671,3.3357377237492409,9.490793294396811,6.0420266666666658,440.63134458308593,357.19433509532632,3436.2095036170394,0.10169026752584735,21.757510581125761,-46896.211768002715,580.48830701823795,3.5273123964755022E-2,5.7554166911030977,-50531.636241179251,1118.0987382847256,5.5676608959264744,3.6160910280655212E-2,6.2457792914194332,-50483.042159489996,1098.3436355370241]
["KBM","KBMS-35H02-B (400 V)",17.600000000000001,6.3,15.305400360670603,5.3328921117319172,1800,58.8,2313,3.43,28,174,2.94,565,10,580.48830701823795,1109.9957651242817,1295.4022988505747,16.185002287604814,0.85034013605442182,0.54738533668413625,0.45091772481747083,2.1851084873146682,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.27797814364577006,0.3954497205998671,3.3357377237492409,9.490793294396811,6.0420266666666658,440.63134458308593,357.19433509532632,3436.2095036170394,0.10169026752584735,21.757510581125761,-46896.211768002715,580.48830701823795,3.5630020267623824E-2,5.9573993785243244,-50512.101080763299,1109.9957651242817,5.7630544131582848,3.6160910280655212E-2,6.2457792914194332,-50483.042159489996,1098.3436355370241]
["KBM","KBMS-35H02-B (480 V)",17.600000000000001,6.3,14.823112654331526,5.16484761474966,2200,58.8,2776,3.43,28,174,2.94,679,10,580.48830701823795,1109.1097688897876,1295.4022988505747,16.20005778082394,0.85034013605442182,0.54720309584716909,0.45091772481747083,2.1851084873146682,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.27797814364577006,0.3954497205998671,3.3357377237492409,9.490793294396811,6.0420266666666658,440.63134458308593,357.19433509532632,3436.2095036170394,0.10169026752584735,21.757510581125761,-46896.211768002715,580.48830701823795,3.5669652063491861E-2,5.9794078050569288,-50509.931785414396,1109.1097688897876,5.7843448708893241,3.6160910280655212E-2,6.2457792914194332,-50483.042159489996,1098.3436355370241]
["KBM","KBMS-35H02-C (120 V)",17.5,8.6999999999999993,16.119212636347161,7.8630305543156886,625,59.2,923,1.8,14.6,124,2.94,160,10,854.80109861304436,923,923,15.460853221357487,0.85034013605442182,0.56469925239506424,0.44787098343356896,2.6002166847237271,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.38606814834503694,0.54921778882767947,4.6328177801404431,13.181226931864307,8.3914296888888877,440.63134458308593,357.19433509532632,3436.2095036170394,5.3339831827869243E-2,11.37778514160213,-48700.353894243271,854.80109861304436,1.7377588270825941E-2,2.6125227532931534,-50694.187134227461,1634.4700989794405,6.7577989017823681,1.8462285792449219E-2,3.2440741894671912,-50634.04889589674,1570.5416711379391]
["KBM","KBMS-35H02-C (240 V)",17.5,8.6999999999999993,15.48350232079725,7.5529279613645128,1400,59.2,1935,1.8,14.6,124,2.94,325,10,854.80109861304436,1605.4560562711852,1817.741935483871,15.187572563190825,0.85034013605442182,0.55306295531844496,0.44787098343356896,1.5281351931662375,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.38606814834503694,0.54921778882767947,4.6328177801404431,13.181226931864307,8.3914296888888877,440.63134458308593,357.19433509532632,3436.2095036170394,5.3339831827869243E-2,11.37778514160213,-48700.353894243271,854.80109861304436,1.7849092266499767E-2,2.9039749617356674,-50668.045819159932,1605.4560562711852,7.5116968005287674,1.8462285792449219E-2,3.2440741894671912,-50634.04889589674,1570.5416711379391]
["KBM","KBMS-35H02-C (400 V)",17.5,8.6999999999999993,14.155427879702691,6.9050867705866787,2550,59.2,3224,1.8,14.6,124,2.94,565,10,854.80109861304436,1598.8889356222885,1817.741935483871,15.402902212731707,0.85034013605442182,0.55116108889338034,0.44787098343356896,1.5281351931662375,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.38606814834503694,0.54921778882767947,4.6328177801404431,13.181226931864307,8.3914296888888877,440.63134458308593,357.19433509532632,3436.2095036170394,5.3339831827869243E-2,11.37778514160213,-48700.353894243271,854.80109861304436,1.7960573805538994E-2,2.9687059101070856,-50661.865014621741,1598.8889356222885,7.6791360051306397,1.8462285792449219E-2,3.2440741894671912,-50634.04889589674,1570.5416711379391]
["KBM","KBMS-35H02-C (480 V)",17.5,8.6999999999999993,13.100441253251635,6.3904591479276274,3200,59.2,3869,1.8,14.6,124,2.94,679,10,854.80109861304436,1599.9065868427708,1817.741935483871,15.300349056836113,0.85034013605442182,0.55209392881809993,0.44787098343356896,1.5281351931662375,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.38606814834503694,0.54921778882767947,4.6328177801404431,13.181226931864307,8.3914296888888877,440.63134458308593,357.19433509532632,3436.2095036170394,5.3339831827869243E-2,11.37778514160213,-48700.353894243271,854.80109861304436,1.7943182572664768E-2,2.9587010495414052,-50662.829226382717,1599.9065868427708,7.653256484786553,1.8462285792449219E-2,3.2440741894671912,-50634.04889589674,1570.5416711379391]
["KBM","KBMS-35H02-D (120 V)",17.45,10.92,15.952942531093511,9.7274039823740921,850,59.4,1165,1.1399999999999999,9.3000000000000007,99,2.94,160,10,1098.4708248491929,1165,1165,15.398150645557577,0.85034013605442182,0.55953513000051769,0.44636300032436504,2.0600858369098711,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.48597057700975893,0.69133826990066571,5.8316469241171074,16.592118477615976,10.562870688315822,440.63134458308593,357.19433509532632,3436.2095036170394,3.4373633840441876E-2,7.2663167473263588,-49458.375001722394,1098.4708248491929,1.1033739022531889E-2,1.6275114126220025,-50737.595634164507,2071.905389275259,8.3257500636762494,1.1785213186108583E-2,2.0648220837527314,-50696.408591022526,1988.3000980328852]
["KBM","KBMS-35H02-D (240 V)",17.45,10.92,15.020785439916175,9.1590155121440091,1850,59.4,2437,1.1399999999999999,9.3000000000000007,99,2.94,325,10,1098.4708248491929,2041.5249569344362,2276.7676767676771,14.769296135048844,0.85034013605442182,0.55281792539653529,0.44636300032436504,1.2070612491416302,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.48597057700975893,0.69133826990066571,5.8316469241171074,16.592118477615976,10.562870688315822,440.63134458308593,357.19433509532632,3436.2095036170394,3.4373633840441876E-2,7.2663167473263588,-49458.375001722394,1098.4708248491929,1.1293148609081162E-2,1.7905832185629182,-50723.377828216537,2041.5249569344362,9.1599654726539743,1.1785213186108583E-2,2.0648220837527314,-50696.408591022526,1988.3000980328852]
["KBM","KBMS-35H02-D (400 V)",17.45,10.92,12.441369265697876,7.5862007717669977,3500,59.4,4061,1.1399999999999999,9.3000000000000007,99,2.94,565,10,1098.4708248491929,2041.5681542910456,2276.7676767676771,14.528439713212974,0.85034013605442182,0.55457011608630224,0.44636300032436504,1.2070612491416302,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.48597057700975893,0.69133826990066571,5.8316469241171074,16.592118477615976,10.562870688315822,440.63134458308593,357.19433509532632,3436.2095036170394,3.4373633840441876E-2,7.2663167473263588,-49458.375001722394,1098.4708248491929,1.1292768784382073E-2,1.7903553086169133,-50723.398645773581,2041.5681542910456,9.1587995691569262,1.1785213186108583E-2,2.0648220837527314,-50696.408591022526,1988.3000980328852]
["KBM","KBMS-35H02-D (480 V)",17.45,10.92,10.548641577020971,6.4320985225737637,4300,59.4,4873,1.1399999999999999,9.3000000000000007,99,2.94,679,10,1098.4708248491929,2047.7942142288907,2276.7676767676771,14.163357709559005,0.85034013605442182,0.55717430253724054,0.44636300032436504,1.2070612491416302,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.48597057700975893,0.69133826990066571,5.8316469241171074,16.592118477615976,10.562870688315822,440.63134458308593,357.19433509532632,3436.2095036170394,3.4373633840441876E-2,7.2663167473263588,-49458.375001722394,1098.4708248491929,1.1238351996572391E-2,1.7573976406762601,-50726.381138979326,2047.7942142288907,8.990200256225874,1.1785213186108583E-2,2.0648220837527314,-50696.408591022526,1988.3000980328852]
["KBM","KBMS-35H02-E (120 V)",17.100000000000001,12,15.580431271101332,10.671528267877624,950,59.4,1305,0.94,7.4,88.4,2.94,160,10,1241.5761845834363,1305,1305,15.012592430302355,0.85034013605442182,0.56899812185608267,0.44636300032436504,1.8390804597701149,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.54496411341303863,0.77526205319494979,6.5395693609564631,18.606289276678794,11.845131643924624,440.63134458308593,357.19433509532632,3436.2095036170394,2.7378895815966042E-2,5.9994622722815141,-49653.670103047094,1241.5761845834363,8.7440660571906914E-3,1.3076932570160862,-50750.452452343918,2335.5308342952744,9.0858411229866167,9.3943586229545423E-3,1.7048282673620456,-50712.178455895257,2234.4267224069108]
["KBM","KBMS-35H02-E (240 V)",17.100000000000001,12,14.533563583806249,9.9544956053467466,2050,59.4,2728,0.94,7.4,88.4,2.94,325,10,1241.5761845834363,2305.990145921799,2549.7737556561083,14.213084348352368,0.85034013605442182,0.56359628184242327,0.44636300032436504,1.074101010309586,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.54496411341303863,0.77526205319494979,6.5395693609564631,18.606289276678794,11.845131643924624,440.63134458308593,357.19433509532632,3436.2095036170394,2.7378895815966042E-2,5.9994622722815141,-49653.670103047094,1241.5761845834363,8.9227156064964272E-3,1.4278419791464791,-50739.937750845449,2305.990145921799,9.9206333761007492,9.3943586229545423E-3,1.7048282673620456,-50712.178455895257,2234.4267224069108]
["KBM","KBMS-35H02-E (400 V)",17.100000000000001,12,11.496360954248335,7.8742198316769416,3850,59.4,4547,0.94,7.4,88.4,2.94,565,10,1241.5761845834363,2311.5124020204676,2549.7737556561083,13.735615285532178,0.85034013605442182,0.56674709686492564,0.44636300032436504,1.074101010309586,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.54496411341303863,0.77526205319494979,6.5395693609564631,18.606289276678794,11.845131643924624,440.63134458308593,357.19433509532632,3436.2095036170394,2.7378895815966042E-2,5.9994622722815141,-49653.670103047094,1241.5761845834363,8.8886124952326367E-3,1.4056996167707505,-50741.944943343282,2311.5124020204676,9.7667884391829531,9.3943586229545423E-3,1.7048282673620456,-50712.178455895257,2234.4267224069108]
["KBM","KBMS-35H02-E (480 V)",17.100000000000001,12,9.1226258870120436,6.2483738952137289,4700,59.4,5457,0.94,7.4,88.4,2.94,679,10,1241.5761845834363,2322.7824832632041,2549.7737556561083,13.1575096059392,0.85034013605442182,0.57053606282076308,0.44636300032436504,1.074101010309586,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.54496411341303863,0.77526205319494979,6.5395693609564631,18.606289276678794,11.845131643924624,440.63134458308593,357.19433509532632,3436.2095036170394,2.7378895815966042E-2,5.9994622722815141,-49653.670103047094,1241.5761845834363,8.8200216950483582E-3,1.3600739961504191,-50745.981963264581,2322.7824832632041,9.4497820327723918,9.3943586229545423E-3,1.7048282673620456,-50712.178455895257,2234.4267224069108]
["KBM","KBMS-35H02-F (120 V)",17.3,14.92,15.597184423005743,13.106877666391382,1200,59.4,1607,0.61,4.9000000000000004,72.099999999999994,2.94,160,10,1556.7687458613204,1607,1607,15.019646139808524,0.85034013605442182,0.55938272456101634,0.44636300032436504,1.4934660858742999,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.6697388448135615,0.95276569439178205,8.0368661377627379,22.866376665402768,14.557187507600084,440.63134458308593,357.19433509532632,3436.2095036170394,1.8154352086988401E-2,3.9024279373386861,-50072.775299383786,1556.7687458613204,5.7972703829910315E-3,0.83900236477589374,-50771.307102282262,2887.8799523471121,11.013806897389667,6.2445880895929881E-3,1.108927626673502,-50746.020740053224,2763.2755019820383]
["KBM","KBMS-35H02-F (240 V)",17.3,14.92,13.873506360085971,11.658408705954598,2650,59.4,3356,0.61,4.9000000000000004,72.099999999999994,2.94,325,10,1556.7687458613204,2863.6073731893789,3126.2135922330099,13.597308508888933,0.85034013605442182,0.55747881343192585,0.44636300032436504,0.86853446146738944,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.6697388448135615,0.95276569439178205,8.0368661377627379,22.866376665402768,14.557187507600084,440.63134458308593,357.19433509532632,3436.2095036170394,1.8154352086988401E-2,3.9024279373386861,-50072.775299383786,1556.7687458613204,5.8786208812246533E-3,0.89417429414825578,-50766.708450953491,2863.6073731893789,11.738063468973856,6.2445880895929881E-3,1.108927626673502,-50746.020740053224,2763.2755019820383]
["KBM","KBMS-35H02-F (400 V)",17.3,14.92,7.6956096012669395,6.4668988245940673,5100,59.4,5593,0.61,4.9000000000000004,72.099999999999994,2.94,565,10,1556.7687458613204,2900.2820401309468,3126.2135922330099,11.838148827480079,0.85034013605442182,0.56651082646240603,0.44636300032436504,0.86853446146738944,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.6697388448135615,0.95276569439178205,8.0368661377627379,22.866376665402768,14.557187507600084,440.63134458308593,357.19433509532632,3436.2095036170394,1.8154352086988401E-2,3.9024279373386861,-50072.775299383786,1556.7687458613204,5.7567815856527475E-3,0.81014367925192587,-50773.595888039235,2900.2820401309468,10.634971267101097,6.2445880895929881E-3,1.108927626673502,-50746.020740053224,2763.2755019820383]
["KBM","KBMS-35H02-F (480 V)",17.3,14.92,6.2689363695640994,5.2680137559362183,5400,59.4,6711,0.61,4.9000000000000004,72.099999999999994,2.94,679,10,1556.7687458613204,2911.0994632577899,3126.2135922330099,11.353236404865838,0.85034013605442182,0.56900335814895109,0.44636300032436504,0.86853446146738944,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.6697388448135615,0.95276569439178205,8.0368661377627379,22.866376665402768,14.557187507600084,440.63134458308593,357.19433509532632,3436.2095036170394,1.8154352086988401E-2,3.9024279373386861,-50072.775299383786,1556.7687458613204,5.7220652218733011E-3,0.78455449031548419,-50775.558364679098,2911.0994632577899,10.299055186957425,6.2445880895929881E-3,1.108927626673502,-50746.020740053224,2763.2755019820383]
["KBM","KBMS-35H02-G (120 V)",17.100000000000001,18.64,15.094049441618461,16.057499405977087,1550,59.4,2032,0.39,3.1,57,2.94,160,10,1983.6417982216799,2032,2032,14.470263526044331,0.85034013605442182,0.56424720100174253,0.44636300032436504,1.1811023622047243,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.84651092283491991,1.2042403892961553,10.158131074019039,28.901769343107727,18.399437820229583,440.63134458308593,357.19433509532632,3436.2095036170394,1.1533272593584727E-2,2.4930806770391358,-50326.901207892748,1983.6417982216799,3.5900655475092362E-3,0.50585735404750631,-50785.469967478923,3691.3391728377082,13.137961292437231,3.9179459104890634E-3,0.70844256003865247,-50766.541127972137,3510.3694044936628]
["KBM","KBMS-35H02-G (240 V)",17.100000000000001,18.64,12.44217172759582,13.236352901697682,3400,59.4,4241,0.39,3.1,57,2.94,325,10,1983.6417982216799,3683.2904620695199,3954.385964912281,12.054078103028216,0.85034013605442182,0.56541882955609923,0.44636300032436504,0.68368873000309693,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.84651092283491991,1.2042403892961553,10.158131074019039,28.901769343107727,18.399437820229583,440.63134458308593,357.19433509532632,3436.2095036170394,1.1533272593584727E-2,2.4930806770391358,-50326.901207892748,1983.6417982216799,3.6033642763321039E-3,0.51562517013107068,-50784.702219446546,3683.2904620695199,13.391647808192545,3.9179459104890634E-3,0.70844256003865247,-50766.541127972137,3510.3694044936628]
["KBM","KBMS-35H02-G (400 V)",17.100000000000001,18.64,3.6056826762543186,3.8358326343131051,5800,59.4,7068,0.39,3.1,57,2.94,565,10,1983.6417982216799,3777.7469815710447,3954.385964912281,8.3106695623892914,0.85034013605442182,0.58063770127765135,0.44636300032436504,0.68368873000309693,26.513962219267285,0,-21.476309397606496,0,0,0,0,0,0.84651092283491991,1.2042403892961553,10.158131074019039,28.901769343107727,18.399437820229583,440.63134458308593,357.19433509532632,3436.2095036170394,1.1533272593584727E-2,2.4930806770391358,-50326.901207892748,1983.6417982216799,3.455028335156748E-3,0.39316298057406496,-50793.26579183642,3777.7469815710447,10.211099985147639,3.9179459104890634E-3,0.70844256003865247,-50766.541127972137,3510.3694044936628]
["KBM","KBMS-35H03-A (120 V)",21.8,10.199999999999999,20.567715722644937,9.3489616921113345,650,76.099999999999994,867,1.41,12,132,3.7,160,10,844.72056596793539,867,867,20.156322356204864,0.67567567567567566,0.50710600131177053,0.39708434567388395,2.7681660899653977,30.218118705782565,0,-24.476676151683879,0,0,0,0,0,0.41411335510357183,0.58911469953933893,4.969360261242862,14.138752788944133,9.0010095820591189,502.19013537042895,407.09648485129111,3916.2681842694205,5.4962565284357029E-2,11.478417209983911,-48914.749335880762,844.72056596793539,1.9514947014241491E-2,2.7090354302651107,-50699.861662040414,1543.9162489328428,8.4035156614431319,1.9822851965122505E-2,2.9016491250004348,-50684.355826953979,1527.504625677723]
["KBM","KBMS-35H03-A (240 V)",21.8,10.199999999999999,19.644267261628229,8.9292123916491946,1400,76.099999999999994,1818,1.41,12,132,3.7,325,10,844.72056596793539,1528.7946957043682,1707.5757575757575,19.445948017300704,0.67567567567567566,0.50324321828074225,0.39708434567388395,1.5711900047014054,30.218118705782565,0,-24.476676151683879,0,0,0,0,0,0.41411335510357183,0.58911469953933893,4.969360261242862,14.138752788944133,9.0010095820591189,502.19013537042895,407.09648485129111,3916.2681842694205,5.4962565284357029E-2,11.478417209983911,-48914.749335880762,844.72056596793539,1.9798142449723253E-2,2.8866661383237511,-50685.600177425607,1528.7946957043682,8.9545318720276992,1.9822851965122505E-2,2.9016491250004348,-50684.355826953979,1527.504625677723]
["KBM","KBMS-35H03-A (400 V)",21.8,10.199999999999999,17.188733853924695,7.8130608426930426,2550,76.099999999999994,3029,1.41,12,132,3.7,565,10,844.72056596793539,1529.8727028452781,1707.5757575757575,19.033470508848961,0.67567567567567566,0.50615132255494288,0.39708434567388395,1.5711900047014054,30.218118705782565,0,-24.476676151683879,0,0,0,0,0,0.41411335510357183,0.58911469953933893,4.969360261242862,14.138752788944133,9.0010095820591189,502.19013537042895,407.09648485129111,3916.2681842694205,5.4962565284357029E-2,11.478417209983911,-48914.749335880762,844.72056596793539,1.9777560945865934E-2,2.8741266101405021,-50686.636644698156,1529.8727028452781,8.9156338493965492,1.9822851965122505E-2,2.9016491250004348,-50684.355826953979,1527.504625677723]
["KBM","KBMS-35H03-A (480 V)",21.8,10.199999999999999,15.586916362161105,7.0849619828005022,3100,76.099999999999994,3635,1.41,12,132,3.7,679,10,844.72056596793539,1532.4823235531294,1707.5757575757575,18.728567467824103,0.67567567567567566,0.50829394307446107,0.39708434567388395,1.5711900047014054,30.218118705782565,0,-24.476676151683879,0,0,0,0,0,0.41411335510357183,0.58911469953933893,4.969360261242862,14.138752788944133,9.0010095820591189,502.19013537042895,407.09648485129111,3916.2681842694205,5.4962565284357029E-2,11.478417209983911,-48914.749335880762,844.72056596793539,1.9727987234651332E-2,2.8436962509883994,-50689.133135217438,1532.4823235531294,8.8212378895426724,1.9822851965122505E-2,2.9016491250004348,-50684.355826953979,1527.504625677723]
["KBM","KBMS-35H03-B (120 V)",21.7,14,19.629109648000426,12.345351979874481,900,76.599999999999994,1197,0.75,6.2,96.2,3.7,160,10,1197,1197,1197,18.945715831840566,0.67567567567567566,0.51405094333054324,0.39449241130264451,2.0050125313283207,30.218118705782565,0,-24.476676151683879,0,0,0,0,0,0.57101019236292649,0.81231501897264957,6.8521223083551179,19.49556045534359,12.411259259259257,502.19013537042895,407.09648485129111,3916.2681842694205,2.8557938666551951E-2,6.1758115339889281,-49774.826233090535,1216.4980246718101,1.0119951450595022E-2,1.3077129613023062,-50758.962899225728,2175.9041265250921,10.464427307424105,1.0471952930822356E-2,1.5510036165956047,-50740.174646518521,2128.4035839382786]
["KBM","KBMS-35H03-B (240 V)",21.7,14,17.910753839658661,11.264625056389095,2050,76.599999999999994,2504,0.75,6.2,96.2,3.7,325,10,1216.4980246718101,2152.6859033033911,2343.0353430353434,17.720947905603268,0.67567567567567566,0.50901608075981963,0.39449241130264451,1.1276056938220216,30.218118705782565,0,-24.476676151683879,0,0,0,0,0,0.57101019236292649,0.81231501897264957,6.8521223083551179,19.49556045534359,12.411259259259257,502.19013537042895,407.09648485129111,3916.2681842694205,2.8557938666551951E-2,6.1758115339889281,-49774.826233090535,1216.4980246718101,1.0287764943078589E-2,1.4288757828049399,-50750.005771254495,2152.6859033033911,11.433982229258064,1.0471952930822356E-2,1.5510036165956047,-50740.174646518521,2128.4035839382786]
["KBM","KBMS-35H03-B (400 V)",21.7,14,13.105153077224749,8.2422346397639927,3800,76.599999999999994,4173,0.75,6.2,96.2,3.7,565,10,1216.4980246718101,2161.1211450204332,2343.0353430353434,16.811972257099107,0.67567567567567566,0.51361105184510991,0.39449241130264451,1.1276056938220216,30.218118705782565,0,-24.476676151683879,0,0,0,0,0,0.57101019236292649,0.81231501897264957,6.8521223083551179,19.49556045534359,12.411259259259257,502.19013537042883,407.09648485129111,3916.2681842694205,2.8557938666551951E-2,6.1758115339889281,-49774.826233090535,1216.4980246718101,1.0225852028374918E-2,1.3854082122513869,-50753.310403628595,2161.1211450204332,11.086151133483803,1.0471952930822356E-2,1.5510036165956047,-50740.174646518521,2128.4035839382786]
["KBM","KBMS-35H03-B (480 V)",21.7,14,10.26549382942725,6.4562854273127357,4800,76.599999999999994,5007,0.75,6.2,96.2,3.7,679,10,1216.4980246718101,2163.7280442737206,2343.0353430353434,16.545591317981422,0.67567567567567566,0.51496483571722851,0.39449241130264451,1.1276056938220216,30.218118705782565,0,-24.476676151683879,0,0,0,0,0,0.57101019236292649,0.81231501897264957,6.8521223083551179,19.49556045534359,12.411259259259257,502.19013537042895,407.09648485129111,3916.2681842694205,2.8557938666551951E-2,6.1758115339889281,-49774.826233090535,1216.4980246718101,1.0206935425789503E-2,1.3718526566982863,-50754.320086626256,2163.7280442737206,10.977678456455422,1.0471952930822356E-2,1.5510036165956047,-50740.174646518521,2128.4035839382786]
["KBM","KBMS-35H03-C (120 V)",20.7,20.2,18.044877685729375,17.185597795932736,1450,75.2,1813,0.36,2.8,63.6,3.7,160,10,1813,1813,1813,17.380181547743007,0.67567567567567566,0.53442932809829957,0.40183668491732133,1.3237727523441809,30.218118705782565,0,-24.476676151683879,0,0,0,0,0,0.86368739724073562,1.2286755190354424,10.364248766888828,29.488212456850619,18.772779101807117,502.19013537042895,407.09648485129111,3916.2681842694205,1.2726010844285641E-2,2.9101750186989843,-50281.723511168246,1876.683248046279,4.3630610066566142E-3,0.55707732326908055,-50785.979640731886,3348.4997656806599,14.047376945704046,4.6130690536149016E-3,0.74447276333356061,-50770.90504473805,3237.8012744465632]
["KBM","KBMS-35H03-C (240 V)",20.7,20.2,14.724399251211478,14.023237382106169,3100,75.2,3783,0.36,2.8,63.6,3.7,325,10,{"$f":"IF(AQ1312<I1312,IF(AQ1312<0,0,AQ1312),I1312)","v":1876.683248046279},{"$f":"IF(AU1312<I1312,IF(AU1312<0,0,AU1312),I1312)","v":3342.9475902452427},{"$f":"IF(UAC_V*0.98/L1312*1000<I1312,IF(UAC_V*0.98/L1312*1000<0,0,UAC_V*0.98/L1312*1000),I1312)","v":3544.0251572327047},{"$f":"C1312+(E1312-C1312)/G1312*Q1312","v":14.256090282764433},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M1312,(inertia/gear^2+gear_inertia)/M1312),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M1312,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M1312))","v":0.67567567567567566},{"$f":"IF((C1312+(E1312-C1312)/G1312*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X1312^2*time1+Y1312^2*time2+Z1312^2*time3+AA1312^2*time4)/time)/(C1312+(E1312-C1312)/G1312*mspeed),SQRT((((X1312-Y1312)*2/PI()+Y1312)^2*time1+Y1312^2*time2+((Z1312-Y1312)*2/PI()+Y1312)^2*time3+AA1312^2*time4)/time)/(C1312+(E1312-C1312)/G1312*mspeed)),IF(AccType=1,SQRT((X1312^2*time1+Y1312^2*time2+Z1312^2*time3+AA1312^2*time4+AB1312^2*time5+AC1312^2*time6+AD1312^2*time7+AE1312^2*time8)/time)/(C1312+(E1312-C1312)/G1312*mspeed),SQRT((((X1312-Y1312)*2/PI()+Y1312)^2*time1+Y1312^2*time2+((Z1312-Y1312)*2/PI()+Y1312)^2*time3+AA1312^2*time4+((AB1312-AC1312)*2/PI()+AC1312)^2*time5+AC1312^2*time6+((AD1312-AC1312)*2/PI()+AC1312)^2*time7+AE1312^2*time8)/time)/(C1312+(E1312-C1312)/G1312*mspeed))))","v":0.53560366702721462},{"$f":"IF(move1,MAX(ABS(X1312),ABS(Z1312))/H1312,MAX(ABS(X1312),ABS(Z1312),ABS(AB1312),ABS(AD1312))/H1312)","v":0.40183668491732133},{"$f":"IF(AZ1312>0,speed/(MIN(AZ1312,I1312)),\"NA\")","v":0.74124376284033422},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M1312+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M1312+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":30.218118705782565},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M1312+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M1312+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-24.476676151683879},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M1312+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M1312+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M1312+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M1312+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH1312/Irms","v":0.86368739724073562},{"$f":"AI1312/Ipeak","v":1.2286755190354424},{"$f":"IF(move1,IF(AccType=1,SQRT((X1312^2*time1+Y1312^2*time2+Z1312^2*time3+AA1312^2*time4)/time)/(C1312/D1312),SQRT((((X1312-Y1312)*2/PI()+Y1312)^2*time1+Y1312^2*time2+((Z1312-AA1312)*2/PI()+AA1312)^2*time3+AA1312^2*time4)/time)/(C1312/D1312)),IF(AccType=1,SQRT((X1312^2*time1+Y1312^2*time2+Z1312^2*time3+AA1312^2*time4+AB1312^2*time5+AC1312^2*time6+AD1312^2*time7+AE1312^2*time8)/time)/(C1312/D1312),SQRT((((X1312-Y1312)*2/PI()+Y1312)^2*time1+Y1312^2*time2+((Z1312-AA1312)*2/PI()+AA1312)^2*time3+AA1312^2*time4+((AB1312-AC1312)*2/PI()+AC1312)^2*time5+AC1312^2*time6+((AD1312-AE1312)*2/PI()+AE1312)^2*time7+AE1312^2*time8)/time)/(C1312/D1312)))","v":10.364248766888828},{"$f":"IF(move1,MAX(ABS(X1312),ABS(Z1312))/(C1312/D1312),MAX(ABS(X1312),ABS(Z1312),ABS(AB1312),ABS(AD1312))/(C1312/D1312))","v":29.488212456850619},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X1312),ABS(Z1312))/(C1312/D1312),MAX(ABS((X1312-Y1312)*2/PI()+Y1312),ABS((Z1312-Y1312)*2/PI()+Y1312))/(C1312/D1312)),IF(AccType=1,MAX(ABS(X1312),ABS(Z1312),ABS(AB1312),ABS(AD1312))/(C1312/D1312),MAX(ABS((X1312-Y1312)*2/PI()+Y1312),ABS((Z1312-Y1312)*2/PI()+Y1312),ABS((AB1312-AC1312)*2/PI()+AC1312),ABS((AD1312-AC1312)*2/PI()+AC1312))/(C1312/D1312)))","v":18.772779101807117},{"$f":"IF((C1312+(E1312-C1312)/G1312*mspeed)<0,\"NA\",U1312*(C1312+(E1312-C1312)/G1312*mspeed)*mspeed/9.55)","v":502.19013537042895},{"$f":"IF(move1,IF(speed1>speed2,AM1312/2*time1/time,AM1312/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z1312*-speed/30*PI(),((Z1312-AA1312)*2/PI()+AA1312)*-speed/30*PI()),IF(AccType=1,X1312*-speed/30*PI(),((X1312-Y1312)*2/PI()+Y1312)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z1312*-speed/30*PI(),((Z1312-AA1312)*2/PI()+AA1312)*-speed/30*PI()),IF(AccType=1,X1312*-speed/30*PI(),((X1312-Y1312)*2/PI()+Y1312)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD1312*-speed/30*PI(),((AD1312-AE1312)*2/PI()+AE1312)*-speed/30*PI()),IF(AccType=1,AB1312*-speed/30*PI(),((AB1312-AC1312)*2/PI()+AC1312)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD1312*-speed/30*PI(),((AD1312-AE1312)*2/PI()+AE1312)*-speed/30*PI()),IF(AccType=1,AB1312*-speed/30*PI(),((AB1312-AC1312)*2/PI()+AC1312)*-speed/30*PI()),0)/2*time7/time)))","v":407.09648485129111},{"$f":"IF(move1,MAX(IF(AccType=1,Z1312*-speed/30*PI(),((Z1312-AA1312)*2/PI()+AA1312)*-speed/30*PI()),IF(AccType=1,X1312*-speed/30*PI(),((X1312-Y1312)*2/PI()+Y1312)*-speed/30*PI()),0),MAX(IF(AccType=1,Z1312*-speed/30*PI(),((Z1312-AA1312)*2/PI()+AA1312)*-speed/30*PI()),IF(AccType=1,X1312*-speed/30*PI(),((X1312-Y1312)*2/PI()+Y1312)*-speed/30*PI()),IF(AccType=1,AD1312*-speed/30*PI(),((AD1312-AE1312)*2/PI()+AE1312)*-speed/30*PI()),IF(AccType=1,AB1312*-speed/30*PI(),((AB1312-AC1312)*2/PI()+AC1312)*-speed/30*PI()),0))","v":3916.2681842694205},{"$f":"(L1312^2)/1000000+((K1312/1000)^2*(D1312/C1312*H1312)^2*PI()*PI()*(O1312/2)^2)/1200","v":1.2726010844285641E-2},{"$f":"SQRT(3)*L1312*J1312*D1312/C1312*H1312/1000","v":2.9101750186989843},{"$f":"0.75*J1312^2*(D1312/C1312*H1312)^2-(UAC_V*0.98)^2","v":-50281.723511168246},{"$f":"-AO1312/2/AN1312+SQRT((AO1312/2/AN1312)^2-AP1312/AN1312)","v":1876.683248046279},{"$f":"(L1312^2)/1000000+((K1312/1000)^2*AV1312^2*PI()*PI()*(O1312/2)^2)/1200","v":4.3747464476843962E-3},{"$f":"SQRT(3)*L1312*J1312*AV1312/1000","v":0.56721715960824703},{"$f":"0.75*J1312^2*AV1312^2-(UAC_V*0.98)^2","v":-50785.275050201119},{"$f":"-AS1312/2/AR1312+SQRT((AS1312/2/AR1312)^2-AT1312/AR1312)","v":3342.9475902452427},{"$f":"D1312+(F1312-D1312)*((0.85*UAC_V-D1312*J1312)/L1312*1000)/G1312","v":14.303065154996347},{"$f":"(L1312^2)/1000000+((K1312/1000)^2*AJ1312^2*PI()*PI()*(O1312/2)^2)/1200","v":4.6130690536149016E-3},{"$f":"SQRT(3)*L1312*J1312*AJ1312/1000","v":0.74447276333356061},{"$f":"0.75*J1312^2*AJ1312^2-(UAC_V*0.98)^2","v":-50770.90504473805},{"$f":"IF(((AX1312/2/AW1312)^2-AY1312/AW1312)>0,-AX1312/2/AW1312+SQRT((AX1312/2/AW1312)^2-AY1312/AW1312),-9999)","v":3237.8012744465632}]
["KBM","KBMS-35H03-C (400 V)",20.7,20.2,5.7009300615516914,5.4294572014778009,5000,75.2,6305,0.36,2.8,63.6,3.7,565,10,1876.683248046279,3401.4178785799973,3544.0251572327047,10.49637906985803,0.67567567567567566,0.549008350907357,0.40183668491732133,0.74124376284033422,30.218118705782565,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-24.476676151683879,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.86368739724073562,1.2286755190354424,10.364248766888828,29.488212456850619,18.772779101807117,502.19013537042906,407.09648485129111,3916.2681842694205,1.2726010844285641E-2,2.9101750186989843,-50281.723511168246,1876.683248046279,4.2565654997417622E-3,0.45435617414160295,-50792.400941011743,3401.4178785799973,11.457139214213091,4.6130690536149016E-3,0.74447276333356061,-50770.90504473805,3237.8012744465632]
["KBM","KBMS-35H03-D (120 V)",20,21.5,17.188733853924695,17.904931097838226,1550,75.7,1996,0.32,2.2999999999999998,57.8,3.7,160,10,1996,1996,1996,16.379814691892705,0.67567567567567566,0.5537141303513009,0.39918254565102462,1.2024048096192386,30.218118705782565,0,-24.476676151683879,0,0,0,0,0,0.95144573302472624,1.3535199003631775,11.417348796296714,32.484477608716261,20.680260740740735,502.19013537042895,407.09648485129111,3916.2681842694205,1.0543996780891933E-2,2.60701054511095,-50296.567551520006,2063.9405895319669,3.5519370258283631E-3,0.44629540080145519,-50790.255096983354,3719.1406985877197,13.931053730039581,3.8060255333628485E-3,0.66251307581032937,-50772.314699445378,3566.3961884353016]
["KBM","KBMS-35H03-D (240 V)",20,21.5,13.298799803649256,13.852916462134642,3400,75.7,4166,0.32,2.2999999999999998,57.8,3.7,325,10,2063.9405895319669,3714.5062416948799,3899.6539792387548,12.678926483473003,0.67567567567567566,0.55577120726904716,0.39918254565102462,0.67294822930285858,30.218118705782565,0,-24.476676151683879,0,0,0,0,0,0.95144573302472624,1.3535199003631775,11.417348796296714,32.484477608716261,20.680260740740735,502.19013537042895,407.09648485129111,3916.2681842694205,1.0543996780891933E-2,2.60701054511095,-50296.567551520006,2063.9405895319669,3.5589424946228213E-3,0.45364034345369808,-50789.760462667415,3714.5062416948799,14.160325173457338,3.8060255333628485E-3,0.66251307581032937,-50772.314699445378,3566.3961884353016]
["KBM","KBMS-35H04-A (120 V)",25.6,10.86,23.786429676643269,9.7485367527226519,550,92.3,778,1.35,11,147,4.46,160,10,778,778,778,23.034622342597206,0.5605381165919282,0.49449126303316099,0.36752194141167766,3.0848329048843186,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.42148582027214077,0.59960271580135838,5.0578298432656892,14.390465179232601,9.1612546666666645,563.74892615777185,456.99863460725584,4396.3268649218007,5.9753067325012302E-2,13.458705545314521,-48709.542954376884,797.25081375830359,2.3353641490252715E-2,2.8783452794923421,-50709.310220417705,1413.2185180100992,8.3739653410712638,2.3697112004753284E-2,3.1489566830060247,-50690.440112552082,1397.6320923513422]
["KBM","KBMS-35H04-A (240 V)",25.6,10.86,22.612734314496489,9.2675140633182327,1250,92.3,1633,1.35,11,147,4.46,325,10,797.25081375830359,1394.9802415319041,1533.3333333333335,22.266258714013073,0.5605381165919282,0.48622657493762439,0.36752194141167766,1.7171901054177272,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.42148582027214077,0.59960271580135838,5.0578298432656892,14.390465179232601,9.1612546666666645,563.74892615777185,456.99863460725584,4396.3268649218007,5.9753067325012302E-2,13.458705545314521,-48709.542954376884,797.25081375830359,2.3757481830311865E-2,3.1941524044677023,-50687.123422845034,1394.9802415319041,9.2927425071913241,2.3697112004753284E-2,3.1489566830060247,-50690.440112552082,1397.6320923513422]
["KBM","KBMS-35H04-A (400 V)",25.6,10.86,20.136560191191975,8.252688602947531,2300,92.3,2721,1.35,11,147,4.46,565,10,797.25081375830359,1391.477483174896,1533.3333333333335,22.294672402331425,0.5605381165919282,0.48609763609427825,0.36752194141167766,1.7171901054177272,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.42148582027214077,0.59960271580135838,5.0578298432656892,14.390465179232601,9.1612546666666645,563.74892615777185,456.99863460725584,4396.3268649218007,5.9753067325012302E-2,13.458705545314521,-48709.542954376884,797.25081375830359,2.3838075192890107E-2,3.2535100364082781,-50682.695661564518,1391.477483174896,9.4654315713351913,2.3697112004753284E-2,3.1489566830060247,-50690.440112552082,1397.6320923513422]
["KBM","KBMS-35H04-A (480 V)",25.6,10.86,18.416500557776462,7.5477461302362556,2800,92.3,3266,1.35,11,147,4.46,679,10,797.25081375830359,1392.7110587860036,1533.3333333333335,22.026950316440068,0.5605381165919282,0.48780510898220814,0.36752194141167766,1.7171901054177272,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.42148582027214077,0.59960271580135838,5.0578298432656892,14.390465179232601,9.1612546666666645,563.74892615777185,456.99863460725584,4396.3268649218007,5.9753067325012302E-2,13.458705545314521,-48709.542954376884,797.25081375830359,2.3809581926142995E-2,3.2326490793862059,-50684.2610681839,1392.7110587860036,9.4047408222686926,2.3697112004753284E-2,3.1489566830060247,-50690.440112552082,1397.6320923513422]
["KBM","KBMS-35H04-B (120 V)",25.9,13.3,23.708598419206478,11.795322596620139,725,93,948,0.9,7.6,122,4.46,160,10,948,948,948,23.034553519183092,0.5605381165919282,0.48594420120123327,0.36475564722900911,2.5316455696202533,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.51020532323022572,0.72581444668204853,6.1224638787627086,17.419546720369166,11.089627867867867,563.74892615777185,456.99863460725584,4396.3268649218007,4.1970652956830092E-2,9.0823407759937265,-49419.630001826154,982.30006368449688,1.6114264472895878E-2,1.9356167095968675,-50742.229805723087,1715.4713721687658,10.177858181545439,1.634456079289957E-2,2.1090163196788394,-50730.449743404468,1698.4275609899603]
["KBM","KBMS-35H04-B (240 V)",25.9,13.3,22.117403059351133,11.003683114105042,1550,93,1984,0.9,7.6,122,4.46,325,10,982.30006368449688,1698.77569460319,1847.5409836065576,21.754333067577626,0.5605381165919282,0.48079209894860264,0.36475564722900911,1.4130717465519196,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.51020532323022572,0.72581444668204853,6.1224638787627086,17.419546720369166,11.089627867867867,563.74892615777185,456.99863460725584,4396.3268649218007,4.1970652956830092E-2,9.0823407759937265,-49419.630001826154,982.30006368449688,1.6339742780307309E-2,2.105534896333241,-50730.696193233052,1698.77569460319,11.07132185051136,1.634456079289957E-2,2.1090163196788394,-50730.449743404468,1698.4275609899603]
["KBM","KBMS-35H04-B (400 V)",25.9,13.3,18.327948183424581,9.1183821808082506,2850,93,3307,0.9,7.6,122,4.46,565,10,982.30006368449688,1698.3676971462471,1847.5409836065576,21.387674313547631,0.5605381165919282,0.48269483453025308,0.36475564722900911,1.4130717465519196,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.51020532323022572,0.72581444668204853,6.1224638787627086,17.419546720369166,11.089627867867867,563.74892615777185,456.99863460725584,4396.3268649218007,4.1970652956830092E-2,9.0823407759937265,-49419.630001826154,982.30006368449688,1.6345389756531888E-2,2.1096147370263223,-50730.407340454876,1698.3676971462471,11.09277446546948,1.634456079289957E-2,2.1090163196788394,-50730.449743404468,1698.4275609899603]
["KBM","KBMS-35H04-B (480 V)",25.9,13.3,16.149545696089383,8.0345998488006884,3400,93,3968,0.9,7.6,122,4.46,679,10,982.30006368449688,1700.6926037962082,1847.5409836065576,21.022786612260678,0.5605381165919282,0.48456328726434889,0.36475564722900911,1.4130717465519196,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.51020532323022572,0.72581444668204853,6.1224638787627086,17.419546720369166,11.089627867867867,563.74892615777185,456.99863460725584,4396.3268649218007,4.1970652956830092E-2,9.0823407759937265,-49419.630001826154,982.30006368449688,1.6313298141186483E-2,2.0863229510742642,-50732.048883092932,1700.6926037962082,10.970301615839901,1.634456079289957E-2,2.1090163196788394,-50730.449743404468,1698.4275609899603]
["KBM","KBMS-35H04-C (120 V)",25.3,14.7,22.977994908892388,13.055678925507038,800,93,1080,0.73,6.1,107,4.46,160,10,1080,1080,1080,22.165293127004723,0.5605381165919282,0.49699948545470868,0.36475564722900911,2.2222222222222223,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.57728453360707244,0.82124085198744778,6.9274144032848692,19.709780447698748,12.547635942028982,563.74892615777185,456.99863460725584,4396.3268649218007,3.3788718806741905E-2,7.3104990884043923,-49638.171683955778,1108.6926798853096,1.2400311866245146E-2,1.5085844718894212,-50755.465111607438,1963.2218640588205,11.150706067605258,1.265359760995686E-2,1.6975757971110943,-50742.233901936037,1936.568616471418]
["KBM","KBMS-35H04-C (240 V)",25.3,14.7,21.088029959676135,11.98183520436144,1800,93,2260,0.73,6.1,107,4.46,325,10,1108.6926798853096,1945.4068157994236,2106.5420560747662,20.747780430894988,0.5605381165919282,0.49179211848641097,0.36475564722900911,1.2393054289875827,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.57728453360707244,0.82124085198744778,6.9274144032848692,19.709780447698748,12.547635942028982,563.74892615777185,456.99863460725584,4396.3268649218007,3.3788718806741905E-2,7.3104990884043923,-49638.171683955778,1108.6926798853096,1.2567767633986471E-2,1.6359805007345241,-50746.717511599629,1945.4068157994236,12.092354147843505,1.265359760995686E-2,1.6975757971110943,-50742.233901936037,1936.568616471418]
["KBM","KBMS-35H04-C (400 V)",25.3,14.7,16.14699240823229,9.1744275046774373,3300,93,3766,0.73,6.1,107,4.46,565,10,1108.6926798853096,1950.8429174938979,2106.5420560747662,19.889066656312753,0.5605381165919282,0.49579682191769153,0.36475564722900911,1.2393054289875827,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.57728453360707244,0.82124085198744778,6.9274144032848692,19.709780447698748,12.547635942028982,563.74892615777185,456.99863460725584,4396.3268649218007,3.3788718806741905E-2,7.3104990884043923,-49638.171683955778,1108.6926798853096,1.2515877998179374E-2,1.5975908173003031,-50749.428136528906,1950.8429174938979,11.808596702383872,1.265359760995686E-2,1.6975757971110943,-50742.233901936037,1936.568616471418]
["KBM","KBMS-35H04-C (480 V)",25.3,14.7,11.206042017217307,6.3670693279643791,4150,93,4520,0.73,6.1,107,4.46,679,10,1108.6926798853096,1961.6972221313283,2106.5420560747662,18.637812476226394,0.5605381165919282,0.50166077779557106,0.36475564722900911,1.2393054289875827,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.57728453360707244,0.82124085198744778,6.9274144032848692,19.709780447698748,12.547635942028982,563.74892615777185,456.99863460725584,4396.3268649218007,3.3788718806741905E-2,7.3104990884043923,-49638.171683955778,1108.6926798853096,1.2414348855613594E-2,1.5196736009905196,-50754.731843533336,1961.6972221313283,11.232671394344443,1.265359760995686E-2,1.6975757971110943,-50742.233901936037,1936.568616471418]
["KBM","KBMS-35H04-D (120 V)",24.7,19.2,21.838826104261813,16.544565230501373,1150,91.5,1443,0.43,3.4,80,4.46,160,10,1443,1443,1443,21.109848755173736,0.5605381165919282,0.50570174642663268,0.37073524800325514,1.6632016632016633,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.77232018244779965,1.0986971722201733,9.2678421893735958,26.368732133284158,16.786856248313089,563.74892615777185,456.99863460725584,4396.3268649218007,1.842450150702819E-2,4.2378388639899969,-50103.625693861562,1538.0607915377375,6.8523671680789603E-3,0.82197089025594117,-50778.767963108279,2662.8881176600112,13.795497521956513,7.0698153330586069E-3,1.0002036644973069,-50766.08158709087,2609.8749726121382]
["KBM","KBMS-35H04-D (240 V)",24.7,19.2,18.65932552809381,14.13585267279834,2500,91.5,3015,0.43,3.4,80,4.46,325,10,1538.0607915377375,2651.5927657377051,2817.5,18.293036508046846,0.5605381165919282,0.50500816429499951,0.37073524800325514,0.91958428092741884,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.77232018244779965,1.0986971722201733,9.2678421893735958,26.368732133284158,16.786856248313089,563.74892615777185,456.99863460725584,4396.3268649218007,1.842450150702819E-2,4.2378388639899969,-50103.625693861562,1538.0607915377375,6.8969165776905442E-3,0.86149476284299809,-50776.168858343524,2651.5927657377051,14.458843989327262,7.0698153330586069E-3,1.0002036644973069,-50766.08158709087,2609.8749726121382]
["KBM","KBMS-35H04-D (400 V)",24.7,19.2,10.111019914073351,7.6598635712676897,4250,91.5,5025,0.43,3.4,80,4.46,565,10,1538.0607915377375,2678.5802802892445,2817.5,15.505234266424562,0.5605381165919282,0.51502064057411656,0.37073524800325514,0.91958428092741884,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.77232018244779965,1.0986971722201733,9.2678421893735958,26.368732133284158,16.786856248313089,563.74892615777185,456.99863460725584,4396.3268649218007,1.842450150702819E-2,4.2378388639899969,-50103.625693861562,1538.0607915377375,6.7921574168157851E-3,0.76531656833161232,-50782.280724618642,2678.5802802892445,12.844643219230727,7.0698153330586069E-3,1.0002036644973069,-50766.08158709087,2609.8749726121382]
["KBM","KBMS-35H04-E (120 V)",24.7,20.7,22.042959618227506,17.776580337280247,1200,92.1,1536,0.37,2.8,75,4.46,160,10,1536,1536,1536,21.298988311331208,0.5605381165919282,0.50306386724196928,0.36832003466121443,1.5625,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.83265769670153389,1.1845328887998743,9.9918923604184062,28.428789331196981,18.09832939271255,563.74892615777185,456.99863460725584,4396.3268649218007,1.5228744898188632E-2,3.7098524518699181,-50193.470879349101,1697.7575592320368,5.9685492522624731E-3,0.70166664701121984,-50783.278396287649,2858.7416502983324,14.598465857056212,6.1530214277205515E-3,0.86988552261819518,-50771.528852335083,2802.7207624982243]
["KBM","KBMS-35H04-E (240 V)",24.7,20.7,18.657856405542191,15.046658391566282,2600,92.1,3208,0.37,2.8,75,4.46,325,10,1697.7575592320368,2848.7353950153893,3005.333333333333,18.07981987719328,0.5605381165919282,0.50411754100324024,0.36832003466121443,0.85631077919469356,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.83265769670153389,1.1845328887998743,9.9918923604184062,28.428789331196981,18.09832939271255,563.74892615777185,456.99863460725584,4396.3268649218007,1.5228744898188632E-2,3.7098524518699181,-50193.470879349101,1697.7575592320368,6.0001059279082489E-3,0.7331845305496828,-50781.268464185006,2848.7353950153893,15.254208507334369,6.1530214277205515E-3,0.86988552261819518,-50771.528852335083,2802.7207624982243]
["KBM","KBMS-35H04-E (400 V)",24.7,20.7,6.8402026628842849,5.5162924700679721,4600,92.1,5347,0.37,2.8,75,4.46,565,10,1697.7575592320368,2890.0138037304619,3005.333333333333,13.479334600849356,0.5605381165919282,0.51957993985990347,0.36832003466121443,0.85631077919469356,33.922275192297846,0,-27.477042905761255,0,0,0,0,0,0.83265769670153389,1.1845328887998743,9.9918923604184062,28.428789331196981,18.09832939271255,563.74892615777185,456.99863460725584,4396.3268649218007,1.5228744898188632E-2,3.7098524518699181,-50193.470879349101,1697.7575592320368,5.8741866991641771E-3,0.59758372088385781,-50789.288608734874,2890.0138037304619,12.432977373536342,6.1530214277205515E-3,0.86988552261819518,-50771.528852335083,2802.7207624982243]
["KBM","KBMS-45H01-A (120 V)",30.7,10.24,28.329579870357374,9.1979155423238232,450,118,617,1.36,21,187,8.35,160,10,479.53169465658493,617,617,27.449890622245555,0.29940119760479045,0.65626712805883602,0.4481500655518601,3.8897893030794166,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.51662472648445101,0.73494664387571051,6.1994967178134122,17.638719453017053,11.229157563035347,878.83273689825057,712.41884848975928,6853.4693224714847,0.1754392238223442,17.337430403901937,-48656.210265877329,479.53169465658493,4.0759937258039378E-2,3.5201974444966071,-50716.568747403129,1073.1241711247278,7.9914554190812712,4.6402822579877406E-2,4.9463895729009986,-50630.242431532904,992.61910364253345]
["KBM","KBMS-45H01-A (240 V)",30.7,10.24,27.341143907997175,8.876994775323757,950,118,1293,1.36,21,187,8.35,325,10,479.53169465658493,1052.4571686788902,1205.3475935828876,26.978892449906173,0.29940119760479045,0.63863156396646292,0.4481500655518601,2.417845869773124,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.51662472648445101,0.73494664387571051,6.1994967178134122,17.638719453017053,11.229157563035347,878.83273689825057,712.41884848975928,6853.4693224714847,0.1754392238223442,17.337430403901937,-48656.210265877329,479.53169465658493,4.2066060005506556E-2,3.8970127987425323,-50696.587344551153,1052.4571686788902,8.8468912723710993,4.6402822579877406E-2,4.9463895729009986,-50630.242431532904,992.61910364253345]
["KBM","KBMS-45H01-A (400 V)",30.7,10.24,24.99187334951591,8.1142445939986718,1750,118,2155,1.36,21,187,8.35,565,10,479.53169465658493,1047.2058019565332,1205.3475935828876,27.284238087605914,0.29940119760479045,0.63592950943091087,0.4481500655518601,2.417845869773124,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.51662472648445101,0.73494664387571051,6.1994967178134122,17.638719453017053,11.229157563035347,878.83273689825057,712.41884848975928,6853.4693224714847,0.1754392238223442,17.337430403901937,-48656.210265877329,479.53169465658493,4.2412967152124142E-2,3.9911202918014097,-50691.280269498493,1047.2058019565332,9.0605315147834293,4.6402822579877406E-2,4.9463895729009986,-50630.242431532904,992.61910364253345]
["KBM","KBMS-45H01-A (480 V)",30.7,10.24,23.64587725936731,7.6772328764179578,2100,118,2586,1.36,21,187,8.35,679,10,479.53169465658493,1047.3409933308415,1205.3475935828876,27.181870515118135,0.29940119760479045,0.63688712413017556,0.4481500655518601,2.417845869773124,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.51662472648445101,0.73494664387571051,6.1994967178134122,17.638719453017053,11.229157563035347,878.83273689825057,712.41884848975928,6853.4693224714847,0.1754392238223442,17.337430403901937,-48656.210265877329,479.53169465658493,4.2403958722057919E-2,3.9887046032730966,-50691.418082786389,1047.3409933308415,9.0550474851274849,4.6402822579877406E-2,4.9463895729009986,-50630.242431532904,992.61910364253345]
["KBM","KBMS-45H01-B (120 V)",30.2,12.5,27.738432938873189,11.184851991481125,525,118,763,0.92,14,150,8.35,160,10,597.25158995064908,763,763,26.622522537829035,0.29940119760479045,0.66184278735307067,0.4481500655518601,3.145478374836173,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.64108656737766478,0.9120051692728941,7.6930388085319779,21.888124062549458,13.934412558253618,878.83273689825057,712.41884848975928,6853.4693224714847,0.11863570911371593,11.674137148365727,-49290.876909346087,597.25158995064908,2.6081583394117362E-2,2.253304883711269,-50748.744634456038,1352.3798138490158,9.4271462404130411,3.0325136257966758E-2,3.3306452523839098,-50681.902246697478,1239.0315923434393]
["KBM","KBMS-45H01-B (240 V)",30.2,12.5,26.101410667070837,10.52476236575437,1200,118,1596,0.92,14,150,8.35,325,10,597.25158995064908,1326.9262066387062,1502.6666666666665,25.667895336572034,0.29940119760479045,0.6485649428452418,0.4481500655518601,1.9369966148004072,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.64108656737766478,0.9120051692728941,7.6930388085319779,21.888124062549458,13.934412558253618,878.83273689825057,712.41884848975928,6853.4693224714847,0.11863570911371593,11.674137148365727,-49290.876909346087,597.25158995064908,2.6926995681427965E-2,2.5051686787858269,-50735.428109898123,1326.9262066387062,10.480868196104467,3.0325136257966758E-2,3.3306452523839098,-50681.902246697478,1239.0315923434393]
["KBM","KBMS-45H01-B (400 V)",30.2,12.5,23.09597313705644,9.3128923939743711,2150,118,2660,0.92,14,150,8.35,565,10,597.25158995064908,1321.9778421769961,1502.6666666666665,25.831922742771376,0.29940119760479045,0.64742958680623353,0.4481500655518601,1.9369966148004072,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.64108656737766478,0.9120051692728941,7.6930388085319779,21.888124062549458,13.934412558253618,878.83273689825057,712.41884848975928,6853.4693224714847,0.11863570911371593,11.674137148365727,-49290.876909346087,597.25158995064908,2.7098209603148116E-2,2.553152794580817,-50732.731231194717,1321.9778421769961,10.681619226329564,3.0325136257966758E-2,3.3306452523839098,-50681.902246697478,1239.0315923434393]
["KBM","KBMS-45H01-B (480 V)",30.2,12.5,20.720171836492035,8.3549079985854977,2650,118,3192,0.92,14,150,8.35,679,10,597.25158995064908,1324.4550434025214,1502.6666666666665,25.462035388019853,0.29940119760479045,0.65022269962146317,0.4481500655518601,1.9369966148004072,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.64108656737766478,0.9120051692728941,7.6930388085319779,21.888124062549458,13.934412558253618,878.83273689825057,712.41884848975928,6853.4693224714847,0.11863570911371593,11.674137148365727,-49290.876909346087,597.25158995064908,2.7012215260138975E-2,2.5291659660443817,-50734.085772402257,1324.4550434025214,10.581265589282344,3.0325136257966758E-2,3.3306452523839098,-50681.902246697478,1239.0315923434393]
["KBM","KBMS-45H01-C (120 V)",31.3,14.3,28.427521373798537,12.69085775616006,650,119,854,0.69,11,135,8.35,160,10,690.06011825454971,854,854,27.526005004959924,0.29940119760479045,0.63425073256269004,0.4443840986144495,2.810304449648712,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.70762848559161229,1.0066672265870724,8.491541827099347,24.160013438089738,15.380742255354395,878.83273689825057,712.41884848975928,6853.4693224714847,9.1764589441662964E-2,8.7716672376422391,-49749.712179315145,690.06011825454971,2.1178724465777999E-2,1.7579500767345217,-50762.767839886277,1507.2380653410978,10.895898550988722,2.4110704680730823E-2,2.4815371491854252,-50720.687755517327,1399.8507538330218]
["KBM","KBMS-45H01-C (240 V)",31.3,14.3,26.601611916788226,11.875719605709028,1400,119,1783,0.69,11,135,8.35,325,10,690.06011825454971,1483.712906364894,1669.6296296296296,26.320672115591197,0.29940119760479045,0.62402717716704736,0.4443840986144495,1.7144684841783346,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.70762848559161229,1.0066672265870724,8.491541827099347,24.160013438089738,15.380742255354395,878.83273689825057,712.41884848975928,6853.4693224714847,9.1764589441662964E-2,8.7716672376422391,-49749.712179315145,690.06011825454971,2.1759408902453769E-2,1.9230029197534693,-50754.433796579149,1483.712906364894,11.918907711992507,2.4110704680730823E-2,2.4815371491854252,-50720.687755517327,1399.8507538330218]
["KBM","KBMS-45H01-C (400 V)",31.3,14.3,22.23076245107594,9.9244475228017581,2500,119,2972,0.69,11,135,8.35,565,10,690.06011825454971,1484.3099827312062,1669.6296296296296,25.915376068148529,0.29940119760479045,0.62660833669865046,0.4443840986144495,1.7144684841783346,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.70762848559161229,1.0066672265870724,8.491541827099347,24.160013438089738,15.380742255354395,878.83273689825057,712.41884848975928,6853.4693224714847,9.1764589441662964E-2,8.7716672376422391,-49749.712179315145,690.06011825454971,2.1744263003364156E-2,1.9188782020437625,-50754.651172094949,1484.3099827312062,11.893342420741508,2.4110704680730823E-2,2.4815371491854252,-50720.687755517327,1399.8507538330218]
["KBM","KBMS-45H01-C (480 V)",31.3,14.3,18.621128341751753,8.3130037239963173,3100,119,3567,0.69,11,135,8.35,679,10,690.06011825454971,1490.1016224630982,1669.6296296296296,25.205546055175127,0.29940119760479045,0.63104921600054054,0.4443840986144495,1.7144684841783346,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,0.70762848559161229,1.0066672265870724,8.491541827099347,24.160013438089738,15.380742255354395,878.83273689825057,712.41884848975928,6853.4693224714847,9.1764589441662964E-2,8.7716672376422391,-49749.712179315145,690.06011825454971,2.1598458333455972E-2,1.8787077315129486,-50756.743775851217,1490.1016224630982,11.644363011461429,2.4110704680730823E-2,2.4815371491854252,-50720.687755517327,1399.8507538330218]
["KBM","KBMS-45H01-D (120 V)",29.7,20.2,26.335954793732576,17.326286048508273,950,118,1263,0.35,5,91.2,8.35,160,10,1048.7004131235039,1263,1263,25.227590425772888,0.29940119760479045,0.66141392537283272,0.4481500655518601,1.9002375296912113,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,1.0534369011799882,1.4986118073083807,12.641242814159858,35.966683375401139,22.897101783264745,878.83273689825057,712.41884848975928,6853.4693224714847,4.1426920880529877E-2,4.4371124731678089,-50213.3923677856,1048.7004131235039,9.3177884450733398E-3,0.7712583916681478,-50787.28071542691,2293.6265575984912,13.950070176828415,1.1012444818804911E-2,1.26591348081932,-50756.992025812033,2090.1643272769002]
["KBM","KBMS-45H01-D (240 V)",29.7,20.2,22.804629703024432,15.003045857252916,2100,118,2635,0.35,5,91.2,8.35,325,10,1048.7004131235039,2270.0641660044325,2471.4912280701756,22.246222370240201,0.29940119760479045,0.658687443967782,0.4481500655518601,1.1482350783044695,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,1.0534369011799882,1.4986118073083807,12.641242814159858,35.966683375401139,22.897101783264745,878.83273689825057,712.41884848975928,6853.4693224714847,4.1426920880529877E-2,4.4371124731678089,-50213.3923677856,1048.7004131235039,9.487473219304883E-3,0.83411003830130548,-50784.247929819903,2270.0641660044325,15.08689395824022,1.1012444818804911E-2,1.26591348081932,-50756.992025812033,2090.1643272769002]
["KBM","KBMS-45H01-D (400 V)",29.7,20.2,12.723792477454767,8.3709161035886623,3700,118,4392,0.35,5,91.2,8.35,565,10,1048.7004131235039,2300.8000233390912,2471.4912280701756,19.143551712410453,0.29940119760479045,0.67273295369383801,0.4481500655518601,1.1482350783044695,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,1.0534369011799882,1.4986118073083807,12.641242814159858,35.966683375401139,22.897101783264745,878.83273689825057,712.41884848975928,6853.4693224714847,4.1426920880529877E-2,4.4371124731678089,-50213.3923677856,1048.7004131235039,9.2674453760484918E-3,0.75160088563732597,-50788.180499958798,2300.8000233390912,13.594516718229052,1.1012444818804911E-2,1.26591348081932,-50756.992025812033,2090.1643272769002]
["KBM","KBMS-45H01-E (120 V)",31.2,23.4,27.345712949425653,19.960374415639162,1100,118,1394,0.26,3.2,82.7,8.35,160,10,1394,1394,1394,26.315567137726692,0.29940119760479045,0.62754129567309491,0.4481500655518601,1.7216642754662841,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,1.1616488600883283,1.6525533667224839,13.939786321059941,39.661280801339615,25.24915555555555,878.83273689825057,712.41884848975928,6853.4693224714847,2.3330214601692188E-2,3.2959662470946212,-50408.064925000006,1400.9686551999566,7.3944621436201289E-3,0.60474750594073823,-50791.791669883081,2580.2849494917887,16.238077171734723,8.1815980062316471E-3,0.94034310145483313,-50772.837743287186,2434.3272763361506]
["KBM","KBMS-45H01-E (240 V)",31.2,23.4,23.167423890072417,16.910528386914173,2300,118,2909,0.26,3.2,82.7,8.35,325,10,1400.9686551999566,2570.180814292889,2725.5139056831922,22.223837823007269,0.29940119760479045,0.6274315461519987,0.4481500655518601,0.98589866010628791,52.881707735119491,0,-42.834183265446789,0,0,0,0,0,1.1616488600883283,1.6525533667224839,13.939786321059941,39.661280801339615,25.24915555555555,878.83273689825057,712.41884848975928,6853.4693224714847,2.3330214601692188E-2,3.2959662470946212,-50408.064925000006,1400.9686551999566,7.4433264022535153E-3,0.63080018008223715,-50790.615037467644,2570.180814292889,16.937617606517719,8.1815980062316471E-3,0.94034310145483313,-50772.837743287186,2434.3272763361506]
["KBM","KBMS-45H02-A (120 V)",43.7,13.3,40.226411866476546,12.00788413924673,400,171,568,0.95,16,202,11.5,160,10,471.75861347407425,568,568,38.767504850396691,0.21739130434782608,0.60289663675708571,0.39903193914445945,4.225352112676056,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,0.60824998751703052,0.86529208542738756,7.2989998502043658,20.767010050257301,13.220689210950079,1133.9777250300008,919.25012708356053,8843.1862225438526,0.18337496924834726,17.298239926827986,-48971.828068289229,471.75861347407425,4.6470749084153162E-2,3.4486836413234689,-50732.290802997675,1008.3989870857157,10.37570833073457,5.0004399070453072E-2,4.3942999509506553,-50686.851304413023,963.8200098588585]
["KBM","KBMS-45H02-A (240 V)",43.7,13.3,38.46847317687061,11.483126321453913,880,171,1188,0.95,16,202,11.5,325,10,471.75861347407425,992.25944653367333,1115.841584158416,37.801100102222236,0.21739130434782608,0.58471596522794245,0.39903193914445945,2.490091485392024,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,0.60824998751703052,0.86529208542738756,7.2989998502043658,20.767010050257301,13.220689210950079,1133.9777250300008,919.25012708356053,8843.1862225438526,0.18337496924834726,17.298239926827986,-48971.828068289229,471.75861347407425,4.7682013201227801E-2,3.7994249293404705,-50716.715057140886,992.25944653367333,11.430948440440311,5.0004399070453072E-2,4.3942999509506553,-50686.851304413023,963.8200098588585]
["KBM","KBMS-45H02-A (400 V)",43.7,13.3,34.85493253712508,10.40445747376868,1600,171,1980,0.95,16,202,11.5,565,10,471.75861347407425,988.66035844987675,1115.841584158416,38.234520269775466,0.21739130434782608,0.58204542759145217,0.39903193914445945,2.490091485392024,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,0.60824998751703052,0.86529208542738756,7.2989998502043658,20.767010050257301,13.220689210950079,1133.977725030001,919.25012708356053,8843.1862225438526,0.18337496924834726,17.298239926827986,-48971.828068289229,471.75861347407425,4.7962522526375923E-2,3.8761275825780945,-50713.107964437171,988.66035844987675,11.661716014668038,5.0004399070453072E-2,4.3942999509506553,-50686.851304413023,963.8200098588585]
["KBM","KBMS-45H02-A (480 V)",43.7,13.3,32.565549894187811,9.7210596699068095,1950,171,2376,0.95,16,202,11.5,679,10,471.75861347407425,989.02339229579593,1115.841584158416,38.052701735898125,0.21739130434782608,0.58320744525705559,0.39903193914445945,2.490091485392024,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,0.60824998751703052,0.86529208542738756,7.2989998502043658,20.767010050257301,13.220689210950079,1133.977725030001,919.25012708356053,8843.1862225438526,0.18337496924834726,17.298239926827986,-48971.828068289229,471.75861347407425,4.7934054675732467E-2,3.8684126565047201,-50713.474034892381,989.02339229579593,11.638504890930461,5.0004399070453072E-2,4.3942999509506553,-50686.851304413023,963.8200098588585]
["KBM","KBMS-45H02-B (120 V)",43.5,14.9,39.894839068368434,13.387529888714239,450,171,638,0.76,12,180,11.5,160,10,557.13240006989486,638,638,38.388682945820136,0.21739130434782608,0.60132940458753692,0.39903193914445945,3.761755485893417,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,0.68455589728107169,0.97384432734307291,8.2146707673728603,23.372263856233751,14.879245295870581,1133.977725030001,919.25012708356053,8843.1862225438526,0.13397977436369921,13.878414256467329,-49318.968778749113,557.13240006989486,3.6289237271611513E-2,2.7156165340823661,-50748.257429319594,1145.7313129837742,11.460979071405355,3.8955152613184926E-2,3.5255560880435985,-50709.253011343048,1096.5812026415604]
["KBM","KBMS-45H02-B (240 V)",43.5,14.9,37.515093728803905,12.588957627115404,1050,171,1334,0.76,12,180,11.5,325,10,557.13240006989486,1129.1917172487395,1252.2222222222224,37.063708009576509,0.21739130434782608,0.58599273497351689,0.39903193914445945,2.1886204087929166,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,0.68455589728107169,0.97384432734307291,8.2146707673728603,23.372263856233751,14.879245295870581,1133.977725030001,919.25012708356053,8843.1862225438526,0.13397977436369921,13.878414256467329,-49318.968778749113,557.13240006989486,3.7136536454360783E-2,2.9968614605942676,-50735.860782299424,1129.1917172487395,12.647944232442363,3.8955152613184926E-2,3.5255560880435985,-50709.253011343048,1096.5812026415604]
["KBM","KBMS-45H02-B (400 V)",43.5,14.9,32.769165125026028,10.996364135914774,1900,171,2223,0.76,12,180,11.5,565,10,557.13240006989486,1127.0591717112945,1252.2222222222224,37.134586386337453,0.21739130434782608,0.58565605413105037,0.39903193914445945,2.1886204087929166,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,0.68455589728107169,0.97384432734307291,8.2146707673728603,23.372263856233751,14.879245295870581,1133.977725030001,919.25012708356053,8843.1862225438526,0.13397977436369921,13.878414256467329,-49318.968778749113,557.13240006989486,3.7249432466540382E-2,3.0323664469678828,-50734.209025704506,1127.0591717112945,12.797789359930526,3.8955152613184926E-2,3.5255560880435985,-50709.253011343048,1096.5812026415604]
["KBM","KBMS-45H02-B (480 V)",43.5,14.9,29.257419325829272,9.8179259482648558,2350,171,2667,0.76,12,180,11.5,679,10,557.13240006989486,1128.6333311467222,1252.2222222222224,36.659722863653087,0.21739130434782608,0.58833458382124149,0.39903193914445945,2.1886204087929166,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,0.68455589728107169,0.97384432734307291,8.2146707673728603,23.372263856233751,14.879245295870581,1133.977725030001,919.25012708356053,8843.1862225438526,0.13397977436369921,13.878414256467329,-49318.968778749113,557.13240006989486,3.7166016470976615E-2,3.0061731680795543,-50735.429466693822,1128.6333311467222,12.68724333202749,3.8955152613184926E-2,3.5255560880435985,-50709.253011343048,1096.5812026415604]
["KBM","KBMS-45H02-C (120 V)",41.8,21.1,37.242256683503506,18.345939252957393,750,168,941,0.38,5.9,123,11.5,160,10,816.6548455372232,941,941,36.081551385569064,0.21739130434782608,0.6140542481601271,0.40615750948632479,2.5504782146652496,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,1.0088302082775629,1.4351546447638797,12.105962499330754,34.443711474333114,21.9275477582846,1133.977725030001,919.25012708356053,8843.1862225438526,6.6603654677383994E-2,6.8653833220766289,-50026.300059504138,816.6548455372232,1.6849227101612949E-2,1.2550498107189336,-50779.13134596825,1699.167589429333,15.502852932498188,1.8570459495418717E-2,1.7751677567601594,-50753.087480920076,1606.0744062914357]
["KBM","KBMS-45H02-C (240 V)",41.8,21.1,33.243488738319641,16.376102826758444,1600,168,1964,0.38,5.9,123,11.5,325,10,816.6548455372232,1684.2634607386785,1832.520325203252,32.792862956595478,0.21739130434782608,0.60892068655654863,0.40615750948632479,1.4943267824943471,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,1.0088302082775629,1.4351546447638797,12.105962499330754,34.443711474333114,21.9275477582846,1133.977725030001,919.25012708356053,8843.1862225438526,6.6603654677383994E-2,6.8653833220766289,-50026.300059504138,816.6548455372232,1.7101270865780924E-2,1.3438517137153592,-50775.317686752998,1684.2634607386785,16.599767836211008,1.8570459495418717E-2,1.7751677567601594,-50753.087480920076,1606.0744062914357]
["KBM","KBMS-45H02-C (400 V)",41.8,21.1,22.654882933908411,11.160040854142075,2900,168,3274,0.38,5.9,123,11.5,565,10,816.6548455372232,1694.1594566655176,1832.520325203252,30.615558232245704,0.21739130434782608,0.61780268287364759,0.40615750948632479,1.4943267824943471,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,1.0088302082775629,1.4351546447638797,12.105962499330754,34.443711474333114,21.9275477582846,1133.977725030001,919.25012708356053,8843.1862225438526,6.6603654677383994E-2,6.8653833220766289,-50026.300059504138,816.6548455372232,1.6932930363397134E-2,1.285221417039321,-50777.864836889144,1694.1594566655176,15.875544097045879,1.8570459495418717E-2,1.7751677567601594,-50753.087480920076,1606.0744062914357]
["KBM","KBMS-45H02-C (480 V)",41.8,21.1,12.34587629984274,6.0817124629767196,3500,168,3929,0.38,5.9,123,11.5,679,10,816.6548455372232,1711.5710246249303,1832.520325203252,27.396335805454967,0.21739130434782608,0.6311178668141022,0.40615750948632479,1.4943267824943471,68.234461593702562,0,-55.269913890899076,0,0,0,0,0,1.0088302082775629,1.4351546447638797,12.105962499330754,34.443711474333114,21.9275477582846,1133.977725030001,919.25012708356053,8843.1862225438526,6.6603654677383994E-2,6.8653833220766289,-50026.300059504138,816.6548455372232,1.6646256994103024E-2,1.1786846936420958,-50782.202474601327,1711.5710246249303,14.559561941890365,1.8570459495418717E-2,1.7751677567601594,-50753.087480920076,1606.0744062914357]
["KBM","KBMS-45H03-A (120 V)",54.6,14.1,50.202016335272141,12.67727685234145,350,218,480,0.93,16,240,14.5,160,10,420.09343880998574,480,480,48.568479545516077,0.17241379310344829,0.59521737321911872,0.38007399970279937,5,82.856131935210257,0,-67.113466867520316,0,0,0,0,0,0.6266993732115087,0.89153804966915795,7.5203924785381044,21.396913192059792,13.621698005698002,1376.9729518221438,1116.2322971728952,10738.154698803251,0.22442625491965246,21.763953091181758,-48749.302126062677,420.09343880998574,6.3981788594328931E-2,4.2567366993775222,-50726.515002917418,857.76450527617283,11.010878491285714,6.7366995075168898E-2,5.2660631805702218,-50684.797927856962,829.18697018255079]
["KBM","KBMS-45H03-A (240 V)",54.6,14.1,47.7464829275686,12.05719265847692,800,218,1005,0.93,16,240,14.5,325,10,420.09343880998574,845.45340929537463,939.16666666666674,47.357088281811023,0.17241379310344829,0.57403186571095066,0.38007399970279937,2.8944014876061361,82.856131935210257,0,-67.113466867520316,0,0,0,0,0,0.6266993732115087,0.89153804966915795,7.5203924785381044,21.396913192059792,13.621698005698002,1376.9729518221438,1116.2322971728952,10738.154698803251,0.22442625491965246,21.763953091181758,-48749.302126062677,420.09343880998574,6.5382656457737678E-2,4.7007755050305633,-50709.25162175046,845.45340929537463,12.159471340633489,6.7366995075168898E-2,5.2660631805702218,-50684.797927856962,829.18697018255079]
["KBM","KBMS-45H03-A (400 V)",54.6,14.1,43.688031878725276,11.032331282506384,1400,218,1676,0.93,16,240,14.5,565,10,420.09343880998574,842.43721267173737,939.16666666666674,48.033822850821764,0.17241379310344829,0.5701111108353325,0.38007399970279937,2.8944014876061361,82.856131935210257,0,-67.113466867520316,0,0,0,0,0,0.6266993732115087,0.89153804966915795,7.5203924785381044,21.396913192059792,13.621698005698002,1376.9729518221438,1116.2322971728952,10738.154698803251,0.22442625491965246,21.763953091181758,-48749.302126062677,420.09343880998574,6.5739111114154175E-2,4.8072207952014292,-50704.858907231697,842.43721267173737,12.434812814352654,6.7366995075168898E-2,5.2660631805702218,-50684.797927856962,829.18697018255079]
["KBM","KBMS-45H03-A (480 V)",54.6,14.1,40.837285986285153,10.312445956132615,1700,218,2011,0.93,16,240,14.5,679,10,420.09343880998574,842.74446721172285,939.16666666666674,47.777381712426219,0.17241379310344829,0.57163444644888251,0.38007399970279937,2.8944014876061361,82.856131935210257,0,-67.113466867520316,0,0,0,0,0,0.6266993732115087,0.89153804966915795,7.5203924785381044,21.396913192059792,13.621698005698002,1376.9729518221441,1116.2322971728952,10738.154698803251,0.22442625491965246,21.763953091181758,-48749.302126062677,420.09343880998574,6.5702561246474944E-2,4.7964148864867981,-50705.309323943962,842.74446721172285,12.406861226963626,6.7366995075168898E-2,5.2660631805702218,-50684.797927856962,829.18697018255079]
["KBM","KBMS-45H03-B (120 V)",53,19.899999999999999,49.482718670389282,18.125537974501569,550,216,699,0.47,7.7,165,14.5,160,10,631.50799271040523,699,699,48.529855182912925,0.17241379310344829,0.5811257356451387,0.38359320340375119,3.4334763948497855,82.856131935210257,0,-67.113466867520316,0,0,0,0,0,0.9111922079074436,1.2962555232002233,10.934306494889324,31.110132556805357,19.805325506638709,1376.9729518221441,1116.2322971728952,10738.154698803251,0.10741161384298485,10.893649239278348,-49715.430029858318,631.50799271040523,3.0448237839317795E-2,2.1840804263589897,-50761.356443445322,1255.8088089125165,16.260211761317287,3.200693785127097E-2,2.6602620194420967,-50740.173829090119,1218.2097604849421]
["KBM","KBMS-45H03-B (240 V)",53,19.899999999999999,45.50447416401321,16.668305554583593,1150,216,1459,0.47,7.7,165,14.5,325,10,631.50799271040523,1251.007800616648,1366.0606060606062,44.846120616919045,0.17241379310344829,0.58176944578311274,0.38359320340375119,1.9701040640526584,82.856131935210257,0,-67.113466867520316,0,0,0,0,0,0.9111922079074436,1.2962555232002233,10.934306494889324,31.110132556805357,19.805325506638709,1376.9729518221438,1116.2322971728952,10738.154698803251,0.10741161384298485,10.893649239278348,-49715.430029858318,631.50799271040523,3.0637044428291536E-2,2.2471382337896437,-50758.790576292391,1251.007800616648,16.72966942855901,3.200693785127097E-2,2.6602620194420967,-50740.173829090119,1218.2097604849421]
["KBM","KBMS-45H03-B (400 V)",53,19.899999999999999,33.533576381687716,12.283361311973522,2150,216,2432,0.47,7.7,165,14.5,565,10,631.50799271040523,1259.4171223184646,1366.0606060606062,41.59704780688044,0.17241379310344829,0.59539190450236013,0.38359320340375119,1.9701040640526584,82.856131935210257,0,-67.113466867520316,0,0,0,0,0,0.9111922079074436,1.2962555232002233,10.934306494889324,31.110132556805357,19.805325506638709,1376.9729518221438,1116.2322971728952,10738.154698803251,0.10741161384298485,10.893649239278348,-49715.430029858318,631.50799271040523,3.0308306886185656E-2,2.1361454810693878,-50763.258094432575,1259.4171223184646,15.903341953882833,3.200693785127097E-2,2.6602620194420967,-50740.173829090119,1218.2097604849421]
["KBM","KBMS-45H03-B (480 V)",53,19.899999999999999,24.699622899069141,9.0474809154099418,2600,216,2918,0.47,7.7,165,14.5,679,10,631.50799271040523,1266.5079289798316,1366.0606060606062,39.21436461867377,0.17241379310344829,0.60562730613845328,0.38359320340375119,1.9701040640526584,82.856131935210257,0,-67.113466867520316,0,0,0,0,0,0.9111922079074436,1.2962555232002233,10.934306494889324,31.110132556805357,19.805325506638709,1376.9729518221438,1116.2322971728952,10738.154698803251,0.10741161384298485,10.893649239278348,-49715.430029858318,631.50799271040523,3.0038275754119954E-2,2.0404624264551954,-50766.92779693503,1266.5079289798316,15.190993309931969,3.200693785127097E-2,2.6602620194420967,-50740.173829090119,1218.2097604849421]
["KBM","KBMS-43H01-A (400 V)",6.12,5.12,4.82490774847009,3.9875270648513141,4750,18,5478,2.9,6.8,72.8,2.85,565,16,1896.8785658498336,2816.8139686512054,3096.1538461538462,5.3519928537260233,0.8771929824561403,1.5282464641116102,1.448628450501225,1.2073160769990061,26.07531210902205,0,-21.12100280830786,0,0,0,0,0,0.63893428060479096,0.90894334149096467,7.6672113672574911,21.814640195783152,13.88763127572016,433.34148777932177,351.28486999264641,3379.3604493292582,1.0819322829054226E-2,5.5065685307322925,-49374.819792387549,1896.8785658498336,5.7989557818424724E-3,1.6558939002490234,-50675.817198666286,2816.8139686512054,4.5283762270662802,9.9941595909412567E-3,5.0782979958515684,-49588.655797294356,1987.880428102653]
["KBM","KBMS-43H02-A (400 V)",11.6,5.12,9.9780405138429078,4.3194980579406526,2450,34.5,2866,3.55,12,139,3.73,565,16,984.94694917748541,1459.5207812695735,1621.5827338129495,10.63376180554139,0.67024128686327078,0.94435243298018945,0.88012566403471437,1.8732039913588383,30.364335409197647,0,-24.595111681450092,0,0,0,0,0,0.39253997223956222,0.55842455924961187,4.7104796668747468,13.402189421990686,8.5320987790549179,504.62008763835053,409.06630655218447,3935.2178690320147,3.6897123643143917E-2,13.014720551425221,-48613.465069203332,984.94694917748541,2.0997656441988408E-2,4.019715707631188,-50596.085490784943,1459.5207812695735,4.7031795437564767,2.4838885889625677E-2,7.2922182030573488,-50117.094600680597,1281.2272507806367]
["KBM","KBMS-43H02-A (480 V)",11.6,5.12,6.8754935415698784,2.9764041305497306,3000,34.5,3439,3.55,12,139,3.73,679,16,984.94694917748541,1480.8192652450364,1621.5827338129495,9.2679532725273592,0.67024128686327078,0.98010004694695874,0.88012566403471437,1.8732039913588383,30.364335409197647,0,-24.595111681450092,0,0,0,0,0,0.39253997223956222,0.55842455924961187,4.7104796668747468,13.402189421990686,8.5320987790549179,504.62008763835053,409.06630655218447,3935.2178690320147,3.6897123643143917E-2,13.014720551425221,-48613.465069203332,984.94694917748541,2.0663480418773313E-2,3.59689100587434,-50637.75633419415,1480.8192652450364,4.2084628442340541,2.4838885889625677E-2,7.2922182030573488,-50117.094600680597,1281.2272507806367]
["KBM","KBMS-43H03-A (400 V)",21,4.78,18.636530433018713,4.2068917456024186,1240,64.5,1491,4.83,19,268,5.69,565,16,516.13441815621945,752.96615612258472,841.04477611940297,19.564828552449509,0.43936731107205623,0.69663336734746084,0.61887069817544205,3.3203895664175289,39.917160032316012,0,-32.332899626175966,0,0,0,0,0,0.26611930015074198,0.37857941459220351,3.193431601808904,9.0859059502128847,5.7842673777777796,663.37696914255048,537.76132434388308,5173.2639401881552,0.11278233636413708,32.916289147443393,-47033.850649232503,516.13441815621945,7.5642368385846689E-2,10.050290784184755,-50453.577155662912,752.96615612258472,4.4826628423743733,7.8181734609906586E-2,12.968534811631828,-50219.760637807332,722.8067526394002]
["KBM","KBMS-43H03-A (480 V)",21,4.78,16.182532804310163,3.652941942282204,1490,64.5,1790,4.83,19,268,5.69,679,16,516.13441815621945,757.24208613911549,841.04477611940297,18.551685295858437,0.43936731107205623,0.71799932838033775,0.61887069817544205,3.3203895664175289,39.917160032316012,0,-32.332899626175966,0,0,0,0,0,0.26611930015074198,0.37857941459220351,3.193431601808904,9.0859059502128847,5.7842673777777796,663.37696914255059,537.76132434388308,5173.2639401881552,0.11278233636413708,32.916289147443393,-47033.850649232503,516.13441815621945,7.5326703404229728E-2,9.625901132897086,-50482.642552418729,757.24208613911549,4.2933752126563274,7.8181734609906586E-2,12.968534811631828,-50219.760637807332,722.8067526394002]
["KBM","KBMS-43S01-A (240 V)",6.12,5.12,4.9618894022767375,4.1007350432039154,2550,18,3284,2.9,6.8,72.8,2.85,325,16,{"$f":"IF(AQ1376<I1376,IF(AQ1376<0,0,AQ1376),I1376)","v":1896.8785658498336},{"$f":"IF(AU1376<I1376,IF(AU1376<0,0,AU1376),I1376)","v":2849.3683876121727},{"$f":"IF(UAC_V*0.98/L1376*1000<I1376,IF(UAC_V*0.98/L1376*1000<0,0,UAC_V*0.98/L1376*1000),I1376)","v":3096.1538461538462},{"$f":"C1376+(E1376-C1376)/G1376*Q1376","v":4.825927950387725},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M1376,(inertia/gear^2+gear_inertia)/M1376),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M1376,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M1376))","v":0.8771929824561403},{"$f":"IF((C1376+(E1376-C1376)/G1376*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X1376^2*time1+Y1376^2*time2+Z1376^2*time3+AA1376^2*time4)/time)/(C1376+(E1376-C1376)/G1376*mspeed),SQRT((((X1376-Y1376)*2/PI()+Y1376)^2*time1+Y1376^2*time2+((Z1376-Y1376)*2/PI()+Y1376)^2*time3+AA1376^2*time4)/time)/(C1376+(E1376-C1376)/G1376*mspeed)),IF(AccType=1,SQRT((X1376^2*time1+Y1376^2*time2+Z1376^2*time3+AA1376^2*time4+AB1376^2*time5+AC1376^2*time6+AD1376^2*time7+AE1376^2*time8)/time)/(C1376+(E1376-C1376)/G1376*mspeed),SQRT((((X1376-Y1376)*2/PI()+Y1376)^2*time1+Y1376^2*time2+((Z1376-Y1376)*2/PI()+Y1376)^2*time3+AA1376^2*time4+((AB1376-AC1376)*2/PI()+AC1376)^2*time5+AC1376^2*time6+((AD1376-AC1376)*2/PI()+AC1376)^2*time7+AE1376^2*time8)/time)/(C1376+(E1376-C1376)/G1376*mspeed))))","v":1.5494232436120423},{"$f":"IF(move1,MAX(ABS(X1376),ABS(Z1376))/H1376,MAX(ABS(X1376),ABS(Z1376),ABS(AB1376),ABS(AD1376))/H1376)","v":1.448628450501225},{"$f":"IF(AZ1376>0,speed/(MIN(AZ1376,I1376)),\"NA\")","v":1.2073160769990061},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M1376+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M1376+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":26.07531210902205},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M1376+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M1376+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-21.12100280830786},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M1376+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M1376+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M1376+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M1376+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH1376/Irms","v":0.63893428060479096},{"$f":"AI1376/Ipeak","v":0.90894334149096467},{"$f":"IF(move1,IF(AccType=1,SQRT((X1376^2*time1+Y1376^2*time2+Z1376^2*time3+AA1376^2*time4)/time)/(C1376/D1376),SQRT((((X1376-Y1376)*2/PI()+Y1376)^2*time1+Y1376^2*time2+((Z1376-AA1376)*2/PI()+AA1376)^2*time3+AA1376^2*time4)/time)/(C1376/D1376)),IF(AccType=1,SQRT((X1376^2*time1+Y1376^2*time2+Z1376^2*time3+AA1376^2*time4+AB1376^2*time5+AC1376^2*time6+AD1376^2*time7+AE1376^2*time8)/time)/(C1376/D1376),SQRT((((X1376-Y1376)*2/PI()+Y1376)^2*time1+Y1376^2*time2+((Z1376-AA1376)*2/PI()+AA1376)^2*time3+AA1376^2*time4+((AB1376-AC1376)*2/PI()+AC1376)^2*time5+AC1376^2*time6+((AD1376-AE1376)*2/PI()+AE1376)^2*time7+AE1376^2*time8)/time)/(C1376/D1376)))","v":7.6672113672574911},{"$f":"IF(move1,MAX(ABS(X1376),ABS(Z1376))/(C1376/D1376),MAX(ABS(X1376),ABS(Z1376),ABS(AB1376),ABS(AD1376))/(C1376/D1376))","v":21.814640195783152},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X1376),ABS(Z1376))/(C1376/D1376),MAX(ABS((X1376-Y1376)*2/PI()+Y1376),ABS((Z1376-Y1376)*2/PI()+Y1376))/(C1376/D1376)),IF(AccType=1,MAX(ABS(X1376),ABS(Z1376),ABS(AB1376),ABS(AD1376))/(C1376/D1376),MAX(ABS((X1376-Y1376)*2/PI()+Y1376),ABS((Z1376-Y1376)*2/PI()+Y1376),ABS((AB1376-AC1376)*2/PI()+AC1376),ABS((AD1376-AC1376)*2/PI()+AC1376))/(C1376/D1376)))","v":13.88763127572016},{"$f":"IF((C1376+(E1376-C1376)/G1376*mspeed)<0,\"NA\",U1376*(C1376+(E1376-C1376)/G1376*mspeed)*mspeed/9.55)","v":433.34148777932177},{"$f":"IF(move1,IF(speed1>speed2,AM1376/2*time1/time,AM1376/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z1376*-speed/30*PI(),((Z1376-AA1376)*2/PI()+AA1376)*-speed/30*PI()),IF(AccType=1,X1376*-speed/30*PI(),((X1376-Y1376)*2/PI()+Y1376)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z1376*-speed/30*PI(),((Z1376-AA1376)*2/PI()+AA1376)*-speed/30*PI()),IF(AccType=1,X1376*-speed/30*PI(),((X1376-Y1376)*2/PI()+Y1376)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD1376*-speed/30*PI(),((AD1376-AE1376)*2/PI()+AE1376)*-speed/30*PI()),IF(AccType=1,AB1376*-speed/30*PI(),((AB1376-AC1376)*2/PI()+AC1376)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD1376*-speed/30*PI(),((AD1376-AE1376)*2/PI()+AE1376)*-speed/30*PI()),IF(AccType=1,AB1376*-speed/30*PI(),((AB1376-AC1376)*2/PI()+AC1376)*-speed/30*PI()),0)/2*time7/time)))","v":351.28486999264641},{"$f":"IF(move1,MAX(IF(AccType=1,Z1376*-speed/30*PI(),((Z1376-AA1376)*2/PI()+AA1376)*-speed/30*PI()),IF(AccType=1,X1376*-speed/30*PI(),((X1376-Y1376)*2/PI()+Y1376)*-speed/30*PI()),0),MAX(IF(AccType=1,Z1376*-speed/30*PI(),((Z1376-AA1376)*2/PI()+AA1376)*-speed/30*PI()),IF(AccType=1,X1376*-speed/30*PI(),((X1376-Y1376)*2/PI()+Y1376)*-speed/30*PI()),IF(AccType=1,AD1376*-speed/30*PI(),((AD1376-AE1376)*2/PI()+AE1376)*-speed/30*PI()),IF(AccType=1,AB1376*-speed/30*PI(),((AB1376-AC1376)*2/PI()+AC1376)*-speed/30*PI()),0))","v":3379.3604493292582},{"$f":"(L1376^2)/1000000+((K1376/1000)^2*(D1376/C1376*H1376)^2*PI()*PI()*(O1376/2)^2)/1200","v":1.0819322829054226E-2},{"$f":"SQRT(3)*L1376*J1376*D1376/C1376*H1376/1000","v":5.5065685307322925},{"$f":"0.75*J1376^2*(D1376/C1376*H1376)^2-(UAC_V*0.98)^2","v":-49374.819792387549},{"$f":"-AO1376/2/AN1376+SQRT((AO1376/2/AN1376)^2-AP1376/AN1376)","v":1896.8785658498336},{"$f":"(L1376^2)/1000000+((K1376/1000)^2*AV1376^2*PI()*PI()*(O1376/2)^2)/1200","v":5.7146233570454646E-3},{"$f":"SQRT(3)*L1376*J1376*AV1376/1000","v":1.5095326688220665},{"$f":"0.75*J1376^2*AV1376^2-(UAC_V*0.98)^2","v":-50697.671430616727},{"$f":"-AS1376/2/AR1376+SQRT((AS1376/2/AR1376)^2-AT1376/AR1376)","v":2849.3683876121727},{"$f":"D1376+(F1376-D1376)*((0.85*UAC_V-D1376*J1376)/L1376*1000)/G1376","v":4.1281218865808755},{"$f":"(L1376^2)/1000000+((K1376/1000)^2*AJ1376^2*PI()*PI()*(O1376/2)^2)/1200","v":9.9941595909412567E-3},{"$f":"SQRT(3)*L1376*J1376*AJ1376/1000","v":5.0782979958515684},{"$f":"0.75*J1376^2*AJ1376^2-(UAC_V*0.98)^2","v":-49588.655797294356},{"$f":"IF(((AX1376/2/AW1376)^2-AY1376/AW1376)>0,-AX1376/2/AW1376+SQRT((AX1376/2/AW1376)^2-AY1376/AW1376),-9999)","v":1987.880428102653}]
["KBM","KBMS-43S02-A (240 V)",11.6,5.12,10.136945606160719,4.3882881411951162,1300,34.5,1717,3.55,12,139,3.73,325,16,984.94694917748541,1472.5696565426545,1621.5827338129495,9.9427311490468213,0.67024128686327078,0.96216820962751626,0.88012566403471437,1.8732039913588383,30.364335409197647,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-24.595111681450092,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0.39253997223956222,0.55842455924961187,4.7104796668747468,13.402189421990686,8.5320987790549179,504.62008763835053,409.06630655218447,3935.2178690320147,3.6897123643143917E-2,13.014720551425221,-48613.465069203332,984.94694917748541,2.078976691404967E-2,3.7622680842141545,-50622.00875087345,1472.5696565426545,4.401958640560502,2.4838885889625677E-2,7.2922182030573488,-50117.094600680597,1281.2272507806367]
["KBM","KBMS-43S03-A (240 V)",21,4.78,18.813539541609121,4.2468486549907727,670,64.5,893,4.83,19,268,5.69,325,16,516.13441815621945,757.81117804089718,841.04477611940297,18.526978842219354,0.43936731107205623,0.71850034806762142,0.61887069817544205,3.3203895664175289,39.917160032316012,0,-32.332899626175966,0,0,0,0,0,0.26611930015074198,0.37857941459220351,3.193431601808904,9.0859059502128847,5.7842673777777796,663.37696914255059,537.76132434388308,5173.2639401881552,0.11278233636413708,32.916289147443393,-47033.850649232503,516.13441815621945,7.52855363974477E-2,9.5691677022271637,-50486.433075457557,757.81117804089718,4.2680707864416467,7.8181734609906586E-2,12.968534811631828,-50219.760637807332,722.8067526394002]
["KBM","KBMS-57H01-A (400 V)",18.8,5.67,13.222102964557459,3.9468964073305846,1625,46.1,1975,3.39,13,203,9.49,565,24,687.34108812770512,992.00408804281051,1110.344827586207,15.394894361944079,0.26343519494204426,1.1906804266543218,1.2676343267872541,3.1151542572934185,58.437942464892416,0,-47.334733396562854,0,0,0,0,0,0.51621219694769338,0.73435978230483157,6.1945463633723206,17.624634775315958,11.220190978723403,971.17092307926509,787.27207312370649,7573.5573434500557,7.9900891930766382E-2,16.572289009537378,-49139.014479509133,687.34108812770512,4.5723503212507274E-2,5.6607959257214659,-50610.757014531628,992.00408804281051,4.7492073928576151,6.6407123158140999E-2,13.373855071836916,-49720.081500870576,770.42733738817299]
["KBM","KBMS-57H01-A (480 V)",18.8,5.67,10.713844949600761,3.1981626715226152,2050,46.1,2370,3.39,13,203,9.49,679,24,687.34108812770512,996.0959010546236,1110.344827586207,14.870933706831792,0.26343519494204426,1.2068529166171682,1.2676343267872541,3.1151542572934185,58.437942464892416,0,-47.334733396562854,0,0,0,0,0,0.51621219694769338,0.73435978230483157,6.1945463633723206,17.624634775315958,11.220190978723403,971.17092307926509,787.27207312370649,7573.5573434500557,7.9900891930766382E-2,16.572289009537378,-49139.014479509133,687.34108812770512,4.548664755345045E-2,5.5102970941131817,-50620.956463967872,996.0959010546236,4.6229442007077584,6.6407123158140999E-2,13.373855071836916,-49720.081500870576,770.42733738817299]
["KBM","KBMS-57H02-A (400 V)",33.5,5.22,26.795904964199107,4.1479729046747842,825,115,1023,4.4000000000000004,22,390,14.9,565,24,299.64593763009827,513.69061511031191,577.9487179487179,29.325659754304787,0.16778523489932887,0.99920155358113183,0.73744076504995315,5.3628112036219857,84.805687980744608,0,-68.692607264403136,0,0,0,0,0,0.38704263993984983,0.55060409360632689,4.6445116792781977,13.214498246551846,8.4126108656716383,1409.3723153944293,1142.4965865181396,10990.817162304502,0.33616593689141883,53.260034962049318,-46142.715351481398,299.64593763009827,0.16446873435830678,13.806301890528491,-50491.856298664679,513.69061511031191,4.6451469190034178,0.19266840697513485,25.003955165302148,-49777.550246698818,447.5264761099674]
["KBM","KBMS-57H02-A (480 V)",33.5,5.22,24.931661036070302,3.8593902532616569,1015,115,1228,4.4000000000000004,22,390,14.9,679,24,299.64593763009827,513.99539609941246,577.9487179487179,29.160998246621602,0.16778523489932887,1.0039970863727472,0.73744076504995315,5.3628112036219857,84.805687980744608,0,-68.692607264403136,0,0,0,0,0,0.38704263993984983,0.55060409360632689,4.6445116792781977,13.214498246551846,8.4126108656716383,1409.3723153944293,1142.4965865181396,10990.817162304502,0.33616593689141883,53.260034962049318,-46142.715351481398,299.64593763009827,0.16437215313642334,13.752293020248407,-50494.30272959439,513.99539609941246,4.6269755694726289,0.19266840697513485,25.003955165302148,-49777.550246698818,447.5264761099674]
["KBM","KBMS-57H03-A (400 V)",59.9,5.47,51.264644827494706,4.635139676988671,475,218,597,5.92,35,669,25.2,565,24,142.88386847746318,287.98760693244202,336.9207772795217,54.66447311338635,9.9206349206349215E-2,0.91797681053522551,0.61929704657456131,9.3512027804446483,135.00675615325437,0,-109.35547248413603,0,0,0,0,0,0.36109721759865715,0.51369432120082181,4.333166611183886,12.328663708819724,7.8486710839052742,2243.6559273807875,1818.8020371581879,17496.875597461767,1.0225387978968383,136.56061042339675,-40388.255757220395,142.88386847746318,0.4844357536686843,34.583144212086097,-50137.098069004038,287.98760693244202,5.0414564952408689,0.53693461792095909,53.839941735916504,-49185.973271192714,256.65147643027376]
["KBM","KBMS-57H03-A (480 V)",59.9,5.47,49.392913373346836,4.465905368295374,580,218,717,5.92,35,669,25.2,679,24,142.88386847746318,287.91670281223924,336.9207772795217,54.684197003950771,9.9206349206349215E-2,0.91746363756295313,0.61929704657456131,9.3512027804446483,135.00675615325437,0,-109.35547248413603,0,0,0,0,0,0.36109721759865715,0.51369432120082181,4.333166611183886,12.328663708819724,7.8486710839052742,2243.6559273807875,1818.8020371581879,17496.875597461767,1.0225387978968383,136.56061042339675,-40388.255757220395,142.88386847746318,0.48452998794970797,34.627305026771914,-50135.390821375688,287.91670281223924,5.0478941639695307,0.53693461792095909,53.839941735916504,-49185.973271192714,256.65147643027376]
["KBM","KBMS-57S01-A (240 V)",18.8,5.67,16.00592325412811,4.7778875385457047,880,46.1,1183,3.39,13,203,9.49,325,24,687.34108812770512,990.68594895974593,1110.344827586207,15.654485713124487,0.26343519494204426,1.182709266410396,1.2676343267872541,3.1151542572934185,58.437942464892416,0,-47.334733396562854,0,0,0,0,0,0.51621219694769338,0.73435978230483157,6.1945463633723206,17.624634775315958,11.220190978723403,971.17092307926509,787.27207312370649,7573.5573434500557,7.9900891930766382E-2,16.572289009537378,-49139.014479509133,687.34108812770512,4.5800775357941317E-2,5.7090366624020508,-50607.429530850968,990.68594895974593,4.7896796632391219,6.6407123158140999E-2,13.373855071836916,-49720.081500870576,770.42733738817299]
["KBM","KBMS-57S02-A (240 V)",33.5,5.22,29.506253494564866,4.5675315007066359,445,115,612,4.4000000000000004,22,390,14.9,325,24,299.64593763009827,514.92663543445417,577.9487179487179,28.878682132984668,0.16778523489932887,1.0122029824391543,0.73744076504995315,5.3628112036219857,84.805687980744608,0,-68.692607264403136,0,0,0,0,0,0.38704263993984983,0.55060409360632689,4.6445116792781977,13.214498246551846,8.4126108656716383,1409.3723153944293,1142.4965865181396,10990.817162304502,0.33616593689141883,53.260034962049318,-46142.715351481398,299.64593763009827,0.16407890047024132,13.586988648813465,-50501.730906405355,514.92663543445417,4.5713587143757834,0.19266840697513485,25.003955165302148,-49777.550246698818,447.5264761099674]
["KBM","KBMS-57S03-A (240 V)",59.9,5.47,53.858032742297389,4.8696232135892759,250,218,357,5.92,35,669,25.2,325,24,142.88386847746318,289.71365913646429,336.9207772795217,52.898238229553073,9.9206349206349215E-2,0.9686481063788116,0.61929704657456131,9.3512027804446483,135.00675615325437,0,-109.35547248413603,0,0,0,0,0,0.36109721759865715,0.51369432120082181,4.333166611183886,12.328663708819724,7.8486710839052742,2243.6559273807875,1818.8020371581879,17496.875597461767,1.0225387978968383,136.56061042339675,-40388.255757220395,142.88386847746318,0.4821748343261375,33.506168416324158,-50178.059268511402,289.71365913646429,4.8844572765618537,0.53693461792095909,53.839941735916504,-49185.973271192714,256.65147643027376]
["KBM","KBMS-79H01-A (400 V)",43.4,4.95,35.571129781038607,4.0102739324733498,600,152,744,6.26,23,534,44.5,565,32,191.54687770136559,364.30310807945347,422.09737827715355,38.646530410802825,5.6179775280898875E-2,2.1465402779801579,1.5070581273045209,12.057696037954575,229.07283535028719,0,-185.54899663373263,0,0,0,0,0,0.76523917772600747,1.0886237855068372,9.1828701327120896,26.126970852164096,16.632946236559139,3806.9252197435744,3086.0539980662397,29687.839461397227,0.61991499195707211,100.37724576294784,-41971.756996946213,191.54687770136559,0.30738606527786633,25.866610186547256,-50218.567465963555,364.30310807945347,4.4674870332490269,0.59329914028911035,96.304238457291817,-42674.078815631685,199.04300062345308]
["KBM","KBMS-79H01-A (480 V)",43.4,4.95,33.814974895278034,3.8122857830076704,730,152,894,6.26,23,534,44.5,679,32,191.54687770136559,364.26805538908837,422.09737827715355,38.617098005818271,5.6179775280898875E-2,2.1486628413665763,1.5070581273045209,12.057696037954575,229.07283535028719,0,-185.54899663373263,0,0,0,0,0,0.76523917772600747,1.0886237855068372,9.1828701327120896,26.126970852164096,16.632946236559139,3806.9252197435744,3086.0539980662397,29687.839461397227,0.61991499195707211,100.37724576294784,-41971.756996946213,191.54687770136559,0.30740967172264577,25.880340615969299,-50217.944554420574,364.26805538908837,4.4698584501050256,0.59329914028911035,96.304238457291817,-42674.078815631685,199.04300062345308]
["KBM","KBMS-79H02-A (400 V)",79.31,5.39,67.254331666546648,4.5137135346675601,350,319,443,6.4,32,901,71.5,565,32,93.79572222971683,213.7642201999553,250.16648168701445,71.946941313457287,3.4965034965034968E-2,1.9882673088209846,1.1306202771907725,18.329613415704117,360.66786842385642,0,-292.14097342332371,0,0,0,0,0,0.71792058166018424,1.021308688902506,8.6150469799222105,24.511408533660145,15.604447321107513,5993.8822608728615,4858.8935288702487,46742.555747731793,1.8251555411105096,216.52940908268576,-36366.589156376664,93.79572222971683,0.86447186435544343,49.36525723278848,-50054.690173755836,213.7642201999553,4.9426062277964666,1.3367960445766682,155.85250381667478,-43324.87759522142,130.93565835620794]
["KBM","KBMS-79H02-A (480 V)",79.31,5.39,64.846386115581552,4.3521064507101714,430,319,532,6.4,32,901,71.5,679,32,93.79572222971683,213.6332443666272,250.16648168701445,72.124165675826731,3.4965034965034968E-2,1.9769473770904875,1.1306202771907725,18.329613415704117,360.66786842385642,0,-292.14097342332371,0,0,0,0,0,0.71792058166018424,1.021308688902506,8.6150469799222105,24.511408533660145,15.604447321107513,5993.8822608728615,4858.8935288702487,46742.555747731793,1.8251555411105096,216.52940908268576,-36366.589156376664,93.79572222971683,0.86481507303783378,49.525830585396328,-50049.800036421067,213.6332443666272,4.9586833414814038,1.3367960445766682,155.85250381667478,-43324.87759522142,130.93565835620794]
["KBM","KBMS-79H03-A (400 V)",143,6.76,122.74824985962429,5.7358995261506687,240,637,307,5.75,34,1300,125,565,32,48.817590135076571,145.97233775161973,173.38461538461539,130.68251953519859,0.02,2.0821630526473616,0.97554315465318198,26.770324577396966,621.42098951407695,0,-503.35100150640233,0,0,0,0,0,0.86040853985595511,1.2240110399519699,10.324902478271461,29.376264958847276,18.70151111111111,10327.297138666079,8371.7422287967111,80536.160241024365,3.8970718944828411,389.87188259144398,-28319.940349793389,48.817590135076571,1.7849519374055203,80.865930881079564,-49837.808109872261,145.97233775161973,6.2458818678877535,2.5412746445054744,242.1299564851185,-42132.539315460745,89.651509194864076]
["KBM","KBMS-79H03-A (480 V)",143,6.76,119.2070523758296,5.5704230082163368,300,637,369,5.75,34,1300,125,679,32,48.817590135076571,145.80028675714135,173.38461538461539,131.43660471199436,0.02,2.0376684915735739,0.97554315465318198,26.770324577396966,621.42098951407695,0,-503.35100150640233,0,0,0,0,0,0.86040853985595511,1.2240110399519699,10.324902478271461,29.376264958847276,18.70151111111111,10327.297138666079,8371.7422287967111,80536.160241024365,3.8970718944828411,389.87188259144398,-28319.940349793389,48.817590135076571,1.7860608431013156,81.33676064324743,-49826.510794092173,145.80028675714135,6.2822475789151921,2.5412746445054744,242.1299564851185,-42132.539315460745,89.651509194864076]
["KBM","KBMS-79S01-A (240 V)",43.4,4.95,38.505228167394037,4.3410629275528798,310,152,445,6.26,23,534,44.5,325,32,191.54687770136559,366.1127368340741,422.09737827715355,37.619231252213851,5.6179775280898875E-2,2.2198039803564007,1.5070581273045209,12.057696037954575,229.07283535028719,0,-185.54899663373263,0,0,0,0,0,0.76523917772600747,1.0886237855068372,9.1828701327120896,26.126970852164096,16.632946236559139,3806.9252197435744,3086.0539980662397,29687.839461397227,0.61991499195707211,100.37724576294784,-41971.756996946213,191.54687770136559,0.30618225174627411,25.1564919603668,-50250.332916095052,366.1127368340741,4.3448407357768932,0.59329914028911035,96.304238457291817,-42674.078815631685,199.04300062345308]
["KBM","KBMS-79S02-A (240 V)",79.31,5.39,71.354466152866408,4.7888903458299605,180,319,265,6.4,32,901,71.5,325,32,93.79572222971683,214.97911098746613,250.16648168701445,69.80848003395846,3.4965034965034968E-2,2.1357953849078131,1.1306202771907725,18.329613415704117,360.66786842385642,0,-292.14097342332371,0,0,0,0,0,0.71792058166018424,1.021308688902506,8.6150469799222105,24.511408533660145,15.604447321107513,5993.8822608728624,4858.8935288702487,46742.555747731793,1.8251555411105096,216.52940908268576,-36366.589156376664,93.79572222971683,0.86133671346589058,47.873523515160137,-50099.360717368982,214.97911098746613,4.7932491135775495,1.3367960445766682,155.85250381667478,-43324.87759522142,130.93565835620794]
["KBM","KBMS-79S03-A (240 V)",143,6.76,128.72451797272495,6.0151643912488302,125,637,184,5.75,34,1300,125,325,32,48.817590135076571,146.93547280583758,173.38461538461539,126.21940239032884,0.02,2.3888323256981328,0.97554315465318198,26.770324577396966,621.42098951407695,0,-503.35100150640233,0,0,0,0,0,0.86040853985595511,1.2240110399519699,10.324902478271461,29.376264958847276,18.70151111111111,10327.297138666077,8371.7422287967111,80536.160241024365,3.8970718944828411,389.87188259144398,-28319.940349793389,48.817590135076571,1.7788562180345515,78.227164246503733,-49899.910114489729,146.93547280583758,6.0420701452387959,2.5412746445054744,242.1299564851185,-42132.539315460745,89.651509194864076]
["KBM","KBMS-118H01-A (400 V)",325,43.7,109.48238123518914,14.443585914932603,785,994,872,0.27600000000000002,2.5,648,315,565,38,231.32211547105618,328.01792284710729,347.83950617283955,234.94440554880509,7.9365079365079361E-3,2.7055459856410859,1.5568009166427539,10.326879411525132,1547.4601111428974,0,-1253.442690025747,0,0,0,0,0,6.0943258972980887,8.6697444688390544,73.131910767577068,208.07386725213729,132.463938005698,25716.99483550181,20847.279667787894,200550.83040411954,0.75139721169624418,41.402748804354658,-49784.576956877951,231.32211547105618,0.44029615513584347,10.268888048746637,-50742.377755869384,328.01792284710729,33.149631414508413,0.74551648037931006,41.033860463416538,-49802.682228574187,232.4032173089503]
["KBM","KBMS-118H02-A (400 V)",445,46.5,239.54167706034417,24.797275058006644,590,1451,685,0.29199999999999998,2.7,585,403,565,38,217.13250714153182,357.05822193806449,385.29914529914532,320.66002801489805,6.2034739454094297E-3,2.4140060585869763,1.3620692220265034,10.099221905067173,1976.3624411604565,0,-1600.8535773399699,0,0,0,0,0,6.04877833407149,8.6049488308952444,72.585340008857884,206.51877194148588,131.47393358302119,32844.854821404668,26625.423323741703,256136.57237439518,0.83981762885279965,44.860044415419679,-49335.057300786459,217.13250714153182,0.3688322205999065,10.373432498918758,-50726.550823427846,357.05822193806449,35.060906484434838,0.71636362275748233,38.899050599170003,-49699.793546996283,237.64207010797799]
["KBM","KBMS-118H02-A (480 V)",445,46.5,139.13728616498514,14.403445772772789,710,1451,822,0.29199999999999998,2.7,585,403,679,38,217.13250714153182,359.91803363160557,385.29914529914532,289.94999081024645,6.2034739454094297E-3,2.773303632011404,1.3620692220265034,10.099221905067173,1976.3624411604565,0,-1600.8535773399699,0,0,0,0,0,6.04877833407149,8.6049488308952444,72.585340008857884,206.51877194148588,131.47393358302119,32844.854821404668,26625.423323741703,256136.57237439518,0.83981762885279965,44.860044415419679,-49335.057300786459,217.13250714153182,0.36500550643311303,9.5985231668077571,-50737.856583399996,359.91803363160557,32.441809707173157,0.71636362275748233,38.899050599170003,-49699.793546996283,237.64207010797799]
["KBM","KBMS-118H03-A (400 V)",560,44,374.83733148884318,29.284166522565872,435,1932,516,0.373,4.3,775,591,565,38,141.981121710824,261.34914300757691,290.83870967741939,448.75378222439798,4.2301184433164128E-3,2.7643145391379456,1.4972328067089054,16.297030124647947,2892.6537825616051,0,-2343.0495638749003,0,0,0,0,0,6.6568572157881531,9.4699975024338272,79.882286589457834,227.27994005841185,144.6909037037037,48072.555700378965,38969.639316006658,374887.93021998403,1.8656705274531626,76.005134736652323,-48400.672796530002,141.981121710824,0.67249754012753904,18.116377114668204,-50668.55100114012,261.34914300757691,36.182634969798372,1.7499558675571656,72.445662919420215,-48620.613038154319,147.26609582504196]
["KBM","KBMS-118H03-A (480 V)",560,44,302.72162633703306,23.650127057580708,535,1932,619,0.373,4.3,775,591,679,38,141.981121710824,262.42226839189476,290.83870967741939,433.80266462651718,4.2301184433164128E-3,2.9654081587204284,1.4972328067089054,16.297030124647947,2892.6537825616051,0,-2343.0495638749003,0,0,0,0,0,6.6568572157881531,9.4699975024338272,79.882286589457834,227.27994005841185,144.6909037037037,48072.555700378965,38969.639316006658,374887.93021998403,1.8656705274531626,76.005134736652323,-48400.672796530002,141.981121710824,0.66868669123339874,17.629549869177804,-50675.794327329939,262.42226839189476,35.210327294514357,1.7499558675571656,72.445662919420215,-48620.613038154319,147.26609582504196]
["KBM","KBMS-118H04-A (400 V)",672,42.8,502.32108656444967,31.395067910278105,340,2400,413,0.45500000000000002,4.5,970,698,565,38,119.08036546919112,209.20004277275663,232.37113402061857,567.59754132837645,3.5816618911174787E-3,2.6866371391818595,1.4225666769758527,18.752078454620751,3414.1600247420465,0,-2765.4696200410576,0,0,0,0,0,6.3689304245944376,9.0603949069295364,76.427165095133248,217.44947776630889,138.43263703703701,56739.385455965414,45995.336715859594,442475.13920656923,2.3457249252312979,116.85020965642296,-47177.258125000008,119.08036546919112,1.0219373655408774,28.064741793375173,-50595.884377742375,209.20004277275663,36.712781758564624,2.0930995803426296,105.82353142755601,-47829.652559305207,127.98581265580239]
["KBM","KBMS-118H04-A (480 V)",672,42.8,450.74953525668928,28.17184595354308,420,2400,495,0.45500000000000002,4.5,970,698,679,38,119.08036546919112,209.38644199519712,232.37113402061857,561.69798189908181,3.5816618911174787E-3,2.7641329058947979,1.4225666769758527,18.752078454620751,3414.1600247420465,0,-2765.4696200410576,0,0,0,0,0,6.3689304245944376,9.0603949069295364,76.427165095133248,217.44947776630889,138.43263703703701,56739.385455965414,45995.336715859594,442475.13920656923,2.3457249252312979,116.85020965642296,-47177.258125000008,119.08036546919112,1.0209111664727109,27.886479770304874,-50598.534494106811,209.38644199519712,36.47958899317225,2.0930995803426296,105.82353142755601,-47829.652559305207,127.98581265580239]
["KBM","KBMS-118S01-A (240 V)",325,43.7,252.45952847951898,33.306006395714903,400,994,523,0.27600000000000002,2.5,648,315,325,38,231.32211547105618,325.43054421012215,347.83950617283955,265.98278718957749,7.9365079365079361E-3,2.2372136224082593,1.5568009166427539,10.326879411525132,1547.4601111428974,0,-1253.442690025747,0,0,0,0,0,6.0943258972980887,8.6697444688390544,73.131910767577068,208.07386725213729,132.463938005698,25716.99483550181,20847.279667787894,200550.83040411954,0.75139721169624418,41.402748804354658,-49784.576956877951,231.32211547105618,0.44441564226318797,11.25843593435734,-50729.69490578321,325.43054421012215,36.344052029406896,0.74551648037931006,41.033860463416538,-49802.682228574187,232.4032173089503]
["KBM","KBMS-118S02-A (240 V)",445,46.5,356.90495988357532,36.946683217761418,320,1451,411,0.29199999999999998,2.7,585,403,325,38,217.13250714153182,354.6390376474169,385.29914529914532,347.36893672375174,6.2034739454094297E-3,2.166080004861004,1.3620692220265034,10.099221905067173,1976.3624411604565,0,-1600.8535773399699,0,0,0,0,0,6.04877833407149,8.6049488308952444,72.585340008857884,206.51877194148588,131.47393358302119,32844.854821404668,26625.423323741703,256136.57237439518,0.83981762885279965,44.860044415419679,-49335.057300786459,217.13250714153182,0.37220374179896987,11.011067651591793,-50716.589899314829,354.6390376474169,37.216033677038425,0.71636362275748233,38.899050599170003,-49699.793546996283,237.64207010797799]
["KBM","KBMS-118S03-A (240 V)",560,44,467.30600312088416,36.508281493819069,235,1932,309,0.373,4.3,775,591,325,38,141.981121710824,260.84865766098193,290.83870967741939,457.11019293979314,4.2301184433164128E-3,2.6622712580903194,1.4972328067089054,16.297030124647947,2892.6537825616051,0,-2343.0495638749003,0,0,0,0,0,6.6568572157881531,9.4699975024338272,79.882286589457834,227.27994005841185,144.6909037037037,48072.555700378965,38969.639316006658,374887.93021998403,1.8656705274531626,76.005134736652323,-48400.672796530002,141.981121710824,0.67429870831617333,18.341975990994822,-50665.127499165777,260.84865766098193,36.633208599396397,1.7499558675571656,72.445662919420215,-48620.613038154319,147.26609582504196]
["KBM","KBMS-118S04-A (240 V)",672,42.8,577.08722068131567,36.067951292582229,185,2400,247,0.45500000000000002,4.5,970,698,325,38,119.08036546919112,209.61236455897944,232.37113402061857,564.46004270349181,3.5816618911174787E-3,2.7251717546684526,1.4225666769758527,18.752078454620751,3414.1600247420465,0,-2765.4696200410576,0,0,0,0,0,6.3689304245944376,9.0603949069295364,76.427165095133248,217.44947776630889,138.43263703703701,56739.385455965414,45995.336715859594,442475.13920656923,2.3457249252312979,116.85020965642296,-47177.258125000008,119.08036546919112,1.0196737539053293,27.670000364250672,-50601.730060538415,209.61236455897944,36.196402308320309,2.0930995803426296,105.82353142755601,-47829.652559305207,127.98581265580239]
["KBM","KBMS-60H01-A (400 V)",54,13.7,34.759439571269944,8.6038216760569171,1250,127,1639,0.91600000000000004,7.8,245,25.6,565,38,425.51109640473891,768.39983697363937,920,42.172445202625894,9.765625E-2,1.0230983121205999,1.0783961590455806,4.3238606222477403,136.95631219878874,0,-110.93461288101886,0,0,0,0,0,1.0176934896016474,1.4477634854347265,12.21232187521977,34.746323650433439,22.120196652949247,2276.0552909530738,1845.0663265034323,17749.538060963019,0.24755724953138974,12.524278422296174,-50151.859083718482,425.51109640473891,8.0535208997474628E-2,4.141901580262453,-50733.709151601084,768.39983697363937,10.655592158994134,0.14841291184423105,8.598271790576435,-50497.245473616735,555.05951964574899]
["KBM","KBMS-60H01-A (480 V)",54,13.7,24.858012674165401,6.1529734341993567,1600,127,1895,0.91600000000000004,7.8,245,25.6,679,38,425.51109640473891,778.03131885337325,920,39.829138229295388,9.765625E-2,1.0515722881463481,1.0783961590455806,4.3238606222477403,136.95631219878874,0,-110.93461288101886,0,0,0,0,0,1.0176934896016474,1.4477634854347265,12.21232187521977,34.746323650433439,22.120196652949247,2276.0552909530729,1845.0663265034323,17749.538060963019,0.24755724953138974,12.524278422296174,-50151.859083718482,425.51109640473891,7.8736807143685139E-2,3.9561486211320567,-50739.974194450297,778.03131885337325,10.177717990218161,0.14841291184423105,8.598271790576435,-50497.245473616735,555.05951964574899]
["KBM","KBMS-60H02-A (400 V)",108,16.399999999999999,88.643815200699777,13.055053785080968,725,255,974,0.92100000000000004,11,411,42,565,38,248.09239201627736,437.5373982077337,548.41849148418498,96.318545191291165,5.9523809523809521E-2,0.79452297163655883,0.85054160810077428,6.4395066210587961,216.88811006569745,0,-175.67936915321494,0,0,0,0,0,0.96463712589459194,1.3722858815885177,11.575645510735104,32.934861158124427,20.966983813443068,3604.4291974167882,2921.90218965846,28108.699064514385,0.70760195024155381,25.38764123306548,-49851.263907479173,248.09239201627736,0.24315859565985604,9.4247207819635346,-50673.700084095566,437.5373982077337,14.374952330202039,0.32685767525951659,13.746686844065005,-50525.485774787048,372.69936056147532]
["KBM","KBMS-60H02-A (480 V)",108,16.399999999999999,84.001439455620698,12.371346017028085,885,255,1169,0.92100000000000004,11,411,42,679,38,248.09239201627736,437.2598349232365,548.41849148418498,96.142817376236621,5.9523809523809521E-2,0.79609224624280439,0.85054160810077428,6.4395066210587961,216.88811006569745,0,-175.67936915321494,0,0,0,0,0,0.96463712589459194,1.3722858815885177,11.575645510735104,32.934861158124427,20.966983813443068,3604.4291974167882,2921.90218965846,28108.699064514385,0.70760195024155381,25.38764123306548,-49851.263907479173,248.09239201627736,0.2434379730817362,9.4424380961217125,-50673.205362626482,437.2598349232365,14.401975469914612,0.32685767525951659,13.746686844065005,-50525.485774787048,372.69936056147532]
["KBM","KBMS-60H03-A (400 V)",154,18.7,119.77083853017209,14.090686885902599,590,393,778,0.86699999999999999,11,515,52.9,565,38,197.44302257055318,359.8100791333855,437.66990291262135,133.12542830995218,4.725897920604915E-2,0.74256650400129265,0.68705728322266857,7.32537638506144,270.01351230650874,0,-218.71094496827206,0,0,0,0,0,0.96031678422750744,1.366139794407931,11.523801410730089,32.787355065790344,20.873078518518515,4487.311854761575,3637.6040743163758,34993.751194923534,1.0833844362918668,36.906289996527782,-49521.274392206804,197.44302257055318,0.3569693275733089,12.358649885316362,-50661.191457264751,359.8100791333855,15.980268615374387,0.4217501343306469,16.14259907939881,-50559.535054163251,327.6282164687529]
["KBM","KBMS-60H03-A (480 V)",154,18.7,110.74531456811052,13.028860537424766,720,393,930,0.86699999999999999,11,515,52.9,679,38,197.44302257055318,359.95803753497887,437.66990291262135,132.37517821908921,4.725897920604915E-2,0.74801203734992383,0.68705728322266857,7.32537638506144,270.01351230650874,0,-218.71094496827206,0,0,0,0,0,0.96031678422750744,1.366139794407931,11.523801410730089,32.787355065790344,20.873078518518515,4487.311854761575,3637.6040743163758,34993.751194923534,1.0833844362918668,36.906289996527782,-49521.274392206804,197.44302257055318,0.35671293022980582,12.341368479004204,-50661.593805321376,359.95803753497887,15.957923009868736,0.4217501343306469,16.14259907939881,-50559.535054163251,327.6282164687529]
["KBM","KBMS-60S01-A (240 V)",54,13.7,44.708070377632424,11.066354053869413,660,127,983,0.91600000000000004,7.8,245,25.6,325,38,425.51109640473891,767.09292517104143,920,43.200343220446371,9.765625E-2,1.0103587452291956,1.0783961590455806,4.3238606222477403,136.95631219878874,0,-110.93461288101886,0,0,0,0,0,1.0176934896016474,1.4477634854347265,12.21232187521977,34.746323650433439,22.120196652949247,2276.0552909530738,1845.0663265034323,17749.538060963019,0.24755724953138974,12.524278422296174,-50151.859083718482,425.51109640473891,8.0784825673562197E-2,4.1670295788612481,-50732.83956888337,767.09292517104143,10.720237274203166,0.14841291184423105,8.598271790576435,-50497.245473616735,555.05951964574899]
["KBM","KBMS-60S02-A (240 V)",108,16.399999999999999,95.989033210228826,14.136823742301742,385,255,584,0.92100000000000004,11,411,42,325,38,248.09239201627736,443.24378540842082,548.41849148418498,94.171983412174015,5.9523809523809521E-2,0.81171100112508598,0.85054160810077428,6.4395066210587961,216.88811006569745,0,-175.67936915321494,0,0,0,0,0,0.96463712589459194,1.3722858815885177,11.575645510735104,32.934861158124427,20.966983813443068,3604.4291974167882,2921.90218965846,28108.699064514385,0.70760195024155381,25.38764123306548,-49851.263907479173,248.09239201627736,0.2375359767012892,9.0607887228541415,-50683.656616346991,443.24378540842082,13.819868935992467,0.32685767525951659,13.746686844065005,-50525.485774787048,372.69936056147532]
["KBM","KBMS-60S03-A (240 V)",154,18.7,133.38699992463609,15.692588226427775,315,393,467,0.86699999999999999,11,515,52.9,325,38,197.44302257055318,363.80447742725966,437.66990291262135,130.19332787102911,4.725897920604915E-2,0.76256542143454253,0.68705728322266857,7.32537638506144,270.01351230650874,0,-218.71094496827206,0,0,0,0,0,0.96031678422750744,1.366139794407931,11.523801410730089,32.787355065790344,20.873078518518515,4487.311854761575,3637.6040743163758,34993.751194923534,1.0833844362918668,36.906289996527782,-49521.274392206804,197.44302257055318,0.35016529171883709,11.891545233500112,-50671.868598321824,363.80447742725966,15.376282105781348,0.4217501343306469,16.14259907939881,-50559.535054163251,327.6282164687529]
["KBM","KBMS-88H01-A (400 V)",205,17,162.33804195373327,13.306396881453548,425,414,542,0.93,13,738,146,565,46,174.39504159521326,255.3751999513465,305.42005420054204,179.36516219674982,1.7123287671232876E-2,1.5931725513272075,1.7482431930063547,14.809666744809077,723.77268190463087,0,-586.25587234275088,0,0,0,0,0,1.7579454031953758,2.5008405675566512,21.095344838344509,60.020173621359632,38.210029268292679,12028.263726211078,9750.6174194220512,93800.939574840129,1.4113098397515564,40.812701158126359,-50040.588749870316,174.39504159521326,0.70753476039577767,17.693661931973377,-50661.45802560803,255.3751999513465,14.883935774361193,1.6181775380491752,45.423156249341943,-49858.090389551653,162.05631371423141]
["KBM","KBMS-88H01-A (480 V)",205,17,151.31962281660205,12.403247771852628,520,414,651,0.93,13,738,146,679,46,174.39504159521326,255.54278313989471,305.42005420054204,178.61993656645228,1.7123287671232876E-2,1.6061196440503467,1.7482431930063547,14.809666744809077,723.77268190463087,0,-586.25587234275088,0,0,0,0,0,1.7579454031953758,2.5008405675566512,21.095344838344509,60.020173621359632,38.210029268292679,12028.26372621108,9750.6174194220512,93800.939574840129,1.4113098397515564,40.812701158126359,-50040.588749870316,174.39504159521326,0.7067412406546113,17.650512120968596,-50662.158067484241,255.54278313989471,14.847638086627576,1.6181775380491752,45.423156249341943,-49858.090389551653,162.05631371423141]
["KBM","KBMS-88H01-B (400 V)",205,32,66.998273370021394,10.197606296806908,935,414,1006,0.26100000000000001,3.7,397,146,565,46,338.86187048871511,515.34771262532388,567.7581863979849,128.93703298705378,1.7123287671232876E-2,1.8386809798247039,1.7482431930063547,7.5984624614615512,723.77268190463087,0,-586.25587234275088,0,0,0,0,0,3.3090737001324722,4.7074645977536962,39.708884401589664,112.97915034608872,71.924760975609757,12028.26372621108,9750.6174194220512,93800.939574840129,0.4063632653612248,11.59813340574218,-50591.789097168643,338.86187048871511,0.18389569685902707,3.7702560031934267,-50782.612381638086,515.34771262532388,21.007733464176027,0.46573934776426867,12.908330273181191,-50540.858801398521,315.85337325445761]
["KBM","KBMS-88H01-B (480 V)",205,32,67.048252621692072,10.20521348884202,940,414,1068,0.26100000000000001,3.7,397,146,679,46,338.86187048871511,515.10291667734577,567.7581863979849,129.40494953691191,1.7123287671232876E-2,1.8336642154647427,1.7482431930063547,7.5984624614615512,723.77268190463087,0,-586.25587234275088,0,0,0,0,0,3.3090737001324722,4.7074645977536962,39.708884401589664,112.97915034608872,71.924760975609757,12028.26372621108,9750.6174194220512,93800.939574840129,0.4063632653612248,11.59813340574218,-50591.789097168643,338.86187048871511,0.18405179938876298,3.7814341919685788,-50782.478483480976,515.10291667734577,21.070017937750698,0.46573934776426867,12.908330273181191,-50540.858801398521,315.85337325445761]
["KBM","KBMS-88H02-A (400 V)",385,15,331.71240770731868,12.907097576160259,190,789,257,1.66,29,1560,247,565,46,80.108775950359927,117.40997571628054,144.48717948717947,352.07107938388015,1.0121457489878543E-2,1.6543157272893365,1.541236480864457,29.575016373820379,1216.0355834020565,0,-984.98882255566571,0,0,0,0,0,1.3876660031936705,1.9740837392890527,16.651992038324046,47.378009742937266,30.161777777777775,20209.103028213231,16382.350479096311,157598.21160890651,5.8912834617309935,137.87986404702104,-48852.203792157197,80.108775950359927,3.1299659836377582,61.876680116793246,-50411.841095673495,117.40997571628054,13.795380723660392,5.7623719173007597,135.28518804185362,-48925.015142225544,81.149574683734244]
["KBM","KBMS-88H02-A (480 V)",385,15,323.05067172269821,12.570065047575806,235,789,309,1.66,29,1560,247,679,46,80.108775950359927,117.22694238326886,144.48717948717947,354.09731771640224,1.0121457489878543E-2,1.6069971929459717,1.541236480864457,29.575016373820379,1216.0355834020565,0,-984.98882255566571,0,0,0,0,0,1.3876660031936705,1.9740837392890527,16.651992038324046,47.378009742937266,30.161777777777775,20209.103028213231,16382.350479096311,157598.21160890651,5.8912834617309935,137.87986404702104,-48852.203792157197,80.108775950359927,3.137439663126937,62.20783665627637,-50407.619839183317,117.22694238326886,13.869211939761136,5.7623719173007597,135.28518804185362,-48925.015142225544,81.149574683734244]
["KBM","KBMS-88H02-B (400 V)",385,31.7,273.02307055855135,22.563890128805898,440,789,545,0.36899999999999999,6.4,733,247,565,46,186.20588181206469,267.54445449260834,307.50341064120056,316.91180340188714,1.0121457489878543E-2,1.5824905117020422,1.541236480864457,12.739831846070288,1216.0355834020565,0,-984.98882255566571,0,0,0,0,0,2.932600820082623,4.1718969690308647,35.191209840991476,100.12552725674075,63.741890370370363,20209.103028213231,16382.350479096311,157598.21160890651,1.2894056295513745,30.434523324444495,-50374.172109876556,186.20588181206469,0.6623749682239376,12.411612432641379,-50733.48157219946,267.54445449260834,26.493372002287835,1.2613647410836395,29.861794826745115,-50390.240473323196,188.38553200686874]
["KBM","KBMS-88H02-B (480 V)",385,31.7,233.08964847367582,19.263607311874036,550,789,654,0.36899999999999999,6.4,733,247,679,46,186.20588181206469,268.56094434037345,307.50341064120056,310.82329552547685,1.0121457489878543E-2,1.6420881180059055,1.541236480864457,12.739831846070288,1216.0355834020565,0,-984.98882255566571,0,0,0,0,0,2.932600820082623,4.1718969690308647,35.191209840991476,100.12552725674075,63.741890370370363,20209.103028213231,16382.350479096311,157598.21160890651,1.2894056295513745,30.434523324444495,-50374.172109876556,186.20588181206469,0.65803811070186513,12.194552814169564,-50735.966736068687,268.56094434037345,26.03004451361079,1.2613647410836395,29.861794826745115,-50390.240473323196,188.38553200686874]
["KBM","KBMS-88H03-A (400 V)",538,18.100000000000001,462.41745283790686,15.413915094596895,165,1200,221,1.41,26,1812,315,565,46,67.116403590875478,102.38538330471637,124.39293598233995,491.0997087131048,7.9365079365079361E-3,1.642411910220982,1.2895500926190813,31.435618165344554,1547.4601111428974,0,-1253.442690025747,0,0,0,0,0,1.5248386723799483,2.1692245981789378,18.298064068559381,52.06139035629451,33.143310477764004,25716.99483550181,20847.279667787894,200550.83040411954,8.0771003636998877,178.65512478481151,-48374.889701496664,67.116403590875478,4.0911682636679778,73.339162534102158,-50395.620764908934,102.38538330471637,16.572881041756926,6.5141630705814704,146.66747609679706,-49167.245381199435,76.346518378500434]
["KBM","KBMS-88H03-A (480 V)",538,18.100000000000001,443.08736156783664,14.769578718927887,225,1200,265,1.41,26,1812,315,679,46,67.116403590875478,102.15342685483375,124.39293598233995,494.90821658809205,7.9365079365079361E-3,1.5650665804081128,1.2895500926190813,31.435618165344554,1547.4601111428974,0,-1253.442690025747,0,0,0,0,0,1.5248386723799483,2.1692245981789378,18.298064068559381,52.06139035629451,33.143310477764004,25716.99483550181,20847.279667787894,200550.83040411954,8.0771003636998877,178.65512478481151,-48374.889701496664,67.116403590875478,4.1047359265325607,73.952475225483042,-50388.742424505654,102.15342685483375,16.711474910631946,6.5141630705814704,146.66747609679706,-49167.245381199435,76.346518378500434]
["KBM","KBMS-88H03-B (400 V)",545,35.5,400.51687418082179,25.839798334246566,345,1200,426,0.37,7,940,315,565,46,141.11383251681428,208.80998431758886,239.78723404255319,457.55211815519181,7.9365079365079361E-3,1.5282420581236684,1.2895500926190813,15.141461968114003,1547.4601111428974,0,-1253.442690025747,0,0,0,0,0,2.9522929498489159,4.1999108521080162,35.427515398186991,100.7978604505924,64.169910975195364,25716.99483550181,20847.279667787894,200550.83040411954,2.1861561239418492,47.087247227828627,-50177.837441292824,141.11383251681428,1.0763399563016063,18.113023785230926,-50712.334731030918,208.80998431758886,30.067737660267884,1.7614758965726756,38.656420942695867,-50382.367197799096,158.50516978176185]
["KBM","KBMS-88H03-B (480 V)",545,35.5,359.5029302781636,23.193737437300879,425,1200,511,0.37,7,940,315,679,46,141.11383251681428,209.0836248078962,239.78723404255319,453.7425888736833,7.9365079365079361E-3,1.5632950674200583,1.2895500926190813,15.141461968114003,1547.4601111428974,0,-1253.442690025747,0,0,0,0,0,2.9522929498489159,4.1999108521080162,35.427515398186991,100.7978604505924,64.169910975195364,25716.99483550181,20847.279667787894,200550.83040411954,2.1861561239418492,47.087247227828627,-50177.837441292824,141.11383251681428,1.0739711677858816,18.001374469807242,-50713.475560547129,209.0836248078962,29.88239906821871,1.7614758965726756,38.656420942695867,-50382.367197799096,158.50516978176185]
["KBM","KBMS-88S01-A (240 V)",205,17,179.31456921686876,14.697915509579408,225,414,325,0.93,13,738,146,325,46,174.39504159521326,257.10471132168476,305.42005420054204,175.64957659257746,1.7123287671232876E-2,1.6577592297314649,1.7482431930063547,14.809666744809077,723.77268190463087,0,-586.25587234275088,0,0,0,0,0,1.7579454031953758,2.5008405675566512,21.095344838344509,60.020173621359632,38.210029268292679,12028.26372621108,9750.6174194220512,93800.939574840129,1.4113098397515564,40.812701158126359,-50040.588749870316,174.39504159521326,0.69942749780035363,17.247725355178094,-50668.610240006477,257.10471132168476,14.508813236472893,1.6181775380491752,45.423156249341943,-49858.090389551653,162.05631371423141]
["KBM","KBMS-88S01-B (240 V)",205,32,156.03550620729419,23.74969653079059,500,414,604,0.26100000000000001,3.7,397,146,325,46,338.86187048871511,502.34737292363548,567.7581863979849,155.80563035339716,1.7123287671232876E-2,1.5822005974879441,1.7482431930063547,7.5984624614615512,723.77268190463087,0,-586.25587234275088,0,0,0,0,0,3.3090737001324722,4.7074645977536962,39.708884401589664,112.97915034608872,71.924760975609757,12028.26372621108,9750.6174194220512,93800.939574840129,0.4063632653612248,11.59813340574218,-50591.789097168643,338.86187048871511,0.19255363384441737,4.3470344185246503,-50775.185968955077,502.34737292363548,24.221522450097719,0.46573934776426867,12.908330273181191,-50540.858801398521,315.85337325445761]
["KBM","KBMS-88S02-A (240 V)",385,15,346.63946605414804,13.487916967087473,100,789,154,1.66,29,1560,247,325,46,80.108775950359927,118.52231108942212,144.48717948717947,339.53420862113398,1.0121457489878543E-2,2.0181425004262992,1.541236480864457,29.575016373820379,1216.0355834020565,0,-984.98882255566571,0,0,0,0,0,1.3876660031936705,1.9740837392890527,16.651992038324046,47.378009742937266,30.161777777777775,20209.103028213231,16382.350479096311,157598.21160890651,5.8912834617309935,137.87986404702104,-48852.203792157197,80.108775950359927,3.0853762611129021,59.862865193817889,-50437.026100713636,118.52231108942212,13.346401503750789,5.7623719173007597,135.28518804185362,-48925.015142225544,81.149574683734244]
["KBM","KBMS-88S02-B (240 V)",385,31.7,323.45702476889028,26.731985518090106,235,789,327,0.36899999999999999,6.4,733,247,325,46,186.20588181206469,267.75201538263673,307.50341064120056,314.87976318819864,1.0121457489878543E-2,1.6022931440259036,1.541236480864457,12.739831846070288,1216.0355834020565,0,-984.98882255566571,0,0,0,0,0,2.932600820082623,4.1718969690308647,35.191209840991476,100.12552725674075,63.741890370370363,20209.103028213231,16382.350479096311,157598.21160890651,1.2894056295513745,30.434523324444495,-50374.172109876556,186.20588181206469,0.66148483270201097,12.367371889669439,-50733.991649513868,267.75201538263673,26.398937764278891,1.2613647410836395,29.861794826745115,-50390.240473323196,188.38553200686874]
["KBM","KBMS-88S03-A (240 V)",538,18.100000000000001,482.76999404541584,16.092333134847195,90,1200,132,1.41,26,1812,315,325,46,67.116403590875478,103.33035226019251,124.39293598233995,474.58960032644768,7.9365079365079361E-3,2.084712813768673,1.2895500926190813,31.435618165344554,1547.4601111428974,0,-1253.442690025747,0,0,0,0,0,1.5248386723799483,2.1692245981789378,18.298064068559381,52.06139035629451,33.143310477764004,25716.99483550181,20847.279667787894,200550.83040411954,8.0771003636998877,178.65512478481151,-48374.889701496664,67.116403590875478,4.0369814350272097,70.836766899948998,-50423.091631224321,103.33035226019251,16.007400011823592,6.5141630705814704,146.66747609679706,-49167.245381199435,76.346518378500434]
["KBM","KBMS-88S03-B (240 V)",545,35.5,463.67140087438844,29.914283927379898,180,1200,255,0.37,7,940,315,325,46,141.11383251681428,209.67668190417362,239.78723404255319,450.26271773015048,7.9365079365079361E-3,1.5950988057811735,1.2895500926190813,15.141461968114003,1547.4601111428974,0,-1253.442690025747,0,0,0,0,0,2.9522929498489159,4.1999108521080162,35.427515398186991,100.7978604505924,64.169910975195364,25716.99483550181,20847.279667787894,200550.83040411954,2.1861561239418492,47.087247227828627,-50177.837441292824,141.11383251681428,1.0688744841942666,17.758770130080457,-50715.930168477527,209.67668190417362,29.479674281422195,1.7614758965726756,38.656420942695867,-50382.367197799096,158.50516978176185]
["KBM","KBMS-163H01-A (400 V)",776,43.2,534.60145384567647,29.535991925175495,300,1966,365,0.37,4.2,1100,1230,565,56,124.63196098866862,184.27134222388634,204.90909090909091,627.72388629749344,2.0325203252032522E-3,5.1164980574933212,3.0554779070715892,32.356959161882394,6007.0695653027442,0,-4865.7263478952227,0,0,0,0,0,9.7947379775037575,13.933924249413584,117.53685573004509,334.41418198592601,212.89468041237114,99830.539007105443,80926.841545034884,778516.21566323563,2.5725241885138996,77.154378213855807,-49575.243041825066,124.63196098866862,1.3555113407012922,25.213717713699701,-50673.810503936751,184.27134222388634,35.766945231635773,6.365404693447779,150.07897207609375,-46151.503417475848,74.172606516970916]
["KBM","KBMS-163H01-A (480 V)",776,43.2,440.54088247836631,24.339275275047861,375,1966,438,0.37,4.2,1100,1230,679,56,124.63196098866862,184.87982411135221,204.90909090909091,610.61433961613579,2.0325203252032522E-3,5.6747379303614869,3.0554779070715892,32.356959161882394,6007.0695653027442,0,-4865.7263478952227,0,0,0,0,0,9.7947379775037575,13.933924249413584,117.53685573004509,334.41418198592601,212.89468041237114,99830.539007105443,80926.841545034884,778516.21566323563,2.5725241885138996,77.154378213855807,-49575.243041825066,124.63196098866862,1.3492741646517348,24.667421018200372,-50679.440648824559,184.87982411135221,34.991995491576951,6.365404693447779,150.07897207609375,-46151.503417475848,74.172606516970916]
["KBM","KBMS-163H02-A (400 V)",1090,40.6,843.68035333013711,31.017660048902101,200,2915,243,0.50900000000000001,6.3,1645,1720,565,56,79.335292413997593,120.98221244592699,137.02127659574467,940.99852088490491,1.4534883720930232E-3,5.5270910503927073,2.8800259763575755,50.245614847189977,8395.2757210823329,0,-6800.1733340766905,0,0,0,0,0,9.1588856164249375,13.029365224615546,109.90662739709924,312.7047653907731,199.07403656133192,139519.7593831555,113100.59599295951,1088027.7334522705,5.7231399054328129,157.46440871065298,-48514.434673127973,79.335292413997593,3.0286989288705195,51.495398114105576,-50560.171869168778,120.98221244592699,35.507828047373188,12.848522424983726,288.70807736341334,-43104.533256448238,47.7653623564768]
["KBM","KBMS-163H02-A (480 V)",1090,40.6,781.87301838940914,28.74533155843416,245,2915,291,0.50900000000000001,6.3,1645,1720,679,56,79.335292413997593,121.01149297110726,137.02127659574467,937.80854665559787,1.4534883720930232E-3,5.6516823652968595,2.8800259763575755,50.245614847189977,8395.2757210823329,0,-6800.1733340766905,0,0,0,0,0,9.1588856164249375,13.029365224615546,109.90662739709924,312.7047653907731,199.07403656133192,139519.7593831555,113100.59599295951,1088027.7334522705,5.7231399054328129,157.46440871065298,-48514.434673127973,79.335292413997593,3.0277826161821659,51.422229151390709,-50560.867573756885,121.01149297110726,35.457375559546463,12.848522424983726,288.70807736341334,-43104.533256448238,47.7653623564768]
["KBM","KBMS-163H03-A (400 V)",1375,38.6,1115.3578411880026,30.810990088066365,150,3930,183,0.64,8.4,2190,1830,565,56,55.760958441430503,89.656740027561341,102.92237442922375,1219.8088697813196,1.366120218579235E-3,5.2902986522022362,2.2726217897211916,58.91744424313783,8931.4036336042827,0,-7234.436943219469,0,0,0,0,0,7.3436582639446231,10.447035765367433,88.12389916733548,250.72885836881841,159.61894874074073,148429.58436553407,120323.27556290179,1157509.9109151151,10.334029821388199,267.83163534448545,-47065.987292419813,55.760958441430503,5.3392207244409331,83.875734552702824,-50438.44856535751,89.656740027561341,34.550283905879404,16.388197533377539,387.4977297040848,-42978.254257531124,40.734964505517063]
["KBM","KBMS-163H03-A (480 V)",1375,38.6,1063.9507945693204,29.390905927329289,180,3930,220,0.64,8.4,2190,1830,679,56,{"$f":"IF(AQ1440<I1440,IF(AQ1440<0,0,AQ1440),I1440)","v":55.760958441430503},{"$f":"IF(AU1440<I1440,IF(AU1440<0,0,AU1440),I1440)","v":89.628564432611356},{"$f":"IF(UAC_V*0.98/L1440*1000<I1440,IF(UAC_V*0.98/L1440*1000<0,0,UAC_V*0.98/L1440*1000),I1440)","v":102.92237442922375},{"$f":"C1440+(E1440-C1440)/G1440*Q1440","v":1220.1172569407986},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M1440,(inertia/gear^2+gear_inertia)/M1440),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M1440,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M1440))","v":1.366120218579235E-3},{"$f":"IF((C1440+(E1440-C1440)/G1440*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X1440^2*time1+Y1440^2*time2+Z1440^2*time3+AA1440^2*time4)/time)/(C1440+(E1440-C1440)/G1440*mspeed),SQRT((((X1440-Y1440)*2/PI()+Y1440)^2*time1+Y1440^2*time2+((Z1440-Y1440)*2/PI()+Y1440)^2*time3+AA1440^2*time4)/time)/(C1440+(E1440-C1440)/G1440*mspeed)),IF(AccType=1,SQRT((X1440^2*time1+Y1440^2*time2+Z1440^2*time3+AA1440^2*time4+AB1440^2*time5+AC1440^2*time6+AD1440^2*time7+AE1440^2*time8)/time)/(C1440+(E1440-C1440)/G1440*mspeed),SQRT((((X1440-Y1440)*2/PI()+Y1440)^2*time1+Y1440^2*time2+((Z1440-Y1440)*2/PI()+Y1440)^2*time3+AA1440^2*time4+((AB1440-AC1440)*2/PI()+AC1440)^2*time5+AC1440^2*time6+((AD1440-AC1440)*2/PI()+AC1440)^2*time7+AE1440^2*time8)/time)/(C1440+(E1440-C1440)/G1440*mspeed))))","v":5.2786628612943147},{"$f":"IF(move1,MAX(ABS(X1440),ABS(Z1440))/H1440,MAX(ABS(X1440),ABS(Z1440),ABS(AB1440),ABS(AD1440))/H1440)","v":2.2726217897211916},{"$f":"IF(AZ1440>0,speed/(MIN(AZ1440,I1440)),\"NA\")","v":58.91744424313783},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M1440+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M1440+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":8931.4036336042827},0,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M1440+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M1440+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-7234.436943219469},0,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M1440+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M1440+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M1440+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M1440+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":0},0,{"$f":"AH1440/Irms","v":7.3436582639446231},{"$f":"AI1440/Ipeak","v":10.447035765367433},{"$f":"IF(move1,IF(AccType=1,SQRT((X1440^2*time1+Y1440^2*time2+Z1440^2*time3+AA1440^2*time4)/time)/(C1440/D1440),SQRT((((X1440-Y1440)*2/PI()+Y1440)^2*time1+Y1440^2*time2+((Z1440-AA1440)*2/PI()+AA1440)^2*time3+AA1440^2*time4)/time)/(C1440/D1440)),IF(AccType=1,SQRT((X1440^2*time1+Y1440^2*time2+Z1440^2*time3+AA1440^2*time4+AB1440^2*time5+AC1440^2*time6+AD1440^2*time7+AE1440^2*time8)/time)/(C1440/D1440),SQRT((((X1440-Y1440)*2/PI()+Y1440)^2*time1+Y1440^2*time2+((Z1440-AA1440)*2/PI()+AA1440)^2*time3+AA1440^2*time4+((AB1440-AC1440)*2/PI()+AC1440)^2*time5+AC1440^2*time6+((AD1440-AE1440)*2/PI()+AE1440)^2*time7+AE1440^2*time8)/time)/(C1440/D1440)))","v":88.12389916733548},{"$f":"IF(move1,MAX(ABS(X1440),ABS(Z1440))/(C1440/D1440),MAX(ABS(X1440),ABS(Z1440),ABS(AB1440),ABS(AD1440))/(C1440/D1440))","v":250.72885836881841},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X1440),ABS(Z1440))/(C1440/D1440),MAX(ABS((X1440-Y1440)*2/PI()+Y1440),ABS((Z1440-Y1440)*2/PI()+Y1440))/(C1440/D1440)),IF(AccType=1,MAX(ABS(X1440),ABS(Z1440),ABS(AB1440),ABS(AD1440))/(C1440/D1440),MAX(ABS((X1440-Y1440)*2/PI()+Y1440),ABS((Z1440-Y1440)*2/PI()+Y1440),ABS((AB1440-AC1440)*2/PI()+AC1440),ABS((AD1440-AC1440)*2/PI()+AC1440))/(C1440/D1440)))","v":159.61894874074073},{"$f":"IF((C1440+(E1440-C1440)/G1440*mspeed)<0,\"NA\",U1440*(C1440+(E1440-C1440)/G1440*mspeed)*mspeed/9.55)","v":148429.58436553407},{"$f":"IF(move1,IF(speed1>speed2,AM1440/2*time1/time,AM1440/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z1440*-speed/30*PI(),((Z1440-AA1440)*2/PI()+AA1440)*-speed/30*PI()),IF(AccType=1,X1440*-speed/30*PI(),((X1440-Y1440)*2/PI()+Y1440)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z1440*-speed/30*PI(),((Z1440-AA1440)*2/PI()+AA1440)*-speed/30*PI()),IF(AccType=1,X1440*-speed/30*PI(),((X1440-Y1440)*2/PI()+Y1440)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD1440*-speed/30*PI(),((AD1440-AE1440)*2/PI()+AE1440)*-speed/30*PI()),IF(AccType=1,AB1440*-speed/30*PI(),((AB1440-AC1440)*2/PI()+AC1440)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD1440*-speed/30*PI(),((AD1440-AE1440)*2/PI()+AE1440)*-speed/30*PI()),IF(AccType=1,AB1440*-speed/30*PI(),((AB1440-AC1440)*2/PI()+AC1440)*-speed/30*PI()),0)/2*time7/time)))","v":120323.27556290179},{"$f":"IF(move1,MAX(IF(AccType=1,Z1440*-speed/30*PI(),((Z1440-AA1440)*2/PI()+AA1440)*-speed/30*PI()),IF(AccType=1,X1440*-speed/30*PI(),((X1440-Y1440)*2/PI()+Y1440)*-speed/30*PI()),0),MAX(IF(AccType=1,Z1440*-speed/30*PI(),((Z1440-AA1440)*2/PI()+AA1440)*-speed/30*PI()),IF(AccType=1,X1440*-speed/30*PI(),((X1440-Y1440)*2/PI()+Y1440)*-speed/30*PI()),IF(AccType=1,AD1440*-speed/30*PI(),((AD1440-AE1440)*2/PI()+AE1440)*-speed/30*PI()),IF(AccType=1,AB1440*-speed/30*PI(),((AB1440-AC1440)*2/PI()+AC1440)*-speed/30*PI()),0))","v":1157509.9109151151},{"$f":"(L1440^2)/1000000+((K1440/1000)^2*(D1440/C1440*H1440)^2*PI()*PI()*(O1440/2)^2)/1200","v":10.334029821388199},{"$f":"SQRT(3)*L1440*J1440*D1440/C1440*H1440/1000","v":267.83163534448545},{"$f":"0.75*J1440^2*(D1440/C1440*H1440)^2-(UAC_V*0.98)^2","v":-47065.987292419813},{"$f":"-AO1440/2/AN1440+SQRT((AO1440/2/AN1440)^2-AP1440/AN1440)","v":55.760958441430503},{"$f":"(L1440^2)/1000000+((K1440/1000)^2*AV1440^2*PI()*PI()*(O1440/2)^2)/1200","v":5.3410983147197353},{"$f":"SQRT(3)*L1440*J1440*AV1440/1000","v":84.020590368486438},{"$f":"0.75*J1440^2*AV1440^2-(UAC_V*0.98)^2","v":-50437.180829117984},{"$f":"-AS1440/2/AR1440+SQRT((AS1440/2/AR1440)^2-AT1440/AR1440)","v":89.628564432611356},{"$f":"D1440+(F1440-D1440)*((0.85*UAC_V-D1440*J1440)/L1440*1000)/G1440","v":34.609953243947572},{"$f":"(L1440^2)/1000000+((K1440/1000)^2*AJ1440^2*PI()*PI()*(O1440/2)^2)/1200","v":16.388197533377539},{"$f":"SQRT(3)*L1440*J1440*AJ1440/1000","v":387.4977297040848},{"$f":"0.75*J1440^2*AJ1440^2-(UAC_V*0.98)^2","v":-42978.254257531124},{"$f":"IF(((AX1440/2/AW1440)^2-AY1440/AW1440)>0,-AX1440/2/AW1440+SQRT((AX1440/2/AW1440)^2-AY1440/AW1440),-9999)","v":40.734964505517063}]
["KBM","KBMS-163S01-A (240 V)",776,43.2,580.77085597351629,32.086787622846202,165,1966,219,0.37,4.2,1100,1230,325,56,124.63196098866862,187.02715822431577,204.90909090909091,554.70816963734001,2.0325203252032522E-3,8.7348187608267125,3.0554779070715892,32.356959161882394,6007.0695653027442,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},-4865.7263478952227,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},0,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":0},9.7947379775037575,13.933924249413584,117.53685573004509,334.41418198592601,212.89468041237114,99830.539007105443,80926.841545034884,778516.21566323563,2.5725241885138996,77.154378213855807,-49575.243041825066,124.63196098866862,1.3279961600197558,22.705046844439746,-50698.647778469385,187.02715822431577,32.208267586241647,6.365404693447779,150.07897207609375,-46151.503417475848,74.172606516970916]
["KBM","KBMS-163S02-A (240 V)",1090,40.6,945.38036196585824,34.756630954627141,110,2915,146,0.50900000000000001,6.3,1645,1720,325,56,79.335292413997593,121.30300122833435,137.02127659574467,930.52003518093852,1.4534883720930232E-3,5.9450960371050803,2.8800259763575755,50.245614847189977,8395.2757210823329,0,-6800.1733340766905,0,0,0,0,0,9.1588856164249375,13.029365224615546,109.90662739709924,312.7047653907731,199.07403656133192,139519.7593831555,113100.59599295951,1088027.7334522705,5.7231399054328129,157.46440871065298,-48514.434673127973,79.335292413997593,3.0187137490896392,50.692371514017324,-50567.753053490349,121.30300122833435,34.954113900524206,12.848522424983726,288.70807736341334,-43104.533256448238,47.7653623564768]
["KBM","KBMS-163S03-A (240 V)",1375,38.6,1209.1796801406749,33.402753595046264,80,3930,110,0.64,8.4,2190,1830,325,56,55.760958441430503,90.135457801201198,102.92237442922375,1188.1713694592265,1.366120218579235E-3,7.150166111941231,2.2726217897211916,58.91744424313783,8931.4036336042827,0,-7234.436943219469,0,0,0,0,0,7.3436582639446231,10.447035765367433,88.12389916733548,250.72885836881841,159.61894874074073,148429.58436553407,120323.27556290179,1157509.9109151151,10.334029821388199,267.83163534448545,-47065.987292419813,55.760958441430503,5.3077208414746826,81.407096059947079,-50459.717072990898,90.135457801201198,33.533396706732432,16.388197533377539,387.4977297040848,-42978.254257531124,40.734964505517063]
["KBM","KBMS-260H01-A (400 V)",1932,33.1,1710.4475354640751,28.84397193025422,85,6494,111,1.06,16,3584,5450,565,58,25.138950014405914,52.088134936346584,62.890625000000007,1796.2322980208542,4.5871559633027525E-4,12.371077019170034,4.0922214114090281,"NA",26574.885845690231,0,-21525.657535009086,0,0,0,0,0,13.33522706324122,18.970598720935701,160.02272475889464,455.29436930245686,289.84939774557159,441643.82469471992,358015.09413736523,3444105.2056014538,34.764057805170467,732.0953520520244,-40373.839099254656,25.138950014405914,14.531281091710188,203.05563080551812,-50002.680252114376,52.088134936346584,30.858907278163738,161.60954167148964,1907.2468045384649,19992.319851823646,-9999]
["KBM","KBMS-260H01-A (480 V)",1932,33.1,1680.6761990504149,28.341925784998566,105,6494,134,1.06,16,3584,5450,679,58,25.138950014405914,52.002407495918554,62.890625000000007,1807.5291170437768,4.5871559633027525E-4,10.973536355872003,4.0922214114090281,"NA",26574.885845690231,0,-21525.657535009086,0,0,0,0,0,13.33522706324122,18.970598720935701,160.02272475889464,455.29436930245686,289.84939774557159,441643.82469471992,358015.09413736523,3444105.2056014538,34.764057805170467,732.0953520520244,-40373.839099254656,25.138950014405914,14.55462479068402,204.45632666340759,-49991.57091341498,52.002407495918554,31.0717747737956,161.60954167148964,1907.2468045384649,19992.319851823646,-9999]
["KBM","KBMS-260H02-A (400 V)",2706,31,2428.9938042061262,27.322764951699956,55,9741,74,1.48,24,5380,7860,565,58,12.164848459155289,33.370192609634884,41.895910780669148,2537.9318162235672,3.1806615776081427E-4,31.196867851143629,3.9339863484277533,"NA",38320.961020034745,0,-31039.978426228143,0,0,0,0,0,12.858148259521323,18.29190982417278,154.29777911425589,439.0058357801467,279.47979524239685,636849.99021774158,516257.43744246394,4966396.548196503,78.559271215097397,1539.012202733609,-30347.329122844534,12.164848459155289,32.327655676717619,401.88661190753004,-49410.133251902669,33.370192609634884,29.140628901903842,340.14312670149798,3854.3844878803893,77512.232832577021,-9999]
["KBM","KBMS-260H02-A (480 V)",2706,31,2406.2823087173174,27.067292561499631,68,9741,89,1.48,24,5380,7860,679,58,12.164848459155289,33.290316813320771,41.895910780669148,2559.2691632741535,3.1806615776081427E-4,18.818882532759364,3.9339863484277533,"NA",38320.961020034745,0,-31039.978426228143,0,0,0,0,0,12.858148259521323,18.29190982417278,154.29777911425589,439.0058357801467,279.47979524239685,636849.9902177417,516257.43744246394,4966396.548196503,78.559271215097397,1539.012202733609,-30347.329122844534,12.164848459155289,32.38618604489789,405.34802733237132,-49385.999270616732,33.290316813320771,29.391614675955541,340.14312670149798,3854.3844878803893,77512.232832577021,-9999]
["KBM","KBMS-260H03-A (400 V)",3444,29.5,3366.1270463935866,28.286781902467116,40,12812,55,1.9,32,7180,10200,565,58,5.4500661577046099,23.720607575128202,31.392757660167131,3397.8201556696526,2.4509803921568627E-4,6.814003470398136,3.881194496285572,"NA",49725.863886410749,0,-40277.949747992701,0,0,0,0,0,12.475252532207561,17.747205098832719,149.70303038649072,425.93292237198523,271.15732008431195,826386.2671156131,669903.53011214477,6444471.9596788324,136.85574434483163,2593.07140327052,-18197.467135752424,5.4500661577046099,57.472626591589183,683.12567954249289,-48542.11941386632,23.720607575128202,28.910921783771027,572.33578224484904,6407.077917851002,148267.276227091,-9999]
["KBM","KBMS-260H03-A (480 V)",3444,29.5,3288.7777440509253,27.636787765133825,50,12812,67,1.9,32,7180,10200,679,58,5.4500661577046099,23.758033230651726,31.392757660167131,3370.244489700503,2.4509803921568627E-4,8.5581944062427464,3.881194496285572,"NA",49725.863886410749,0,-40277.949747992701,0,0,0,0,0,12.475252532207561,17.747205098832719,149.70303038649072,425.93292237198523,271.15732008431195,826386.2671156131,669903.53011214477,6444471.9596788324,136.85574434483163,2593.07140327052,-18197.467135752424,5.4500661577046099,57.417601772080118,679.94365465045928,-48563.152966867579,23.758033230651726,28.776253631888334,572.33578224484904,6407.077917851002,148267.276227091,-9999]
["KBM","KBMS-260S01-A (240 V)",1932,33.1,1761.3147035503084,29.701765658521222,45,6494,67,1.06,16,3584,5450,325,58,25.138950014405914,52.546058664218023,62.890625000000007,1732.6924533252236,4.5871559633027525E-4,42.604482086622646,4.0922214114090281,"NA",26574.885845690231,0,-21525.657535009086,0,0,0,0,0,13.33522706324122,18.970598720935701,160.02272475889464,455.29436930245686,289.84939774557159,441643.82469471992,358015.09413736523,3444105.2056014538,34.764057805170467,732.0953520520244,-40373.839099254656,25.138950014405914,14.409112507809995,195.5615555973325,-50060.820659874735,52.546058664218023,29.720012626153419,161.60954167148964,1907.2468045384649,19992.319851823646,-9999]
["KBM","KBMS-260S02-A (240 V)",2706,31,2482.8171122335671,27.928201487441697,28,9741,44,1.48,24,5380,7860,325,58,12.164848459155289,33.749365090397923,41.895910780669148,2436.9899728157625,3.1806615776081427E-4,"NA",3.9339863484277533,"NA",38320.961020034745,0,-31039.978426228143,0,0,0,0,0,12.858148259521323,18.29190982417278,154.29777911425589,439.0058357801467,279.47979524239685,"NA",516257.43744246394,4966396.548196503,78.559271215097397,1539.012202733609,-30347.329122844534,12.164848459155289,32.056614746298315,385.45253587329114,-49521.89227454058,33.749365090397923,27.949000972855991,340.14312670149798,3854.3844878803893,77512.232832577021,-9999]
["KBM","KBMS-260S03-A (240 V)",3444,29.5,3317.1240770731874,27.874992244312498,19,12812,33,1.9,32,7180,10200,325,58,5.4500661577046099,24.018758094503625,31.392757660167131,3283.6104157475793,2.4509803921568627E-4,40.774381657816974,3.881194496285572,"NA",49725.863886410749,0,-40277.949747992701,0,0,0,0,0,12.475252532207561,17.747205098832719,149.70303038649072,425.93292237198523,271.15732008431195,826386.2671156131,669903.53011214477,6444471.9596788324,136.85574434483163,2593.07140327052,-18197.467135752424,5.4500661577046099,57.04172036785944,657.79525378934704,-48706.835790517071,24.018758094503625,27.838899490319438,572.33578224484904,6407.077917851002,148267.276227091,-9999]

{"sheet":"LinMotor","index":4,"n_rows":352,"n_cols":51,"rows_kept":352,"cut":false,"hidden":true,"merged":[[0,0,1,0]]}
["Motor\nLinie","Typ","Fn","In","Fmax","Imax","Vmax","RU-V","LU-V","KE eff","G","UDCmax","PolPitch","Vmax","Vmax","Vmax",null,"Gext/Gmot","Frms","Fpk","v","F (t1)","F (t2)","F (t3)","F (t4)","F (t5)","F (t6)","F (t7)","F (t8)","Irms","Ipeak","Irms","Ipeak","Ipeak","P","PbrRMS","PbrPEAK","Koeff","Koeff","Koeff","nmax","Koeff","Koeff","Koeff","nmax","Koeff","Koeff","Koeff","nmax",null,"KE Peak"]
[null,"Kein Motor","[N]","[A]","[N]","[A] ","[m/s]","[W]","[mH]","[V/m/s]","[kg]","[V]","[mm]","bei F=0","bei Fmax","bei Fn",null," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," ","trapez"," "," "," ","A","B","C","theo","A","B","C","theo","A","B","C","theo",null,"[V/m/s]"]
["Other","power_linear_test",175.16066937328301,2.86372222365137,404.68872564616998,8.9,"NA",3.8,47,34.699696967550501,2.5,675,32,{"$f":"IFERROR(IF(G3=\"NA\",(UAC_V*0.98)/J3,(IF((UAC_V*0.98)/J3<G3,(UAC_V*0.98)/J3,G3))),0)","v":6.4957339601779038},{"$f":"IFERROR(IF(AO3<G3,IF(AO3<0,0,AO3),G3),0)","v":2.7439355436424613},{"$f":"IFERROR(IF(AS3<G3,IF(AS3<0,0,AS3),G3),0)","v":5.3239174042108184},null,{"$f":"IFERROR(IF(move1,Gewicht/K3,MAX(Gewicht,Gewicht2)/K3),0)","v":2},{"$f":"IFERROR(IF(move1,IF(AccType=1,SQRT((V3^2*Ltime1+W3^2*Ltime2+X3^2*Ltime3+Y3^2*Ltime4)/ltime)/C3,SQRT((((V3-W3)*2/PI()+W3)^2*Ltime1+W3^2*Ltime2+((X3-W3)*2/PI()+W3)^2*Ltime3+Y3^2*Ltime4)/ltime)/C3),IF(AccType=1,SQRT((V3^2*Ltime1+W3^2*Ltime2+X3^2*Ltime3+Y3^2*Ltime4+Z3^2*Ltime5+AA3^2*Ltime6+AB3^2*Ltime7+AC3^2*Ltime8)/ltime)/C3,SQRT((((V3-W3)*2/PI()+W3)^2*Ltime1+W3^2*Ltime2+((X3-W3)*2/PI()+W3)^2*Ltime3+Y3^2*Ltime4+((Z3-AA3)*2/PI()+AA3)^2*Ltime5+AA3^2*Ltime6+((AB3-AA3)*2/PI()+AA3)^2*Ltime7+AC3^2*Ltime8)/ltime)/C3)),0)","v":0.86726809642745961},{"$f":"IFERROR( IF(move1,MAX(ABS(V3),ABS(X3))/E3,MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))/E3),0)","v":0.97037543947628513},{"$f":"IFERROR(IF(AW3>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW3,G3),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW3,G3)),\"NA\"),0)","v":0.23642818329453044},{"$f":"((Gewicht+K3)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":235.62},{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},{"$f":"((Gewicht+K3)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-392.7},{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},{"$f":"((Gewicht2+K3)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},{"$f":"((Gewicht2+K3)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},{"$f":"(Ltorque2+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},{"$f":"AF3/Irms","v":0.20696791013359461},{"$f":"AG3/Ipeak","v":0.35769636303584768},{"$f":"D3*S3","v":2.4836149216031354},{"$f":"IFERROR(IF(move1,IF(MAX(ABS(V3),ABS(X3))<=C3,MAX(ABS(V3),ABS(X3))/C3*D3,D3+(MAX(ABS(V3),ABS(X3))-C3)/(E3-C3)*(F3-D3)),IF(MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))<=C3,MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))/C3*D3,D3+(MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))-C3)/(E3-C3)*(F3-D3))),0)","v":8.5847127128603447},{"$f":"IFERROR(IF(AccType=1,IF(move1,IF(MAX(ABS(V3),ABS(X3))<=C3,MAX(ABS(V3),ABS(X3))/C3*D3,D3+(MAX(ABS(V3),ABS(X3))-C3)/(E3-C3)*(F3-D3)),IF(MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))<=C3,MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))/C3*D3,D3+(MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))-C3)/(E3-C3)*(F3-D3))),IF(move1,IF(MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3))<=C3,MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3))/C3*D3,D3+(MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3))-C3)/(E3-C3)*(F3-D3)),IF(MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3),ABS((Z3-AA3)*2/PI()+AA3),ABS((AB3-AA3)*2/PI()+AA3))<=C3,MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3),ABS((Z3-AA3)*2/PI()+AA3),ABS((AB3-AA3)*2/PI()+AA3))/C3*D3,D3+(MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3),ABS((Z3-AA3)*2/PI()+AA3),ABS((AB3-AA3)*2/PI()+AA3))-C3)/(E3-C3)*(F3-D3)))),0)","v":4.8319108819588612},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V3)+Ltime2*ABS(Lspeed2)*ABS(W3)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X3)+Ltime4*ABS(Lspeed1)*ABS(Y3))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V3)+Ltime2*ABS(Lspeed2)*ABS(W3)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X3)+Ltime4*ABS(Lspeed1)*ABS(Y3)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z3)+Ltime6*ABS(Lspeed6)*ABS(AA3)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB3)+Ltime8*ABS(Lspeed1)*ABS(AC3))/ltime)","v":181.24615384615385},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK3/2*Ltime1/ltime,AK3/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X3*-ABS(Lspeed2-Lspeed1),((X3-Y3)*2/PI()+Y3)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V3*-ABS(Lspeed2-Lspeed1),((V3-W3)*2/PI()+W3)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X3*-ABS(Lspeed2-Lspeed1),((X3-Y3)*2/PI()+Y3)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V3*-ABS(Lspeed2-Lspeed1),((V3-W3)*2/PI()+W3)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB3*-ABS(Lspeed6-Lspeed1),((AB3-AC3)*2/PI()+AB3)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z3*-ABS(Lspeed6-Lspeed1),((Z3-AA3)*2/PI()+AA3)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB3*-ABS(Lspeed6-Lspeed1),((AB3-AC3)*2/PI()+AB3)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z3*-ABS(Lspeed6-Lspeed1),((Z3-AA3)*2/PI()+AA3)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":28.846221301009521},{"$f":"IF(move1,MAX(IF(AccType=1,X3*-ABS(Lspeed2-Lspeed1),((X3-Y3)*2/PI()+Y3)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V3*-ABS(Lspeed2-Lspeed1),((V3-W3)*2/PI()+W3)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X3*-ABS(Lspeed2-Lspeed1),((X3-Y3)*2/PI()+Y3)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V3*-ABS(Lspeed2-Lspeed1),((V3-W3)*2/PI()+W3)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB3*-ABS(Lspeed6-Lspeed1),((AB3-AC3)*2/PI()+AB3)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z3*-ABS(Lspeed6-Lspeed1),((Z3-AA3)*2/PI()+AA3)*-ABS(Lspeed6-Lspeed1)),0))","v":250.00058460874919},{"$f":"IFERROR((J3^2)+3*(I3/1000)^2*(F3/2)^2*(2000*PI()/M3)^2,0)","v":6263.4428302573924},{"$f":"SQRT(3)*H3*F3/2*J3","v":1016.3187012017462},{"$f":"3*F3^2*H3^2/4-(UAC_V*0.98)^2","v":-49947.315700000006},{"$f":"IFERROR(-AM3/2/AL3+SQRT((AM3/2/AL3)^2-AN3/AL3),0)","v":2.7439355436424613},{"$f":"IFERROR((J3^2)+3*(I3/1000)^2*(D3/2)^2*(2000*PI()/M3)^2,0)","v":1727.8847032599797},{"$f":"SQRT(3)*H3*D3/2*J3","v":327.01735403864456},{"$f":"3*D3^2*H3^2/4-(UAC_V*0.98)^2","v":-50716.344199129038},{"$f":"IFERROR(-AQ3/2/AP3+SQRT((AQ3/2/AP3)^2-AR3/AP3),0)","v":5.3239174042108184},{"$f":"IFERROR((J3^2)+3*(I3/1000)^2*(AH3/2)^2*(2000*PI()/M3)^2,0)","v":2695.3331650561522},{"$f":"SQRT(3)*H3*AH3/2*J3","v":551.77094290730486},{"$f":"3*AH3^2*H3^2/4-(UAC_V*0.98)^2","v":-50552.308061187992},{"$f":"IFERROR(IF((AU3/2/AT3)^2-AV3/AT3>=0,-AU3/2/AT3+SQRT((AU3/2/AT3)^2-AV3/AT3),-9999),0)","v":4.2296141943206909},null,36.299999999999997]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IFERROR(IF(AO4<G4,IF(AO4<0,0,AO4),G4),0)","v":0},{"$f":"IFERROR(IF(AS4<G4,IF(AS4<0,0,AS4),G4),0)","v":0},null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,{"$f":"IFERROR((J4^2)+3*(I4/1000)^2*(F4/2)^2*(2000*PI()/M4)^2,0)","v":0},0,-50805.16,{"$f":"IFERROR(-AM4/2/AL4+SQRT((AM4/2/AL4)^2-AN4/AL4),0)","v":0},{"$f":"IFERROR((J4^2)+3*(I4/1000)^2*(D4/2)^2*(2000*PI()/M4)^2,0)","v":0},0,-50805.16,{"$f":"IFERROR(-AQ4/2/AP4+SQRT((AQ4/2/AP4)^2-AR4/AP4),0)","v":0},{"$f":"IFERROR((J4^2)+3*(I4/1000)^2*(AH4/2)^2*(2000*PI()/M4)^2,0)","v":0},0,-50805.16,{"$f":"IFERROR(IF((AU4/2/AT4)^2-AV4/AT4>=0,-AU4/2/AT4+SQRT((AU4/2/AT4)^2-AV4/AT4),-9999),0)","v":0},null,36.4]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-50805.16,0,0,0,-50805.16,0,0,0,-50805.16,0,null,72.8]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-50805.16,0,0,0,-50805.16,0,0,0,-50805.16,0,null,30.9]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-50805.16,0,0,0,-50805.16,0,0,0,-50805.16,0,null,51.4]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-50805.16,0,0,0,-50805.16,0,0,0,-50805.16,0,null,61.7]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-50805.16,0,0,0,-50805.16,0,0,0,-50805.16,0,null,103]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-50805.16,0,0,0,-50805.16,0,0,0,-50805.16,0,null,103]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-50805.16,0,0,0,-50805.16,0,0,0,-50805.16,0,null,154]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-50805.16,0,0,0,-50805.16,0,0,0,-50805.16,0,null,154]
["Leerzeile"]
["ALT","L1S040P 2608-GL-X0",110,1.8,600,15,"NA",11.1,25,30.1,1.8,330,24,{"$f":"IF(G14=\"NA\",(UAC_V*0.98)/J14,(IF((UAC_V*0.98)/J14<G14,(UAC_V*0.98)/J14,G14)))","v":7.4883720930232558},{"$f":"IF(AO14<G14,IF(AO14<0,0,AO14),G14)","v":1.6724858285273914},{"$f":"IF(AS14<G14,IF(AS14<0,0,AS14),G14)","v":6.8179987896746779},null,{"$f":"IF(move1,Gewicht/K14,MAX(Gewicht,Gewicht2)/K14)","v":2.7777777777777777},{"$f":"IF(move1,IF(AccType=1,SQRT((V14^2*Ltime1+W14^2*Ltime2+X14^2*Ltime3+Y14^2*Ltime4)/ltime)/C14,SQRT((((V14-W14)*2/PI()+W14)^2*Ltime1+W14^2*Ltime2+((X14-W14)*2/PI()+W14)^2*Ltime3+Y14^2*Ltime4)/ltime)/C14),IF(AccType=1,SQRT((V14^2*Ltime1+W14^2*Ltime2+X14^2*Ltime3+Y14^2*Ltime4+Z14^2*Ltime5+AA14^2*Ltime6+AB14^2*Ltime7+AC14^2*Ltime8)/ltime)/C14,SQRT((((V14-W14)*2/PI()+W14)^2*Ltime1+W14^2*Ltime2+((X14-W14)*2/PI()+W14)^2*Ltime3+Y14^2*Ltime4+((Z14-AA14)*2/PI()+AA14)^2*Ltime5+AA14^2*Ltime6+((AB14-AA14)*2/PI()+AA14)^2*Ltime7+AC14^2*Ltime8)/ltime)/C14))","v":1.2521170545636631},{"$f":" IF(move1,MAX(ABS(V14),ABS(X14))/E14,MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))/E14)","v":0.59341333333333335},{"$f":"IF(AW14>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW14,G14),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW14,G14)),\"NA\")","v":0.20194074754772759},213.62879999999998,0,-356.048,0,0,0,0,0,0.18781755818454948,0.35117632653061226,2.2538106982145938,{"$f":"IF(move1,IF(MAX(ABS(V14),ABS(X14))<=C14,MAX(ABS(V14),ABS(X14))/C14*D14,D14+(MAX(ABS(V14),ABS(X14))-C14)/(E14-C14)*(F14-D14)),IF(MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))<=C14,MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))/C14*D14,D14+(MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))-C14)/(E14-C14)*(F14-D14)))","v":8.4282318367346942},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V14),ABS(X14))<=C14,MAX(ABS(V14),ABS(X14))/C14*D14,D14+(MAX(ABS(V14),ABS(X14))-C14)/(E14-C14)*(F14-D14)),IF(MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))<=C14,MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))/C14*D14,D14+(MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))-C14)/(E14-C14)*(F14-D14))),IF(move1,IF(MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14))<=C14,MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14))/C14*D14,D14+(MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14))-C14)/(E14-C14)*(F14-D14)),IF(MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14),ABS((Z14-AA14)*2/PI()+AA14),ABS((AB14-AA14)*2/PI()+AA14))<=C14,MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14),ABS((Z14-AA14)*2/PI()+AA14),ABS((AB14-AA14)*2/PI()+AA14))/C14*D14,D14+(MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14),ABS((Z14-AA14)*2/PI()+AA14),ABS((AB14-AA14)*2/PI()+AA14))-C14)/(E14-C14)*(F14-D14))))","v":4.9428714216275722},164.32984615384612,26.153907312915297,226.6671967119326,{"$f":"(J14^2)+3*(I14/1000)^2*(F14/2)^2*(2000*PI()/M14)^2","v":8134.7241609541206},4340.2162148762818,-30013.472500000003,{"$f":"-AM14/2/AL14+SQRT((AM14/2/AL14)^2-AN14/AL14)","v":1.6724858285273914},{"$f":"(J14^2)+3*(I14/1000)^2*(D14/2)^2*(2000*PI()/M14)^2","v":1010.1034839177395},520.82594578515386,-50505.759700000002,{"$f":"-AQ14/2/AP14+SQRT((AQ14/2/AP14)^2-AR14/AP14)","v":6.8179987896746779},{"$f":"(J14^2)+3*(I14/1000)^2*(AH14/2)^2*(2000*PI()/M14)^2","v":1690.9512647063507},1430.2087128131045,-48547.462003061206,{"$f":"IF((AU14/2/AT14)^2-AV14/AT14>=0,-AU14/2/AT14+SQRT((AU14/2/AT14)^2-AV14/AT14),-9999)","v":4.9519475992018673},null,30.1]
["ALT","L1S050P 1708-KL-X0",80,1,460,7,"NA",23.5,57,41.5,1.3,330,24,{"$f":"IF(G15=\"NA\",(UAC_V*0.98)/J15,(IF((UAC_V*0.98)/J15<G15,(UAC_V*0.98)/J15,G15)))","v":5.4313253012048195},{"$f":"IF(AO15<G15,IF(AO15<0,0,AO15),G15)","v":1.4817655298155255},{"$f":"IF(AS15<G15,IF(AS15<0,0,AS15),G15)","v":4.9458341901855247},null,{"$f":"IF(move1,Gewicht/K15,MAX(Gewicht,Gewicht2)/K15)","v":3.8461538461538458},{"$f":"IF(move1,IF(AccType=1,SQRT((V15^2*Ltime1+W15^2*Ltime2+X15^2*Ltime3+Y15^2*Ltime4)/ltime)/C15,SQRT((((V15-W15)*2/PI()+W15)^2*Ltime1+W15^2*Ltime2+((X15-W15)*2/PI()+W15)^2*Ltime3+Y15^2*Ltime4)/ltime)/C15),IF(AccType=1,SQRT((V15^2*Ltime1+W15^2*Ltime2+X15^2*Ltime3+Y15^2*Ltime4+Z15^2*Ltime5+AA15^2*Ltime6+AB15^2*Ltime7+AC15^2*Ltime8)/ltime)/C15,SQRT((((V15-W15)*2/PI()+W15)^2*Ltime1+W15^2*Ltime2+((X15-W15)*2/PI()+W15)^2*Ltime3+Y15^2*Ltime4+((Z15-AA15)*2/PI()+AA15)^2*Ltime5+AA15^2*Ltime6+((AB15-AA15)*2/PI()+AA15)^2*Ltime7+AC15^2*Ltime8)/ltime)/C15))","v":1.5950682331114312},{"$f":" IF(move1,MAX(ABS(V15),ABS(X15))/E15,MAX(ABS(V15),ABS(X15),ABS(Z15),ABS(AB15))/E15)","v":0.7171043478260869},{"$f":"IF(AW15>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW15,G15),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW15,G15)),\"NA\")","v":0.29315109873087514},{"$f":"((Gewicht+K15)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":197.92079999999999},0,{"$f":"((Gewicht+K15)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-329.86799999999999},0,{"$f":"((Gewicht2+K15)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K15)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF15/Irms","v":0.13292235275928593},{"$f":"AG15/Ipeak","v":0.20605350877192982},{"$f":"D15*S15","v":1.5950682331114312},{"$f":"IF(move1,IF(MAX(ABS(V15),ABS(X15))<=C15,MAX(ABS(V15),ABS(X15))/C15*D15,D15+(MAX(ABS(V15),ABS(X15))-C15)/(E15-C15)*(F15-D15)),IF(MAX(ABS(V15),ABS(X15),ABS(Z15),ABS(AB15))<=C15,MAX(ABS(V15),ABS(X15),ABS(Z15),ABS(AB15))/C15*D15,D15+(MAX(ABS(V15),ABS(X15),ABS(Z15),ABS(AB15))-C15)/(E15-C15)*(F15-D15)))","v":4.9452842105263155},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V15),ABS(X15))<=C15,MAX(ABS(V15),ABS(X15))/C15*D15,D15+(MAX(ABS(V15),ABS(X15))-C15)/(E15-C15)*(F15-D15)),IF(MAX(ABS(V15),ABS(X15),ABS(Z15),ABS(AB15))<=C15,MAX(ABS(V15),ABS(X15),ABS(Z15),ABS(AB15))/C15*D15,D15+(MAX(ABS(V15),ABS(X15),ABS(Z15),ABS(AB15))-C15)/(E15-C15)*(F15-D15))),IF(move1,IF(MAX(ABS((V15-W15)*2/PI()+W15),ABS((X15-W15)*2/PI()+W15))<=C15,MAX(ABS((V15-W15)*2/PI()+W15),ABS((X15-W15)*2/PI()+W15))/C15*D15,D15+(MAX(ABS((V15-W15)*2/PI()+W15),ABS((X15-W15)*2/PI()+W15))-C15)/(E15-C15)*(F15-D15)),IF(MAX(ABS((V15-W15)*2/PI()+W15),ABS((X15-W15)*2/PI()+W15),ABS((Z15-AA15)*2/PI()+AA15),ABS((AB15-AA15)*2/PI()+AA15))<=C15,MAX(ABS((V15-W15)*2/PI()+W15),ABS((X15-W15)*2/PI()+W15),ABS((Z15-AA15)*2/PI()+AA15),ABS((AB15-AA15)*2/PI()+AA15))/C15*D15,D15+(MAX(ABS((V15-W15)*2/PI()+W15),ABS((X15-W15)*2/PI()+W15),ABS((Z15-AA15)*2/PI()+AA15),ABS((AB15-AA15)*2/PI()+AA15))-C15)/(E15-C15)*(F15-D15))))","v":3.0526393327055157},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V15)+Ltime2*ABS(Lspeed2)*ABS(W15)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X15)+Ltime4*ABS(Lspeed1)*ABS(Y15))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V15)+Ltime2*ABS(Lspeed2)*ABS(W15)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X15)+Ltime4*ABS(Lspeed1)*ABS(Y15)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z15)+Ltime6*ABS(Lspeed6)*ABS(AA15)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB15)+Ltime8*ABS(Lspeed1)*ABS(AC15))/ltime)","v":152.24676923076922},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK15/2*Ltime1/ltime,AK15/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X15*-ABS(Lspeed2-Lspeed1),((X15-Y15)*2/PI()+Y15)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V15*-ABS(Lspeed2-Lspeed1),((V15-W15)*2/PI()+W15)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X15*-ABS(Lspeed2-Lspeed1),((X15-Y15)*2/PI()+Y15)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V15*-ABS(Lspeed2-Lspeed1),((V15-W15)*2/PI()+W15)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB15*-ABS(Lspeed6-Lspeed1),((AB15-AC15)*2/PI()+AB15)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z15*-ABS(Lspeed6-Lspeed1),((Z15-AA15)*2/PI()+AA15)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB15*-ABS(Lspeed6-Lspeed1),((AB15-AC15)*2/PI()+AB15)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z15*-ABS(Lspeed6-Lspeed1),((Z15-AA15)*2/PI()+AA15)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":24.230825892847999},{"$f":"IF(move1,MAX(IF(AccType=1,X15*-ABS(Lspeed2-Lspeed1),((X15-Y15)*2/PI()+Y15)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V15*-ABS(Lspeed2-Lspeed1),((V15-W15)*2/PI()+W15)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X15*-ABS(Lspeed2-Lspeed1),((X15-Y15)*2/PI()+Y15)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V15*-ABS(Lspeed2-Lspeed1),((V15-W15)*2/PI()+W15)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB15*-ABS(Lspeed6-Lspeed1),((AB15-AC15)*2/PI()+AB15)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z15*-ABS(Lspeed6-Lspeed1),((Z15-AA15)*2/PI()+AA15)*-ABS(Lspeed6-Lspeed1)),0))","v":210.00049107134933},{"$f":"(J15^2)+3*(I15/1000)^2*(F15/2)^2*(2000*PI()/M15)^2","v":9905.8483867595151},{"$f":"SQRT(3)*H15*F15/2*J15","v":5912.138925285416},{"$f":"3*F15^2*H15^2/4-(UAC_V*0.98)^2","v":-30509.972500000003},{"$f":"-AM15/2/AL15+SQRT((AM15/2/AL15)^2-AN15/AL15)","v":1.4817655298155255},{"$f":"(J15^2)+3*(I15/1000)^2*(D15/2)^2*(2000*PI()/M15)^2","v":1889.2622119746841},{"$f":"SQRT(3)*H15*D15/2*J15","v":844.59127504077378},{"$f":"3*D15^2*H15^2/4-(UAC_V*0.98)^2","v":-50390.972500000003},{"$f":"-AQ15/2/AP15+SQRT((AQ15/2/AP15)^2-AR15/AP15)","v":4.9458341901855247},{"$f":"(J15^2)+3*(I15/1000)^2*(AH15/2)^2*(2000*PI()/M15)^2","v":3278.5711501534888},{"$f":"SQRT(3)*H15*AH15/2*J15","v":2578.2325462493682},{"$f":"3*AH15^2*H15^2/4-(UAC_V*0.98)^2","v":-46945.50950643664},{"$f":"IF((AU15/2/AT15)^2-AV15/AT15>=0,-AU15/2/AT15+SQRT((AU15/2/AT15)^2-AV15/AT15),-9999)","v":3.4112101381480455},null,41.5]
["ALT","L1S050P 2608-GL-X0",130,2,725,17,"NA",9.4,23,32.6,2,330,24,6.9141104294478524,1.6476524973859363,6.345496170951038,null,2.5,1.090644945717218,0.50554482758620689,0.19496174672137831,219.91200000000001,0,-366.52,0,0,0,0,0,0.18177415761953633,0.33177871148459381,2.1812898914344361,7.9626890756302515,4.605055772306704,169.16307692307691,26.92313988094222,233.33387896816592,8921.4839085569893,4511.5420205069577,-31653.13,1.6476524973859363,1171.5312651703389,530.76964947140675,-50540.08,6.345496170951038,1639.4255101476365,1222.1119190317538,-49399.802682600523,5.129211328974753,null,32.6]
["ALT","L1S075P 3208-KL-X0",240,2.4,1400,22,"NA",9.1,25.5,47.5,3.5,330,24,4.7452631578947368,0.86071759785190505,4.3591001774923877,null,1.4285714285714286,0.71735872917709864,0.31790000000000002,0.23887587609180042,267.036,0,-445.06,0,0,0,0,0,0.14347174583541972,0.2443669540229885,1.7216609500250366,5.8648068965517242,3.1321951029675419,205.41230769230768,32.692384141144124,283.33399588991574,18434.227951641893,8235.4685772881185,-20745.130000000008,0.86071759785190505,2448.7813078542504,898.41475388597644,-50447.420800000007,4.3591001774923877,2584.1764820604244,1172.5042885647688,-50195.845293428138,4.1862745471028573,null,47.5]
["ALT","L1S080P 4111-IL-X0",450,4.5,2400,31,"NA",4,27,51.1,13.2,330,24,4.4109589041095889,0.93983733189419494,3.7570384337521836,null,0.37878787878787878,0.81919553700537717,0.39706333333333332,0.30291727264678492,571.77120000000002,0,-952.952,0,0,0,0,0,0.30719832637701644,0.47229119658119662,3.6863799165241975,11.334988717948718,6.6290791081572475,439.82400000000001,70.000163690449781,606.66808531723143,38623.39169618109,5487.483368539717,-39273.160000000003,0.93983733189419494,3370.0514977603198,796.57016640092661,-50562.16,3.7570384337521836,4257.9781107800572,1173.4503662821612,-50277.823722133522,3.3012313601741843,null,51.1]
["ALT","L1S120P 4711-IL-X0",1000,10.4,4200,50,"NA",2.73,20.3,55,21.5,330,24,4.0981818181818186,0.75511596710387918,2.9483851299330981,null,0.23255813953488372,0.536753119713688,0.33036666666666664,0.3213151213557176,832.524,0,-1387.54,0,0,0,0,0,0.46518603708519629,0.63315864583333337,5.5822324450223553,15.195807500000001,9.1866881490895036,640.40307692307692,101.92331526356698,883.33539895091383,55982.88121933482,6501.6857189116727,-36830.972500000003,0.75511596710387918,5316.1697730733022,1352.3506295336281,-50200.580752000002,2.9483851299330981,4812.7572201240218,1194.5791828606068,-50333.418041611934,3.1122095834790553,null,55]
["ALT","L1S160P 5611-IL-X0",1750,16.2,6550,84,"NA",1.36,11.6,56.6,32.200000000000003,330,24,3.9823321554770317,0.83585370880624288,3.0644639028339533,null,0.15527950310559005,0.43055991489701767,0.29737282442748092,0.29276802779574929,1168.6752000000001,0,-1947.7920000000001,0,0,0,0,0,0.58125588511097381,0.79140883333333345,6.9750706213316862,18.993812000000002,11.478883985418411,898.9809230769232,143.07725765300725,1240.0028996593962,52009.543331738962,5599.70640446372,-41017.076800000003,0.83585370880624288,5018.8437677978418,1079.9433780037173,-50441.103232000001,3.0644639028339533,4114.9700817530502,765.21881153861329,-50622.375900581676,3.4156735198477812,null,56.6]
["ALT","L1S200P 7411-IL-X0",2500,23,10900,130,"NA",0.82,7.5,59,48,330,24,3.8203389830508474,0.84821865547813202,3.0811871251244245,null,0.10416666666666667,0.42940249577095035,0.25459449541284401,0.29623014975345235,1665.048,0,-2775.08,0,0,0,0,0,0.82302145022765483,1.1043331349206349,9.8762574027318575,26.503995238095236,16.253371340696813,1280.8061538461538,203.84663052713395,1766.6707979018277,52347.10772804985,5446.7801745618472,-42282.490000000005,0.84821865547813202,5010.5959164578917,963.66110780709619,-50538.385300000002,3.0811871251244245,4244.8497820722996,680.98877529460856,-50671.938020086978,3.375753618705875,null,59]
["ICH","ICH11-030-A1",175.16066937328333,2.8637222236513655,404.68872564617027,8.9,"NA",3.8,47,34.699696967550494,2.5,675,32,6.4957339601779047,2.7439355436424613,5.3239174042108219,null,2,0.86726809642745806,0.97037543947628446,0.23642818329453011,235.62,0,-392.7,0,0,0,0,0,0.20696791013359392,0.3576963630358474,2.4836149216031269,8.5847127128603375,4.8319108819588505,181.24615384615385,28.846221301009521,250.00058460874919,6263.4428302573915,1016.318701201746,-49947.315700000006,2.7439355436424613,1727.8847032599774,327.01735403864399,-50716.344199129038,5.3239174042108219,2695.3331650561454,551.77094290730361,-50552.308061187992,4.2296141943206971,null,49.072782061746295]
["ICH","ICH11-030-A5",175.16066937328333,4.9601123901282884,404.68872564617027,15.5,"NA",1.3,16,20.033879385013719,2.5,675,32,11.250941251478721,4.7338148935203694,9.2331072912061583,null,2,0.86726809642745806,0.97037543947628446,0.13680380310850007,235.62,0,-392.7,0,0,0,0,0,0.35847893588773411,0.62289499358159961,4.3017472306528095,14.94947984595839,8.3967480159548877,181.24615384615385,28.846221301009521,250.00058460874919,2179.7356662345665,349.5994469480712,-50500.643125000002,4.7338148935203694,583.47062082317848,111.87435796058872,-50773.976058835477,9.2331072912061583,923.25145937003572,189.38699758323503,-50715.794434343938,7.3097383060827106,null,28.332183933233065]
["ICH","ICH11-050-A1",298.57480806320996,2.9348587565849433,674.48120941028378,8.9,"NA",5.0999999999999996,78,57.714632204180219,3.5,675,32,3.9054220982053574,1.624687831441479,3.1561906049677511,null,1.4285714285714286,0.57662632731578334,0.65985529884387351,0.31155101235027605,267.036,0,-445.06,0,0,0,0,0,0.14102640216667853,0.21914110429004943,1.6923168260001424,5.2593865029611866,2.7850482908111887,205.41230769230768,32.692384141144124,283.33399588991574,17265.44258576358,2268.6983063372681,-49259.970925000001,1.624687831441479,4846.2300492097247,748.12461689925408,-50637.134179069079,3.1561906049677511,4695.4855843492178,709.93644274503902,-50653.850193643208,3.2097472335467891,null,81.620815610526378]
["ICH","ICH11-050-A5",298.57480806320996,5.083324479443541,674.48120941028378,15.5,"NA",1.7,26,33.321558439263704,3.5,675,32,6.7643894990939266,2.8780765048410202,5.5283115064931776,null,1.4285714285714286,0.57662632731578334,0.65985529884387351,0.17795356623800243,267.036,0,-445.06,0,0,0,0,0,0.24426489376132876,0.38093956729248241,2.9311787251359451,9.1425496150195773,4.8238451412178396,205.41230769230768,32.692384141144124,283.33399588991574,5806.3592094868563,760.39027929007466,-50284.418125000004,2.8780765048410202,1615.410016403242,249.37487229975144,-50749.151393023029,5.5283115064931776,1565.1618614497397,236.64548091501308,-50754.723397881069,5.6194434376356295,null,47.12379986421422]
["ICH","ICH11-075-A1",454.73089841680786,2.9839137873774302,1011.7218141154258,8.9,"NA",6.7,117,86.454612708295386,4.8,675,32,2.6071483399100659,1.057460934219332,2.0759205331961397,null,1.0416666666666667,0.43651614792753829,0.50718289636627134,0.43908710015146118,307.8768,0,-513.12800000000004,0,0,0,0,0,0.10854387935115561,0.15017413986999115,1.3025265522138674,3.6041793568797877,2.1435698636604563,236.8283076923077,37.692395833319111,326.6674305554323,38826.943642965867,4464.6108531582267,-48138.357325000004,1.057460934219332,10998.638704487381,1496.8554921363757,-50505.393283368554,2.0759205331961397,9293.1293122144234,1075.303963797907,-50650.461481656959,2.2774524682120116,null,122.26528582178425]
["ICH","ICH11-075-A5",454.73089841680786,5.1682902851429846,1011.7218141154258,15.5,"NA",2.2000000000000002,39,49.914593919819197,4.8,675,32,4.5157133875930864,1.8998949513873042,3.6526072222829495,null,1.0416666666666667,0.43651614792753829,0.50718289636627134,0.25055028208032837,307.8768,0,-513.12800000000004,0,0,0,0,0,0.18800351388682782,0.2604794607150524,2.2560421666419339,6.2515070571612572,3.7127719134334014,236.8283076923077,37.692395833319111,326.6674305554323,13057.54082967803,1474.0511466764369,-49933.052500000005,1.8998949513873042,3666.2129014957954,491.50478846269067,-50708.198255168449,3.6526072222829495,3097.7097707381431,353.08488363513379,-50755.121628729321,3.9912148240144161,null,70.589895681753688]
["ICH","ICH11-100-A1",611.81557163638524,3.0134151426335043,1348.9624188205676,8.9,"NA",8.3000000000000007,156,115.18118325320502,6.1,675,32,1.956916864662684,0.77110817811617149,1.5380392238605438,null,0.81967213114754101,0.36747784080949153,0.43084669512747031,0.57022839875448805,348.7176,0,-581.19600000000003,0,0,0,0,0,9.2280274173132171E-2,0.11927510704966897,1.107363290077586,2.8626025691920551,1.8223893959778996,268.2443076923077,42.69240752549409,370.00086522094881,69004.560236807534,7368.5199964111671,-46712.577325000006,0.77110817811617149,19656.518331788568,2494.8774984250767,-50335.98444031192,1.5380392238605438,15603.672081840174,1508.7991803944744,-50633.566905034488,1.7536832647834331,null,162.89079148686278]
["ICH","ICH11-100-A5",611.81557163638524,5.2193881313386443,1348.9624188205676,15.5,"NA",2.8,52,66.49988715681755,6.1,675,32,3.389479435784156,1.4060458660721982,2.7167119923355298,null,0.81967213114754101,0.36747784080949153,0.43084669512747031,0.32520129980042917,348.7176,0,-581.19600000000003,0,0,0,0,0,0.15983412340425099,0.2065905454882434,1.9180094808510117,4.9581730917178417,3.1564710250084795,268.2443076923077,42.69240752549409,370.00086522094881,23206.366802531826,2499.4316765945491,-49392.490000000005,1.4060458660721982,6552.1727772628574,841.64542115544771,-50644.976966702518,2.7167119923355298,5201.22402728006,508.99249459090703,-50746.575741129498,3.0750184596853827,null,94.045042313451447]
["ICH","ICH11-150-A1",927.18464906955387,6.0944012777031107,2023.4436282308516,17.899999999999999,"NA",2.9,59,86.308816616386423,8.6,675,32,2.6115524327233794,1.0607400041230501,2.0678681380842612,null,0.58139534883720934,0.29709912937022914,0.35192282605006581,0.41187027241830354,427.25759999999997,0,-712.096,0,0,0,0,0,0.15088677613653387,0.1950258225533581,1.8106413136384063,4.6806197412805943,2.9797750742332596,328.65969230769224,52.307814625830595,453.33439342386521,39699.316510951685,3880.0455370404484,-48784.173925000003,1.0607400041230501,11187.623803502884,1321.0365630438862,-50570.888557365884,2.0678681380842612,8342.9123911101942,645.90295967391796,-50749.15533224777,2.4279489610368876,null,122.05909901126559]
["ICH","ICH11-150-A5",927.18464906955387,10.555812654694471,2023.4436282308516,30.9,"NA",1,20,49.830418506908735,8.6,675,32,4.523341500106997,1.8756765523610455,3.6072017321127126,null,0.58139534883720934,0.29709912937022914,0.35192282605006581,0.23663860899963704,427.25759999999997,0,-712.096,0,0,0,0,0,0.26134356245874785,0.33779463345032851,3.1361227495049744,8.1070712028078837,5.1611218236993288,328.65969230769224,52.307814625830595,453.33439342386521,13526.348317406637,1333.4712167231698,-50089.052500000005,1.8756765523610455,3771.8078603226631,455.52984932547804,-50721.591114399249,3.6072017321127126,2791.1546874208452,222.72515850824755,-50785.182116140706,4.2258531024475969,null,70.470853671197361]
["ICH","ICH11-200-A1",1250.5593222258879,10.578973306845628,2697.9248376411351,30.6,"NA",1.2,27,67.062656446351482,11.2,675,32,3.361035961650499,1.3900770916491951,2.6656284721008654,null,0.44642857142857145,0.2623852514697389,0.31440164239031615,0.31495710804762028,508.93919999999997,0,-848.23199999999997,0,0,0,0,0,0.23131388095069547,0.298980341786864,2.7757665714083455,7.1755282028847365,4.5680831311376409,391.49169230769229,62.307838010180561,540.00126275489822,24234.867246387279,2132.6228427731326,-49793.891200000005,1.3900770916491951,6856.441571014193,737.28627866883051,-50684.292149674897,2.6656284721008654,4937.2620158679001,318.3659618676715,-50782.623225827578,3.1750355030844517,null,94.84091827519741]
["ICH","ICH11-200-A5",1250.5593222258879,18.323319259371566,2697.9248376411351,53,"NA",0.4,9,38.718642751872416,11.2,675,32,5.8214850516447862,2.4558911870857068,4.6594912344019042,null,0.44642857142857145,0.2623852514697389,0.31440164239031615,0.18104267739070662,508.93919999999997,0,-848.23199999999997,0,0,0,0,0,0.4006473943025432,0.51784914243915681,4.8077687316305182,12.428379418539762,7.9121520763287165,391.49169230769229,62.307838010180561,540.00126275489822,8078.101713858041,710.8641583313256,-50468.08,2.4558911870857068,2285.4805236713973,245.76209288961013,-50764.870716558304,4.6594912344019042,1645.7540052892998,106.12198728922385,-50797.647741942528,5.523559496647902,null,54.756429696376514]
["ICH","ICH11-250-A1",1568.82610601437,10.620308277258449,3372.4060470514191,30.6,"NA",1.5,33,83.802632253092327,13.8,675,32,2.6896529851147095,1.1164628242450831,2.1338249525590691,null,0.36231884057971014,0.24272345482797436,0.29188893219446638,0.39119486245530288,590.62080000000003,0,-984.36800000000005,0,0,0,0,0,0.21481649303285863,0.27765695791559225,2.5777979163943034,6.6637669899742136,4.2422858242679862,454.32369230769234,72.307861394530534,626.66813208593135,36507.24598941439,3331.2020671749046,-49225.052500000005,1.1164628242450831,10574.473995864924,1156.1566303018985,-50614.825275411997,2.1338249525590691,7589.5753817369559,461.82716690680746,-50774.79008103755,2.5562707897633956,null,118.51481909488771]
["ICH","ICH11-250-A5",1568.82610601437,18.39491352825593,3372.4060470514191,53,"NA",0.5,11,48.383472290122072,13.8,675,32,4.6586156249479735,1.9875588674276534,3.7398704953701283,null,0.36231884057971014,0.24272345482797436,0.29188893219446638,0.22469132626261659,590.62080000000003,0,-984.36800000000005,0,0,0,0,0,0.3720730802366769,0.48091595818481941,4.4648769628401226,11.541982996435665,7.3478545878613675,454.32369230769234,72.307861394530534,626.66813208593135,12168.802100659146,1110.3848773534733,-50278.472500000003,1.9875588674276534,3524.8246652883081,385.38554343396623,-50741.715091803999,3.7398704953701283,2529.8584605789852,153.94238896893586,-50795.036693679183,4.4505500796733548,null,68.424562707393221]
["ICH","ICH22-030-A1",342.42727740624485,2.8200649546478425,710.11417896403464,8.9,"NA",7.5,94,69.489983101853994,4.9000000000000004,675,32,3.2436329660581875,1.2982533108654852,2.6210761966565044,null,1.0204081632653061,0.58559255299412794,0.72997274995441797,0.37704817677526697,311.01840000000004,0,-518.36400000000003,0,0,0,0,0,0.13761741970012498,0.23872040562945882,1.6514090364014997,5.7292897351070113,2.7177262812724416,239.2449230769231,38.077012117332572,330.00077168354898,25066.353193966188,4017.0210525400244,-47463.488125000003,1.2982533108654852,6860.7233332588894,1272.8382350955856,-50469.652669675488,2.6210761966565044,6715.92848397329,1226.6476052710909,-50493.561600347173,2.6521809720778271,null,98.273676551718765]
["ICH","ICH22-030-A5",342.42727740624485,4.8844957820944845,710.11417896403464,15.5,"NA",2.5,31,40.120060449837951,4.9000000000000004,675,32,5.6181370983181163,2.368752356871032,4.6305574503071538,null,1.0204081632653061,0.58559255299412794,0.72997274995441797,0.21357286226604499,311.01840000000004,0,-518.36400000000003,0,0,0,0,0,0.23836036292714657,0.41516551684861042,2.8603243551257589,9.9639724043666504,4.7072400002290937,239.2449230769231,38.077012117332572,330.00077168354898,8285.4885811371605,1346.3684225984211,-49678.988125000003,2.368752356871032,2272.5740345890254,424.27941169852852,-50693.324223225165,4.6305574503071538,2225.330536344301,408.88253509036366,-50701.293866782391,4.682242815823261,null,56.738333611389045]
["ICH","ICH22-050-A1",583.67665954224049,2.890117015516144,1183.5236316067244,8.9,"NA",10.1,156,115.57658677919602,6.8,675,32,1.9502219807772727,0.74224515665521285,1.540765754118973,null,0.73529411764705888,0.4094853642431639,0.52204111814922016,0.58309733168406652,370.70880000000005,0,-617.84800000000007,0,0,0,0,0,9.8621718233666167E-2,0.134686691533043,1.183460618803994,3.2324805967930321,1.9476228818410022,285.16061538461543,45.384721513588318,393.33425311776546,69095.802672728169,8997.2932723875565,-44745.000925,0.74224515665521285,19235.561853783965,2921.7112786647422,-50166.109962379021,1.540765754118973,16027.140408162546,1968.913960891698,-50514.949081663224,1.7149795508613637,null,163.44997651592939]
["ICH","ICH22-050-A5",583.67665954224049,5.0058295106932906,1183.5236316067244,15.5,"NA",3.4,52,66.728173488986982,6.8,675,32,3.3778835567438499,1.3839742862959583,2.733218745442529,null,0.73529411764705888,0.4094853642431639,0.52204111814922016,0.33119180571590584,370.70880000000005,0,-617.84800000000007,0,0,0,0,0,0.17081782671045176,0.23348535152943803,2.0498139205254211,5.6036484367065125,3.3733817853323318,285.16061538461543,45.384721513588318,393.33425311776546,23236.780947838703,3045.4430616318159,-48722.192500000005,1.3839742862959583,6411.8539512613243,983.54637103565619,-50587.904286788595,2.733218745442529,5342.3801360541838,662.80271950809663,-50706.497960514469,3.0193983750243913,null,94.36788794050986]
["ICH","ICH22-075-A1",888.92530223322842,5.8768484107682353,1775.2854474100868,17.899999999999999,"NA",3.3,59,86.563288020543851,9.3000000000000007,675,32,2.6038752126248528,1.0468273759207254,2.0808641819662239,null,0.5376344086021505,0.32583630544733377,0.42176203330699696,0.41694020735255782,449.24880000000002,0,-748.74800000000005,0,0,0,0,0,0.15957421448656306,0.2062546051775089,1.9148905738387567,4.9501105242602135,3.1513382351489057,345.57600000000002,55.000128613924829,476.66778132068185,39743.307518158297,4428.2420016453707,-48188.211325000004,1.0468273759207254,10969.477181860942,1453.8607245735616,-50523.076216391586,2.0808641819662239,8492.7771854884777,779.60270023895987,-50724.049107398903,2.3984254393446309,null,122.41897592226115]
["ICH","ICH22-075-A5",888.92530223322842,10.179000035830994,1775.2854474100868,30.9,"NA",1.1000000000000001,20,49.977337640600098,9.3000000000000007,675,32,4.5100441648354588,1.8668518057592127,3.6390944801692,null,0.5376344086021505,0.32583630544733377,0.42176203330699696,0.23916349675064136,449.24880000000002,0,-748.74800000000005,0,0,0,0,0,0.27639064706862077,0.35724345546250413,3.316687764823449,8.5738429311000992,5.458277935112342,345.57600000000002,55.000128613924829,476.66778132068185,13541.011986475507,1471.1430799091427,-49938.669925000002,1.8668518057592127,3696.1052109145839,484.62024152452045,-50711.132072130531,3.6390944801692,2842.316071113677,259.86756674631994,-50778.123035799639,4.1812400871635873,null,70.678628702635791]
["ICH","ICH22-100-A1",1202.9831045137794,10.239008031593199,2367.0472632134488,30.6,"NA",1.4,27,67.237972465825109,11.8,675,32,3.3522724099773167,1.3769511797616734,2.6819155566796358,null,0.42372881355932202,0.28286450722955631,0.37162249088588545,0.31765940719838337,527.78880000000004,0,-879.64800000000002,0,0,0,0,0,0.2413543301146733,0.31195793271397132,2.8962519613760795,7.4869903851353117,4.7663661147031133,405.99138461538467,64.615535714261327,560.00130952359825,24258.412298060965,2494.5643001769172,-49428.710800000001,1.3769511797616734,6730.8027948695726,834.70143479859883,-50651.049190357589,2.6819155566796358,4999.8212684021119,388.56231213435768,-50771.7641784691,3.1480257701780703,null,95.08885256763827]
["ICH","ICH22-100-A5",1202.9831045137794,17.734482129825221,2367.0472632134488,53,"NA",0.5,9,38.819861502908779,11.8,675,32,5.8063061348920773,2.4391115356992596,4.6898872535516567,null,0.42372881355932202,0.28286450722955631,0.37162249088588545,0.1825124604996034,527.78880000000004,0,-879.64800000000002,0,0,0,0,0,0.41803796238536522,0.54032698928475154,5.0164555486243829,12.967847742834037,8.2555882781404595,405.99138461538467,64.615535714261327,560.00130952359825,8085.950064415937,890.90313517218283,-50278.472500000003,2.4391115356992596,2243.6009316231912,298.10765528521398,-50746.189026922548,4.6898872535516567,1666.6070894673712,138.77225433369921,-50792.380986659096,5.4790779613766318,null,54.899574626858602]
["ICH","ICH22-150-A1",1823.0643897122618,10.353804682819181,3550.5708948201736,30.6,"NA",1.9,40,100.76622866476333,16.8,675,32,2.2368605334022935,0.90384357655723857,1.7723102796471393,null,0.29761904761904762,0.24220504721961481,0.32148294846477393,0.47107766225110298,684.86880000000008,0,-1141.4480000000001,0,0,0,0,0,0.20897864600874072,0.27011136017024018,2.5077437521048886,6.4826726440857643,4.1269975830114269,526.82215384615392,83.846349914934351,726.66836592943105,53473.377106525775,5073.6518602411443,-48269.965300000003,0.90384357655723857,15113.367871085928,1716.7189669790525,-50514.912557657517,1.7723102796471393,10941.802425763957,684.27937791688328,-50759.045564746637,2.1227922275519839,null,142.50496720689634]
["ICH","ICH22-150-A5",1823.0643897122618,17.933315762287386,3550.5708948201736,53,"NA",0.6,13,58.177409244824503,16.8,675,32,3.8743560932983918,1.6640314167334556,3.1447419466181037,null,0.29761904761904762,0.24220504721961481,0.32148294846477393,0.26963049324699595,684.86880000000008,0,-1141.4480000000001,0,0,0,0,0,0.36196163258408992,0.46784659951639235,4.3435395910090788,11.228318388393417,7.1481694964897455,526.82215384615392,83.846349914934351,726.66836592943105,17111.100607248991,1602.183035769737,-50046.73,1.6640314167334556,4956.1636096308193,542.12177904601651,-50718.326970157927,3.1447419466181037,3634.2988091444195,216.08822460533159,-50791.363991669357,3.7087793296581868,null,82.275281177760405]
["ICH","ICH22-200-A1",2444.5479347532541,10.417697510043947,4734.0945264268976,30.6,"NA",2.5,53,134.28879580831176,21.7,675,32,1.6784721215442528,0.65668693779293574,1.3134592555496059,null,0.2304147465437788,0.22122866930384436,0.2953071579361054,0.62614939638685452,838.80719999999997,0,-1398.0119999999999,0,0,0,0,0,0.19205777977974958,0.24824061749072115,2.304693357356995,5.9577748197773079,3.7928372495839375,645.23630769230772,102.6925478315939,890.00208120714717,94086.355583760698,8896.7594089418708,-46415.972500000003,0.65668693779293574,26848.357924610704,3028.880664771038,-50296.433024636994,1.3134592555496059,19201.906640304009,1102.7438067588594,-50737.727432491418,1.5970629465913739,null,189.91303630686505]
["ICH","ICH22-200-A5",2444.5479347532541,18.043981385279899,4734.0945264268976,53,"NA",0.8,18,77.531672409079505,21.7,675,32,2.9071989936025688,1.193638036521721,2.3113423587922233,null,0.2304147465437788,0.22122866930384436,0.2953071579361054,0.35891703822411491,838.80719999999997,0,-1398.0119999999999,0,0,0,0,0,0.33265383256740083,0.42996536199620028,3.9918459908088102,10.319168687908807,6.5693868211191786,645.23630769230772,102.6925478315939,890.00208120714717,32327.033895792491,2846.9224711362099,-49456.840000000004,1.193638036521721,9061.3776285086824,969.24181272673252,-50648.879073168486,2.3113423587922233,6415.4713813224571,352.87801816283519,-50784.444715261365,2.7861591774742669,null,109.64634263438774]
["ICH","ICH22-250-A1",3066.6708916086786,10.458402331377483,5917.6181580336224,30.6,"NA",3,66,167.80882279225321,26.7,675,32,1.3431951684628911,0.50803129552572546,1.0396348360115704,null,0.18726591760299627,0.20937305725982022,0.28048649907339446,0.78211643155205146,995.88720000000001,0,-1659.8119999999999,0,0,0,0,0,0.18247563918114459,0.23585540455215415,2.189707670173735,5.6605297092516995,3.6036051349837481,766.06707692307691,121.92336203226692,1056.66913761298,146097.26027439127,13340.991382883771,-44484.73,0.50803129552572546,41936.323465044428,4559.6554046287101,-50066.857289556508,1.0396348360115704,29795.424382817342,1571.1001651350946,-50717.504702710052,1.2785820111406878,null,237.31751307866699]
["ICH","ICH22-250-A5",3066.6708916086786,18.114484203942595,5917.6181580336224,53,"NA",1,22,96.884469011501594,26.7,675,32,2.3264822762587651,0.95538802947242019,1.8482132550227706,null,0.18726591760299627,0.20937305725982022,0.28048649907339446,0.44745467907825426,995.88720000000001,0,-1659.8119999999999,0,0,0,0,0,0.31605707820534851,0.40851354392404277,3.7926849384641819,9.8043250541770259,6.2416271842079531,766.06707692307691,121.92336203226692,1056.66913761298,48697.96717488116,4446.9338039947097,-48698.41,0.95538802947242019,13978.774488348139,1519.8851348762362,-50559.059096518838,1.8482132550227706,9931.8081276057801,523.70005504503138,-50775.941567570022,2.2348632090739908,null,137.01533005938091]
["ICH","ICH33-030-A1",511.19187514079709,2.8053615583674194,1065.171268446052,8.9,"NA",11.3,141,104.28169119278212,7.2,675,32,2.1614532466999452,0.79850486864634496,1.7123076102726806,null,0.69444444444444442,0.48339771313324809,0.59970825248780446,0.54557727217154928,383.27519999999998,0,-638.79199999999992,0,0,0,0,0,0.11300878015222797,0.17538175820929669,1.3561053618267356,4.2091621970231206,2.231744589482159,294.8270769230769,46.923186649642155,406.66761763023197,56409.035863584788,9082.5364106771831,-43219.416324999998,0.79850486864634496,15398.820662455146,2862.8987077512552,-50051.464654008611,1.7123076102726806,13737.848468897062,2277.5170217194959,-50328.172353392147,1.8329209279919632,null,147.47658199203488]
["ICH","ICH33-030-A5",511.19187514079709,4.8590287526929732,1065.171268446052,15.5,"NA",3.8,47,60.207062481702174,7.2,675,32,3.7437468414690125,1.5151535833665943,3.0457805507036468,null,0.69444444444444442,0.48339771313324809,0.59970825248780446,0.30835954268103355,383.27519999999998,0,-638.79199999999992,0,0,0,0,0,0.19573694892504015,0.30458346083414939,2.3488433871004819,7.3100030600195849,3.8654950185000465,294.8270769230769,46.923186649642155,406.66761763023197,18970.359000542881,3071.095805627433,-48203.252500000002,1.5151535833665943,5132.940220818381,962.74469818183786,-50549.461962656853,3.0457805507036468,4579.2828229656861,765.89067987027283,-50643.33757967694,3.2429675803300757,null,85.145644312267251]
["ICH","ICH33-050-A1",768.78560211416482,8.7788455646958372,1908.9090832366524,30.6,"NA",1.3,20,50.560016241167531,10.199999999999999,675,32,4.4580681882074309,1.8613119965258726,3.7632768498352887,null,0.49019607843137258,0.40046729112412499,0.41692504215578385,0.24406643977105238,477.52319999999997,0,-795.87199999999996,0,0,0,0,0,0.29297004187423176,0.387385833359638,3.5156405024907813,9.2972600006313115,5.7856947482526033,367.32553846153849,58.461675170045964,506.66785147373167,13386.201309108725,1741.8173623584621,-49618.323700000001,1.8613119965258726,3447.6808082345478,499.71064137420876,-50707.476145923676,3.7632768498352887,2943.4766569950789,329.33410345792669,-50762.73137073496,4.0972449999190976,null,71.502660682062825]
["ICH","ICH33-050-A5",768.78560211416482,15.20540654985388,1908.9090832366524,53,"NA",0.4,7,29.190838987069938,10.199999999999999,675,32,7.7216006055817985,3.1768302922936238,6.4958948596132844,null,0.49019607843137258,0.40046729112412499,0.41692504215578385,0.14091961936334771,477.52319999999997,0,-795.87199999999996,0,0,0,0,0,0.50743899762175093,0.67097119842779185,6.0892679714610107,16.103308762267005,10.021117261057933,367.32553846153849,58.461675170045964,506.66785147373167,4831.9748640805865,535.93617215637607,-50468.08,3.1768302922936238,1179.6819262473703,153.75712042283354,-50777.41547339844,6.4958948596132844,994.38690066686536,101.33357029474672,-50793.109265060819,7.096243975947707,null,41.282080392563458]
["ICH","ICH33-075-A1",1170.8433585035712,8.9255805782743938,2863.3636248549783,30.6,"NA",1.7,30,75.735883204766836,13.8,675,32,2.9761321907422249,1.2174926591904538,2.4834020386251763,null,0.36231884057971014,0.32522787075702958,0.34378029791792708,0.3584316872992977,590.62080000000003,0,-984.36800000000005,0,0,0,0,0,0.24190396389520649,0.31266835136626331,2.9028475667424778,7.504040432790319,4.777220512160099,454.32369230769234,72.307861394530534,626.66813208593135,30103.167655109683,3411.9501233123901,-48775.599700000006,1.2174926591904538,7809.1015821296896,995.21685472803904,-50632.483969581037,2.4834020386251763,6329.825104828622,532.6679122730435,-50755.693670856243,2.7899319045555808,null,107.10671318648558]
["ICH","ICH33-075-A5",1170.8433585035712,15.45955904862125,2863.3636248549783,53,"NA",0.6,10,43.726132555586183,13.8,675,32,5.1548121644068035,2.1741025646772396,4.3481199179729177,null,0.36231884057971014,0.32522787075702958,0.34378029791792708,0.20568564316453644,590.62080000000003,0,-984.36800000000005,0,0,0,0,0,0.4189899560188049,0.54155747048516578,5.027879472225659,12.997379291643979,8.2743886460215048,454.32369230769234,72.307861394530534,626.66813208593135,10034.157899516744,1204.2005429557923,-50046.73,2.1741025646772396,2603.0338607098961,351.25300755107253,-50740.630549185997,4.3481199179729177,2109.9417016095404,188.00043962578002,-50786.674312984345,4.8617880403060445,null,61.838089690233488]
["ICH","ICH33-100-A1",1575.2892534803184,9.0138259976361308,3817.8181664733047,30.6,"NA",2.1,40,100.89984816513028,17.5,675,32,2.2338983070729279,0.89329683915610025,1.8456351004065232,null,0.2857142857142857,0.28930165039983513,0.30857938975345844,0.47410750875117136,706.86,0,-1178.0999999999999,0,0,0,0,0,0.2173095614610894,0.2808793259278663,2.6077147375330729,6.7411038222687916,4.2915199808389906,543.73846153846159,86.538663903028564,750.00175382624752,53500.323626952748,5615.1565081904509,-47708.149300000005,0.89329683915610025,13939.667194585236,1654.05371615434,-50536.428736974958,1.8456351004065232,11032.825873670223,787.50184151756264,-50744.245297060304,2.1092262441361922,null,142.69393371651279]
["ICH","ICH33-100-A5",1575.2892534803184,15.612404598491,3817.8181664733047,53,"NA",0.7,13,58.254554499330339,17.5,675,32,3.8692253667924121,1.651286779123754,3.2663636927009243,null,0.2857142857142857,0.28930165039983513,0.30857938975345844,0.27118452748909633,706.86,0,-1178.0999999999999,0,0,0,0,0,0.37639120142111854,0.48649726330276272,4.5166944170534222,11.675934319266306,7.4331306485101463,543.73846153846159,86.538663903028564,750.00175382624752,17120.08278072465,1871.6921834631667,-49772.852500000001,1.651286779123754,4584.6907025800228,551.35123871811334,-50715.582912324986,3.2663636927009243,3663.5853590150782,262.50061383918751,-50784.855099020104,3.6875260150681259,null,82.384381042955283]
["ICH","ICH33-150-A1",2387.2665234552542,9.1148862796546126,5726.7272497099566,30.6,"NA",2.9,60,151.21296389849255,24.9,675,32,1.490612935484211,0.56445465104949166,1.2094185268520896,null,0.20080321285140562,0.2536874503807538,0.27337848158898986,0.70764348720796622,939.33839999999998,0,-1565.5639999999999,0,0,0,0,0,0.19269435506634111,0.24906341072723584,2.3123322607960932,5.9775218574536604,3.8054086042143913,722.56799999999998,115.00026892002462,996.6689973068801,120334.33505218121,11620.881752758818,-44899.069300000003,0.56445465104949166,31513.566999203613,3461.5364590101303,-50281.125634447293,1.2094185268520896,24372.752207249749,1445.170046094981,-50713.820243226481,1.4131409644502451,null,213.84742435188062]
["ICH","ICH33-150-A5",2387.2665234552542,15.78744614157425,5726.7272497099566,53,"NA",1,20,87.30284541175584,24.9,675,32,2.5818173386780425,1.053045010032027,2.1390755262629133,null,0.20080321285140562,0.2536874503807538,0.27337848158898986,0.40495333405210776,939.33839999999998,0,-1565.5639999999999,0,0,0,0,0,0.33375641330662004,0.43139048168596777,4.0050769596794407,10.353371560463227,6.5911610460590904,722.56799999999998,115.00026892002462,996.6689973068801,40110.519741981137,4007.1435433100528,-48698.41,1.053045010032027,10504.522333067873,1193.6332617276312,-50618.227408245169,2.1390755262629133,8124.2507357499162,498.33449865344181,-50772.577447048687,2.4694203403479671,null,123.4648680150664]
["ICH","ICH33-200-A1",3201.0792522061433,13.756700702128253,7635.6363329466094,45.9,"NA",1.7,35,134.34500088183421,32.200000000000003,675,32,1.6777699097136858,0.65907380494491874,1.3729822932930413,null,0.15527950310559005,0.23538306667993056,0.25509229552952567,0.62325759223608634,1168.6752000000001,0,-1947.7920000000001,0,0,0,0,0,0.26984119988874183,0.34877809251797509,3.2380943986649022,8.3706742204314022,5.328936716774221,898.9809230769232,143.07725765300725,1240.0028996593962,92673.262940994799,9078.4927090477304,-46238.649325000006,0.65907380494491874,24751.833778263797,2720.9173643752315,-50394.967530204303,1.3729822932930413,19054.440929418106,1054.0024647104906,-50743.608274543229,1.6044730340343867,null,189.99252228411467]
["ICH","ICH33-200-A5",3201.0792522061433,23.827304560604581,7635.6363329466094,79.5,"NA",0.6,12,77.564122423407497,32.200000000000003,675,32,2.9059827270343512,1.183750532246834,2.4018840241477561,null,0.15527950310559005,0.23538306667993056,0.25509229552952567,0.35787896965074073,1168.6752000000001,0,-1947.7920000000001,0,0,0,0,0,0.46737866818265017,0.60410137680809128,5.608544018191802,14.498433043394192,9.2299891437722312,898.9809230769232,143.07725765300725,1240.0028996593962,32332.066756557018,3204.128271031746,-49098.692500000005,1.183750532246834,8380.1163126618085,960.32377566184641,-50651.870080491579,2.4018840241477561,6370.9132835178571,372.00086989782017,-50782.157971109584,2.7942407484181437,null,109.69223388474958]
["ICH","ICH33-250-A1",4015.7289257162465,13.810451931099834,9544.5454161832604,45.9,"NA",2,44,167.87880569164045,39.6,675,32,1.3426352366004699,0.50797635434845356,1.0864570777876703,null,0.12626262626262627,0.22495682467769296,0.24466916947563108,0.77927947743184922,1401.1536000000001,0,-2335.2559999999999,0,0,0,0,0,0.25889628448201096,0.33463145101214087,3.1067554137841316,8.0311548242913808,5.1127919560891817,1077.8104615384614,171.53886267000328,1486.6701431400286,146120.75266792095,13346.555102610415,-44484.73,0.50797635434845356,38860.119708755214,4015.7289257162606,-50232.974252376349,1.0864570777876703,29646.624622680392,1486.6701431400338,-50726.73807524125,1.2832366679224574,null,237.41648384411462]
["ICH","ICH33-250-A5",4015.7289257162465,23.920404420152629,9544.5454161832604,79.5,"NA",0.7,15,96.92487365730149,39.6,675,32,2.3255124458242746,0.93454753190943851,1.9111315626017036,null,0.12626262626262627,0.22495682467769296,0.24466916947563108,0.44681392049980345,1401.1536000000001,0,-2335.2559999999999,0,0,0,0,0,0.44842151861364887,0.57959867496352369,5.3810582233637865,13.910368199124569,8.8556154364759259,1077.8104615384614,171.53886267000328,1486.6701431400286,50512.983741677104,4671.2277683698949,-48482.468125000007,0.93454753190943851,13116.981628372785,1405.505124000691,-50594.881737748306,1.9111315626017036,9904.6318437134305,520.33455009901172,-50776.339942651161,2.238068140046769,null,137.07247085745402]
["ICH","ICH44-030-A1",599.91929812416197,4.2717615244621898,1527.1272665893216,15.3,"NA",5.0999999999999996,64,81.082140536308216,9.6,675,32,2.7798970094908495,1.083951853971536,2.3171938960205067,null,0.52083333333333337,0.49293394567377158,0.50058434337783264,0.41010940402645379,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.17547468860254609,0.25953190957658939,2.1056962632305529,6.2287658298381459,3.4653474389536467,352.82584615384616,56.153977465965212,486.66780470503181,34298.821844961727,5479.2036686226365,-46238.649325000006,1.083951853971536,8735.5136735873893,1529.794210216618,-50449.18818322452,2.3171938960205067,7996.5589841628016,1241.0029019978354,-50570.901594236537,2.4383737368175438,null,114.66746281268797]
["ICH","ICH44-030-A5",599.91929812416197,7.3989079981863934,1527.1272665893216,26.5,"NA",1.7,21,46.812795665108624,9.6,675,32,4.8149228602469325,2.0224107698676224,4.1009612102740931,null,0.52083333333333337,0.49293394567377158,0.50058434337783264,0.23271059578649109,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.30393107610193715,0.44951966343569111,3.6471729132232458,10.788471922456587,6.0021578301464036,352.82584615384616,56.153977465965212,486.66780470503181,11146.144850434186,1826.3752155803427,-49283.033125000002,2.0224107698676224,2889.5012684521448,509.93140340553953,-50686.502727741507,4.1009612102740931,2650.8203470388812,413.66763399927856,-50727.073864745515,4.2971829306710507,null,66.203290522196809]
["ICH","ICH44-050-A1",1022.575911581599,4.3778745761609796,2545.2121109822028,15.3,"NA",6.8,106,134.85641663498313,13.5,675,32,1.671407305816911,0.61163886910579435,1.3636853312516271,null,0.37037037037037035,0.36644168694010099,0.3805812473625988,0.65704046419460771,581.19600000000003,0,-968.66,0,0,0,0,0,0.13368631207505074,0.1727936910320724,1.6042357449006091,4.1470485847697374,2.6400931260334106,447.0738461538462,71.15401254249015,616.66810870158133,94239.128011742403,12150.736160907079,-42686.918799999999,0.61163886910579435,24412.974070659635,3476.7580993774491,-50140.490548296591,1.3636853312516271,20450.747589258492,2096.6715695853841,-50563.437219354011,1.5219762777103658,null,190.71577337822913]
["ICH","ICH44-050-A5",1022.575911581599,7.5827011950748808,2545.2121109822028,26.5,"NA",2.2999999999999998,35,77.859388446155833,13.5,675,32,2.8949623738167021,1.1812159095625892,2.4274712996173022,null,0.37037037037037035,0.36644168694010099,0.3805812473625988,0.37327816214838866,581.19600000000003,0,-968.66,0,0,0,0,0,0.23155148479049659,0.29928745209490804,2.778617817485959,7.1828988502777928,4.57277543100321,447.0738461538462,71.15401254249015,616.66810870158133,30936.270514906533,4109.7492969511104,-48018.983125000006,1.1812159095625892,8098.6809818064557,1175.9622983188428,-50577.03923446079,2.4274712996173022,6802.7409391623469,709.16832500682085,-50722.198483372587,2.6789673262548686,null,110.10980309862825]
["ICH","ICH44-075-A1",1557.3551744449078,8.9020981182865899,3817.8181664733047,30.6,"NA",2.2000000000000002,40,101.00309132098027,18.3,675,32,2.2316148649717626,0.88773577041157314,1.8478368824256608,null,0.27322404371584696,0.30303790451791829,0.319551101389137,0.47652907071312745,731.99279999999999,0,-1219.9880000000001,0,0,0,0,0,0.2248060966315393,0.29056882937775258,2.6976731595784718,6.9736519050660615,4.4395646883739071,563.07138461538466,89.615594175136266,776.6684828511809,53521.168723600684,5888.5640750391212,-47406.173200000005,0.88773577041157314,13867.905721827114,1713.0906918894045,-50517.492116205409,1.8478368824256608,11113.471098138622,854.33533113630199,-50733.613663321215,2.0985078591396249,null,142.83994158773805]
["ICH","ICH44-075-A5",1557.3551744449078,15.41888623483567,3817.8181664733047,53,"NA",0.7,13,58.31416196315233,18.3,675,32,3.8652703290570516,1.6509083987142033,3.2749741345470786,null,0.27322404371584696,0.30303790451791829,0.319551101389137,0.27222876745519353,731.99279999999999,0,-1219.9880000000001,0,0,0,0,0,0.38937558121706473,0.50327997557807957,4.6725069746047767,12.078719413873911,7.689551603752296,563.07138461538466,89.615594175136266,776.6684828511809,17127.031146273963,1873.6073440041844,-49772.852500000001,1.6509083987142033,4562.2943614487904,545.07431105571959,-50717.789795624376,3.2749741345470786,3689.4828900675002,271.83396899791427,-50783.430017578969,3.6733810660351729,null,82.468678726711005]
["ICH","ICH44-100-A1",2095.3102447660631,8.9901113712910679,5090.4242219644057,30.6,"NA",2.8,53,134.56206312578115,23.2,675,32,1.6750634968290325,0.64261041721352796,1.3700743252253786,null,0.21551724137931036,0.2726022745991778,0.29006462636825098,0.63208365201589845,885.93119999999999,0,-1476.5519999999999,0,0,0,0,0,0.20422706739282323,0.2639697979225471,2.4507248087138787,6.33527515014113,4.0331614239688411,681.48553846153845,108.4617920917958,940.00219812889691,94159.823736780963,9984.6472617043455,-45299.363200000007,0.64261041721352796,24671.468086482346,2933.4343426724986,-50329.92603748689,1.3700743252253786,19428.134920628898,1316.0030773804604,-50709.513620497877,1.5820690771082426,null,190.29949465338356]
["ICH","ICH44-100-A5",2095.3102447660631,15.57132966077884,5090.4242219644057,53,"NA",0.9,18,77.689443368381149,23.2,675,32,2.9012950824118739,1.1833320239806941,2.4133307777612605,null,0.21551724137931036,0.2726022745991778,0.29006462636825098,0.36178309195792346,885.93119999999999,0,-1476.5519999999999,0,0,0,0,0,0.35373165700516296,0.45720910166554102,4.2447798840619555,10.973018439972984,6.9856405014408738,681.48553846153845,108.4617920917958,940.00219812889691,32351.523280132573,3209.3052055498797,-49098.692500000005,1.1833320239806941,8307.1742512266719,942.88961014473159,-50657.861718251675,2.4133307777612605,6492.8204465952904,423.00098915800504,-50775.514502271668,2.7640871622499792,null,109.86946446478075]
["ICH","ICH44-150-A1",3175.3235352486199,18.181811544229408,7635.6363329466094,61.2,"NA",1,20,100.83010119097844,33,675,32,2.2354435564145523,0.89864644152589779,1.8450966046786548,null,0.15151515151515152,0.24239536862641561,0.26057815134736489,0.46698841774313765,1193.808,0,-1989.68,0,0,0,0,0,0.36726557596329218,0.47470211029600745,4.4071869115595064,11.392850647104179,7.2529139855773153,918.31384615384616,146.15418792511494,1266.6696286843294,53486.253573389353,5344.0714607696264,-47996.08,0.89864644152589779,13990.158632738754,1587.6617676243154,-50557.226296727596,1.8450966046786548,10775.132958685555,633.33481434216685,-50765.706429038364,2.1413807323804765,null,142.59529659973276]
["ICH","ICH44-150-A5",3175.3235352486199,31.491821368247681,7635.6363329466094,106,"NA",0.3,7,58.21428606502861,33,675,32,3.8719018171624677,1.5689789206496334,3.2039545297726595,null,0.15151515151515152,0.24239536862641561,0.26057815134736489,0.26855993340961559,1193.808,0,-1989.68,0,0,0,0,0,0.63612263743946906,0.82220817349285003,7.6334716492736288,19.7329961638284,12.562415525946793,918.31384615384616,146.15418792511494,1266.6696286843294,19308.382235307159,1603.1986089365571,-50046.73,1.5689789206496334,4794.0207295702421,476.29853028729462,-50738.217900116455,3.2039545297726595,3612.4987943556912,190.00044430265007,-50794.507535840363,3.7235636280664779,null,82.327432877030247]
["ICH","ICH44-200-A1",4257.7776655133157,18.294010622656721,10180.848443928811,61.2,"NA",1.2,27,134.37343686076341,42.7,675,32,1.6774148616408282,0.6516314132380665,1.3673840840178892,null,0.11709601873536299,0.22691546891003742,0.2453206148539995,0.62195472041211475,1498.5432000000001,0,-2497.5720000000001,0,0,0,0,0,0.3459328332237796,0.44712888084130736,4.151193998685355,10.731093140191376,6.8316260721639477,1152.7255384615385,183.46196747442056,1590.003718111645,97006.089960757206,8546.2722801756208,-46760.084800000004,0.6516314132380665,25110.72358497079,2554.6665993079982,-50443.715509365175,1.3673840840178892,19039.997718476039,954.0022308669902,-50754.755196026941,1.6078340869209704,null,190.0327368311757]
["ICH","ICH44-200-A5",4257.7776655133157,31.686155872646193,10180.848443928811,106,"NA",0.4,9,77.58053994349693,42.7,675,32,2.905367765733033,1.1934763381293558,2.4104182510459657,null,0.11709601873536299,0.22691546891003742,0.2453206148539995,0.35664557691659915,1498.5432000000001,0,-2497.5720000000001,0,0,0,0,0,0.59917324314983722,0.77444993914855464,7.1900789177980471,18.586798539565311,11.832723455300162,1152.7255384615385,183.46196747442056,1590.003718111645,32334.613847168195,2848.7168614481839,-49456.840000000004,1.1934763381293558,8370.2411949902635,851.55553310266612,-50684.67850312173,2.4104182510459657,6346.6659061586797,318.00074362233011,-50788.358398675649,2.8039041130008124,null,109.7154517643206]
["ICH","ICH44-250-A1",5341.3447862142475,18.365490374602974,12726.060554911015,61.2,"NA",1.5,33,167.91421232181924,52.5,675,32,1.3423521266204987,0.50794855740284417,1.0872011518585234,null,9.5238095238095233E-2,0.21804490109140398,0.23657753214431815,0.77766362036438264,1806.42,0,-3010.7,0,0,0,0,0,0.33370846101878643,0.43132850187158295,4.0045015322254374,10.351884044917991,6.5902140642512892,1389.5538461538461,221.15436330773969,1916.6711486670772,146132.64196712643,13349.369969792322,-44484.73,0.50794855740284417,38815.903226360802,4006.0085896607002,-50235.981038069367,1.0872011518585234,29562.74766533625,1437.5033615003133,-50731.870320116148,1.2859030226094919,null,237.46655638071138]
["ICH","ICH44-250-A5",5341.3447862142475,31.80996243472952,12726.060554911015,106,"NA",0.5,11,96.945315684766314,52.5,675,32,2.3250220849548344,0.95525027528149753,1.926938173048969,null,9.5238095238095233E-2,0.21804490109140398,0.23657753214431815,0.44525989489957823,1806.42,0,-3010.7,0,0,0,0,0,0.57800000940015617,0.74708287999414924,6.9360001128018745,17.929989119859581,11.414585592038218,1389.5538461538461,221.15436330773969,1916.6711486670772,48709.761072459543,4449.7266265282096,-48698.41,0.95525027528149753,12938.634408786933,1335.3361965535667,-50615.433679356458,1.926938173048969,9854.2492217787512,479.16778716677101,-50780.730106705385,2.2458793425029557,null,137.10138024993716]
["IL","IL06-015A1",21,2.5,60,7.2,"NA",4.2,0.5,4.8790367901871781,0.23,330,32,46.197643037521104,42.962222629680397,45.195564883626382,null,21.739130434782609,5.0444183577764381,4.564046666666667,2.8978858014993246E-2,164.30568000000002,0,-273.84280000000001,0,0,0,0,0,1.0509204912034245,1.3737832905982907,12.611045894441094,32.970798974358978,20.978681607752698,126.38898461538462,20.115431653903975,174.33374100050111,24.179736542103861,127.77518294254169,-50119.316800000001,42.962222629680397,23.850179463505963,44.366382966160316,-50722.472500000003,45.195564883626382,26.98639383855738,372.29928893387995,-44982.569765147127,34.507916063587267,null,6.9]
["IL","IL06-015A4",21,4.9000000000000004,60,14.4,"NA",1.1000000000000001,0.13,2.4041630560342613,0.23,330,32,{"$f":"IF(G79=\"NA\",(UAC_V*0.98)/J79,(IF((UAC_V*0.98)/J79<G79,(UAC_V*0.98)/J79,G79)))","v":93.754040282028143},{"$f":"IF(AO79<G79,IF(AO79<0,0,AO79),G79)","v":90.009182368973626},{"$f":"IF(AS79<G79,IF(AS79<0,0,AS79),G79)","v":92.67513158850943},null,{"$f":"IF(move1,Gewicht/K79,MAX(Gewicht,Gewicht2)/K79)","v":21.739130434782609},{"$f":"IF(move1,IF(AccType=1,SQRT((V79^2*Ltime1+W79^2*Ltime2+X79^2*Ltime3+Y79^2*Ltime4)/ltime)/C79,SQRT((((V79-W79)*2/PI()+W79)^2*Ltime1+W79^2*Ltime2+((X79-W79)*2/PI()+W79)^2*Ltime3+Y79^2*Ltime4)/ltime)/C79),IF(AccType=1,SQRT((V79^2*Ltime1+W79^2*Ltime2+X79^2*Ltime3+Y79^2*Ltime4+Z79^2*Ltime5+AA79^2*Ltime6+AB79^2*Ltime7+AC79^2*Ltime8)/ltime)/C79,SQRT((((V79-W79)*2/PI()+W79)^2*Ltime1+W79^2*Ltime2+((X79-W79)*2/PI()+W79)^2*Ltime3+Y79^2*Ltime4+((Z79-AA79)*2/PI()+AA79)^2*Ltime5+AA79^2*Ltime6+((AB79-AA79)*2/PI()+AA79)^2*Ltime7+AC79^2*Ltime8)/ltime)/C79))","v":5.0444183577764381},{"$f":" IF(move1,MAX(ABS(V79),ABS(X79))/E79,MAX(ABS(V79),ABS(X79),ABS(Z79),ABS(AB79))/E79)","v":4.564046666666667},{"$f":"IF(AW79>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW79,G79),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW79,G79)),\"NA\")","v":1.2654929010338834E-2},{"$f":"((Gewicht+K79)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":164.30568000000002},0,{"$f":"((Gewicht+K79)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-273.84280000000001},0,{"$f":"((Gewicht2+K79)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K79)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF79/Irms","v":2.0598041627587125},{"$f":"AG79/Ipeak","v":2.7704130341880346},{"$f":"D79*S79","v":24.717649953104548},{"$f":"IF(move1,IF(MAX(ABS(V79),ABS(X79))<=C79,MAX(ABS(V79),ABS(X79))/C79*D79,D79+(MAX(ABS(V79),ABS(X79))-C79)/(E79-C79)*(F79-D79)),IF(MAX(ABS(V79),ABS(X79),ABS(Z79),ABS(AB79))<=C79,MAX(ABS(V79),ABS(X79),ABS(Z79),ABS(AB79))/C79*D79,D79+(MAX(ABS(V79),ABS(X79),ABS(Z79),ABS(AB79))-C79)/(E79-C79)*(F79-D79)))","v":66.489912820512828},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V79),ABS(X79))<=C79,MAX(ABS(V79),ABS(X79))/C79*D79,D79+(MAX(ABS(V79),ABS(X79))-C79)/(E79-C79)*(F79-D79)),IF(MAX(ABS(V79),ABS(X79),ABS(Z79),ABS(AB79))<=C79,MAX(ABS(V79),ABS(X79),ABS(Z79),ABS(AB79))/C79*D79,D79+(MAX(ABS(V79),ABS(X79),ABS(Z79),ABS(AB79))-C79)/(E79-C79)*(F79-D79))),IF(move1,IF(MAX(ABS((V79-W79)*2/PI()+W79),ABS((X79-W79)*2/PI()+W79))<=C79,MAX(ABS((V79-W79)*2/PI()+W79),ABS((X79-W79)*2/PI()+W79))/C79*D79,D79+(MAX(ABS((V79-W79)*2/PI()+W79),ABS((X79-W79)*2/PI()+W79))-C79)/(E79-C79)*(F79-D79)),IF(MAX(ABS((V79-W79)*2/PI()+W79),ABS((X79-W79)*2/PI()+W79),ABS((Z79-AA79)*2/PI()+AA79),ABS((AB79-AA79)*2/PI()+AA79))<=C79,MAX(ABS((V79-W79)*2/PI()+W79),ABS((X79-W79)*2/PI()+W79),ABS((Z79-AA79)*2/PI()+AA79),ABS((AB79-AA79)*2/PI()+AA79))/C79*D79,D79+(MAX(ABS((V79-W79)*2/PI()+W79),ABS((X79-W79)*2/PI()+W79),ABS((Z79-AA79)*2/PI()+AA79),ABS((AB79-AA79)*2/PI()+AA79))-C79)/(E79-C79)*(F79-D79))))","v":42.250526653968215},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V79)+Ltime2*ABS(Lspeed2)*ABS(W79)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X79)+Ltime4*ABS(Lspeed1)*ABS(Y79))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V79)+Ltime2*ABS(Lspeed2)*ABS(W79)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X79)+Ltime4*ABS(Lspeed1)*ABS(Y79)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z79)+Ltime6*ABS(Lspeed6)*ABS(AA79)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB79)+Ltime8*ABS(Lspeed1)*ABS(AC79))/ltime)","v":126.38898461538462},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK79/2*Ltime1/ltime,AK79/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X79*-ABS(Lspeed2-Lspeed1),((X79-Y79)*2/PI()+Y79)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V79*-ABS(Lspeed2-Lspeed1),((V79-W79)*2/PI()+W79)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X79*-ABS(Lspeed2-Lspeed1),((X79-Y79)*2/PI()+Y79)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V79*-ABS(Lspeed2-Lspeed1),((V79-W79)*2/PI()+W79)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB79*-ABS(Lspeed6-Lspeed1),((AB79-AC79)*2/PI()+AB79)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z79*-ABS(Lspeed6-Lspeed1),((Z79-AA79)*2/PI()+AA79)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB79*-ABS(Lspeed6-Lspeed1),((AB79-AC79)*2/PI()+AB79)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z79*-ABS(Lspeed6-Lspeed1),((Z79-AA79)*2/PI()+AA79)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":20.115431653903975},{"$f":"IF(move1,MAX(IF(AccType=1,X79*-ABS(Lspeed2-Lspeed1),((X79-Y79)*2/PI()+Y79)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V79*-ABS(Lspeed2-Lspeed1),((V79-W79)*2/PI()+W79)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X79*-ABS(Lspeed2-Lspeed1),((X79-Y79)*2/PI()+Y79)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V79*-ABS(Lspeed2-Lspeed1),((V79-W79)*2/PI()+W79)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB79*-ABS(Lspeed6-Lspeed1),((AB79-AC79)*2/PI()+AB79)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z79*-ABS(Lspeed6-Lspeed1),((Z79-AA79)*2/PI()+AA79)*-ABS(Lspeed6-Lspeed1)),0))","v":174.33374100050111},{"$f":"(J79^2)+3*(I79/1000)^2*(F79/2)^2*(2000*PI()/M79)^2","v":5.881328760984883},{"$f":"SQRT(3)*H79*F79/2*J79","v":32.979929896832708},{"$f":"3*F79^2*H79^2/4-(UAC_V*0.98)^2","v":-50616.980800000005},{"$f":"-AM79/2/AL79+SQRT((AM79/2/AL79)^2-AN79/AL79)","v":90.009182368973626},{"$f":"(J79^2)+3*(I79/1000)^2*(D79/2)^2*(2000*PI()/M79)^2","v":5.7917327524655029},{"$f":"SQRT(3)*H79*D79/2*J79","v":11.222337256561131},{"$f":"3*D79^2*H79^2/4-(UAC_V*0.98)^2","v":-50783.370925000003},{"$f":"-AQ79/2/AP79+SQRT((AQ79/2/AP79)^2-AR79/AP79)","v":92.67513158850943},{"$f":"(J79^2)+3*(I79/1000)^2*(AH79/2)^2*(2000*PI()/M79)^2","v":6.6523123109210225},{"$f":"SQRT(3)*H79*AH79/2*J79","v":96.765236607787045},{"$f":"3*AH79^2*H79^2/4-(UAC_V*0.98)^2","v":-49185.17539519706},{"$f":"IF((AU79/2/AT79)^2-AV79/AT79>=0,-AU79/2/AT79+SQRT((AU79/2/AT79)^2-AV79/AT79),-9999)","v":79.020593413287358},null,3.4]
["IL","IL06-030A1",30.3,1.8,120,7.1,"NA",6.1,1.3,9.6873629022556997,0.27,330,32,23.267426055393845,20.839746638079887,22.742328672350059,null,18.518518518518519,3.5228705908103066,2.2994766666666662,5.144111106839655E-2,165.56232,0,-275.93719999999996,0,0,0,0,0,0.52843058862154602,0.6797366963953918,6.3411670634585517,16.313680713489404,10.389136125911516,127.35563076923074,20.269278167509356,175.66707745174776,96.30834049057097,363.34934760279248,-49398.342925000004,20.839746638079887,94.003326189038859,92.116736011975576,-50714.739700000006,22.742328672350059,99.119321774203343,531.67406105726093,-47792.987724427301,19.439704532633272,null,13.7]
["IL","IL06-030A4",30.3,3.6,120,14.2,"NA",1.5,0.33,4.8790367901871781,0.27,330,32,46.197643037521104,43.636699018546302,45.672211892250665,null,18.518518518518519,3.5228705908103066,2.2994766666666662,2.3770399723319083E-2,165.56232,0,-275.93719999999996,0,0,0,0,0,1.056861177243092,1.3594733927907836,12.682334126917103,32.627361426978808,20.778272251823033,127.35563076923074,20.269278167509356,175.66707745174776,24.439929655439482,90.000376874210914,-50464.892500000002,43.636699018546302,23.845808809435109,22.816996954025306,-50783.29,45.672211892250665,25.164464239552064,131.69382629993186,-50076.604491261642,42.069128480788081,null,6.9]
["IL","IL06-050A1",49.7,1.7,200,7,"NA",8.6,3,16.475588001646557,0.32,330,32,13.680847079780929,11.58413379940545,13.262561637324291,null,15.625,2.1681231516471056,1.392776,8.4260026692970252E-2,167.13312000000002,0,-278.55520000000001,0,0,0,0,0,0.30715077981667327,0.40708653803504102,3.6858093578000792,9.7700769128409846,6.2007243145959574,128.56393846153847,20.46158630951609,177.33374801580612,284.19645177992305,858.95032065306305,-48087.130000000005,11.58413379940545,272.19707542130567,208.60222073002959,-50644.851700000007,13.262561637324291,281.45072123034367,760.87344832906319,-48672.394967038781,11.868023774118139,null,23.3]
["IL","IL06-050A4",49.7,3.5,200,14,"NA",2.2000000000000002,0.75,8.2024386617639511,0.32,330,32,27.479632496456521,25.154953222879616,27.024729075409642,null,15.625,2.1681231516471056,1.392776,3.9249283398801307E-2,167.13312000000002,0,-278.55520000000001,0,0,0,0,0,0.6323692525637391,0.81199534264803719,7.5884310307648697,19.487888223552893,12.416529302501425,128.56393846153847,20.46158630951609,177.33374801580612,70.467862944980766,218.78842382539347,-50093.68,25.154953222879616,67.479241434061294,54.697105956348366,-50760.692500000005,27.024729075409642,69.787517691555365,194.0423482482928,-50245.522174290854,25.478172170413192,null,11.6]
["IL","IL06-075A1",67.599999999999994,1.6,300,7,"NA",11.7,5,24.678026663410506,0.38,330,32,9.1336314314869824,7.1786591675776048,8.7745835997084818,null,13.157894736842104,1.6119971999886353,0.93898933333333334,0.12386111744597364,169.01808,0,-281.6968,0,0,0,0,0,0.21493295999848472,0.27394627079747563,2.5791955199818166,6.5747104991394156,4.1962231692790493,130.0139076923077,20.692356079924163,179.33375269267609,644.42569938867507,1750.3502566736461,-45774.452500000007,7.1786591675776048,610.85555082520409,400.08005866826193,-50542.331200000001,8.7745835997084818,621.73352872232488,1049.2657573439262,-48997.361000756115,8.0735586810460109,null,34.9]
["IL","IL06-075A4",67.599999999999994,3.2,300,14,"NA",2.9,1.25,12.37436867076458,0.38,330,32,18.215070683365468,16.201820157040551,17.855180497397598,null,13.157894736842104,1.6119971999886353,0.93898933333333334,5.8360870466754984E-2,169.01808,0,-281.6968,0,0,0,0,0,0.42986591999696944,0.54789254159495127,5.1583910399636332,13.149420998278831,8.3924463385580985,130.0139076923077,20.692356079924163,179.33375269267609,161.98017484716877,435.09061556186191,-49568.890000000007,16.201820157040551,153.58763770630102,99.449283556997017,-50740.571200000006,17.855180497397598,156.30713218058122,260.81961739379551,-50360.902871396276,17.134768415931109,null,17.5]
["IL","IL06-100A1",82.8,1.5,400,7,"NA",14.7,7,32.880465325174455,0.45,330,32,6.8551341281482943,4.9617528288497139,6.5370536451657157,null,11.111111111111111,1.3331986612157507,0.71340500000000007,0.16366089388418129,171.21720000000002,0,-285.36200000000002,0,0,0,0,0,0.16664983265196884,0.20884444619588063,1.9997979918236259,5.0122667087011354,3.2142780679475651,131.70553846153848,20.961587478733588,181.66709148235776,1150.5495708018032,2930.1102489390219,-42863.852500000008,4.9617528288497139,1084.3128629449805,627.8807676297904,-50440.508125,6.5370536451657157,1095.7630765317917,1345.4555871190112,-49130.746091423505,6.1101951496591171,null,46.5]
["IL","IL06-100A4",82.8,2.9,400,14,"NA",3.7,1.75,16.475588001646557,0.45,330,32,13.680847079780929,11.781285503282293,13.372165108633569,null,11.111111111111111,1.3331986612157507,0.71340500000000007,7.7284657371437526E-2,171.21720000000002,0,-285.36200000000002,0,0,0,0,0,0.32218967646047308,0.41618303383774696,3.8662761175256768,9.9883928121059267,6.3597248280396315,131.70553846153848,20.961587478733588,181.66709148235776,288.80114270045084,739.09678753868218,-48792.73,11.781285503282293,272.1897202046469,153.09862027586988,-50718.810325000006,13.372165108633569,275.02657286397692,335.74658500243498,-50389.879669396025,12.939178797078744,null,23.3]
["IL","IL12-015A1",41,2.4,120,7.1,"NA",8.5,1,9.6873629022556997,0.35,330,32,23.267426055393845,19.959764201283591,22.282918814457229,null,14.285714285714286,2.6430089189767423,2.3343833333333333,5.5752882959229089E-2,168.07559999999998,0,-280.12599999999998,0,0,0,0,0,0.52860178379534839,0.69277014767932465,6.3432214055441811,16.626483544303792,10.570488945125735,129.28892307692306,20.576971194720127,178.33375035424109,95.302597923414766,506.30646797110433,-48073.568125000005,19.959764201283591,94.011549574268358,171.14584832826063,-50493.04,22.282918814457229,97.075808346588815,753.78970739918532,-44750.506870041565,17.936292204499612,null,13.7]
["IL","IL12-015A2",41,4.9000000000000004,120,14.3,"NA",2.1,0.25,4.8790367901871781,0.35,330,32,46.197643037521104,42.988161435769975,45.216946344578943,null,14.285714285714286,2.6430089189767423,2.3343833333333333,2.4336918782949499E-2,168.07559999999998,0,-280.12599999999998,0,0,0,0,0,1.0792286419155033,1.3897069620253164,12.950743702986038,33.352967088607592,21.240977890251472,129.28892307692306,20.576971194720127,178.33375035424109,24.174549939693378,126.88785528321849,-50128.809325000002,42.988161435769975,23.848390356751128,43.479055306837104,-50725.746925000007,45.216946344578943,24.620361262745195,188.47707193092813,-49312.884988714293,41.089835936856652,null,6.9]
["IL","IL12-015A4",41,9.8000000000000007,120,28.6,"NA",0.5,0.06,2.4041630560342613,0.35,330,32,93.754040282028143,90.426932723320064,92.779594835358594,null,14.285714285714286,2.6430089189767423,2.3343833333333333,1.1321414662920649E-2,168.07559999999998,0,-280.12599999999998,0,0,0,0,0,2.1584572838310065,2.7794139240506328,25.901487405972077,66.705934177215184,42.481955780502943,129.28892307692306,20.576971194720127,178.33375035424109,5.8651443061053525,29.773547823529526,-50651.792500000003,90.426932723320064,5.7899971381954582,10.202124778691935,-50787.152500000004,92.779594835358594,5.9678592349364923,44.225123848526948,-50466.775643699388,88.32818422199054,null,3.4]
["IL","IL12-030A1",62.1,1.8,240,7.1,"NA",12.2,2.6,19.445436482630054,0.42,330,32,11.591408616687115,9.0735850213545692,11.062546817409357,null,11.904761904761905,1.7678132706518332,1.1824633333333334,0.10198537322671131,170.27472,0,-283.7912,0,0,0,0,0,0.26517199059777502,0.35019284242083565,3.1820638871733,8.404628218100056,5.3323528525170918,130.98055384615387,20.846202593529551,180.66708914392277,387.97836196228388,1458.7017604491668,-45177.891700000007,9.0735850213545692,378.75830475615544,369.81171391669028,-50443.478800000004,11.062546817409357,383.68283307652433,1095.5369708877211,-47631.074037469509,9.805327650044692,null,27.5]
["IL","IL12-030A2",62.1,3.7,240,14.2,"NA",3.1,0.65,9.7580735803743561,0.42,330,32,23.098821518760552,20.653547638456725,22.553651998536715,null,11.904761904761905,1.7678132706518332,1.1824633333333334,4.6860338506200916E-2,170.27472,0,-283.7912,0,0,0,0,0,0.54507575845098188,0.69936003372681277,6.5409091014117831,16.784640809443506,10.69805753800556,130.98055384615387,20.846202593529551,180.66708914392277,97.683340490570998,372.00155774673851,-49351.839700000004,20.653547638456725,95.387244253699251,96.92998335654454,-50706.489325000002,22.553651998536715,96.618162389560638,280.26014570438781,-49980.272904114216,21.340008029768551,null,13.8]
["IL","IL12-030A4",62.1,7.4,240,28.5,"NA",0.8,0.16,4.8790367901871781,0.42,330,32,46.197643037521104,43.518847034861167,45.624895292522766,null,11.904761904761905,1.7678132706518332,1.1824633333333334,2.2577093672098564E-2,170.27472,{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},-283.7912,{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},0,{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0,0,1.0901515169019638,1.4039123852351507,13.081818202823566,33.693897245643619,21.462763243039745,130.98055384615387,20.846202593529551,180.66708914392277,24.406243963108864,96.338431583662398,-50415.280000000006,43.518847034861167,23.845534465275275,25.014189253301819,-50778.875200000002,45.624895292522766,24.145982647557346,72.550489413541356,-50584.047901107151,44.29268064896366,null,6.9]
["IL","IL12-050A1",88.4,1.6,400,7,"NA",17.2,6,32.880465325174455,0.52,330,32,6.8551341281482943,4.6148895111989274,6.456383899341037,null,9.615384615384615,1.2647815336888746,0.72256799999999999,0.16749757052687872,173.41631999999998,0,-289.02719999999999,0,0,0,0,0,0.16863753782518329,0.21153547282841248,2.0236504539021993,5.0768513478818997,3.2567468660751375,133.39716923076921,21.230818877543008,184.00043027203941,1132.130807119692,3428.4283184864744,-39933.040000000008,4.6148895111989274,1083.789793188294,783.64075851119424,-50237.147200000007,6.456383899341037,1092.1655714340686,1595.074740256297,-48451.811934786732,5.970235847925494,null,46.5]
["IL","IL12-050A2",88.4,3.1,400,14,"NA",4.3,1.5,16.475588001646557,0.52,330,32,13.680847079780929,11.58413379940545,13.302125101842531,null,9.615384615384615,1.2647815336888746,0.72256799999999999,7.791808889488247E-2,173.41631999999998,0,-289.02719999999999,0,0,0,0,0,0.32673522953629258,0.42158703465982028,3.9208227544355112,10.118088831835687,6.4441742296701845,133.39716923076921,21.230818877543008,184.00043027203941,284.19645177992305,858.95032065306305,-48087.130000000005,11.58413379940545,272.07021148778091,190.19614243032112,-50671.893325000005,13.302125101842531,274.14670613660013,395.37325149424362,-50229.279037016233,12.833990337584863,null,23.3]
["IL","IL12-050A4",88.4,6.2,400,28.1,"NA",1.1000000000000001,0.38,8.2024386617639511,0.52,330,32,27.479632496456521,25.13008441055127,27.08066457777721,null,9.615384615384615,1.2647815336888746,0.72256799999999999,3.7643209505664334E-2,173.41631999999998,0,-289.02719999999999,0,0,0,0,0,0.65347045907258516,0.84585682498930248,7.8416455088710224,20.300563799743259,12.919028956860281,133.39716923076921,21.230818877543008,184.00043027203941,70.576862817433252,219.56981105334131,-50088.588925000004,25.13008441055127,67.440498735707678,48.446008132765698,-50770.275700000006,27.08066457777721,67.976863920724782,100.94764224378849,-50653.69706191172,26.565216227100024,null,11.6]
["IL","IL12-075A1",119,1.4,600,7,"NA",23.3,10,49.356053326821012,0.65,330,32,4.5668157157434912,2.3623236767552775,4.2490235908911096,null,7.6923076923076916,0.9616791268058783,0.4930566666666667,0.24766119227890493,177.50040000000001,0,-295.834,0,0,0,0,0,0.11219589812735246,0.1441155925155925,1.3463507775282295,3.4587742203742202,2.2072123345865071,136.53876923076925,21.73082004676051,188.33377373859108,2577.7027975547003,6971.4805094864887,-30853.952500000003,2.3623236767552775,2441.6873119021875,1394.2961018972976,-50007.111700000001,4.2490235908911096,2450.1067002173236,2198.2196815525722,-48821.526955786452,4.0377743109378432,null,69.8]
["IL","IL12-075A2",119,2.8,600,14,"NA",5.8,2.5,24.678026663410506,0.65,330,32,9.1336314314869824,7.1962083475426359,8.8253920397527228,null,7.6923076923076916,0.9616791268058783,0.4930566666666667,0.11590855091363383,177.50040000000001,0,-295.834,0,0,0,0,0,0.22439179625470493,0.288231185031185,2.692701555056459,6.9175484407484404,4.4144246691730142,136.53876923076925,21.73082004676051,188.33377373859108,644.42569938867507,1735.3899980695976,-45860.08,7.1962083475426359,610.42182797554688,347.07799961391953,-50607.356800000001,8.8253920397527228,612.52667505433089,547.19631557961009,-50313.49932761817,8.6274911740128939,null,34.9]
["IL","IL12-075A4",119,5.6,600,28.1,"NA",1.5,0.63,12.37436867076458,0.65,330,32,18.215070683365468,16.128151147046516,17.893339352314687,null,7.6923076923076916,0.9616791268058783,0.4930566666666667,5.655238642243416E-2,177.50040000000001,0,-295.834,0,0,0,0,0,0.44878359250940986,0.57799419611919611,5.3854031101129181,13.871860706860707,8.8432638443207878,136.53876923076925,21.73082004676051,188.33377373859108,162.18680645595052,451.70121788011045,-49472.693125000005,16.128151147046516,153.48489697503652,90.018748047281775,-50752.240000000005,17.893339352314687,154.0224852250505,142.15348927099097,-50673.191905228297,17.682719744666745,null,17.5]
["IL","IL12-100A2",148,2.6,800,14,"NA",7.4,3.5,32.880465325174455,0.77,330,32,6.8551341281482943,4.9473067914094599,6.5806809447109682,null,6.4935064935064934,0.78966483955838329,0.37764649999999994,0.1540598917326774,181.27032,0,-302.11719999999997,0,0,0,0,0,0.17109404857098306,0.22061196830265847,2.0531285828517967,5.2946872392638031,3.3751612381174443,139.43870769230767,22.192359587576657,192.33378309233103,1150.5495708018032,2950.0429717209199,-42755.44,4.9473067914094599,1083.5194392786743,547.86512331959943,-50527.526800000007,6.5806809447109682,1085.1600245527145,711.20504920951748,-50337.302331348263,6.4909821028252193,null,46.5]
["IL","IL12-100A4",148,5.2,800,28.1,"NA",1.8,0.88,16.475588001646557,0.77,330,32,13.680847079780929,11.814916703481737,13.413527643897583,null,6.4935064935064934,0.78966483955838329,0.37764649999999994,7.5044146533160078E-2,181.27032,0,-302.11719999999997,0,0,0,0,0,0.34218809714196613,0.44220883691206542,4.1062571657035933,10.61301208588957,6.757122136218376,139.43870769230767,22.192359587576657,192.33378309233103,289.12568258878332,721.68948868159362,-48886.407700000003,11.814916703481737,272.0504706211936,133.55107975602442,-50739.452800000006,13.413527643897583,272.46737430428146,173.5424917952497,-50694.209360060035,13.325489677707584,null,23.3]
["IL","IL18-015A1",62,2.4,180,7.1,"NA",12.7,1.5,14.637110370561532,0.46,330,32,15.39921434584037,11.94767006572906,14.406263296347115,null,10.869565217391305,1.7837322176729984,1.5882533333333333,8.4032481994561981E-2,171.53136000000001,0,-285.88560000000001,0,0,0,0,0,0.35674644353459967,0.47156155367231634,4.2809573224151958,11.317477288135592,7.1796779686211547,131.94720000000001,21.000049107134934,182.00042559516942,217.52459532768322,1143.0047863024784,-44707.188325000003,11.94767006572906,214.61973654210382,386.36781508816171,-50108.387200000005,14.406263296347115,217.59861722766814,1155.8318707386529,-44569.554439005748,11.900160226907415,null,20.7]
["IL","IL18-015A2",62,4.9000000000000004,180,14.2,"NA",3.2,0.38,7.2831998462214393,0.46,330,32,30.947935627077246,27.691008484651096,29.946121076830369,null,10.869565217391305,1.7837322176729984,1.5882533333333333,3.6167521569086029E-2,171.53136000000001,0,-285.88560000000001,0,0,0,0,0,0.72835732221647442,0.93938420903954789,8.7402878665976935,22.545221016949149,14.357660661314199,131.94720000000001,21.000049107134934,182.00042559516942,53.886908560564379,286.60989582357411,-49256.5648,27.691008484651096,53.145249080237797,98.900597854613608,-50620.763200000001,29.946121076830369,53.905707537253498,289.79208636686553,-49221.986216969352,27.649116019460507,null,10.3]
["IL","IL18-015A3",62,7.3,180,21.3,"NA",1.4,0.17,4.8790367901871781,0.46,330,32,46.197643037521104,43.001710375412209,45.222454350544105,null,10.869565217391305,1.7837322176729984,1.5882533333333333,2.3277215064247674E-2,171.53136000000001,0,-285.88560000000001,0,0,0,0,0,1.085103765751074,1.4109457627118644,13.021245189012888,33.862698305084749,21.537338629935356,131.94720000000001,21.000049107134934,182.00042559516942,24.184121219880186,126.00052762389528,-50138.235700000005,43.001710375412209,23.849531221334864,43.183279420396033,-50726.823700000001,45.222454350544105,24.192617127836787,127.40450849701205,-50123.29027576706,42.96046572753184,null,6.9]
["IL","IL18-015A4",62,14.7,180,42.6,"NA",0.4,0.04,2.4041630560342613,0.46,330,32,93.754040282028143,89.904877294359849,92.597909924509693,null,10.869565217391305,1.7837322176729984,1.5882533333333333,1.1129160342310783E-2,171.53136000000001,0,-285.88560000000001,0,0,0,0,{"$f":"(Ltorque2+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},2.1850719666494229,2.8181526271186446,26.220863599793073,67.635663050847469,43.072981983942597,131.94720000000001,21.000049107134934,182.00042559516942,5.8639576403886906,35.478409434471544,-50587.388800000001,89.904877294359849,5.7899971381954582,12.242549734430321,-50779.229200000002,92.597909924509693,5.8658323305848361,35.872321370655683,-50582.526186761315,89.854038331913088,null,3.4]
["IL","IL18-030A1",92.1,1.8,360,7.1,"NA",18.2,3.8,29.132799384885757,0.56999999999999995,330,32,7.7369839067693116,5.0197638367051551,7.1985828232859861,null,8.7719298245614041,1.2249666592117847,0.81012555555555554,0.15292351433281562,174.98712,0,-291.64519999999999,0,0,0,0,0,0.18374499888176773,0.23948761353738959,2.2049399865812127,5.7477027248973505,3.651084861632393,134.60547692307691,21.423127019549739,185.66710083609775,869.76771401410952,3260.1875649931549,-38281.803700000004,5.0197638367051551,850.07279891699488,826.52642492784207,-50000.246800000001,7.1985828232859861,854.28585760530541,1676.5100654406594,-47493.483593736637,6.5392167081881638,null,41.2]
["IL","IL18-030A2",92.1,3.6,360,14.3,"NA",4.5999999999999996,0.95,14.566399692442879,0.56999999999999995,330,32,15.473967813538623,13.00187599382159,14.946654732556027,null,8.7719298245614041,1.2249666592117847,0.81012555555555554,6.9790898210461152E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,0.36748999776353547,0.48207876695284319,4.4098799731624254,11.569890406868236,7.3370958527295489,134.60547692307691,21.423127019549739,185.66710083609775,217.51630112917235,829.80629169342888,-47559.903700000003,13.00187599382159,212.51819972924872,208.90228322352056,-50599.484800000006,14.946654732556027,213.5848069256472,425.76002107361836,-49950.83067798752,14.328515976172193,null,20.6]
["IL","IL18-030A3",92.1,5.5,360,21.4,"NA",2,0.42,9.6873629022556997,0.56999999999999995,330,32,23.267426055393845,20.880340564111869,22.741857174466492,null,8.7719298245614041,1.2249666592117847,0.81012555555555554,4.5154920980492286E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,0.56144305213873469,0.72262950727883535,6.7373166256648158,17.343108174692048,11.053254584897179,134.60547692307691,21.423127019549739,185.66710083609775,96.180861942853397,359.07070139458602,-49431.280000000006,20.880340564111869,93.999292566537036,92.284526059356224,-50714.41,22.741857174466492,94.468160576442429,185.46261105102585,-50438.636689244355,22.145980510784582,null,13.7]
["IL","IL18-030A4",92.1,11,360,42.8,"NA",0.5,0.11,4.8790367901871781,0.56999999999999995,330,32,46.197643037521104,43.621849047993969,45.661628333015273,null,8.7719298245614041,1.2249666592117847,0.81012555555555554,2.2208685707036775E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,1.1228861042774694,1.4452590145576707,13.474633251329632,34.686216349384097,22.106509169794357,134.60547692307691,21.423127019549739,185.66710083609775,24.445905431032347,90.422913854841013,-50461.69,43.621849047993969,23.847334241612213,23.239533934655402,-50782.472500000003,45.661628333015273,23.975980566325482,46.704088184382428,-50713.529172311093,45.027428150921693,null,6.9]
["IL","IL18-050A1",131,1.5,600,7,"NA",25.7,9,49.356053326821012,0.72,330,32,4.5668157157434912,2.052691441435746,4.1866927994903387,null,6.9444444444444446,0.88440957648344953,0.49916533333333329,0.25118768353017301,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.11055119706043119,0.14483347547974412,1.3266143647251742,3.4760034115138589,2.1997209358326222,138.23039999999997,22.000051445569927,190.6671125282727,2550.7830660193072,7689.5729224808038,-26532.152500000004,2.052691441435746,2441.2897326233351,1647.7656262458868,-49690.583125000005,4.1866927994903387,2447.3529047536563,2416.4163635989526,-48408.18951442567,3.9810869145575705,null,69.8]
["IL","IL18-050A2",131,3.1,600,14,"NA",6.4,2.25,24.678026663410506,0.72,330,32,9.1336314314869824,7.0122166178778258,8.7558640928767861,null,6.9444444444444446,0.88440957648344953,0.49916533333333329,0.11670736488697021,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.22847247392489115,0.29233664534470499,2.7416696870986939,7.0160794882729203,4.4867196728319243,138.23039999999997,22.000051445569927,190.6671125282727,637.69576650482679,1914.9131013181773,-44784.04,7.0122166178778258,610.411725847507,424.01647243473923,-50509.940800000004,8.7558640928767861,611.95175447416693,613.69130596056129,-50186.74632685844,8.5684395407992362,null,34.9]
["IL","IL18-050A3",131,4.5999999999999996,600,21,"NA",2.9,1,16.475588001646557,0.72,330,32,13.680847079780929,11.560058192976351,13.302161223333055,null,6.9444444444444446,0.88440957648344953,0.49916533333333329,7.6261998064171568E-2,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.33902367098532227,0.43717012082444912,4.0682840518238672,10.492082899786778,6.6864406086645456,138.23039999999997,22.000051445569927,190.6671125282727,284.19645177992305,868.93811507926137,-48023.552500000005,11.560058192976351,272.05683836658312,190.3388252078382,-50671.693300000006,13.302161223333055,272.7377395216634,276.67157614678092,-50523.161211856757,13.112690794680439,null,23.3]
["IL","IL18-050A4",131,9.1999999999999993,600,42.1,"NA",0.7,0.25,8.2024386617639511,0.72,330,32,27.479632496456521,25.231576017677295,27.102939943841882,null,6.9444444444444446,0.88440957648344953,0.49916533333333329,3.7163502754163441E-2,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.67804734197064453,0.87583721393034819,8.1365681036477344,21.020093134328356,13.385603416162414,138.23039999999997,22.000051445569927,190.6671125282727,70.483061316504177,209.34074188747874,-50153.799325,25.231576017677295,67.432959591645783,45.746670436218622,-50774.054800000005,27.102939943841882,67.603800092354632,66.559433485772189,-50739.313415785575,26.908120222547364,null,11.6]
["IL","IL18-075A1",173,1.4,900,7,"NA",35,15,74.246212024587479,0.91,330,32,3.0358451138942444,0.32759035787964952,2.7066181564639238,null,5.4945054945054945,0.69194261915321109,0.34383066666666667,0.37641160886289504,185.66856000000001,0,-309.44760000000002,0,0,0,0,0,8.0726638901207959E-2,0.10212669417698304,0.96871966681449551,2.4510406602475929,1.5848728744999843,142.82196923076924,22.730822385195506,197.00046067169438,5831.2862944980752,15753.280908274312,-5786.4100000000035,0.32759035787964952,5525.2514517799209,3150.6561816548619,-49004.41,2.7066181564639238,5528.8415191193581,3566.7067994146332,-48497.423511475637,2.656666203842406,null,105]
["IL","IL18-075A2",173,2.7,900,14,"NA",8.8000000000000007,3.75,37.052395334175088,0.91,330,32,6.0832774228796875,4.0235220050079068,5.7806134125751578,null,5.4945054945054945,0.69194261915321109,0.34383066666666667,0.17436891533490831,185.66856000000001,0,-309.44760000000002,0,0,0,0,0,0.1556870893094725,0.20086874598807891,1.86824507171367,4.8208499037138939,3.0730470503303255,142.82196923076924,22.730822385195506,197.00046067169438,1452.5765736245191,3953.2804856726266,-39421.480000000003,4.0235220050079068,1375.8442246006261,762.41837937972093,-50381.756800000003,5.7806134125751578,1376.7199184237229,867.75835254462163,-50256.674656480573,5.7349671418171742,null,52.4]
["IL","IL18-075A3",173,4,900,21,"NA",3.9,1.67,24.678026663410506,0.91,330,32,9.1336314314869824,7.1779949963556433,8.8385160779923684,null,5.4945054945054945,0.69194261915321109,0.34383066666666667,0.11371652002676792,185.66856000000001,0,-309.44760000000002,0,0,0,0,0,0.23064753971773702,0.29961079779917471,2.7677704766128444,7.1906591471801935,4.5612212261606668,142.82196923076924,22.730822385195506,197.00046067169438,644.56752386902735,1750.3502566736461,-45774.452500000007,7.1779949963556433,610.29525029910292,333.40004889021833,-50622.640000000007,8.8385160779923684,610.68270755080994,380.17784495026694,-50567.829939013594,8.7937970645303629,null,34.9]
["IL","IL18-075A4",173,8.1,900,42.1,"NA",1,0.42,12.37436867076458,0.91,330,32,18.215070683365468,16.131211444378799,17.905761567904364,null,5.4945054945054945,0.69194261915321109,0.34383066666666667,5.5994359523269456E-2,185.66856000000001,0,-309.44760000000002,0,0,0,0,0,0.46706126792841746,0.60338826226501607,5.6047352151410097,14.481318294360385,9.2224424523213333,142.82196923076924,22.730822385195506,197.00046067169438,162.16532025970136,451.1653919988766,-49475.852500000001,16.131211444378799,153.45964910051228,86.80379275987886,-50755.952500000007,17.905761567904364,153.55882195996392,98.832467082865435,-50741.369916410222,17.858941659729712,null,17.5]
["IL","IL18-100A1",211,1.2,1200,7,"NA",44.2,21,98.994949366116643,1.1000000000000001,330,32,2.2768838354206835,{"$error":"#NUM!"},2.0074569575466001,null,4.545454545454545,0.5855663114108014,0.26616333333333331,0.4954027476333539,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,5.8556631141080139E-2,7.648705763397369E-2,0.70267957369296163,1.8356893832153687,1.1564008084271999,147.41353846153845,23.461593324821077,203.33380881511599,10424.821137216228,26525.524424599029,20991.110000000015,{"$error":"#NUM!"},9818.3620905630869,4547.2327585026915,-48695.228800000004,2.0074569575466001,9817.0520424903971,4382.0196983659653,-48845.762383993133,2.0185596563144155,null,140]
["IL","IL18-100A2",211,2.5,1200,14,"NA",11.1,5.25,49.42676400493967,1.1000000000000001,330,32,4.5602823599269762,2.4907535149133371,4.2935506333980875,null,4.545454545454545,0.5855663114108014,0.26616333333333331,0.23233909094600508,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,0.12199298154391695,0.15668410852713177,1.4639157785270034,3.7604186046511625,2.4091683508899999,147.41353846153845,23.461593324821077,203.33380881511599,2599.210284304057,6651.8710878481397,-32693.290000000005,2.4907535149133371,2447.9860358515321,1187.8341228300249,-50227.613125000003,4.2935506333980875,2447.6306625679249,1144.6769499317122,-50268.818355302195,4.3040540269325449,null,69.900000000000006]
["IL","IL18-100A3",211,3.7,1200,21,"NA",4.9000000000000004,2.33,32.951176003293114,1.1000000000000001,330,32,6.8404235398904643,4.9519530765976354,6.5834335846456051,null,4.545454545454545,0.5855663114108014,0.26616333333333331,0.15166656647963486,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,0.18054961268499711,0.23317116616110548,2.1665953522199652,5.5961079878665316,3.5655691593172003,147.41353846153845,23.461593324821077,203.33380881511599,1155.0063565680243,2936.4115613023323,-42863.852500000001,4.9519530765976354,1087.9289995950483,517.36775127707756,-50558.637325000003,6.5834335846456051,1087.7756786663647,498.57040485914587,-50576.225548636547,6.5934109488413561,null,46.6]
["IL","IL18-100A4",211,7.4,1200,42.1,"NA",1.2,0.57999999999999996,16.475588001646557,1.1000000000000001,330,32,13.680847079780929,11.825010118347414,13.428544854597845,null,4.545454545454545,0.5855663114108014,0.26616333333333331,7.441385712137609E-2,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,0.36109922536999423,0.46679900572969329,4.3331907044399305,11.203176137512639,7.1311383186344006,147.41353846153845,23.461593324821077,203.33380881511599,288.68515722995204,720.83339201649085,-48890.957200000004,11.825010118347414,271.97764820775791,126.70230643520266,-50746.019200000002,13.428544854597845,271.93964628441495,122.09887465938266,-50750.238615582944,13.438357299083487,null,23.3]
["IL","IL24-015A1",83,2.4,240,7.1,"NA",16.899999999999999,2,19.445436482630054,0.56999999999999995,330,32,11.591408616687115,7.9100216132839662,10.573587300717087,null,8.7719298245614041,1.3592702326916308,1.2151883333333333,0.11191151564677272,174.98712,0,-291.64519999999999,0,0,0,0,0,0.27185404653832618,0.36025277070063688,3.2622485584599139,8.6460664968152852,5.4734737192971927,134.60547692307691,21.423127019549739,185.66710083609775,383.95539169365907,2020.660635376305,-40006.959925000003,7.9100216132839662,378.79119829707344,683.040214775089,-49571.324800000002,10.573587300717087,381.59003087834537,1557.7511103310667,-44387.735810280545,8.9356309243126386,null,27.5]
["IL","IL24-015A2",83,4.9000000000000004,240,14.2,"NA",4.2,0.5,9.7580735803743561,0.56999999999999995,330,32,23.098821518760552,19.85918078924956,22.112021034908462,null,8.7719298245614041,1.3592702326916308,1.2151883333333333,4.832675832044387E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,0.55503534501574936,0.71913491507431004,6.6604241401889919,17.259237961783441,10.981554380736998,134.60547692307691,21.423127019549739,185.66710083609775,96.677597923414794,504.00211049558112,-48137.462800000001,19.85918078924956,95.393561427004514,173.91622122734842,-50487.507700000002,22.112021034908462,96.091743434577609,389.76947777559451,-49209.694280555981,20.692470067394648,null,13.8]
["IL","IL24-015A3",83,9.8000000000000007,240,28.4,"NA",1.1000000000000001,0.13,4.8790367901871781,0.56999999999999995,330,32,46.197643037521104,42.842930944866673,45.167613587595682,null,8.7719298245614041,1.3592702326916308,1.2151883333333333,2.2884227898072925E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,1.1100706900314987,1.4382698301486201,13.320848280377984,34.518475923566882,21.963108761473997,134.60547692307691,21.423127019549739,185.66710083609775,24.199134478491359,132.00055274884269,-50073.2068,42.842930944866673,23.851931009862017,45.549486511924599,-50718.003700000001,45.167613587595682,24.040719424709788,102.08248227456046,-50367.401832079988,43.698218897925315,null,6.9]
["IL","IL24-030A1",109,1.6,480,7.1,"NA",24.3,5.0999999999999996,38.890872965260108,0.72,330,32,5.7957043083435575,2.803757174456575,5.3109831683590647,null,6.9444444444444446,1.0629142616452467,0.6239566666666666,0.20511479339898256,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.14172190155269956,0.18433800539083559,1.7006628186323949,4.4241121293800543,2.8106984337075467,138.23039999999997,22.000051445569927,190.6671125282727,1550.4121219880183,5810.8938981827469,-28480.209325000003,2.803757174456575,1514.4253130785421,1309.4972164918868,-49671.419200000004,5.3109831683590647,1518.4414151455564,2300.3761095863365,-47306.495374839295,4.8753187589684615,null,55]
["IL","IL24-030A2",109,3.2,480,14.2,"NA",6.1,1.28,19.445436482630054,0.72,330,32,11.591408616687115,9.0765006868115101,11.125393382704122,null,6.9444444444444446,1.0629142616452467,0.6239566666666666,9.3176597878629835E-2,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.28344380310539913,0.36867601078167117,3.4013256372647898,8.8482242587601085,5.6213968674150934,138.23039999999997,22.000051445569927,190.6671125282727,387.67751375089102,1458.7017604491668,-45177.891700000007,9.0765006868115101,378.61011079552225,328.72152348150246,-50519.387200000005,11.125393382704122,379.62202646281889,577.4606694846359,-49923.280132755986,10.732308570684047,null,27.5]
["IL","IL24-030A3",109,6.4,480,28.5,"NA",1.5,0.32,9.7580735803743561,0.72,330,32,23.098821518760552,20.728347633991376,22.646884064934699,null,6.9444444444444446,1.0629142616452467,0.6239566666666666,4.4903445510757603E-2,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.56688760621079826,0.73949150044923628,6.8026512745295795,17.74779601078167,11.264806433624869,138.23039999999997,22.000051445569927,190.6671125282727,97.624975852435455,361.26911843873398,-49434.488125000003,20.728347633991376,95.341277698880589,81.127100280978865,-50736.04,22.646884064934699,95.595723593305948,142.79391893539074,-50591.023229521881,22.270005978949392,null,13.8]
["IL","IL24-050A1",155,1.4,800,7,"NA",34.299999999999997,12,65.831641328467569,0.92,330,32,3.4238854667980201,0.47740102237739634,3.0614290255900936,null,5.4347826086956523,0.77360400942301466,0.38746400000000003,0.33888930091930397,185.98272,0,-309.97120000000001,0,0,0,0,0,9.0253801099351702E-2,0.11439526614987079,1.0830456131922204,2.7454863875968991,1.7675492260360213,143.06363076923077,22.769284013596849,197.33379478450604,4537.8282284787683,13688.550890563158,-7569.1525000000111,0.47740102237739634,4341.9659291391499,2737.7101781126312,-49075.719700000001,3.0614290255900936,4346.8134805198843,3456.4553617385141,-48048.440750358888,2.9508160844479394,null,93.1]
["IL","IL24-050A2",155,2.7,800,14,"NA",8.6,3,32.880465325174455,0.92,330,32,6.8551341281482943,4.6148895111989274,6.523386456843383,null,5.4347826086956523,0.77360400942301466,0.38746400000000003,0.15568101019026473,185.98272,0,-309.97120000000001,0,0,0,0,0,0.1740609021201783,0.22562497157622741,2.0887308254421395,5.4149993178294578,3.4416618311084006,143.06363076923077,22.769284013596849,197.33379478450604,1132.130807119692,3428.4283184864744,-39933.040000000008,4.6148895111989274,1083.0221037444005,661.19688999382015,-50400.7837,6.523386456843383,1084.2074777024889,842.82077745900392,-50148.115844220978,6.4233910017532336,null,46.5]
["IL","IL24-050A3",155,5.4,800,28.1,"NA",2.1,0.75,16.475588001646557,0.92,330,32,13.680847079780929,11.623227696140953,13.361652166224014,null,5.4347826086956523,0.77360400942301466,0.38746400000000003,7.5378486302719233E-2,185.98272,0,-309.97120000000001,0,0,0,0,0,0.3481218042403566,0.45225104909560726,4.177461650884279,10.854025178294574,6.889887041253159,143.06363076923077,22.769284013596849,197.33379478450604,284.28769622441973,841.97107012852575,-48193.524925000005,11.623227696140953,271.91927593610018,161.80226970441421,-50708.713300000003,13.361652166224014,272.217089726604,206.44432616329482,-50648.151177568143,13.266384734551583,null,23.3]
["IL","IL24-075A1",211,1.2,1200,7,"NA",46.6,20,98.994949366116643,1.17,330,32,2.2768838354206835,{"$error":"#NUM!"},1.9910165075834276,null,4.2735042735042734,0.59228592482043363,0.26921766666666663,0.50018396723444036,193.83672000000001,0,-323.06119999999999,0,0,0,0,0,5.9228592482043367E-2,7.7382665992585101E-2,0.71074310978452038,1.8571839838220423,1.1696709816386597,149.10516923076921,23.730824723630498,205.66714760479766,10366.731190218801,27965.824393355542,28999.67,{"$error":"#NUM!"},9816.6549574268356,4794.1413245752356,-48459.875200000002,1.9910165075834276,9815.8237155023835,4672.9733243586497,-48576.927378554334,1.9992644017142029,null,140]
["IL","IL24-075A2",211,2.5,1200,14,"NA",11.7,5,49.42676400493967,1.17,330,32,4.5602823599269762,2.3464244370288583,4.2786507244370089,null,4.2735042735042734,0.59228592482043363,0.26921766666666663,0.23329684676230417,193.83672000000001,0,-323.06119999999999,0,0,0,0,0,0.123392901004257,0.15845988372093023,1.480714812051084,3.8030372093023255,2.4368145450805407,149.10516923076921,23.730824723630498,205.66714760479766,2584.6877975547004,7011.4316871912815,-30682.330000000005,2.3464244370288583,2447.5229463505962,1252.0413727127288,-50163.488125000003,4.2786507244370089,2447.2974575473049,1220.3970512275935,-50195.513698561816,4.286384552033212,null,69.900000000000006]
["IL","IL24-075A3",211,4.9000000000000004,1200,28,"NA",2.9,1.25,24.678026663410506,1.17,330,32,9.1336314314869824,7.1962083475426359,8.8664031475805345,null,4.2735042735042734,0.59228592482043363,0.26921766666666663,0.11269399948661016,193.83672000000001,0,-323.06119999999999,0,0,0,0,0,0.24185008596834376,0.31322521570610046,2.902201031620125,7.5174051769464114,4.7761565083578601,149.10516923076921,23.730824723630498,205.66714760479766,644.42569938867507,1735.3899980695976,-45860.08,7.1962083475426359,610.0897589187781,303.6932496621796,-50653.716925000001,8.8664031475805345,610.03561905710785,296.01765120783011,-50661.275385215886,8.8735869217137502,null,34.9]
["IL","IL24-075A4",211,9.9,1200,56.1,"NA",0.73,0.31,12.37436867076458,1.17,330,32,18.215070683365468,16.192314620777754,17.941184804564024,null,4.2735042735042734,0.59228592482043363,0.26921766666666663,5.5714613265677948E-2,193.83672000000001,0,-323.06119999999999,0,0,0,0,0,0.48863588797685775,0.63061709807886757,5.863630655722293,15.134810353892821,9.6497855985189425,149.10516923076921,23.730824723630498,205.66714760479766,161.87020820648439,438.87354628337272,-49547.298843250006,16.192314620777754,153.39734212407734,77.448272873536354,-50765.987853250001,17.941184804564024,153.38374964314053,75.490831131840039,-50767.942918628731,17.948612426536094,null,17.5]
["IL","IL24-100A1",262,1.2,1600,7,"NA",58.9,28,131.52186130069782,1.42,330,32,1.7137835320370736,{"$error":"#NUM!"},1.4318509636244854,null,3.5211267605633805,0.49632075883074706,0.21009450000000002,0.67070676732954149,201.69072,0,-336.15120000000002,0,0,0,0,0,4.9632075883074701E-2,6.3393029397110112E-2,0.59558491059689644,1.5214327055306427,0.9801549637790351,155.1467076923077,24.692365433664154,214.00050042508934,18408.793132828851,46961.49487415194,76688.307499999995,{"$error":"#NUM!"},17330.643716556599,8050.5419784260466,-47058.413200000003,1.4318509636244854,17319.77843125588,6575.6489010548194,-48305.497699737345,1.4909645298221141,null,186]
["IL","IL24-100A2",262,2.2999999999999998,1600,14,"NA",14.7,7,65.831641328467569,1.42,330,32,3.4238854667980201,1.1251728689280462,3.1771951351991068,null,3.5211267605633805,0.49632075883074706,0.21009450000000002,0.30998209170844487,201.69072,0,-336.15120000000002,0,0,0,0,0,9.5128145442559833E-2,0.12285030642750373,1.1415377453107181,2.9484073542600897,1.8786303472431507,155.1467076923077,24.692365433664154,214.00050042508934,4611.5032832072129,11733.043620482707,-19039.930000000008,1.1251728689280462,4341.3000199906428,1927.5714519364446,-49947.822925,3.1771951351991068,4338.8053429402607,1574.43227221189,-50233.182954474811,3.2259928129672559,null,93.1]
["IL","IL24-100A3",262,4.5999999999999996,1600,28.1,"NA",3.7,1.75,32.951176003293114,1.42,330,32,6.8404235398904643,4.9287181314606574,6.6002784998063522,null,3.5211267605633805,0.49632075883074706,0.21009450000000002,0.15045074838831651,201.69072,0,-336.15120000000002,0,0,0,0,0,0.19025629088511967,0.24593152715495767,2.2830754906214361,5.9023566517189838,3.7572606944863014,155.1467076923077,24.692365433664154,214.00050042508934,1155.7013461107294,2966.9456756909958,-42697.839325000001,4.9287181314606574,1087.6537549976608,485.69217466827683,-50587.899700000002,6.6002784998063522,1087.0300857350653,396.7113298914548,-50660.213621116396,6.646693424342291,null,46.6]
["IL","IL24-100A4",262,9.1999999999999993,1600,56.1,"NA",0.92,0.44,16.475588001646557,1.42,330,32,13.680847079780929,11.782592292000416,13.441433705523007,null,3.5211267605633805,0.49632075883074706,0.21009450000000002,7.4141171329498171E-2,201.69072,0,-336.15120000000002,0,0,0,0,0,0.38051258177023933,0.49163214000996519,4.5661509812428722,11.799171360239164,7.5145213889726028,155.1467076923077,24.692365433664154,214.00050042508934,289.06281798933799,736.4143513213603,-48807.311092000004,11.782592292000416,271.91880763108202,120.76670289049045,-50751.430528000004,13.441433705523007,271.76110331207661,98.641736081118481,-50769.314093473462,13.487782591885423,null,23.3]
["IC/ICD","ICD05-030A1",57,2.1,165,7.9,"NA",3.2,9.1,15.414927829866736,0.62,330,32,14.62218976875668,10.975084468961112,14.12337365723422,null,8.064516129032258,1.9970556324335824,1.7834133333333333,9.7164743508294585E-2,176.55792,0,-294.26319999999998,0,0,0,0,0,0.34948473567587696,0.61841302469135806,4.1938168281105233,14.841912592592593,9.0994062418602333,135.81378461538463,21.615435161556469,187.33377140015605,387.05695538207198,337.48089880169516,-50325.851200000005,10.975084468961112,248.1794772189543,89.710112339691122,-50771.291200000007,14.12337365723422,435.87764224701073,388.71845532465147,-50169.26219043017,10.291798896321213,null,21.8]
["IC/ICD","ICD05-030A5",57,3.7,165,13.7,"NA",1.1000000000000001,3,8.9095454429504972,0.62,330,32,25.298709282452037,19.423736008402607,24.557811810006356,null,8.064516129032258,1.9970556324335824,1.7834133333333333,5.4711737649293719E-2,176.55792,0,-294.26319999999998,0,0,0,0,0,0.61575882000035465,1.0695339506172838,7.3891058400042553,25.668814814814812,15.767941796310748,135.81378461538463,21.615435161556469,187.33377140015605,128.22326499130119,116.27850283478882,-50634.831325000006,19.423736008402607,82.942599487084593,31.403683247351729,-50792.736325000005,24.557811810006356,144.08138380393891,133.83012152270837,-50579.530100443655,18.277613597471056,null,12.6]
["IC/ICD","ICD05-050A1",87,2,295,8.5,"NA",4.5,14.4,25.667976157071671,0.95,330,32,8.7813701641569057,6.3686496367034637,8.4753674193487072,null,5.2631578947368425,1.3852444425488804,1.0560745762711865,0.13463344116547232,186.92520000000002,0,-311.54200000000003,0,0,0,0,0,0.23087407375814673,0.37570572916666672,2.7704888850977607,9.0169375000000009,5.4791811600919083,143.78861538461538,22.884668898800893,198.33379712294106,1092.0404426720638,850.26381765271799,-49707.863125000003,6.3686496367034637,682.8281386946469,200.06207474181602,-50744.41,8.4753674193487072,838.84700700212761,548.08817538712879,-50349.209589813705,7.4275751354445578,null,36.299999999999997]
["IC/ICD","ICD05-050A5",87,3.4,295,14.7,"NA",1.5,4.8,14.849242404917497,0.95,330,32,15.179225569471221,11.381700512244302,14.775023031620035,null,5.2631578947368425,1.3852444425488804,1.0560745762711865,7.6165358654509671E-2,186.92520000000002,0,-311.54200000000003,0,0,0,0,0,0.39248592538884947,0.64994483173076933,4.7098311046661934,15.598675961538463,9.4484226321597777,143.78861538461538,22.884668898800893,198.33379712294106,364.45879001461935,283.55905634893764,-50440.508125,11.381700512244302,228.20125231417001,65.585087863019595,-50785.652500000004,14.775023031620035,279.9733142103355,182.25753779327704,-50654.512335226907,13.129328314937188,null,21]
["IC/ICD","ICD05-075A1",125,1.9,441,8.5,"NA",6.1,21,38.395898218429529,1.36,330,32,{"$f":"IF(G143=\"NA\",(UAC_V*0.98)/J143,(IF((UAC_V*0.98)/J143<G143,(UAC_V*0.98)/J143,G143)))","v":5.8704187285247817},{"$f":"IF(AO143<G143,IF(AO143<0,0,AO143),G143)","v":4.1673985229559918},{"$f":"IF(AS143<G143,IF(AS143<0,0,AS143),G143)","v":5.6497666825435253},null,{"$f":"IF(move1,Gewicht/K143,MAX(Gewicht,Gewicht2)/K143)","v":3.6764705882352939},{"$f":"IF(move1,IF(AccType=1,SQRT((V143^2*Ltime1+W143^2*Ltime2+X143^2*Ltime3+Y143^2*Ltime4)/ltime)/C143,SQRT((((V143-W143)*2/PI()+W143)^2*Ltime1+W143^2*Ltime2+((X143-W143)*2/PI()+W143)^2*Ltime3+Y143^2*Ltime4)/ltime)/C143),IF(AccType=1,SQRT((V143^2*Ltime1+W143^2*Ltime2+X143^2*Ltime3+Y143^2*Ltime4+Z143^2*Ltime5+AA143^2*Ltime6+AB143^2*Ltime7+AC143^2*Ltime8)/ltime)/C143,SQRT((((V143-W143)*2/PI()+W143)^2*Ltime1+W143^2*Ltime2+((X143-W143)*2/PI()+W143)^2*Ltime3+Y143^2*Ltime4+((Z143-AA143)*2/PI()+AA143)^2*Ltime5+AA143^2*Ltime6+((AB143-AA143)*2/PI()+AA143)^2*Ltime7+AC143^2*Ltime8)/ltime)/C143))","v":1.030565989850281},{"$f":" IF(move1,MAX(ABS(V143),ABS(X143))/E143,MAX(ABS(V143),ABS(X143),ABS(Z143),ABS(AB143))/E143)","v":0.75512380952380964},{"$f":"IF(AW143>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW143,G143),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW143,G143)),\"NA\")","v":0.18855645710583158},{"$f":"((Gewicht+K143)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":199.80576000000002},0,{"$f":"((Gewicht+K143)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-333.00960000000003},0,{"$f":"((Gewicht2+K143)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K143)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF143/Irms","v":0.16317294839296115},{"$f":"AG143/Ipeak","v":0.26018767932489451},{"$f":"D143*S143","v":1.9580753807155338},{"$f":"IF(move1,IF(MAX(ABS(V143),ABS(X143))<=C143,MAX(ABS(V143),ABS(X143))/C143*D143,D143+(MAX(ABS(V143),ABS(X143))-C143)/(E143-C143)*(F143-D143)),IF(MAX(ABS(V143),ABS(X143),ABS(Z143),ABS(AB143))<=C143,MAX(ABS(V143),ABS(X143),ABS(Z143),ABS(AB143))/C143*D143,D143+(MAX(ABS(V143),ABS(X143),ABS(Z143),ABS(AB143))-C143)/(E143-C143)*(F143-D143)))","v":6.2445043037974681},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V143),ABS(X143))<=C143,MAX(ABS(V143),ABS(X143))/C143*D143,D143+(MAX(ABS(V143),ABS(X143))-C143)/(E143-C143)*(F143-D143)),IF(MAX(ABS(V143),ABS(X143),ABS(Z143),ABS(AB143))<=C143,MAX(ABS(V143),ABS(X143),ABS(Z143),ABS(AB143))/C143*D143,D143+(MAX(ABS(V143),ABS(X143),ABS(Z143),ABS(AB143))-C143)/(E143-C143)*(F143-D143))),IF(move1,IF(MAX(ABS((V143-W143)*2/PI()+W143),ABS((X143-W143)*2/PI()+W143))<=C143,MAX(ABS((V143-W143)*2/PI()+W143),ABS((X143-W143)*2/PI()+W143))/C143*D143,D143+(MAX(ABS((V143-W143)*2/PI()+W143),ABS((X143-W143)*2/PI()+W143))-C143)/(E143-C143)*(F143-D143)),IF(MAX(ABS((V143-W143)*2/PI()+W143),ABS((X143-W143)*2/PI()+W143),ABS((Z143-AA143)*2/PI()+AA143),ABS((AB143-AA143)*2/PI()+AA143))<=C143,MAX(ABS((V143-W143)*2/PI()+W143),ABS((X143-W143)*2/PI()+W143),ABS((Z143-AA143)*2/PI()+AA143),ABS((AB143-AA143)*2/PI()+AA143))/C143*D143,D143+(MAX(ABS((V143-W143)*2/PI()+W143),ABS((X143-W143)*2/PI()+W143),ABS((Z143-AA143)*2/PI()+AA143),ABS((AB143-AA143)*2/PI()+AA143))-C143)/(E143-C143)*(F143-D143))))","v":3.7170989618298975},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V143)+Ltime2*ABS(Lspeed2)*ABS(W143)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X143)+Ltime4*ABS(Lspeed1)*ABS(Y143))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V143)+Ltime2*ABS(Lspeed2)*ABS(W143)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X143)+Ltime4*ABS(Lspeed1)*ABS(Y143)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z143)+Ltime6*ABS(Lspeed6)*ABS(AA143)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB143)+Ltime8*ABS(Lspeed1)*ABS(AC143))/ltime)","v":153.69673846153847},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK143/2*Ltime1/ltime,AK143/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X143*-ABS(Lspeed2-Lspeed1),((X143-Y143)*2/PI()+Y143)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V143*-ABS(Lspeed2-Lspeed1),((V143-W143)*2/PI()+W143)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X143*-ABS(Lspeed2-Lspeed1),((X143-Y143)*2/PI()+Y143)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V143*-ABS(Lspeed2-Lspeed1),((V143-W143)*2/PI()+W143)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB143*-ABS(Lspeed6-Lspeed1),((AB143-AC143)*2/PI()+AB143)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z143*-ABS(Lspeed6-Lspeed1),((Z143-AA143)*2/PI()+AA143)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB143*-ABS(Lspeed6-Lspeed1),((AB143-AC143)*2/PI()+AB143)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z143*-ABS(Lspeed6-Lspeed1),((Z143-AA143)*2/PI()+AA143)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":24.46159566325608},{"$f":"IF(move1,MAX(IF(AccType=1,X143*-ABS(Lspeed2-Lspeed1),((X143-Y143)*2/PI()+Y143)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V143*-ABS(Lspeed2-Lspeed1),((V143-W143)*2/PI()+W143)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X143*-ABS(Lspeed2-Lspeed1),((X143-Y143)*2/PI()+Y143)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V143*-ABS(Lspeed2-Lspeed1),((V143-W143)*2/PI()+W143)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB143*-ABS(Lspeed6-Lspeed1),((AB143-AC143)*2/PI()+AB143)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z143*-ABS(Lspeed6-Lspeed1),((Z143-AA143)*2/PI()+AA143)*-ABS(Lspeed6-Lspeed1)),0))","v":212.00049574821935},{"$f":"(J143^2)+3*(I143/1000)^2*(F143/2)^2*(2000*PI()/M143)^2","v":2395.5373910994413},{"$f":"SQRT(3)*H143*F143/2*J143","v":1724.107035941903},{"$f":"3*F143^2*H143^2/4-(UAC_V*0.98)^2","v":-48788.843125000007},{"$f":"-AM143/2/AL143+SQRT((AM143/2/AL143)^2-AN143/AL143)","v":4.1673985229559918},{"$f":"(J143^2)+3*(I143/1000)^2*(D143/2)^2*(2000*PI()/M143)^2","v":1520.2777409255223},{"$f":"SQRT(3)*H143*D143/2*J143","v":385.38863156348418},{"$f":"3*D143^2*H143^2/4-(UAC_V*0.98)^2","v":-50704.413925000001},{"$f":"-AQ143/2/AP143+SQRT((AQ143/2/AP143)^2-AR143/AP143)","v":5.6497666825435253},{"$f":"(J143^2)+3*(I143/1000)^2*(AH143/2)^2*(2000*PI()/M143)^2","v":1650.4295738121589},{"$f":"SQRT(3)*H143*AH143/2*J143","v":753.96193804509051},{"$f":"3*AH143^2*H143^2/4-(UAC_V*0.98)^2","v":-50419.566964906982},{"$f":"IF((AU143/2/AT143)^2-AV143/AT143>=0,-AU143/2/AT143+SQRT((AU143/2/AT143)^2-AV143/AT143),-9999)","v":5.3034513659679519},null,54.3]
["IC/ICD","ICD05-075A5",125,3.3,441,14.7,"NA",2,7,22.203152929257591,1.36,330,32,10.151711368117695,7.576524452548199,9.8692377577072605,null,3.6764705882352939,1.030565989850281,0.75512380952380964,0.10680788031633376,199.80576000000002,0,-333.00960000000003,0,0,0,0,0,0.28340564720882727,0.45017265822784819,3.400867766505927,10.804143797468356,6.4386254795243687,153.69673846153847,24.46159566325608,212.00049574821935,799.14235723595277,565.31773773692953,-50156.890000000007,7.576524452548199,508.40925665370685,126.90806357359644,-50772.490000000005,9.8692377577072605,551.71587613073939,247.61014899456256,-50680.792305803261,9.3626050534688261,null,31.4]
["IC/ICD","ICD05-100A1",157,1.8,588,8.5,"NA",7.7,27.6,51.194530957906039,1.71,330,32,4.4028140463935861,3.0344840628263272,4.2252823327882529,null,2.9239766081871346,0.86566841323851618,0.59750952380952382,0.24530310919435344,210.80135999999999,0,-351.3356,0,0,0,0,0,0.12985026198577743,0.20087476024748649,1.5582031438293291,4.8209942459396755,2.8363577052608004,162.15489230769231,25.807752657303187,223.66718969662762,4212.2715914827904,2901.7757763393779,-47592.383125,3.0344840628263272,2692.2448270782593,614.49369381304473,-50661.085300000006,4.2252823327882529,2798.0789764752976,968.29106848933372,-50447.422296130993,4.0765891768933953,null,72.400000000000006]
["IC/ICD","ICD05-100A5",157,3.1,588,14.7,"NA",2.6,9.1999999999999993,29.557063453597682,1.71,330,32,7.6259267215046815,5.6149372256920937,7.4075892220322439,null,2.9239766081871346,0.86566841323851618,0.59750952380952382,0.13887354807869393,210.80135999999999,0,-351.3356,0,0,0,0,0,0.22363100675328337,0.34709908739365813,2.6835720810394004,8.3303780974477952,4.8942909523918336,162.15489230769231,25.807752657303187,223.66718969662762,1402.4686105398168,978.3237537778582,-49709.583700000003,5.6149372256920937,897.13906681145625,206.31317256539867,-50756.437300000005,7.4075892220322439,932.24411033074489,325.72796575680184,-50683.712794491817,7.2007953554505653,null,41.8]
["IC/ICD","ICD10-030A1",104,1.9,330,7.9,"NA",6.4,18.3,30.900566337852126,1.1000000000000001,330,32,7.2943646901349117,5.1824416901813368,6.9940824923372631,null,4.545454545454545,1.1880239587276837,0.96786666666666654,0.15961300230850142,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,0.18810379346521658,0.31743657817109144,2.2572455215825991,7.6184778761061942,4.5371807650030789,147.41353846153845,23.461593324821077,203.33380881511599,1559.1795246697509,1353.0197502416586,-48887.924800000001,5.1824416901813368,989.8016997926261,325.40981334925959,-50694.260800000004,6.9940824923372631,1154.1854284846384,777.07533993237007,-50172.757794478683,6.2651537502389134,null,43.7]
["IC/ICD","ICD10-030A4",104,3.9,330,15.8,"NA",1.6,4.5999999999999996,15.414927829866736,1.1000000000000001,330,32,14.62218976875668,10.930332174287598,14.172196028154087,null,4.545454545454545,1.1880239587276837,0.96786666666666654,7.7441523769838136E-2,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,0.38610778658649719,0.63506865781710908,4.6332934390379661,15.241647787610617,9.1304085172561074,147.41353846153845,23.461593324821077,203.33380881511599,390.35932983381923,337.48089880169516,-50325.851200000005,10.930332174287598,246.92606155572983,83.302247172570318,-50775.9568,14.172196028154087,288.62551366519358,195.02142233102808,-50645.100429391394,12.912969054845474,null,21.8]
["IC/ICD","ICD10-030A5",104,3.4,330,13.7,"NA",2.1,6.1,17.819090885900994,1.1000000000000001,330,32,12.649354641226019,9.4109215778804209,12.238146054492752,null,4.545454545454545,1.1880239587276837,0.96786666666666654,8.9820498909846155E-2,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,0.33660678830617702,0.55069668141592909,4.0392814596741244,13.216720353982298,7.9271603132552855,147.41353846153845,23.461593324821077,203.33380881511599,519.45976559181304,443.97246536919369,-50184.375325000001,9.4109215778804209,329.95765618968159,110.18294760987288,-50766.925300000003,12.238146054492752,385.13078770981906,256.89349690896194,-50597.317127884497,11.133316026263795,null,25.2]
["IC/ICD","ICD10-030A8",104,6.8,330,27.4,"NA",0.5,1.5,8.9095454429504972,1.1000000000000001,330,32,25.298709282452037,19.469857278612988,24.671721334072632,null,4.545454545454545,1.1880239587276837,0.96786666666666654,4.403557051322609E-2,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,0.67321357661235404,1.1013933628318582,8.0785629193482489,26.433440707964596,15.854320626510571,147.41353846153845,23.461593324821077,203.33380881511599,128.22326499130119,105.70772984980803,-50664.392500000002,19.469857278612988,82.388301685222629,26.234035145207834,-50796.490000000005,24.671721334072632,95.733052657575158,61.165118311657615,-50758.030097025963,22.708914369569705,null,12.6]
["IC/ICD","ICD10-050A1",171,1.9,550,7.9,"NA",9,29,51.477373670380658,1.9,330,32,4.378622760424391,2.9998782260147636,4.1615679988381036,null,2.6315789473684212,0.81730034779310312,0.65688000000000002,0.2493613654825251,216.77040000000002,0,-361.28399999999999,0,0,0,0,0,0.12940588840057465,0.20468381706244498,1.5528706608068958,4.9124116094986796,2.8340454539321778,166.74646153846155,26.538523596928759,230.00053784004925,4167.5685868412329,3169.6887169562879,-47013.752500000002,2.9998782260147636,2737.7057939191927,762.33019774898048,-50585.852500000001,4.1615679988381036,2845.2327802092536,1137.0939112240615,-50317.227321676568,4.0102443217896102,null,72.8]
["IC/ICD","ICD10-050A4",171,3.8,550,15.8,"NA",2.2000000000000002,7.3,25.738686835190329,1.9,330,32,8.757245520848782,6.5430183709823293,8.474344816754968,null,2.6315789473684212,0.81730034779310312,0.65688000000000002,0.12129040420697502,216.77040000000002,0,-361.28399999999999,0,0,0,0,0,0.25881177680114931,0.40936763412488997,3.1057413216137917,9.8248232189973592,5.6680909078643555,166.74646153846155,26.538523596928759,230.00053784004925,1047.1434634614473,774.81279747820372,-49898.966800000002,6.5430183709823293,684.73020194032722,186.34738167197307,-50752.7428,8.474344816754968,711.98400978526104,277.95628941032612,-50688.538066020476,8.2446753025371908,null,36.4]
["IC/ICD","ICD10-050A5",171,3.3,550,13.7,"NA",3,9.6999999999999993,29.698484809834994,1.9,330,32,7.5896127847356105,5.5967428148774587,7.3215160502366796,null,2.6315789473684212,0.81730034779310312,0.65688000000000002,0.14060632060556247,216.77040000000002,0,-361.28399999999999,0,0,0,0,0,0.22475759564310335,0.35506306068601573,2.6970911477172401,8.521513456464378,4.9190121201491079,166.74646153846155,26.538523596928759,230.00053784004925,1392.6292003368367,1057.0772984980804,-49538.252500000002,5.5967428148774587,911.62732160300561,254.62445876231132,-50731.652500000004,7.3215160502366796,947.82946071087872,379.54569658733823,-50641.832408392329,7.1120558143702635,null,42]
["IC/ICD","ICD10-050A8",171,6.6,550,27.4,"NA",0.7,2.4,14.849242404917497,1.9,330,32,15.179225569471221,11.741051503318733,14.803295553484697,null,2.6315789473684212,0.81730034779310312,0.65688000000000002,6.9146777877274593E-2,216.77040000000002,0,-361.28399999999999,0,0,0,0,0,0.44951519128620671,0.71012612137203146,5.3941822954344802,17.043026912928756,9.8380242402982159,166.74646153846155,26.538523596928759,230.00053784004925,345.53875837773109,246.65136964955204,-50529.255700000002,11.741051503318733,227.75489945513073,59.412373711205966,-50789.151700000002,14.803295553484697,236.61978716950415,88.560662537045573,-50769.590880049887,14.461989852583638,null,21]
["IC/ICD","ICD10-075A1",246,1.8,824,7.9,"NA",12.2,42.4,77.216060505570979,2.7,330,32,2.9190818402829275,1.8599928728315334,2.7511763562426195,null,1.8518518518518516,0.63399279364862671,0.48928640776699034,0.36522339990650882,241.9032,0,-403.17200000000003,0,0,0,0,0,9.5098919047294006E-2,0.14411398500576703,1.1411870285675281,3.4587356401384088,1.9125784219314768,186.07938461538461,29.615453869036447,256.66726686498254,9206.5149149580193,6445.0337244777857,-43838.331700000002,1.8599928728315334,6130.7415914831581,1468.4886967164575,-50443.478800000004,2.7511763562426195,6152.4677802945989,1560.3332189945404,-50396.822347157176,2.7380501913513307,null,109.2]
["IC/ICD","ICD10-075A4",246,3.7,824,15.8,"NA",3,10.6,38.60803025278549,2.7,330,32,5.838163680565855,4.2882044095757772,5.6281144829173213,null,1.8518518518518516,0.63399279364862671,0.48928640776699034,0.1782387424538982,241.9032,0,-403.17200000000003,0,0,0,0,0,0.19548111137499324,0.2912616205305652,2.3457733364999189,6.9902788927335653,3.9233112959624372,186.07938461538461,29.615453869036447,256.66726686498254,2301.6287287395048,1584.8443584781439,-49120.090000000004,4.2882044095757772,1535.0570753743141,371.13443837779323,-50712.752500000002,5.6281144829173213,1540.5878647558836,393.53403632655977,-50701.261492206075,5.6104525101137988,null,54.6]
["IC/ICD","ICD10-075A5",246,3.2,824,13.7,"NA",4.0999999999999996,14.1,44.61843789287115,2.7,330,32,5.0517232481599939,3.6345077129108123,4.8501915202103518,null,1.8518518518518516,0.63399279364862671,0.48928640776699034,0.20688175510138399,241.9032,{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},-403.17200000000003,{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},0,{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0,0,0.16906474497296711,0.25230002883506347,2.0287769396756055,6.0552006920415238,3.3937825295541812,186.07938461538461,29.615453869036447,256.66726686498254,3069.7527236578439,2170.4481578923678,-48438.858325000001,3.6345077129108123,2049.6702815294175,506.96599308434872,-50676.059200000003,4.8501915202103518,2057.0155641234305,537.66635325242135,-50659.949842591435,4.8336790236042919,null,63.1]
["IC/ICD","ICD10-075A8",246,6.4,824,27.4,"NA",1,3.5,22.273863607376246,2.7,330,32,10.119483712980815,7.7803573156941184,9.8515214665947273,null,1.8518518518518516,0.63399279364862671,0.48928640776699034,0.10176319198399836,241.9032,0,-403.17200000000003,0,0,0,0,0,0.33812948994593423,0.50460005767012694,4.0575538793512109,12.110401384083048,6.7875650591083625,186.07938461538461,29.615453869036447,256.66726686498254,762.0494427304177,528.53864924904019,-50242.090000000004,7.7803573156941184,510.63331846960131,123.45428303627217,-50774.44,9.8515214665947273,512.44368438231515,130.93030905223051,-50770.60672042628,9.8267357823960939,null,31.5]
["IC/ICD","ICD10-100A1",315,1.8,1099,7.9,"NA",15.4,55.8,103.02545801887996,3.4,330,32,2.1878087643026469,1.2649308360201736,2.0356790647478977,null,1.4705882352941178,0.5401289254980508,0.40020382165605095,0.48644366756660973,263.89440000000002,0,-439.82400000000001,0,0,0,0,0,8.1019338824707618E-2,0.11546696428571429,0.97223206589649147,2.771207142857143,1.6000037414959949,202.99569230769234,32.307767857130663,280.00065476179913,16233.045649146652,10854.829287747527,-39704.293300000005,1.2649308360201736,10905.943671739064,2473.2522427779172,-50228.861200000007,2.0356790647478977,10844.724040772286,2198.4515789489051,-50349.810670397856,2.0557364946334058,null,145.69999999999999]
["IC/ICD","ICD10-100A4",315,3.5,1099,15.8,"NA",3.9,13.9,51.477373670380658,3.4,330,32,4.378622760424391,3.1205396766001665,4.2067260596698244,null,1.4705882352941178,0.5401289254980508,0.40020382165605095,0.23634841375497881,263.89440000000002,0,-439.82400000000001,0,0,0,0,0,0.15753760327026481,0.2274306547619048,1.8904512392431778,5.458335714285715,3.1111183862422123,202.99569230769234,32.307767857130663,280.00065476179913,4044.5686728351702,2747.0635546954495,-47957.3917,3.1205396766001665,2718.3563332888589,608.52673679962493,-50665.418125000004,4.2067260596698244,2703.9934051216328,540.91391982208245,-50694.746150277264,4.2310417240062161,null,72.8]
["IC/ICD","ICD10-100A5",315,3.1,1099,13.7,"NA",5.0999999999999996,18.600000000000001,59.46768029778864,3.4,330,32,3.7902941374422792,2.6372389223954862,3.6225063730199087,null,1.4705882352941178,0.5401289254980508,0.40020382165605095,0.27427885881219982,263.89440000000002,0,-439.82400000000001,0,0,0,0,0,0.13953330575366313,0.19948630952380952,1.6743996690439575,4.7876714285714286,2.7555619992431026,202.99569230769234,32.307767857130663,280.00065476179913,5413.9401062656179,3598.3414611016788,-47143.797325000007,2.6372389223954862,3632.5375183611936,814.22325032227775,-50617.692925000003,3.6225063730199087,3612.3619129568474,723.75569273815256,-50657.037173917903,3.6459244592551889,null,84.1]
["IC/ICD","ICD10-100A8",315,6.1,1099,27.4,"NA",1.3,4.5999999999999996,29.698484809834994,3.4,330,32,7.5896127847356105,5.7645237885021299,7.378172893410202,null,1.4705882352941178,0.5401289254980508,0.40020382165605095,0.13494220425126016,263.89440000000002,0,-439.82400000000001,0,0,0,0,0,0.27456553712817583,0.39546934523809524,3.2947864455381097,9.4912642857142853,5.4222349017364273,202.99569230769234,32.307767857130663,280.00065476179913,1341.3437720959705,916.13365869833626,-49853.5717,5.7645237885021299,904.7665056205592,203.95676343284129,-50757.996325,7.378172893410202,899.9884342492212,181.29532477553309,-50767.894699789722,7.4105800001459627,null,42]
["IC/ICD","IC11-015A1",73,3.9,190,11.3,"NA",1.4,9.1,10.889444430272832,1.7,330,32,20.698943958369846,10.7475713858543,17.935275583303532,null,2.9411764705882355,1.8590053771422639,1.8463789473684211,0.10599482384374768,210.4872,0,-350.81200000000001,0,0,0,0,0,0.60417674757123574,0.89462564102564102,7.2501209708548293,21.471015384615384,13.408295139489216,161.91323076923078,25.769291028901844,223.33385558381596,424.32595149393956,149.19107176369502,-50617.455700000006,10.7475713858543,154.99942142863827,51.490723883045185,-50782.801300000006,17.935275583303532,549.05798880801092,177.02636481277335,-50540.879903534958,9.4344229627113716,null,15.4]
["IC/ICD","IC11-015A5",73,6.7,190,19.100000000000001,"NA",0.47,3,6.293250352560273,1.7,330,32,35.816150220100631,19.239880884193891,31.304735153912677,null,2.9411764705882355,1.8590053771422639,1.8463789473684211,5.8961431128633793E-2,210.4872,0,-350.81200000000001,0,0,0,0,0,1.0379446689044307,1.505971794871795,12.455336026853168,36.143323076923082,22.632818882387337,161.91323076923078,25.769291028901844,223.33385558381596,134.5408596700762,48.925679461646212,-50744.720103250002,19.239880884193891,51.286891232668289,17.162411120053907,-50797.72284925,31.304735153912677,172.90828410091217,57.975185442574684,-50720.293894025985,16.960239615255269,null,8.9]
["IC/ICD","IC11-030A1",144,4,320,11.3,"NA",1.9,16.7,21.849599538664314,2.5,330,32,10.315978542359083,5.6530667537841754,9.0312967254907779,null,2,1.0549393076133804,1.2271874999999999,0.1467665396337825,235.62,0,-392.7,0,0,0,0,0,0.35164643587112682,0.59647490530303038,4.2197572304535216,14.315397727272728,8.3966151570674388,181.24615384615385,28.846221301009521,250.00058460874919,1507.1053793279168,406.26195840661103,-50459.439325000007,5.6530667537841754,606.43002991030346,143.80954279880035,-50761.840000000004,9.0312967254907779,1045.946908362082,301.87834669883642,-50614.27273194537,6.8135421227156971,null,30.9]
["IC/ICD","IC11-030A5",144,6.9,320,19.100000000000001,"NA",0.63,5.6,12.586500705120546,2.5,330,32,17.908075110050316,10.046594108160324,15.755853565869845,null,2,1.0549393076133804,1.2271874999999999,8.3124058289544639E-2,235.62,0,-392.7,0,0,0,0,0,0.60659010187769369,1.0058096590909091,7.2790812225323247,24.139431818181819,14.247767796742844,181.24615384615385,28.846221301009521,250.00058460874919,489.21872880595447,131.16245983334943,-50696.565183250001,10.046594108160324,201.59131514610752,47.38329700785922,-50790.987693250005,15.755853565869845,342.49328152036139,97.841480175663477,-50744.732306255748,12.030211476402135,null,17.8]
["IC/ICD","IC11-050A1",263,4.4000000000000004,533,11.3,"NA",2.6,26.7,36.345288552988542,3.6,330,32,6.2016291237139232,3.4470181180078181,5.3258814032209898,null,1.3888888888888888,0.66232539343392149,0.84483302063789867,0.19448966447184007,270.17759999999998,0,-450.29599999999999,0,0,0,0,0,0.24285264425910458,0.38276888888888894,2.9142317311092549,9.1864533333333345,5.0048319460163846,207.82892307692308,33.077000425157586,286.66733701803241,3953.0682907923506,924.76321106216142,-50157.771700000005,3.4470181180078181,1720.0498512784079,360.08479014809831,-50707.004800000002,5.3258814032209898,1837.3042995405849,409.58269568359276,-50678.164901964119,5.1416613973581553,null,51.4]
["IC/ICD","IC11-050A5",263,7.6,533,19.100000000000001,"NA",0.87,8.9,21.001071401240459,3.6,330,32,10.732785756191774,6.1784112860707339,9.306138276226962,null,1.3888888888888888,0.66232539343392149,0.84483302063789867,0.1110379998338933,270.17759999999998,0,-450.29599999999999,0,0,0,0,0,0.41947274917481692,0.64905925925925934,5.033672990097803,15.577422222222223,8.60805324336064,207.82892307692308,33.077000425157586,286.66733701803241,1276.5860493851928,302.22104508952339,-50598.066483250004,6.1784112860707339,573.33537310514703,120.25549438117159,-50772.371092000001,9.306138276226962,610.756372567482,136.20601295260283,-50763.096088234888,9.0059259127140674,null,29.7]
["IC/ICD","IC11-075A1",413,4.5999999999999996,800,11.3,"NA",3.5,39.4,54.51793282948281,5,330,32,4.1344194158092824,2.2831035981097467,3.4966585586150845,null,1,0.49043183307934396,0.65450000000000008,0.27231120738499937,314.16000000000003,0,-523.6,0,0,0,0,{"$f":"(Ltorque2+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0.18799886934708185,0.27144918173987942,2.2559864321649821,6.5147803617571061,3.7126801911226672,241.66153846153847,38.461628401346033,333.33411281166559,8703.732415301678,1867.3103300293646,-49632.008125,2.2831035981097467,3921.9984067490282,760.14402815354651,-50610.752500000002,3.4966585586150845,3590.9170421220906,613.51558167953556,-50678.519553273218,3.6722689807848372,null,77.099999999999994]
["IC/ICD","IC11-075A5",413,8,800,19.100000000000001,"NA",1.2,13.1,31.466251762801363,5,330,32,7.1632300440201266,4.1327985476301059,6.1295802150949363,null,1,0.49043183307934396,0.65450000000000008,0.155656426424059,314.16000000000003,0,-523.6,0,0,0,0,0,0.32695455538622931,0.46551033591731272,3.9234546646347517,11.172248062015505,6.4568351149959433,241.66153846153847,38.461628401346033,333.33411281166559,2800.3408753313083,624.58314206356852,-50411.165200000003,4.1327985476301059,1307.698027113302,261.60550452924338,-50736.04,6.1295802150949363,1196.997625912094,211.14295099008112,-50760.134022721577,6.4244054869644316,null,44.5]
["IC/ICD","IC11-100A1",574,4.8,1067,11.3,"NA",4.4000000000000004,52,72.831998462214386,6.5,330,32,3.094793562707725,1.6897626138505228,2.5729907724577425,null,0.76923076923076927,0.40580243749309125,0.56432989690721647,0.35613345197061491,361.28399999999999,0,-602.14,0,0,0,0,0,0.16232097499723649,0.21545892494929006,1.9478516999668378,5.1710141987829612,3.2055824089205474,277.91076923076923,44.230872661547934,383.33422973341544,15288.041273271494,3136.0572227878747,-48951.101200000005,1.6897626138505228,7105.9001952868284,1332.1305017152033,-50470.619200000001,2.5729907724577425,6107.9181212421172,889.63627139265816,-50655.955985412875,2.807936166812298,null,103]
["IC/ICD","IC11-100A5",574,8.1999999999999993,1067,19.100000000000001,"NA",1.5,17.3,41.93143212436226,6.5,330,32,5.3754424445007709,3.0913722580901011,4.5597750008963596,null,0.76923076923076927,0.40580243749309125,0.56432989690721647,0.20234770348040004,361.28399999999999,0,-602.14,0,0,0,0,0,0.27729833228694567,0.36759009465855302,3.327579987443348,8.8221622718052721,5.476203281905935,277.91076923076923,44.230872661547934,383.33422973341544,4915.2842711841222,1040.3870877631916,-50189.543125000004,3.0913722580901011,2340.1350813969466,446.65833087215543,-50691.692500000005,4.5597750008963596,2017.765919997968,298.29168505033226,-50754.553895975725,4.9419883833614291,null,59.3]
["IC/ICD","IC11-150A1",861,4.8,1600,11.3,"NA",6.2,77.3,108.89444430272832,9.4,330,32,2.0698943958369846,1.0853020393748447,1.6928534151577723,null,0.53191489361702127,0.33875681738553715,0.47124000000000005,0.52442478118010771,452.3904,0,-753.98400000000004,0,0,0,0,0,0.13550272695421486,0.17514146341463413,1.6260327234505783,4.2033951219512193,2.6759644457075873,347.99261538461542,55.384744897938283,480.00112244879847,33919.595538005335,6607.0331781064942,-47123.857300000003,1.0853020393748447,15838.728022520501,2806.5273676912539,-50140.916800000006,1.6928534151577723,13095.202272471155,1564.6182191348128,-50598.714547845462,1.9068511555645982,null,154]
["IC/ICD","IC11-150A5",861,8.3000000000000007,1600,19.100000000000001,"NA",2.1,25.8,62.932503525602726,9.4,330,32,3.5816150220100633,2.0279753065896293,3.004578399404763,null,0.53191489361702127,0.33875681738553715,0.47124000000000005,0.29884027105818345,452.3904,0,-753.98400000000004,0,0,0,0,0,0.23430679869166324,0.30284878048780489,2.8116815842999587,7.2683707317073178,4.6271885207027035,347.99261538461542,55.384744897938283,480.00112244879847,10981.956181198837,2186.0409972224902,-49598.550925000003,2.0279753065896293,5286.4179198015072,949.95498832181511,-50577.306325000005,3.004578399404763,4372.5926258232457,529.59286953577987,-50734.343535547749,3.3462692175289268,null,89]
["IC/ICD","IC11-200A1",1197,5,2135,11.3,"NA",8,103,145.66399692442877,12.3,330,32,1.5473967813538625,0.77087213911992813,1.2259941506176262,null,0.4065040650406504,0.29273904796730199,0.42427540983606554,0.69914324986117227,543.49680000000001,0,-905.82799999999997,0,0,0,0,0,0.12197460331970916,0.1576559454191033,1.46369523983651,3.783742690058479,2.4088054100425293,418.07446153846155,66.538617134328632,576.6680151641815,60387.892517802247,11403.844446501362,-44676.04,0.77087213911992813,28886.94285335622,5045.9488701333457,-49605.16,1.2259941506176262,22997.913629740076,2430.9417874350383,-50526.647511834395,1.4303220408672592,null,206]
["IC/ICD","IC11-200A5",1197,8.6,2135,19.100000000000001,"NA",2.7,34.200000000000003,84.145706961199153,12.3,330,32,2.6786868652008038,1.4916282607402378,2.2068796357563434,null,0.4065040650406504,0.29273904796730199,0.42427540983606554,0.39680000405396132,543.49680000000001,0,-905.82799999999997,0,0,0,0,0,0.20979631770989973,0.27116822612085767,2.5175558125187969,6.5080374269005841,4.1431453052731504,418.07446153846155,66.538617134328632,576.6680151641815,19418.364322723108,3758.0255345510232,-48810.561325000002,1.4916282607402378,9581.8251975236453,1692.0952668659054,-50400.7837,2.2068796357563434,7661.0419203947004,815.18564662679012,-50711.306792109834,2.5201612645750093,null,119]
["IC/ICD","IC11-250A1",1496,4.9000000000000004,3125,11.3,"NA",9.6999999999999993,128,174.65537495307723,15.2,330,32,1.2905414451777153,0.59271178056159479,1.0004684713025684,null,0.32894736842105265,0.27349442584543682,0.33845503999999998,0.83902926065865502,634.60320000000002,0,-1057.672,0,0,0,0,0,0.11167689055355338,0.14434583333333334,1.3401226866426406,3.4643000000000002,2.2054418774130125,488.15630769230768,77.692489370718974,673.33490787956453,90996.489726804808,16579.169241124157,-41794.395925000004,0.59271178056159479,41879.021680167461,7189.1972815494146,-49110.834325000003,1.0004684713025684,32808.763902079998,3235.7870917781356,-50461.921523600846,1.1918535465795075,null,247]
["IC/ICD","IC11-250A5",1496,8.6,3125,19.100000000000001,"NA",3.2,42.6,101.11626970967629,15.2,330,32,2.229117041670599,1.1906262383656103,1.8037129533222052,null,0.32894736842105265,0.27349442584543682,0.33845503999999998,0.47688639128293481,634.60320000000002,0,-1057.672,0,0,0,0,0,0.19600433852256305,0.25334166666666663,2.3520520622707566,6.0801999999999996,3.8707755399493684,488.15630769230768,77.692489370718974,673.33490787956453,29367.366743874161,5352.2330675709554,-48003.419200000004,1.1906262383656103,14105.441926967276,2409.9059885398015,-50237.147200000007,1.8037129533222052,11010.705753510667,1084.6750179089963,-50690.091302804452,2.0969354929792994,null,143]
["IC/ICD","IC22-015A1",143,3.8,375,11,"NA",2.9,18.3,21.849599538664314,3.2,330,32,10.315978542359083,5.3286794111093982,8.8970774628140106,null,1.5625,1.1614660460884658,1.1449386666666665,0.15023942873965349,257.6112,0,-429.35199999999998,0,0,0,0,0,0.36779758126134748,0.52861609195402293,4.41357097513617,12.686786206896549,7.8448474225865246,198.16246153846154,31.538535289103745,273.33397250556578,1649.0838573151716,603.62163358970145,-50041.952500000007,5.3286794111093982,617.23179917050459,208.52383705826048,-50714.079700000002,8.8970774628140106,1073.3308511191524,430.48360149851243,-50416.9861619398,6.6560423477972446,null,30.9]
["IC/ICD","IC22-015A2",143,7.6,375,22,"NA",0.73,4.5999999999999996,10.889444430272832,3.2,330,32,20.698943958369846,10.866136355280796,17.994688306240516,null,1.5625,1.1614660460884658,1.1449386666666665,7.393463687664717E-2,257.6112,0,-429.35199999999998,0,0,0,0,0,0.73559516252269497,1.0572321839080459,8.8271419502723401,25.373572413793099,15.689694845173049,198.16246153846154,31.538535289103745,273.33397250556578,414.70976942624782,151.45440028602667,-50611.717300000004,10.866136355280796,153.91978405384313,52.320611007900119,-50782.074772,17.994688306240516,269.19412415636504,108.01242379302036,-50706.773394386553,13.525460355860051,null,15.4]
["IC/ICD","IC22-015A6",143,13.1,375,38.1,"NA",0.24,1.5,6.293250352560273,3.2,330,32,35.816150220100631,19.271340879659554,31.463213508917818,null,1.5625,1.1614660460884658,1.1449386666666665,4.1874281918867225E-2,257.6112,0,-429.35199999999998,0,0,0,0,0,1.2679337669799084,1.8315373563218389,15.215205203758902,43.956896551724135,27.144609106203209,198.16246153846154,31.538535289103745,273.33397250556578,134.04446386864348,49.835848612820868,-50742.450448000003,19.271340879659554,50.76967673445202,17.135160546665443,-50797.746448000005,31.463213508917818,87.541988314820145,35.505895802386924,-50773.328952487573,23.881006531348582,null,8.9]
["IC/ICD","IC22-030A1",280,3.9,624,11,"NA",3.9,33.4,43.628488399209978,4.8,330,32,5.1663490593013881,2.7813017765042072,4.4803299103628333,null,1.0416666666666667,0.70891921471619168,0.82232051282051288,0.23689858521896809,307.8768,0,-513.12800000000004,0,0,0,0,0,0.23039874478276232,0.36298556201550386,2.7647849373931477,8.7116534883720931,4.8631940608824689,236.8283076923077,37.692395833319111,326.6674305554323,5806.4521547866852,1620.9069712162691,-49424.852500000001,2.7813017765042072,2394.0626762339293,574.68519888576816,-50631.651925000006,4.4803299103628333,2666.3266647326714,716.61683233290466,-50535.365136275104,4.2212155850390092,null,61.7]
["IC/ICD","IC22-030A2",280,7.9,624,22,"NA",1,8.4,21.849599538664314,4.8,330,32,10.315978542359083,5.7277116731770414,9.038828039456094,null,1.0416666666666667,0.70891921471619168,0.82232051282051288,0.11709438752757793,307.8768,0,-513.12800000000004,0,0,0,0,0,0.46670514968815957,0.727314050387597,5.6004617962579148,17.455537209302328,9.8128220082313824,236.8283076923077,37.692395833319111,326.6674305554323,1464.8774258372423,416.29078178600105,-50442.16,5.7277116731770414,604.7358968935996,149.48623527770039,-50758.352500000001,9.038828039456094,673.86197760607388,185.68124296970538,-50732.941393176079,8.5401189682509866,null,30.9]
["IC/ICD","IC22-030A6",280,13.7,624,38.1,"NA",0.33,2.8,12.586500705120546,4.8,330,32,17.908075110050316,10.057208623420253,15.775226796362151,null,1.0416666666666667,0.70891921471619168,0.82232051282051288,6.7022754507751914E-2,307.8768,0,-513.12800000000004,0,0,0,0,0,0.80934943680098537,1.2598259689922482,9.7121932416118248,30.235823255813955,17.010131702187639,236.8283076923077,37.692395833319111,326.6674305554323,487.48906521340666,137.0485836852574,-50686.599753250004,10.057208623420253,200.96791083686682,49.279936915696226,-50789.83041925,15.775226796362151,224.01223940189169,61.186731183320539,-50781.527781385565,14.920305907217511,null,17.8]
["IC/ICD","IC22-050A1",526,4.4000000000000004,1039,11,"NA",5.3,53.4,72.831998462214386,6.9,330,32,3.094793562707725,1.6607860603126703,2.5979566551178834,null,0.72463768115942029,0.45823675475951559,0.59969586140519737,0.36162036624894284,373.85040000000004,0,-623.08400000000006,0,0,0,0,0,0.16802014341182239,0.23537641325536066,2.0162417209418688,5.649033918128656,3.3181319670758205,287.57723076923077,45.769337797601786,396.66759424588213,15281.246281960197,3677.2352391096761,-48255.9925,1.6607860603126703,6900.7794051136307,1470.8940956438705,-50397.2932,2.5979566551178834,6212.3014386733721,1109.2319815770468,-50573.206830247276,2.7653309750579442,null,103]
["IC/ICD","IC22-050A2",526,8.6999999999999993,1039,22,"NA",1.3,13.4,36.345288552988542,6.9,330,32,6.2016291237139232,3.502733963246571,5.3364436616501596,null,0.72463768115942029,0.45823675475951559,0.59969586140519737,0.17711402286482458,373.85040000000004,0,-623.08400000000006,0,0,0,0,0,0.33222164720064878,0.46737469135802473,3.9866597664077852,11.216992592592593,6.5608518439908252,287.57723076923077,45.769337797601786,396.66759424588213,3833.8846029384245,900.21197537024568,-50191.69,3.502733963246571,1713.9588210669615,355.9929175327789,-50709.222925000002,5.3364436616501596,1544.4664009332741,268.46169993593179,-50750.600745255426,5.6460803262495558,null,51.4]
["IC/ICD","IC22-050A6",526,15.1,1039,38.1,"NA",0.44,4.5,21.001071401240459,6.9,330,32,10.732785756191774,6.1432261746060641,9.2958695494010168,null,0.72463768115942029,0.45823675475951559,0.59969586140519737,0.10179367561363675,373.85040000000004,0,-623.08400000000006,0,0,0,0,0,0.57661458307239044,0.81052891487979217,6.9193749968686848,19.452693957115013,11.387225614282928,287.57723076923077,45.769337797601786,396.66759424588213,1291.000174817791,304.89460190652767,-50594.386228000003,6.1432261746060641,574.55074838297094,120.83749314405689,-50772.052948000004,9.2958695494010168,516.96949671716391,91.126079277863738,-50786.332074675935,9.8237930202614212,null,29.7]
["IC/ICD","IC22-075A1",825,4.5999999999999996,1558,11,"NA",7.1,78.900000000000006,108.89444430272832,9.6,330,32,2.0698943958369846,1.0679483896132231,1.690962021346567,null,0.52083333333333337,0.35844919601234282,0.49066495507060337,0.529098391686597,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.13740552513806473,0.17760088888888889,1.6488663016567768,4.2624213333333332,2.713541698961389,352.82584615384616,56.153977465965212,486.66780470503181,33638.127622045999,7365.2482330875982,-46230.452500000007,1.0679483896132231,15666.822318037133,3080.0128974729955,-50005.153300000005,1.690962021346567,13183.403305645554,1816.9007457895352,-50526.771711920177,1.8900076350871504,null,154]
["IC/ICD","IC22-075A2",825,9.1999999999999993,1558,22,"NA",1.8,19.7,54.51793282948281,9.6,330,32,4.1344194158092824,2.3214852929433198,3.4935657490415584,null,0.52083333333333337,0.35844919601234282,0.49066495507060337,0.25973146957083881,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.27481105027612945,0.35520177777777778,3.2977326033135537,8.5248426666666663,5.4270833979227779,352.82584615384616,56.153977465965212,486.66780470503181,8403.4432900109878,1869.6710257689717,-49629.04,2.3214852929433198,3921.9984067490282,781.86242895793362,-50599.484800000006,3.4935657490415584,3302.7164326347106,461.22093561491079,-50733.588640874543,3.8501302966957622,null,77.099999999999994]
["IC/ICD","IC22-075A6",825,15.9,1558,38.1,"NA",0.59,6.6,31.466251762801363,9.6,330,32,7.1632300440201266,4.1225382572420317,6.1300586873910836,null,0.52083333333333337,0.35844919601234282,0.49066495507060337,0.14873171616613581,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.47494518471635422,0.61388133333333339,5.6993422165962508,14.733152000000002,9.3794158724969758,352.82584615384616,56.153977465965212,486.66780470503181,2818.4730204969378,612.56563919925645,-50426.18091925,4.1225382572420317,1308.5470713978484,255.63762895716999,-50739.157629250003,6.1300586873910836,1100.9302911847849,150.80073173889139,-50782.192333601335,6.7235155068269581,null,44.5]
["IC/ICD","IC22-100A1",1148,4.8,2077,11,"NA",8.8000000000000007,104,145.66399692442877,12.5,330,32,1.5473967813538625,0.76375683996968213,1.2288147490642869,null,0.4,0.30876272417952599,0.44116514203177659,0.70364872055489447,549.78,0,-916.3,0,0,0,0,0,0.1235050896718104,0.15963414634146339,1.4820610760617248,3.8312195121951214,2.4390300937438942,422.90769230769229,67.307849702355554,583.33469742041473,59059.913824601797,12211.196265722698,-43777.48,0.76375683996968213,28423.600781147314,5328.5220068608132,-49466.996800000001,1.2288147490642869,23078.467293991667,2707.5886520646113,-50459.649758281223,1.4211636727078878,null,206]
["IC/ICD","IC22-100A2",1148,9.5,2077,22,"NA",2.2000000000000002,26,72.831998462214386,12.5,330,32,3.094793562707725,1.7221663202195097,2.5806680684405086,null,0.4,0.30876272417952599,0.44116514203177659,0.34365899682885614,549.78,0,-916.3,0,0,0,0,0,0.24443715664212473,0.31594258130081299,2.9332458797054968,7.5826219512195117,4.8272470605347912,422.90769230769229,67.307849702355554,583.33469742041473,14764.978456150449,3052.7990664306744,-49048.240000000005,1.7221663202195097,7068.5664889825985,1318.2541423223367,-50477.552500000005,2.5806680684405086,5759.9773580803712,669.8461509014013,-50720.572599514111,2.9098612555690049,null,103]
["IC/ICD","IC22-100A6",1148,16.5,2077,38.1,"NA",0.73,8.6999999999999993,41.938503192174132,12.5,330,32,5.3745361146332096,3.0892462013334541,4.5480874684962229,null,0.4,0.30876272417952599,0.44116514203177659,0.19628427726380276,549.78,0,-916.3,0,0,0,0,0,0.42454874574684826,0.54874237804878045,5.0945849489621793,13.16981707317073,8.3841659472446377,422.90769230769229,67.307849702355554,583.33469742041473,4935.7816145411662,1010.1628521981629,-50224.987773250003,3.0892462013334541,2354.6750072036102,437.47210134566114,-50696.348481250003,4.5480874684962229,1912.6815954721824,222.293254240718,-50777.065150175185,5.0946515632325298,null,59.31]
["IC/ICD","IC22-150A1",1723,4.8,3117,11,"NA",12.4,155,217.78888860545663,18.100000000000001,330,32,1.0349471979184923,0.44053468906103488,0.78719868106108282,null,0.27624309392265189,0.27155350070382267,0.38803849855630418,1.0546493955576852,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,0.10862140028152906,0.1403965177016831,1.3034568033783487,3.3695164248403944,2.1451007793707184,558.23815384615386,88.84636160710933,770.00180059494755,131488.21113499062,25726.500870503161,-36851.440000000002,0.44053468906103488,63437.414087191595,11226.109470765015,-48148.1872,0.78719868106108282,50628.5377756003,5016.9033697997993,-50274.519937976293,0.94818240470446824,null,308]
["IC/ICD","IC22-150A2",1723,9.6,3117,22,"NA",3.1,38.700000000000003,108.89444430272832,18.100000000000001,330,32,2.0698943958369846,1.1067510143411547,1.6923302921465369,null,0.27624309392265189,0.27155350070382267,0.38803849855630418,0.51227138766207669,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,0.21724280056305811,0.2807930354033662,2.6069136067566974,6.7390328496807888,4.2902015587414368,558.23815384615386,88.84636160710933,770.00180059494755,32817.857957088709,6431.6252176257904,-47316.73,1.1067510143411547,15849.034110176231,2806.5273676912539,-50140.916800000006,1.6923302921465369,12655.073491969002,1254.2258424499498,-50672.499984494076,1.9520902866815133,null,154]
["IC/ICD","IC22-150A6",1723,16.600000000000001,3117,38.1,"NA",1,12.9,62.932503525602726,18.100000000000001,330,32,3.5816150220100633,2.0385162342916439,3.0093830751060038,null,0.27624309392265189,0.27155350070382267,0.38803849855630418,0.29251371252769848,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,0.37564900930695472,0.48553795705165409,4.5077881116834568,11.652910969239699,7.4184735286570689,558.23815384615386,88.84636160710933,770.00180059494755,10945.242747724871,2076.4936922008696,-49716.452500000007,2.0385162342916439,5286.4179198015072,904.71903649696674,-50598.490000000005,3.0093830751060038,4225.3070643409746,404.3153146460769,-50763.884687878461,3.4186431513199875,null,89]
["IC/ICD","IC22-200A1",2393,5,4156,11,"NA",15.9,205,290.62088706767099,23.7,330,32,0.77558086851312813,0.26464479260731277,0.55219119513473069,null,0.2109704641350211,0.24292258924666826,0.36158132820019251,1.418198805695958,901.63919999999996,0,-1502.732,0,0,0,0,0,0.10121774551944511,0.13082706505084271,1.2146129462333413,3.1398495612202253,1.9988903129324704,693.56861538461533,110.38487351186312,956.66890376948027,231493.26890522285,44019.718930312913,-27862.652500000004,0.26464479260731277,114839.17126140966,20008.963150142237,-46064.972500000003,0.55219119513473069,89315.695167183498,7999.144522528416,-50047.571386478936,0.70511975893906231,null,411]
["IC/ICD","IC22-200A2",2393,10,4156,22,"NA",4,51.3,145.66399692442877,23.7,330,32,1.5473967813538625,0.78999586591288318,1.2271735325497808,null,0.2109704641350211,0.24292258924666826,0.36158132820019251,0.68599343828576498,901.63919999999996,0,-1502.732,0,0,0,0,0,0.20243549103889022,0.26165413010168542,2.4292258924666825,6.2796991224404506,3.9977806258649409,693.56861538461533,110.38487351186312,956.66890376948027,58047.950515187244,11101.087514293362,-44997.16,0.78999586591288318,28827.493908096534,5045.9488701333457,-49605.16,1.2271735325497808,22434.168334993472,2017.2596632124178,-50613.373000809508,1.4577398910679216,null,206]
["IC/ICD","IC22-200A6",2393,17.3,4156,38.1,"NA",1.3,17.100000000000001,84.145706961199153,23.7,330,32,2.6786868652008038,1.5000815062133768,2.2068877908123303,null,0.2109704641350211,0.24292258924666826,0.36158132820019251,0.39057023269185071,901.63919999999996,0,-1502.732,0,0,0,0,0,0.35021339949728009,0.45266164507591583,4.2025607939673613,10.86387948182198,6.9161604827463474,693.56861538461533,110.38487351186312,956.66890376948027,19353.85272436891,3609.3660020615112,-48965.244325000007,1.5000815062133768,9610.9949241713475,1638.8984733770117,-50425.809925000001,2.2068877908123303,7484.9300233113308,655.19565646262447,-50744.531322894225,2.5603589733602989,null,119]
["IC/ICD","IC22-250A1",3000,5,6250,11,"NA",19.3,256,349.31074990615446,29.3,330,32,0.64527072258885765,0.14681748916319354,0.42970048004411088,null,0.17064846416382251,0.23158027680728926,0.28735168,1.7245765928991212,1077.5688,0,-1795.9479999999999,0,0,0,0,0,9.6491782003037194E-2,0.1247186111111111,1.1579013840364463,2.9932466666666664,1.9055600115733551,828.8990769230769,131.92338541661687,1143.336006944013,351308.64944610791,64223.294040519293,-17001.692500000005,0.14681748916319354,169392.10112522892,29192.406382054221,-43820.972500000003,0.42970048004411088,128898.91566656852,11125.576448648266,-49790.732199882666,0.57985247168346254,null,494]
["IC/ICD","IC22-250A2",3000,9.9,6250,22,"NA",4.8,63.9,174.65537495307723,29.3,330,32,1.2905414451777153,0.61068679159111317,0.9983320805610858,null,0.17064846416382251,0.23158027680728926,0.28735168,0.82541299657058242,1077.5688,0,-1795.9479999999999,0,0,0,0,0,0.19105372836601364,0.24694284999999996,2.2926447403921637,5.9266283999999994,3.7730088229152434,828.8990769230769,131.92338541661687,1143.336006944013,87648.168989553349,15972.632714740545,-42441.64,0.61068679159111317,42076.092970384547,7187.6847216332462,-49111.547200000001,0.9983320805610858,32185.231738774251,2739.3129162682153,-50559.168908415682,1.2115147255432006,null,247]
["IC/ICD","IC22-250A6",3000,17.2,6250,38.1,"NA",1.6,21.3,101.11626970967629,29.3,330,32,2.229117041670599,1.1929328468861806,1.8037129533222052,null,0.17064846416382251,0.23158027680728926,0.28735168,0.47032550377060378,1077.5688,0,-1795.9479999999999,0,0,0,0,0,0.33193173009044791,0.42903202222222214,3.9831807610853751,10.296768533333331,6.5551264398123408,828.8990769230769,131.92338541661687,1143.336006944013,29267.273494473273,5338.2219862422362,-48018.068800000001,1.1929328468861806,14105.441926967276,2409.9059885398015,-50237.147200000007,1.8037129533222052,10788.192681697983,918.44409668252024,-50722.658209327506,2.1261870597766674,null,143]
["IC/ICD","IC33-015A1",216,3.8,565,11.1,"NA",4.3,27.4,32.739043968937146,5,330,32,6.8847459386370558,3.4439290379346361,5.879076302407805,null,1,0.93772382898967155,0.9267256637168142,0.20322833588409295,314.16000000000003,0,-523.6,0,0,0,0,0,0.29694587918006266,0.42641833810888247,3.5633505501607519,10.23404011461318,6.2542665430520312,241.66153846153847,38.461628401346033,333.33411281166559,3746.5021909236548,1353.2812332717003,-49096.545325000006,3.4439290379346361,1385.3102206552842,463.28546724616763,-50604.9133,5.879076302407805,1920.9764784430113,762.50284149471963,-50262.720950242321,4.9205736771388473,null,46.3]
["IC/ICD","IC33-015A3",216,11.4,565,33.299999999999997,"NA",0.48,3,10.889444430272832,5,330,32,20.698943958369846,10.965935552219999,18.085792648456135,null,1,0.93772382898967155,0.9267256637168142,6.5202268242777375E-2,314.16000000000003,0,-523.6,0,0,0,0,0,0.89083763754018797,1.2792550143266475,10.690051650482255,30.702120343839539,18.762799629156092,241.66153846153847,38.461628401346033,333.33411281166559,407.15055845385484,150.73767958728828,-50613.543808000002,10.965935552219999,152.39997292487351,51.603890309161763,-50782.702912000001,18.085792648456135,210.19336479551913,84.932759118925617,-50744.327030093162,15.336889757830972,null,15.4]
["IC/ICD","IC33-015A5",216,6.6,565,19.100000000000001,"NA",1.4,9.1,18.879751057680817,5,330,32,11.938716740033545,6.2177283061262383,10.331521900511436,null,1,0.93772382898967155,0.9267256637168142,0.11453135260816116,314.16000000000003,0,-523.6,0,0,0,0,0,0.5157481059443193,0.73404966571155705,6.1889772713318321,17.617191977077368,10.802511203856218,241.66153846153847,38.461628401346033,333.33411281166559,1229.9603932532236,437.20819944449806,-50268.889300000003,6.2177283061262383,460.74677497905861,151.07717886563802,-50741.126800000005,10.331521900511436,635.86229174750963,247.27468444591588,-50633.619454985128,8.7312336511141755,null,26.7]
["IC/ICD","IC33-015A7",216,19.8,565,57.7,"NA",0.16,1,6.293250352560273,5,330,32,35.816150220100631,19.140627018779917,31.409297920568864,null,1,0.93772382898967155,0.9267256637168142,3.7466474573848503E-2,314.16000000000003,0,-523.6,0,0,0,0,0,1.5472443178329582,2.2168385864374405,18.566931813995499,53.204126074498575,32.542013970092057,241.66153846153847,38.461628401346033,333.33411281166559,135.87094307569177,50.315458704457818,-50741.237632000004,19.140627018779917,50.940780398641806,17.265963298930068,-50797.632832000003,31.409297920568864,70.225332184721367,28.377233276812071,-50784.827532673997,26.690528302281134,null,8.9]
["IC/ICD","IC33-030A1",431,4,944,11.1,"NA",5.8,50.1,65.478087937874292,7.3,330,32,{"$f":"IF(G207=\"NA\",(UAC_V*0.98)/J207,(IF((UAC_V*0.98)/J207<G207,(UAC_V*0.98)/J207,G207)))","v":3.4423729693185279},{"$f":"IF(AO207<G207,IF(AO207<0,0,AO207),G207)","v":1.7657956458124699},{"$f":"IF(AS207<G207,IF(AS207<0,0,AS207),G207)","v":2.9231075296169147},null,{"$f":"IF(move1,Gewicht/K207,MAX(Gewicht,Gewicht2)/K207)","v":0.68493150684931503},{"$f":"IF(move1,IF(AccType=1,SQRT((V207^2*Ltime1+W207^2*Ltime2+X207^2*Ltime3+Y207^2*Ltime4)/ltime)/C207,SQRT((((V207-W207)*2/PI()+W207)^2*Ltime1+W207^2*Ltime2+((X207-W207)*2/PI()+W207)^2*Ltime3+Y207^2*Ltime4)/ltime)/C207),IF(AccType=1,SQRT((V207^2*Ltime1+W207^2*Ltime2+X207^2*Ltime3+Y207^2*Ltime4+Z207^2*Ltime5+AA207^2*Ltime6+AB207^2*Ltime7+AC207^2*Ltime8)/ltime)/C207,SQRT((((V207-W207)*2/PI()+W207)^2*Ltime1+W207^2*Ltime2+((X207-W207)*2/PI()+W207)^2*Ltime3+Y207^2*Ltime4+((Z207-AA207)*2/PI()+AA207)^2*Ltime5+AA207^2*Ltime6+((AB207-AA207)*2/PI()+AA207)^2*Ltime7+AC207^2*Ltime8)/ltime)/C207))","v":0.57803820623196278},{"$f":" IF(move1,MAX(ABS(V207),ABS(X207))/E207,MAX(ABS(V207),ABS(X207),ABS(Z207),ABS(AB207))/E207)","v":0.68223305084745767},{"$f":"IF(AW207>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW207,G207),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW207,G207)),\"NA\")","v":0.33796211142014154},{"$f":"((Gewicht+K207)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":386.41680000000002},0,{"$f":"((Gewicht+K207)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-644.02800000000002},0,{"$f":"((Gewicht2+K207)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K207)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF207/Irms","v":0.19267940207732093},{"$f":"AG207/Ipeak","v":0.28951419753086421},{"$f":"D207*S207","v":2.3121528249278511},{"$f":"IF(move1,IF(MAX(ABS(V207),ABS(X207))<=C207,MAX(ABS(V207),ABS(X207))/C207*D207,D207+(MAX(ABS(V207),ABS(X207))-C207)/(E207-C207)*(F207-D207)),IF(MAX(ABS(V207),ABS(X207),ABS(Z207),ABS(AB207))<=C207,MAX(ABS(V207),ABS(X207),ABS(Z207),ABS(AB207))/C207*D207,D207+(MAX(ABS(V207),ABS(X207),ABS(Z207),ABS(AB207))-C207)/(E207-C207)*(F207-D207)))","v":6.9483407407407407},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V207),ABS(X207))<=C207,MAX(ABS(V207),ABS(X207))/C207*D207,D207+(MAX(ABS(V207),ABS(X207))-C207)/(E207-C207)*(F207-D207)),IF(MAX(ABS(V207),ABS(X207),ABS(Z207),ABS(AB207))<=C207,MAX(ABS(V207),ABS(X207),ABS(Z207),ABS(AB207))/C207*D207,D207+(MAX(ABS(V207),ABS(X207),ABS(Z207),ABS(AB207))-C207)/(E207-C207)*(F207-D207))),IF(move1,IF(MAX(ABS((V207-W207)*2/PI()+W207),ABS((X207-W207)*2/PI()+W207))<=C207,MAX(ABS((V207-W207)*2/PI()+W207),ABS((X207-W207)*2/PI()+W207))/C207*D207,D207+(MAX(ABS((V207-W207)*2/PI()+W207),ABS((X207-W207)*2/PI()+W207))-C207)/(E207-C207)*(F207-D207)),IF(MAX(ABS((V207-W207)*2/PI()+W207),ABS((X207-W207)*2/PI()+W207),ABS((Z207-AA207)*2/PI()+AA207),ABS((AB207-AA207)*2/PI()+AA207))<=C207,MAX(ABS((V207-W207)*2/PI()+W207),ABS((X207-W207)*2/PI()+W207),ABS((Z207-AA207)*2/PI()+AA207),ABS((AB207-AA207)*2/PI()+AA207))/C207*D207,D207+(MAX(ABS((V207-W207)*2/PI()+W207),ABS((X207-W207)*2/PI()+W207),ABS((Z207-AA207)*2/PI()+AA207),ABS((AB207-AA207)*2/PI()+AA207))-C207)/(E207-C207)*(F207-D207))))","v":3.8051133063419833},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V207)+Ltime2*ABS(Lspeed2)*ABS(W207)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X207)+Ltime4*ABS(Lspeed1)*ABS(Y207))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V207)+Ltime2*ABS(Lspeed2)*ABS(W207)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X207)+Ltime4*ABS(Lspeed1)*ABS(Y207)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z207)+Ltime6*ABS(Lspeed6)*ABS(AA207)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB207)+Ltime8*ABS(Lspeed1)*ABS(AC207))/ltime)","v":297.2436923076923},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK207/2*Ltime1/ltime,AK207/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X207*-ABS(Lspeed2-Lspeed1),((X207-Y207)*2/PI()+Y207)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V207*-ABS(Lspeed2-Lspeed1),((V207-W207)*2/PI()+W207)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X207*-ABS(Lspeed2-Lspeed1),((X207-Y207)*2/PI()+Y207)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V207*-ABS(Lspeed2-Lspeed1),((V207-W207)*2/PI()+W207)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB207*-ABS(Lspeed6-Lspeed1),((AB207-AC207)*2/PI()+AB207)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z207*-ABS(Lspeed6-Lspeed1),((Z207-AA207)*2/PI()+AA207)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB207*-ABS(Lspeed6-Lspeed1),((AB207-AC207)*2/PI()+AB207)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z207*-ABS(Lspeed6-Lspeed1),((Z207-AA207)*2/PI()+AA207)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":47.307802933655616},{"$f":"IF(move1,MAX(IF(AccType=1,X207*-ABS(Lspeed2-Lspeed1),((X207-Y207)*2/PI()+Y207)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V207*-ABS(Lspeed2-Lspeed1),((V207-W207)*2/PI()+W207)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X207*-ABS(Lspeed2-Lspeed1),((X207-Y207)*2/PI()+Y207)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V207*-ABS(Lspeed2-Lspeed1),((V207-W207)*2/PI()+W207)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB207*-ABS(Lspeed6-Lspeed1),((AB207-AC207)*2/PI()+AB207)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z207*-ABS(Lspeed6-Lspeed1),((Z207-AA207)*2/PI()+AA207)*-ABS(Lspeed6-Lspeed1)),0))","v":410.0009587583487},{"$f":"(J207^2)+3*(I207/1000)^2*(F207/2)^2*(2000*PI()/M207)^2","v":13229.540338577286},{"$f":"SQRT(3)*H207*F207/2*J207","v":3650.7121641748195},{"$f":"3*F207^2*H207^2/4-(UAC_V*0.98)^2","v":-47696.5717},{"$f":"-AM207/2/AL207+SQRT((AM207/2/AL207)^2-AN207/AL207)","v":1.7657956458124699},{"$f":"(J207^2)+3*(I207/1000)^2*(D207/2)^2*(2000*PI()/M207)^2","v":5448.6052691927316},{"$f":"SQRT(3)*H207*D207/2*J207","v":1315.5719510539889},{"$f":"3*D207^2*H207^2/4-(UAC_V*0.98)^2","v":-50401.48},{"$f":"-AQ207/2/AP207+SQRT((AQ207/2/AP207)^2-AR207/AP207)","v":2.9231075296169147},{"$f":"(J207^2)+3*(I207/1000)^2*(AH207/2)^2*(2000*PI()/M207)^2","v":5338.208110779934},{"$f":"SQRT(3)*H207*AH207/2*J207","v":1251.4750841014545},{"$f":"3*AH207^2*H207^2/4-(UAC_V*0.98)^2","v":-50439.857674074439},{"$f":"IF((AU207/2/AT207)^2-AV207/AT207>=0,-AU207/2/AT207+SQRT((AU207/2/AT207)^2-AV207/AT207),-9999)","v":2.9589115649619027},null,92.6]
["IC/ICD","IC33-030A3",431,11.9,944,33.1,"NA",0.64,5.6,21.849599538664314,7.3,330,32,10.315978542359083,5.7229697182851691,9.0355744120386419,null,0.68493150684931503,0.57803820623196278,0.68223305084745767,0.10949288982849487,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.57322122118002972,0.8626456790123459,6.878654654160357,20.703496296296301,11.3202120863674,297.2436923076923,47.307802933655616,410.0009587583487,1470.8711749049962,400.85017824339297,-50468.588608000005,5.7229697182851691,605.81268615501529,144.11229973100836,-50761.657408000006,9.0355744120386419,593.60502581041135,137.09090732850103,-50765.793179643806,9.1330131259331875,null,30.9]
["IC/ICD","IC33-030A5",431,6.9,944,19.100000000000001,"NA",1.9,16.7,37.830212793480293,7.3,330,32,5.9582006908204788,3.2420161620696621,5.1669397499792593,null,0.68493150684931503,0.57803820623196278,0.68223305084745767,0.19139141064174883,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.33237196858337864,0.49859012345679021,3.9884636230005435,11.966162962962965,6.5638204534399218,297.2436923076923,47.307802933655616,410.0009587583487,4372.9763225986171,1188.9302694899206,-49817.436925000002,3.2420161620696621,1815.0551046268474,429.50884081049486,-50676.255925000005,5.1669397499792593,1778.5550441266159,408.58245133988368,-50688.510776806426,5.2248948719638451,null,53.5]
["IC/ICD","IC33-030A7",431,20.6,944,57.3,"NA",0.21,1.9,12.586500705120546,7.3,330,32,17.908075110050316,9.9279583814474197,15.712997429125767,null,0.68493150684931503,0.57803820623196278,0.68223305084745767,6.2958341792432565E-2,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.99229892069820291,1.493333950617284,11.907587048378435,35.840014814814815,19.596333527661216,297.2436923076923,47.307802933655616,410.0009587583487,501.13845340897501,131.1624598333494,-50696.565183250001,9.9279583814474197,202.71581392098557,47.154392191396127,-50791.124293000001,15.712997429125767,198.50463102978097,44.856951294987482,-50792.458661283425,15.883518713007104,null,17.8]
["IC/ICD","IC33-050A1",789,4.4000000000000004,1572,11.1,"NA",7.9,80.2,108.89444430272832,10.4,330,32,2.0698943958369846,1.0253578891178414,1.6937373105168829,null,0.48076923076923073,0.39534151391017025,0.51294147582697203,0.5367576999188024,483.8064,0,-806.34400000000005,0,0,0,0,0,0.14495855510039576,0.18951707109408264,1.7395026612047493,4.5484097062579831,2.8627020892418842,372.15876923076922,59.230907738072894,513.33453372996507,34772.782404907819,8269.6365884692896,-45038.007925000005,1.0253578891178414,15458.602121248401,3278.0541431770162,-49898.966800000002,1.6937373105168829,13382.130275207403,2132.7482828001948,-50421.569576843722,1.863038015386224,null,154]
["IC/ICD","IC33-050A3",789,13.1,1572,33.1,"NA",0.88,8.9,36.345288552988542,10.4,330,32,6.2016291237139232,3.5013944726901038,5.3341774137159543,null,0.48076923076923073,0.39534151391017025,0.51294147582697203,0.17351357787238905,483.8064,0,-806.34400000000005,0,0,0,0,0,0.43158115268526914,0.56429225202213706,5.1789738322232299,13.54301404853129,8.5230448566065178,372.15876923076922,59.230907738072894,513.33453372996507,3830.305756193392,916.83127337708117,-50168.829712000006,3.5013944726901038,1714.0262418381978,362.85467314923756,-50705.488912000001,5.3341774137159543,1487.3559717317457,236.07837066261436,-50762.969355861023,5.7632377377144062,null,51.4]
["IC/ICD","IC33-050A5",789,7.6,1572,19.100000000000001,"NA",2.6,26.7,62.932503525602726,10.4,330,32,3.5816150220100633,1.9504999596347226,3.0286781810594361,null,0.48076923076923073,0.39534151391017025,0.51294147582697203,0.30379192308914532,483.8064,0,-806.34400000000005,0,0,0,0,0,0.25038295880977451,0.32728054491272884,3.0045955057172939,7.8547330779054922,4.9446672450541627,372.15876923076922,59.230907738072894,513.33453372996507,11480.369444466736,2706.5269489421303,-48955.573300000004,1.9504999596347226,5151.113357946324,1076.9426603120519,-50512.316800000001,3.0286781810594361,4464.4851124353509,700.67409174295983,-50681.199847786942,3.2917267510978494,null,89]
["IC/ICD","IC33-050A7",789,22.7,1572,57.3,"NA",0.28999999999999998,3,21.001071401240459,10.4,330,32,10.732785756191774,6.1340636315693082,9.2921627344819342,null,0.48076923076923073,0.39534151391017025,0.51294147582697203,9.9769905606494902E-2,483.8064,0,-806.34400000000005,0,0,0,0,0,0.74785436381340542,0.97776726266496394,8.974252365760865,23.466414303959134,14.768940324043356,372.15876923076922,59.230907738072894,513.33453372996507,1295.4677370306856,302.22104508952333,-50598.066483250004,6.1340636315693082,575.1408283199296,119.72805800230681,-50772.658083250004,9.2921627344819342,497.80759271062038,77.896764041835738,-50791.40198018754,10.023062504881244,null,29.7]
["IC/ICD","IC33-075A1",1238,4.5999999999999996,2358,11.1,"NA",10.6,118,163.34166645409246,14.4,330,32,1.3799295972246566,0.62696619228590178,1.086202728825765,null,0.34722222222222221,0.31740209474946035,0.43078201865988119,0.79587164758401507,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.12167080298729312,0.1572632740980075,1.4600496358475175,3.77431857835218,2.4028058341932979,468.82338461538455,74.6155590986113,646.66817885463115,76286.135258166352,16643.952121096419,-40422.253300000004,0.62696619228590178,35199.737416303869,6897.4936718057224,-49022.006800000003,1.086202728825765,29004.961801136407,3602.8995730274223,-50318.62918785926,1.2564840110030888,null,231]
["IC/ICD","IC33-075A3",1238,13.8,2358,33.1,"NA",1.2,13.1,54.51793282948281,14.4,330,32,4.1344194158092824,2.3202956598253874,3.4956527276120997,null,0.34722222222222221,0.31740209474946035,0.43078201865988119,0.25634008100531053,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.36501240896187942,0.47178982229402261,4.3801489075425533,11.322955735056542,7.2084175025798949,468.82338461538455,74.6155590986113,646.66817885463115,8408.7078786813254,1875.3366955440295,-49621.9012,2.3202956598253874,3917.1832388040189,781.86242895793362,-50599.484800000006,3.4956527276120997,3230.0409671960047,408.40513170362306,-50749.041814477183,3.9010676601108014,null,77.099999999999994]
["IC/ICD","IC33-075A5",1238,8,2358,19.100000000000001,"NA",3.5,39.4,94.752308678997366,14.4,330,32,2.3788338579022064,1.2641923627495508,1.9638544922511816,null,0.34722222222222221,0.31740209474946035,0.43078201865988119,0.45104276864170523,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.21160139649964024,0.27350134625740435,2.5392167579956828,6.5640323101777049,4.1787927551187796,468.82338461538455,74.6155590986113,646.66817885463115,25352.959013048832,5485.5710417193577,-47453.468124999999,1.2641923627495508,11850.721079014076,2297.621378730621,-50217.16,1.9638544922511816,9761.8178568316853,1200.1604464306927,-50644.725037070988,2.2170846525518066,null,134]
["IC/ICD","IC33-075A7",1238,23.9,2358,57.3,"NA",0.39,4.4000000000000004,31.466251762801363,14.4,330,32,7.1632300440201266,4.1165130029585466,6.1276455831520495,null,0.34722222222222221,0.31740209474946035,0.43078201865988119,0.14696011471307974,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.63215917204267513,0.81708527194399549,7.5859100645121016,19.610046526655893,12.484143355917354,468.82338461538455,74.6155590986113,646.66817885463115,2828.0832432126745,608.96856351197937,-50430.618693250006,4.1165130029585466,1309.8835739016388,254.00259455386225,-50739.999219250007,6.1276455831520495,1077.3706716839199,132.67802523788157,-50787.380973734609,6.8045673613712685,null,44.5]
["IC/ICD","IC33-100A1",1722,4.8,3144,11.1,"NA",13.2,156,217.78888860545663,18.899999999999999,330,32,1.0349471979184923,0.41596817905811934,0.77776427302347395,null,0.26455026455026459,0.28112110887202557,0.39802926208651401,1.0639794688636701,750.8424,0,-1251.404,0,0,0,0,0,0.11244844354881023,0.1453430894308943,1.3493813225857227,3.4882341463414632,2.2206788282087269,577.57107692307693,91.923291879217018,796.66852961988081,134131.4211176915,27635.241257669521,-34704.077200000007,0.41596817905811934,63644.601757581462,11950.374597911145,-47794.292800000003,0.77776427302347395,50902.098034288923,5528.7383039051365,-50160.722758621443,0.93986775991833726,null,308]
["IC/ICD","IC33-100A3",1722,14.3,3144,33.1,"NA",1.5,17.3,72.831998462214386,18.899999999999999,330,32,3.094793562707725,1.7168023798420238,2.5768590793817094,null,0.26455026455026459,0.28112110887202557,0.39802926208651401,0.34093005866924558,750.8424,0,-1251.404,0,0,0,0,0,0.3350026547391638,0.43300128726287263,4.0200318568699656,10.392030894308943,6.6157723423718329,577.57107692307693,91.923291879217018,796.66852961988081,14785.829447937384,3131.6420175265084,-48956.318125000005,1.7168023798420238,7074.1416232132915,1352.9450408045036,-50460.083125000005,2.5768590793817094,5683.2689360368495,625.92841830094858,-50731.300751279727,2.9331529285018347,null,103]
["IC/ICD","IC33-100A5",1722,8.1999999999999993,3144,19.100000000000001,"NA",4.4000000000000004,52,125.86500705120545,18.899999999999999,330,32,1.7908075110050317,0.91480923629720712,1.4463898380044713,null,0.26455026455026459,0.28112110887202557,0.39802926208651401,0.59735025798015517,750.8424,{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},-1251.404,{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},0,{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0,0,0.19209942439588412,0.2482944444444444,2.3051930927506095,5.9590666666666658,3.793659664856575,577.57107692307693,91.923291879217018,796.66852961988081,44364.951616431783,9160.5527502656751,-45508.118800000004,0.91480923629720712,21099.211333814514,3932.8027514229589,-49828.835200000001,1.4463898380044713,16967.238193603331,1819.4774595012489,-50596.190284961929,1.6740597105981687,null,178]
["IC/ICD","IC33-100A7",1722,24.7,3144,57.3,"NA",0.49,5.8,41.93143212436226,18.899999999999999,330,32,5.3754424445007709,3.0831083595835063,4.5504560265909522,null,0.26455026455026459,0.28112110887202557,0.39802926208651401,0.1946905571360826,750.8424,0,-1251.404,0,0,0,0,0,0.57864094909491925,0.74791131436314362,6.9436913891390315,17.949871544715446,11.427243136824075,577.57107692307693,91.923291879217018,796.66852961988081,4951.8873193013615,1019.5793460079275,-50213.921553250002,3.0831083595835063,2351.6769668937454,439.50453484111358,-50695.298043250004,4.5504560265909522,1885.2614488459858,203.33300321320539,-50781.645466931121,5.1363559420143385,null,59.3]
["IC/ICD","IC33-150A1",2583,4.8,4716,11.1,"NA",18.5,232,327.39043968937148,27.3,330,32,0.68847459386370558,0.17398350905924945,0.47907059174478872,null,0.18315018315018314,0.25328345373964922,0.35861492790500421,1.618537324252715,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,0.10131338149585968,0.13095067750677505,1.2157605779503162,3.1428162601626011,2.0007789721378484,780.56676923076918,124.23105973634766,1076.6691843816798,298937.85479284299,58222.564687270824,-19178.693125000005,0.17398350905924945,143041.95714168577,25177.325270171172,-44891.08,0.47907059174478872,113414.60321897359,10494.638119840281,-49777.610034600111,0.61784179148398932,null,463]
["IC/ICD","IC33-150A3",2583,14.4,4716,33.1,"NA",2.1,25.8,108.89444430272832,27.3,330,32,2.0698943958369846,1.1013556257111119,1.6905911428577789,null,0.18315018315018314,0.25328345373964922,0.35861492790500421,0.50948979201595834,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,0.30394014448757906,0.39285203252032513,3.6472817338509489,9.4284487804878037,6.0023369164135456,780.56676923076918,124.23105973634766,1076.6691843816798,32945.079868104651,6555.1652328030596,-47181.429925000004,1.1013556257111119,15849.034110176231,2851.7939381378869,-50119.316800000001,1.6905911428577789,12551.427711803251,1188.7102800617645,-50685.9972297247,1.962747862019339,null,154]
["IC/ICD","IC33-150A5",2583,8.3000000000000007,4716,19.100000000000001,"NA",6.2,77.3,188.79751057680818,27.3,330,32,1.1938716740033546,0.54835239464078167,0.92866504619369283,null,0.18315018315018314,0.25328345373964922,0.35861492790500421,0.89995735766535523,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,0.17518772216992406,0.22643554652213185,2.1022526660390888,5.4344531165311647,3.4596803059883632,780.56676923076918,124.23105973634766,1076.6691843816798,98674.421436445497,19362.07740397063,-40287.687699999995,0.54835239464078167,47546.945897197802,8413.887039421792,-48819.061300000001,0.92866504619369283,37712.506836201006,3507.1517213371453,-50460.082549159677,1.1111637584631484,null,267]
["IC/ICD","IC33-150A7",2583,24.9,4716,57.3,"NA",0.69,8.6,62.932503525602726,27.3,330,32,3.5816150220100633,2.0300634963149222,3.006022506609884,null,0.18315018315018314,0.25328345373964922,0.35861492790500421,0.29118788675658985,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,0.52556316650977208,0.67930663956639548,6.3067579981172655,16.303359349593492,10.379040917965089,780.56676923076918,124.23105973634766,1076.6691843816798,10981.956181198835,2154.8118401193115,-49632.779223250007,2.0300634963149222,5286.4179198015063,936.38420277436035,-50583.769929250004,3.006022506609884,4190.8734329963636,390.31204640687571,-50766.694277598712,3.4342087891723367,null,89]
["IC/ICD","IC33-200A1",3590,5,6291,11.1,"NA",23.9,308,436.28488399209976,35.700000000000003,330,32,0.51663490593013883,0,0.31586874377867152,null,0.14005602240896359,0.2296300202065181,0.33874614528691782,2.195898543139613,1278.6312,0,-2131.0520000000001,0,0,0,0,0,9.5679175086049215E-2,0.12366829155060355,1.1481501010325905,2.9680389972144852,1.8895123107847898,983.56246153846166,156.53882759347835,1356.6698391434791,528306.93774279603,100235.52689835991,1978.9280749999889,-2.2383487818676315E-2,258918.97401647508,45151.138242504458,-40094.972500000003,0.31586874377867152,200137.63921141202,17062.72631103162,-49275.635221689256,0.45539444576079441,null,617]
["IC/ICD","IC33-200A3",3590,14.9,6291,33.1,"NA",2.7,34.200000000000003,145.66399692442877,35.700000000000003,330,32,1.5473967813538625,0.78555000823250098,1.2285335116757352,null,0.14005602240896359,0.2296300202065181,0.33874614528691782,0.68271702158152958,1278.6312,0,-2131.0520000000001,0,0,0,0,0,0.28512394175642664,0.36853150882079855,3.4214873010771196,8.8447562116991651,5.6307466861386732,983.56246153846166,156.53882759347835,1356.6698391434791,58271.500536220658,11273.91126309543,-44814.912325000005,0.78555000823250098,28726.372189051162,5074.9630761366134,-49591.320325000001,1.2285335116757352,22290.272666368637,1917.8410418276753,-50631.811227178878,1.4647357080441281,null,206]
["IC/ICD","IC33-200A5",3590,8.6,6291,19.100000000000001,"NA",8,103,251.73001410241091,35.700000000000003,330,32,0.89540375550251583,0.351050333875218,0.65898853218119979,null,0.14005602240896359,0.2296300202065181,0.33874614528691782,1.2084897037585018,1278.6312,0,-2131.0520000000001,0,0,0,0,0,0.16456818114800462,0.21270946146703806,1.9748181737760555,5.1050270752089135,3.249961174549838,983.56246153846166,156.53882759347835,1356.6698391434791,175276.28169331537,33311.100910056994,-33294.28,0.351050333875218,86055.800537369039,14998.715593009954,-47255.08,0.65898853218119979,66608.050940964182,5668.0515517904187,-50298.172113468099,0.82747912281744573,null,356]
["IC/ICD","IC33-200A7",3765,25.9,6291,57.3,"NA",0.89,11.4,84.145706961199153,35.700000000000003,330,32,2.6786868652008038,1.4933526907927976,2.2054815887922548,null,0.14005602240896359,0.21895664609333332,0.33874614528691782,0.38805237457253283,1278.6312,0,-2131.0520000000001,0,0,0,0,0,0.47258142781811108,0.61082610447100494,5.6709771338173329,14.659826507304118,9.332735414028182,983.56246153846166,156.53882759347835,1356.6698391434791,19418.3643227231,3716.2696952782326,-48854.639493250004,1.4933526907927976,9601.2528930815988,1679.7798448116271,-50406.648549250007,2.2054815887922548,7407.8019956870039,605.28729132989338,-50753.416097020629,2.5769717324924781,null,119]
["IC/ICD","IC33-250A1",4496,5,9375,11.1,"NA",29,384,523.96612485923163,44.1,330,32,0.43018048172590512,{"$error":"#NUM!"},0.22892547327069318,null,0.11337868480725623,0.22119937368178072,0.27422677333333334,2.6924564871848737,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,9.2166405700741971E-2,0.11912792852906288,1.1059968684089037,2.8590702846975091,1.8201406738270443,1186.5581538461538,188.84659545060902,1636.6704939052781,799867.16996755078,146067.91110440285,26909.547500000001,{"$error":"#NUM!"},381132.22753176495,65796.356353334617,-35036.410000000003,0.22892547327069318,288665.6608388279,23951.724877664565,-48715.540710258283,0.37140804494321117,null,741]
["IC/ICD","IC33-250A3",4496,14.9,9375,33.1,"NA",3.2,42.6,174.65537495307723,44.1,330,32,1.2905414451777153,0.60898688670337964,0.99709062382815283,null,0.11337868480725623,0.22119937368178072,0.27422677333333334,0.82238145796507178,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,0.27465588898821108,0.35500122701660741,3.2958706678585328,8.5200294483985779,5.4240192080045917,1186.5581538461538,188.84659545060902,1636.6704939052781,87995.018991409146,16021.034632057943,-42390.875200000002,0.60898688670337964,42154.147339183415,7211.8856802919436,-49100.123200000002,0.99709062382815283,32048.270292423043,2625.3292923380377,-50579.214520047601,1.2159807231967918,null,247]
["IC/ICD","IC33-250A5",4496,8.6,9375,19.100000000000001,"NA",9.6999999999999993,128,302.64170234784234,44.1,330,32,0.74477508635255985,0.22944314905247687,0.51984360703272114,null,0.11337868480725623,0.22119937368178072,0.27422677333333334,1.467448092196961,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,{"$f":"(Ltorque2+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0.15852621780527618,0.20490003706998816,1.902314613663314,4.9176008896797159,3.1306419589825158,1186.5581538461538,188.84659545060902,1636.6704939052781,264417.45831494767,48558.415217062015,-25061.430325000001,0.22944314905247687,126629.88519221931,21863.998474698077,-45585.987700000005,0.51984360703272114,96235.09731395432,7959.1105832580843,-50113.533643150819,0.68145510925900599,null,428]
["IC/ICD","IC33-250A7",4496,25.7,9375,57.3,"NA",1.1000000000000001,14.2,101.11626970967629,44.1,330,32,2.229117041670599,1.1856200254362532,1.8027332634282673,null,0.11337868480725623,0.22119937368178072,0.27422677333333334,0.46899532297225133,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,0.47373532530181373,0.61231755263938326,5.6848239036217647,14.695621263345197,9.3555230634710078,1186.5581538461538,188.84659545060902,1636.6704939052781,29367.366743874154,5519.4903509325477,-47825.574325000001,1.1856200254362532,14075.415409744932,2475.5829322681757,-50205.765325,1.8027332634282673,10734.809766047823,901.18183729066561,-50725.730325799545,2.1322174252453392,null,143]
["IC/ICD","IC44-015A1",286,3.8,750,11.1,"NA",5.8,36.5,43.628488399209978,6.4,330,32,5.1663490593013881,2.5015297377348387,4.3623400814157378,null,0.78125,0.80736054423222625,0.79587200000000002,0.25557429810771742,358.14240000000001,0,-596.904,0,0,0,0,0,0.25566417234020494,0.36214073275862074,3.0679700680824595,8.6913775862068974,5.2788932905575017,275.49415384615384,43.846256377534473,380.00088860529877,6649.7181666684946,2432.4939582028765,-47696.5717,2.5015297377348387,2459.7000485081817,832.74567938476855,-50440.838800000005,4.3623400814157378,2976.9214927540506,1156.8356788539481,-50102.082796366863,3.9127565150488173,null,61.7]
["IC/ICD","IC44-015A2",286,7.6,750,22.1,"NA",1.5,9.1,21.849599538664314,6.4,330,32,10.315978542359083,5.3218402870913115,8.9015762624642996,null,0.78125,0.80736054423222625,0.79587200000000002,0.12416885972252657,358.14240000000001,0,-596.904,0,0,0,0,0,0.51132834468040989,0.72148958333333335,6.1359401361649191,17.315750000000001,10.537527768915586,275.49415384615384,43.846256377534473,380.00088860529877,1646.8730880973844,627.27451891845169,-49980.968125000007,5.3218402870913115,615.70781273623561,215.71431419820053,-50707.69,8.9015762624642996,743.28231988534526,299.09152316001581,-50617.780858126374,8.0535490318155922,null,30.9]
["IC/ICD","IC44-015A3",286,15.1,750,44.1,"NA",0.36,2.2999999999999998,10.889444430272832,6.4,330,32,20.698943958369846,10.851346672417877,18.025161844611656,null,0.78125,0.80736054423222625,0.79587200000000002,6.121718638589578E-2,358.14240000000001,0,-596.904,0,0,0,0,0,1.0159286848255513,1.4388125,12.191144217906617,34.531500000000001,20.975055537831174,275.49415384615384,43.846256377534473,380.00088860529877,416.05734342864724,149.71918175223905,-50616.124468000002,10.851346672417877,153.45631649115637,51.264391030812007,-50782.997428000002,18.025161844611656,185.87502431187636,71.210162184395784,-50762.396572791979,16.335281953278344,null,15.4]
["IC/ICD","IC44-015A7",286,26.2,750,76.400000000000006,"NA",0.12,0.8,6.293250352560273,6.4,330,32,35.816150220100631,18.371559850786806,30.99958416989638,null,0.78125,0.80736054423222625,0.79587200000000002,3.5755545823580731E-2,358.14240000000001,0,-596.904,0,0,0,0,0,1.7627371882403606,2.4931915229885058,21.152846258884328,59.836596551724142,36.369923724107757,275.49415384615384,43.846256377534473,380.00088860529877,147.62091144684229,49.96665136508549,-50742.120832000001,18.371559850786806,52.307921084532083,17.135160546665443,-50797.746448000005,30.99958416989638,64.083556164402012,23.78643061383827,-50790.874069401674,27.967689402199014,null,8.9]
["IC/ICD","IC44-030A1",560,3.9,1259,11.1,"NA",7.8,66.8,86.974134085945337,9.6,330,32,2.5915750972267939,1.2557039185933703,2.1763497628161645,null,0.52083333333333337,0.52807247626818365,0.60719301032565531,0.44443507648731623,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.17162355478715971,0.25024935622317596,2.0594826574459164,6.0059845493562234,3.3892936399100431,352.82584615384616,56.153977465965212,486.66780470503181,23461.673935248509,6521.3622743526512,-45183.087700000004,1.2557039185933703,9526.9707049357166,2291.2894477455261,-50111.127700000005,2.1763497628161645,9046.6506940753807,1991.2442954966427,-50280.993981843094,2.2500474262826082,null,123]
["IC/ICD","IC44-030A2",560,7.9,1259,22.1,"NA",2,16.7,43.628488399209978,9.6,330,32,5.1663490593013881,2.7667298999150929,4.4637073009462016,null,0.52083333333333337,0.52807247626818365,0.60719301032565531,0.21748475461977659,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.34764771354322094,0.50222789699570825,4.171772562518651,12.053469527896997,6.865492244945985,352.82584615384616,56.153977465965212,486.66780470503181,5842.0146786557134,1670.0253642834289,-49339.93,2.7667298999150929,2406.7232572938779,596.97739266240217,-50617.93,4.4637073009462016,2283.5445431346338,518.802994902759,-50663.755048703766,4.5980234419110255,null,61.7]
["IC/ICD","IC44-030A3",560,15.8,1259,44.1,"NA",0.49,4.2,21.849599538664314,9.6,330,32,10.315978542359083,5.7223583745232718,9.0414342176554765,null,0.52083333333333337,0.52807247626818365,0.60719301032565531,0.10754936103768148,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.69529542708644188,1.003237052932761,8.3435451250373021,24.077689270386266,13.73098448989197,352.82584615384616,56.153977465965212,486.66780470503181,1469.3710374444872,408.892159255168,-50454.948339250004,5.7223583745232718,604.7358968935996,146.49651057214638,-50760.206077000003,9.0414342176554765,573.57131562114,127.31274142338206,-50771.208671193774,9.2980561702234148,null,30.9]
["IC/ICD","IC44-030A7",560,27.3,1259,76.400000000000006,"NA",0.16,1.4,12.586500705120546,9.6,330,32,17.908075110050316,10.044145680764252,15.791597758949194,null,0.52083333333333337,0.52807247626818365,0.60719301032565531,6.1620376798287163E-2,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,1.2013648835101178,1.7359018597997142,14.416378602121414,41.661644635193142,23.725055479370301,352.82584615384616,56.153977465965212,486.66780470503181,489.21872880595447,133.244403640228,-50693.090368000005,10.044145680764252,200.65790887581716,47.612201824322305,-50790.850432000007,15.791597758949194,190.32006648208068,41.377367391099725,-50794.352737456022,16.22839800661194,null,17.8]
["IC/ICD","IC44-050A1",1053,4.4000000000000004,2096,11.1,"NA",10.6,107,145.66399692442877,13.9,330,32,1.5473967813538625,0.69654320932667835,1.2318934551562413,null,0.35971223021582732,0.36354831523907261,0.47213931297709921,0.72017377316776554,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.13330104892099329,0.17229572649572653,1.5996125870519196,4.1350974358974364,2.632484788358795,456.74030769230768,72.692477678543995,630.00147321404791,62006.2015276319,14842.658601497238,-40422.253300000004,0.69654320932667835,27627.05431032346,5883.5763825754821,-49173.692800000004,1.2318934551562413,23512.142230615398,3520.0966655175043,-50221.170908917549,1.3885537591870185,null,206]
["IC/ICD","IC44-050A2",1053,8.6999999999999993,2096,22.1,"NA",2.7,26.7,72.831998462214386,13.9,330,32,3.094793562707725,1.6513589863216565,2.6035939736782741,null,0.35971223021582732,0.36354831523907261,0.47213931297709921,0.34906590093797968,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.26357252854832763,0.34067564102564102,3.1628703425799314,8.176215384615384,5.205140376982162,456.74030769230768,72.692477678543995,630.00147321404791,15372.150106554091,3763.6471135107104,-48134.778324999999,1.6513589863216565,6864.7064588462126,1481.6167369929037,-50391.324925000001,2.6035939736782741,5862.9810726213609,886.43943688900288,-50657.026363413694,2.8647885608788672,null,103]
["IC/ICD","IC44-050A3",1053,17.399999999999999,2096,44.1,"NA",0.66,6.7,36.345288552988542,13.9,330,32,6.2016291237139232,3.4948995138472316,5.3347171785442722,null,0.35971223021582732,0.36354831523907261,0.47213931297709921,0.17181862089815711,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.52714505709665527,0.68135128205128204,6.3257406851598628,16.352430769230768,10.410280753964324,456.74030769230768,72.692477678543995,630.00147321404791,3845.319876467292,916.13880262679629,-50169.790573000006,3.4948995138472316,1713.9588210669615,361.4697316486679,-50706.248308000002,5.3347171785442722,1461.6480713713081,216.26444773119405,-50769.754232045547,5.8200909469104332,null,51.4]
["IC/ICD","IC44-050A7",1053,30.2,2096,76.400000000000006,"NA",0.22,2.2000000000000002,21.001071401240459,13.9,330,32,10.732785756191774,6.2215746236038223,9.3431659675874386,null,0.35971223021582732,0.36354831523907261,0.47213931297709921,9.860516392537072E-2,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.9149299266849994,1.1825752136752137,10.979159120219993,28.381805128205126,18.068418320098999,456.74030769230768,72.692477678543995,630.00147321404791,1257.9153303167445,305.69485020549496,-50593.278352000001,6.2215746236038223,568.68308833058359,120.83749314405689,-50772.052948000004,9.3431659675874386,486.73347672308648,72.296105128440885,-50793.309221016585,10.141456696495627,null,29.7]
["IC/ICD","IC44-075A1",1651,4.5999999999999996,3144,11.1,"NA",14.1,158,217.78888860545663,19.2,330,32,1.0349471979184923,0.39131810431895675,0.77961636956896396,null,0.26041666666666669,0.29689097509962514,0.4030254452926208,1.071672400037089,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.11380820712152297,0.147100625883303,1.3656984854582757,3.5304150211992722,2.2475320071589708,584.82092307692312,93.077140731257387,806.66855300423072,136368.73359558065,29519.462252510628,-32433.624925000004,0.39131810431895675,62705.932983381921,12233.290663202602,-47650.045300000005,0.77961636956896396,51078.254581950168,5977.1113735710524,-50051.958356129355,0.93312097984924458,null,308]
["IC/ICD","IC44-075A2",1651,9.1999999999999993,3144,22.1,"NA",3.5,39.4,108.89444430272832,19.2,330,32,2.0698943958369846,1.0679501502915787,1.6931632885420307,null,0.26041666666666669,0.29689097509962514,0.4030254452926208,0.51703884162783076,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.22761641424304593,0.294201251766606,2.7313969709165513,7.0608300423985444,4.4950640143179417,584.82092307692312,93.077140731257387,806.66855300423072,33780.901596894764,7294.5192167647356,-46317.893125000002,1.0679501502915787,15657.173626996115,3036.6324341283057,-50027.530000000006,1.6931632885420307,12764.953975778908,1483.6801281913963,-50619.521045472255,1.9340906707349641,null,154]
["IC/ICD","IC44-075A3",1651,18.3,3144,44.1,"NA",0.88,9.9,54.51793282948281,19.2,330,32,4.1344194158092824,2.3142188175827862,3.4969499157625088,null,0.26041666666666669,0.29689097509962514,0.4030254452926208,0.2547220979087052,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.45275873702692837,0.58520466384009684,5.4331048443231404,14.044911932162325,8.9412686371759058,584.82092307692312,93.077140731257387,806.66855300423072,8483.6897692706461,1832.2776052535924,-49675.614352000004,2.3142188175827862,3921.2648744252888,760.33288381271529,-50610.655888000001,3.4969499157625088,3198.7683821644564,371.49402010099141,-50758.727197763685,3.9258470631723892,null,77.099999999999994]
["IC/ICD","IC44-075A7",1651,31.8,3144,76.400000000000006,"NA",0.28999999999999998,3.3,31.466251762801363,19.2,330,32,7.1632300440201266,4.1176766726266125,6.1318246419800966,null,0.26041666666666669,0.29689097509962514,0.4030254452926208,0.14609709449830327,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.78676108401400668,1.01691302241066,9.4411330081680802,24.405912537855841,15.537286484272887,584.82092307692312,93.077140731257387,806.66855300423072,2828.0832432126754,603.76370399478299,-50436.993748000001,4.1176766726266125,1308.5470713978484,251.30478778840444,-50741.376037000002,6.1318246419800966,1066.1399948341198,122.78599002320259,-50789.933236363111,6.844763090149022,null,44.5]
["IC/ICD","IC44-100A1",2296,4.8,4192,11.1,"NA",17.600000000000001,208,290.62088706767099,25,330,32,0.77558086851312813,0.21880348051440002,0.54649519965513227,null,0.2,0.26465376358245085,0.37471374045801525,1.4401431906108109,942.48,0,-1570.8,0,0,0,0,0,0.10586150543298034,0.13682926829268291,1.2703380651957641,3.2839024390243901,2.0905972232090524,724.98461538461538,115.38488520403808,1000.0023384349968,238592.8042092293,49169.195484424999,-22181.0128,0.21880348051440002,113282.90312458924,21262.354804075672,-45452.5072,0.54649519965513227,89927.99572111835,9260.6291483929708,-49789.782963112164,0.69437539719634955,null,411]
["IC/ICD","IC44-100A2",2296,9.5,4192,22.1,"NA",4.4000000000000004,52.1,145.66399692442877,25,330,32,1.5473967813538625,0.75993847548201798,1.2325569130196348,null,0.2,0.26465376358245085,0.37471374045801525,0.69113103694249445,942.48,0,-1570.8,0,0,0,0,0,0.20951756283610692,0.2708079268292683,2.5142107540332832,6.4993902439024387,4.1376403376012494,724.98461538461538,115.38488520403808,1000.0023384349968,59551.726277169684,12266.701703294166,-43713.446800000005,0.75993847548201798,28301.431536034401,5273.016569289347,-49494.73,1.2325569130196348,22561.698908335038,2296.61537451909,-50556.576618980231,1.4469036210903157,null,206]
["IC/ICD","IC44-100A3",2296,19,4192,44.1,"NA",1.1000000000000001,13,72.831998462214386,25,330,32,3.094793562707725,1.7194336534207588,2.5806680684405086,null,0.2,0.26465376358245085,0.37471374045801525,0.33906906398386172,942.48,0,-1570.8,0,0,0,0,0,0.41903512567221385,0.54161585365853659,5.0284215080665664,12.998780487804877,8.2752806752024988,724.98461538461538,115.38488520403808,1000.0023384349968,14808.029497058862,3059.7372461271079,-49040.244925000006,1.7194336534207588,7068.5664889825985,1318.2541423223367,-50477.552500000005,2.5806680684405086,5639.1364263447622,574.1538436297725,-50743.014154745062,2.9492516605631582,null,103]
["IC/ICD","IC44-100A7",2296,33,4192,76.400000000000006,"NA",0.37,4.3,41.93143212436226,25,330,32,5.3754424445007709,3.1043933446164176,4.5602217127598506,null,0.2,0.26465376358245085,0.37471374045801525,0.19373581478083204,942.48,0,-1570.8,0,0,0,0,0,0.7277978498517399,0.94070121951219499,8.7335741982208788,22.576829268292681,14.372855909562235,724.98461538461538,115.38488520403808,1000.0023384349968,4878.8921916439267,1026.515259926349,-50205.850132000007,3.1043933446164176,2340.4632765857968,443.390099182847,-50693.346925000005,4.5602217127598506,1868.6895011829702,193.11460628125963,-50783.949502510084,5.161668229136013,null,59.3]
["IC/ICD","IC44-150A1",3445,4.8,6289,11.1,"NA",24.7,309,436.28488399209976,36.200000000000003,330,32,0.51663490593013883,{"$error":"#NUM!"},0.31962952657360805,null,0.13812154696132595,0.24223488821320421,0.34301669581809507,2.2098197636646346,1294.3392000000001,0,-2157.232,0,0,0,0,0,9.6893955285281677E-2,0.12523843251088532,1.1627274634233802,3.0057223802612478,1.9135022975220604,995.64553846153854,158.46190901354564,1373.3365447840622,530505.06162632722,103590.69097863973,5571.7316749999882,{"$error":"#NUM!"},253953.7796028778,44795.97447724962,-40262.804800000005,0.31962952657360805,200453.21560302028,17857.750017074315,-49129.780697354967,0.45252559346363119,null,617]
["IC/ICD","IC44-150A2",3445,9.6,6289,22.1,"NA",6.2,77.400000000000006,217.78888860545663,36.200000000000003,330,32,1.0349471979184923,0.4385275277327888,0.78742901584072755,null,0.13812154696132595,0.24223488821320421,0.34301669581809507,1.0412860045805694,1294.3392000000001,0,-2157.232,0,0,0,0,0,0.19378791057056335,0.25047686502177063,2.3254549268467604,6.0114447605224957,3.8270045950441207,995.64553846153854,158.46190901354564,1373.3365447840622,132035.34070100577,25843.439510823631,-36724.299700000003,0.4385275277327888,63396.136440704926,11226.109470765015,-48148.1872,0.78742901584072755,49969.00271618228,4475.2471384464625,-50382.916852964809,0.96035094642686614,null,308]
["IC/ICD","IC44-150A3",3445,19.2,6289,44.1,"NA",1.5,19.3,108.89444430272832,36.200000000000003,330,32,2.0698943958369846,1.1122779473510804,1.696843492836585,null,0.13812154696132595,0.24223488821320421,0.34301669581809507,0.50707773699317604,1294.3392000000001,0,-2157.232,0,0,0,0,0,0.38757582114112671,0.50095373004354127,4.6509098536935207,12.022889521044991,7.6540091900882414,995.64553846153854,158.46190901354564,1373.3365447840622,32804.566286150628,6238.2992396766285,-47523.293125000004,1.1122779473510804,15828.435258830717,2715.9942267979877,-50183.08,1.696843492836585,12488.977132618058,1082.7210818822086,-50706.299741849201,1.9720842132208567,null,154]
["IC/ICD","IC44-150A7",3445,33.200000000000003,6289,76.400000000000006,"NA",0.51,6.4,62.932503525602726,36.200000000000003,330,32,3.5816150220100633,2.0417883865043156,3.0131409784817764,null,0.13812154696132595,0.24223488821320421,0.34301669581809507,0.29016512369644537,1294.3392000000001,0,-2157.232,0,0,0,0,0,0.67018319072319832,0.86623249153362369,8.0421982886783798,20.789579796806969,13.23505755786092,995.64553846153854,158.46190901354564,1373.3365447840622,10873.518332597905,2123.5826830161336,-49666.515028000002,2.0417883865043156,5265.9407306068078,922.81341722690615,-50590.140532000005,3.0131409784817764,4167.9591815013455,367.87616542663926,-50770.989346524686,3.446313558503828,null,89]
["IC/ICD","IC44-200A1",4786,5,8388,11.1,"NA",31.8,410,581.94888091652854,47.4,330,32,0.38731924296342124,{"$error":"#NUM!"},0.19002599729170858,null,0.10548523206751055,0.22176208495688879,0.32709394372913686,3.0307969908260657,1646.1984,0,-2743.6639999999998,0,0,0,0,0,9.2400868732036998E-2,0.11943097924502018,1.1088104247844439,2.8663435018804844,1.82477094769445,1266.3064615384615,201.53893282305319,1746.6707511331276,937537.47377892572,177895.74799561495,42641.0003,{"$error":"#NUM!"},460179.18504563865,80133.219817844569,-31844.410000000003,0.19002599729170858,354849.23052027554,29244.954293763181,-48279.748119970362,0.32994621646613248,null,823]
["IC/ICD","IC44-200A2",4786,10,8388,22.1,"NA",8,103,290.62088706767099,47.4,330,32,0.77558086851312813,0.25972585262464443,0.55069652293235549,null,0.10548523206751055,0.22176208495688879,0.32709394372913686,1.4038167445227032,1646.1984,0,-2743.6639999999998,0,0,0,0,0,0.184801737464074,0.23886195849004035,2.2176208495688878,5.7326870037609687,3.6495418953889001,1266.3064615384615,201.53893282305319,1746.6707511331276,234284.03516030853,44497.920565347762,-27361.48,0.25972585262464443,115136.27141342487,20134.805685677718,-46005.16,0.55069652293235549,88546.253862929283,7348.2816905395466,-50165.840509782458,0.71234369008755438,null,411]
["IC/ICD","IC44-200A3",4786,20,8388,44.1,"NA",2,25.7,145.66399692442877,47.4,330,32,1.5473967813538625,0.78765991569744287,1.2265839805330043,null,0.10548523206751055,0.22176208495688879,0.32709394372913686,0.68103329630104015,1646.1984,0,-2743.6639999999998,0,0,0,0,0,0.36960347492814799,0.47772391698008071,4.4352416991377757,11.465374007521937,7.2990837907778001,1266.3064615384615,201.53893282305319,1746.6707511331276,58359.93016279531,11126.317258644029,-44970.73,0.78765991569744287,28857.189465869735,5045.9488701333457,-49605.16,1.2265839805330043,22235.475565623969,1841.5401803541929,-50645.330127445617,1.4683569884635503,null,206]
["IC/ICD","IC44-200A7",4786,34.6,8388,76.400000000000006,"NA",0.66,8.6,84.145706961199153,47.4,330,32,2.6786868652008038,1.4898577717334625,2.2020887304541565,null,0.10548523206751055,0.22176208495688879,0.32709394372913686,0.38842698183305618,1646.1984,0,-2743.6639999999998,0,0,0,0,0,0.639414011625696,0.82646237637553976,7.6729681395083524,19.835097033012953,12.627414958045595,1266.3064615384615,201.53893282305319,1746.6707511331276,19563.088766575711,3674.5138560054443,-48898.225168000004,1.4898577717334625,9640.6778953074499,1664.1122960443504,-50414.047828000002,2.2020887304541565,7421.4940889362879,607.32475430456725,-50753.067159495644,2.5744864460260244,null,119]
["IC/ICD","IC44-250A1",6029,5,12500,11.1,"NA",38.6,512,698.62149981230891,58.5,330,32,0.32263536129442882,{"$error":"#NUM!"},0.11674970083096184,null,8.5470085470085472E-2,0.21333255993402445,0.26598880000000003,3.7472574565307779,1994.9159999999999,0,-3324.86,0,0,0,0,0,8.8888566639176839E-2,0.11489122021341296,1.0666627996701221,2.7573892851219108,1.7554085390231189,1534.5507692307692,244.23134034854732,2116.6716163540768,1421986.0799423126,259228.56867264147,86878.318700000003,{"$error":"#NUM!"},677568.40450091567,116769.62552821689,-22868.410000000003,0.11674970083096184,511429.01709733409,40995.679550152781,-47361.721856081043,0.26686183471519542,null,988]
["IC/ICD","IC44-250A2",6029,10,12500,22.1,"NA",9.6999999999999993,128,349.31074990615446,58.5,330,32,0.64527072258885765,0.14202871851356258,0.42891347647582395,null,8.5470085470085472E-2,0.21333255993402445,0.26598880000000003,1.7066173721362237,1994.9159999999999,0,-3324.86,0,0,0,0,0,0.17777713327835368,0.22978244042682591,2.1333255993402442,5.5147785702438217,3.5108170780462378,1534.5507692307692,244.23134034854732,2116.6716163540768,353397.84730573057,64849.493845813078,-16339.287325000005,0.14202871851356258,169392.10112522892,29343.662373671075,-43748.41,0.42891347647582395,127857.25427433352,10302.023099390723,-49935.356528869677,0.58595442442278101,null,494]
["IC/ICD","IC44-250A3",6029,19.899999999999999,12500,44.1,"NA",2.4,32,174.65537495307723,58.5,330,32,1.2905414451777153,0.60886996727644083,0.99607207393419184,null,8.5470085470085472E-2,0.21333255993402445,0.26598880000000003,0.82012232347395531,1994.9159999999999,0,-3324.86,0,0,0,0,0,0.35377649522392379,0.45726705644938348,4.2453179426870857,10.974409354785204,6.9865259853120127,1534.5507692307692,244.23134034854732,2116.6716163540768,88088.016005847778,16008.934152728592,-42403.580800000003,0.60886996727644083,42229.886116626185,7223.9861596212913,-49094.396800000002,0.99607207393419184,31949.751928236761,2536.2093980768086,-50594.294124116343,1.2193303015629438,null,247]
["IC/ICD","IC44-250A7",6029,34.5,12500,76.400000000000006,"NA",0.8,10.7,101.11626970967629,58.5,330,32,2.229117041670599,1.1872484489871331,1.7998037858940821,null,8.5470085470085472E-2,0.21333255993402445,0.26598880000000003,0.4678962147221436,1994.9159999999999,0,-3324.86,0,0,0,0,0,0.61333110981032035,0.79274941947254929,7.3599733177238438,19.025986067341183,12.11231891925952,1534.5507692307692,244.23134034854732,2116.6716163540768,29547.533908670266,5352.2330675709554,-48003.419200000004,1.1872484489871331,14164.777320693438,2416.911529204162,-50233.840000000004,1.7998037858940821,10710.172142382151,848.53342728568191,-50734.740030591114,2.1372260953079989,null,143]
["IC/ICD","IC11-030A1AC",254,9.6999999999999993,315,13.8,"NA",1.6,10.3,17.53624817342638,2.5,330,32,12.853376490278048,7.3352947384459926,9.0196022782090353,null,2,0.59807582793829439,1.2466666666666666,0.1100022426920806,235.62,0,-392.7,0,0,0,0,0,0.48344462758345458,0.79260245901639348,5.8013355310014552,19.022459016393444,9.5472664200979018,181.24615384615385,28.846221301009521,250.00058460874919,891.70939079726395,335.32534782804595,-50439.515200000002,7.3352947384459926,596.14833322891491,235.69970100956851,-50624.5072,9.0196022782090353,587.13056473169854,231.98843718306901,-50630.151431495055,9.0907237482349359,null,24.8]
["IC/ICD","IC11-030A5AC",254,16.899999999999999,315,23.9,"NA",0.53,3.4,10.111626970967629,2.5,330,32,22.291170416705988,12.960657056537158,15.823525426039122,null,2,0.59807582793829439,1.2466666666666666,6.2710957789331612E-2,235.62,0,-392.7,0,0,0,0,0,0.84229012434643113,1.367349726775956,10.107481492157174,32.816393442622946,16.633897164912838,181.24615384615385,28.846221301009521,250.00058460874919,293.17522284622652,110.92397949430838,-50684.820333250005,12.960657056537158,197.71178270182727,78.43578466333939,-50744.989113250005,15.823525426039122,194.72906324407967,77.200755984570122,-50746.869064261446,15.946176477791253,null,14.3]
["IC/ICD","IC11-050A1AC",432,9.9,525,13.8,"NA",2.1,16.5,29.274220741123063,3.6,330,32,7.6996071729201851,4.4614319227316148,5.4081149947387113,null,1.3888888888888888,0.40322124646555868,0.85770666666666662,0.15718339496561828,270.17759999999998,0,-450.29599999999999,0,0,0,0,0,0.33265752833408591,0.44446881720430104,3.9918903400090309,10.667251612903225,6.569459806663243,207.82892307692308,33.077000425157586,286.66733701803241,2356.1369577203795,734.70730191961468,-50175.279700000006,4.4614319227316148,1628.5215533825583,527.07262963798439,-50480.991925000002,5.4081149947387113,1196.7212275527024,349.75580359586263,-50662.415569384364,6.3619951727008841,null,41.4]
["IC/ICD","IC11-050A5AC",432,17.2,525,23.9,"NA",0.7,5.5,16.899852070358484,3.6,330,32,13.337394851836638,7.872669690699742,9.4898355398202856,null,1.3888888888888888,0.40322124646555868,0.85770666666666662,8.988229747158083E-2,270.17759999999998,0,-450.29599999999999,0,0,0,0,0,0.57795045326730077,0.77158745519713257,6.9354054392076092,18.518098924731181,11.413606936829067,207.82892307692308,33.077000425157586,286.66733701803241,785.22777172131077,244.85528129565628,-50595.240325000006,7.872669690699742,544.36867848257657,176.21384260607903,-50696.438800000004,9.4898355398202856,399.54920610050164,116.93229862407262,-50757.285619434151,11.125661316302935,null,23.9]
["IC/ICD","IC11-075A1AC",649,9.9,798,13.8,"NA",2.8,24.4,43.982041789803255,5,330,32,{"$f":"IF(G271=\"NA\",(UAC_V*0.98)/J271,(IF((UAC_V*0.98)/J271<G271,(UAC_V*0.98)/J271,G271)))","v":5.1248189221687399},{"$f":"IF(AO271<G271,IF(AO271<0,0,AO271),G271)","v":2.9493562291070279},{"$f":"IF(AS271<G271,IF(AS271<0,0,AS271),G271)","v":3.5812073806578728},null,{"$f":"IF(move1,Gewicht/K271,MAX(Gewicht,Gewicht2)/K271)","v":1},{"$f":"IF(move1,IF(AccType=1,SQRT((V271^2*Ltime1+W271^2*Ltime2+X271^2*Ltime3+Y271^2*Ltime4)/ltime)/C271,SQRT((((V271-W271)*2/PI()+W271)^2*Ltime1+W271^2*Ltime2+((X271-W271)*2/PI()+W271)^2*Ltime3+Y271^2*Ltime4)/ltime)/C271),IF(AccType=1,SQRT((V271^2*Ltime1+W271^2*Ltime2+X271^2*Ltime3+Y271^2*Ltime4+Z271^2*Ltime5+AA271^2*Ltime6+AB271^2*Ltime7+AC271^2*Ltime8)/ltime)/C271,SQRT((((V271-W271)*2/PI()+W271)^2*Ltime1+W271^2*Ltime2+((X271-W271)*2/PI()+W271)^2*Ltime3+Y271^2*Ltime4+((Z271-AA271)*2/PI()+AA271)^2*Ltime5+AA271^2*Ltime6+((AB271-AA271)*2/PI()+AA271)^2*Ltime7+AC271^2*Ltime8)/ltime)/C271))","v":0.31209298468685526},{"$f":" IF(move1,MAX(ABS(V271),ABS(X271))/E271,MAX(ABS(V271),ABS(X271),ABS(Z271),ABS(AB271))/E271)","v":0.65614035087719302},{"$f":"IF(AW271>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW271,G271),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW271,G271)),\"NA\")","v":0.22215956104891751},{"$f":"((Gewicht+K271)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":314.16000000000003},0,{"$f":"((Gewicht+K271)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-523.6},0,{"$f":"((Gewicht2+K271)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K271)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF271/Irms","v":0.25747671236665559},{"$f":"AG271/Ipeak","v":0.33279661016949152},{"$f":"D271*S271","v":3.0897205483998671},{"$f":"IF(move1,IF(MAX(ABS(V271),ABS(X271))<=C271,MAX(ABS(V271),ABS(X271))/C271*D271,D271+(MAX(ABS(V271),ABS(X271))-C271)/(E271-C271)*(F271-D271)),IF(MAX(ABS(V271),ABS(X271),ABS(Z271),ABS(AB271))<=C271,MAX(ABS(V271),ABS(X271),ABS(Z271),ABS(AB271))/C271*D271,D271+(MAX(ABS(V271),ABS(X271),ABS(Z271),ABS(AB271))-C271)/(E271-C271)*(F271-D271)))","v":7.987118644067797},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V271),ABS(X271))<=C271,MAX(ABS(V271),ABS(X271))/C271*D271,D271+(MAX(ABS(V271),ABS(X271))-C271)/(E271-C271)*(F271-D271)),IF(MAX(ABS(V271),ABS(X271),ABS(Z271),ABS(AB271))<=C271,MAX(ABS(V271),ABS(X271),ABS(Z271),ABS(AB271))/C271*D271,D271+(MAX(ABS(V271),ABS(X271),ABS(Z271),ABS(AB271))-C271)/(E271-C271)*(F271-D271))),IF(move1,IF(MAX(ABS((V271-W271)*2/PI()+W271),ABS((X271-W271)*2/PI()+W271))<=C271,MAX(ABS((V271-W271)*2/PI()+W271),ABS((X271-W271)*2/PI()+W271))/C271*D271,D271+(MAX(ABS((V271-W271)*2/PI()+W271),ABS((X271-W271)*2/PI()+W271))-C271)/(E271-C271)*(F271-D271)),IF(MAX(ABS((V271-W271)*2/PI()+W271),ABS((X271-W271)*2/PI()+W271),ABS((Z271-AA271)*2/PI()+AA271),ABS((AB271-AA271)*2/PI()+AA271))<=C271,MAX(ABS((V271-W271)*2/PI()+W271),ABS((X271-W271)*2/PI()+W271),ABS((Z271-AA271)*2/PI()+AA271),ABS((AB271-AA271)*2/PI()+AA271))/C271*D271,D271+(MAX(ABS((V271-W271)*2/PI()+W271),ABS((X271-W271)*2/PI()+W271),ABS((Z271-AA271)*2/PI()+AA271),ABS((AB271-AA271)*2/PI()+AA271))-C271)/(E271-C271)*(F271-D271))))","v":5.0847576530593059},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V271)+Ltime2*ABS(Lspeed2)*ABS(W271)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X271)+Ltime4*ABS(Lspeed1)*ABS(Y271))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V271)+Ltime2*ABS(Lspeed2)*ABS(W271)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X271)+Ltime4*ABS(Lspeed1)*ABS(Y271)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z271)+Ltime6*ABS(Lspeed6)*ABS(AA271)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB271)+Ltime8*ABS(Lspeed1)*ABS(AC271))/ltime)","v":241.66153846153847},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK271/2*Ltime1/ltime,AK271/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X271*-ABS(Lspeed2-Lspeed1),((X271-Y271)*2/PI()+Y271)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V271*-ABS(Lspeed2-Lspeed1),((V271-W271)*2/PI()+W271)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X271*-ABS(Lspeed2-Lspeed1),((X271-Y271)*2/PI()+Y271)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V271*-ABS(Lspeed2-Lspeed1),((V271-W271)*2/PI()+W271)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB271*-ABS(Lspeed6-Lspeed1),((AB271-AC271)*2/PI()+AB271)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z271*-ABS(Lspeed6-Lspeed1),((Z271-AA271)*2/PI()+AA271)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB271*-ABS(Lspeed6-Lspeed1),((AB271-AC271)*2/PI()+AB271)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z271*-ABS(Lspeed6-Lspeed1),((Z271-AA271)*2/PI()+AA271)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":38.461628401346033},{"$f":"IF(move1,MAX(IF(AccType=1,X271*-ABS(Lspeed2-Lspeed1),((X271-Y271)*2/PI()+Y271)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V271*-ABS(Lspeed2-Lspeed1),((V271-W271)*2/PI()+W271)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X271*-ABS(Lspeed2-Lspeed1),((X271-Y271)*2/PI()+Y271)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V271*-ABS(Lspeed2-Lspeed1),((V271-W271)*2/PI()+W271)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB271*-ABS(Lspeed6-Lspeed1),((AB271-AC271)*2/PI()+AB271)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z271*-ABS(Lspeed6-Lspeed1),((Z271-AA271)*2/PI()+AA271)*-ABS(Lspeed6-Lspeed1)),0))","v":333.33411281166559},{"$f":"(J271^2)+3*(I271/1000)^2*(F271/2)^2*(2000*PI()/M271)^2","v":5212.7968093605332},{"$f":"SQRT(3)*H271*F271/2*J271","v":1471.7808109307578},{"$f":"3*F271^2*H271^2/4-(UAC_V*0.98)^2","v":-49685.372800000005},{"$f":"-AM271/2/AL271+SQRT((AM271/2/AL271)^2-AN271/AL271)","v":2.9493562291070279},{"$f":"(J271^2)+3*(I271/1000)^2*(D271/2)^2*(2000*PI()/M271)^2","v":3621.6375545338469},{"$f":"SQRT(3)*H271*D271/2*J271","v":1055.8427556677177},{"$f":"3*D271^2*H271^2/4-(UAC_V*0.98)^2","v":-50228.861200000007},{"$f":"-AQ271/2/AP271+SQRT((AQ271/2/AP271)^2-AR271/AP271)","v":3.5812073806578728},{"$f":"(J271^2)+3*(I271/1000)^2*(AH271/2)^2*(2000*PI()/M271)^2","v":2379.5032119054868},{"$f":"SQRT(3)*H271*AH271/2*J271","v":542.29338710188426},{"$f":"3*AH271^2*H271^2/4-(UAC_V*0.98)^2","v":-50653.134008904774},{"$f":"IF((AU271/2/AT271)^2-AV271/AT271>=0,-AU271/2/AT271+SQRT((AU271/2/AT271)^2-AV271/AT271),-9999)","v":4.5012692466556015},null,62.2]
["IC/ICD","IC11-075A5AC",649,17.100000000000001,798,23.9,"NA",0.93,8.1,25.385133444597052,5,330,32,8.8792127286600468,5.2628590815680063,6.3527740003649571,null,1,0.31209298468685526,0.65614035087719302,0.12659952938304558,314.16000000000003,0,-523.6,0,0,0,0,0,0.44473250317876878,0.57483050847457628,5.3367900381452253,13.795932203389832,8.7827632189206213,241.66153846153847,38.461628401346033,333.33411281166559,1728.0496298391799,488.64215640275415,-50434.630353250002,5.2628590815680063,1199.1371059002374,349.6142625308409,-50615.480943250004,6.3527740003649571,790.74175827856573,179.56604010327058,-50755.12320208818,7.8989235179093935,null,35.9]
["IC/ICD","IC11-100A1AC",864,9.9,1051,13.8,"NA",3.5,32.1,58.619152160364791,6.5,330,32,3.8451596738105622,2.1898158491789244,2.6670416680791842,null,0.76923076923076927,0.26959560083453055,0.57292102759276875,0.28928333373266246,361.28399999999999,0,-602.14,0,0,0,0,0,0.22241637068848771,0.28748003472222222,2.6689964482618524,6.8995208333333338,4.392371382362052,277.91076923076923,44.230872661547934,383.33422973341544,9110.2043417985569,2451.9820985964602,-49055.4925,2.1898158491789244,6356.3303701411287,1759.0306359496344,-49904.693125000005,2.6670416680791842,4011.0214853569287,780.43594202457518,-50627.906239062053,3.4568185698666531,null,82.9]
["IC/ICD","IC11-100A5AC",864,17.2,1051,23.9,"NA",1.2,10.7,33.799704140716969,6.5,330,32,6.6686974259183192,3.9315641623593827,4.7376084917513746,null,0.76923076923076927,0.26959560083453055,0.57292102759276875,0.16487706448312262,361.28399999999999,0,-602.14,0,0,0,0,0,0.38642036119616047,0.49946026234567897,4.6370443343539254,11.987046296296295,7.631190684507807,277.91076923076923,44.230872661547934,383.33422973341544,3033.388963119764,839.50382158510729,-50188.253200000006,3.9315641623593827,2121.7870594866181,604.16174607798519,-50485.652800000003,4.7376084917513746,1335.2049868244662,268.05078422129606,-50742.266123035617,6.0651249652880823,null,47.8]
["IC/ICD","IC11-150A1AC",1285,9.8000000000000007,1576,13.8,"NA",5,47.7,87.681240867131891,9.4,330,32,2.57067529805561,1.4044218346540627,1.7423689267595774,null,0.53191489361702127,0.22698024884742996,0.47841624365482238,0.42569753881007666,452.3904,0,-753.98400000000004,0,0,0,0,0,0.18536720322540115,0.23959284046692611,2.2244064387048139,5.7502281712062269,3.6607089494149614,347.99261538461542,55.384744897938283,480.00112244879847,20216.987453926919,5239.4585598132171,-47234.41,1.4044218346540627,14006.44126798541,3720.7749192876472,-49004.41,1.7423689267595774,8569.6337425811362,1389.8646985505122,-50553.895187268878,2.3490856977825896,null,124]
["IC/ICD","IC11-150A5AC",1285,17,1576,23.9,"NA",1.7,15.9,50.699556211075453,9.4,330,32,4.4457982839455461,2.5816557484667122,3.14070421921455,null,0.53191489361702127,0.22698024884742996,0.47841624365482238,0.24240226713226368,452.3904,0,-753.98400000000004,0,0,0,0,0,0.32155535253385908,0.41562023346303506,3.8586642304063092,9.9748856031128419,6.3502094020463611,347.99261538461542,55.384744897938283,480.00112244879847,6745.9700551690776,1783.945620868353,-49567.062325000006,2.5816557484667122,4683.0248584476176,1268.9152951783265,-50178.752500000002,3.14070421921455,2865.2205004927901,473.99281399069662,-50717.755216892481,4.1253739572260804,null,71.7]
["IC/ICD","IC11-200A1AC",1712,9.8000000000000007,2102,13.8,"NA",6.4,63.3,117.37972567696688,12.3,330,32,1.9202634756559978,1.0016681447146754,1.2640745464057308,null,0.4065040650406504,0.20467794416872689,0.43093625118934348,0.56758936973174956,543.49680000000001,0,-905.82799999999997,0,0,0,0,0,0.16715365440446031,0.21605126557632401,2.0058438528535238,5.185230373831776,3.3010201802622539,418.07446153846155,66.538617134328632,576.6680151641815,35842.121294105455,8978.0657644283274,-44954.843200000003,1.0016681447146754,24905.064740001515,6375.7278616954791,-47854.811200000004,1.2640745464057308,15040.480916673769,2147.5924831956208,-50470.412324439087,1.7618370838633106,null,166]
["IC/ICD","IC11-200A5AC",1712,17,2102,23.9,"NA",2.1,21.1,67.670118959552596,12.3,330,32,3.3308645450250327,1.9051893245772271,2.3279602755799611,null,0.4065040650406504,0.20467794416872689,0.43093625118934348,0.3211172335541479,543.49680000000001,0,-905.82799999999997,0,0,0,0,0,0.28996042090569646,0.37478280763239874,3.4795250508683573,8.9947873831775702,5.7262594963732969,418.07446153846155,66.538617134328632,576.6680151641815,11932.536047869249,2941.336872802633,-48915.882925000005,1.9051893245772271,8299.5949813277311,2092.1643028303247,-49849.292500000003,2.3279602755799611,5001.3572968655653,704.72210041502149,-50696.706916835996,3.1141274759125519,null,95.7]
["IC/ICD","IC11-250A1AC",2410,9.9,3125,13.8,"NA",7.7,78.900000000000006,140.71424945612296,15.2,330,32,1.6018278239140484,0.77313286985204122,0.99660843567846058,null,0.32894736842105265,0.16977081371982303,0.33845503999999998,0.67402942718495729,634.60320000000002,0,-1057.672,0,0,0,0,0,0.140060921318854,0.18103307053941908,1.680731055826248,4.344793692946058,2.7659815717874232,488.15630769230768,77.692489370718974,673.33490787956453,54079.900862334209,12949.068308389991,-42336.7693,0.77313286985204122,37442.403373857254,9289.5490038449916,-46446.900325000002,0.99660843567846058,21177.625799340567,2595.4263994799458,-50464.954540788494,1.4836147498432508,null,199]
["IC/ICD","IC11-250A5AC",2410,17.2,3125,23.9,"NA",2.6,26.3,81.317279836452954,15.2,330,32,2.7718585822512667,1.5129816231571389,1.8620297802123698,null,0.32894736842105265,0.16977081371982303,0.33845503999999998,0.38236655753853127,634.60320000000002,0,-1057.672,0,0,0,0,0,0.24333816633174632,0.31452210235131395,2.9200579959809558,7.5485304564315348,4.8055437408831994,488.15630769230768,77.692489370718974,673.33490787956453,18036.766941220281,4376.0746627257158,-47909.125300000007,1.5129816231571389,12529.334670069864,3149.3089622963307,-49305.251200000006,1.8620297802123698,7074.3677192541709,879.89197510874988,-50688.077219227111,2.6152914795620679,null,115]
["IC/ICD","IC22-030A1AC",519,9.9,630,13.8,"NA",3.1,20.6,35.14320702497141,4.8,330,32,6.4137572828751637,3.5423709082089601,4.3458911507408455,null,1.0416666666666667,0.38246123337289728,0.81448888888888893,0.18995795540538263,307.8768,0,-513.12800000000004,0,0,0,0,0,0.31553051753264028,0.40783294797687869,3.7863662103916833,9.7879907514450881,6.2312284441209638,236.8283076923077,37.692395833319111,326.6674305554323,3571.8025631890559,1302.0054521135846,-49432.563700000006,3.5423709082089601,2437.65794249191,934.04738955974562,-50098.752925000001,4.3458911507408455,1711.4790922533705,587.90531939208279,-50525.305691396265,5.2643228227316667,null,49.7]
["IC/ICD","IC22-030A2AC",519,19.8,630,27.6,"NA",0.78,5.2,17.606958851545031,4.8,330,32,12.801756504373321,7.2853892820061246,8.8727946279621932,null,1.0416666666666667,0.38246123337289728,0.81448888888888893,9.3688739159485196E-2,307.8768,0,-513.12800000000004,0,0,0,0,0,0.63106103506528055,0.81566589595375738,7.5727324207833666,19.575981502890176,12.462456888241928,236.8283076923077,37.692395833319111,326.6674305554323,905.59293956670797,328.2605295119107,-50457.568912000002,7.2853892820061246,616.52450197927442,235.49124943245766,-50626.272148000004,8.8727946279621932,431.43753703959965,148.22219917223384,-50734.290754899266,10.673641346562603,null,24.9]
["IC/ICD","IC22-030A6AC",519,34.299999999999997,630,47.8,"NA",0.26,1.7,10.182337649086284,4.8,330,32,22.136370622145531,12.932317500256783,15.656618124330919,null,1.0416666666666667,0.38246123337289728,0.81448888888888893,5.348636404882031E-2,307.8768,0,-513.12800000000004,0,0,0,0,0,1.0932016920575314,1.4129969813744381,13.118420304690376,33.911927552986512,21.589003599328183,236.8283076923077,37.692395833319111,326.6674305554323,294.61022284622652,109.59213068391361,-50689.318612000003,12.932317500256783,201.99213471243371,78.640378294105361,-50745.511957000002,15.656618124330919,142.62790335629913,49.497592129561831,-50781.529486625928,18.69635406675313,null,14.4]
["IC/ICD","IC22-050A1AC",864,9.9,1051,13.8,"NA",4.2,33,58.619152160364791,6.9,330,32,3.8451596738105622,2.1119011231710751,2.5980308588214096,null,0.72463768115942029,0.27897283912442733,0.59284871550903906,0.29413376438722899,373.85040000000004,0,-623.08400000000006,0,0,0,0,0,0.23015259227765253,0.29747934027777784,2.7618311073318305,7.1395041666666677,4.5451495174007324,287.57723076923077,45.769337797601786,396.66759424588213,9432.8328308815198,2942.378518315752,-48285.638800000001,2.1119011231710751,6522.3712135302339,2110.8367631395613,-49508.487700000005,2.5980308588214096,4086.7019609753684,969.09784800964644,-50531.849577886969,3.3998136938930057,null,82.9]
["IC/ICD","IC22-050A2AC",864,19.8,1051,27.6,"NA",1.1000000000000001,8.3000000000000007,29.274220741123063,6.9,330,32,7.6996071729201851,4.434925809170533,5.3838836479188563,null,0.72463768115942029,0.27897283912442733,0.59284871550903906,0.14442739992847595,373.85040000000004,{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},-623.08400000000006,{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},0,{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0,0,0.46030518455530506,0.59495868055555567,5.5236622146636609,14.279008333333335,9.0902990348014647,287.57723076923077,45.769337797601786,396.66759424588213,2374.3636226608915,769.6933639157869,-50113.862800000003,4.434925809170533,1637.901911662434,552.17132628741228,-50449.383700000006,5.3838836479188563,1021.5814164980461,253.50517547452063,-50730.170065588034,6.92389394599103,null,41.4]
["IC/ICD","IC22-050A6AC",864,34.299999999999997,1051,47.8,"NA",0.35,2.8,16.899852070358484,6.9,330,32,13.337394851836638,7.7840781233005032,9.4230498973886672,null,0.72463768115942029,0.27897283912442733,0.59284871550903906,8.2841189289515837E-2,373.85040000000004,0,-623.08400000000006,0,0,0,0,0,0.79739736516398807,1.0306607445987654,9.5687683819678568,24.735857870370371,15.747336206752031,287.57723076923077,45.769337797601786,396.66759424588213,803.56103706381168,244.85528129565628,-50595.240325000006,7.7840781233005032,552.3064311922077,175.70159306361947,-50697.069981250002,9.4230498973886672,341.81988230857814,80.665657668651505,-50782.376966344724,12.071289760280607,null,23.9]
["IC/ICD","IC22-075A1AC",1284,9.8000000000000007,1576,13.8,"NA",5.7,48.6,87.681240867131891,9.6,330,32,2.57067529805561,1.3562255231881983,1.7015152670258868,null,0.52083333333333337,0.23031198341914549,0.48506091370558374,0.42975788839890583,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.18808811979230219,0.24310970924195227,2.2570574375076262,5.8346330218068543,3.714442746191053,352.82584615384616,56.153977465965212,486.66780470503181,20694.239735012779,5972.9827581870686,-46164.613300000005,1.3562255231881983,14247.122370041103,4241.6834079879181,-48464.905300000006,1.7015152670258868,8630.2820523278933,1607.7030782081292,-50468.95953334029,2.3268915521843532,null,124]
["IC/ICD","IC22-075A2AC",1284,19.600000000000001,1576,27.6,"NA",1.4,12.2,43.982041789803255,9.6,330,32,5.1248189221687399,2.9493562291070279,3.599289120675607,null,0.52083333333333337,0.23031198341914549,0.48506091370558374,0.21086839566656912,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.37617623958460439,0.48621941848390454,4.5141148750152524,11.669266043613709,7.4288854923821059,352.82584615384616,56.153977465965212,486.66780470503181,5212.7968093605332,1471.7808109307578,-49685.372800000005,2.9493562291070279,3587.7244989024657,1045.1776773276397,-50240.444800000005,3.599289120675607,2171.9333544488195,396.14822877861877,-50724.03314070138,4.7422943435356117,null,62.2]
["IC/ICD","IC22-075A6AC",1284,34,1576,47.8,"NA",0.48,4.0999999999999996,25.385133444597052,9.6,330,32,8.8792127286600468,5.2177251706769177,6.3299773409445681,null,0.52083333333333337,0.23031198341914549,0.48506091370558374,0.12084860010223178,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.65255061968757888,0.84344184839044656,7.830607436250947,20.242604361370717,12.886842180662837,352.82584615384616,56.153977465965212,486.66780470503181,1754.9714519187082,504.40480660929455,-50410.339648000001,5.2177251706769177,1206.2889036510333,358.7816616049376,-50605.403200000001,6.3299773409445681,725.12511589852159,135.98713677702381,-50776.462982799931,8.2748165816902368,null,35.9]
["IC/ICD","IC22-100A1AC",1715,9.8000000000000007,2106,13.8,"NA",7.1,64.099999999999994,117.37972567696688,12.5,330,32,1.9202634756559978,0.96617057113912908,1.2353083967680867,null,0.4,0.20668198679772354,0.43509021842355172,0.57180087917834699,549.78,0,-916.3,0,0,0,0,0,0.1687902892181409,0.21816666666666665,2.025483470617691,5.2359999999999998,3.3333411281166558,422.90769230769229,67.307849702355554,583.33469742041473,36403.348391004853,9960.0417074126744,-43605.099700000006,0.96617057113912908,25188.094830246304,7073.0730965684206,-47174.127700000005,1.2353083967680867,15098.068975176873,2405.8128015272396,-50385.074701989237,1.7488605499119843,null,166]
["IC/ICD","IC22-100A2AC",1715,19.600000000000001,2106,27.6,"NA",1.8,16,58.760573516602093,12.5,330,32,3.8359053785667347,2.1855970176691679,2.6754002472108205,null,0.4,0.20668198679772354,0.43509021842355172,0.27921126325929668,549.78,0,-916.3,0,0,0,0,0,0.33758057843628181,0.4363333333333333,4.0509669412353819,10.472,6.6666822562333117,422.90769230769229,67.307849702355554,583.33469742041473,9091.5073864303704,2528.1232625060034,-48954.083200000001,2.1855970176691679,6296.4354200418657,1795.333911054988,-49871.6512,2.6754002472108205,3781.7933519999992,610.65922085940019,-50697.159494897453,3.5815174084554187,null,83.1]
["IC/ICD","IC22-100A6AC",1715,34,2106,47.8,"NA",0.59,5.3,33.941125496954278,12.5,330,32,6.6409111866436596,3.9502115687038102,4.7756536194830126,null,0.4,0.20668198679772354,0.43509021842355172,0.15956303612010533,549.78,0,-916.3,0,0,0,0,0,0.58559896259355004,0.75690476190476186,7.0271875511226005,18.165714285714284,11.564652893465947,422.90769230769229,67.307849702355554,583.33469742041473,3007.7889134084789,828.96611671165397,-50208.645397,3.9502115687038102,2090.9243815322743,589.64117088276646,-50503.357300000003,4.7756536194830126,1260.6270503915814,200.55869038105982,-50770.243517111667,6.2671156447993761,null,48]
["IC/ICD","IC22-150A1AC",2566,9.8000000000000007,3152,13.8,"NA",9.9,95.4,176.06958851545033,18.100000000000001,330,32,1.2801756504373318,0.5573301116165853,0.75998292222223374,null,0.27624309392265189,0.18234087362146784,0.38372969543147212,0.85986280408892779,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,0.14891171345753207,0.19247299298519097,1.7869405614903848,4.6193518316445834,2.9407707115473447,558.23815384615386,88.84636160710933,770.00180059494755,81116.449815707674,20831.918219025105,-36806.3917,0.5573301116165853,56274.265071941642,14793.681054090292,-43745.4997,0.75998292222223374,33276.33159131572,4439.2677510042422,-50169.457409231909,1.162976227422182,null,249]
["IC/ICD","IC22-150A2AC",2566,19.7,3152,27.6,"NA",2.5,23.9,87.681240867131891,18.100000000000001,330,32,2.57067529805561,1.4027526336467386,1.7361341751794586,null,0.27624309392265189,0.18234087362146784,0.38372969543147212,0.41522498221270032,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,0.29934293419524299,0.38690999610288385,3.5921152103429161,9.2858399064692119,5.9115492874982332,558.23815384615386,88.84636160710933,770.00180059494755,20269.574961534734,5239.4585598132171,-47234.41,1.4027526336467386,14097.871123217305,3739.7584647942163,-48985.988125000003,1.7361341751794586,8265.1908996129496,1122.2216491355198,-50641.348679788185,2.4083329347648617,null,124]
["IC/ICD","IC22-150A6AC",2566,34.1,3152,47.8,"NA",0.83,8,50.770266889194104,18.100000000000001,330,32,4.4396063643300234,2.5751599914820491,3.1291974496683488,null,0.27624309392265189,0.18234087362146784,0.38372969543147212,0.23739039767766401,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,0.51815198254100447,0.66972745518316446,6.2178237904920532,16.073458924395947,10.232681761608617,558.23815384615386,88.84636160710933,770.00180059494755,6805.8325474596877,1744.399956190477,-49624.640293000004,2.5751599914820491,4729.459005055759,1244.4359520103612,-50204.365143250005,3.1291974496683488,2771.387061345682,373.42865306822523,-50751.060109817452,4.2124703011695983,null,71.8]
["IC/ICD","IC22-200A1AC",3458,9.9,4204,13.8,"NA",12.7,127,234.75945135393377,23.7,330,32,0.96013173782799888,0.33256495885533238,0.50757415356816604,null,0.2109704641350211,0.16810692772333058,0.35745290199809704,1.1569717116296598,901.63919999999996,0,-1502.732,0,0,0,0,0,0.13868821537174772,0.17925880566801619,1.6642585844609727,4.3022113360323884,2.738872801422167,693.56861538461533,110.38487351186312,956.66890376948027,143927.06913157762,35631.698502574924,-27768.109300000004,0.33256495885533238,100820.70051242344,25561.870664890703,-38949.135325000003,0.50757415356816604,58610.422132404383,7071.7891229838697,-49897.73146538045,0.86432536763707357,null,332]
["IC/ICD","IC22-200A2AC",3458,19.8,4204,27.6,"NA",3.2,31.6,117.37972567696688,23.7,330,32,1.9202634756559978,1.0025344829393923,1.2576184321923418,null,0.2109704641350211,0.16810692772333058,0.35745290199809704,0.55601127957708152,901.63919999999996,0,-1502.732,0,0,0,0,{"$f":"(Ltorque2+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0.27737643074349544,0.35851761133603238,3.3285171689219455,8.6044226720647767,5.4777456028443341,693.56861538461533,110.38487351186312,956.66890376948027,35772.46349606997,8978.0657644283274,-44954.843200000003,1.0025344829393923,25097.45687486777,6440.7863092637999,-47794.292800000003,1.2576184321923418,14644.361065046493,1781.8681254762507,-50574.716247888791,1.7985246643928328,null,166]
["IC/ICD","IC22-200A6AC",3458,34.299999999999997,4204,47.8,"NA",1.1000000000000001,10.5,67.670118959552596,23.7,330,32,3.3308645450250327,1.9010705114893018,2.3144557749058756,null,0.2109704641350211,0.16810692772333058,0.35745290199809704,0.3158269543974232,901.63919999999996,0,-1502.732,0,0,0,0,0,0.4805056350758532,0.62106838731443992,5.7660676209102384,14.905641295546557,9.4892259685636695,693.56861538461533,110.38487351186312,956.66890376948027,11863.001771209854,3081.4005334122826,-48731.667700000005,1.9010705114893018,8329.7338761404226,2211.1305082853828,-49737.495325000004,2.3144557749058756,4866.2974242547634,611.71769793309159,-50723.443790894671,3.1662908630073496,null,95.7]
["IC/ICD","IC22-250A1AC",4806,9.9,6250,13.8,"NA",15.5,158,281.42849891224591,29.3,330,32,0.80091391195702422,0.18066288670975345,0.36170192229251713,null,0.17064846416382251,0.14455697678357632,0.28735168,1.3849234290262851,1077.5688,0,-1795.9479999999999,0,0,0,0,0,0.11925950584645047,0.15414659800249689,1.4311140701574057,3.6995183520599251,2.3551865311580795,828.8990769230769,131.92338541661687,1143.336006944013,216667.39685043733,52132.61267014152,-16490.252500000002,0.18066288670975345,149948.60546792357,37399.483002492831,-33144.983124999999,0.36170192229251713,83205.924092578483,8897.2483474491546,-49805.677308196937,0.72206158047530622,null,398]
["IC/ICD","IC22-250A2AC",4806,19.7,6250,27.6,"NA",3.9,39.4,140.71424945612296,29.3,330,32,1.6018278239140484,0.77002724350509311,0.99755048886017794,null,0.17064846416382251,0.14455697678357632,0.28735168,0.66363054901333429,1077.5688,0,-1795.9479999999999,0,0,0,0,0,0.23731437021970445,0.30673615966153417,2.8477724426364532,7.3616678318768196,4.6865832993751679,828.8990769230769,131.92338541661687,1143.336006944013,53993.062642965044,13117.238026680769,-42115.382800000007,0.77002724350509311,37220.411305540198,9362.6662726670693,-46378.023325000002,0.99755048886017794,20786.384794125657,2227.3561112235857,-50554.604951076741,1.5068625178373263,null,199]
["IC/ICD","IC22-250A6AC",4806,34.200000000000003,6250,47.8,"NA",1.3,13.1,81.317279836452954,29.3,330,32,2.7718585822512667,1.5163600456161461,1.8709873732948632,null,0.17064846416382251,0.14455697678357632,0.28735168,0.37734171816476586,1077.5688,0,-1795.9479999999999,0,0,0,0,0,0.4119873838331925,0.53250642946317106,4.9438486059983102,12.780154307116105,8.1360989258188194,828.8990769230769,131.92338541661687,1143.336006944013,17950.055551086825,4376.0746627257158,-47909.125300000007,1.5163600456161461,12416.345553637539,3130.9990264690273,-49322.641300000003,1.8709873732948632,6940.9702762502138,744.85724608170813,-50721.256435986332,2.6501177894233021,null,115]
["IC/ICD","IC33-030A1AC",769,9.8000000000000007,945,13.8,"NA",4.7,31,52.67945519839779,7.3,330,32,4.2787078786428943,2.2539061317160538,2.8199063000990288,null,0.68493150684931503,0.32397199855133413,0.68151111111111118,0.2762721803307821,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.26457713215025619,0.34197412223667101,3.1749255858030745,8.2073789336801042,5.2249797084939109,297.2436923076923,47.307802933655616,410.0009587583487,8066.9150325777218,2959.026475352578,-47650.045300000005,2.2539061317160538,5443.805501621322,2101.3376419170481,-49214.0173,2.8199063000990288,3533.7264133383164,1120.3516877256143,-50352.860408381741,3.6196188802024687,null,74.5]
["IC/ICD","IC33-030A3AC",769,29.5,945,41.4,"NA",0.52,3.4,17.53624817342638,7.3,330,32,12.853376490278048,7.3869878885315385,9.0055496033300564,null,0.68493150684931503,0.32397199855133413,0.68151111111111118,8.8913740012223519E-2,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.7964311631053631,1.0294118985695708,9.5571739572643573,24.7058855656697,15.728255244956159,297.2436923076923,47.307802933655616,410.0009587583487,880.42097293380448,326.94221413234482,-50457.568912000002,7.3869878885315385,598.40606017389177,232.96607045662253,-50628.673300000002,9.0055496033300564,390.20752150520298,124.20846845953217,-50754.991738953366,11.246855658782589,null,24.8]
["IC/ICD","IC33-030A5AC",769,17,945,23.9,"NA",1.6,10.3,30.40559159102154,7.3,330,32,7.4131101618347826,4.1253715010892469,5.0734920206202361,null,0.68493150684931503,0.32397199855133413,0.68151111111111118,0.1562281701306423,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.45896033128105668,0.59322041612483745,5.5075239753726803,14.2372899869961,9.0637403106527028,297.2436923076923,47.307802933655616,410.0009587583487,2676.7307389062435,1006.9362434633086,-49708.436800000003,4.1253715010892469,1811.0297938479796,716.23080078980115,-50250.280000000006,5.0734920206202361,1176.5057212435213,381.86646946174039,-50647.429334235618,6.4008942763892867,null,43]
["IC/ICD","IC33-050A1AC",1283,9.8000000000000007,1575,13.8,"NA",6.4,49.5,87.681240867131891,10.4,330,32,2.57067529805561,1.3071291977666926,1.6602632475163881,null,0.48076923076923073,0.24312116482862378,0.51196444444444444,0.43695160066337752,483.8064,0,-806.34400000000005,0,0,0,0,0,0.19854895127670943,0.25663065731358797,2.3825874153205131,6.1591357755261118,3.9210276153964596,372.15876923076922,59.230907738072894,513.33453372996507,21180.412619483417,6706.5069565609183,-44954.843200000003,1.3071291977666926,14492.302184284748,4762.5918966881891,-47854.811200000004,1.6602632475163881,8777.2592166022005,1905.5361579365092,-50332.856663735249,2.2885829883259508,null,124]
["IC/ICD","IC33-050A3AC",1283,29.5,1575,41.4,"NA",0.71,5.5,29.274220741123063,10.4,330,32,7.6996071729201851,4.4584472466138898,5.4234426179876145,null,0.48076923076923073,0.24312116482862378,0.51196444444444444,0.14098437225141805,483.8064,0,-806.34400000000005,0,0,0,0,0,0.59767286353703353,0.77251065211743308,7.1720743624444019,18.540255650818395,11.80309333206077,372.15876923076922,59.230907738072894,513.33453372996507,2356.1369577203786,745.20312051846622,-50157.154573000007,4.4584472466138898,1618.1654083270087,531.00222355784433,-50476.140231250007,5.4234426179876145,978.83352724020131,212.45656963339101,-50752.48923291047,7.0929847332064266,null,41.4]
["IC/ICD","IC33-050A5AC",1283,17,1575,23.9,"NA",2.1,16.5,50.699556211075453,10.4,330,32,4.4457982839455461,2.4796115551434568,3.0497896644407341,null,0.48076923076923073,0.24312116482862378,0.51196444444444444,0.24697179097937505,483.8064,0,-806.34400000000005,0,0,0,0,0,0.34442165017388371,0.44517563003377503,4.1330598020866045,10.684215120810601,6.8017825981367155,372.15876923076922,59.230907738072894,513.33453372996507,7067.0499454917972,2203.6975316609069,-48915.882925000005,2.4796115551434568,4845.4731494496409,1567.4835999261682,-49849.292500000003,3.0497896644407341,2934.6403741473873,627.15780428485311,-50652.141004660523,4.0490454235055182,null,71.7]
["IC/ICD","IC33-075A1AC",1926,9.8000000000000007,2365,13.8,"NA",8.5,73.099999999999994,132.22896808188437,14.4,330,32,1.7046189142186934,0.79680498636305175,1.0493316652059865,null,0.34722222222222221,0.20402066111102382,0.42950697674418598,0.65035195978477112,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.16661687324066946,0.21535745932848738,1.9994024788880336,5.1685790238836971,3.2904196016486944,468.82338461538455,74.6155590986113,646.66817885463115,46909.330526516787,13432.450614230822,-40485.692500000005,0.79680498636305175,32323.613231288979,9538.9866680769592,-45600.9925,1.0493316652059865,19157.355254240025,3202.7825216842853,-50218.479461168106,1.5376289483788781,null,187]
["IC/ICD","IC33-075A3AC",1926,29.5,2365,41.4,"NA",0.94,8.1,43.982041789803255,14.4,330,32,5.1248189221687399,2.9551566928311059,3.5984957013858785,null,0.34722222222222221,0.20402066111102382,0.42950697674418598,0.20795562277548171,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.5015507918979335,0.64826990308065069,6.0186095027752025,15.558477673935617,9.9048345151669874,468.82338461538455,74.6155590986113,646.66817885463115,5185.9799337531922,1482.2935310088349,-49669.318708000006,2.9551566928311059,3585.3745335647945,1056.2236513227203,-50228.445325000001,3.5984957013858785,2120.5367795499974,354.63459245277903,-50740.145321613643,4.8087182575469249,null,62.2]
["IC/ICD","IC33-075A5AC",1926,17,2365,23.9,"NA",2.8,24.4,76.367532368147124,14.4,330,32,2.9515160829527378,1.6047977757964622,1.9909552480708095,null,0.34722222222222221,0.20402066111102382,0.42950697674418598,0.36599215497435061,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.28902926990728378,0.37357926618206988,3.4683512388874052,8.9659023883696776,5.7078707375538569,468.82338461538455,74.6155590986113,646.66817885463115,15665.236805685934,4425.8360468503561,-47446.445200000002,1.6047977757964622,10807.062475872683,3148.0842174249397,-49105.840000000004,1.9909552480708095,6392.852880709037,1056.991634352644,-50613.590844463055,2.7322990026113585,null,108]
["IC/ICD","IC33-100A1AC",2593,9.8000000000000007,3152,13.8,"NA",10.6,96.2,176.06958851545033,18.899999999999999,330,32,1.2801756504373318,0.52919802948911987,0.73941452733858859,null,0.26455026455026459,0.18669130330799383,0.39701903553299495,0.86736983651870669,750.8424,0,-1251.404,0,0,0,0,0,0.15246456436819497,0.197065162617303,1.8295747724183395,4.7295639028152721,3.0109338952081885,577.57107692307693,91.923291879217018,796.66852961988081,81960.493079176464,22304.882133501626,-34756.781199999998,0.52919802948911987,56699.921000441653,15839.698906399706,-42711.869200000001,0.73941452733858859,33426.404102750843,4866.559829303158,-50041.19152942091,1.1529107399141529,null,249]
["IC/ICD","IC33-100A3AC",2593,29.7,3152,41.4,"NA",1.2,10.7,58.619152160364791,18.899999999999999,330,32,3.8451596738105622,2.1838011932991743,2.6618223933896044,null,0.26455026455026459,0.18669130330799383,0.39701903553299495,0.27607255109313877,750.8424,0,-1251.404,0,0,0,0,0,0.46206097568728471,0.59722809487080608,5.5447317082474168,14.333474276899345,9.1249731313962439,577.57107692307693,91.923291879217018,796.66852961988081,9110.2043417985533,2522.0387299849303,-48954.083200000001,2.1838011932991743,6356.3303701411269,1809.2886541196237,-49852.502800000002,2.6618223933896044,3711.851058946248,555.88250356167134,-50715.233654579402,3.6222362420327308,null,82.9]
["IC/ICD","IC33-100A5AC",2593,17.100000000000001,3152,23.9,"NA",3.5,32.1,101.82337649086284,18.899999999999999,330,32,2.2136370622145529,1.1620991712082529,1.4557656519542694,null,0.26455026455026459,0.18669130330799383,0.39701903553299495,0.48680651931387053,750.8424,0,-1251.404,0,0,0,0,0,0.26603510721389123,0.34385860007713082,3.1924212865666948,8.2526064018511391,5.253772408985717,577.57107692307693,91.923291879217018,796.66852961988081,27386.720668077884,7376.3934114172625,-45557.168125000004,1.1620991712082529,19080.109575379727,5277.6705998006364,-48118.643125000002,1.4557656519542694,11190.382043633021,1621.5017649677004,-50551.565480922713,2.0542042070624897,null,144]
["IC/ICD","IC33-150A1AC",3849,9.8000000000000007,4724,13.8,"NA",14.9,143,263.7508293825822,27.3,330,32,0.85459446905870151,0.21957399744919212,0.40926486074954671,null,0.18315018315018314,0.1699743208650335,0.35800762066045722,1.3198395638641611,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,0.13881236203977737,0.17941926907421837,1.6657483444773284,4.3060624577812412,2.7413245016732821,780.56676923076918,124.23105973634766,1076.6691843816798,182167.84482433071,46966.675544957936,-19095.471699999998,0.21957399744919212,126351.02193304306,33353.146401491867,-34813.779699999999,0.40926486074954671,74007.885709566515,9329.7752488067053,-49553.879444641359,0.75766784644055474,null,373]
["IC/ICD","IC33-150A3AC",3849,29.3,4724,41.4,"NA",1.7,15.9,87.681240867131891,27.3,330,32,2.57067529805561,1.3997241069914241,1.741664626599972,null,0.18315018315018314,0.1699743208650335,0.35800762066045722,0.41238779007279669,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,0.41502063344545675,0.53642699835455088,4.9802476013454813,12.874247960509221,8.1960008060231786,780.56676923076918,124.23105973634766,1076.6691843816798,20216.987453926915,5344.2477310094819,-47090.151700000002,1.3997241069914241,13963.531773974722,3782.2816067289327,-48944.382925000005,1.741664626599972,8179.04272026536,1058.0062490565522,-50659.559424682273,2.4249020559592105,null,124]
["IC/ICD","IC33-150A5AC",3849,16.98,4724,23.9,"NA",5,47.7,152.02795795510769,27.3,330,32,1.4826220323669566,0.69344413789828296,0.91432014006745876,null,0.18315018315018314,0.1699743208650335,0.35800762066045722,0.7304346897510684,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,0.24051366402402241,0.31087134580410491,2.8861639682882689,7.460912299298518,4.7497642896339105,780.56676923076918,124.23105973634766,1076.6691843816798,60692.225496521693,15733.378804114196,-40094.972500000003,0.69344413789828296,42081.008056664505,11177.940254973182,-45399.152500000004,0.91432014006745876,24596.732433360859,3126.7715815508236,-50382.155109867228,1.3690477930898919,null,215]
["IC/ICD","IC33-200A1AC",5135,9.8000000000000007,6306,13.8,"NA",19.100000000000001,190,351.43207024971412,35.700000000000003,330,32,0.64137572828751632,0,0.22741820713366995,null,0.14005602240896359,0.16053978043649464,0.33794037424674916,1.7933380501965821,1278.6312,0,-2131.0520000000001,0,0,0,0,0,0.13110748735647063,0.16946048036351835,1.5732898482776476,4.0670515287244404,2.5891654184237773,983.56246153846166,156.53882759347835,1356.6698391434791,322290.78530286765,80220.33592054667,1300.6523000000088,-1.743471654066453E-2,223753.58023780407,56968.064639228789,-24527.895699999994,0.22741820713366995,130502.07949714675,15050.994175349144,-48970.956180168389,0.55761935118165928,null,497]
["IC/ICD","IC33-200A3AC",5135,29.5,6306,41.4,"NA",2.1,21.1,117.37972567696688,35.700000000000003,330,32,1.9202634756559978,1.0056529520575062,1.2647911632631224,null,0.14005602240896359,0.16053978043649464,0.33794037424674916,0.55308885998981283,1278.6312,0,-2131.0520000000001,0,0,0,0,0,0.39466029357304927,0.51011062966569298,4.7359235228765915,12.242655111976632,7.7939163105613698,983.56246153846166,156.53882759347835,1356.6698391434791,35842.121294105455,8837.7834868591326,-45136.237300000008,1.0056529520575062,24980.887789793967,6297.4544169648416,-47926.808125000003,1.2647911632631224,14559.983213419406,1663.7909388270853,-50604.24547770917,1.8080277372037807,null,166]
["IC/ICD","IC33-200A5AC",5135,17,6306,23.9,"NA",6.4,63.3,202.93964620053913,35.700000000000003,330,32,1.110675041668626,0.44527712138734632,0.63215959597539939,null,0.14005602240896359,0.16053978043649464,0.33794037424674916,0.98293715350017563,1278.6312,0,-2131.0520000000001,0,0,0,0,0,0.22743135561836739,0.29396205777345019,2.7291762674204088,7.0550893865628046,4.4914093993065523,983.56246153846166,156.53882759347835,1356.6698391434791,107364.11943082322,26882.855988276242,-33257.588800000005,0.44527712138734632,74667.649831949559,19121.696728062601,-41927.08,0.63215959597539939,43521.688552834094,5051.9628479476296,-50185.452862192258,1.0173590411544264,null,287]
["IC/ICD","IC33-250A1AC",7216,9.8000000000000007,9375,13.8,"NA",23.2,237,421.43564158718232,44.1,330,32,0.53483848483036178,{"$error":"#NUM!"},0.102668210374063,null,0.11337868480725623,0.13782045233831569,0.27422677333333334,2.1524558381724486,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,0.1125533694096245,0.1454787093495935,1.350640432915494,3.4914890243902441,2.222750947931226,1186.5581538461538,188.84659545060902,1636.6704939052781,486905.14291348396,116850.06677136988,26071.659200000009,{"$error":"#NUM!"},333588.34869465977,82980.482199958307,-12035.732799999998,0.102668210374063,185632.15563797843,18820.912803035466,-48810.729801250709,0.46458560601598869,null,596]
["IC/ICD","IC33-250A3AC",7216,29.6,9375,41.4,"NA",2.6,26.3,140.71424945612296,44.1,330,32,1.6018278239140484,0.76949297240833037,0.99595491293383465,null,0.11337868480725623,0.13782045233831569,0.27422677333333334,0.6611545854279185,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,0.33995711576784537,0.43940508130081302,4.0794853892141445,10.545721951219512,6.713615108037172,1186.5581538461538,188.84659545060902,1636.6704939052781,54079.900862334194,13117.238026680767,-42115.382800000007,0.76949297240833037,37323.80267890892,9378.5083475785214,-46363.0288,0.99595491293383465,20701.95783852696,2127.1518693633748,-50576.641776958357,1.5125055804502525,null,199]
["IC/ICD","IC33-250A5AC",7216,17.100000000000001,9375,23.9,"NA",7.7,78.8,243.24473272817232,44.1,330,32,0.92663877022934782,0.29421228985166376,0.47074067845208389,null,0.11337868480725623,0.13782045233831569,0.27422677333333334,1.1753718244205325,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,0.19639414458209989,0.25384550304878051,2.3567297349851986,6.0922920731707322,3.8784735928187719,1186.5581538461538,188.84659545060902,1636.6704939052781,161725.93797147687,38767.045373337387,-25404.879325000005,0.29421228985166376,111668.7731696566,27737.091041174452,-37802.418325000006,0.47074067845208389,61868.816984658704,6291.0862657780835,-50136.255078362265,0.85079459897127263,null,344]
["IC/ICD","IC44-030A1AC",1036,9.9,1260,13.8,"NA",6.2,41.3,70.28641404994282,9.6,330,32,3.2068786414375818,1.6056766703082586,2.0327009182585072,null,0.52083333333333337,0.28544458176658577,0.60671111111111109,0.36390967818791081,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.23549177995743328,0.3043804054054054,2.8259013594891993,7.30512972972973,4.6505900256561921,352.82584615384616,56.153977465965212,486.66780470503181,14332.639251475019,5208.0218084543385,-45314.774799999999,1.6056766703082586,9774.0118170398364,3736.1895582389825,-47979.5317,2.0327009182585072,6006.867629173471,1755.0995852027297,-50181.625117874493,2.7479346110812513,null,99.4]
["IC/ICD","IC44-030A3AC",1201,19.7,1500,27.6,"NA",1.6,10.3,35.14320702497141,9.6,330,32,6.4137572828751637,3.5334006738954167,4.3495347315576778,null,0.52083333333333337,0.24622863173204232,0.50963733333333339,0.17188195691389618,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.40422533709343611,0.52247374410213709,4.8507040451212333,12.539369858451289,7.9828107849201713,352.82584615384616,56.153977465965212,486.66780470503181,3571.8025631890559,1344.0056279882162,-49342.580800000003,3.5334006738954167,2425.5410127836067,959.30836490463264,-50060.027200000004,4.3495347315576778,1430.5271755281185,388.72980514846887,-50682.807485386555,5.8179463275540169,null,226]
["IC/ICD","IC44-030A5AC",1201,39.5,1500,55.2,"NA",0.39,2.6,17.53624817342638,9.6,330,32,12.853376490278048,7.2958743776074684,8.902638759161162,null,0.52083333333333337,0.24622863173204232,0.50963733333333339,8.485924824917522E-2,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.81050257945130599,1.0475996391895641,9.7260309534156715,25.142391340549541,16.0061434519973,352.82584615384616,56.153977465965212,486.66780470503181,903.10793956670818,326.94221413234487,-50457.568912000002,7.2958743776074684,612.49337833075901,233.95321482296416,-50627.174481250004,8.902638759161162,357.59732813389377,94.802246012969746,-50775.934369637413,11.784219406041219,null,210.02857142857101]
["IC/ICD","IC44-050A1AC",1990,9.8000000000000007,2500,13.8,"NA",8.5,66.099999999999994,117.37972567696688,13.9,330,32,1.9202634756559978,0.8887687423621522,1.1732354150120528,null,0.35971223021582732,0.19237003816419268,0.39584159999999996,0.57337430453975557,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.15710219783409071,0.20305944723618088,1.8852263740090884,4.8734267336683414,3.1025198178380249,456.74030769230768,72.692477678543995,630.00147321404791,37837.252786929144,11923.993593381372,-40485.692500000005,0.8887687423621522,25911.22115971789,8467.7635663143064,-45600.9925,1.1732354150120528,14994.054645237873,2680.7555384956049,-50283.571216637043,1.7440614134299139,null,194.057142857142]
["IC/ICD","IC44-050A3AC",1990,19.600000000000001,2500,27.6,"NA",2.1,16.5,58.619152160364791,13.9,330,32,3.8451596738105622,2.1119011231710751,2.6120219873606629,null,0.35971223021582732,0.19237003816419268,0.39584159999999996,0.27824027466977813,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.31420439566818142,0.40611889447236177,3.7704527480181769,9.7468534673366829,6.2050396356760498,456.74030769230768,72.692477678543995,630.00147321404791,9432.8328308815198,2942.378518315752,-48285.638800000001,2.1119011231710751,6460.3393041265554,2089.5151796735049,-49534.550800000005,2.6120219873606629,3739.2994973265295,661.50635251126835,-50677.812925418373,3.5940160035667827,null,178.085714285714]
["IC/ICD","IC44-050A5AC",1990,39.1,2500,55.2,"NA",0.53,4.0999999999999996,29.274220741123063,13.9,330,32,7.6996071729201851,4.4760972491994302,5.4552110998106089,null,0.35971223021582732,0.19237003816419268,0.39584159999999996,0.1370935862537698,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.62680570768499455,0.81016575376884414,7.5216684922199342,19.443978090452259,12.378420905863956,456.74030769230768,72.692477678543995,630.00147321404791,2338.0204236858522,741.70451431884908,-50163.224848000005,4.4760972491994302,1600.0714625784915,525.3740309758515,-50483.077953250002,5.4552110998106089,931.45649828598266,166.32483090612527,-50772.879259053945,7.2942872626362707,null,162.11428571428499]
["IC/ICD","IC44-075A1AC",2980,9.8000000000000007,3750,13.8,"NA",11.3,97.3,176.06958851545033,19.2,330,32,1.2801756504373318,0.49901837300961588,0.71748366992117263,null,0.26041666666666669,0.16448557043271178,0.3378965333333333,0.85731165555172251,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.13432988252004796,0.17362552572706935,1.6119585902405755,4.1670126174496644,2.6528026239736446,584.82092307692312,93.077140731257387,806.66855300423072,83132.561246121477,23777.846047978146,-32567.1973,0.49901837300961588,57291.001796248209,16885.716758709121,-41607.649300000005,0.71748366992117263,32926.944940008725,4570.8646658346224,-50131.209457480516,1.1664369585135881,null,146.142857142857]
["IC/ICD","IC44-075A3AC",2980,19.5,3750,27.6,"NA",2.8,24.3,87.681240867131891,19.2,330,32,2.57067529805561,1.3611129398636566,1.7102814768502401,null,0.26041666666666669,0.16448557043271178,0.3378965333333333,0.41273950696011613,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.26728905195315661,0.34547936241610738,3.2074686234378795,8.2915046979865767,5.2785358334169459,584.82092307692312,93.077140731257387,806.66855300423072,20694.239735012779,5868.1935869908029,-46326.011200000001,1.3611129398636566,14180.363289275636,4146.0063386348065,-48569.29,1.7102814768502401,8163.7299995357371,1122.2996422593651,-50641.325909597363,2.4228356702878751,null,130.17142857142801]
["IC/ICD","IC44-075A5AC",2980,39.1,3750,55.2,"NA",0.71,6.1,43.982041789803255,19.2,330,32,5.1248189221687399,2.9464321017218764,3.6012212998350299,null,0.26041666666666669,0.16448557043271178,0.3378965333333333,0.20403895466406491,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.53594881699325259,0.69273041387024603,6.4313858039190306,16.625529932885904,10.584141081364235,584.82092307692312,93.077140731257387,806.66855300423072,5212.7968093605332,1492.8062510869117,-49653.150352000004,2.9464321017218764,3579.3000310854059,1057.404427853229,-50227.155159250004,3.6012212998350299,2054.9491111354168,286.23318783779558,-50762.806510158196,4.9010249128477756,null,114.2]
["IC/ICD","IC44-100A1AC",4015,9.9,5000,13.8,"NA",14.1,128,234.05234457274722,25,330,32,0.96303243794228288,0.27998195513753343,0.4743201928583759,null,0.2,0.15134372134129692,0.31415999999999999,1.1479014427734966,942.48,0,-1570.8,0,0,0,0,0,0.12485857010656996,0.16138356164383563,1.4983028412788395,3.873205479452055,2.4657591906616361,724.98461538461538,115.38488520403808,1000.0023384349968,144999.73818288595,39440.446845974628,-22409.127700000001,0.27998195513753343,101211.85651283685,28294.233606894839,-36191.133925000002,0.4743201928583759,57660.830371723016,7047.1481372654825,-49898.591113834955,0.87115492910598213,null,98.228571428571499]
["IC/ICD","IC44-100A3AC",4015,19.8,5000,27.6,"NA",3.5,32.1,117.37972567696688,25,330,32,1.9202634756559978,0.96953997513151646,1.2303193896271591,null,0.2,0.15134372134129692,0.31415999999999999,0.55308350951949459,942.48,0,-1570.8,0,0,0,0,0,0.24971714021313993,0.32276712328767126,2.996605682557679,7.7464109589041099,4.9315183813232721,724.98461538461538,115.38488520403808,1000.0023384349968,36473.997367194221,9819.7594298434815,-43806.490000000005,0.96953997513151646,25458.501480564511,7044.6100257572807,-47203.292500000003,1.2303193896271591,14502.590141193143,1754.5769611755677,-50581.721161802292,1.8080452278694323,null,82.257142857142497]
["IC/ICD","IC44-030A2AC",1036,19.7,1260,27.6,"NA",1.6,10.3,35.14,9.6,330,32,6.4143426294820713,3.5335228328548327,4.3497453149001721,null,0.52083333333333337,0.28544458176658577,0.60671111111111109,0.17647050476742776,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.4686048550668116,0.60568626126126124,5.6232582608017392,14.53647027027027,9.2542043944875729,352.82584615384616,56.153977465965212,486.66780470503181,3571.5771631890557,1343.8829795455854,-49342.580800000003,3.5335228328548327,2425.3156127836073,959.22082235681273,-50060.027200000004,4.3497453149001721,1497.5278235133028,450.60028170245687,-50640.730625968092,5.6666693469138654,null,49.7]
["IC/ICD","IC44-030A3AC",1036,39.5,1260,55.2,"NA",0.39,2.6,17.54,9.6,330,32,{"$f":"IF(G335=\"NA\",(UAC_V*0.98)/J335,(IF((UAC_V*0.98)/J335<G335,(UAC_V*0.98)/J335,G335)))","v":12.850627137970354},{"$f":"IF(AO335<G335,IF(AO335<0,0,AO335),G335)","v":7.2953179451804466},{"$f":"IF(AS335<G335,IF(AS335<0,0,AS335),G335)","v":8.9016625925069626},null,{"$f":"IF(move1,Gewicht/K335,MAX(Gewicht,Gewicht2)/K335)","v":0.52083333333333337},{"$f":"IF(move1,IF(AccType=1,SQRT((V335^2*Ltime1+W335^2*Ltime2+X335^2*Ltime3+Y335^2*Ltime4)/ltime)/C335,SQRT((((V335-W335)*2/PI()+W335)^2*Ltime1+W335^2*Ltime2+((X335-W335)*2/PI()+W335)^2*Ltime3+Y335^2*Ltime4)/ltime)/C335),IF(AccType=1,SQRT((V335^2*Ltime1+W335^2*Ltime2+X335^2*Ltime3+Y335^2*Ltime4+Z335^2*Ltime5+AA335^2*Ltime6+AB335^2*Ltime7+AC335^2*Ltime8)/ltime)/C335,SQRT((((V335-W335)*2/PI()+W335)^2*Ltime1+W335^2*Ltime2+((X335-W335)*2/PI()+W335)^2*Ltime3+Y335^2*Ltime4+((Z335-AA335)*2/PI()+AA335)^2*Ltime5+AA335^2*Ltime6+((AB335-AA335)*2/PI()+AA335)^2*Ltime7+AC335^2*Ltime8)/ltime)/C335))","v":0.28544458176658577},{"$f":" IF(move1,MAX(ABS(V335),ABS(X335))/E335,MAX(ABS(V335),ABS(X335),ABS(Z335),ABS(AB335))/E335)","v":0.60671111111111109},{"$f":"IF(AW335>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW335,G335),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW335,G335)),\"NA\")","v":8.7030592412122507E-2},{"$f":"((Gewicht+K335)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":458.67360000000002},0,{"$f":"((Gewicht+K335)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-764.45600000000002},0,{"$f":"((Gewicht2+K335)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K335)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF335/Irms","v":0.93958841498167811},{"$f":"AG335/Ipeak","v":1.2144470720720719},{"$f":"D335*S335","v":11.275060979780138},{"$f":"IF(move1,IF(MAX(ABS(V335),ABS(X335))<=C335,MAX(ABS(V335),ABS(X335))/C335*D335,D335+(MAX(ABS(V335),ABS(X335))-C335)/(E335-C335)*(F335-D335)),IF(MAX(ABS(V335),ABS(X335),ABS(Z335),ABS(AB335))<=C335,MAX(ABS(V335),ABS(X335),ABS(Z335),ABS(AB335))/C335*D335,D335+(MAX(ABS(V335),ABS(X335),ABS(Z335),ABS(AB335))-C335)/(E335-C335)*(F335-D335)))","v":29.146729729729728},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V335),ABS(X335))<=C335,MAX(ABS(V335),ABS(X335))/C335*D335,D335+(MAX(ABS(V335),ABS(X335))-C335)/(E335-C335)*(F335-D335)),IF(MAX(ABS(V335),ABS(X335),ABS(Z335),ABS(AB335))<=C335,MAX(ABS(V335),ABS(X335),ABS(Z335),ABS(AB335))/C335*D335,D335+(MAX(ABS(V335),ABS(X335),ABS(Z335),ABS(AB335))-C335)/(E335-C335)*(F335-D335))),IF(move1,IF(MAX(ABS((V335-W335)*2/PI()+W335),ABS((X335-W335)*2/PI()+W335))<=C335,MAX(ABS((V335-W335)*2/PI()+W335),ABS((X335-W335)*2/PI()+W335))/C335*D335,D335+(MAX(ABS((V335-W335)*2/PI()+W335),ABS((X335-W335)*2/PI()+W335))-C335)/(E335-C335)*(F335-D335)),IF(MAX(ABS((V335-W335)*2/PI()+W335),ABS((X335-W335)*2/PI()+W335),ABS((Z335-AA335)*2/PI()+AA335),ABS((AB335-AA335)*2/PI()+AA335))<=C335,MAX(ABS((V335-W335)*2/PI()+W335),ABS((X335-W335)*2/PI()+W335),ABS((Z335-AA335)*2/PI()+AA335),ABS((AB335-AA335)*2/PI()+AA335))/C335*D335,D335+(MAX(ABS((V335-W335)*2/PI()+W335),ABS((X335-W335)*2/PI()+W335),ABS((Z335-AA335)*2/PI()+AA335),ABS((AB335-AA335)*2/PI()+AA335))-C335)/(E335-C335)*(F335-D335))))","v":18.555384445799959},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V335)+Ltime2*ABS(Lspeed2)*ABS(W335)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X335)+Ltime4*ABS(Lspeed1)*ABS(Y335))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V335)+Ltime2*ABS(Lspeed2)*ABS(W335)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X335)+Ltime4*ABS(Lspeed1)*ABS(Y335)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z335)+Ltime6*ABS(Lspeed6)*ABS(AA335)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB335)+Ltime8*ABS(Lspeed1)*ABS(AC335))/ltime)","v":352.82584615384616},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK335/2*Ltime1/ltime,AK335/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X335*-ABS(Lspeed2-Lspeed1),((X335-Y335)*2/PI()+Y335)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V335*-ABS(Lspeed2-Lspeed1),((V335-W335)*2/PI()+W335)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X335*-ABS(Lspeed2-Lspeed1),((X335-Y335)*2/PI()+Y335)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V335*-ABS(Lspeed2-Lspeed1),((V335-W335)*2/PI()+W335)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB335*-ABS(Lspeed6-Lspeed1),((AB335-AC335)*2/PI()+AB335)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z335*-ABS(Lspeed6-Lspeed1),((Z335-AA335)*2/PI()+AA335)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB335*-ABS(Lspeed6-Lspeed1),((AB335-AC335)*2/PI()+AB335)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z335*-ABS(Lspeed6-Lspeed1),((Z335-AA335)*2/PI()+AA335)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":56.153977465965212},{"$f":"IF(move1,MAX(IF(AccType=1,X335*-ABS(Lspeed2-Lspeed1),((X335-Y335)*2/PI()+Y335)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V335*-ABS(Lspeed2-Lspeed1),((V335-W335)*2/PI()+W335)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X335*-ABS(Lspeed2-Lspeed1),((X335-Y335)*2/PI()+Y335)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V335*-ABS(Lspeed2-Lspeed1),((V335-W335)*2/PI()+W335)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB335*-ABS(Lspeed6-Lspeed1),((AB335-AC335)*2/PI()+AB335)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z335*-ABS(Lspeed6-Lspeed1),((Z335-AA335)*2/PI()+AA335)*-ABS(Lspeed6-Lspeed1)),0))","v":486.66780470503181},{"$f":"(J335^2)+3*(I335/1000)^2*(F335/2)^2*(2000*PI()/M335)^2","v":903.23953956670812},{"$f":"SQRT(3)*H335*F335/2*J335","v":327.0121624174563},{"$f":"3*F335^2*H335^2/4-(UAC_V*0.98)^2","v":-50457.568912000002},{"$f":"-AM335/2/AL335+SQRT((AM335/2/AL335)^2-AN335/AL335)","v":7.2953179451804466},{"$f":"(J335^2)+3*(I335/1000)^2*(D335/2)^2*(2000*PI()/M335)^2","v":612.62497833075895},{"$f":"SQRT(3)*H335*D335/2*J335","v":234.00326839654932},{"$f":"3*D335^2*H335^2/4-(UAC_V*0.98)^2","v":-50627.174481250004},{"$f":"-AQ335/2/AP335+SQRT((AQ335/2/AP335)^2-AR335/AP335)","v":8.9016625925069626},{"$f":"(J335^2)+3*(I335/1000)^2*(AH335/2)^2*(2000*PI()/M335)^2","v":374.95045155414385},{"$f":"SQRT(3)*H335*AH335/2*J335","v":109.92457232080213},{"$f":"3*AH335^2*H335^2/4-(UAC_V*0.98)^2","v":-50765.883716047923},{"$f":"IF((AU335/2/AT335)^2-AV335/AT335>=0,-AU335/2/AT335+SQRT((AU335/2/AT335)^2-AV335/AT335),-9999)","v":11.490212490621973},null,24.8]
["IC/ICD","IC44-050A1AC",1711,9.8000000000000007,2101,13.8,"NA",8.5,66.099999999999994,117.39,13.9,330,32,1.9200954084675015,0.88873296590270068,1.173174932161559,null,0.35971223021582732,0.22373838453930067,0.47101570680628269,0.58687390484182977,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.18271968070709554,0.23617083576855638,2.1926361684851465,5.6681000584453534,3.6084245689641556,456.74030769230768,72.692477678543995,630.00147321404791,37839.664886929146,11925.037308224943,-40485.692500000005,0.88873296590270068,25913.633259717892,8468.5047551162625,-45600.9925,1.173174932161559,15425.386807476567,3118.1592470154392,-50099.599308549572,1.7039435417894635,null,166]
["IC/ICD","IC44-050A2AC",1711,19.600000000000001,2101,27.6,"NA",2.1,16.5,58.62,13.9,330,32,3.8451040600477655,2.1118886605954432,2.6120008620038924,null,0.35971223021582732,0.22373838453930067,0.47101570680628269,0.28331902905036982,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.36543936141419109,0.47234167153711276,4.3852723369702931,11.336200116890707,7.2168491379283113,456.74030769230768,72.692477678543995,630.00147321404791,9432.932230881519,2942.4210754841461,-48285.638800000001,2.1118886605954432,6460.4387041265545,2089.5454014307702,-49534.550800000005,2.6120008620038924,3846.3047104547459,769.38438413151641,-50632.895770281175,3.5295899585418073,null,82.9]
["IC/ICD","IC44-050A3AC",1711,39.1,2101,55.2,"NA",0.53,4.0999999999999996,29.27,13.9,330,32,7.7007174581482749,4.4763477951061628,5.4556430480162943,null,0.35971223021582732,0.22373838453930067,0.47101570680628269,0.13925845686654101,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.72901423629055462,0.9422734365867913,8.7481708354866559,22.614562478082991,14.39687761698964,456.74030769230768,72.692477678543995,630.00147321404791,2337.7733236858521,741.59757576795027,-50163.224848000005,4.4763477951061628,1599.8243625784917,525.29828283563143,-50483.077953250002,5.4556430480162943,957.47833645026662,193.41828875701779,-50761.493374817648,7.1808924391453983,null,41.4]
["IC/ICD","IC44-075A1AC",2568,9.8000000000000007,3154,13.8,"NA",11.3,97.3,176.07,19.2,330,32,1.2801726586016926,0.4990177752108203,0.71748263148015523,null,0.26041666666666669,0.19087499995696303,0.4017476220672162,0.87540401294263526,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.15588124996485314,0.20148133437175494,1.8705749995782377,4.8355520249221184,3.078408029377516,584.82092307692312,93.077140731257387,806.66855300423072,83132.706146121491,23777.901618144213,-32567.1973,0.4990177752108203,57291.146696248208,16885.756221580672,-41607.649300000005,0.71748263148015523,33594.818827922725,5304.2089321046215,-49897.610093016665,1.1423296960206297,null,249]
["IC/ICD","IC44-075A2AC",2568,19.5,3154,27.6,"NA",2.8,24.3,87.68,19.2,330,32,2.5707116788321165,1.3611212381072728,1.7102954719155246,null,0.26041666666666669,0.19087499995696303,0.4017476220672162,0.41883967063682459,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.31017187493006493,0.40090673676012462,3.7220624991607791,9.6217616822429903,6.1254037319246484,584.82092307692312,93.077140731257387,806.66855300423072,20694.022135012779,5868.1105401671766,-46326.011200000001,1.3611212381072728,14180.145689275636,4145.9476642485488,-48569.29,1.7102954719155246,8328.4061395607641,1302.3386305103763,-50584.539043231038,2.3875484346541254,null,124]
["IC/ICD","IC44-075A3AC",2568,39.1,3154,55.2,"NA",0.71,6.1,43.98,19.2,330,32,5.1250568440200093,2.9464868476529933,3.6013146805043466,null,0.26041666666666669,0.19087499995696303,0.4017476220672162,0.2065542403129427,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.62193437485977121,0.80386940550363439,7.4632124983172545,19.292865732087225,12.282219790679681,584.82092307692312,93.077140731257387,806.66855300423072,5212.6172093605328,1492.7369501527653,-49653.150352000004,2.9464868476529933,3579.1204310854059,1057.355339691542,-50227.155159250004,3.6013146805043466,2096.546350805831,332.1399150624116,-50748.126281141856,4.8413433608767216,null,62.2]
["IC/ICD","IC44-100A1AC",3457,9.9,4202,13.8,"NA",14.1,128,234.05,25,330,32,0.96304208502456734,0.27998358527175315,0.47432326069040975,null,0.2,0.17577235787830695,0.37382198952879581,1.1734009207467111,942.48,0,-1570.8,0,0,0,0,0,0.14501219524960324,0.18743274515475847,1.7401463429952388,4.498385883714203,2.8637613973116771,724.98461538461538,115.38488520403808,1000.0023384349968,144998.64068288595,39440.051759153423,-22409.127700000001,0.27998358527175315,101210.75901283688,28293.950175044843,-36191.133925000002,0.47432326069040975,58664.613807289454,8184.5578069447874,-49582.310106826728,0.85222363671202439,null,331]
["IC/ICD","IC44-100A2AC",3457,19.8,4202,27.5,"NA",3.5,32.1,117.38,25,330,32,{"$f":"IF(G343=\"NA\",(UAC_V*0.98)/J343,(IF((UAC_V*0.98)/J343<G343,(UAC_V*0.98)/J343,G343)))","v":1.9202589879025389},{"$f":"IF(AO343<G343,IF(AO343<0,0,AO343),G343)","v":0.97252069729330926},{"$f":"IF(AS343<G343,IF(AS343<0,0,AS343),G343)","v":1.2303177001632162},null,{"$f":"IF(move1,Gewicht/K343,MAX(Gewicht,Gewicht2)/K343)","v":0.2},{"$f":"IF(move1,IF(AccType=1,SQRT((V343^2*Ltime1+W343^2*Ltime2+X343^2*Ltime3+Y343^2*Ltime4)/ltime)/C343,SQRT((((V343-W343)*2/PI()+W343)^2*Ltime1+W343^2*Ltime2+((X343-W343)*2/PI()+W343)^2*Ltime3+Y343^2*Ltime4)/ltime)/C343),IF(AccType=1,SQRT((V343^2*Ltime1+W343^2*Ltime2+X343^2*Ltime3+Y343^2*Ltime4+Z343^2*Ltime5+AA343^2*Ltime6+AB343^2*Ltime7+AC343^2*Ltime8)/ltime)/C343,SQRT((((V343-W343)*2/PI()+W343)^2*Ltime1+W343^2*Ltime2+((X343-W343)*2/PI()+W343)^2*Ltime3+Y343^2*Ltime4+((Z343-AA343)*2/PI()+AA343)^2*Ltime5+AA343^2*Ltime6+((AB343-AA343)*2/PI()+AA343)^2*Ltime7+AC343^2*Ltime8)/ltime)/C343))","v":0.17577235787830695},{"$f":" IF(move1,MAX(ABS(V343),ABS(X343))/E343,MAX(ABS(V343),ABS(X343),ABS(Z343),ABS(AB343))/E343)","v":0.37382198952879581},{"$f":"IF(AW343>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW343,G343),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW343,G343)),\"NA\")","v":0.56107416086448691},{"$f":"((Gewicht+K343)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":942.48},0,{"$f":"((Gewicht+K343)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-1570.8},0,{"$f":"((Gewicht2+K343)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K343)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF343/Irms","v":0.29002439049920647},{"$f":"AG343/Ipeak","v":0.37486549030951694},{"$f":"D343*S343","v":3.4802926859904777},{"$f":"IF(move1,IF(MAX(ABS(V343),ABS(X343))<=C343,MAX(ABS(V343),ABS(X343))/C343*D343,D343+(MAX(ABS(V343),ABS(X343))-C343)/(E343-C343)*(F343-D343)),IF(MAX(ABS(V343),ABS(X343),ABS(Z343),ABS(AB343))<=C343,MAX(ABS(V343),ABS(X343),ABS(Z343),ABS(AB343))/C343*D343,D343+(MAX(ABS(V343),ABS(X343),ABS(Z343),ABS(AB343))-C343)/(E343-C343)*(F343-D343)))","v":8.996771767428406},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V343),ABS(X343))<=C343,MAX(ABS(V343),ABS(X343))/C343*D343,D343+(MAX(ABS(V343),ABS(X343))-C343)/(E343-C343)*(F343-D343)),IF(MAX(ABS(V343),ABS(X343),ABS(Z343),ABS(AB343))<=C343,MAX(ABS(V343),ABS(X343),ABS(Z343),ABS(AB343))/C343*D343,D343+(MAX(ABS(V343),ABS(X343),ABS(Z343),ABS(AB343))-C343)/(E343-C343)*(F343-D343))),IF(move1,IF(MAX(ABS((V343-W343)*2/PI()+W343),ABS((X343-W343)*2/PI()+W343))<=C343,MAX(ABS((V343-W343)*2/PI()+W343),ABS((X343-W343)*2/PI()+W343))/C343*D343,D343+(MAX(ABS((V343-W343)*2/PI()+W343),ABS((X343-W343)*2/PI()+W343))-C343)/(E343-C343)*(F343-D343)),IF(MAX(ABS((V343-W343)*2/PI()+W343),ABS((X343-W343)*2/PI()+W343),ABS((Z343-AA343)*2/PI()+AA343),ABS((AB343-AA343)*2/PI()+AA343))<=C343,MAX(ABS((V343-W343)*2/PI()+W343),ABS((X343-W343)*2/PI()+W343),ABS((Z343-AA343)*2/PI()+AA343),ABS((AB343-AA343)*2/PI()+AA343))/C343*D343,D343+(MAX(ABS((V343-W343)*2/PI()+W343),ABS((X343-W343)*2/PI()+W343),ABS((Z343-AA343)*2/PI()+AA343),ABS((AB343-AA343)*2/PI()+AA343))-C343)/(E343-C343)*(F343-D343))))","v":5.7275227946233542},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V343)+Ltime2*ABS(Lspeed2)*ABS(W343)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X343)+Ltime4*ABS(Lspeed1)*ABS(Y343))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V343)+Ltime2*ABS(Lspeed2)*ABS(W343)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X343)+Ltime4*ABS(Lspeed1)*ABS(Y343)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z343)+Ltime6*ABS(Lspeed6)*ABS(AA343)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB343)+Ltime8*ABS(Lspeed1)*ABS(AC343))/ltime)","v":724.98461538461538},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK343/2*Ltime1/ltime,AK343/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X343*-ABS(Lspeed2-Lspeed1),((X343-Y343)*2/PI()+Y343)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V343*-ABS(Lspeed2-Lspeed1),((V343-W343)*2/PI()+W343)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X343*-ABS(Lspeed2-Lspeed1),((X343-Y343)*2/PI()+Y343)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V343*-ABS(Lspeed2-Lspeed1),((V343-W343)*2/PI()+W343)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB343*-ABS(Lspeed6-Lspeed1),((AB343-AC343)*2/PI()+AB343)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z343*-ABS(Lspeed6-Lspeed1),((Z343-AA343)*2/PI()+AA343)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB343*-ABS(Lspeed6-Lspeed1),((AB343-AC343)*2/PI()+AB343)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z343*-ABS(Lspeed6-Lspeed1),((Z343-AA343)*2/PI()+AA343)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":115.38488520403808},{"$f":"IF(move1,MAX(IF(AccType=1,X343*-ABS(Lspeed2-Lspeed1),((X343-Y343)*2/PI()+Y343)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V343*-ABS(Lspeed2-Lspeed1),((V343-W343)*2/PI()+W343)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X343*-ABS(Lspeed2-Lspeed1),((X343-Y343)*2/PI()+Y343)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V343*-ABS(Lspeed2-Lspeed1),((V343-W343)*2/PI()+W343)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB343*-ABS(Lspeed6-Lspeed1),((AB343-AC343)*2/PI()+AB343)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z343*-ABS(Lspeed6-Lspeed1),((Z343-AA343)*2/PI()+AA343)*-ABS(Lspeed6-Lspeed1)),0))","v":1000.0023384349968},{"$f":"(J343^2)+3*(I343/1000)^2*(F343/2)^2*(2000*PI()/M343)^2","v":36309.895959730922},{"$f":"SQRT(3)*H343*F343/2*J343","v":9784.2034575109246},{"$f":"3*F343^2*H343^2/4-(UAC_V*0.98)^2","v":-43857.113125000003},{"$f":"-AM343/2/AL343+SQRT((AM343/2/AL343)^2-AN343/AL343)","v":0.97252069729330926},{"$f":"(J343^2)+3*(I343/1000)^2*(D343/2)^2*(2000*PI()/M343)^2","v":25458.565880564514},{"$f":"SQRT(3)*H343*D343/2*J343","v":7044.6264894078658},{"$f":"3*D343^2*H343^2/4-(UAC_V*0.98)^2","v":-47203.292500000003},{"$f":"-AQ343/2/AP343+SQRT((AQ343/2/AP343)^2-AR343/AP343)","v":1.2303177001632162},{"$f":"(J343^2)+3*(I343/1000)^2*(AH343/2)^2*(2000*PI()/M343)^2","v":14755.447354869169},{"$f":"SQRT(3)*H343*AH343/2*J343","v":2037.7908483682349},{"$f":"3*AH343^2*H343^2/4-(UAC_V*0.98)^2","v":-50503.76849672808},{"$f":"IF((AU343/2/AT343)^2-AV343/AT343>=0,-AU343/2/AT343+SQRT((AU343/2/AT343)^2-AV343/AT343),-9999)","v":1.7822955854164249},null,166]
["IC/ICD","IC44-100A3AC",3457,39.5,4202,55.1,"NA",0.88,8,58.62,25,330,32,3.8451040600477655,2.1953186489357588,2.6730062394485952,null,0.2,0.17577235787830695,0.37382198952879581,0.27433745483611793,942.48,0,-1570.8,0,0,0,0,0,0.57858401134942705,0.74783772056696562,6.9430081361931242,17.948105293607174,11.42611870644558,724.98461538461538,115.38488520403808,1000.0023384349968,9054.5952108283691,2461.561647827386,-49041.845392000003,2.1953186489357588,6323.6263250249376,1764.6403827437703,-49898.966800000002,2.6730062394485952,3677.905262722807,510.45545537766787,-50729.332965606656,3.6451457224365296,null,82.9]
["IC/ICD","IC44-150A1AC",5133,9.8000000000000007,6303,13.8,"NA",19.8,191,351.43207024971412,36.200000000000003,330,32,0.64137572828751632,0,0.21162885501799572,null,0.13812154696132595,0.16257533409204919,0.34225479930191971,1.8071040260047708,1294.3392000000001,0,-2157.232,0,0,0,0,0,0.13276985617517351,0.17160914345087344,1.5932382741020821,4.1186194428209628,2.6219945721573756,995.64553846153854,158.46190901354564,1373.3365447840622,324388.77906188124,83160.348231770899,5189.9132000000027,-0.10741769923580208,224811.61069682357,59055.899468938755,-22566.518799999994,0.21162885501799572,130756.39244953195,15800.433455247861,-48783.746226625626,0.55337157441392359,null,497]
["IC/ICD","IC44-150A2AC",5133,19.600000000000001,6303,27.6,"NA",5,47.7,176.06958851545033,36.200000000000003,330,32,1.2801756504373318,0.55371835385723878,0.75742242583785002,null,0.13812154696132595,0.16257533409204919,0.34225479930191971,0.84845009524795911,1294.3392000000001,0,-2157.232,0,0,0,0,0,0.26553971235034701,0.34321828690174688,3.1864765482041641,8.2372388856419256,5.2439891443147513,995.64553846153854,158.46190901354564,1373.3365447840622,81116.449815707674,21042.341635378889,-36522.160000000003,0.55371835385723878,56274.265071941642,14943.112175848777,-43602.16,0.75742242583785002,32809.678297908016,3998.0366343075798,-50289.545834768302,1.1786197038586583,null,249]
["IC/ICD","IC44-150A3AC",5133,39.200000000000003,6303,55.3,"NA",1.2,11.9,87.681240867131891,36.200000000000003,330,32,2.57067529805561,1.4135172721717502,1.7515423315163314,null,0.13812154696132595,0.16257533409204919,0.34225479930191971,0.41024248175294781,1294.3392000000001,0,-2157.232,0,0,0,0,0,0.53107942470069402,0.68643657380349377,6.3729530964083283,16.474477771283851,10.487978288629503,995.64553846153854,158.46190901354564,1373.3365447840622,20209.755770210184,5038.9923192638416,-47502.4228,1.4135172721717502,13979.976621595761,3571.9439225161414,-49145.588800000005,1.7515423315163314,8138.4001490214496,955.67526294773961,-50686.362496330621,2.4375827577072093,null,124]
["IC/ICD","IC44-200A1AC",6916,9.9,8407,13.8,"NA",25.5,253,468.81179592668099,47.4,330,32,0.4807899501642468,{"$error":"#NUM!"},2.6573097910632199E-2,null,0.10548523206751055,0.15346346712025299,0.32635470441298914,2.488659024627812,1646.1984,0,-2743.6639999999998,0,0,0,0,0,0.12660736037420872,0.16364392712550607,1.5192883244905047,3.9274542510121457,2.500295031263442,1266.3064615384615,201.53893282305319,1746.6707511331276,572252.95805959147,142872.4292604551,42070.047500000001,{"$error":"#NUM!"},401182.49188416591,102495.43838250039,-3006.9081250000017,2.6573097910632199E-2,231354.79951493928,25885.740940902426,-47756.393667253556,0.40182282510540135,null,663]
["IC/ICD","IC44-200A2AC",6916,19.8,8407,27.6,"NA",6.4,63.3,234.75945135393377,47.4,330,32,0.96013173782799888,0.32954026020429272,0.50588559908929942,null,0.10548523206751055,0.15346346712025299,0.32635470441298914,1.1436991493065916,1646.1984,{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},-2743.6639999999998,{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},0,{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0,0,0.25321472074841744,0.32728785425101214,3.0385766489810093,7.8549085020242915,5.000590062526884,1266.3064615384615,201.53893282305319,1746.6707511331276,143368.48517642182,35912.26305771331,-27403.892799999998,0.32954026020429272,100533.22512151387,25763.1452370552,-38761.691200000001,0.50588559908929942,58009.149927254919,6506.6125278714671,-50036.978722095846,0.87435581342023883,null,332]
["IC/ICD","IC44-200A3AC",6916,39.6,8407,55.2,"NA",1.6,15.8,117.37972567696688,47.4,330,32,1.9202634756559978,1.0025344829393923,1.2576184321923418,null,0.10548523206751055,0.15346346712025299,0.32635470441298914,0.55155548375913266,1646.1984,0,-2743.6639999999998,0,0,0,0,0,0.50642944149683489,0.65457570850202429,6.0771532979620186,15.709817004048583,10.001180125053768,1266.3064615384615,201.53893282305319,1746.6707511331276,35772.46349606997,8978.0657644283274,-44954.843200000003,1.0025344829393923,25097.45687486777,6440.7863092637999,-47794.292800000003,1.2576184321923418,14500.000861356231,1626.6531319678668,-50613.114680523962,1.8130542247254777,null,166]
["IC/ICD","IC44-250A3AC",9620,19.8,12500,27.6,"NA",7.7,78.900000000000006,280.72139213105936,58.5,330,32,0.80293132735238193,0.184874012254406,0.36461216439315958,null,8.5470085470085472E-2,0.13369875299815315,0.26598880000000003,1.3670563859751008,1994.9159999999999,0,-3324.86,0,0,0,0,0,0.22060294244695269,0.2851361226611227,2.6472353093634324,6.8432669438669445,4.3565590440551683,1534.5507692307692,244.23134034854732,2116.6716163540768,215922.10344933684,51666.131843525895,-16931.597199999997,0.184874012254406,149372.11349542902,37064.833713833788,-33372.121299999999,0.36461216439315958,82220.84922509703,8155.3099258789643,-49961.184338874817,0.73149872255394566,null,397]
["IC/ICD","IC44-250A5AC",9620,39.5,12500,55,"NA",1.9,19.7,140.71424945612296,58.5,330,32,1.6018278239140484,0.77982482629342875,1.0015042029853745,null,8.5470085470085472E-2,0.13369875299815315,0.26598880000000003,0.65898991725083156,1994.9159999999999,0,-3324.86,0,0,0,0,0,0.44009172861892076,0.56883216389466396,5.2811007434270492,13.651971933471934,8.6911152646555134,1534.5507692307692,244.23134034854732,2116.6716163540768,53745.739312568672,12734.590986511894,-42614.972500000003,0.77982482629342875,37308.949466920749,9145.7517084949068,-46580.783125000002,1.0015042029853745,20648.126479147402,2012.3236020366917,-50600.647675598404,1.5174739003167019,null,199]

{"sheet":"Hilfe","index":5,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,0,8]]}
[]
[]
[]
[null,null,null,null,null,"Farben:"]
[]
[null,null,null,null,null,"Eingabefelder",null,"2. Fahrsatz"]
[]
[null,null,null,null,null,"Ergebnisfelder"]

{"sheet":"Help","index":6,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":true,"merged":[[0,0,0,8]]}
[]
[]
[]
[null,null,null,null,null,"Colours:"]
[]
[null,null,null,null,null,"Input cells",null,"2. Motion task"]
[]
[null,null,null,null,null,"result cells"]

{"sheet":"Changes","index":7,"n_rows":25,"n_cols":4,"rows_kept":25,"cut":false,"hidden":true,"merged":[]}
["Version","Date","Name","Description"]
["V1.0","2003-10-15","M. Scholz","Initial version"]
["V1.1","2003-10-15","M. Scholz","Error in Lmin Check solved\nJext/Jmot and Gext/Gmot calculation error corrected\nOther motorlinie: no motor curves displayed "]
["V1.2","2003-10-29","M. Scholz","New feature: Lmax-Check \nIrms and Ipeak calculation correction"]
["V1.3","2003-11-07","M. Scholz","KT=Mo/Io not Mn/In because In data in some datasheets not correct\nCorrection working curve with 2 motion tasks and different load\nDry friction added\nClearInput, OpenDom and SaveDim added"]
["V1.4","2003-12-02","M. Scholz","Power Calculation corrected\nMotor curve correction (nn-knee, nmax(M=0) limited by mechanical, nmax(Mmax)\nlimited by voltage)\nwL-losses in speed curve and % calculation\nInertia formula correction\nSpeed calculation only with 2% losses (prev. 15 %)\nKe Baumüler Peak->RMS"]
["V1.5","2003-12-19","M. Scholz","Calculation error Inertia2/3 Cylinder Material corrected\nLmax of SR620 wrong type (text)"]
["V1.6","2004-02-10","M. Scholz","Calculation error of Trms (^3) corrected, appeared only with 2 motion tasks.\nWorking point calculation corrected (load and dry friction and sine2)\nTrms calculation error (load and dry friction an sine2)\nAdd Goldline BH and Bautz MWF Motor series to database\nLinMotor: wL and pol pitch added\nAdd L3S LinMotorLine\nFormat 3123 -> 3.1k"]
["V1.7","2004-04-09","M. Scholz","Error if you load Dim with different Inertia type "]
["V1.7-V2.16",null,"H. Goergen","diverses"]
["V2.17","2009-10-08","R.Fetzner","AKD Drives included"]
["V2.18","2009-12-10","R.Fetzner","fieldlength"]
["V2.19","2010-06-11","R.Fetzner","AKM8 Motors added"]
["V2.20","2010-06-14","R.Fetzner","AKM8 Data corrected"]
["V2.22","2011-03-29","R.Fetzner","Kollmorgen Logo, S700 min/max motorinductance + power internal brakeresistor "]
["V2.23","2011-05-25","R.Fetzner","Cart.DDR from Motor Database V6.2 included"]
["V2.24","2011-05-26","R.Fetzner","KBM from Motor Database V6.2 included"]
["V2.25","2011-05-27","R.Fetzner","Speicherproblem active.shape gelöst"]
["V2.26","2012-03-26","A.Schwalb","Aktualisierung von Mmax "]
["V2.29","2015-03-12","N. Will","AKMH and ICH motors added, Bautz motors deleted"]
["V2.30","2015-05-16","G.Schilling","Logik, Layout, PDF, DE_EN_Texte, Userform other L+R-Motors, 100% skalierung bei Start, Motorselektion check"]
["V2.33","2015-11-09","G.Schilling","Berechnung der Massenträgheit überarbeitet, da Formelfehler"]
["V2.34","2015-11-12","G.Schilling","Inertia / Zahnstange / Formel in H14 war falsch"]
["V2.35","2016-01-28","G.Schilling","Verbesserte AKMH-Werte, PDF-Druck der Drehmomentenkurve hinzugefügt"]
["V2.37","2018-07-03","G.Schilling","IC55 aus der Datenbank entnommen, diverse Rahman neu integriert, da diese sich verschoben"]

{"sheet":"Calc","index":8,"n_rows":201,"n_cols":26,"rows_kept":201,"cut":false,"hidden":true,"merged":[]}
["AC-Voltage","Selected",null,null,null,null,null,null,null,null,0,{"$f":"IF(ABS(MIN($O$1:$O$100))>MAX($O$1:$O$100),O1/MIN($O$1:$O$100)*-1,O1/MAX($O$1:$O$100))","v":0},{"$f":"IF(ABS(MIN($P$1:$P$100))>MAX($P$1:$P$100),P1/MIN($P$1:$P$100)*-1,P1/MAX($P$1:$P$100))","v":0},{"$f":"IF(ABS(MIN($Q$1:$Q$100))>MAX($Q$1:$Q$100),Q1/MIN($Q$1:$Q$100)*-1,Q1/MAX($Q$1:$Q$100))","v":0},0,{"$f":"IF($A$90=TRUE,(Main!$E$46),Lspeed1)","v":0},0,null,null,0,0,{"$f":"IF($A$90=TRUE,Main!$E$46,Lspeed1)","v":0},{"$f":"IF(move1,IF(ABS(MIN($U$1:$U$101))>MAX($U$1:$U$101),U1/MIN($U$1:$U$101)*-1,U1/MAX($U$1:$U$101)),IF(ABS(MIN($U$1:$U$201))>MAX($U$1:$U$201),U1/MIN($U$1:$U$201)*-1,U1/MAX($U$1:$U$201)))","v":0},{"$f":"IF(move1,IF(ABS(MIN($V$1:$V$101))>MAX($V$1:$V$101),V1/MIN($V$1:$V$101)*-1,V1/MAX($V$1:$V$101)),IF(ABS(MIN($V$1:$V$201))>MAX($V$1:$V$201),V1/MIN($V$1:$V$201)*-1,V1/MAX($V$1:$V$201)))","v":0},{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W1*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W1>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W1*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W1>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W1*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W1>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W1*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W1>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W1*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W1>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W1*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W1>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":0},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X1*speed,X1*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X1*speed,X1*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":0}]
[50,"230",null,null,null,null,null,null,null,null,1,{"$f":"IF(ABS(MIN($O$1:$O$100))>MAX($O$1:$O$100),O2/MIN($O$1:$O$100)*-1,O2/MAX($O$1:$O$100))","v":0.18604675103410034},{"$f":"IF(ABS(MIN($P$1:$P$100))>MAX($P$1:$P$100),P2/MIN($P$1:$P$100)*-1,P2/MAX($P$1:$P$100))","v":1.7330874436944199E-2},{"$f":"IF(ABS(MIN($Q$1:$Q$100))>MAX($Q$1:$Q$100),Q2/MIN($Q$1:$Q$100)*-1,Q2/MAX($Q$1:$Q$100))","v":9.222430029345647E-4},{"$f":"IF($A$90=TRUE,(IF(K2<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K2*PI()*Main!$D$45/100/Main!$D$46))),(IF(K2<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K2-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R2)))))))),(IF(K2<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K2*PI()*Main!$D$71/100/Main!$D$72))),(IF(K2<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K2-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R2)))))))))","v":143.87446532884132},{"$f":"IF($A$90=TRUE,(IF(K2<=(Main!$D$46/Main!$D$45*100),O2*Main!$D$45/100000+P1,IF(K2<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O2*Main!$D$45/100000+P1,IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S2))))),(IF(K2<=(Main!$D$72/Main!$D$71*100),O2*Main!$D$71/100000+P1,IF(K2<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O2*Main!$D$71/100000+P1,IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S2))))))","v":0.69203617823172681},{"$f":"IF($A$90=TRUE,P2*Main!$D$45/100000+Q1,P2*100+Q1)","v":3.3286940172946059E-3},{"$f":"IF($A$90=TRUE,(IF(K2<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K2-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K2<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K2<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K2-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K2<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K2-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K2<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K2<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K2-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O2*Main!$D$45/100000+P1,IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O2*Main!$D$45/100000+P1,Main!$E$52)))),(IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O2*Main!$D$71/100000+P1,IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O2*Main!$D$71/100000+P1,Main!$E$78)))))","v":0.69203617823172681},9.9999999999999995E-7,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T2*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T2*PI()/50))))","v":4.8738901138358954E-5},{"$f":"IF($A$90=TRUE,U2*2*Main!$D$46/100000*(T2-T1)+V1,U2*2*Ltime1*(T2-T1)/100000+V1)","v":7.89570198441415E-14},{"$f":"IF(move1,IF(ABS(MIN($U$1:$U$101))>MAX($U$1:$U$101),U2/MIN($U$1:$U$101)*-1,U2/MAX($U$1:$U$101)),IF(ABS(MIN($U$1:$U$201))>MAX($U$1:$U$201),U2/MIN($U$1:$U$201)*-1,U2/MAX($U$1:$U$201)))","v":6.2831853071795822E-8},{"$f":"IF(move1,IF(ABS(MIN($V$1:$V$101))>MAX($V$1:$V$101),V2/MIN($V$1:$V$101)*-1,V2/MAX($V$1:$V$101)),IF(ABS(MIN($V$1:$V$201))>MAX($V$1:$V$201),V2/MIN($V$1:$V$201)*-1,V2/MAX($V$1:$V$201)))","v":1.9739254961035377E-15},{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W2*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W2>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W2*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W2>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W2*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W2>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W2*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W2>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W2*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W2>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W2*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W2>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad))),0)","v":9.45042899648619E-7},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X2*speed,X2*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X2*speed,X2*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":4.7374211906484902E-12}]
[115,null,null,null,null,null,null,null,null,null,2,0.36563722717525282,5.1391199803686456E-2,3.6569679358167619E-3,{"$f":"IF($A$90=TRUE,(IF(K3<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K3*PI()*Main!$D$45/100/Main!$D$46))),(IF(K3<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K3-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R1)))))))),(IF(K3<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K3*PI()*Main!$D$71/100/Main!$D$72))),(IF(K3<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K3-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R1)))))))))","v":282.7561366794173},{"$f":"IF($A$90=TRUE,(IF(K3<=(Main!$D$46/Main!$D$45*100),O3*Main!$D$45/100000+P2,IF(K3<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O3*Main!$D$45/100000+P2,IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S3))))),(IF(K3<=(Main!$D$72/Main!$D$71*100),O3*Main!$D$71/100000+P2,IF(K3<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O3*Main!$D$71/100000+P2,IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S3))))))","v":2.0520931956597241},{"$f":"IF($A$90=TRUE,P3*Main!$D$45/100000+Q2,P3*100+Q2)","v":1.319926228841788E-2},{"$f":"IF($A$90=TRUE,(IF(K3<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K3-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K3<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K3<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K3-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K3<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K3-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K3<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K3<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K3-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O3*Main!$D$45/100000+P2,IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O3*Main!$D$45/100000+P2,Main!$E$52)))),(IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O3*Main!$D$71/100000+P2,IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O3*Main!$D$71/100000+P2,Main!$E$78)))))","v":2.0520931956597241},9.9999999999999995E-7,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T3*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T3*PI()/50))))","v":4.8738901138358954E-5},{"$f":"IF($A$90=TRUE,U3*2*Main!$D$46/100000*(T3-T2)+V2,U3*2*Ltime1*(T3-T2)/100000+V2)","v":7.89570198441415E-14},6.2831853071795822E-8,1.9739254961035377E-15,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W3*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W3>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W3*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W3>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W3*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W3>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W3*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W3>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W3*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W3>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W3*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W3>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9.45042899648619E-7},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X3*speed,X3*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X3*speed,X3*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":4.7374211906484902E-12}]
[230,null,null,null,null,null,null,null,null,null,3,0.53253920197672888,0.10099899994483222,9.0315161931136725E-3,{"$f":"IF($A$90=TRUE,(IF(K4<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K4*PI()*Main!$D$45/100/Main!$D$46))),(IF(K4<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K4-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R4)))))))),(IF(K4<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K4*PI()*Main!$D$71/100/Main!$D$72))),(IF(K4<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K4-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R4)))))))))","v":411.82548217144802},{"$f":"IF($A$90=TRUE,(IF(K4<=(Main!$D$46/Main!$D$45*100),O4*Main!$D$45/100000+P3,IF(K4<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O4*Main!$D$45/100000+P3,IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S4))))),(IF(K4<=(Main!$D$72/Main!$D$71*100),O4*Main!$D$71/100000+P3,IF(K4<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O4*Main!$D$71/100000+P3,IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S4))))))","v":4.0329737649043889},{"$f":"IF($A$90=TRUE,P4*Main!$D$45/100000+Q3,P4*100+Q3)","v":3.2597866097607994E-2},{"$f":"IF($A$90=TRUE,(IF(K4<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K4-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K4<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K4<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K4-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K4<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K4-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K4<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K4<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K4-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O4*Main!$D$45/100000+P3,IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O4*Main!$D$45/100000+P3,Main!$E$52)))),(IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O4*Main!$D$71/100000+P3,IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O4*Main!$D$71/100000+P3,Main!$E$78)))))","v":4.0329737649043889},1,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T4*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T4*PI()/50))))","v":48.706838556368119},{"$f":"IF($A$90=TRUE,U4*2*Main!$D$46/100000*(T4-T3)+V3,U4*2*Ltime1*(T4-T3)/100000+V3)","v":7.8904999556316843E-2},6.2790519529313374E-2,1.9726249889079209E-3,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W4*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W4>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W4*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W4>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W4*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W4>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W4*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W4>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W4*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W4>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W4*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W4>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":0.94442120907400362},4.7342999733790103]
[400,null,null,null,null,null,null,null,null,null,4,0.68096077085806817,0.1644327635049537,1.7781620877524287E-2,{"$f":"IF($A$90=TRUE,(IF(K5<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K5*PI()*Main!$D$45/100/Main!$D$46))),(IF(K5<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K5-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R5)))))))),(IF(K5<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K5*PI()*Main!$D$71/100/Main!$D$72))),(IF(K5<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K5-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R5)))))))))","v":526.60348150429581},{"$f":"IF($A$90=TRUE,(IF(K5<=(Main!$D$46/Main!$D$45*100),O5*Main!$D$45/100000+P4,IF(K5<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O5*Main!$D$45/100000+P4,IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S5))))),(IF(K5<=(Main!$D$72/Main!$D$71*100),O5*Main!$D$71/100000+P4,IF(K5<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O5*Main!$D$71/100000+P4,IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S5))))))","v":6.5659365109400518},{"$f":"IF($A$90=TRUE,P5*Main!$D$45/100000+Q4,P5*100+Q4)","v":6.4180020715229644E-2},{"$f":"IF($A$90=TRUE,(IF(K5<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K5-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K5<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K5<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K5-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K5<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K5-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K5<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K5<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K5-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O5*Main!$D$45/100000+P4,IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O5*Main!$D$45/100000+P4,Main!$E$52)))),(IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O5*Main!$D$71/100000+P4,IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O5*Main!$D$71/100000+P4,Main!$E$78)))))","v":6.5659365109400518},2,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T5*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T5*PI()/50))))","v":97.221453472992167},{"$f":"IF($A$90=TRUE,U5*2*Main!$D$46/100000*(T5-T4)+V4,U5*2*Ltime1*(T5-T4)/100000+V4)","v":0.23640375418256415},0.12533323356430426,5.9100938545641035E-3,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W5*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W5>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W5*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W5>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W5*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W5>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W5*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W5>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W5*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W5>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W5*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W5>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":1.8851152191008012},14.184225250953848]
[480,null,null,null,null,null,null,null,null,null,5,0.8057513442851113,0.2394911845608782,3.0525875071355044E-2,{"$f":"IF($A$90=TRUE,(IF(K6<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K6*PI()*Main!$D$45/100/Main!$D$46))),(IF(K6<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K6-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R6)))))))),(IF(K6<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K6*PI()*Main!$D$71/100/Main!$D$72))),(IF(K6<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K6-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R6)))))))))","v":623.10705885838001},{"$f":"IF($A$90=TRUE,(IF(K6<=(Main!$D$46/Main!$D$45*100),O6*Main!$D$45/100000+P5,IF(K6<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O6*Main!$D$45/100000+P5,IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S6))))),(IF(K6<=(Main!$D$72/Main!$D$71*100),O6*Main!$D$71/100000+P5,IF(K6<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O6*Main!$D$71/100000+P5,IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S6))))))","v":9.5630814640488602},{"$f":"IF($A$90=TRUE,P6*Main!$D$45/100000+Q5,P6*100+Q5)","v":0.11017844255730466},{"$f":"IF($A$90=TRUE,(IF(K6<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K6-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K6<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K6<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K6-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K6<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K6-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K6<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K6<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K6-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O6*Main!$D$45/100000+P5,IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O6*Main!$D$45/100000+P5,Main!$E$52)))),(IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O6*Main!$D$71/100000+P5,IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O6*Main!$D$71/100000+P5,Main!$E$78)))))","v":9.5630814640488602},4,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T6*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T6*PI()/50))))","v":192.90966654743403},{"$f":"IF($A$90=TRUE,U6*2*Main!$D$46/100000*(T6-T5)+V5,U6*2*Ltime1*(T6-T5)/100000+V5)","v":0.8614310737962505},0.24868988716485479,2.1535776844906263E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W6*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W6>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W6*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W6>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W6*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W6>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W6*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W6>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W6*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W6>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W6*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W6>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":3.7405010450831351},51.68586442777503]
[null,null,null,null,null,null,null,null,null,null,6,0.90258038575767607,0.32356955329276665,4.7744265151592268E-2,{"$f":"IF($A$90=TRUE,(IF(K7<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K7*PI()*Main!$D$45/100/Main!$D$46))),(IF(K7<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K7-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R7)))))))),(IF(K7<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K7*PI()*Main!$D$71/100/Main!$D$72))),(IF(K7<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K7-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R7)))))))))","v":697.98730531651904},{"$f":"IF($A$90=TRUE,(IF(K7<=(Main!$D$46/Main!$D$45*100),O7*Main!$D$45/100000+P6,IF(K7<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O7*Main!$D$45/100000+P6,IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S7))))),(IF(K7<=(Main!$D$72/Main!$D$71*100),O7*Main!$D$71/100000+P6,IF(K7<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O7*Main!$D$71/100000+P6,IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S7))))))","v":12.920400402621317},{"$f":"IF($A$90=TRUE,P7*Main!$D$45/100000+Q6,P7*100+Q6)","v":0.1723255684939132},{"$f":"IF($A$90=TRUE,(IF(K7<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K7-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K7<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K7<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K7-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K7<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K7-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K7<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K7<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K7-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O7*Main!$D$45/100000+P6,IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O7*Main!$D$45/100000+P6,Main!$E$52)))),(IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O7*Main!$D$71/100000+P6,IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O7*Main!$D$71/100000+P6,Main!$E$78)))))","v":12.920400402621317},6,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T7*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T7*PI()/50))))","v":285.55557894177389},{"$f":"IF($A$90=TRUE,U7*2*Main!$D$46/100000*(T7-T6)+V6,U7*2*Ltime1*(T7-T6)/100000+V6)","v":1.7866311495675977},0.36812455268467797,4.4665778739189942E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W7*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W7>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W7*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W7>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W7*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W7>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W7*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W7>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W7*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W7>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W7*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W7>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":5.5368969351174933},107.19786897405587]
[null,null,null,null,null,null,null,null,null,null,7,0.96808769196184929,0.41375014575184554,6.9761514094864641E-2,{"$f":"IF($A$90=TRUE,(IF(K8<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K8*PI()*Main!$D$45/100/Main!$D$46))),(IF(K8<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K8-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R8)))))))),(IF(K8<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K8*PI()*Main!$D$71/100/Main!$D$72))),(IF(K8<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K8-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R8)))))))))","v":748.6456941508967},{"$f":"IF($A$90=TRUE,(IF(K8<=(Main!$D$46/Main!$D$45*100),O8*Main!$D$45/100000+P7,IF(K8<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O8*Main!$D$45/100000+P7,IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S8))))),(IF(K8<=(Main!$D$72/Main!$D$71*100),O8*Main!$D$71/100000+P7,IF(K8<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O8*Main!$D$71/100000+P7,IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S8))))))","v":16.521386191487128},{"$f":"IF($A$90=TRUE,P8*Main!$D$45/100000+Q7,P8*100+Q7)","v":0.25179343607496629},{"$f":"IF($A$90=TRUE,(IF(K8<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K8-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K8<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K8<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K8-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K8<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K8-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K8<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K8<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K8-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O8*Main!$D$45/100000+P7,IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O8*Main!$D$45/100000+P7,Main!$E$52)))),(IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O8*Main!$D$71/100000+P7,IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O8*Main!$D$71/100000+P7,Main!$E$78)))))","v":16.521386191487128},7,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T8*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T8*PI()/50))))","v":330.27857342736598},{"$f":"IF($A$90=TRUE,U8*2*Main!$D$46/100000*(T8-T7)+V7,U8*2*Ltime1*(T8-T7)/100000+V7)","v":2.3216824385199306},0.42577929156507266,5.8042060962998264E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W8*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W8>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W8*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W8>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W8*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W8>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W8*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W8>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W8*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W8>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W8*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W8>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":6.4040717667709961},139.30094631119584]
["Massenträgheit",1,2,3,4,null,null,null,null,null,8,1,0.50690347597994312,9.6735812800137586E-2,{"$f":"IF($A$90=TRUE,(IF(K9<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K9*PI()*Main!$D$45/100/Main!$D$46))),(IF(K9<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K9-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R9)))))))),(IF(K9<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K9*PI()*Main!$D$71/100/Main!$D$72))),(IF(K9<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K9-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R9)))))))))","v":773.32425602245917},{"$f":"IF($A$90=TRUE,(IF(K9<=(Main!$D$46/Main!$D$45*100),O9*Main!$D$45/100000+P8,IF(K9<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O9*Main!$D$45/100000+P8,IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S9))))),(IF(K9<=(Main!$D$72/Main!$D$71*100),O9*Main!$D$71/100000+P8,IF(K9<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O9*Main!$D$71/100000+P8,IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S9))))))","v":20.241075862955157},{"$f":"IF($A$90=TRUE,P9*Main!$D$45/100000+Q8,P9*100+Q8)","v":0.34915301097578061},{"$f":"IF($A$90=TRUE,(IF(K9<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K9-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K9<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K9<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K9-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K9<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K9-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K9<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K9<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K9-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O9*Main!$D$45/100000+P8,IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O9*Main!$D$45/100000+P8,Main!$E$52)))),(IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O9*Main!$D$71/100000+P8,IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O9*Main!$D$71/100000+P8,Main!$E$78)))))","v":20.241075862955157},8,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T9*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T9*PI()/50))))","v":373.69810927356764},{"$f":"IF($A$90=TRUE,U9*2*Main!$D$46/100000*(T9-T8)+V8,U9*2*Ltime1*(T9-T8)/100000+V8)","v":2.9270733755431104},0.48175367410171538,7.3176834388577763E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W9*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W9>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W9*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W9>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W9*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W9>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W9*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W9>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W9*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W9>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W9*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W9>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.2459726529031432},175.62440253258663]
[{"$f":"IF(deutsch,\"Nicht benutzt\",\"Not used\")","v":"Nicht benutzt"},"Zahnstange","Nicht benutzt","Nicht benutzt",null,null,null,null,null,null,9,0.99720987514393422,0.59979689678594583,0.12865333047965738,{"$f":"IF($A$90=TRUE,(IF(K10<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K10*PI()*Main!$D$45/100/Main!$D$46))),(IF(K10<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K10-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R10)))))))),(IF(K10<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K10*PI()*Main!$D$71/100/Main!$D$72))),(IF(K10<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K10-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R10)))))))))","v":771.16658479393232},{"$f":"IF($A$90=TRUE,(IF(K10<=(Main!$D$46/Main!$D$45*100),O10*Main!$D$45/100000+P9,IF(K10<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O10*Main!$D$45/100000+P9,IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S10))))),(IF(K10<=(Main!$D$72/Main!$D$71*100),O10*Main!$D$71/100000+P9,IF(K10<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O10*Main!$D$71/100000+P9,IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S10))))))","v":23.950387135813969},{"$f":"IF($A$90=TRUE,P10*Main!$D$45/100000+Q9,P10*100+Q9)","v":0.46435437309904581},{"$f":"IF($A$90=TRUE,(IF(K10<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K10-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K10<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K10<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K10-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K10<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K10-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K10<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K10<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K10-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O10*Main!$D$45/100000+P9,IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O10*Main!$D$45/100000+P9,Main!$E$52)))),(IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O10*Main!$D$71/100000+P9,IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O10*Main!$D$71/100000+P9,Main!$E$78)))))","v":23.950387135813969},9,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T10*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T10*PI()/50))))","v":415.64282940889279},{"$f":"IF($A$90=TRUE,U10*2*Main!$D$46/100000*(T10-T9)+V9,U10*2*Ltime1*(T10-T9)/100000+V9)","v":3.6004147591855169},0.53582679497899666,9.001036897963792E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W10*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W10>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W10*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W10>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W10*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W10>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W10*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W10>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W10*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W10>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W10*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W10>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":8.0592769953443},216.02488555113101]
[{"$f":"IF(deutsch,\"Zylinder\",\"Cylinder\")","v":"Zylinder"},null,null,null,null,null,null,null,null,null,10,0.95981414151423672,0.68920678046801953,0.16532869462093508,{"$f":"IF($A$90=TRUE,(IF(K11<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K11*PI()*Main!$D$45/100/Main!$D$46))),(IF(K11<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K11-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R11)))))))),(IF(K11<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K11*PI()*Main!$D$71/100/Main!$D$72))),(IF(K11<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K11-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R11)))))))))","v":742.24755690633242},{"$f":"IF($A$90=TRUE,(IF(K11<=(Main!$D$46/Main!$D$45*100),O11*Main!$D$45/100000+P10,IF(K11<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O11*Main!$D$45/100000+P10,IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S11))))),(IF(K11<=(Main!$D$72/Main!$D$71*100),O11*Main!$D$71/100000+P10,IF(K11<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O11*Main!$D$71/100000+P10,IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S11))))))","v":27.520597884533426},{"$f":"IF($A$90=TRUE,P11*Main!$D$45/100000+Q10,P11*100+Q10)","v":0.59672844892365162},{"$f":"IF($A$90=TRUE,(IF(K11<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K11-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K11<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K11<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K11-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K11<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K11-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K11<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K11<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K11-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O11*Main!$D$45/100000+P10,IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O11*Main!$D$45/100000+P10,Main!$E$52)))),(IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O11*Main!$D$71/100000+P10,IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O11*Main!$D$71/100000+P10,Main!$E$78)))))","v":27.520597884533426},10,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T11*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T11*PI()/50))))","v":455.94719718568729},{"$f":"IF($A$90=TRUE,U11*2*Main!$D$46/100000*(T11-T10)+V10,U11*2*Ltime1*(T11-T10)/100000+V10)","v":4.3390492186263305},0.58778525229247314,0.10847623046565827,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W11*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W11>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W11*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W11>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W11*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W11>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W11*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W11>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W11*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W11>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W11*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W11>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":8.840775053418259},260.34295311757984]
["Block",null,null,null,null,null,null,null,null,null,11,0.88911052204772134,0.77203038653760703,0.20641142386392164,{"$f":"IF($A$90=TRUE,(IF(K12<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K12*PI()*Main!$D$45/100/Main!$D$46))),(IF(K12<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K12-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R12)))))))),(IF(K12<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K12*PI()*Main!$D$71/100/Main!$D$72))),(IF(K12<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K12-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R12)))))))))","v":687.57073298429441},{"$f":"IF($A$90=TRUE,(IF(K12<=(Main!$D$46/Main!$D$45*100),O12*Main!$D$45/100000+P11,IF(K12<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O12*Main!$D$45/100000+P11,IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S12))))),(IF(K12<=(Main!$D$72/Main!$D$71*100),O12*Main!$D$71/100000+P11,IF(K12<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O12*Main!$D$71/100000+P11,IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S12))))))","v":30.827813110187883},{"$f":"IF($A$90=TRUE,P12*Main!$D$45/100000+Q11,P12*100+Q11)","v":0.7450102299836554},{"$f":"IF($A$90=TRUE,(IF(K12<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K12-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K12<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K12<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K12-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K12<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K12-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K12<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K12<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K12-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O12*Main!$D$45/100000+P11,IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O12*Main!$D$45/100000+P11,Main!$E$52)))),(IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O12*Main!$D$71/100000+P11,IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O12*Main!$D$71/100000+P11,Main!$E$78)))))","v":30.827813110187883},11,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T12*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T12*PI()/50))))","v":494.4521496776502},{"$f":"IF($A$90=TRUE,U12*2*Main!$D$46/100000*(T12-T11)+V11,U12*2*Ltime1*(T12-T11)/100000+V11)","v":5.1400617011041234},0.63742398974868963,0.1285015425276031,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W12*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W12>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W12*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W12>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W12*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W12>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W12*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W12>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W12*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W12>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W12*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W12>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9.5873826113223064},308.40370206624743]
[{"$f":"IF(deutsch,\"Spindel\",\"Spindle\")","v":"Spindel"},null,null,null,null,null,null,null,null,null,12,0.7875526043543033,0.84539353436302167,0.25139809055688561,{"$f":"IF($A$90=TRUE,(IF(K13<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K13*PI()*Main!$D$45/100/Main!$D$46))),(IF(K13<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K13-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R13)))))))),(IF(K13<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K13*PI()*Main!$D$71/100/Main!$D$72))),(IF(K13<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K13-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R13)))))))))","v":609.03353184084176},{"$f":"IF($A$90=TRUE,(IF(K13<=(Main!$D$46/Main!$D$45*100),O13*Main!$D$45/100000+P12,IF(K13<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O13*Main!$D$45/100000+P12,IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S13))))),(IF(K13<=(Main!$D$72/Main!$D$71*100),O13*Main!$D$71/100000+P12,IF(K13<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O13*Main!$D$71/100000+P12,IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S13))))))","v":33.757264398342329},{"$f":"IF($A$90=TRUE,P13*Main!$D$45/100000+Q12,P13*100+Q12)","v":0.90738267173968201},{"$f":"IF($A$90=TRUE,(IF(K13<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K13-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K13<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K13<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K13-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K13<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K13-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K13<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K13<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K13-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O13*Main!$D$45/100000+P12,IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O13*Main!$D$45/100000+P12,Main!$E$52)))),(IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O13*Main!$D$71/100000+P12,IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O13*Main!$D$71/100000+P12,Main!$E$78)))))","v":33.757264398342329},12,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T13*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T13*PI()/50))))","v":531.00572542853536},{"$f":"IF($A$90=TRUE,U13*2*Main!$D$46/100000*(T13-T12)+V12,U13*2*Ltime1*(T13-T12)/100000+V12)","v":6.0002909762983503},0.68454710592868862,0.15000727440745876,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W13*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W13>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W13*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W13>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W13*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W13>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W13*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W13>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W13*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W13>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W13*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W13>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":10.296153150117942},360.01745857790104]
[{"$f":"IF(deutsch,\"Zahnstange\",\"Rack\")","v":"Zahnstange"},null,null,null,null,null,null,null,null,null,13,0.65866469525761528,0.90675034422994361,0.29964979092071453,{"$f":"IF($A$90=TRUE,(IF(K14<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K14*PI()*Main!$D$45/100/Main!$D$46))),(IF(K14<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K14-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R14)))))))),(IF(K14<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K14*PI()*Main!$D$71/100/Main!$D$72))),(IF(K14<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K14-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R14)))))))))","v":509.36138542835511},{"$f":"IF($A$90=TRUE,(IF(K14<=(Main!$D$46/Main!$D$45*100),O14*Main!$D$45/100000+P13,IF(K14<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O14*Main!$D$45/100000+P13,IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S14))))),(IF(K14<=(Main!$D$72/Main!$D$71*100),O14*Main!$D$71/100000+P13,IF(K14<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O14*Main!$D$71/100000+P13,IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S14))))))","v":36.207292662252719},{"$f":"IF($A$90=TRUE,P14*Main!$D$45/100000+Q13,P14*100+Q13)","v":1.0815397494451175},{"$f":"IF($A$90=TRUE,(IF(K14<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K14-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K14<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K14<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K14-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K14<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K14-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K14<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K14<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K14-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O14*Main!$D$45/100000+P13,IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O14*Main!$D$45/100000+P13,Main!$E$52)))),(IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O14*Main!$D$71/100000+P13,IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O14*Main!$D$71/100000+P13,Main!$E$78)))))","v":36.207292662252719},13,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T14*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T14*PI()/50))))","v":565.46366417459421},{"$f":"IF($A$90=TRUE,U14*2*Main!$D$46/100000*(T14-T13)+V13,U14*2*Ltime1*(T14-T13)/100000+V13)","v":6.9163421122611926},0.72896862742141155,0.17290855280652981,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W14*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W14>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W14*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W14>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W14*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W14>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W14*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W14>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W14*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W14>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W14*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W14>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":10.964289476295001},414.98052673567156]
[null,null,null,null,null,null,null,null,null,null,14,0.50691951877396046,0.95397158556136263,0.35041431656443534,{"$f":"IF($A$90=TRUE,(IF(K15<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K15*PI()*Main!$D$45/100/Main!$D$46))),(IF(K15<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K15-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R15)))))))),(IF(K15<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K15*PI()*Main!$D$71/100/Main!$D$72))),(IF(K15<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K15-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R15)))))))))","v":392.01315971913601},{"$f":"IF($A$90=TRUE,(IF(K15<=(Main!$D$46/Main!$D$45*100),O15*Main!$D$45/100000+P14,IF(K15<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O15*Main!$D$45/100000+P14,IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S15))))),(IF(K15<=(Main!$D$72/Main!$D$71*100),O15*Main!$D$71/100000+P14,IF(K15<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O15*Main!$D$71/100000+P14,IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S15))))))","v":38.092875960501765},{"$f":"IF($A$90=TRUE,P15*Main!$D$45/100000+Q14,P15*100+Q14)","v":1.264766482815131},{"$f":"IF($A$90=TRUE,(IF(K15<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K15-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K15<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K15<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K15-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K15<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K15-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K15<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K15<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K15-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O15*Main!$D$45/100000+P14,IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O15*Main!$D$45/100000+P14,Main!$E$52)))),(IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O15*Main!$D$71/100000+P14,IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O15*Main!$D$71/100000+P14,Main!$E$78)))))","v":38.092875960501765},14,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T15*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T15*PI()/50))))","v":597.68997617393075},{"$f":"IF($A$90=TRUE,U15*2*Main!$D$46/100000*(T15-T14)+V14,U15*2*Ltime1*(T15-T14)/100000+V14)","v":7.8845998736629603},0.77051324277578925,0.19711499684157402,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W15*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W15>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W15*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W15>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W15*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W15>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W15*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W15>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W15*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W15>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W15*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W15>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.589154761016509},473.07599241977766]
[null,null,null,null,null,null,null,null,null,null,15,0.33758300170728384,0.98541856639879366,0.40285225794642465,{"$f":"IF($A$90=TRUE,(IF(K16<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K16*PI()*Main!$D$45/100/Main!$D$46))),(IF(K16<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K16-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R16)))))))),(IF(K16<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K16*PI()*Main!$D$71/100/Main!$D$72))),(IF(K16<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K16-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R16)))))))))","v":261.06112364111385},{"$f":"IF($A$90=TRUE,(IF(K16<=(Main!$D$46/Main!$D$45*100),O16*Main!$D$45/100000+P15,IF(K16<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O16*Main!$D$45/100000+P15,IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S16))))),(IF(K16<=(Main!$D$72/Main!$D$71*100),O16*Main!$D$71/100000+P15,IF(K16<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O16*Main!$D$71/100000+P15,IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S16))))))","v":39.348579965215521},{"$f":"IF($A$90=TRUE,P16*Main!$D$45/100000+Q15,P16*100+Q15)","v":1.4540331524478176},{"$f":"IF($A$90=TRUE,(IF(K16<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K16-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K16<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K16<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K16-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K16<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K16-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K16<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K16<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K16-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O16*Main!$D$45/100000+P15,IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O16*Main!$D$45/100000+P15,Main!$E$52)))),(IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O16*Main!$D$71/100000+P15,IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O16*Main!$D$71/100000+P15,Main!$E$78)))))","v":39.348579965215521},15,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T16*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T16*PI()/50))))","v":627.55747889588508},{"$f":"IF($A$90=TRUE,U16*2*Main!$D$46/100000*(T16-T15)+V15,U16*2*Ltime1*(T16-T15)/100000+V15)","v":8.9012429894742944},0.80901699437494734,0.22253107473685735,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W16*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W16>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W16*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W16>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W16*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W16>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W16*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W16>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W16*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W16>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W16*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W16>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.168282946477465},534.07457936845765]
[null,null,null,null,null,null,null,null,null,null,16,0.15653153317763188,1,0.45606613392769774,{"$f":"IF($A$90=TRUE,(IF(K17<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K17*PI()*Main!$D$45/100/Main!$D$46))),(IF(K17<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K17-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R17)))))))),(IF(K17<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K17*PI()*Main!$D$71/100/Main!$D$72))),(IF(K17<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K17-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R17)))))))))","v":121.04963143864707},{"$f":"IF($A$90=TRUE,(IF(K17<=(Main!$D$46/Main!$D$45*100),O17*Main!$D$45/100000+P16,IF(K17<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O17*Main!$D$45/100000+P16,IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S17))))),(IF(K17<=(Main!$D$72/Main!$D$71*100),O17*Main!$D$71/100000+P16,IF(K17<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O17*Main!$D$71/100000+P16,IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S17))))))","v":39.930828692435412},{"$f":"IF($A$90=TRUE,P17*Main!$D$45/100000+Q16,P17*100+Q16)","v":1.6461004384584319},{"$f":"IF($A$90=TRUE,(IF(K17<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K17-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K17<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K17<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K17-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K17<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K17-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K17<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K17<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K17-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O17*Main!$D$45/100000+P16,IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O17*Main!$D$45/100000+P16,Main!$E$52)))),(IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O17*Main!$D$71/100000+P16,IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O17*Main!$D$71/100000+P16,Main!$E$78)))))","v":39.930828692435412},16,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T17*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T17*PI()/50))))","v":654.94829895237785},{"$f":"IF($A$90=TRUE,U17*2*Main!$D$46/100000*(T17-T16)+V16,U17*2*Ltime1*(T17-T16)/100000+V16)","v":9.9622592337771465},0.84432792550201496,0.24905648084442866,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W17*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W17>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W17*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W17>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W17*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W17>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W17*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W17>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W17*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W17>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W17*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W17>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.699388478308357},597.73555402662873]
[null,null,null,null,null,null,null,null,null,null,17,-1.9652485865697976E-2,0.99816930549434957,0.50918259155858747,{"$f":"IF($A$90=TRUE,(IF(K18<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K18*PI()*Main!$D$45/100/Main!$D$46))),(IF(K18<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K18-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R18)))))))),(IF(K18<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K18*PI()*Main!$D$71/100/Main!$D$72))),(IF(K18<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K18-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R18)))))))))","v":-15.197744011082783},{"$f":"IF($A$90=TRUE,(IF(K18<=(Main!$D$46/Main!$D$45*100),O18*Main!$D$45/100000+P17,IF(K18<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O18*Main!$D$45/100000+P17,IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S18))))),(IF(K18<=(Main!$D$72/Main!$D$71*100),O18*Main!$D$71/100000+P17,IF(K18<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O18*Main!$D$71/100000+P17,IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S18))))))","v":39.857727543742101},{"$f":"IF($A$90=TRUE,P18*Main!$D$45/100000+Q17,P18*100+Q17)","v":1.8378161079438313},{"$f":"IF($A$90=TRUE,(IF(K18<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K18-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K18<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K18<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K18-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K18<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K18-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K18<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K18<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K18-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O18*Main!$D$45/100000+P17,IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O18*Main!$D$45/100000+P17,Main!$E$52)))),(IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O18*Main!$D$71/100000+P17,IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O18*Main!$D$71/100000+P17,Main!$E$78)))))","v":39.857727543742101},17,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T18*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T18*PI()/50))))","v":679.75433729032147},{"$f":"IF($A$90=TRUE,U18*2*Main!$D$46/100000*(T18-T17)+V17,U18*2*Ltime1*(T18-T17)/100000+V17)","v":11.063461260187466},0.87630668004386358,0.27658653150468665,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W18*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W18>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W18*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W18>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W18*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W18>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W18*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W18>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W18*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W18>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W18*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W18>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":13.18037532561409},663.80767561124799]
["Material",null,1,null,2,null,2,null,4,null,18,-0.14170223493149772,0.98496927040971627,0.56159662415953526,{"$f":"IF($A$90=TRUE,(IF(K19<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K19*PI()*Main!$D$45/100/Main!$D$46))),(IF(K19<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K19-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R19)))))))),(IF(K19<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K19*PI()*Main!$D$71/100/Main!$D$72))),(IF(K19<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K19-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R19)))))))))","v":-109.5817754051202},{"$f":"IF($A$90=TRUE,(IF(K19<=(Main!$D$46/Main!$D$45*100),O19*Main!$D$45/100000+P18,IF(K19<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O19*Main!$D$45/100000+P18,IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S19))))),(IF(K19<=(Main!$D$72/Main!$D$71*100),O19*Main!$D$71/100000+P18,IF(K19<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O19*Main!$D$71/100000+P18,IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S19))))))","v":39.330639204043472},{"$f":"IF($A$90=TRUE,P19*Main!$D$45/100000+Q18,P19*100+Q18)","v":2.0269964825152806},{"$f":"IF($A$90=TRUE,(IF(K19<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K19-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K19<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K19<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K19-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K19<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K19-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K19<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K19<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K19-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O19*Main!$D$45/100000+P18,IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O19*Main!$D$45/100000+P18,Main!$E$52)))),(IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O19*Main!$D$71/100000+P18,IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O19*Main!$D$71/100000+P18,Main!$E$78)))))","v":39.330639204043472},18,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T19*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T19*PI()/50))))","v":701.87769580919678},{"$f":"IF($A$90=TRUE,U19*2*Main!$D$46/100000*(T19-T18)+V18,U19*2*Ltime1*(T19-T18)/100000+V18)","v":12.200503127398365},0.90482705246601958,0.30501257818495914,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W19*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W19>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W19*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W19>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W19*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W19>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W19*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W19>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W19*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W19>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W19*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W19>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":13.60934525305033},732.03018764390197]
[{"$f":"IF(deutsch,\"Stahl\",\"Steel\")","v":"Stahl"},1,"Aluminium",0.33,"Aluminium",0.33,"Aluminium",0.33,null,null,19,-0.26052244869821545,0.96070073671429879,0.61271923401816764,{"$f":"IF($A$90=TRUE,(IF(K20<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K20*PI()*Main!$D$45/100/Main!$D$46))),(IF(K20<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K20-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R20)))))))),(IF(K20<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K20*PI()*Main!$D$71/100/Main!$D$72))),(IF(K20<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K20-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R20)))))))))","v":-201.46832881669675},{"$f":"IF($A$90=TRUE,(IF(K20<=(Main!$D$46/Main!$D$45*100),O20*Main!$D$45/100000+P19,IF(K20<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O20*Main!$D$45/100000+P19,IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S20))))),(IF(K20<=(Main!$D$72/Main!$D$71*100),O20*Main!$D$71/100000+P19,IF(K20<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O20*Main!$D$71/100000+P19,IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S20))))))","v":38.361576542435159},{"$f":"IF($A$90=TRUE,P20*Main!$D$45/100000+Q19,P20*100+Q19)","v":2.2115156656843937},{"$f":"IF($A$90=TRUE,(IF(K20<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K20-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K20<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K20<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K20-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K20<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K20-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K20<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K20<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K20-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O20*Main!$D$45/100000+P19,IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O20*Main!$D$45/100000+P19,Main!$E$52)))),(IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O20*Main!$D$71/100000+P19,IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O20*Main!$D$71/100000+P19,Main!$E$78)))))","v":38.361576542435159},19,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T20*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T20*PI()/50))))","v":721.23106372013092},{"$f":"IF($A$90=TRUE,U20*2*Main!$D$46/100000*(T20-T19)+V19,U20*2*Ltime1*(T20-T19)/100000+V19)","v":13.368897450624978},0.92977648588825124,0.33422243626562442,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W20*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W20>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W20*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W20>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W20*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W20>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W20*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W20>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W20*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W20>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W20*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W20>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":13.984605312291205},802.13384703749864]
["Aluminium",0.33,null,null,null,null,null,null,null,null,20,-0.37340509595667792,0.92591680850179181,0.66199085623475817,{"$f":"IF($A$90=TRUE,(IF(K21<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K21*PI()*Main!$D$45/100/Main!$D$46))),(IF(K21<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K21-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R21)))))))),(IF(K21<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K21*PI()*Main!$D$71/100/Main!$D$72))),(IF(K21<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K21-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R21)))))))))","v":-288.76321802569294},{"$f":"IF($A$90=TRUE,(IF(K21<=(Main!$D$46/Main!$D$45*100),O21*Main!$D$45/100000+P20,IF(K21<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O21*Main!$D$45/100000+P20,IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S21))))),(IF(K21<=(Main!$D$72/Main!$D$71*100),O21*Main!$D$71/100000+P20,IF(K21<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O21*Main!$D$71/100000+P20,IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S21))))))","v":36.972625463731575},{"$f":"IF($A$90=TRUE,P21*Main!$D$45/100000+Q20,P21*100+Q20)","v":2.3893539941649427},{"$f":"IF($A$90=TRUE,(IF(K21<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K21-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K21<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K21<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K21-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K21<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K21-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K21<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K21<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K21-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O21*Main!$D$45/100000+P20,IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O21*Main!$D$45/100000+P20,Main!$E$52)))),(IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O21*Main!$D$71/100000+P20,IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O21*Main!$D$71/100000+P20,Main!$E$78)))))","v":36.972625463731575},20,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T21*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T21*PI()/50))))","v":737.73806212169245},{"$f":"IF($A$90=TRUE,U21*2*Main!$D$46/100000*(T21-T20)+V20,U21*2*Ltime1*(T21-T20)/100000+V20)","v":14.56403311126212},0.95105651629515353,0.364100827781553,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W21*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W21>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W21*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W21>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W21*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W21>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W21*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W21>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W21*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W21>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W21*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W21>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":14.304674523322911},873.84198667572718]
[{"$f":"IF(deutsch,\"Kupfer\",\"Copper\")","v":"Kupfer"},1.2,null,null,null,null,null,null,null,null,21,-0.47777746856187103,0.88141024619730335,0.70889411176452488,{"$f":"IF($A$90=TRUE,(IF(K22<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K22*PI()*Main!$D$45/100/Main!$D$46))),(IF(K22<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K22-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R22)))))))),(IF(K22<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K22*PI()*Main!$D$71/100/Main!$D$72))),(IF(K22<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K22-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R22)))))))))","v":-369.47690541990278},{"$f":"IF($A$90=TRUE,(IF(K22<=(Main!$D$46/Main!$D$45*100),O22*Main!$D$45/100000+P21,IF(K22<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O22*Main!$D$45/100000+P21,IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S22))))),(IF(K22<=(Main!$D$72/Main!$D$71*100),O22*Main!$D$71/100000+P21,IF(K22<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O22*Main!$D$71/100000+P21,IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S22))))))","v":35.19544154866184},{"$f":"IF($A$90=TRUE,P22*Main!$D$45/100000+Q21,P22*100+Q21)","v":2.5586440680140061},{"$f":"IF($A$90=TRUE,(IF(K22<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K22-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K22<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K22<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K22-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K22<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K22-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K22<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K22<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K22-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O22*Main!$D$45/100000+P21,IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O22*Main!$D$45/100000+P21,Main!$E$52)))),(IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O22*Main!$D$71/100000+P21,IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O22*Main!$D$71/100000+P21,Main!$E$78)))))","v":35.19544154866184},21,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T22*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T22*PI()/50))))","v":751.33354543252028},{"$f":"IF($A$90=TRUE,U22*2*Main!$D$46/100000*(T22-T21)+V21,U22*2*Ltime1*(T22-T21)/100000+V21)","v":15.781193454862802},0.96858316112863097,0.39452983637157002,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W22*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W22>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W22*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W22>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W22*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W22>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W22*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W22>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W22*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W22>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W22*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W22>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":14.568289719195208},946.8716072917681]
[{"$f":"IF(deutsch,\"Messing\",\"Brass\")","v":"Messing"},1.1000000000000001,null,null,null,null,null,null,null,null,22,-0.57126081601814871,0.82819539875639225,0.75296559900220861,{"$f":"IF($A$90=TRUE,(IF(K23<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K23*PI()*Main!$D$45/100/Main!$D$46))),(IF(K23<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K23-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R23)))))))),(IF(K23<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K23*PI()*Main!$D$71/100/Main!$D$72))),(IF(K23<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K23-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R23)))))))))","v":-441.76984554201778},{"$f":"IF($A$90=TRUE,(IF(K23<=(Main!$D$46/Main!$D$45*100),O23*Main!$D$45/100000+P22,IF(K23<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O23*Main!$D$45/100000+P22,IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S23))))),(IF(K23<=(Main!$D$72/Main!$D$71*100),O23*Main!$D$71/100000+P22,IF(K23<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O23*Main!$D$71/100000+P22,IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S23))))))","v":33.070528591604734},{"$f":"IF($A$90=TRUE,P23*Main!$D$45/100000+Q22,P23*100+Q22)","v":2.7177133105396249},{"$f":"IF($A$90=TRUE,(IF(K23<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K23-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K23<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K23<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K23-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K23<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K23-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K23<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K23<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K23-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O23*Main!$D$45/100000+P22,IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O23*Main!$D$45/100000+P22,Main!$E$52)))),(IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O23*Main!$D$71/100000+P22,IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O23*Main!$D$71/100000+P22,Main!$E$78)))))","v":33.070528591604734},22,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T23*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T23*PI()/50))))","v":761.96385849117235},{"$f":"IF($A$90=TRUE,U23*2*Main!$D$46/100000*(T23-T22)+V22,U23*2*Ltime1*(T23-T22)/100000+V22)","v":17.0155749056185},0.98228725072868861,0.4253893726404625,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W23*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W23>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W23*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W23>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W23*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W23>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W23*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W23>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W23*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W23>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W23*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W23>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":14.774410531164326},1020.93449433711]
[null,null,null,null,null,null,null,null,null,null,23,-0.65172455957611897,0.7674850856404366,0.79380645516695558,{"$f":"IF($A$90=TRUE,(IF(K24<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K24*PI()*Main!$D$45/100/Main!$D$46))),(IF(K24<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K24-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R24)))))))),(IF(K24<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K24*PI()*Main!$D$71/100/Main!$D$72))),(IF(K24<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K24-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R24)))))))))","v":-503.99441016576708},{"$f":"IF($A$90=TRUE,(IF(K24<=(Main!$D$46/Main!$D$45*100),O24*Main!$D$45/100000+P23,IF(K24<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O24*Main!$D$45/100000+P23,IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S24))))),(IF(K24<=(Main!$D$72/Main!$D$71*100),O24*Main!$D$71/100000+P23,IF(K24<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O24*Main!$D$71/100000+P23,IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S24))))))","v":30.646315478707393},{"$f":"IF($A$90=TRUE,P24*Main!$D$45/100000+Q23,P24*100+Q23)","v":2.8651220879922077},{"$f":"IF($A$90=TRUE,(IF(K24<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K24-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K24<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K24<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K24-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K24<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K24-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K24<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K24<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K24-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O24*Main!$D$45/100000+P23,IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O24*Main!$D$45/100000+P23,Main!$E$52)))),(IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O24*Main!$D$71/100000+P23,IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O24*Main!$D$71/100000+P23,Main!$E$78)))))","v":30.646315478707393},23,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T24*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T24*PI()/50))))","v":769.58704830853412},{"$f":"IF($A$90=TRUE,U24*2*Main!$D$46/100000*(T24-T23)+V23,U24*2*Ltime1*(T24-T23)/100000+V23)","v":18.262305923878326},0.99211470131447776,0.45655764809695815,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W24*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W24>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W24*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W24>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W24*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W24>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W24*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W24>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W24*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W24>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W24*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W24>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":14.922223494553066},1095.7383554326996]
[null,null,null,null,null,null,null,null,null,null,24,-0.71733485024785071,0.70066295545117563,0.83109144678300662,{"$f":"IF($A$90=TRUE,(IF(K25<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K25*PI()*Main!$D$45/100/Main!$D$46))),(IF(K25<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K25-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R25)))))))),(IF(K25<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K25*PI()*Main!$D$71/100/Main!$D$72))),(IF(K25<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K25-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R25)))))))))","v":-554.73243938690132},{"$f":"IF($A$90=TRUE,(IF(K25<=(Main!$D$46/Main!$D$45*100),O25*Main!$D$45/100000+P24,IF(K25<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O25*Main!$D$45/100000+P24,IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S25))))),(IF(K25<=(Main!$D$72/Main!$D$71*100),O25*Main!$D$71/100000+P24,IF(K25<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O25*Main!$D$71/100000+P24,IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S25))))))","v":27.978052445256399},{"$f":"IF($A$90=TRUE,P25*Main!$D$45/100000+Q24,P25*100+Q24)","v":2.9996965202538908},{"$f":"IF($A$90=TRUE,(IF(K25<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K25-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K25<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K25<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K25-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K25<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K25-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K25<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K25<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K25-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O25*Main!$D$45/100000+P24,IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O25*Main!$D$45/100000+P24,Main!$E$52)))),(IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O25*Main!$D$71/100000+P24,IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O25*Main!$D$71/100000+P24,Main!$E$78)))))","v":27.978052445256399},24,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T25*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T25*PI()/50))))","v":774.17302963710074},{"$f":"IF($A$90=TRUE,U25*2*Main!$D$46/100000*(T25-T24)+V24,U25*2*Ltime1*(T25-T24)/100000+V24)","v":19.51646623189043},0.99802672842827156,0.48791165579726076,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W25*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W25>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W25*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W25>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W25*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W25>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W25*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W25>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W25*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W25>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W25*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W25>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":15.011145259124239},1170.9879739134258]
[null,null,null,null,null,null,null,null,null,null,25,-0.76659636405479226,0.62925195119872068,0.86457638207506948,{"$f":"IF($A$90=TRUE,(IF(K26<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K26*PI()*Main!$D$45/100/Main!$D$46))),(IF(K26<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K26-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R26)))))))),(IF(K26<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K26*PI()*Main!$D$71/100/Main!$D$72))),(IF(K26<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K26-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R26)))))))))","v":-592.82756290219447},{"$f":"IF($A$90=TRUE,(IF(K26<=(Main!$D$46/Main!$D$45*100),O26*Main!$D$45/100000+P25,IF(K26<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O26*Main!$D$45/100000+P25,IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S26))))),(IF(K26<=(Main!$D$72/Main!$D$71*100),O26*Main!$D$71/100000+P25,IF(K26<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O26*Main!$D$71/100000+P25,IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S26))))))","v":25.126551867696843},{"$f":"IF($A$90=TRUE,P26*Main!$D$45/100000+Q25,P26*100+Q25)","v":3.1205552347375125},{"$f":"IF($A$90=TRUE,(IF(K26<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K26-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K26<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K26<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K26-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K26<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K26-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K26<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K26<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K26-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O26*Main!$D$45/100000+P25,IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O26*Main!$D$45/100000+P25,Main!$E$52)))),(IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O26*Main!$D$71/100000+P25,IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O26*Main!$D$71/100000+P25,Main!$E$78)))))","v":25.126551867696843},25,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T26*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T26*PI()/50))))","v":775.7037037037037},{"$f":"IF($A$90=TRUE,U26*2*Main!$D$46/100000*(T26-T25)+V25,U26*2*Ltime1*(T26-T25)/100000+V25)","v":20.773106231890431},1,0.51932765579726081,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W26*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W26>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W26*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W26>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W26*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W26>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W26*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W26>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W26*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W26>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W26*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W26>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":15.040824891297582},1246.386373913426]
[null,null,null,null,null,null,null,null,null,null,26,-0.79838638195300871,0.55487960091103605,0.89410367634248766,{"$f":"IF($A$90=TRUE,(IF(K27<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K27*PI()*Main!$D$45/100/Main!$D$46))),(IF(K27<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K27-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R27)))))))),(IF(K27<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K27*PI()*Main!$D$71/100/Main!$D$72))),(IF(K27<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K27-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R27)))))))))","v":-617.4115548422734},{"$f":"IF($A$90=TRUE,(IF(K27<=(Main!$D$46/Main!$D$45*100),O27*Main!$D$45/100000+P26,IF(K27<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O27*Main!$D$45/100000+P26,IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S27))))),(IF(K27<=(Main!$D$72/Main!$D$71*100),O27*Main!$D$71/100000+P26,IF(K27<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O27*Main!$D$71/100000+P26,IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S27))))))","v":22.15680228890551},{"$f":"IF($A$90=TRUE,P27*Main!$D$45/100000+Q26,P27*100+Q26)","v":3.227129453747148},{"$f":"IF($A$90=TRUE,(IF(K27<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K27-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K27<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K27<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K27-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K27<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K27-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K27<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K27<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K27-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O27*Main!$D$45/100000+P26,IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O27*Main!$D$45/100000+P26,Main!$E$52)))),(IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O27*Main!$D$71/100000+P26,IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O27*Main!$D$71/100000+P26,Main!$E$78)))))","v":22.15680228890551},26,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T27*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T27*PI()/50))))","v":774.17302963710074},{"$f":"IF($A$90=TRUE,U27*2*Main!$D$46/100000*(T27-T26)+V26,U27*2*Ltime1*(T27-T26)/100000+V26)","v":22.027266539902534},0.99802672842827156,0.55068166349756331,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W27*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W27>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W27*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W27>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W27*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W27>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W27*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W27>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W27*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W27>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W27*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W27>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":15.011145259124239},1321.635992394152]
[null,null,null,null,null,null,null,null,null,null,27,-0.81198037772024023,0.47924092464652723,0.9196059434717786,{"$f":"IF($A$90=TRUE,(IF(K28<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K28*PI()*Main!$D$45/100/Main!$D$46))),(IF(K28<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K28-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R28)))))))),(IF(K28<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K28*PI()*Main!$D$71/100/Main!$D$72))),(IF(K28<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K28-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R28)))))))))","v":-627.92412150534017},{"$f":"IF($A$90=TRUE,(IF(K28<=(Main!$D$46/Main!$D$45*100),O28*Main!$D$45/100000+P27,IF(K28<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O28*Main!$D$45/100000+P27,IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S28))))),(IF(K28<=(Main!$D$72/Main!$D$71*100),O28*Main!$D$71/100000+P27,IF(K28<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O28*Main!$D$71/100000+P27,IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S28))))))","v":19.136487264464826},{"$f":"IF($A$90=TRUE,P28*Main!$D$45/100000+Q27,P28*100+Q27)","v":3.3191759574892239},{"$f":"IF($A$90=TRUE,(IF(K28<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K28-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K28<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K28<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K28-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K28<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K28-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K28<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K28<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K28-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O28*Main!$D$45/100000+P27,IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O28*Main!$D$45/100000+P27,Main!$E$52)))),(IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O28*Main!$D$71/100000+P27,IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O28*Main!$D$71/100000+P27,Main!$E$78)))))","v":19.136487264464826},27,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T28*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T28*PI()/50))))","v":769.58704830853424},{"$f":"IF($A$90=TRUE,U28*2*Main!$D$46/100000*(T28-T27)+V27,U28*2*Ltime1*(T28-T27)/100000+V27)","v":23.27399755816236},0.99211470131447788,0.58184993895405901,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W28*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W28>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W28*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W28>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W28*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W28>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W28*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W28>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W28*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W28>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W28*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W28>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":14.922223494553066},1396.4398534897416]
[null,null,null,null,null,null,null,null,null,null,28,-0.80706853063130857,0.40405980329592345,0.94110753173338546,{"$f":"IF($A$90=TRUE,(IF(K29<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K29*PI()*Main!$D$45/100/Main!$D$46))),(IF(K29<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K29-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R29)))))))),(IF(K29<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K29*PI()*Main!$D$71/100/Main!$D$72))),(IF(K29<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K29-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R29)))))))))","v":-624.12567100959598},{"$f":"IF($A$90=TRUE,(IF(K29<=(Main!$D$46/Main!$D$45*100),O29*Main!$D$45/100000+P28,IF(K29<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O29*Main!$D$45/100000+P28,IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S29))))),(IF(K29<=(Main!$D$72/Main!$D$71*100),O29*Main!$D$71/100000+P28,IF(K29<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O29*Main!$D$71/100000+P28,IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S29))))))","v":16.134442786908668},{"$f":"IF($A$90=TRUE,P29*Main!$D$45/100000+Q28,P29*100+Q28)","v":3.3967826272942547},{"$f":"IF($A$90=TRUE,(IF(K29<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K29-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K29<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K29<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K29-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K29<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K29-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K29<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K29<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K29-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O29*Main!$D$45/100000+P28,IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O29*Main!$D$45/100000+P28,Main!$E$52)))),(IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O29*Main!$D$71/100000+P28,IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O29*Main!$D$71/100000+P28,Main!$E$78)))))","v":16.134442786908668},28,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T29*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T29*PI()/50))))","v":761.96385849117246},{"$f":"IF($A$90=TRUE,U29*2*Main!$D$46/100000*(T29-T28)+V28,U29*2*Ltime1*(T29-T28)/100000+V28)","v":24.508379008918059},0.98228725072868872,0.61270947522295149,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W29*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W29>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W29*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W29>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W29*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W29>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W29*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W29>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W29*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W29>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W29*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W29>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":14.77441053116433},1470.5027405350836]
["Bewegung",1.5708,null,null,null,null,null,null,null,null,29,-0.78376278658152754,0.33104968961700043,0.95872396886030353,{"$f":"IF($A$90=TRUE,(IF(K30<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K30*PI()*Main!$D$45/100/Main!$D$46))),(IF(K30<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K30-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R30)))))))),(IF(K30<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K30*PI()*Main!$D$71/100/Main!$D$72))),(IF(K30<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K30-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R30)))))))))","v":-606.10277383124924},{"$f":"IF($A$90=TRUE,(IF(K30<=(Main!$D$46/Main!$D$45*100),O30*Main!$D$45/100000+P29,IF(K30<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O30*Main!$D$45/100000+P29,IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S30))))),(IF(K30<=(Main!$D$72/Main!$D$71*100),O30*Main!$D$71/100000+P29,IF(K30<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O30*Main!$D$71/100000+P29,IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S30))))))","v":13.219088444780359},{"$f":"IF($A$90=TRUE,P30*Main!$D$45/100000+Q29,P30*100+Q29)","v":3.4603664427136485},{"$f":"IF($A$90=TRUE,(IF(K30<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K30-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K30<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K30<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K30-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K30<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K30-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K30<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K30<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K30-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O30*Main!$D$45/100000+P29,IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O30*Main!$D$45/100000+P29,Main!$E$52)))),(IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O30*Main!$D$71/100000+P29,IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O30*Main!$D$71/100000+P29,Main!$E$78)))))","v":13.219088444780359},29,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T30*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T30*PI()/50))))","v":751.33354543252028},{"$f":"IF($A$90=TRUE,U30*2*Main!$D$46/100000*(T30-T29)+V29,U30*2*Ltime1*(T30-T29)/100000+V29)","v":25.725539352518741},0.96858316112863097,0.64313848381296856,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W30*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W30>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W30*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W30>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W30*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W30>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W30*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W30>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W30*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W30>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W30*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W30>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":14.568289719195208},1543.5323611511246]
[true,null,null,null,null,null,null,null,null,null,30,-0.74259430672806936,0.26187455693685546,0.97265932905579222,{"$f":"IF($A$90=TRUE,(IF(K31<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K31*PI()*Main!$D$45/100/Main!$D$46))),(IF(K31<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K31-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R31)))))))),(IF(K31<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K31*PI()*Main!$D$71/100/Main!$D$72))),(IF(K31<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K31-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R31)))))))))","v":-574.26618977699809},{"$f":"IF($A$90=TRUE,(IF(K31<=(Main!$D$46/Main!$D$45*100),O31*Main!$D$45/100000+P30,IF(K31<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O31*Main!$D$45/100000+P30,IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S31))))),(IF(K31<=(Main!$D$72/Main!$D$71*100),O31*Main!$D$71/100000+P30,IF(K31<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O31*Main!$D$71/100000+P30,IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S31))))))","v":10.456868071952998},{"$f":"IF($A$90=TRUE,P31*Main!$D$45/100000+Q30,P31*100+Q30)","v":3.5106639781397422},{"$f":"IF($A$90=TRUE,(IF(K31<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K31-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K31<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K31<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K31-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K31<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K31-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K31<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K31<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K31-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O31*Main!$D$45/100000+P30,IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O31*Main!$D$45/100000+P30,Main!$E$52)))),(IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O31*Main!$D$71/100000+P30,IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O31*Main!$D$71/100000+P30,Main!$E$78)))))","v":10.456868071952998},30,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T31*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T31*PI()/50))))","v":737.73806212169245},{"$f":"IF($A$90=TRUE,U31*2*Main!$D$46/100000*(T31-T30)+V30,U31*2*Ltime1*(T31-T30)/100000+V30)","v":26.920675013155883},0.95105651629515353,0.67301687532889709,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W31*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W31>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W31*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W31>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W31*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W31>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W31*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W31>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W31*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W31>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W31*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W31>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":14.304674523322911},1615.2405007893531]
[null,null,null,null,null,null,null,null,null,null,31,-0.68450136179729648,0.19811097553976942,0.98320158193869456,{"$f":"IF($A$90=TRUE,(IF(K32<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K32*PI()*Main!$D$45/100/Main!$D$46))),(IF(K32<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K32-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R32)))))))),(IF(K32<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K32*PI()*Main!$D$71/100/Main!$D$72))),(IF(K32<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K32-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R32)))))))))","v":-529.34150635825449},{"$f":"IF($A$90=TRUE,(IF(K32<=(Main!$D$46/Main!$D$45*100),O32*Main!$D$45/100000+P31,IF(K32<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O32*Main!$D$45/100000+P31,IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S32))))),(IF(K32<=(Main!$D$72/Main!$D$71*100),O32*Main!$D$71/100000+P31,IF(K32<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O32*Main!$D$71/100000+P31,IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S32))))))","v":7.9107354263697944},{"$f":"IF($A$90=TRUE,P32*Main!$D$45/100000+Q31,P32*100+Q31)","v":3.5487146155405811},{"$f":"IF($A$90=TRUE,(IF(K32<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K32-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K32<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K32<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K32-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K32<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K32-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K32<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K32<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K32-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O32*Main!$D$45/100000+P31,IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O32*Main!$D$45/100000+P31,Main!$E$52)))),(IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O32*Main!$D$71/100000+P31,IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O32*Main!$D$71/100000+P31,Main!$E$78)))))","v":7.9107354263697944},31,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T32*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T32*PI()/50))))","v":721.23106372013103},{"$f":"IF($A$90=TRUE,U32*2*Main!$D$46/100000*(T32-T31)+V31,U32*2*Ltime1*(T32-T31)/100000+V31)","v":28.089069336382494},0.92977648588825146,0.70222673340956232,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W32*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W32>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W32*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W32>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W32*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W32>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W32*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W32>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W32*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W32>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W32*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W32>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":13.984605312291206},1685.3441601829495]
[null,null,null,null,null,null,null,null,null,null,32,-0.61080794795886884,0.1412121810576103,0.99071602942853931,{"$f":"IF($A$90=TRUE,(IF(K33<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K33*PI()*Main!$D$45/100/Main!$D$46))),(IF(K33<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K33-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R33)))))))),(IF(K33<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K33*PI()*Main!$D$71/100/Main!$D$72))),(IF(K33<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K33-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R33)))))))))","v":-472.35260192789724},{"$f":"IF($A$90=TRUE,(IF(K33<=(Main!$D$46/Main!$D$45*100),O33*Main!$D$45/100000+P32,IF(K33<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O33*Main!$D$45/100000+P32,IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S33))))),(IF(K33<=(Main!$D$72/Main!$D$71*100),O33*Main!$D$71/100000+P32,IF(K33<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O33*Main!$D$71/100000+P32,IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S33))))))","v":5.6387194110966092},{"$f":"IF($A$90=TRUE,P33*Main!$D$45/100000+Q32,P33*100+Q32)","v":3.5758368559079559},{"$f":"IF($A$90=TRUE,(IF(K33<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K33-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K33<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K33<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K33-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K33<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K33-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K33<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K33<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K33-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O33*Main!$D$45/100000+P32,IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O33*Main!$D$45/100000+P32,Main!$E$52)))),(IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O33*Main!$D$71/100000+P32,IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O33*Main!$D$71/100000+P32,Main!$E$78)))))","v":5.6387194110966092},32,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T33*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T33*PI()/50))))","v":701.87769580919667},{"$f":"IF($A$90=TRUE,U33*2*Main!$D$46/100000*(T33-T32)+V32,U33*2*Ltime1*(T33-T32)/100000+V32)","v":29.226111203593391},0.90482705246601935,0.73065278008983481,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W33*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W33>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W33*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W33>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W33*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W33>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W33*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W33>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W33*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W33>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W33*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W33>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":13.609345253050327},1753.5666722156036]
[null,null,null,null,null,null,null,null,null,null,33,-0.52319361163219202,9.2474953780005684E-2,0.9956369801503625,{"$f":"IF($A$90=TRUE,(IF(K34<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K34*PI()*Main!$D$45/100/Main!$D$46))),(IF(K34<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K34-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R34)))))))),(IF(K34<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K34*PI()*Main!$D$71/100/Main!$D$72))),(IF(K34<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K34-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R34)))))))))","v":-404.59831047116836},{"$f":"IF($A$90=TRUE,(IF(K34<=(Main!$D$46/Main!$D$45*100),O34*Main!$D$45/100000+P33,IF(K34<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O34*Main!$D$45/100000+P33,IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S34))))),(IF(K34<=(Main!$D$72/Main!$D$71*100),O34*Main!$D$71/100000+P33,IF(K34<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O34*Main!$D$71/100000+P33,IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S34))))))","v":3.6926015377302894},{"$f":"IF($A$90=TRUE,P34*Main!$D$45/100000+Q33,P34*100+Q33)","v":3.5935982693044384},{"$f":"IF($A$90=TRUE,(IF(K34<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K34-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K34<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K34<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K34-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K34<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K34-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K34<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K34<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K34-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O34*Main!$D$45/100000+P33,IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O34*Main!$D$45/100000+P33,Main!$E$52)))),(IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O34*Main!$D$71/100000+P33,IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O34*Main!$D$71/100000+P33,Main!$E$78)))))","v":3.6926015377302894},33,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T34*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T34*PI()/50))))","v":679.75433729032136},{"$f":"IF($A$90=TRUE,U34*2*Main!$D$46/100000*(T34-T33)+V33,U34*2*Ltime1*(T34-T33)/100000+V33)","v":30.32731323000371},0.87630668004386347,0.75818283075009274,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W34*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W34>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W34*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W34>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W34*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W34>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W34*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W34>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W34*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W34>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W34*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W34>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":13.18037532561409},1819.6387938002226]
[true,null,null,null,null,null,null,null,null,null,34,-0.42365517094797217,5.3010063737848112E-2,0.99845785110786767,{"$f":"IF($A$90=TRUE,(IF(K35<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K35*PI()*Main!$D$45/100/Main!$D$46))),(IF(K35<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K35-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R35)))))))),(IF(K35<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K35*PI()*Main!$D$71/100/Main!$D$72))),(IF(K35<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K35-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R35)))))))))","v":-327.62281988340834},{"$f":"IF($A$90=TRUE,(IF(K35<=(Main!$D$46/Main!$D$45*100),O35*Main!$D$45/100000+P34,IF(K35<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O35*Main!$D$45/100000+P34,IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S35))))),(IF(K35<=(Main!$D$72/Main!$D$71*100),O35*Main!$D$71/100000+P34,IF(K35<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O35*Main!$D$71/100000+P34,IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S35))))))","v":2.1167357740910955},{"$f":"IF($A$90=TRUE,P35*Main!$D$45/100000+Q34,P35*100+Q34)","v":3.6037797683778163},{"$f":"IF($A$90=TRUE,(IF(K35<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K35-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K35<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K35<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K35-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K35<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K35-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K35<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K35<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K35-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O35*Main!$D$45/100000+P34,IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O35*Main!$D$45/100000+P34,Main!$E$52)))),(IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O35*Main!$D$71/100000+P34,IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O35*Main!$D$71/100000+P34,Main!$E$78)))))","v":2.1167357740910955},34,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T35*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T35*PI()/50))))","v":654.94829895237785},{"$f":"IF($A$90=TRUE,U35*2*Main!$D$46/100000*(T35-T34)+V34,U35*2*Ltime1*(T35-T34)/100000+V34)","v":31.388329474306563},0.84432792550201496,0.78470823685766411,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W35*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W35>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W35*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W35>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W35*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W35>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W35*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W35>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W35*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W35>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W35*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W35>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.699388478308357},1883.2997684583938]
[null,null,null,null,null,null,null,null,null,null,35,-0.31446120627094748,2.3716955146164644E-2,0.99971992221766903,{"$f":"IF($A$90=TRUE,(IF(K36<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K36*PI()*Main!$D$45/100/Main!$D$46))),(IF(K36<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K36-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R36)))))))),(IF(K36<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K36*PI()*Main!$D$71/100/Main!$D$72))),(IF(K36<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K36-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R36)))))))))","v":-243.18047838740554},{"$f":"IF($A$90=TRUE,(IF(K36<=(Main!$D$46/Main!$D$45*100),O36*Main!$D$45/100000+P35,IF(K36<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O36*Main!$D$45/100000+P35,IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S36))))),(IF(K36<=(Main!$D$72/Main!$D$71*100),O36*Main!$D$71/100000+P35,IF(K36<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O36*Main!$D$71/100000+P35,IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S36))))))","v":0.94703767304767483},{"$f":"IF($A$90=TRUE,P36*Main!$D$45/100000+Q35,P36*100+Q35)","v":3.6083350195851756},{"$f":"IF($A$90=TRUE,(IF(K36<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K36-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K36<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K36<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K36-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K36<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K36-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K36<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K36<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K36-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O36*Main!$D$45/100000+P35,IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O36*Main!$D$45/100000+P35,Main!$E$52)))),(IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O36*Main!$D$71/100000+P35,IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O36*Main!$D$71/100000+P35,Main!$E$78)))))","v":0.94703767304767483},35,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T36*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T36*PI()/50))))","v":627.5574788958852},{"$f":"IF($A$90=TRUE,U36*2*Main!$D$46/100000*(T36-T35)+V35,U36*2*Ltime1*(T36-T35)/100000+V35)","v":32.404972590117893},0.80901699437494745,0.81012431475294733,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W36*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W36>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W36*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W36>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W36*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W36>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W36*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W36>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W36*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W36>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W36*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W36>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.168282946477467},1944.2983554070736]
[null,null,null,null,null,null,null,null,null,null,36,-0.19810035699019821,5.2632471731526992E-3,1,{"$f":"IF($A$90=TRUE,(IF(K37<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K37*PI()*Main!$D$45/100/Main!$D$46))),(IF(K37<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K37-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R37)))))))),(IF(K37<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K37*PI()*Main!$D$71/100/Main!$D$72))),(IF(K37<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K37-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R37)))))))))","v":-153.1958111872286},{"$f":"IF($A$90=TRUE,(IF(K37<=(Main!$D$46/Main!$D$45*100),O37*Main!$D$45/100000+P36,IF(K37<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O37*Main!$D$45/100000+P36,IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S37))))),(IF(K37<=(Main!$D$72/Main!$D$71*100),O37*Main!$D$71/100000+P36,IF(K37<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O37*Main!$D$71/100000+P36,IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S37))))))","v":0.21016582123710537},{"$f":"IF($A$90=TRUE,P37*Main!$D$45/100000+Q36,P37*100+Q36)","v":3.6093459171853262},{"$f":"IF($A$90=TRUE,(IF(K37<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K37-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K37<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K37<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K37-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K37<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K37-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K37<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K37<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K37-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O37*Main!$D$45/100000+P36,IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O37*Main!$D$45/100000+P36,Main!$E$52)))),(IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O37*Main!$D$71/100000+P36,IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O37*Main!$D$71/100000+P36,Main!$E$78)))))","v":0.21016582123710537},36,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T37*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T37*PI()/50))))","v":597.68997617393075},{"$f":"IF($A$90=TRUE,U37*2*Main!$D$46/100000*(T37-T36)+V36,U37*2*Ltime1*(T37-T36)/100000+V36)","v":33.373230351519659},0.77051324277578925,0.83433075878799146,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W37*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W37>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W37*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W37>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W37*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W37>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W37*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W37>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W37*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W37>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W37*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W37>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.589154761016509},2002.3938210911795]
[null,null,null,null,null,null,null,null,null,null,37,-7.7224602944750476E-2,-1.9304817666933563E-3,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K38<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K38*PI()*Main!$D$45/100/Main!$D$46))),(IF(K38<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K38-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R38)))))))),(IF(K38<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K38*PI()*Main!$D$71/100/Main!$D$72))),(IF(K38<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K38-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R38)))))))))","v":-59.719658618878967},{"$f":"IF($A$90=TRUE,(IF(K38<=(Main!$D$46/Main!$D$45*100),O38*Main!$D$45/100000+P37,IF(K38<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O38*Main!$D$45/100000+P37,IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S38))))),(IF(K38<=(Main!$D$72/Main!$D$71*100),O38*Main!$D$71/100000+P37,IF(K38<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O38*Main!$D$71/100000+P37,IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S38))))))","v":-7.708573671970248E-2},{"$f":"IF($A$90=TRUE,P38*Main!$D$45/100000+Q37,P38*100+Q37)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K38<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K38-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K38<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K38<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K38-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K38<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K38-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K38<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K38<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K38-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O38*Main!$D$45/100000+P37,IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O38*Main!$D$45/100000+P37,Main!$E$52)))),(IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O38*Main!$D$71/100000+P37,IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O38*Main!$D$71/100000+P37,Main!$E$78)))))","v":-7.708573671970248E-2},37,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T38*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T38*PI()/50))))","v":565.4636641745941},{"$f":"IF($A$90=TRUE,U38*2*Main!$D$46/100000*(T38-T37)+V37,U38*2*Ltime1*(T38-T37)/100000+V37)","v":34.289281487482505},0.72896862742141144,0.85723203718706265,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W38*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W38>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W38*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W38>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W38*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W38>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W38*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W38>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W38*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W38>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W38*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W38>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":10.964289476294999},2057.3568892489502]
[null,"bk","copy","bk","copy",null,null,null,null,null,38,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K39<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K39*PI()*Main!$D$45/100/Main!$D$46))),(IF(K39<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K39-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R39)))))))),(IF(K39<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K39*PI()*Main!$D$71/100/Main!$D$72))),(IF(K39<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K39-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R39)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K39<=(Main!$D$46/Main!$D$45*100),O39*Main!$D$45/100000+P38,IF(K39<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O39*Main!$D$45/100000+P38,IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S39))))),(IF(K39<=(Main!$D$72/Main!$D$71*100),O39*Main!$D$71/100000+P38,IF(K39<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O39*Main!$D$71/100000+P38,IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S39))))))","v":0},{"$f":"IF($A$90=TRUE,P39*Main!$D$45/100000+Q38,P39*100+Q38)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K39<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K39-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K39<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K39<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K39-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K39<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K39-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K39<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K39<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K39-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O39*Main!$D$45/100000+P38,IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O39*Main!$D$45/100000+P38,Main!$E$52)))),(IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O39*Main!$D$71/100000+P38,IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O39*Main!$D$71/100000+P38,Main!$E$78)))))","v":-7.708573671970248E-2},38,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T39*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T39*PI()/50))))","v":531.00572542853547},{"$f":"IF($A$90=TRUE,U39*2*Main!$D$46/100000*(T39-T38)+V38,U39*2*Ltime1*(T39-T38)/100000+V38)","v":35.149510762676734},0.68454710592868884,0.87873776906691836,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W39*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W39>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W39*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W39>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W39*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W39>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W39*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W39>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W39*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W39>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W39*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W39>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":10.296153150117947},2108.9706457606039]
[{"$f":"AND((AutoCalcRot=TRUE),(AutoCalcLin=TRUE))","v":true},81,{"$f":"time1","v":81},50,{"$f":"Ltime1","v":50},null,null,null,null,null,39,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K40<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K40*PI()*Main!$D$45/100/Main!$D$46))),(IF(K40<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K40-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R40)))))))),(IF(K40<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K40*PI()*Main!$D$71/100/Main!$D$72))),(IF(K40<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K40-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R40)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K40<=(Main!$D$46/Main!$D$45*100),O40*Main!$D$45/100000+P39,IF(K40<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O40*Main!$D$45/100000+P39,IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S40))))),(IF(K40<=(Main!$D$72/Main!$D$71*100),O40*Main!$D$71/100000+P39,IF(K40<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O40*Main!$D$71/100000+P39,IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S40))))))","v":0},{"$f":"IF($A$90=TRUE,P40*Main!$D$45/100000+Q39,P40*100+Q39)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K40<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K40-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K40<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K40<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K40-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K40<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K40-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K40<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K40<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K40-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O40*Main!$D$45/100000+P39,IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O40*Main!$D$45/100000+P39,Main!$E$52)))),(IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O40*Main!$D$71/100000+P39,IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O40*Main!$D$71/100000+P39,Main!$E$78)))))","v":0},39,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T40*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T40*PI()/50))))","v":494.45214967765037},{"$f":"IF($A$90=TRUE,U40*2*Main!$D$46/100000*(T40-T39)+V39,U40*2*Ltime1*(T40-T39)/100000+V39)","v":35.950523245154528},0.63742398974868986,0.89876308112886316,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W40*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W40>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W40*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W40>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W40*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W40>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W40*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W40>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W40*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W40>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W40*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W40>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9.58738261132231},2157.0313947092718]
[{"$f":"AND((ctime1=btime1),(ctime2=btime2),(ctime3=btime3),(ctime4=btime4),(ctime5=btime5),(ctime6=btime6),(ctime7=btime7),(ctime8=btime8),(cspeed1=bspeed1),(cspeed2=bspeed2),(cspeed6=bspeed6),(cinertia=bInertia),(cinertia2=binertia2),(ctorque=btorque),(ctorque2=btorque2),(cgear=bgear),(cgear_inertia=bgear_inertia),(cWirkungsgrad=bWirkungsgrad),(cULU=bULU),(cDryTorq=bDryTorq),(cDryTorq2=bDryTorq2))","v":true},0,{"$f":"time2","v":0},0,{"$f":"Ltime2","v":0},null,null,null,null,null,40,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K41<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K41*PI()*Main!$D$45/100/Main!$D$46))),(IF(K41<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K41-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R41)))))))),(IF(K41<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K41*PI()*Main!$D$71/100/Main!$D$72))),(IF(K41<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K41-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R41)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K41<=(Main!$D$46/Main!$D$45*100),O41*Main!$D$45/100000+P40,IF(K41<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O41*Main!$D$45/100000+P40,IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S41))))),(IF(K41<=(Main!$D$72/Main!$D$71*100),O41*Main!$D$71/100000+P40,IF(K41<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O41*Main!$D$71/100000+P40,IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S41))))))","v":0},{"$f":"IF($A$90=TRUE,P41*Main!$D$45/100000+Q40,P41*100+Q40)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K41<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K41-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K41<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K41<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K41-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K41<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K41-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K41<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K41<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K41-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O41*Main!$D$45/100000+P40,IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O41*Main!$D$45/100000+P40,Main!$E$52)))),(IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O41*Main!$D$71/100000+P40,IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O41*Main!$D$71/100000+P40,Main!$E$78)))))","v":0},40,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T41*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T41*PI()/50))))","v":455.9471971856874},{"$f":"IF($A$90=TRUE,U41*2*Main!$D$46/100000*(T41-T40)+V40,U41*2*Ltime1*(T41-T40)/100000+V40)","v":36.689157704595338},0.58778525229247325,0.91722894261488341,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W41*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W41>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W41*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W41>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W41*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W41>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W41*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W41>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W41*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W41>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W41*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W41>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":8.8407750534182608},2201.3494622757203]
[{"$f":"AND((cltime1=bltime1),(cltime2=bltime2),(cltime3=bltime3),(cltime4=bltime4),(cltime5=bltime5),(cltime6=bltime6),(cltime7=bltime7),(cltime8=bltime8),(clspeed1=blspeed1),(clspeed2=blspeed2),(clspeed6=blspeed6),(cltorque=bltorque),(cltorque2=bltorque2),(cgewicht=bgewicht),(cgewicht2=bgewicht2),(clwirkungsgrad=blwirkungsgrad),(clDryTorq=blDrytorq),(clDryTorq2=blDryTorq2))","v":true},100,{"$f":"time3","v":100},30,{"$f":"Ltime3","v":30},null,null,null,null,null,41,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K42<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K42*PI()*Main!$D$45/100/Main!$D$46))),(IF(K42<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K42-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R42)))))))),(IF(K42<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K42*PI()*Main!$D$71/100/Main!$D$72))),(IF(K42<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K42-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R42)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K42<=(Main!$D$46/Main!$D$45*100),O42*Main!$D$45/100000+P41,IF(K42<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O42*Main!$D$45/100000+P41,IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S42))))),(IF(K42<=(Main!$D$72/Main!$D$71*100),O42*Main!$D$71/100000+P41,IF(K42<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O42*Main!$D$71/100000+P41,IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S42))))))","v":0},{"$f":"IF($A$90=TRUE,P42*Main!$D$45/100000+Q41,P42*100+Q41)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K42<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K42-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K42<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K42<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K42-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K42<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K42-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K42<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K42<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K42-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O42*Main!$D$45/100000+P41,IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O42*Main!$D$45/100000+P41,Main!$E$52)))),(IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O42*Main!$D$71/100000+P41,IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O42*Main!$D$71/100000+P41,Main!$E$78)))))","v":0},41,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T42*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T42*PI()/50))))","v":415.64282940889308},{"$f":"IF($A$90=TRUE,U42*2*Main!$D$46/100000*(T42-T41)+V41,U42*2*Ltime1*(T42-T41)/100000+V41)","v":37.362499088237747},0.53582679497899699,0.93406247720594371,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W42*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W42>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W42*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W42>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W42*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W42>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W42*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W42>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W42*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W42>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W42*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W42>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":8.0592769953443053},2241.7499452942648]
[null,300,{"$f":"time4","v":300},50,{"$f":"Ltime4","v":50},null,null,null,null,null,42,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K43<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K43*PI()*Main!$D$45/100/Main!$D$46))),(IF(K43<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K43-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R43)))))))),(IF(K43<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K43*PI()*Main!$D$71/100/Main!$D$72))),(IF(K43<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K43-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R43)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K43<=(Main!$D$46/Main!$D$45*100),O43*Main!$D$45/100000+P42,IF(K43<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O43*Main!$D$45/100000+P42,IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S43))))),(IF(K43<=(Main!$D$72/Main!$D$71*100),O43*Main!$D$71/100000+P42,IF(K43<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O43*Main!$D$71/100000+P42,IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S43))))))","v":0},{"$f":"IF($A$90=TRUE,P43*Main!$D$45/100000+Q42,P43*100+Q42)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K43<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K43-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K43<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K43<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K43-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K43<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K43-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K43<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K43<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K43-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O43*Main!$D$45/100000+P42,IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O43*Main!$D$45/100000+P42,Main!$E$52)))),(IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O43*Main!$D$71/100000+P42,IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O43*Main!$D$71/100000+P42,Main!$E$78)))))","v":0},42,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T43*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T43*PI()/50))))","v":373.69810927356752},{"$f":"IF($A$90=TRUE,U43*2*Main!$D$46/100000*(T43-T42)+V42,U43*2*Ltime1*(T43-T42)/100000+V42)","v":37.967890025260928},0.48175367410171521,0.94919725063152316,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W43*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W43>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W43*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W43>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W43*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W43>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W43*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W43>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W43*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W43>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W43*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W43>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.2459726529031423},2278.0734015156554]
[null,0,{"$f":"speed1","v":0},0,{"$f":"Lspeed1","v":0},null,null,null,null,null,43,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K44<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K44*PI()*Main!$D$45/100/Main!$D$46))),(IF(K44<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K44-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R44)))))))),(IF(K44<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K44*PI()*Main!$D$71/100/Main!$D$72))),(IF(K44<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K44-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R44)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K44<=(Main!$D$46/Main!$D$45*100),O44*Main!$D$45/100000+P43,IF(K44<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O44*Main!$D$45/100000+P43,IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S44))))),(IF(K44<=(Main!$D$72/Main!$D$71*100),O44*Main!$D$71/100000+P43,IF(K44<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O44*Main!$D$71/100000+P43,IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S44))))))","v":0},{"$f":"IF($A$90=TRUE,P44*Main!$D$45/100000+Q43,P44*100+Q43)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K44<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K44-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K44<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K44<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K44-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K44<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K44-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K44<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K44<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K44-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O44*Main!$D$45/100000+P43,IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O44*Main!$D$45/100000+P43,Main!$E$52)))),(IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O44*Main!$D$71/100000+P43,IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O44*Main!$D$71/100000+P43,Main!$E$78)))))","v":0},43,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T44*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T44*PI()/50))))","v":330.27857342736615},{"$f":"IF($A$90=TRUE,U44*2*Main!$D$46/100000*(T44-T43)+V43,U44*2*Ltime1*(T44-T43)/100000+V43)","v":38.50294131421326},0.42577929156507288,0.96257353285533154,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W44*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W44>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W44*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W44>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W44*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W44>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W44*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W44>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W44*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W44>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W44*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W44>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":6.4040717667709988},2310.1764788527958]
[null,2400,{"$f":"speed2","v":2400},1,{"$f":"Lspeed2","v":1},null,null,null,null,null,44,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K45<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K45*PI()*Main!$D$45/100/Main!$D$46))),(IF(K45<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K45-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R45)))))))),(IF(K45<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K45*PI()*Main!$D$71/100/Main!$D$72))),(IF(K45<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K45-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R45)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K45<=(Main!$D$46/Main!$D$45*100),O45*Main!$D$45/100000+P44,IF(K45<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O45*Main!$D$45/100000+P44,IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S45))))),(IF(K45<=(Main!$D$72/Main!$D$71*100),O45*Main!$D$71/100000+P44,IF(K45<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O45*Main!$D$71/100000+P44,IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S45))))))","v":0},{"$f":"IF($A$90=TRUE,P45*Main!$D$45/100000+Q44,P45*100+Q44)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K45<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K45-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K45<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K45<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K45-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K45<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K45-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K45<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K45<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K45-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O45*Main!$D$45/100000+P44,IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O45*Main!$D$45/100000+P44,Main!$E$52)))),(IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O45*Main!$D$71/100000+P44,IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O45*Main!$D$71/100000+P44,Main!$E$78)))))","v":0},44,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T45*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T45*PI()/50))))","v":285.55557894177406},{"$f":"IF($A$90=TRUE,U45*2*Main!$D$46/100000*(T45-T44)+V44,U45*2*Ltime1*(T45-T44)/100000+V44)","v":38.965541352098931},0.3681245526846782,0.97413853380247328,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W45*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W45>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W45*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W45>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W45*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W45>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W45*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W45>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W45*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W45>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W45*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W45>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":5.5368969351174968},2337.9324811259357]
[null,25,{"$f":"inertia","v":25},5,{"$f":"Gewicht","v":5},null,null,null,null,null,45,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K46<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K46*PI()*Main!$D$45/100/Main!$D$46))),(IF(K46<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K46-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R46)))))))),(IF(K46<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K46*PI()*Main!$D$71/100/Main!$D$72))),(IF(K46<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K46-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R46)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K46<=(Main!$D$46/Main!$D$45*100),O46*Main!$D$45/100000+P45,IF(K46<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O46*Main!$D$45/100000+P45,IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S46))))),(IF(K46<=(Main!$D$72/Main!$D$71*100),O46*Main!$D$71/100000+P45,IF(K46<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O46*Main!$D$71/100000+P45,IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S46))))))","v":0},{"$f":"IF($A$90=TRUE,P46*Main!$D$45/100000+Q45,P46*100+Q45)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K46<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K46-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K46<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K46<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K46-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K46<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K46-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K46<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K46<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K46-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O46*Main!$D$45/100000+P45,IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O46*Main!$D$45/100000+P45,Main!$E$52)))),(IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O46*Main!$D$71/100000+P45,IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O46*Main!$D$71/100000+P45,Main!$E$78)))))","v":0},46,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T46*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T46*PI()/50))))","v":192.90966654743437},{"$f":"IF($A$90=TRUE,U46*2*Main!$D$46/100000*(T46-T45)+V45,U46*2*Ltime1*(T46-T45)/100000+V45)","v":39.590568671712617},0.24868988716485524,0.98976421679281545,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W46*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W46>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W46*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W46>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W46*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W46>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W46*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W46>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W46*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W46>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W46*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W46>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":3.7405010450831417},2375.434120302757]
[null,0,{"$f":"torque","v":0},0,{"$f":"Ltorque","v":0},null,null,null,null,null,46,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K47<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K47*PI()*Main!$D$45/100/Main!$D$46))),(IF(K47<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K47-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R47)))))))),(IF(K47<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K47*PI()*Main!$D$71/100/Main!$D$72))),(IF(K47<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K47-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R47)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K47<=(Main!$D$46/Main!$D$45*100),O47*Main!$D$45/100000+P46,IF(K47<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O47*Main!$D$45/100000+P46,IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S47))))),(IF(K47<=(Main!$D$72/Main!$D$71*100),O47*Main!$D$71/100000+P46,IF(K47<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O47*Main!$D$71/100000+P46,IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S47))))))","v":0},{"$f":"IF($A$90=TRUE,P47*Main!$D$45/100000+Q46,P47*100+Q46)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K47<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K47-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K47<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K47<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K47-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K47<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K47-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K47<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K47<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K47-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O47*Main!$D$45/100000+P46,IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O47*Main!$D$45/100000+P46,Main!$E$52)))),(IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O47*Main!$D$71/100000+P46,IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O47*Main!$D$71/100000+P46,Main!$E$78)))))","v":0},48,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T47*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T47*PI()/50))))","v":97.22145347299238},{"$f":"IF($A$90=TRUE,U47*2*Main!$D$46/100000*(T47-T46)+V46,U47*2*Ltime1*(T47-T46)/100000+V46)","v":39.90556618096511},0.12533323356430454,0.99763915452412777,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W47*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W47>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W47*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W47>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W47*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W47>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W47*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W47>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W47*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W47>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W47*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W47>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":1.8851152191008054},2394.3339708579065]
[null,1,{"$f":"gear","v":1},1,{"$f":"LWirkungsgrad","v":1},null,null,null,null,null,47,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K48<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K48*PI()*Main!$D$45/100/Main!$D$46))),(IF(K48<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K48-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R48)))))))),(IF(K48<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K48*PI()*Main!$D$71/100/Main!$D$72))),(IF(K48<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K48-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R48)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K48<=(Main!$D$46/Main!$D$45*100),O48*Main!$D$45/100000+P47,IF(K48<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O48*Main!$D$45/100000+P47,IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S48))))),(IF(K48<=(Main!$D$72/Main!$D$71*100),O48*Main!$D$71/100000+P47,IF(K48<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O48*Main!$D$71/100000+P47,IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S48))))))","v":0},{"$f":"IF($A$90=TRUE,P48*Main!$D$45/100000+Q47,P48*100+Q47)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K48<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K48-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K48<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K48<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K48-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K48<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K48-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K48<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K48<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K48-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O48*Main!$D$45/100000+P47,IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O48*Main!$D$45/100000+P47,Main!$E$52)))),(IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O48*Main!$D$71/100000+P47,IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O48*Main!$D$71/100000+P47,Main!$E$78)))))","v":0},49,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T48*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T48*PI()/50))))","v":48.706838556368282},{"$f":"IF($A$90=TRUE,U48*2*Main!$D$46/100000*(T48-T47)+V47,U48*2*Ltime1*(T48-T47)/100000+V47)","v":39.984471259426428},6.2790519529313582E-2,0.99961178148566066,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W48*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W48>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W48*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W48>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W48*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W48>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W48*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W48>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W48*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W48>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W48*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W48>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":0.94442120907400673},2399.0682755655857]
[null,0,{"$f":"gear_inertia","v":0},1,{"$f":"Ltime5","v":1},null,null,null,null,null,48,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K49<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K49*PI()*Main!$D$45/100/Main!$D$46))),(IF(K49<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K49-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R49)))))))),(IF(K49<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K49*PI()*Main!$D$71/100/Main!$D$72))),(IF(K49<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K49-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R49)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K49<=(Main!$D$46/Main!$D$45*100),O49*Main!$D$45/100000+P48,IF(K49<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O49*Main!$D$45/100000+P48,IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S49))))),(IF(K49<=(Main!$D$72/Main!$D$71*100),O49*Main!$D$71/100000+P48,IF(K49<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O49*Main!$D$71/100000+P48,IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S49))))))","v":0},{"$f":"IF($A$90=TRUE,P49*Main!$D$45/100000+Q48,P49*100+Q48)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K49<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K49-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K49<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K49<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K49-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K49<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K49-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K49<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K49<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K49-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O49*Main!$D$45/100000+P48,IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O49*Main!$D$45/100000+P48,Main!$E$52)))),(IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O49*Main!$D$71/100000+P48,IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O49*Main!$D$71/100000+P48,Main!$E$78)))))","v":0},49.999989999999997,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T49*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T49*PI()/50))))","v":4.8738901133884096E-4},{"$f":"IF($A$90=TRUE,U49*2*Main!$D$46/100000*(T49-T48)+V48,U49*2*Ltime1*(T49-T48)/100000+V48)","v":39.984472048988728},6.2831853066027051E-7,0.99961180122471816,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W49*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W49>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W49*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W49>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W49*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W49>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W49*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W49>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W49*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W49>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W49*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W49>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9.45042899561852E-6},2399.0683229393235]
[null,1,{"$f":"Wirkungsgrad","v":1},0,{"$f":"Ltime6","v":0},null,null,null,null,null,49,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K50<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K50*PI()*Main!$D$45/100/Main!$D$46))),(IF(K50<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K50-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R50)))))))),(IF(K50<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K50*PI()*Main!$D$71/100/Main!$D$72))),(IF(K50<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K50-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R50)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K50<=(Main!$D$46/Main!$D$45*100),O50*Main!$D$45/100000+P49,IF(K50<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O50*Main!$D$45/100000+P49,IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S50))))),(IF(K50<=(Main!$D$72/Main!$D$71*100),O50*Main!$D$71/100000+P49,IF(K50<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O50*Main!$D$71/100000+P49,IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S50))))))","v":0},{"$f":"IF($A$90=TRUE,P50*Main!$D$45/100000+Q49,P50*100+Q49)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K50<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K50-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K50<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K50<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K50-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K50<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K50-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K50<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K50<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K50-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O50*Main!$D$45/100000+P49,IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O50*Main!$D$45/100000+P49,Main!$E$52)))),(IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O50*Main!$D$71/100000+P49,IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O50*Main!$D$71/100000+P49,Main!$E$78)))))","v":0},49.999989999999997,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T50*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T50*PI()/50))))","v":4.8738901133884096E-4},{"$f":"IF($A$90=TRUE,U50*2*Main!$D$46/100000*(T50-T49)+V49,U50*2*Ltime1*(T50-T49)/100000+V49)","v":39.984472048988728},6.2831853066027051E-7,0.99961180122471816,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W50*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W50>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W50*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W50>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W50*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W50>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W50*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W50>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W50*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W50>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W50*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W50>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad))),0)","v":9.45042899561852E-6},2399.0683229393235]
[null,1,{"$f":"ULU","v":1},1,{"$f":"Ltime7","v":1},null,null,null,null,null,50,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K51<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K51*PI()*Main!$D$45/100/Main!$D$46))),(IF(K51<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K51-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R51)))))))),(IF(K51<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K51*PI()*Main!$D$71/100/Main!$D$72))),(IF(K51<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K51-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R51)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K51<=(Main!$D$46/Main!$D$45*100),O51*Main!$D$45/100000+P50,IF(K51<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O51*Main!$D$45/100000+P50,IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S51))))),(IF(K51<=(Main!$D$72/Main!$D$71*100),O51*Main!$D$71/100000+P50,IF(K51<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O51*Main!$D$71/100000+P50,IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S51))))))","v":0},{"$f":"IF($A$90=TRUE,P51*Main!$D$45/100000+Q50,P51*100+Q50)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K51<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K51-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K51<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K51<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K51-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K51<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K51-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K51<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K51<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K51-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O51*Main!$D$45/100000+P50,IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O51*Main!$D$45/100000+P50,Main!$E$52)))),(IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O51*Main!$D$71/100000+P50,IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O51*Main!$D$71/100000+P50,Main!$E$78)))))","v":0},50,0,{"$f":"IF($A$90=TRUE,Main!$E$48,Lspeed2)","v":40},0,1,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W51*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W51>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W51*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W51>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W51*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W51>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W51*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W51>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W51*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W51>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W51*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W51>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":0},2400]
[null,1,{"$f":"time5","v":1},0,{"$f":"Ltime8","v":0},null,null,null,null,null,51,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K52<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K52*PI()*Main!$D$45/100/Main!$D$46))),(IF(K52<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K52-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R52)))))))),(IF(K52<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K52*PI()*Main!$D$71/100/Main!$D$72))),(IF(K52<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K52-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R52)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K52<=(Main!$D$46/Main!$D$45*100),O52*Main!$D$45/100000+P51,IF(K52<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O52*Main!$D$45/100000+P51,IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S52))))),(IF(K52<=(Main!$D$72/Main!$D$71*100),O52*Main!$D$71/100000+P51,IF(K52<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O52*Main!$D$71/100000+P51,IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S52))))))","v":0},{"$f":"IF($A$90=TRUE,P52*Main!$D$45/100000+Q51,P52*100+Q51)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K52<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K52-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K52<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K52<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K52-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K52<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K52-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K52<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K52<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K52-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O52*Main!$D$45/100000+P51,IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O52*Main!$D$45/100000+P51,Main!$E$52)))),(IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O52*Main!$D$71/100000+P51,IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O52*Main!$D$71/100000+P51,Main!$E$78)))))","v":0},50.000000999999997,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T52-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T52-50)*PI()/50))))","v":-3.9478509822397092E-5},{"$f":"IF($A$90=TRUE,U52*2*Main!$D$50*(T52-T51)/100000+V51,U52*2*Ltime3*(T52-T51)/100000+V51)","v":39.999999999999922},-5.0893800859660119E-8,0.999999999999998,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W52*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W52<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W52*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W52<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W52*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+Ltorque)/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W52*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W52<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W52*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W52<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W52*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+Ltorque)/LWirkungsgrad))),0)","v":0},2399.999999999995]
[null,0,{"$f":"time6","v":0},0,{"$f":"Lspeed6","v":0},null,null,null,null,null,52,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K53<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K53*PI()*Main!$D$45/100/Main!$D$46))),(IF(K53<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K53-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R53)))))))),(IF(K53<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K53*PI()*Main!$D$71/100/Main!$D$72))),(IF(K53<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K53-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R53)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K53<=(Main!$D$46/Main!$D$45*100),O53*Main!$D$45/100000+P52,IF(K53<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O53*Main!$D$45/100000+P52,IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S53))))),(IF(K53<=(Main!$D$72/Main!$D$71*100),O53*Main!$D$71/100000+P52,IF(K53<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O53*Main!$D$71/100000+P52,IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S53))))))","v":0},{"$f":"IF($A$90=TRUE,P53*Main!$D$45/100000+Q52,P53*100+Q52)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K53<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K53-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K53<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K53<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K53-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K53<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K53-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K53<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K53<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K53-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O53*Main!$D$45/100000+P52,IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O53*Main!$D$45/100000+P52,Main!$E$52)))),(IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O53*Main!$D$71/100000+P52,IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O53*Main!$D$71/100000+P52,Main!$E$78)))))","v":0},50.000000999999997,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T53-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T53-50)*PI()/50))))","v":-3.9478509822397092E-5},{"$f":"IF($A$90=TRUE,U53*2*Main!$D$50*(T53-T52)/100000+V52,U53*2*Ltime3*(T53-T52)/100000+V52)","v":39.999999999999922},-5.0893800859660119E-8,0.999999999999998,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W53*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W53<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W53*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W53<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W53*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W53<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W53*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W53<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W53*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W53<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W53*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W53<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.6548474678271822E-7},2399.999999999995]
[null,1,{"$f":"time7","v":1},5,{"$f":"Gewicht2","v":5},null,null,null,null,null,53,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K54<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K54*PI()*Main!$D$45/100/Main!$D$46))),(IF(K54<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K54-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R54)))))))),(IF(K54<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K54*PI()*Main!$D$71/100/Main!$D$72))),(IF(K54<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K54-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R54)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K54<=(Main!$D$46/Main!$D$45*100),O54*Main!$D$45/100000+P53,IF(K54<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O54*Main!$D$45/100000+P53,IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S54))))),(IF(K54<=(Main!$D$72/Main!$D$71*100),O54*Main!$D$71/100000+P53,IF(K54<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O54*Main!$D$71/100000+P53,IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S54))))))","v":0},{"$f":"IF($A$90=TRUE,P54*Main!$D$45/100000+Q53,P54*100+Q53)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K54<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K54-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K54<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K54<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K54-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K54<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K54-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K54<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K54<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K54-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O54*Main!$D$45/100000+P53,IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O54*Main!$D$45/100000+P53,Main!$E$52)))),(IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O54*Main!$D$71/100000+P53,IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O54*Main!$D$71/100000+P53,Main!$E$78)))))","v":0},51,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T54-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T54-50)*PI()/50))))","v":-39.452539230658175},{"$f":"IF($A$90=TRUE,U54*2*Main!$D$50*(T54-T53)/100000+V53,U54*2*Ltime3*(T54-T53)/100000+V53)","v":39.921095000443685},-5.086032081874383E-2,0.99802737501109218,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W54*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W54<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W54*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W54<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W54*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W54<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W54*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W54<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W54*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W54<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W54*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W54<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":0.76498117934994281},2395.2657000266213]
[null,0,{"$f":"time8","v":0},0,{"$f":"Ltorque2","v":0},null,null,null,null,null,54,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K55<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K55*PI()*Main!$D$45/100/Main!$D$46))),(IF(K55<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K55-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R55)))))))),(IF(K55<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K55*PI()*Main!$D$71/100/Main!$D$72))),(IF(K55<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K55-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R55)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K55<=(Main!$D$46/Main!$D$45*100),O55*Main!$D$45/100000+P54,IF(K55<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O55*Main!$D$45/100000+P54,IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S55))))),(IF(K55<=(Main!$D$72/Main!$D$71*100),O55*Main!$D$71/100000+P54,IF(K55<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O55*Main!$D$71/100000+P54,IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S55))))))","v":0},{"$f":"IF($A$90=TRUE,P55*Main!$D$45/100000+Q54,P55*100+Q54)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K55<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K55-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K55<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K55<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K55-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K55<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K55-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K55<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K55<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K55-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O55*Main!$D$45/100000+P54,IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O55*Main!$D$45/100000+P54,Main!$E$52)))),(IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O55*Main!$D$71/100000+P54,IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O55*Main!$D$71/100000+P54,Main!$E$78)))))","v":0},52,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T55-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T55-50)*PI()/50))))","v":-78.749377313123645},{"$f":"IF($A$90=TRUE,U55*2*Main!$D$50*(T55-T54)/100000+V54,U55*2*Ltime3*(T55-T54)/100000+V54)","v":39.763596245817439},-0.10151991918708644,0.99408990614543602,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W55*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W55<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W55*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W55<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W55*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W55<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W55*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W55<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W55*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W55<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W55*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W55<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":1.5269433274716488},2385.8157747490463]
[null,0,{"$f":"speed6","v":0},0,{"$f":"LDryTorq","v":0},null,null,null,null,null,55,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K56<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K56*PI()*Main!$D$45/100/Main!$D$46))),(IF(K56<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K56-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R56)))))))),(IF(K56<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K56*PI()*Main!$D$71/100/Main!$D$72))),(IF(K56<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K56-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R56)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K56<=(Main!$D$46/Main!$D$45*100),O56*Main!$D$45/100000+P55,IF(K56<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O56*Main!$D$45/100000+P55,IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S56))))),(IF(K56<=(Main!$D$72/Main!$D$71*100),O56*Main!$D$71/100000+P55,IF(K56<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O56*Main!$D$71/100000+P55,IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S56))))))","v":0},{"$f":"IF($A$90=TRUE,P56*Main!$D$45/100000+Q55,P56*100+Q55)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K56<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K56-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K56<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K56<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K56-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K56<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K56-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K56<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K56<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K56-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O56*Main!$D$45/100000+P55,IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O56*Main!$D$45/100000+P55,Main!$E$52)))),(IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O56*Main!$D$71/100000+P55,IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O56*Main!$D$71/100000+P55,Main!$E$78)))))","v":0},54,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T56-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T56-50)*PI()/50))))","v":-156.25682990342156},{"$f":"IF($A$90=TRUE,U56*2*Main!$D$50*(T56-T55)/100000+V55,U56*2*Ltime3*(T56-T55)/100000+V55)","v":39.138568926203753},-0.20143880860353239,0.97846422315509385,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W56*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W56<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W56*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W56<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W56*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W56<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W56*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W56<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W56*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W56<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W56*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W56<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":3.0298058465173394},2348.314135572225]
[null,25,{"$f":"inertia2","v":25},0,{"$f":"LDryTorq2","v":0},null,null,null,null,null,56,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K57<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K57*PI()*Main!$D$45/100/Main!$D$46))),(IF(K57<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K57-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R57)))))))),(IF(K57<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K57*PI()*Main!$D$71/100/Main!$D$72))),(IF(K57<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K57-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R57)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K57<=(Main!$D$46/Main!$D$45*100),O57*Main!$D$45/100000+P56,IF(K57<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O57*Main!$D$45/100000+P56,IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S57))))),(IF(K57<=(Main!$D$72/Main!$D$71*100),O57*Main!$D$71/100000+P56,IF(K57<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O57*Main!$D$71/100000+P56,IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S57))))))","v":0},{"$f":"IF($A$90=TRUE,P57*Main!$D$45/100000+Q56,P57*100+Q56)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K57<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K57-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K57<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K57<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K57-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K57<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K57-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K57<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K57<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K57-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O57*Main!$D$45/100000+P56,IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O57*Main!$D$45/100000+P56,Main!$E$52)))),(IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O57*Main!$D$71/100000+P56,IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O57*Main!$D$71/100000+P56,Main!$E$78)))))","v":0},56,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T57-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T57-50)*PI()/50))))","v":-231.3000189428368},{"$f":"IF($A$90=TRUE,U57*2*Main!$D$50*(T57-T56)/100000+V56,U57*2*Ltime3*(T57-T56)/100000+V56)","v":38.213368850432403},-0.29818088767458906,0.95533422126081002,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W57*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W57<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W57*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W57<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W57*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W57<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W57*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W57<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W57*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W57<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W57*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W57<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":4.484886517445168},2292.8021310259442]
[null,0,{"$f":"torque2","v":0},null,null,null,null,null,null,null,57,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K58<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K58*PI()*Main!$D$45/100/Main!$D$46))),(IF(K58<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K58-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R58)))))))),(IF(K58<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K58*PI()*Main!$D$71/100/Main!$D$72))),(IF(K58<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K58-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R58)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K58<=(Main!$D$46/Main!$D$45*100),O58*Main!$D$45/100000+P57,IF(K58<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O58*Main!$D$45/100000+P57,IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S58))))),(IF(K58<=(Main!$D$72/Main!$D$71*100),O58*Main!$D$71/100000+P57,IF(K58<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O58*Main!$D$71/100000+P57,IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S58))))))","v":0},{"$f":"IF($A$90=TRUE,P58*Main!$D$45/100000+Q57,P58*100+Q57)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K58<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K58-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K58<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K58<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K58-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K58<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K58-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K58<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K58<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K58-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O58*Main!$D$45/100000+P57,IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O58*Main!$D$45/100000+P57,Main!$E$52)))),(IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O58*Main!$D$71/100000+P57,IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O58*Main!$D$71/100000+P57,Main!$E$78)))))","v":0},57,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T58-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T58-50)*PI()/50))))","v":-267.52564447616641},{"$f":"IF($A$90=TRUE,U58*2*Main!$D$50*(T58-T57)/100000+V57,U58*2*Ltime3*(T58-T57)/100000+V57)","v":37.678317561480071},-0.34488122616770878,0.94195793903700176,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W58*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W58<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W58*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W58<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W58*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W58<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W58*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W58<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W58*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W58<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W58*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W58<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":5.1872981310845052},2260.6990536888043]
[null,0,{"$f":"DryTorq","v":0},null,null,null,null,null,null,null,58,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K59<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K59*PI()*Main!$D$45/100/Main!$D$46))),(IF(K59<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K59-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R59)))))))),(IF(K59<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K59*PI()*Main!$D$71/100/Main!$D$72))),(IF(K59<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K59-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R59)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K59<=(Main!$D$46/Main!$D$45*100),O59*Main!$D$45/100000+P58,IF(K59<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O59*Main!$D$45/100000+P58,IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S59))))),(IF(K59<=(Main!$D$72/Main!$D$71*100),O59*Main!$D$71/100000+P58,IF(K59<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O59*Main!$D$71/100000+P58,IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S59))))))","v":0},{"$f":"IF($A$90=TRUE,P59*Main!$D$45/100000+Q58,P59*100+Q58)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K59<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K59-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K59<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K59<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K59-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K59<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K59-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K59<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K59<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K59-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O59*Main!$D$45/100000+P58,IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O59*Main!$D$45/100000+P58,Main!$E$52)))),(IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O59*Main!$D$71/100000+P58,IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O59*Main!$D$71/100000+P58,Main!$E$78)))))","v":0},58,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T59-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T59-50)*PI()/50))))","v":-302.69546851158975},{"$f":"IF($A$90=TRUE,U59*2*Main!$D$50*(T59-T58)/100000+V58,U59*2*Ltime3*(T59-T58)/100000+V58)","v":37.07292662445689},-0.39022047602238941,0.92682316561142231,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W59*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W59<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W59*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W59<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W59*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W59<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W59*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W59<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W59*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W59<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W59*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W59<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":5.8692378488515464},2224.3755974674136]
[15,0,{"$f":"DryTorq2","v":0},null,null,null,null,null,null,null,59,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K60<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K60*PI()*Main!$D$45/100/Main!$D$46))),(IF(K60<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K60-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R60)))))))),(IF(K60<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K60*PI()*Main!$D$71/100/Main!$D$72))),(IF(K60<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K60-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R60)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K60<=(Main!$D$46/Main!$D$45*100),O60*Main!$D$45/100000+P59,IF(K60<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O60*Main!$D$45/100000+P59,IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S60))))),(IF(K60<=(Main!$D$72/Main!$D$71*100),O60*Main!$D$71/100000+P59,IF(K60<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O60*Main!$D$71/100000+P59,IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S60))))))","v":0},{"$f":"IF($A$90=TRUE,P60*Main!$D$45/100000+Q59,P60*100+Q59)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K60<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K60-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K60<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K60<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K60-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K60<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K60-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K60<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K60<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K60-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O60*Main!$D$45/100000+P59,IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O60*Main!$D$45/100000+P59,Main!$E$52)))),(IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O60*Main!$D$71/100000+P59,IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O60*Main!$D$71/100000+P59,Main!$E$78)))))","v":0},59,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T60-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T60-50)*PI()/50))))","v":-336.67069182120315},{"$f":"IF($A$90=TRUE,U60*2*Main!$D$50*(T60-T59)/100000+V59,U60*2*Ltime3*(T60-T59)/100000+V59)","v":36.399585240814481},-0.43401970393298728,0.90998963102036201,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W60*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W60<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W60*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W60<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W60*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W60<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W60*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W60<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W60*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W60<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W60*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W60<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":6.5280143662288825},2183.9751144488687]
[12,null,null,null,null,null,null,null,null,null,60,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K61<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K61*PI()*Main!$D$45/100/Main!$D$46))),(IF(K61<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K61-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R61)))))))),(IF(K61<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K61*PI()*Main!$D$71/100/Main!$D$72))),(IF(K61<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K61-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R61)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K61<=(Main!$D$46/Main!$D$45*100),O61*Main!$D$45/100000+P60,IF(K61<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O61*Main!$D$45/100000+P60,IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S61))))),(IF(K61<=(Main!$D$72/Main!$D$71*100),O61*Main!$D$71/100000+P60,IF(K61<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O61*Main!$D$71/100000+P60,IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S61))))))","v":0},{"$f":"IF($A$90=TRUE,P61*Main!$D$45/100000+Q60,P61*100+Q60)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K61<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K61-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K61<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K61<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K61-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K61<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K61-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K61<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K61<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K61-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O61*Main!$D$45/100000+P60,IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O61*Main!$D$45/100000+P60,Main!$E$52)))),(IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O61*Main!$D$71/100000+P60,IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O61*Main!$D$71/100000+P60,Main!$E$78)))))","v":0},60,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T61-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T61-50)*PI()/50))))","v":-369.31722972040666},{"$f":"IF($A$90=TRUE,U61*2*Main!$D$50*(T61-T60)/100000+V60,U61*2*Ltime3*(T61-T60)/100000+V60)","v":35.660950781373671},-0.47610605435690317,0.89152376953434176,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W61*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W61<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W61*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W61<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W61*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W61<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W61*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W61<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W61*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W61<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W61*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W61<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.1610277932687882},2139.6570468824202]
[13,null,null,null,null,null,null,null,null,null,61,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K62<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K62*PI()*Main!$D$45/100/Main!$D$46))),(IF(K62<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K62-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R62)))))))),(IF(K62<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K62*PI()*Main!$D$71/100/Main!$D$72))),(IF(K62<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K62-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R62)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K62<=(Main!$D$46/Main!$D$45*100),O62*Main!$D$45/100000+P61,IF(K62<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O62*Main!$D$45/100000+P61,IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S62))))),(IF(K62<=(Main!$D$72/Main!$D$71*100),O62*Main!$D$71/100000+P61,IF(K62<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O62*Main!$D$71/100000+P61,IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S62))))))","v":0},{"$f":"IF($A$90=TRUE,P62*Main!$D$45/100000+Q61,P62*100+Q61)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K62<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K62-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K62<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K62<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K62-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K62<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K62-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K62<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K62<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K62-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O62*Main!$D$45/100000+P61,IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O62*Main!$D$45/100000+P61,Main!$E$52)))),(IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O62*Main!$D$71/100000+P61,IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O62*Main!$D$71/100000+P61,Main!$E$78)))))","v":0},61,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T62-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T62-50)*PI()/50))))","v":-400.50624123889662},{"$f":"IF($A$90=TRUE,U62*2*Main!$D$50*(T62-T61)/100000+V61,U62*2*Ltime3*(T62-T61)/100000+V61)","v":34.859938298895877},-0.51631343169643851,0.87149845747239696,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W62*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W62<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W62*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W62<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W62*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W62<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W62*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W62<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W62*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W62<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W62*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W62<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.7657799151710662},2091.5962979337528]
[12,null,null,null,null,null,null,null,null,null,62,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K63<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K63*PI()*Main!$D$45/100/Main!$D$46))),(IF(K63<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K63-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R63)))))))),(IF(K63<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K63*PI()*Main!$D$71/100/Main!$D$72))),(IF(K63<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K63-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R63)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K63<=(Main!$D$46/Main!$D$45*100),O63*Main!$D$45/100000+P62,IF(K63<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O63*Main!$D$45/100000+P62,IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S63))))),(IF(K63<=(Main!$D$72/Main!$D$71*100),O63*Main!$D$71/100000+P62,IF(K63<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O63*Main!$D$71/100000+P62,IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S63))))))","v":0},{"$f":"IF($A$90=TRUE,P63*Main!$D$45/100000+Q62,P63*100+Q62)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K63<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K63-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K63<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K63<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K63-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K63<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K63-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K63<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K63<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K63-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O63*Main!$D$45/100000+P62,IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O63*Main!$D$45/100000+P62,Main!$E$52)))),(IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O63*Main!$D$71/100000+P62,IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O63*Main!$D$71/100000+P62,Main!$E$78)))))","v":0},62,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T63-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T63-50)*PI()/50))))","v":-430.11463759711359},{"$f":"IF($A$90=TRUE,U63*2*Main!$D$50*(T63-T62)/100000+V62,U63*2*Ltime3*(T63-T62)/100000+V62)","v":33.999709023701648},-0.55448315580223773,0.84999272559254124,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W63*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W63<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W63*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W63<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W63*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W63<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W63*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W63<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W63*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W63<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W63*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W63<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":8.3398840515955328},2039.9825414220991]
[20,null,null,null,null,null,null,null,null,null,63,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K64<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K64*PI()*Main!$D$45/100/Main!$D$46))),(IF(K64<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K64-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R64)))))))),(IF(K64<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K64*PI()*Main!$D$71/100/Main!$D$72))),(IF(K64<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K64-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R64)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K64<=(Main!$D$46/Main!$D$45*100),O64*Main!$D$45/100000+P63,IF(K64<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O64*Main!$D$45/100000+P63,IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S64))))),(IF(K64<=(Main!$D$72/Main!$D$71*100),O64*Main!$D$71/100000+P63,IF(K64<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O64*Main!$D$71/100000+P63,IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S64))))))","v":0},{"$f":"IF($A$90=TRUE,P64*Main!$D$45/100000+Q63,P64*100+Q63)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K64<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K64-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K64<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K64<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K64-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K64<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K64-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K64<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K64<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K64-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O64*Main!$D$45/100000+P63,IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O64*Main!$D$45/100000+P63,Main!$E$52)))),(IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O64*Main!$D$71/100000+P63,IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O64*Main!$D$71/100000+P63,Main!$E$78)))))","v":0},63,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T64-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T64-50)*PI()/50))))","v":-458.02556798142126},{"$f":"IF($A$90=TRUE,U64*2*Main!$D$50*(T64-T63)/100000+V63,U64*2*Ltime3*(T64-T63)/100000+V63)","v":33.083657887738802},-0.59046458821134329,0.82709144719347005,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W64*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W64<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W64*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W64<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W64*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W64<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W64*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W64<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W64*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W64<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W64*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W64<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":8.8810744757989486},1985.0194732643281]
[20,null,null,null,null,null,null,null,null,null,64,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K65<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K65*PI()*Main!$D$45/100/Main!$D$46))),(IF(K65<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K65-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R65)))))))),(IF(K65<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K65*PI()*Main!$D$71/100/Main!$D$72))),(IF(K65<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K65-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R65)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K65<=(Main!$D$46/Main!$D$45*100),O65*Main!$D$45/100000+P64,IF(K65<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O65*Main!$D$45/100000+P64,IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S65))))),(IF(K65<=(Main!$D$72/Main!$D$71*100),O65*Main!$D$71/100000+P64,IF(K65<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O65*Main!$D$71/100000+P64,IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S65))))))","v":0},{"$f":"IF($A$90=TRUE,P65*Main!$D$45/100000+Q64,P65*100+Q64)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K65<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K65-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K65<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K65<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K65-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K65<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K65-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K65<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K65<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K65-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O65*Main!$D$45/100000+P64,IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O65*Main!$D$45/100000+P64,Main!$E$52)))),(IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O65*Main!$D$71/100000+P64,IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O65*Main!$D$71/100000+P64,Main!$E$78)))))","v":0},64,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T65-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T65-50)*PI()/50))))","v":-484.12888070088383},{"$f":"IF($A$90=TRUE,U65*2*Main!$D$50*(T65-T64)/100000+V64,U65*2*Ltime3*(T65-T64)/100000+V64)","v":32.115400126337036},-0.62411572664838921,0.80288500315842593,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W65*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W65<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W65*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W65<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W65*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W65<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W65*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W65<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W65*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W65<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W65*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W65<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9.3872153564233702},1926.9240075802222]
[null,null,null,null,null,null,null,null,null,null,65,{"$f":"IF(ABS(MIN($O$1:$O$100))>MAX($O$1:$O$100),O66/MIN($O$1:$O$100)*-1,O66/MAX($O$1:$O$100))","v":0},{"$f":"IF(ABS(MIN($P$1:$P$100))>MAX($P$1:$P$100),P66/MIN($P$1:$P$100)*-1,P66/MAX($P$1:$P$100))","v":0},{"$f":"IF(ABS(MIN($Q$1:$Q$100))>MAX($Q$1:$Q$100),Q66/MIN($Q$1:$Q$100)*-1,Q66/MAX($Q$1:$Q$100))","v":0.99989727158268316},{"$f":"IF($A$90=TRUE,(IF(K66<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K66*PI()*Main!$D$45/100/Main!$D$46))),(IF(K66<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K66-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R66)))))))),(IF(K66<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K66*PI()*Main!$D$71/100/Main!$D$72))),(IF(K66<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K66-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R66)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K66<=(Main!$D$46/Main!$D$45*100),O66*Main!$D$45/100000+P65,IF(K66<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O66*Main!$D$45/100000+P65,IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S66))))),(IF(K66<=(Main!$D$72/Main!$D$71*100),O66*Main!$D$71/100000+P65,IF(K66<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O66*Main!$D$71/100000+P65,IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S66))))))","v":0},{"$f":"IF($A$90=TRUE,P66*Main!$D$45/100000+Q65,P66*100+Q65)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K66<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K66-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K66<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K66<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K66-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K66<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K66-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K66<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K66<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K66-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O66*Main!$D$45/100000+P65,IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O66*Main!$D$45/100000+P65,Main!$E$52)))),(IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O66*Main!$D$71/100000+P65,IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O66*Main!$D$71/100000+P65,Main!$E$78)))))","v":0},65,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T66-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T66-50)*PI()/50))))","v":-508.32155790566685},{"$f":"IF($A$90=TRUE,U66*2*Main!$D$50*(T66-T65)/100000+V65,U66*2*Ltime3*(T66-T65)/100000+V65)","v":31.098757010525702},{"$f":"IF(move1,IF(ABS(MIN($U$1:$U$101))>MAX($U$1:$U$101),U66/MIN($U$1:$U$101)*-1,U66/MAX($U$1:$U$101)),IF(ABS(MIN($U$1:$U$201))>MAX($U$1:$U$201),U66/MIN($U$1:$U$201)*-1,U66/MAX($U$1:$U$201)))","v":-0.65530376544370728},{"$f":"IF(move1,IF(ABS(MIN($V$1:$V$101))>MAX($V$1:$V$101),V66/MIN($V$1:$V$101)*-1,V66/MAX($V$1:$V$101)),IF(ABS(MIN($V$1:$V$201))>MAX($V$1:$V$201),V66/MIN($V$1:$V$201)*-1,V66/MAX($V$1:$V$201)))","v":0.7774689252631426},{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W66*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W66<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W66*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W66<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W66*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W66<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W66*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W66<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W66*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W66<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W66*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W66<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9.8563091866467456},1865.9254206315422]
[null,null,null,null,null,null,null,null,null,null,66,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K67<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K67*PI()*Main!$D$45/100/Main!$D$46))),(IF(K67<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K67-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R67)))))))),(IF(K67<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K67*PI()*Main!$D$71/100/Main!$D$72))),(IF(K67<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K67-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R67)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K67<=(Main!$D$46/Main!$D$45*100),O67*Main!$D$45/100000+P66,IF(K67<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O67*Main!$D$45/100000+P66,IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S67))))),(IF(K67<=(Main!$D$72/Main!$D$71*100),O67*Main!$D$71/100000+P66,IF(K67<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O67*Main!$D$71/100000+P66,IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S67))))))","v":0},{"$f":"IF($A$90=TRUE,P67*Main!$D$45/100000+Q66,P67*100+Q66)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K67<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K67-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K67<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K67<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K67-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K67<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K67-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K67<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K67<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K67-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O67*Main!$D$45/100000+P66,IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O67*Main!$D$45/100000+P66,Main!$E$52)))),(IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O67*Main!$D$71/100000+P66,IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O67*Main!$D$71/100000+P66,Main!$E$78)))))","v":0},66,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T67-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T67-50)*PI()/50))))","v":-530.50812215142605},{"$f":"IF($A$90=TRUE,U67*2*Main!$D$50*(T67-T66)/100000+V66,U67*2*Ltime3*(T67-T66)/100000+V66)","v":30.03774076622285},-0.6839056196566321,0.75094351915557123,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W67*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W67<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W67*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W67<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W67*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W67<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W67*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W67<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W67*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W67<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W67*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W67<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":10.286504667429769},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X67*speed,X67*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X67*speed,X67*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":1802.264445973371}]
[null,null,null,null,null,null,null,null,null,null,67,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K68<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K68*PI()*Main!$D$45/100/Main!$D$46))),(IF(K68<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K68-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R68)))))))),(IF(K68<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K68*PI()*Main!$D$71/100/Main!$D$72))),(IF(K68<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K68-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R68)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K68<=(Main!$D$46/Main!$D$45*100),O68*Main!$D$45/100000+P67,IF(K68<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O68*Main!$D$45/100000+P67,IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S68))))),(IF(K68<=(Main!$D$72/Main!$D$71*100),O68*Main!$D$71/100000+P67,IF(K68<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O68*Main!$D$71/100000+P67,IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S68))))))","v":0},{"$f":"IF($A$90=TRUE,P68*Main!$D$45/100000+Q67,P68*100+Q67)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K68<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K68-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K68<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K68<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K68-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K68<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K68-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K68<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K68<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K68-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O68*Main!$D$45/100000+P67,IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O68*Main!$D$45/100000+P67,Main!$E$52)))),(IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O68*Main!$D$71/100000+P67,IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O68*Main!$D$71/100000+P67,Main!$E$78)))))","v":0},67,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T68-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T68-50)*PI()/50))))","v":-550.60101320516037},{"$f":"IF($A$90=TRUE,U68*2*Main!$D$50*(T68-T67)/100000+V67,U68*2*Ltime3*(T68-T67)/100000+V67)","v":28.93653873981253},-0.70980841083552948,0.72341346849531329,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W68*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W68<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W68*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W68<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W68*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W68<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W68*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W68<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W68*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W68<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W68*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W68<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":10.676104013747413},1736.192324388752]
[null,null,null,null,null,null,null,null,null,null,68,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K69<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K69*PI()*Main!$D$45/100/Main!$D$46))),(IF(K69<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K69-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R69)))))))),(IF(K69<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K69*PI()*Main!$D$71/100/Main!$D$72))),(IF(K69<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K69-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R69)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K69<=(Main!$D$46/Main!$D$45*100),O69*Main!$D$45/100000+P68,IF(K69<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O69*Main!$D$45/100000+P68,IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S69))))),(IF(K69<=(Main!$D$72/Main!$D$71*100),O69*Main!$D$71/100000+P68,IF(K69<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O69*Main!$D$71/100000+P68,IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S69))))))","v":0},{"$f":"IF($A$90=TRUE,P69*Main!$D$45/100000+Q68,P69*100+Q68)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K69<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K69-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K69<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K69<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K69-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K69<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K69-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K69<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K69<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K69-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O69*Main!$D$45/100000+P68,IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O69*Main!$D$45/100000+P68,Main!$E$52)))),(IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O69*Main!$D$71/100000+P68,IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O69*Main!$D$71/100000+P68,Main!$E$78)))))","v":0},68,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T69-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T69-50)*PI()/50))))","v":-568.52093360544939},{"$f":"IF($A$90=TRUE,U69*2*Main!$D$50*(T69-T68)/100000+V68,U69*2*Ltime3*(T69-T68)/100000+V68)","v":27.79949687260163},-0.73290991249747584,0.6949874218150407,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W69*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W69<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W69*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W69<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W69*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W69<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W69*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W69<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W69*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W69<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W69*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W69<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.023569654970766},1667.9698123560977]
["C041B (240 V)",null,null,null,null,null,null,null,null,null,69,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K70<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K70*PI()*Main!$D$45/100/Main!$D$46))),(IF(K70<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K70-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R70)))))))),(IF(K70<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K70*PI()*Main!$D$71/100/Main!$D$72))),(IF(K70<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K70-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R70)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K70<=(Main!$D$46/Main!$D$45*100),O70*Main!$D$45/100000+P69,IF(K70<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O70*Main!$D$45/100000+P69,IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S70))))),(IF(K70<=(Main!$D$72/Main!$D$71*100),O70*Main!$D$71/100000+P69,IF(K70<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O70*Main!$D$71/100000+P69,IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S70))))))","v":0},{"$f":"IF($A$90=TRUE,P70*Main!$D$45/100000+Q69,P70*100+Q69)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K70<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K70-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K70<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K70<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K70-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K70<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K70-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K70<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K70<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K70-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O70*Main!$D$45/100000+P69,IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O70*Main!$D$45/100000+P69,Main!$E$52)))),(IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O70*Main!$D$71/100000+P69,IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O70*Main!$D$71/100000+P69,Main!$E$78)))))","v":0},69,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T70-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T70-50)*PI()/50))))","v":-584.19716161330598},{"$f":"IF($A$90=TRUE,U70*2*Main!$D$50*(T70-T69)/100000+V69,U70*2*Ltime3*(T70-T69)/100000+V69)","v":26.631102549375019},-0.75311895356948344,0.66577756373437547,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W70*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W70<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W70*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W70<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W70*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W70<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W70*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W70<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W70*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W70<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W70*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W70<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.327530302955875},1597.866152962501]
[true,null,null,null,null,null,null,null,null,null,70,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K71<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K71*PI()*Main!$D$45/100/Main!$D$46))),(IF(K71<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K71-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R71)))))))),(IF(K71<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K71*PI()*Main!$D$71/100/Main!$D$72))),(IF(K71<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K71-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R71)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K71<=(Main!$D$46/Main!$D$45*100),O71*Main!$D$45/100000+P70,IF(K71<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O71*Main!$D$45/100000+P70,IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S71))))),(IF(K71<=(Main!$D$72/Main!$D$71*100),O71*Main!$D$71/100000+P70,IF(K71<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O71*Main!$D$71/100000+P70,IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S71))))))","v":0},{"$f":"IF($A$90=TRUE,P71*Main!$D$45/100000+Q70,P71*100+Q70)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K71<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K71-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K71<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K71<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K71-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K71<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K71-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K71<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K71<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K71-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O71*Main!$D$45/100000+P70,IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O71*Main!$D$45/100000+P70,Main!$E$52)))),(IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O71*Main!$D$71/100000+P70,IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O71*Main!$D$71/100000+P70,Main!$E$78)))))","v":0},70,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T71-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T71-50)*PI()/50))))","v":-597.56783031857083},{"$f":"IF($A$90=TRUE,U71*2*Main!$D$50*(T71-T70)/100000+V70,U71*2*Ltime3*(T71-T70)/100000+V70)","v":25.435966888737877},-0.7703557781990743,0.63589917221844694,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W71*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W71<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W71*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W71<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W71*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W71<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W71*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W71<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W71*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W71<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W71*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W71<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.586786363891557},1526.1580133242726]
[{"$f":"IF(A71,10,1)","v":10},null,null,null,null,null,null,null,null,null,71,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K72<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K72*PI()*Main!$D$45/100/Main!$D$46))),(IF(K72<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K72-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R72)))))))),(IF(K72<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K72*PI()*Main!$D$71/100/Main!$D$72))),(IF(K72<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K72-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R72)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K72<=(Main!$D$46/Main!$D$45*100),O72*Main!$D$45/100000+P71,IF(K72<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O72*Main!$D$45/100000+P71,IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S72))))),(IF(K72<=(Main!$D$72/Main!$D$71*100),O72*Main!$D$71/100000+P71,IF(K72<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O72*Main!$D$71/100000+P71,IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S72))))))","v":0},{"$f":"IF($A$90=TRUE,P72*Main!$D$45/100000+Q71,P72*100+Q71)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K72<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K72-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K72<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K72<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K72-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K72<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K72-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K72<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K72<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K72-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O72*Main!$D$45/100000+P71,IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O72*Main!$D$45/100000+P71,Main!$E$52)))),(IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O72*Main!$D$71/100000+P71,IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O72*Main!$D$71/100000+P71,Main!$E$78)))))","v":0},71,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T72-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T72-50)*PI()/50))))","v":-608.58017180034142},{"$f":"IF($A$90=TRUE,U72*2*Main!$D$50*(T72-T71)/100000+V71,U72*2*Ltime3*(T72-T71)/100000+V71)","v":24.218806545137195},-0.78455236051419108,0.60547016362842987,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W72*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W72<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W72*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W72<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W72*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W72<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W72*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W72<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W72*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W72<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W72*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W72<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.800314672548119},1453.1283927082318]
[null,null,null,null,null,null,null,null,null,null,72,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K73<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K73*PI()*Main!$D$45/100/Main!$D$46))),(IF(K73<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K73-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R73)))))))),(IF(K73<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K73*PI()*Main!$D$71/100/Main!$D$72))),(IF(K73<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K73-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R73)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K73<=(Main!$D$46/Main!$D$45*100),O73*Main!$D$45/100000+P72,IF(K73<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O73*Main!$D$45/100000+P72,IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S73))))),(IF(K73<=(Main!$D$72/Main!$D$71*100),O73*Main!$D$71/100000+P72,IF(K73<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O73*Main!$D$71/100000+P72,IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S73))))))","v":0},{"$f":"IF($A$90=TRUE,P73*Main!$D$45/100000+Q72,P73*100+Q72)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K73<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K73-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K73<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K73<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K73-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K73<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K73-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K73<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K73<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K73-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O73*Main!$D$45/100000+P72,IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O73*Main!$D$45/100000+P72,Main!$E$52)))),(IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O73*Main!$D$71/100000+P72,IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O73*Main!$D$71/100000+P72,Main!$E$78)))))","v":0},72,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T73-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T73-50)*PI()/50))))","v":-617.19072537784962},{"$f":"IF($A$90=TRUE,U73*2*Main!$D$50*(T73-T72)/100000+V72,U73*2*Ltime3*(T73-T72)/100000+V72)","v":22.984425094381496},-0.79565267309023779,0.57461062735953738,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W73*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W73<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W73*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W73<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W73*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W73<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W73*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W73<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W73*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W73<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W73*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W73<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.967272530243106},1379.0655056628898]
[null,null,null,null,null,null,null,null,null,null,73,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K74<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K74*PI()*Main!$D$45/100/Main!$D$46))),(IF(K74<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K74-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R74)))))))),(IF(K74<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K74*PI()*Main!$D$71/100/Main!$D$72))),(IF(K74<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K74-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R74)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K74<=(Main!$D$46/Main!$D$45*100),O74*Main!$D$45/100000+P73,IF(K74<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O74*Main!$D$45/100000+P73,IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S74))))),(IF(K74<=(Main!$D$72/Main!$D$71*100),O74*Main!$D$71/100000+P73,IF(K74<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O74*Main!$D$71/100000+P73,IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S74))))))","v":0},{"$f":"IF($A$90=TRUE,P74*Main!$D$45/100000+Q73,P74*100+Q73)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K74<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K74-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K74<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K74<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K74-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K74<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K74-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K74<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K74<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K74-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O74*Main!$D$45/100000+P73,IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O74*Main!$D$45/100000+P73,Main!$E$52)))),(IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O74*Main!$D$71/100000+P73,IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O74*Main!$D$71/100000+P73,Main!$E$78)))))","v":0},73,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T74-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T74-50)*PI()/50))))","v":-623.36550912991265},{"$f":"IF($A$90=TRUE,U74*2*Main!$D$50*(T74-T73)/100000+V73,U74*2*Ltime3*(T74-T73)/100000+V73)","v":21.73769407612167},-0.80361290806472696,0.5434423519030418,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W74*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W74<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W74*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W74<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W74*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W74<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W74*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W74<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W74*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W74<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W74*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W74<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.087001030587983},1304.2616445673002]
[null,null,null,null,null,null,null,null,null,null,74,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K75<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K75*PI()*Main!$D$45/100/Main!$D$46))),(IF(K75<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K75-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R75)))))))),(IF(K75<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K75*PI()*Main!$D$71/100/Main!$D$72))),(IF(K75<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K75-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R75)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K75<=(Main!$D$46/Main!$D$45*100),O75*Main!$D$45/100000+P74,IF(K75<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O75*Main!$D$45/100000+P74,IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S75))))),(IF(K75<=(Main!$D$72/Main!$D$71*100),O75*Main!$D$71/100000+P74,IF(K75<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O75*Main!$D$71/100000+P74,IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S75))))))","v":0},{"$f":"IF($A$90=TRUE,P75*Main!$D$45/100000+Q74,P75*100+Q74)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K75<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K75-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K75<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K75<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K75-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K75<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K75-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K75<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K75<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K75-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O75*Main!$D$45/100000+P74,IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O75*Main!$D$45/100000+P74,Main!$E$52)))),(IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O75*Main!$D$71/100000+P74,IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O75*Main!$D$71/100000+P74,Main!$E$78)))))","v":0},74,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T75-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T75-50)*PI()/50))))","v":-627.08015400605154},{"$f":"IF($A$90=TRUE,U75*2*Main!$D$50*(T75-T74)/100000+V74,U75*2*Ltime3*(T75-T74)/100000+V74)","v":20.483533768109567},-0.8084016500268999,0.51208834420273919,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W75*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W75<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W75*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W75<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W75*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W75<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W75*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W75<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W75*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W75<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W75*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W75<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.159027659890633},1229.012026086574]
[null,null,null,null,null,null,null,null,null,null,75,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K76<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K76*PI()*Main!$D$45/100/Main!$D$46))),(IF(K76<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K76-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R76)))))))),(IF(K76<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K76*PI()*Main!$D$71/100/Main!$D$72))),(IF(K76<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K76-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R76)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K76<=(Main!$D$46/Main!$D$45*100),O76*Main!$D$45/100000+P75,IF(K76<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O76*Main!$D$45/100000+P75,IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S76))))),(IF(K76<=(Main!$D$72/Main!$D$71*100),O76*Main!$D$71/100000+P75,IF(K76<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O76*Main!$D$71/100000+P75,IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S76))))))","v":0},{"$f":"IF($A$90=TRUE,P76*Main!$D$45/100000+Q75,P76*100+Q75)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K76<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K76-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K76<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K76<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K76-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K76<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K76-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K76<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K76<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K76-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O76*Main!$D$45/100000+P75,IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O76*Main!$D$45/100000+P75,Main!$E$52)))),(IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O76*Main!$D$71/100000+P75,IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O76*Main!$D$71/100000+P75,Main!$E$78)))))","v":0},75,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T76-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T76-50)*PI()/50))))","v":-628.31999999999994},{"$f":"IF($A$90=TRUE,U76*2*Main!$D$50*(T76-T75)/100000+V75,U76*2*Ltime3*(T76-T75)/100000+V75)","v":19.226893768109566},-0.80999999999999994,0.48067234420273913,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W76*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W76<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W76*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W76<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W76*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W76<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W76*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W76<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W76*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W76<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W76*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W76<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.183068161951041},1153.613626086574]
[null,null,null,null,null,null,null,null,null,null,76,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K77<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K77*PI()*Main!$D$45/100/Main!$D$46))),(IF(K77<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K77-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R77)))))))),(IF(K77<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K77*PI()*Main!$D$71/100/Main!$D$72))),(IF(K77<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K77-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R77)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K77<=(Main!$D$46/Main!$D$45*100),O77*Main!$D$45/100000+P76,IF(K77<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O77*Main!$D$45/100000+P76,IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S77))))),(IF(K77<=(Main!$D$72/Main!$D$71*100),O77*Main!$D$71/100000+P76,IF(K77<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O77*Main!$D$71/100000+P76,IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S77))))))","v":0},{"$f":"IF($A$90=TRUE,P77*Main!$D$45/100000+Q76,P77*100+Q76)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K77<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K77-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K77<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K77<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K77-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K77<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K77-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K77<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K77<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K77-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O77*Main!$D$45/100000+P76,IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O77*Main!$D$45/100000+P76,Main!$E$52)))),(IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O77*Main!$D$71/100000+P76,IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O77*Main!$D$71/100000+P76,Main!$E$78)))))","v":0},76,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T77-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T77-50)*PI()/50))))","v":-627.08015400605154},{"$f":"IF($A$90=TRUE,U77*2*Main!$D$50*(T77-T76)/100000+V76,U77*2*Ltime3*(T77-T76)/100000+V76)","v":17.972733460097462},-0.8084016500268999,0.44931833650243658,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W77*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W77<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W77*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W77<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W77*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W77<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W77*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W77<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W77*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W77<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W77*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W77<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.159027659890633},1078.3640076058477]
[null,null,null,null,null,null,null,null,null,null,77,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K78<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K78*PI()*Main!$D$45/100/Main!$D$46))),(IF(K78<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K78-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R78)))))))),(IF(K78<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K78*PI()*Main!$D$71/100/Main!$D$72))),(IF(K78<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K78-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R78)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K78<=(Main!$D$46/Main!$D$45*100),O78*Main!$D$45/100000+P77,IF(K78<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O78*Main!$D$45/100000+P77,IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S78))))),(IF(K78<=(Main!$D$72/Main!$D$71*100),O78*Main!$D$71/100000+P77,IF(K78<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O78*Main!$D$71/100000+P77,IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S78))))))","v":0},{"$f":"IF($A$90=TRUE,P78*Main!$D$45/100000+Q77,P78*100+Q77)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K78<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K78-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K78<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K78<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K78-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K78<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K78-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K78<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K78<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K78-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O78*Main!$D$45/100000+P77,IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O78*Main!$D$45/100000+P77,Main!$E$52)))),(IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O78*Main!$D$71/100000+P77,IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O78*Main!$D$71/100000+P77,Main!$E$78)))))","v":0},77,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T78-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T78-50)*PI()/50))))","v":-623.36550912991265},{"$f":"IF($A$90=TRUE,U78*2*Main!$D$50*(T78-T77)/100000+V77,U78*2*Ltime3*(T78-T77)/100000+V77)","v":16.726002441837636},-0.80361290806472696,0.41815006104594088,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W78*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W78<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W78*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W78<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W78*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W78<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W78*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W78<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W78*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W78<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W78*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W78<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.087001030587983},1003.5601465102582]
[null,null,null,null,null,null,null,null,null,null,78,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K79<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K79*PI()*Main!$D$45/100/Main!$D$46))),(IF(K79<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K79-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R79)))))))),(IF(K79<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K79*PI()*Main!$D$71/100/Main!$D$72))),(IF(K79<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K79-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R79)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K79<=(Main!$D$46/Main!$D$45*100),O79*Main!$D$45/100000+P78,IF(K79<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O79*Main!$D$45/100000+P78,IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S79))))),(IF(K79<=(Main!$D$72/Main!$D$71*100),O79*Main!$D$71/100000+P78,IF(K79<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O79*Main!$D$71/100000+P78,IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S79))))))","v":0},{"$f":"IF($A$90=TRUE,P79*Main!$D$45/100000+Q78,P79*100+Q78)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K79<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K79-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K79<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K79<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K79-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K79<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K79-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K79<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K79<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K79-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O79*Main!$D$45/100000+P78,IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O79*Main!$D$45/100000+P78,Main!$E$52)))),(IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O79*Main!$D$71/100000+P78,IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O79*Main!$D$71/100000+P78,Main!$E$78)))))","v":0},78,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T79-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T79-50)*PI()/50))))","v":-617.19072537784962},{"$f":"IF($A$90=TRUE,U79*2*Main!$D$50*(T79-T78)/100000+V78,U79*2*Ltime3*(T79-T78)/100000+V78)","v":15.491620991081938},-0.79565267309023779,0.38729052477704845,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W79*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W79<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W79*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W79<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W79*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W79<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W79*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W79<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W79*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W79<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W79*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W79<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.967272530243106},929.49725946491628]
["alle","alle",null,null,null,null,null,null,null,null,79,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K80<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K80*PI()*Main!$D$45/100/Main!$D$46))),(IF(K80<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K80-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R80)))))))),(IF(K80<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K80*PI()*Main!$D$71/100/Main!$D$72))),(IF(K80<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K80-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R80)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K80<=(Main!$D$46/Main!$D$45*100),O80*Main!$D$45/100000+P79,IF(K80<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O80*Main!$D$45/100000+P79,IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S80))))),(IF(K80<=(Main!$D$72/Main!$D$71*100),O80*Main!$D$71/100000+P79,IF(K80<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O80*Main!$D$71/100000+P79,IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S80))))))","v":0},{"$f":"IF($A$90=TRUE,P80*Main!$D$45/100000+Q79,P80*100+Q79)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K80<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K80-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K80<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K80<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K80-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K80<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K80-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K80<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K80<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K80-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O80*Main!$D$45/100000+P79,IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O80*Main!$D$45/100000+P79,Main!$E$52)))),(IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O80*Main!$D$71/100000+P79,IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O80*Main!$D$71/100000+P79,Main!$E$78)))))","v":0},79,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T80-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T80-50)*PI()/50))))","v":-608.58017180034142},{"$f":"IF($A$90=TRUE,U80*2*Main!$D$50*(T80-T79)/100000+V79,U80*2*Ltime3*(T80-T79)/100000+V79)","v":14.274460647481256},-0.78455236051419108,0.35686151618703138,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W80*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W80<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W80*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W80<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W80*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W80<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W80*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W80<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W80*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W80<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W80*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W80<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.800314672548119},856.46763884887537]
[null,null,null,null,null,null,null,null,null,null,80,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K81<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K81*PI()*Main!$D$45/100/Main!$D$46))),(IF(K81<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K81-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R81)))))))),(IF(K81<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K81*PI()*Main!$D$71/100/Main!$D$72))),(IF(K81<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K81-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R81)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K81<=(Main!$D$46/Main!$D$45*100),O81*Main!$D$45/100000+P80,IF(K81<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O81*Main!$D$45/100000+P80,IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S81))))),(IF(K81<=(Main!$D$72/Main!$D$71*100),O81*Main!$D$71/100000+P80,IF(K81<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O81*Main!$D$71/100000+P80,IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S81))))))","v":0},{"$f":"IF($A$90=TRUE,P81*Main!$D$45/100000+Q80,P81*100+Q80)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K81<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K81-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K81<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K81<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K81-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K81<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K81-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K81<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K81<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K81-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O81*Main!$D$45/100000+P80,IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O81*Main!$D$45/100000+P80,Main!$E$52)))),(IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O81*Main!$D$71/100000+P80,IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O81*Main!$D$71/100000+P80,Main!$E$78)))))","v":0},80,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T81-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T81-50)*PI()/50))))","v":-597.56783031857083},{"$f":"IF($A$90=TRUE,U81*2*Main!$D$50*(T81-T80)/100000+V80,U81*2*Ltime3*(T81-T80)/100000+V80)","v":13.079324986844114},-0.7703557781990743,0.32698312467110285,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W81*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W81<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W81*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W81<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W81*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W81<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W81*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W81<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W81*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W81<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W81*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W81<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.586786363891557},784.75949921064682]
[null,null,null,null,null,null,null,null,null,null,81,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K82<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K82*PI()*Main!$D$45/100/Main!$D$46))),(IF(K82<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K82-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R82)))))))),(IF(K82<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K82*PI()*Main!$D$71/100/Main!$D$72))),(IF(K82<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K82-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R82)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K82<=(Main!$D$46/Main!$D$45*100),O82*Main!$D$45/100000+P81,IF(K82<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O82*Main!$D$45/100000+P81,IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S82))))),(IF(K82<=(Main!$D$72/Main!$D$71*100),O82*Main!$D$71/100000+P81,IF(K82<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O82*Main!$D$71/100000+P81,IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S82))))))","v":0},{"$f":"IF($A$90=TRUE,P82*Main!$D$45/100000+Q81,P82*100+Q81)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K82<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K82-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K82<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K82<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K82-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K82<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K82-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K82<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K82<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K82-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O82*Main!$D$45/100000+P81,IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O82*Main!$D$45/100000+P81,Main!$E$52)))),(IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O82*Main!$D$71/100000+P81,IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O82*Main!$D$71/100000+P81,Main!$E$78)))))","v":0},81,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T82-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T82-50)*PI()/50))))","v":-584.19716161330609},{"$f":"IF($A$90=TRUE,U82*2*Main!$D$50*(T82-T81)/100000+V81,U82*2*Ltime3*(T82-T81)/100000+V81)","v":11.910930663617501},-0.75311895356948366,0.29777326659043751,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W82*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W82<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W82*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W82<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W82*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W82<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W82*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W82<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W82*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W82<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W82*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W82<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.327530302955878},714.65583981705004]
[null,null,null,null,null,null,null,null,null,null,82,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K83<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K83*PI()*Main!$D$45/100/Main!$D$46))),(IF(K83<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K83-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R83)))))))),(IF(K83<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K83*PI()*Main!$D$71/100/Main!$D$72))),(IF(K83<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K83-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R83)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K83<=(Main!$D$46/Main!$D$45*100),O83*Main!$D$45/100000+P82,IF(K83<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O83*Main!$D$45/100000+P82,IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S83))))),(IF(K83<=(Main!$D$72/Main!$D$71*100),O83*Main!$D$71/100000+P82,IF(K83<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O83*Main!$D$71/100000+P82,IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S83))))))","v":0},{"$f":"IF($A$90=TRUE,P83*Main!$D$45/100000+Q82,P83*100+Q82)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K83<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K83-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K83<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K83<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K83-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K83<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K83-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K83<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K83<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K83-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O83*Main!$D$45/100000+P82,IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O83*Main!$D$45/100000+P82,Main!$E$52)))),(IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O83*Main!$D$71/100000+P82,IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O83*Main!$D$71/100000+P82,Main!$E$78)))))","v":0},82,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T83-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T83-50)*PI()/50))))","v":-568.52093360544927},{"$f":"IF($A$90=TRUE,U83*2*Main!$D$50*(T83-T82)/100000+V82,U83*2*Ltime3*(T83-T82)/100000+V82)","v":10.773888796406602},-0.73290991249747572,0.26934721991016508,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W83*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W83<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W83*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W83<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W83*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W83<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W83*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W83<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W83*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W83<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W83*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W83<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":11.023569654970764},646.43332778439617]
[null,null,null,null,null,null,null,null,null,null,83,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K84<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K84*PI()*Main!$D$45/100/Main!$D$46))),(IF(K84<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K84-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R84)))))))),(IF(K84<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K84*PI()*Main!$D$71/100/Main!$D$72))),(IF(K84<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K84-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R84)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K84<=(Main!$D$46/Main!$D$45*100),O84*Main!$D$45/100000+P83,IF(K84<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O84*Main!$D$45/100000+P83,IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S84))))),(IF(K84<=(Main!$D$72/Main!$D$71*100),O84*Main!$D$71/100000+P83,IF(K84<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O84*Main!$D$71/100000+P83,IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S84))))))","v":0},{"$f":"IF($A$90=TRUE,P84*Main!$D$45/100000+Q83,P84*100+Q83)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K84<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K84-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K84<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K84<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K84-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K84<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K84-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K84<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K84<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K84-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O84*Main!$D$45/100000+P83,IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O84*Main!$D$45/100000+P83,Main!$E$52)))),(IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O84*Main!$D$71/100000+P83,IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O84*Main!$D$71/100000+P83,Main!$E$78)))))","v":0},83,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T84-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T84-50)*PI()/50))))","v":-550.60101320516026},{"$f":"IF($A$90=TRUE,U84*2*Main!$D$50*(T84-T83)/100000+V83,U84*2*Ltime3*(T84-T83)/100000+V83)","v":9.6726867699962824},-0.70980841083552937,0.24181716924990707,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W84*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W84<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W84*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W84<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W84*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W84<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W84*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W84<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W84*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W84<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W84*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W84<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":10.676104013747413},580.36120619977692]
[{"$f":"time1+time2+time3+time4","v":481},null,null,null,null,null,null,null,null,null,84,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K85<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K85*PI()*Main!$D$45/100/Main!$D$46))),(IF(K85<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K85-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R85)))))))),(IF(K85<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K85*PI()*Main!$D$71/100/Main!$D$72))),(IF(K85<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K85-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R85)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K85<=(Main!$D$46/Main!$D$45*100),O85*Main!$D$45/100000+P84,IF(K85<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O85*Main!$D$45/100000+P84,IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S85))))),(IF(K85<=(Main!$D$72/Main!$D$71*100),O85*Main!$D$71/100000+P84,IF(K85<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O85*Main!$D$71/100000+P84,IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S85))))))","v":0},{"$f":"IF($A$90=TRUE,P85*Main!$D$45/100000+Q84,P85*100+Q84)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K85<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K85-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K85<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K85<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K85-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K85<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K85-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K85<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K85<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K85-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O85*Main!$D$45/100000+P84,IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O85*Main!$D$45/100000+P84,Main!$E$52)))),(IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O85*Main!$D$71/100000+P84,IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O85*Main!$D$71/100000+P84,Main!$E$78)))))","v":0},84,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T85-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T85-50)*PI()/50))))","v":-530.50812215142594},{"$f":"IF($A$90=TRUE,U85*2*Main!$D$50*(T85-T84)/100000+V84,U85*2*Ltime3*(T85-T84)/100000+V84)","v":8.6116705256934303},-0.68390561965663199,0.21529176314233575,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W85*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W85<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W85*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W85<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W85*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W85<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W85*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W85<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W85*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W85<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W85*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W85<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":10.286504667429769},516.70023154160583]
[{"$f":"Ltime1+Ltime2+Ltime3+Ltime4","v":130},null,null,null,null,null,null,null,null,null,85,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K86<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K86*PI()*Main!$D$45/100/Main!$D$46))),(IF(K86<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K86-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R86)))))))),(IF(K86<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K86*PI()*Main!$D$71/100/Main!$D$72))),(IF(K86<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K86-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R86)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K86<=(Main!$D$46/Main!$D$45*100),O86*Main!$D$45/100000+P85,IF(K86<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O86*Main!$D$45/100000+P85,IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S86))))),(IF(K86<=(Main!$D$72/Main!$D$71*100),O86*Main!$D$71/100000+P85,IF(K86<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O86*Main!$D$71/100000+P85,IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S86))))))","v":0},{"$f":"IF($A$90=TRUE,P86*Main!$D$45/100000+Q85,P86*100+Q85)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K86<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K86-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K86<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K86<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K86-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K86<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K86-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K86<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K86<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K86-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O86*Main!$D$45/100000+P85,IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O86*Main!$D$45/100000+P85,Main!$E$52)))),(IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O86*Main!$D$71/100000+P85,IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O86*Main!$D$71/100000+P85,Main!$E$78)))))","v":0},85,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T86-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T86-50)*PI()/50))))","v":-508.32155790566691},{"$f":"IF($A$90=TRUE,U86*2*Main!$D$50*(T86-T85)/100000+V85,U86*2*Ltime3*(T86-T85)/100000+V85)","v":7.5950274098820962},-0.65530376544370739,0.18987568524705239,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W86*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W86<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W86*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W86<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W86*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W86<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W86*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W86<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W86*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W86<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W86*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W86<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9.8563091866467474},455.70164459292573]
[null,null,null,null,null,null,null,null,null,null,86,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K87<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K87*PI()*Main!$D$45/100/Main!$D$46))),(IF(K87<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K87-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R87)))))))),(IF(K87<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K87*PI()*Main!$D$71/100/Main!$D$72))),(IF(K87<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K87-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R87)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K87<=(Main!$D$46/Main!$D$45*100),O87*Main!$D$45/100000+P86,IF(K87<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O87*Main!$D$45/100000+P86,IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S87))))),(IF(K87<=(Main!$D$72/Main!$D$71*100),O87*Main!$D$71/100000+P86,IF(K87<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O87*Main!$D$71/100000+P86,IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S87))))))","v":0},{"$f":"IF($A$90=TRUE,P87*Main!$D$45/100000+Q86,P87*100+Q86)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K87<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K87-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K87<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K87<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K87-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K87<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K87-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K87<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K87<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K87-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O87*Main!$D$45/100000+P86,IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O87*Main!$D$45/100000+P86,Main!$E$52)))),(IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O87*Main!$D$71/100000+P86,IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O87*Main!$D$71/100000+P86,Main!$E$78)))))","v":0},86,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T87-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T87-50)*PI()/50))))","v":-484.12888070088383},{"$f":"IF($A$90=TRUE,U87*2*Main!$D$50*(T87-T86)/100000+V86,U87*2*Ltime3*(T87-T86)/100000+V86)","v":6.6267696484803285},-0.62411572664838921,0.16566924121200821,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W87*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W87<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W87*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W87<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W87*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W87<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W87*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W87<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W87*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W87<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W87*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W87<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9.3872153564233702},397.60617890881969]
[null,null,null,null,null,null,null,null,null,null,87,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K88<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K88*PI()*Main!$D$45/100/Main!$D$46))),(IF(K88<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K88-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R88)))))))),(IF(K88<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K88*PI()*Main!$D$71/100/Main!$D$72))),(IF(K88<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K88-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R88)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K88<=(Main!$D$46/Main!$D$45*100),O88*Main!$D$45/100000+P87,IF(K88<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O88*Main!$D$45/100000+P87,IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S88))))),(IF(K88<=(Main!$D$72/Main!$D$71*100),O88*Main!$D$71/100000+P87,IF(K88<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O88*Main!$D$71/100000+P87,IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S88))))))","v":0},{"$f":"IF($A$90=TRUE,P88*Main!$D$45/100000+Q87,P88*100+Q87)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K88<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K88-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K88<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K88<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K88-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K88<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K88-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K88<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K88<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K88-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O88*Main!$D$45/100000+P87,IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O88*Main!$D$45/100000+P87,Main!$E$52)))),(IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O88*Main!$D$71/100000+P87,IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O88*Main!$D$71/100000+P87,Main!$E$78)))))","v":0},87,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T88-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T88-50)*PI()/50))))","v":-458.0255679814212},{"$f":"IF($A$90=TRUE,U88*2*Main!$D$50*(T88-T87)/100000+V87,U88*2*Ltime3*(T88-T87)/100000+V87)","v":5.7107185125174862},-0.59046458821134318,0.14276796281293716,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W88*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W88<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W88*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W88<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W88*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W88<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W88*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W88<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W88*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W88<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W88*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W88<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":8.8810744757989468},342.64311075104916]
[null,null,null,null,null,null,null,null,null,null,88,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K89<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K89*PI()*Main!$D$45/100/Main!$D$46))),(IF(K89<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K89-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R89)))))))),(IF(K89<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K89*PI()*Main!$D$71/100/Main!$D$72))),(IF(K89<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K89-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R89)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K89<=(Main!$D$46/Main!$D$45*100),O89*Main!$D$45/100000+P88,IF(K89<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O89*Main!$D$45/100000+P88,IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S89))))),(IF(K89<=(Main!$D$72/Main!$D$71*100),O89*Main!$D$71/100000+P88,IF(K89<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O89*Main!$D$71/100000+P88,IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S89))))))","v":0},{"$f":"IF($A$90=TRUE,P89*Main!$D$45/100000+Q88,P89*100+Q88)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K89<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K89-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K89<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K89<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K89-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K89<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K89-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K89<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K89<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K89-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O89*Main!$D$45/100000+P88,IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O89*Main!$D$45/100000+P88,Main!$E$52)))),(IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O89*Main!$D$71/100000+P88,IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O89*Main!$D$71/100000+P88,Main!$E$78)))))","v":0},88,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T89-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T89-50)*PI()/50))))","v":-430.1146375971137},{"$f":"IF($A$90=TRUE,U89*2*Main!$D$50*(T89-T88)/100000+V88,U89*2*Ltime3*(T89-T88)/100000+V88)","v":4.8504892373232584},-0.55448315580223784,0.12126223093308146,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W89*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W89<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W89*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W89<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W89*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W89<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W89*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W89<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W89*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W89<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W89*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W89<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":8.3398840515955346},291.0293542393955]
[true,null,null,null,null,null,null,null,null,null,89,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K90<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K90*PI()*Main!$D$45/100/Main!$D$46))),(IF(K90<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K90-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R90)))))))),(IF(K90<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K90*PI()*Main!$D$71/100/Main!$D$72))),(IF(K90<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K90-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R90)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K90<=(Main!$D$46/Main!$D$45*100),O90*Main!$D$45/100000+P89,IF(K90<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O90*Main!$D$45/100000+P89,IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S90))))),(IF(K90<=(Main!$D$72/Main!$D$71*100),O90*Main!$D$71/100000+P89,IF(K90<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O90*Main!$D$71/100000+P89,IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S90))))))","v":0},{"$f":"IF($A$90=TRUE,P90*Main!$D$45/100000+Q89,P90*100+Q89)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K90<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K90-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K90<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K90<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K90-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K90<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K90-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K90<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K90<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K90-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O90*Main!$D$45/100000+P89,IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O90*Main!$D$45/100000+P89,Main!$E$52)))),(IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O90*Main!$D$71/100000+P89,IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O90*Main!$D$71/100000+P89,Main!$E$78)))))","v":0},89,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T90-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T90-50)*PI()/50))))","v":-400.50624123889679},{"$f":"IF($A$90=TRUE,U90*2*Main!$D$50*(T90-T89)/100000+V89,U90*2*Ltime3*(T90-T89)/100000+V89)","v":4.0494767548454647},-0.51631343169643873,0.10123691887113662,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W90*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W90<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W90*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W90<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W90*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W90<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W90*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W90<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W90*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W90<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W90*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W90<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.7657799151710698},242.96860529072788]
[null,null,null,null,null,null,null,null,null,null,90,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K91<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K91*PI()*Main!$D$45/100/Main!$D$46))),(IF(K91<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K91-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R91)))))))),(IF(K91<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K91*PI()*Main!$D$71/100/Main!$D$72))),(IF(K91<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K91-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R91)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K91<=(Main!$D$46/Main!$D$45*100),O91*Main!$D$45/100000+P90,IF(K91<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O91*Main!$D$45/100000+P90,IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S91))))),(IF(K91<=(Main!$D$72/Main!$D$71*100),O91*Main!$D$71/100000+P90,IF(K91<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O91*Main!$D$71/100000+P90,IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S91))))))","v":0},{"$f":"IF($A$90=TRUE,P91*Main!$D$45/100000+Q90,P91*100+Q90)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K91<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K91-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K91<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K91<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K91-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K91<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K91-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K91<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K91<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K91-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O91*Main!$D$45/100000+P90,IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O91*Main!$D$45/100000+P90,Main!$E$52)))),(IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O91*Main!$D$71/100000+P90,IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O91*Main!$D$71/100000+P90,Main!$E$78)))))","v":0},90,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T91-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T91-50)*PI()/50))))","v":-369.31722972040677},{"$f":"IF($A$90=TRUE,U91*2*Main!$D$50*(T91-T90)/100000+V90,U91*2*Ltime3*(T91-T90)/100000+V90)","v":3.310842295404651},-0.47610605435690329,8.2771057385116281E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W91*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W91<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W91*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W91<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W91*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W91<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W91*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W91<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W91*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W91<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W91*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W91<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.16102779326879},198.65053772427908]
[null,null,null,null,null,null,null,null,null,null,91,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K92<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K92*PI()*Main!$D$45/100/Main!$D$46))),(IF(K92<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K92-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R92)))))))),(IF(K92<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K92*PI()*Main!$D$71/100/Main!$D$72))),(IF(K92<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K92-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R92)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K92<=(Main!$D$46/Main!$D$45*100),O92*Main!$D$45/100000+P91,IF(K92<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O92*Main!$D$45/100000+P91,IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S92))))),(IF(K92<=(Main!$D$72/Main!$D$71*100),O92*Main!$D$71/100000+P91,IF(K92<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O92*Main!$D$71/100000+P91,IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S92))))))","v":0},{"$f":"IF($A$90=TRUE,P92*Main!$D$45/100000+Q91,P92*100+Q91)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K92<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K92-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K92<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K92<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K92-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K92<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K92-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K92<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K92<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K92-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O92*Main!$D$45/100000+P91,IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O92*Main!$D$45/100000+P91,Main!$E$52)))),(IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O92*Main!$D$71/100000+P91,IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O92*Main!$D$71/100000+P91,Main!$E$78)))))","v":0},91,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T92-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T92-50)*PI()/50))))","v":-336.67069182120338},{"$f":"IF($A$90=TRUE,U92*2*Main!$D$50*(T92-T91)/100000+V91,U92*2*Ltime3*(T92-T91)/100000+V91)","v":2.6375009117622445},-0.43401970393298756,6.5937522794056111E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W92*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W92<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W92*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W92<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W92*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W92<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W92*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W92<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W92*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W92<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W92*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W92<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":6.5280143662288861},158.25005470573467]
[null,null,null,null,null,null,null,null,null,null,92,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K93<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K93*PI()*Main!$D$45/100/Main!$D$46))),(IF(K93<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K93-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R93)))))))),(IF(K93<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K93*PI()*Main!$D$71/100/Main!$D$72))),(IF(K93<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K93-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R93)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K93<=(Main!$D$46/Main!$D$45*100),O93*Main!$D$45/100000+P92,IF(K93<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O93*Main!$D$45/100000+P92,IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S93))))),(IF(K93<=(Main!$D$72/Main!$D$71*100),O93*Main!$D$71/100000+P92,IF(K93<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O93*Main!$D$71/100000+P92,IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S93))))))","v":0},{"$f":"IF($A$90=TRUE,P93*Main!$D$45/100000+Q92,P93*100+Q92)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K93<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K93-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K93<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K93<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K93-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K93<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K93-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K93<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K93<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K93-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O93*Main!$D$45/100000+P92,IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O93*Main!$D$45/100000+P92,Main!$E$52)))),(IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O93*Main!$D$71/100000+P92,IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O93*Main!$D$71/100000+P92,Main!$E$78)))))","v":0},92,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T93-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T93-50)*PI()/50))))","v":-302.6954685115897},{"$f":"IF($A$90=TRUE,U93*2*Main!$D$50*(T93-T92)/100000+V92,U93*2*Ltime3*(T93-T92)/100000+V92)","v":2.0321099747390652},-0.3902204760223893,5.0802749368476632E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W93*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W93<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W93*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W93<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W93*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W93<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W93*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W93<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W93*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W93<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W93*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W93<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":5.8692378488515438},121.92659848434391]
[null,null,null,null,null,null,null,null,null,null,93,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K94<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K94*PI()*Main!$D$45/100/Main!$D$46))),(IF(K94<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K94-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R94)))))))),(IF(K94<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K94*PI()*Main!$D$71/100/Main!$D$72))),(IF(K94<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K94-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R94)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K94<=(Main!$D$46/Main!$D$45*100),O94*Main!$D$45/100000+P93,IF(K94<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O94*Main!$D$45/100000+P93,IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S94))))),(IF(K94<=(Main!$D$72/Main!$D$71*100),O94*Main!$D$71/100000+P93,IF(K94<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O94*Main!$D$71/100000+P93,IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S94))))))","v":0},{"$f":"IF($A$90=TRUE,P94*Main!$D$45/100000+Q93,P94*100+Q93)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K94<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K94-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K94<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K94<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K94-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K94<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K94-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K94<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K94<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K94-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O94*Main!$D$45/100000+P93,IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O94*Main!$D$45/100000+P93,Main!$E$52)))),(IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O94*Main!$D$71/100000+P93,IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O94*Main!$D$71/100000+P93,Main!$E$78)))))","v":0},93,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T94-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T94-50)*PI()/50))))","v":-267.52564447616658},{"$f":"IF($A$90=TRUE,U94*2*Main!$D$50*(T94-T93)/100000+V93,U94*2*Ltime3*(T94-T93)/100000+V93)","v":1.4970586857867321},-0.344881226167709,3.7426467144668303E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W94*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W94<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W94*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W94<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W94*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W94<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W94*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W94<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W94*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W94<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W94*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W94<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":5.1872981310845088},89.823521147203934]
[null,null,null,null,null,null,null,null,null,null,94,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K95<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K95*PI()*Main!$D$45/100/Main!$D$46))),(IF(K95<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K95-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R95)))))))),(IF(K95<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K95*PI()*Main!$D$71/100/Main!$D$72))),(IF(K95<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K95-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R95)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K95<=(Main!$D$46/Main!$D$45*100),O95*Main!$D$45/100000+P94,IF(K95<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O95*Main!$D$45/100000+P94,IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S95))))),(IF(K95<=(Main!$D$72/Main!$D$71*100),O95*Main!$D$71/100000+P94,IF(K95<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O95*Main!$D$71/100000+P94,IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S95))))))","v":0},{"$f":"IF($A$90=TRUE,P95*Main!$D$45/100000+Q94,P95*100+Q94)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K95<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K95-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K95<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K95<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K95-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K95<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K95-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K95<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K95<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K95-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O95*Main!$D$45/100000+P94,IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O95*Main!$D$45/100000+P94,Main!$E$52)))),(IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O95*Main!$D$71/100000+P94,IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O95*Main!$D$71/100000+P94,Main!$E$78)))))","v":0},94,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T95-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T95-50)*PI()/50))))","v":-231.30001894283694},{"$f":"IF($A$90=TRUE,U95*2*Main!$D$50*(T95-T94)/100000+V94,U95*2*Ltime3*(T95-T94)/100000+V94)","v":1.0344586479010582},-0.29818088767458928,2.5861466197526457E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W95*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W95<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W95*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W95<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W95*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W95<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W95*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W95<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W95*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W95<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W95*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W95<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":4.4848865174451715},62.067518874063495]
[null,null,null,null,null,null,null,null,null,null,95,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K96<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K96*PI()*Main!$D$45/100/Main!$D$46))),(IF(K96<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K96-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R96)))))))),(IF(K96<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K96*PI()*Main!$D$71/100/Main!$D$72))),(IF(K96<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K96-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R96)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K96<=(Main!$D$46/Main!$D$45*100),O96*Main!$D$45/100000+P95,IF(K96<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O96*Main!$D$45/100000+P95,IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S96))))),(IF(K96<=(Main!$D$72/Main!$D$71*100),O96*Main!$D$71/100000+P95,IF(K96<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O96*Main!$D$71/100000+P95,IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S96))))))","v":0},{"$f":"IF($A$90=TRUE,P96*Main!$D$45/100000+Q95,P96*100+Q95)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K96<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K96-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K96<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K96<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K96-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K96<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K96-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K96<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K96<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K96-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O96*Main!$D$45/100000+P95,IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O96*Main!$D$45/100000+P95,Main!$E$52)))),(IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O96*Main!$D$71/100000+P95,IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O96*Main!$D$71/100000+P95,Main!$E$78)))))","v":0},96,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T96-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T96-50)*PI()/50))))","v":-156.25682990342182},{"$f":"IF($A$90=TRUE,U96*2*Main!$D$50*(T96-T95)/100000+V95,U96*2*Ltime3*(T96-T95)/100000+V95)","v":0.40943132828737094},-0.20143880860353272,1.0235783207184273E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W96*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W96<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W96*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W96<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W96*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W96<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W96*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W96<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W96*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W96<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W96*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W96<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":3.0298058465173443},24.565879697242256]
[null,null,null,null,null,null,null,null,null,null,96,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K97<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K97*PI()*Main!$D$45/100/Main!$D$46))),(IF(K97<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K97-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R97)))))))),(IF(K97<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K97*PI()*Main!$D$71/100/Main!$D$72))),(IF(K97<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K97-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R97)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K97<=(Main!$D$46/Main!$D$45*100),O97*Main!$D$45/100000+P96,IF(K97<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O97*Main!$D$45/100000+P96,IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S97))))),(IF(K97<=(Main!$D$72/Main!$D$71*100),O97*Main!$D$71/100000+P96,IF(K97<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O97*Main!$D$71/100000+P96,IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S97))))))","v":0},{"$f":"IF($A$90=TRUE,P97*Main!$D$45/100000+Q96,P97*100+Q96)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K97<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K97-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K97<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K97<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K97-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K97<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K97-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K97<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K97<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K97-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O97*Main!$D$45/100000+P96,IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O97*Main!$D$45/100000+P96,Main!$E$52)))),(IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O97*Main!$D$71/100000+P96,IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O97*Main!$D$71/100000+P96,Main!$E$78)))))","v":0},98,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T97-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T97-50)*PI()/50))))","v":-78.749377313123816},{"$f":"IF($A$90=TRUE,U97*2*Main!$D$50*(T97-T96)/100000+V96,U97*2*Ltime3*(T97-T96)/100000+V96)","v":9.4433819034875688E-2},-0.10151991918708667,2.3608454758718921E-3,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W97*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W97<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W97*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W97<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W97*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W97<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W97*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W97<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W97*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W97<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W97*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W97<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":1.5269433274716522},5.6660291420925413]
[null,null,null,null,null,null,null,null,null,null,97,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K98<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K98*PI()*Main!$D$45/100/Main!$D$46))),(IF(K98<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K98-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R98)))))))),(IF(K98<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K98*PI()*Main!$D$71/100/Main!$D$72))),(IF(K98<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K98-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R98)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K98<=(Main!$D$46/Main!$D$45*100),O98*Main!$D$45/100000+P97,IF(K98<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O98*Main!$D$45/100000+P97,IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S98))))),(IF(K98<=(Main!$D$72/Main!$D$71*100),O98*Main!$D$71/100000+P97,IF(K98<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O98*Main!$D$71/100000+P97,IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S98))))))","v":0},{"$f":"IF($A$90=TRUE,P98*Main!$D$45/100000+Q97,P98*100+Q97)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K98<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K98-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K98<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K98<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K98-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K98<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K98-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K98<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K98<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K98-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O98*Main!$D$45/100000+P97,IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O98*Main!$D$45/100000+P97,Main!$E$52)))),(IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O98*Main!$D$71/100000+P97,IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O98*Main!$D$71/100000+P97,Main!$E$78)))))","v":0},99,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T98-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T98-50)*PI()/50))))","v":-39.452539230658303},{"$f":"IF($A$90=TRUE,U98*2*Main!$D$50*(T98-T97)/100000+V97,U98*2*Ltime3*(T98-T97)/100000+V97)","v":1.5528740573559074E-2},-5.086032081874399E-2,3.8821851433897686E-4,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W98*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W98<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W98*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W98<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W98*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W98<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W98*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W98<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W98*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W98<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W98*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W98<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":0.76498117934994525},0.93172443441354447]
[null,null,null,null,null,null,null,null,null,null,98,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K99<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K99*PI()*Main!$D$45/100/Main!$D$46))),(IF(K99<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K99-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R99)))))))),(IF(K99<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K99*PI()*Main!$D$71/100/Main!$D$72))),(IF(K99<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K99-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R99)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K99<=(Main!$D$46/Main!$D$45*100),O99*Main!$D$45/100000+P98,IF(K99<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O99*Main!$D$45/100000+P98,IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S99))))),(IF(K99<=(Main!$D$72/Main!$D$71*100),O99*Main!$D$71/100000+P98,IF(K99<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O99*Main!$D$71/100000+P98,IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S99))))))","v":0},{"$f":"IF($A$90=TRUE,P99*Main!$D$45/100000+Q98,P99*100+Q98)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K99<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K99-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K99<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K99<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K99-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K99<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K99-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K99<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K99<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K99-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O99*Main!$D$45/100000+P98,IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O99*Main!$D$45/100000+P98,Main!$E$52)))),(IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O99*Main!$D$71/100000+P98,IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O99*Main!$D$71/100000+P98,Main!$E$78)))))","v":0},99.999999000000003,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T99-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T99-50)*PI()/50))))","v":-3.9478509987729358E-5},{"$f":"IF($A$90=TRUE,U99*2*Main!$D$50*(T99-T98)/100000+V98,U99*2*Ltime3*(T99-T98)/100000+V98)","v":1.5528661616618056E-2},-5.0893801072798543E-8,3.8821654041545141E-4,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W99*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W99<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W99*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W99<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W99*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W99<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W99*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W99<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W99*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W99<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W99*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W99<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.6548474998849599E-7},0.93171969699708335]
[0,12.2,null,null,null,null,null,null,null,null,99,0,0,0.99989727158268316,{"$f":"IF($A$90=TRUE,(IF(K100<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K100*PI()*Main!$D$45/100/Main!$D$46))),(IF(K100<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K100-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R100)))))))),(IF(K100<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K100*PI()*Main!$D$71/100/Main!$D$72))),(IF(K100<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K100-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R100)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K100<=(Main!$D$46/Main!$D$45*100),O100*Main!$D$45/100000+P99,IF(K100<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O100*Main!$D$45/100000+P99,IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S100))))),(IF(K100<=(Main!$D$72/Main!$D$71*100),O100*Main!$D$71/100000+P99,IF(K100<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O100*Main!$D$71/100000+P99,IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S100))))))","v":0},{"$f":"IF($A$90=TRUE,P100*Main!$D$45/100000+Q99,P100*100+Q99)","v":3.6089751347917045},{"$f":"IF($A$90=TRUE,(IF(K100<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K100-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K100<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K100<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K100-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K100<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K100-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K100<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K100<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K100-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O100*Main!$D$45/100000+P99,IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O100*Main!$D$45/100000+P99,Main!$E$52)))),(IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O100*Main!$D$71/100000+P99,IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O100*Main!$D$71/100000+P99,Main!$E$78)))))","v":0},99.999999000000003,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T100-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T100-50)*PI()/50))))","v":-3.9478509987729358E-5},{"$f":"IF($A$90=TRUE,U100*2*Main!$D$50*(T100-T99)/100000+V99,U100*2*Ltime3*(T100-T99)/100000+V99)","v":1.5528661616618056E-2},-5.0893801072798543E-8,3.8821654041545141E-4,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W100*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W100<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W100*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W100<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W100*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+Ltorque)/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W100*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W100<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W100*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W100<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W100*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+Ltorque)/LWirkungsgrad))),0)","v":0},0.93171969699708335]
[2308.0112950990879,12.2,null,null,null,null,null,null,null,null,100,null,null,null,null,null,null,null,null,100,0,{"$f":"IF($A$90=TRUE,Main!$E$46,Lspeed1)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W101*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W101<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W101*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W101<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W101*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W101<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W101*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W101<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W101*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W101<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W101*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W101<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":0},0]
[2500,4.0107045659157627,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"100+T2","v":100.000001},{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T102-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T102-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U102*2*Main!$D$55*(T102-T101)/100000+V101,U102*2*Ltime5*(T102-T101)/100000+V101)","v":0},0,0,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W102*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W102>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W102*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W102>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W102*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W102>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W102*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W102>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W102*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W102>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W102*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W102>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad))),0)","v":0},0]
[0,4.51,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"100+T3","v":100.000001},{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T103-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T103-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U103*2*Main!$D$55*(T103-T102)/100000+V102,U103*2*Ltime5*(T103-T102)/100000+V102)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W103*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W103>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W103*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W103>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W103*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W103>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W103*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W103>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W103*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W103>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W103*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W103>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[2500,4.0107045659157627,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,101,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T104-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T104-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U104*2*Main!$D$55*(T104-T103)/100000+V103,U104*2*Ltime5*(T104-T103)/100000+V103)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W104*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W104>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W104*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W104>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W104*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W104>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W104*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W104>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W104*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W104>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W104*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W104>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[2500,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,102,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T105-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T105-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U105*2*Main!$D$55*(T105-T104)/100000+V104,U105*2*Ltime5*(T105-T104)/100000+V104)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W105*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W105>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W105*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W105>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W105*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W105>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W105*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W105>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W105*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W105>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W105*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W105>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T106-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T106-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U106*2*Main!$D$55*(T106-T105)/100000+V105,U106*2*Ltime5*(T106-T105)/100000+V105)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W106*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W106>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W106*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W106>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W106*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W106>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W106*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W106>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W106*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W106>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W106*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W106>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[0.58600000000000008,305,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,106,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T107-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T107-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U107*2*Main!$D$55*(T107-T106)/100000+V106,U107*2*Ltime5*(T107-T106)/100000+V106)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W107*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W107>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W107*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W107>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W107*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W107>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W107*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W107>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W107*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W107>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W107*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W107>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[4.51,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,107,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T108-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T108-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U108*2*Main!$D$55*(T108-T107)/100000+V107,U108*2*Ltime5*(T108-T107)/100000+V107)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W108*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W108>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W108*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W108>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W108*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W108>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W108*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W108>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W108*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W108>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W108*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W108>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[4.6900000000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,108,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T109-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T109-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U109*2*Main!$D$55*(T109-T108)/100000+V108,U109*2*Ltime5*(T109-T108)/100000+V108)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W109*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W109>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W109*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W109>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W109*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W109>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W109*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W109>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W109*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W109>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W109*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W109>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[4.0107045659157627,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,109,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T110-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T110-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U110*2*Main!$D$55*(T110-T109)/100000+V109,U110*2*Ltime5*(T110-T109)/100000+V109)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W110*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W110>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W110*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W110>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W110*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W110>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W110*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W110>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W110*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W110>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W110*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W110>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[4.1347469751708896,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,110,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T111-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T111-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U111*2*Main!$D$55*(T111-T110)/100000+V110,U111*2*Ltime5*(T111-T110)/100000+V110)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W111*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W111>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W111*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W111>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W111*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W111>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W111*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W111>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W111*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W111>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W111*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W111>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[2500,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,111,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T112-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T112-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U112*2*Main!$D$55*(T112-T111)/100000+V111,U112*2*Ltime5*(T112-T111)/100000+V111)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W112*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W112>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W112*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W112>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W112*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W112>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W112*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W112>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W112*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W112>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W112*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W112>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[12.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,112,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T113-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T113-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U113*2*Main!$D$55*(T113-T112)/100000+V112,U113*2*Ltime5*(T113-T112)/100000+V112)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W113*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W113>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W113*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W113>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W113*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W113>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W113*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W113>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W113*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W113>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W113*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W113>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[2500,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,113,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T114-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T114-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U114*2*Main!$D$55*(T114-T113)/100000+V113,U114*2*Ltime5*(T114-T113)/100000+V113)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W114*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W114>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W114*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W114>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W114*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W114>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W114*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W114>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W114*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W114>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W114*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W114>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[2.87,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,114,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T115-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T115-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U115*2*Main!$D$55*(T115-T114)/100000+V114,U115*2*Ltime5*(T115-T114)/100000+V114)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W115*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W115>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W115*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W115>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W115*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W115>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W115*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W115>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W115*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W115>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W115*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W115>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[11.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T116-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T116-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U116*2*Main!$D$55*(T116-T115)/100000+V115,U116*2*Ltime5*(T116-T115)/100000+V115)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W116*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W116>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W116*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W116>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W116*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W116>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W116*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W116>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W116*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W116>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W116*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W116>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[58.7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,116,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T117-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T117-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U117*2*Main!$D$55*(T117-T116)/100000+V116,U117*2*Ltime5*(T117-T116)/100000+V116)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W117*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W117>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W117*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W117>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W117*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W117>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W117*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W117>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W117*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W117>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W117*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W117>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[325,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,117,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T118-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T118-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U118*2*Main!$D$55*(T118-T117)/100000+V117,U118*2*Ltime5*(T118-T117)/100000+V117)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W118*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W118>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W118*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W118>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W118*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W118>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W118*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W118>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W118*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W118>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W118*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W118>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,118,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T119-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T119-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U119*2*Main!$D$55*(T119-T118)/100000+V118,U119*2*Ltime5*(T119-T118)/100000+V118)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W119*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W119>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W119*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W119>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W119*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W119>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W119*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W119>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W119*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W119>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W119*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W119>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,119,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T120-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T120-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U120*2*Main!$D$55*(T120-T119)/100000+V119,U120*2*Ltime5*(T120-T119)/100000+V119)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W120*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W120>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W120*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W120>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W120*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W120>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W120*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W120>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W120*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W120>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W120*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W120>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T121-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T121-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U121*2*Main!$D$55*(T121-T120)/100000+V120,U121*2*Ltime5*(T121-T120)/100000+V120)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W121*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W121>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W121*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W121>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W121*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W121>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W121*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W121>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W121*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W121>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W121*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W121>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,121,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T122-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T122-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U122*2*Main!$D$55*(T122-T121)/100000+V121,U122*2*Ltime5*(T122-T121)/100000+V121)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W122*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W122>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W122*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W122>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W122*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W122>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W122*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W122>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W122*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W122>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W122*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W122>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,122,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T123-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T123-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U123*2*Main!$D$55*(T123-T122)/100000+V122,U123*2*Ltime5*(T123-T122)/100000+V122)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W123*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W123>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W123*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W123>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W123*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W123>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W123*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W123>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W123*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W123>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W123*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W123>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,123,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T124-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T124-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U124*2*Main!$D$55*(T124-T123)/100000+V123,U124*2*Ltime5*(T124-T123)/100000+V123)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W124*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W124>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W124*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W124>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W124*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W124>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W124*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W124>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W124*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W124>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W124*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W124>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,124,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T125-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T125-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U125*2*Main!$D$55*(T125-T124)/100000+V124,U125*2*Ltime5*(T125-T124)/100000+V124)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W125*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W125>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W125*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W125>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W125*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W125>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W125*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W125>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W125*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W125>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W125*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W125>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,125,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T126-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T126-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U126*2*Main!$D$55*(T126-T125)/100000+V125,U126*2*Ltime5*(T126-T125)/100000+V125)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W126*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W126>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W126*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W126>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W126*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W126>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W126*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W126>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W126*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W126>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W126*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W126>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,126,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T127-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T127-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U127*2*Main!$D$55*(T127-T126)/100000+V126,U127*2*Ltime5*(T127-T126)/100000+V126)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W127*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W127>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W127*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W127>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W127*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W127>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W127*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W127>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W127*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W127>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W127*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W127>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,127,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T128-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T128-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U128*2*Main!$D$55*(T128-T127)/100000+V127,U128*2*Ltime5*(T128-T127)/100000+V127)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W128*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W128>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W128*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W128>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W128*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W128>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W128*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W128>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W128*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W128>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W128*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W128>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,128,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T129-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T129-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U129*2*Main!$D$55*(T129-T128)/100000+V128,U129*2*Ltime5*(T129-T128)/100000+V128)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W129*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W129>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W129*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W129>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W129*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W129>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W129*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W129>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W129*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W129>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W129*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W129>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[{"$f":"IF(move1,C130,C131)","v":5.2839362256037736},{"$f":"IF(move1,ABS(IF(Rotativ,((time1/2+time2+time3/2)/time*(speed2-speed1)+(speed1))*gear,((Ltime1/2+Ltime2+Ltime3/2)/ltime*(Lspeed2-Lspeed1)+(Lspeed1)))),ABS(IF(Rotativ,((time1/2+time2+time3/2)/time*(ABS(speed2)-ABS(speed1))+(time5/2+time6+time7/2)/time*(ABS(speed6)-ABS(speed1))+ABS(speed1))*gear,((Ltime1/2+Ltime2+Ltime3/2)/ltime*(ABS(Lspeed2)-ABS(Lspeed1))+((Ltime5/2+Ltime6+Ltime7/2)/ltime*(ABS(Lspeed6)-ABS(Lspeed1))+ABS(Lspeed1))))))","v":451.55925155925161},{"$f":"IF($A$90=TRUE,IF($B$30=1,SQRT((D130^2*time1+D131^2*time2+D132^2*time3+D133^2*time4)/time),SQRT((((D130-D131)*2/3.1415+D131)^2*time1+D131^2*time2+((D132-D131)*2/3.145+D131)^2*time3+D133^2*time4)/time)),IF($B$30=1,SQRT((D130^2*Ltime1+D131^2*Ltime2+D132^2*Ltime3+D133^2*Ltime4)/ltime),SQRT((((D130-D131)*2/3.1415+D131)^2*Ltime1+D131^2*Ltime2+((D132-D131)*2/3.145+D131)^2*Ltime3+D133^2*Ltime4)/ltime)))","v":5.2839362256037736},{"$f":"IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1297,$B$107,1),INDEX(LinMotor!$V$1:$V$1305,$B$107,1))","v":15.040824891297582},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,129,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T130-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T130-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U130*2*Main!$D$55*(T130-T129)/100000+V129,U130*2*Ltime5*(T130-T129)/100000+V129)","v":0},{"$f":"IF(move1,IF(ABS(MIN($U$1:$U$101))>MAX($U$1:$U$101),U130/MIN($U$1:$U$101)*-1,U130/MAX($U$1:$U$101)),IF(ABS(MIN($U$1:$U$201))>MAX($U$1:$U$201),U130/MIN($U$1:$U$201)*-1,U130/MAX($U$1:$U$201)))","v":0},{"$f":"IF(move1,IF(ABS(MIN($V$1:$V$101))>MAX($V$1:$V$101),V130/MIN($V$1:$V$101)*-1,V130/MAX($V$1:$V$101)),IF(ABS(MIN($V$1:$V$201))>MAX($V$1:$V$201),V130/MIN($V$1:$V$201)*-1,V130/MAX($V$1:$V$201)))","v":0},{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W130*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W130>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W130*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W130>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W130*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W130>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W130*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W130>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W130*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W130>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W130*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W130>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,{"$f":"IF($A$90=TRUE,IF($B$30=1,SQRT((D130^2*time1+D131^2*time2+D132^2*time3+D133^2*time4+D134^2*time5+D135^2*time6+D136^2*time7+D137^2*time8)/time),SQRT((((D130-D131)*2/3.1415+D131)^2*time1+D131^2*time2+((D132-D131)*2/3.145+D131)^2*time3+D133^2*time4+((D134-D135)*2/3.1415+D135)^2*time5+D135^2*time6+((D136-D135)*2/3.145+D135)^2*time7+D137^2*time8)/time)),IF($B$30=1,SQRT((D130^2*Ltime1+D131^2*Ltime2+D132^2*Ltime3+D133^2*Ltime4+D134^2*Ltime5+D135^2*Ltime6+D136^2*Ltime7+D137^2*Ltime8)/ltime),SQRT((((D130-D131)*2/3.1415+D131)^2*Ltime1+D131^2*Ltime2+((D132-D131)*2/3.145+D131)^2*Ltime3+D133^2*Ltime4+((D134-D135)*2/3.1415+D135)^2*Ltime5+D135^2*Ltime6+((D136-D135)*2/3.145+D135)^2*Ltime7+D137^2*Ltime8)/ltime)))","v":5.2839362256037736},{"$f":"IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1297,$B$107,1),INDEX(LinMotor!$W$1:$W$1305,$B$107,1))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,130,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T131-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T131-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U131*2*Main!$D$55*(T131-T130)/100000+V130,U131*2*Ltime5*(T131-T130)/100000+V130)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W131*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W131>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W131*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W131>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W131*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W131>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W131*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W131>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W131*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W131>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W131*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W131>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X131*speed,X131*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X131*speed,X131*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":0}]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1297,$B$107,1),INDEX(LinMotor!$X$1:$X$1305,$B$107,1))","v":-12.183068161951041},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,131,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T132-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T132-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U132*2*Main!$D$55*(T132-T131)/100000+V131,U132*2*Ltime5*(T132-T131)/100000+V131)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W132*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W132>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W132*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W132>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W132*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W132>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W132*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W132>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W132*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W132>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W132*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W132>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1297,$B$107,1),INDEX(LinMotor!$Y$1:$Y$1305,$B$107,1))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,132,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T133-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T133-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U133*2*Main!$D$55*(T133-T132)/100000+V132,U133*2*Ltime5*(T133-T132)/100000+V132)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W133*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W133>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W133*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W133>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W133*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W133>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W133*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W133>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W133*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W133>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W133*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W133>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1297,$B$107,1),INDEX(LinMotor!$Z$1:$Z$1305,$B$107,1))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T134-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T134-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U134*2*Main!$D$55*(T134-T133)/100000+V133,U134*2*Ltime5*(T134-T133)/100000+V133)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W134*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W134>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W134*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W134>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W134*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W134>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W134*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W134>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W134*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W134>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W134*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W134>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$AC$1:$AC$1297,$B$107,1),INDEX(LinMotor!$AA$1:$AA$1305,$B$107,1))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,134,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T135-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T135-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U135*2*Main!$D$55*(T135-T134)/100000+V134,U135*2*Ltime5*(T135-T134)/100000+V134)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W135*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W135>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W135*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W135>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W135*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W135>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W135*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W135>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W135*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W135>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W135*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W135>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1297,$B$107,1),INDEX(LinMotor!$AB$1:$AB$1305,$B$107,1))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,135,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T136-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T136-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U136*2*Main!$D$55*(T136-T135)/100000+V135,U136*2*Ltime5*(T136-T135)/100000+V135)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W136*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W136>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W136*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W136>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W136*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W136>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W136*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W136>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W136*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W136>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W136*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W136>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$AE$1:$AE$1297,$B$107,1),INDEX(LinMotor!$AC$1:$AC$1305,$B$107,1))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,136,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T137-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T137-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U137*2*Main!$D$55*(T137-T136)/100000+V136,U137*2*Ltime5*(T137-T136)/100000+V136)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W137*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W137>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W137*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W137>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W137*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W137>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W137*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W137>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W137*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W137>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W137*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W137>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,137,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T138-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T138-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U138*2*Main!$D$55*(T138-T137)/100000+V137,U138*2*Ltime5*(T138-T137)/100000+V137)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W138*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W138>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W138*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W138>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W138*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W138>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W138*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W138>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W138*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W138>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W138*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W138>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,138,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T139-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T139-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U139*2*Main!$D$55*(T139-T138)/100000+V138,U139*2*Ltime5*(T139-T138)/100000+V138)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W139*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W139>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W139*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W139>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W139*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W139>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W139*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W139>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W139*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W139>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W139*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W139>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
["","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,139,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T140-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T140-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U140*2*Main!$D$55*(T140-T139)/100000+V139,U140*2*Ltime5*(T140-T139)/100000+V139)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W140*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W140>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W140*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W140>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W140*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W140>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W140*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W140>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W140*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W140>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W140*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W140>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,140,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T141-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T141-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U141*2*Main!$D$55*(T141-T140)/100000+V140,U141*2*Ltime5*(T141-T140)/100000+V140)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W141*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W141>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W141*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W141>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W141*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W141>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W141*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W141>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W141*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W141>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W141*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W141>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,141,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T142-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T142-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U142*2*Main!$D$55*(T142-T141)/100000+V141,U142*2*Ltime5*(T142-T141)/100000+V141)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W142*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W142>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W142*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W142>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W142*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W142>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W142*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W142>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W142*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W142>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W142*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W142>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,142,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T143-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T143-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U143*2*Main!$D$55*(T143-T142)/100000+V142,U143*2*Ltime5*(T143-T142)/100000+V142)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W143*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W143>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W143*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W143>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W143*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W143>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W143*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W143>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W143*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W143>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W143*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W143>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,143,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T144-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T144-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U144*2*Main!$D$55*(T144-T143)/100000+V143,U144*2*Ltime5*(T144-T143)/100000+V143)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W144*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W144>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W144*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W144>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W144*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W144>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W144*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W144>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W144*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W144>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W144*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W144>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,144,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T145-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T145-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U145*2*Main!$D$55*(T145-T144)/100000+V144,U145*2*Ltime5*(T145-T144)/100000+V144)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W145*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W145>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W145*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W145>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W145*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W145>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W145*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W145>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W145*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W145>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W145*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W145>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,146,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T146-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T146-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U146*2*Main!$D$55*(T146-T145)/100000+V145,U146*2*Ltime5*(T146-T145)/100000+V145)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W146*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W146>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W146*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W146>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W146*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W146>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W146*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W146>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W146*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W146>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W146*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W146>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,148,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T147-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T147-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U147*2*Main!$D$55*(T147-T146)/100000+V146,U147*2*Ltime5*(T147-T146)/100000+V146)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W147*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W147>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W147*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W147>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W147*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W147>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W147*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W147>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W147*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W147>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W147*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W147>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,149,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T148-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T148-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U148*2*Main!$D$55*(T148-T147)/100000+V147,U148*2*Ltime5*(T148-T147)/100000+V147)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W148*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W148>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W148*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W148>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W148*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W148>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W148*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W148>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W148*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W148>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W148*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W148>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,149.99999,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T149-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T149-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U149*2*Main!$D$55*(T149-T148)/100000+V148,U149*2*Ltime5*(T149-T148)/100000+V148)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W149*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W149>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W149*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W149>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W149*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W149>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W149*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W149>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W149*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W149>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W149*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W149>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,149.99999,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T150-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T150-100)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U150*2*Main!$D$55*(T150-T149)/100000+V149,U150*2*Ltime5*(T150-T149)/100000+V149)","v":0},0,0,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W150*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W150>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W150*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W150>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W150*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W150>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W150*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W150>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W150*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W150>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W150*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W150>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad))),0)","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,0,{"$f":"IF($A$90=TRUE,Main!$E$57,Lspeed6)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W151*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W151>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W151*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W151>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W151*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W151>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W151*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W151>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W151*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W151>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W151*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W151>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150.000001,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T152-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T152-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U152*2*Main!$D$59*(T152-T151)/100000+V151,U152*2*Ltime7*(T152-T151)/100000+V151)","v":0},0,0,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W152*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W152<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W152*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W152<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W152*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W152<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W152*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W152<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W152*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W152<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W152*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W152<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad))),0)","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150.000001,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T153-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T153-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U153*2*Main!$D$59*(T153-T152)/100000+V152,U153*2*Ltime7*(T153-T152)/100000+V152)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W153*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W153<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W153*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W153<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W153*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W153<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W153*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W153<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W153*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W153<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W153*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W153<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,151,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T154-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T154-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U154*2*Main!$D$59*(T154-T153)/100000+V153,U154*2*Ltime7*(T154-T153)/100000+V153)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W154*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W154<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W154*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W154<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W154*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W154<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W154*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W154<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W154*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W154<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W154*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W154<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,152,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T155-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T155-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U155*2*Main!$D$59*(T155-T154)/100000+V154,U155*2*Ltime7*(T155-T154)/100000+V154)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W155*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W155<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W155*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W155<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W155*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W155<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W155*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W155<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W155*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W155<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W155*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W155<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,154,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T156-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T156-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U156*2*Main!$D$59*(T156-T155)/100000+V155,U156*2*Ltime7*(T156-T155)/100000+V155)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W156*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W156<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W156*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W156<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W156*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W156<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W156*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W156<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W156*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W156<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W156*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W156<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,156,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T157-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T157-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U157*2*Main!$D$59*(T157-T156)/100000+V156,U157*2*Ltime7*(T157-T156)/100000+V156)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W157*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W157<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W157*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W157<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W157*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W157<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W157*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W157<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W157*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W157<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W157*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W157<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,157,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T158-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T158-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U158*2*Main!$D$59*(T158-T157)/100000+V157,U158*2*Ltime7*(T158-T157)/100000+V157)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W158*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W158<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W158*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W158<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W158*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W158<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W158*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W158<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W158*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W158<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W158*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W158<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,158,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T159-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T159-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U159*2*Main!$D$59*(T159-T158)/100000+V158,U159*2*Ltime7*(T159-T158)/100000+V158)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W159*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W159<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W159*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W159<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W159*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W159<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W159*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W159<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W159*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W159<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W159*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W159<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,159,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T160-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T160-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U160*2*Main!$D$59*(T160-T159)/100000+V159,U160*2*Ltime7*(T160-T159)/100000+V159)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W160*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W160<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W160*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W160<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W160*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W160<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W160*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W160<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W160*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W160<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W160*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W160<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,160,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T161-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T161-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U161*2*Main!$D$59*(T161-T160)/100000+V160,U161*2*Ltime7*(T161-T160)/100000+V160)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W161*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W161<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W161*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W161<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W161*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W161<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W161*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W161<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W161*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W161<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W161*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W161<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,161,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T162-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T162-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U162*2*Main!$D$59*(T162-T161)/100000+V161,U162*2*Ltime7*(T162-T161)/100000+V161)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W162*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W162<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W162*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W162<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W162*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W162<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W162*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W162<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W162*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W162<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W162*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W162<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,162,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T163-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T163-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U163*2*Main!$D$59*(T163-T162)/100000+V162,U163*2*Ltime7*(T163-T162)/100000+V162)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W163*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W163<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W163*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W163<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W163*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W163<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W163*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W163<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W163*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W163<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W163*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W163<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,163,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T164-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T164-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U164*2*Main!$D$59*(T164-T163)/100000+V163,U164*2*Ltime7*(T164-T163)/100000+V163)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W164*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W164<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W164*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W164<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W164*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W164<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W164*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W164<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W164*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W164<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W164*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W164<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,164,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T165-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T165-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U165*2*Main!$D$59*(T165-T164)/100000+V164,U165*2*Ltime7*(T165-T164)/100000+V164)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W165*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W165<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W165*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W165<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W165*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W165<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W165*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W165<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W165*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W165<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W165*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W165<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,165,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T166-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T166-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U166*2*Main!$D$59*(T166-T165)/100000+V165,U166*2*Ltime7*(T166-T165)/100000+V165)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W166*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W166<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W166*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W166<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W166*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W166<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W166*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W166<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W166*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W166<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W166*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W166<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"100+T67","v":166},{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T167-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T167-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U167*2*Main!$D$59*(T167-T166)/100000+V166,U167*2*Ltime7*(T167-T166)/100000+V166)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W167*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W167<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W167*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W167<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W167*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W167<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W167*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W167<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W167*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W167<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W167*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W167<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,167,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T168-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T168-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U168*2*Main!$D$59*(T168-T167)/100000+V167,U168*2*Ltime7*(T168-T167)/100000+V167)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W168*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W168<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W168*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W168<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W168*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W168<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W168*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W168<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W168*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W168<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W168*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W168<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,168,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T169-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T169-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U169*2*Main!$D$59*(T169-T168)/100000+V168,U169*2*Ltime7*(T169-T168)/100000+V168)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W169*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W169<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W169*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W169<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W169*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W169<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W169*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W169<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W169*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W169<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W169*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W169<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,169,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T170-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T170-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U170*2*Main!$D$59*(T170-T169)/100000+V169,U170*2*Ltime7*(T170-T169)/100000+V169)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W170*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W170<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W170*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W170<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W170*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W170<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W170*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W170<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W170*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W170<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W170*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W170<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,170,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T171-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T171-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U171*2*Main!$D$59*(T171-T170)/100000+V170,U171*2*Ltime7*(T171-T170)/100000+V170)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W171*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W171<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W171*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W171<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W171*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W171<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W171*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W171<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W171*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W171<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W171*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W171<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,171,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T172-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T172-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U172*2*Main!$D$59*(T172-T171)/100000+V171,U172*2*Ltime7*(T172-T171)/100000+V171)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W172*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W172<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W172*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W172<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W172*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W172<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W172*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W172<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W172*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W172<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W172*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W172<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,172,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T173-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T173-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U173*2*Main!$D$59*(T173-T172)/100000+V172,U173*2*Ltime7*(T173-T172)/100000+V172)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W173*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W173<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W173*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W173<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W173*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W173<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W173*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W173<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W173*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W173<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W173*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W173<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,173,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T174-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T174-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U174*2*Main!$D$59*(T174-T173)/100000+V173,U174*2*Ltime7*(T174-T173)/100000+V173)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W174*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W174<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W174*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W174<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W174*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W174<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W174*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W174<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W174*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W174<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W174*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W174<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,174,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T175-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T175-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U175*2*Main!$D$59*(T175-T174)/100000+V174,U175*2*Ltime7*(T175-T174)/100000+V174)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W175*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W175<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W175*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W175<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W175*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W175<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W175*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W175<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W175*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W175<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W175*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W175<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,175,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T176-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T176-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U176*2*Main!$D$59*(T176-T175)/100000+V175,U176*2*Ltime7*(T176-T175)/100000+V175)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W176*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W176<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W176*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W176<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W176*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W176<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W176*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W176<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W176*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W176<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W176*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W176<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,176,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T177-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T177-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U177*2*Main!$D$59*(T177-T176)/100000+V176,U177*2*Ltime7*(T177-T176)/100000+V176)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W177*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W177<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W177*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W177<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W177*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W177<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W177*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W177<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W177*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W177<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W177*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W177<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,177,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T178-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T178-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U178*2*Main!$D$59*(T178-T177)/100000+V177,U178*2*Ltime7*(T178-T177)/100000+V177)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W178*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W178<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W178*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W178<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W178*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W178<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W178*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W178<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W178*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W178<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W178*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W178<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,178,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T179-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T179-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U179*2*Main!$D$59*(T179-T178)/100000+V178,U179*2*Ltime7*(T179-T178)/100000+V178)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W179*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W179<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W179*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W179<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W179*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W179<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W179*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W179<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W179*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W179<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W179*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W179<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,179,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T180-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T180-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U180*2*Main!$D$59*(T180-T179)/100000+V179,U180*2*Ltime7*(T180-T179)/100000+V179)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W180*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W180<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W180*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W180<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W180*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W180<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W180*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W180<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W180*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W180<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W180*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W180<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,180,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T181-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T181-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U181*2*Main!$D$59*(T181-T180)/100000+V180,U181*2*Ltime7*(T181-T180)/100000+V180)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W181*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W181<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W181*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W181<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W181*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W181<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W181*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W181<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W181*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W181<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W181*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W181<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,181,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T182-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T182-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U182*2*Main!$D$59*(T182-T181)/100000+V181,U182*2*Ltime7*(T182-T181)/100000+V181)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W182*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W182<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W182*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W182<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W182*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W182<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W182*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W182<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W182*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W182<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W182*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W182<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,182,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T183-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T183-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U183*2*Main!$D$59*(T183-T182)/100000+V182,U183*2*Ltime7*(T183-T182)/100000+V182)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W183*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W183<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W183*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W183<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W183*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W183<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W183*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W183<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W183*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W183<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W183*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W183<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,183,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T184-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T184-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U184*2*Main!$D$59*(T184-T183)/100000+V183,U184*2*Ltime7*(T184-T183)/100000+V183)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W184*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W184<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W184*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W184<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W184*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W184<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W184*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W184<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W184*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W184<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W184*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W184<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,184,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T185-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T185-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U185*2*Main!$D$59*(T185-T184)/100000+V184,U185*2*Ltime7*(T185-T184)/100000+V184)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W185*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W185<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W185*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W185<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W185*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W185<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W185*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W185<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W185*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W185<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W185*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W185<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,185,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T186-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T186-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U186*2*Main!$D$59*(T186-T185)/100000+V185,U186*2*Ltime7*(T186-T185)/100000+V185)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W186*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W186<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W186*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W186<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W186*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W186<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W186*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W186<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W186*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W186<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W186*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W186<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,186,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T187-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T187-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U187*2*Main!$D$59*(T187-T186)/100000+V186,U187*2*Ltime7*(T187-T186)/100000+V186)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W187*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W187<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W187*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W187<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W187*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W187<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W187*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W187<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W187*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W187<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W187*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W187<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,187,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T188-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T188-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U188*2*Main!$D$59*(T188-T187)/100000+V187,U188*2*Ltime7*(T188-T187)/100000+V187)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W188*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W188<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W188*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W188<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W188*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W188<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W188*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W188<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W188*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W188<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W188*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W188<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,188,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T189-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T189-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U189*2*Main!$D$59*(T189-T188)/100000+V188,U189*2*Ltime7*(T189-T188)/100000+V188)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W189*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W189<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W189*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W189<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W189*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W189<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W189*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W189<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W189*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W189<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W189*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W189<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,189,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T190-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T190-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U190*2*Main!$D$59*(T190-T189)/100000+V189,U190*2*Ltime7*(T190-T189)/100000+V189)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W190*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W190<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W190*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W190<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W190*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W190<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W190*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W190<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W190*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W190<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W190*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W190<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,190,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T191-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T191-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U191*2*Main!$D$59*(T191-T190)/100000+V190,U191*2*Ltime7*(T191-T190)/100000+V190)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W191*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W191<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W191*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W191<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W191*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W191<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W191*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W191<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W191*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W191<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W191*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W191<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,191,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T192-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T192-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U192*2*Main!$D$59*(T192-T191)/100000+V191,U192*2*Ltime7*(T192-T191)/100000+V191)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W192*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W192<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W192*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W192<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W192*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W192<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W192*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W192<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W192*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W192<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W192*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W192<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,192,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T193-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T193-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U193*2*Main!$D$59*(T193-T192)/100000+V192,U193*2*Ltime7*(T193-T192)/100000+V192)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W193*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W193<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W193*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W193<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W193*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W193<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W193*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W193<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W193*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W193<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W193*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W193<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,193,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T194-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T194-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U194*2*Main!$D$59*(T194-T193)/100000+V193,U194*2*Ltime7*(T194-T193)/100000+V193)","v":0},{"$f":"IF(move1,IF(ABS(MIN($U$1:$U$101))>MAX($U$1:$U$101),U194/MIN($U$1:$U$101)*-1,U194/MAX($U$1:$U$101)),IF(ABS(MIN($U$1:$U$201))>MAX($U$1:$U$201),U194/MIN($U$1:$U$201)*-1,U194/MAX($U$1:$U$201)))","v":0},{"$f":"IF(move1,IF(ABS(MIN($V$1:$V$101))>MAX($V$1:$V$101),V194/MIN($V$1:$V$101)*-1,V194/MAX($V$1:$V$101)),IF(ABS(MIN($V$1:$V$201))>MAX($V$1:$V$201),V194/MIN($V$1:$V$201)*-1,V194/MAX($V$1:$V$201)))","v":0},{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W194*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W194<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W194*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W194<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W194*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W194<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W194*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W194<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W194*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W194<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W194*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W194<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,194,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T195-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T195-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U195*2*Main!$D$59*(T195-T194)/100000+V194,U195*2*Ltime7*(T195-T194)/100000+V194)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W195*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W195<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W195*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W195<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W195*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W195<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W195*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W195<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W195*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W195<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W195*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W195<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X195*speed,X195*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X195*speed,X195*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,196,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T196-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T196-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U196*2*Main!$D$59*(T196-T195)/100000+V195,U196*2*Ltime7*(T196-T195)/100000+V195)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W196*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W196<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W196*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W196<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W196*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W196<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W196*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W196<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W196*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W196<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W196*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W196<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,198,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T197-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T197-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U197*2*Main!$D$59*(T197-T196)/100000+V196,U197*2*Ltime7*(T197-T196)/100000+V196)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W197*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W197<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W197*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W197<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W197*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W197<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W197*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W197<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W197*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W197<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W197*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W197<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,199,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T198-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T198-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U198*2*Main!$D$59*(T198-T197)/100000+V197,U198*2*Ltime7*(T198-T197)/100000+V197)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W198*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W198<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W198*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W198<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W198*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W198<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W198*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W198<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W198*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W198<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W198*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W198<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,199.999999,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T199-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T199-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U199*2*Main!$D$59*(T199-T198)/100000+V198,U199*2*Ltime7*(T199-T198)/100000+V198)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W199*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W199<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W199*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W199<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W199*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W199<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W199*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W199<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W199*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W199<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W199*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W199<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},0]
["Steuerung Rotatorisch Others",null,{"$f":"IF((SUM(Motor!O3:O12))>0,1,0)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,199.999999,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T200-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T200-150)*PI()/50))))","v":0},{"$f":"IF($A$90=TRUE,U200*2*Main!$D$59*(T200-T199)/100000+V199,U200*2*Ltime7*(T200-T199)/100000+V199)","v":0},0,0,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W200*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W200<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W200*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W200<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W200*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W200<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W200*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W200<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W200*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W200<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W200*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W200<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad))),0)","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,0,{"$f":"IF($A$90=TRUE,Main!$E$46,Lspeed1)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W201*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W201<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W201*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W201<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W201*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W201<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W201*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W201<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W201*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W201<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W201*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W201<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":0},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X201*speed,X201*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X201*speed,X201*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":0}]

{"sheet":"Graphic","index":9,"n_rows":46,"n_cols":14,"rows_kept":46,"cut":false,"hidden":false,"merged":[[44,13,44,16],[43,8,43,10],[42,8,42,10],[0,0,0,18],[1,1,5,11],[1,12,5,17],[41,8,41,10],[42,13,42,16],[43,13,43,16]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Mo [Nm]",{"$f":"IF(I46=\"Linear\",Main!R71,Main!R43)","v":4.51},null,"Mmax[Nm]",{"$f":"IF(I46=\"Linear\",Main!R76,Main!R48)","v":12.2},null,"Motor",{"$f":"IFERROR(Calc!A70,\"no data\")","v":"C041B (240 V)"}]
[null,"Io [A]",{"$f":"IF(I46=\"Linear\",Main!R72,Main!R44)","v":4.6900000000000004},null,"nmax[min-1]",{"$f":"IF(I46=\"Linear\",Main!R77,Main!R49)","v":2500},null,"Drive",{"$f":"IFERROR(Drives!A2,\"no data\")","v":"S712"},null,null,null,null,"AnyDim Application Support"]
[null,"Mn [Nm]",{"$f":"IF(I46=\"Linear\",Main!R73,Main!R45)","v":4.0107045659157627},null,"Ru-v [Ohm]",{"$f":"IF(I46=\"Linear\",Main!R78,Main!R50)","v":2.87},null,"Voltage",{"$f":"IFERROR(CONCATENATE(Calc!B2,\" V\"),\"no data\")","v":"230 V"},null,null,null,null,"Email: technik@kollmorgen.com"]
[null,"In [A]",{"$f":"IF(I46=\"Linear\",Main!R74,Main!R46)","v":4.1347469751708896},null,"Lu-v [mH]",{"$f":"IF(I46=\"Linear\",Main!R79,Main!R51)","v":11.4},null,null,null,null,null,null,null,"Tel.: +49 (0)2102 93940"]
[null,"nn [min-1]",{"$f":"IF(I46=\"Linear\",Main!R75,Main!R47)","v":2500},null,"Ke [V/10^3]",{"$f":"IF(I46=\"Linear\",Main!R80,Main!R52)","v":58.7},null,"Motortype","Rotative"]